{"text_format":"1","workbook":"xlsx","n_sheets":12,"sheets":["Startseite","Schadstoffbelastung","Schadstoffkonzentration Boden","Tabelle1","Schadstoffbelastung GW","Bodencharakterisierung","Grundwassercharakterisierung","Heterogenität","Stoffdatenbank","Sanierungsdesign","Calculation","Berechnung"],"not_rendered":{"charts":6,"images":34,"macros":1,"external_links":1,"defined_names":39,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"row_number_cap","date_system":"1900"}

{"sheet":"Startseite","index":0,"n_rows":5,"n_cols":13,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
[]
["Berechnung der Sanierungsdauer",null,null,null,null,null,null,null,null,null,null,"Excel-Version",{"$f":"INFO(\"version\")","v":"16.0"}]
[" Anaerober mikrobieller LCKW-Abbau"]
[]
["  Version 1.0"]

{"sheet":"Schadstoffbelastung","index":1,"n_rows":54,"n_cols":26,"rows_kept":54,"cut":false,"hidden":true,"merged":[[1,3,2,3],[1,9,2,9],[1,4,2,4],[1,1,2,1],[1,7,2,8],[1,20,2,20],[1,21,2,21],[1,22,2,22],[1,23,2,23],[1,25,2,25],[1,24,2,24],[53,8,54,10],[10,7,11,8],[1,12,2,13],[1,14,2,14],[1,15,2,15],[1,10,2,10]]}
[]
[null,"Schadstoff",null,"MB + 2 s \n[mg/m² OS]","Inventar \n[kg]",null,null,"Geometrie des Schadensherdes",null,"Einheit","Wert",null," Schadstoffstatistik",null,"Einheit","LCKW","AKW",null,null,null,"Mittl. Konz. (GW) \n[µg/L]","Mittl. Konz. (GW) \n[µmol/L]","Ci [µg/L]","Grenzkonz. Boden [mg/kg]","Mittlere Konz. Boden [mg/kg]","Residualphase [mg/kg]"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,"Tetrachlorethen","PCE",null,{"$f":"IF($R$3,'Schadstoffkonzentration Boden'!$Z$27,'Schadstoffbelastung GW'!V8)","v":48.585599999999999},null,null,"Mittlere Länge (Schadensherd)",null,"m",10,null," Minimum",null,"mg/kg OS",{"$f":"IF($R$3,'Schadstoffkonzentration Boden'!$W$93,\"\")","v":""},null,null,null,"PCE",{"$f":"'Schadstoffbelastung GW'!Y8","v":700},{"$f":"U4/Stoffdatenbank!R5","v":4.2168674698795181},{"$f":"Stoffdatenbank!N5*1000*(Schadstoffbelastung!V4/Schadstoffbelastung!V$17)","v":25965.560764859943},{"$f":"U4/1000*Bodencharakterisierung!$E$9*Stoffdatenbank!J5","v":2.5199999999999996},{"$f":"IFERROR(E4*1000/$K$12,0)","v":26.724752475247527},{"$f":"IF(Y4<X4,0,Y4-X4)","v":24.204752475247528}]
[null,"Trichlorethen","TCE",null,{"$f":"IF($R$3,'Schadstoffkonzentration Boden'!Z28,'Schadstoffbelastung GW'!V9)","v":18.763919999999999},null,null,"Mittlere Breite (Schadensherd)",null,"m",20,null," Maximum",null,"mg/kg OS",{"$f":"IF($R$3,'Schadstoffkonzentration Boden'!$X$93,\"\")","v":""},null,null,null,"TCE",{"$f":"'Schadstoffbelastung GW'!Y9","v":680},{"$f":"U5/Stoffdatenbank!R6","v":5.1908396946564883},{"$f":"Stoffdatenbank!N6*1000*(Schadstoffbelastung!V5/Schadstoffbelastung!V$17)","v":199767.75484851352},{"$f":"U5/1000*Bodencharakterisierung!$E$9*Stoffdatenbank!J6","v":0.88400000000000012},{"$f":"IFERROR(E5*1000/$K$12,0)","v":10.321188118811882},{"$f":"IF(Y5<X5,0,Y5-X5)","v":9.437188118811882}]
[null,"cis-1,2-Dichlorethen","cDCE",null,{"$f":"IF($R$3,'Schadstoffkonzentration Boden'!Z29,'Schadstoffbelastung GW'!V10)","v":16.965},null,null,"Fläche der Belastung",null,"m²",{"$f":"K4*K5","v":200},null," Median",null,"mg/kg OS",{"$f":"IF($R$3,'Schadstoffkonzentration Boden'!$Y$93,\"\")","v":""},null,null,null,"cDCE",{"$f":"'Schadstoffbelastung GW'!Y10","v":1300},{"$f":"U6/Stoffdatenbank!R7","v":13.402061855670103},{"$f":"Stoffdatenbank!N7*1000*(Schadstoffbelastung!V6/Schadstoffbelastung!V$17)","v":1805208.7670930335},{"$f":"U6/1000*Bodencharakterisierung!$E$9*Stoffdatenbank!J7","v":0.65},9.3316831683168324,8.6816831683168321]
[null,"trans-1,2-Dichlorethen","tDCE",null,{"$f":"IF($R$3,'Schadstoffkonzentration Boden'!Z30,'Schadstoffbelastung GW'!V11)","v":1.4868E-10},null,null,"Oberkante der Belastung",null,"m u. GOK",2,null," Mittlere Konzentration (arithm.)",null,"mg/kg OS",{"$f":"IF($R$3,'Schadstoffkonzentration Boden'!$Z$93,\"\")","v":""},null,null,null,"tDCE",{"$f":"'Schadstoffbelastung GW'!Y11","v":1E-8},{"$f":"U7/Stoffdatenbank!R8","v":1.0309278350515464E-10},{"$f":"Stoffdatenbank!N8*1000*(Schadstoffbelastung!V7/Schadstoffbelastung!V$17)","v":2.4995198313595848E-5},{"$f":"U7/1000*Bodencharakterisierung!$E$9*Stoffdatenbank!J8","v":6.0000000000000011E-12},8.1782178217821798E-11,7.5782178217821793E-11]
[null,"1,1-Dichlorethen","11DCE",null,{"$f":"IF($R$3,'Schadstoffkonzentration Boden'!Z31,'Schadstoffbelastung GW'!V12)","v":1.6778718000000002E-10},null,null,"Unterkante der Belastung",null,"m u. GOK",8,null," Standardabweichung",null,"mg/kg OS",{"$f":"IF($R$3,'Schadstoffkonzentration Boden'!$AA$93,\"\")","v":""},null,null,null,"11DCE",{"$f":"'Schadstoffbelastung GW'!Y12","v":1E-8},{"$f":"U8/Stoffdatenbank!R9","v":1.0309278350515464E-10},{"$f":"Stoffdatenbank!N9*1000*(Schadstoffbelastung!V8/Schadstoffbelastung!V$17)","v":9.9187294895221612E-6},{"$f":"U8/1000*Bodencharakterisierung!$E$9*Stoffdatenbank!J9","v":7.0510000000000014E-12},9.2292178217821796E-11,8.5241178217821796E-11]
[null,"Vinylchlorid","VC",null,{"$f":"IF($R$3,'Schadstoffkonzentration Boden'!Z32,'Schadstoffbelastung GW'!V13)","v":2.9736000000000002},null,null,"Mittlere Mächtigkeit (Schadensherd)",null,"m",{"$f":"K8-K7","v":6},null," MW + 2 s",null,"mg/kg OS",{"$f":"IF($R$3,'Schadstoffkonzentration Boden'!$AB$93,\"\")","v":""},null,null,null,"VC",{"$f":"'Schadstoffbelastung GW'!Y13","v":200},{"$f":"U9/Stoffdatenbank!R10","v":3.1746031746031744},{"$f":"Stoffdatenbank!N10*1000*(Schadstoffbelastung!V9/Schadstoffbelastung!V$17)","v":134390.91257549395},{"$f":"U9/1000*Bodencharakterisierung!$E$9*Stoffdatenbank!J10","v":0.12},1.635643564356436,1.5156435643564361]
[null,"Tetrachlormethan","CT",null,{"$f":"IF($R$3,'Schadstoffkonzentration Boden'!Z33,'Schadstoffbelastung GW'!V14)","v":5.5882079999999999E-10},null,null,"Bodenlagerungsdichte",null,"kg/L",{"$f":"Bodencharakterisierung!E11","v":1.5149999999999999},null," Schadstoffinventar (mittelwertbezogen)",null,"kg",{"$f":"IF($R$3,'Schadstoffkonzentration Boden'!$AC$93,\"\")","v":""},null,null,null,"CT",{"$f":"'Schadstoffbelastung GW'!Y14","v":1E-8},{"$f":"U10/Stoffdatenbank!R11","v":6.4935064935064938E-11},{"$f":"Stoffdatenbank!N11*1000*(Schadstoffbelastung!V10/Schadstoffbelastung!V$17)","v":1.9992036581478439E-6},{"$f":"U10/1000*Bodencharakterisierung!$E$9*Stoffdatenbank!J11","v":2.8560000000000006E-11},3.0738217821782181E-10,{"$f":"IF(Y10<X10,0,Y10-X10)","v":2.7882217821782181E-10}]
[null,"Trichlormethan","CF",null,{"$f":"IF($R$3,'Schadstoffkonzentration Boden'!Z34,'Schadstoffbelastung GW'!V15)","v":1.3269977999999999E-10},null,null,"Volumen kontaminierter Boden",null,"m³",{"$f":"K9*K6","v":1200},null," Schadstoffinventar (flächengewichtet)",null,"kg",{"$f":"IF($R$3,'Schadstoffkonzentration Boden'!$W$93,\"\")","v":""},null,null,null,"CF",{"$f":"'Schadstoffbelastung GW'!Y15","v":1E-8},{"$f":"U11/Stoffdatenbank!R12","v":8.4033613445378151E-11},{"$f":"Stoffdatenbank!N12*1000*(Schadstoffbelastung!V11/Schadstoffbelastung!V$17)","v":2.6518848524255219E-5},{"$f":"U11/1000*Bodencharakterisierung!$E$9*Stoffdatenbank!J12","v":5.1210000000000005E-12},7.2992178217821783E-11,6.7871178217821783E-11]
[null,"Dichlormethan","DCM",null,{"$f":"IF($R$3,'Schadstoffkonzentration Boden'!Z35,'Schadstoffbelastung GW'!V16)","v":6.1688699999999995E-11},null,null,null,null,"t",{"$f":"K11*K10","v":1817.9999999999998},null," Schadstoffinventrar (residuale Phase)",null,"kg",{"$f":"Z17","v":43.839267327460682},null,null,null,"DCM",{"$f":"'Schadstoffbelastung GW'!Y16","v":1E-8},{"$f":"U12/Stoffdatenbank!R13","v":1.1764705882352941E-10},{"$f":"Stoffdatenbank!N13*1000*(Schadstoffbelastung!V12/Schadstoffbelastung!V$17)","v":8.0586899858110502E-5},{"$f":"U12/1000*Bodencharakterisierung!$E$9*Stoffdatenbank!J13","v":1.215E-12},3.3932178217821784E-11,3.2717178217821785E-11]
[null,"1,1,1-Trichlorethan","111TCA",null,{"$f":"IF($R$3,'Schadstoffkonzentration Boden'!Z36,'Schadstoffbelastung GW'!V17)","v":3.0139200000000002E-11},null,null,"Grundwasserflurabstand",null,"m u. GOK",3,null,null,null,null,null,null,null,null,"111TCA",{"$f":"'Schadstoffbelastung GW'!Y17","v":1.0000000000000001E-9},{"$f":"U13/Stoffdatenbank!R14","v":7.4960271056340151E-12},{"$f":"Stoffdatenbank!N14*1000*(Schadstoffbelastung!V13/Schadstoffbelastung!V$17)","v":3.7502677239925182E-7},{"$f":"U13/1000*Bodencharakterisierung!$E$9*Stoffdatenbank!J14","v":1.4399999999999999E-12},1.6578217821782181E-11,1.513821782178218E-11]
[null,"1,1,2-Trichlorethan","112TCA",null,{"$f":"IF($R$3,'Schadstoffkonzentration Boden'!Z37,'Schadstoffbelastung GW'!V18)","v":1.1893752E-10},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"112TCA",{"$f":"'Schadstoffbelastung GW'!Y18","v":1E-8},{"$f":"U14/Stoffdatenbank!R15","v":7.4960271056340138E-11},{"$f":"Stoffdatenbank!N15*1000*(Schadstoffbelastung!V14/Schadstoffbelastung!V$17)","v":1.298169596766641E-5},{"$f":"U14/1000*Bodencharakterisierung!$E$9*Stoffdatenbank!J15","v":4.3640000000000004E-12},6.542217821782179E-11,6.1058178217821796E-11]
[null,"1,1-Dichlorethan","11DCA",null,{"$f":"IF($R$3,'Schadstoffkonzentration Boden'!Z38,'Schadstoffbelastung GW'!V19)","v":1.0457532E-10},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"11DCA",{"$f":"'Schadstoffbelastung GW'!Y19","v":1E-8},{"$f":"U15/Stoffdatenbank!R16","v":1.0105092966855296E-10},{"$f":"Stoffdatenbank!N16*1000*(Schadstoffbelastung!V15/Schadstoffbelastung!V$17)","v":3.3794642880367487E-5},{"$f":"U15/1000*Bodencharakterisierung!$E$9*Stoffdatenbank!J16","v":3.5740000000000007E-12},5.752217821782179E-11,5.3948178217821787E-11]
[null,"1,2-Dichlorethan","12DCA",null,{"$f":"IF($R$3,'Schadstoffkonzentration Boden'!Z39,'Schadstoffbelastung GW'!V20)","v":1.115928E-10},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12DCA",{"$f":"'Schadstoffbelastung GW'!Y20","v":1E-8},{"$f":"U16/Stoffdatenbank!R17","v":1.0105092966855296E-10},{"$f":"Stoffdatenbank!N17*1000*(Schadstoffbelastung!V16/Schadstoffbelastung!V$17)","v":3.3794642880367487E-5},{"$f":"U16/1000*Bodencharakterisierung!$E$9*Stoffdatenbank!J17","v":3.9600000000000009E-12},{"$f":"IFERROR(E16*1000/$K$12,0)","v":6.1382178217821796E-11},5.7422178217821798E-11]
[null,"LCKW",null,null,{"$f":"SUM(E4:E16)","v":87.288120001434933},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S LCKW",{"$f":"'Schadstoffbelastung GW'!Y21","v":2880.0000000809991},{"$f":"SUM(V4:V16)","v":25.984372195566642},{"$f":"SUM(W4:W16)","v":2165332.9955068654},4.1740000000612856,48.013267327521973,{"$f":"SUM(Z4:Z16)","v":43.839267327460682}]
[null,"Benzol","B","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"U18/Stoffdatenbank!R19","v":{"$error":"#VALUE!"}},{"$f":"Stoffdatenbank!N19*1000*(Schadstoffbelastung!V18/Schadstoffbelastung!V$35)","v":{"$error":"#VALUE!"}},{"$f":"(W18/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J19*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":{"$error":"#VALUE!"}},{"$f":"(E18/$K$12)*1000","v":0},{"$f":"IF(Y18<X18,0,Y18-X18)","v":{"$error":"#VALUE!"}}]
[null,"Toluol","T","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"U19/Stoffdatenbank!R20","v":{"$error":"#VALUE!"}},{"$f":"Stoffdatenbank!N20*1000*(Schadstoffbelastung!V19/Schadstoffbelastung!V$35)","v":{"$error":"#VALUE!"}},{"$f":"(W19/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J20*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"}]
[null,"Ethylbenzol","ETBE","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"U20/Stoffdatenbank!R21","v":{"$error":"#VALUE!"}},{"$f":"Stoffdatenbank!N21*1000*(Schadstoffbelastung!V20/Schadstoffbelastung!V$35)","v":{"$error":"#VALUE!"}},{"$f":"(W20/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J21*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"}]
[null,"o-Xylol","oX","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"U21/Stoffdatenbank!R22","v":{"$error":"#VALUE!"}},{"$f":"Stoffdatenbank!N22*1000*(Schadstoffbelastung!V21/Schadstoffbelastung!V$35)","v":{"$error":"#VALUE!"}},{"$f":"(W21/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J22*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"}]
[null,"m-Xylol","mX","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"U22/Stoffdatenbank!R23","v":{"$error":"#VALUE!"}},{"$f":"Stoffdatenbank!N23*1000*(Schadstoffbelastung!V22/Schadstoffbelastung!V$35)","v":{"$error":"#VALUE!"}},{"$f":"(W22/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J23*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"}]
[null,"p-Xylol","pX","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"U23/Stoffdatenbank!R24","v":{"$error":"#VALUE!"}},{"$f":"Stoffdatenbank!N24*1000*(Schadstoffbelastung!V23/Schadstoffbelastung!V$35)","v":{"$error":"#VALUE!"}},{"$f":"(W23/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J24*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"}]
[null,"n-Propylbenzol","nPB","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"U24/Stoffdatenbank!R25","v":{"$error":"#VALUE!"}},{"$f":"Stoffdatenbank!N25*1000*(Schadstoffbelastung!V24/Schadstoffbelastung!V$35)","v":{"$error":"#VALUE!"}},{"$f":"(W24/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J25*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"}]
[null,"Isopropylbenzol","iPB","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"U25/Stoffdatenbank!R26","v":{"$error":"#VALUE!"}},{"$f":"Stoffdatenbank!N26*1000*(Schadstoffbelastung!V25/Schadstoffbelastung!V$35)","v":{"$error":"#VALUE!"}},{"$f":"(W25/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J26*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"}]
[null,"o-Ethyltoluol","oET","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"U26/Stoffdatenbank!R27","v":{"$error":"#VALUE!"}},{"$f":"Stoffdatenbank!N27*1000*(Schadstoffbelastung!V26/Schadstoffbelastung!V$35)","v":{"$error":"#VALUE!"}},{"$f":"(W26/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J27*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"}]
[null,"m-Ethyltoluol","oET","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"U27/Stoffdatenbank!R28","v":{"$error":"#VALUE!"}},{"$f":"Stoffdatenbank!N28*1000*(Schadstoffbelastung!V27/Schadstoffbelastung!V$35)","v":{"$error":"#VALUE!"}},{"$f":"(W27/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J28*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"}]
[null,"p-Ethyltoluol","pET","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"U28/Stoffdatenbank!R29","v":{"$error":"#VALUE!"}},{"$f":"Stoffdatenbank!N29*1000*(Schadstoffbelastung!V28/Schadstoffbelastung!V$35)","v":{"$error":"#VALUE!"}},{"$f":"(W28/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J29*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"}]
[null,"1,2-Diethylbenzol","12DEB","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"U29/Stoffdatenbank!R30","v":{"$error":"#VALUE!"}},{"$f":"Stoffdatenbank!N30*1000*(Schadstoffbelastung!V29/Schadstoffbelastung!V$35)","v":{"$error":"#VALUE!"}},{"$f":"(W29/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J30*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"}]
[null,"1,3-Diethylbenzol","13DEB","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"U30/Stoffdatenbank!R31","v":{"$error":"#VALUE!"}},{"$f":"Stoffdatenbank!N31*1000*(Schadstoffbelastung!V30/Schadstoffbelastung!V$35)","v":{"$error":"#VALUE!"}},{"$f":"(W30/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J31*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"}]
[null,"1,4-Diethylbenzol","14DEB","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"U31/Stoffdatenbank!R32","v":{"$error":"#VALUE!"}},{"$f":"Stoffdatenbank!N32*1000*(Schadstoffbelastung!V31/Schadstoffbelastung!V$35)","v":{"$error":"#VALUE!"}},{"$f":"(W31/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J32*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"}]
[null,"1,2,3-Trimethylbenzol","123TMB","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"U32/Stoffdatenbank!R33","v":{"$error":"#VALUE!"}},{"$f":"Stoffdatenbank!N33*1000*(Schadstoffbelastung!V32/Schadstoffbelastung!V$35)","v":{"$error":"#VALUE!"}},{"$f":"(W32/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J33*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"}]
[null,"1,2,4-Trimethylbenzol","124TMB","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"U33/Stoffdatenbank!R34","v":{"$error":"#VALUE!"}},{"$f":"Stoffdatenbank!N34*1000*(Schadstoffbelastung!V33/Schadstoffbelastung!V$35)","v":{"$error":"#VALUE!"}},{"$f":"(W33/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J34*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"}]
[null,"1,3,5-Trimethylbenzol","135TMB","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"U34/Stoffdatenbank!R35","v":{"$error":"#VALUE!"}},{"$f":"Stoffdatenbank!N35*1000*(Schadstoffbelastung!V34/Schadstoffbelastung!V$35)","v":{"$error":"#VALUE!"}},{"$f":"(W34/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J35*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"}]
[null,"AKW",null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"SUM(V18:V34)","v":{"$error":"#VALUE!"}}]
[null,{"$f":"Stoffdatenbank!A37","v":"n-Pentan"},"nC5","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"U36/Stoffdatenbank!R37","v":2.7777777777777776E-2},{"$f":"Stoffdatenbank!N37*1000*(Schadstoffbelastung!V36/Schadstoffbelastung!V$42)","v":1693.6391253367933},{"$f":"(W36/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J37*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":23.169745372213733},0,0]
[null,{"$f":"Stoffdatenbank!A38","v":"n-Hexan"},"nC6","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,{"$f":"U37/Stoffdatenbank!R38","v":4.6511627906976744E-2},{"$f":"Stoffdatenbank!N38*1000*(Schadstoffbelastung!V37/Schadstoffbelastung!V$42)","v":708.96521525726234},{"$f":"(W37/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J38*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":22.265726102108815},0,0]
[null,{"$f":"Stoffdatenbank!A39","v":"n-Heptan"},"nC7","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,44,{"$f":"U38/Stoffdatenbank!R39","v":0.44},{"$f":"Stoffdatenbank!N39*1000*(Schadstoffbelastung!V38/Schadstoffbelastung!V$42)","v":1475.4984059934143},{"$f":"(W38/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J39*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":118.09512989477757},0,0]
[null,{"$f":"Stoffdatenbank!A40","v":"n-Octan"},"nC8","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,{"$f":"U39/Stoffdatenbank!R40","v":5.2631578947368418E-2},{"$f":"Stoffdatenbank!N40*1000*(Schadstoffbelastung!V39/Schadstoffbelastung!V$42)","v":56.157507840114732},{"$f":"(W39/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J40*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":14.814740862901754},0,0]
[null,{"$f":"Stoffdatenbank!A41","v":"n-Nonan"},"nC9","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,{"$f":"U40/Stoffdatenbank!R41","v":4.6875E-2},{"$f":"Stoffdatenbank!N41*1000*(Schadstoffbelastung!V40/Schadstoffbelastung!V$42)","v":8.5740480720175167},{"$f":"(W40/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J41*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":3.5816452464695452},0,0]
[null,{"$f":"Stoffdatenbank!A42","v":"n-Decan"},"nC10","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,{"$f":"U41/Stoffdatenbank!R42","v":4.2253521126760563E-2},{"$f":"Stoffdatenbank!N42*1000*(Schadstoffbelastung!V41/Schadstoffbelastung!V$42)","v":3.2202997453586915},{"$f":"(W41/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J42*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":10.675348239944745},0,0]
[null,{"$f":"Stoffdatenbank!A36","v":"n-Alkane"},null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,68,{"$f":"SUM(V36:V41)","v":0.65604950575888354}]
[null,"MTBE (Methyl-tert-butylether)",null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"U43/Stoffdatenbank!R44","v":5.6722784408041023E-2},{"$f":"Stoffdatenbank!N44*1000*(Schadstoffbelastung!V43/Schadstoffbelastung!V$46)","v":4778172.8713134844},{"$f":"(W43/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J44*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":3185.1300360175683},0,0]
[null,"ETBE (Ethyl-tert-butylether)",null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,{"$f":"U44/Stoffdatenbank!R45","v":0.53829319949733201},{"$f":"Stoffdatenbank!N45*1000*(Schadstoffbelastung!V44/Schadstoffbelastung!V$46)","v":10615350.215575002},{"$f":"(W44/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J45*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":6754.5473421703746},0,0]
[null,"TBA (tert-Butylalkohol) ",null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"U45/Stoffdatenbank!R46","v":1.3491343953719294E-2},null,{"$f":"(W45/(1000)*Bodencharakterisierung!$E$11*((Stoffdatenbank!J46*Bodencharakterisierung!$E$9)+Bodencharakterisierung!$E$8))","v":0},0,0]
[null,"Oxigenate",null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,61,{"$f":"SUM(V43:V45)","v":0.60850732785909234}]
[null,"DOC"]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null," Berechnung der Schadstoffinventare mit Daten aus "]

{"sheet":"Schadstoffkonzentration Boden","index":2,"n_rows":93,"n_cols":29,"rows_kept":93,"cut":false,"hidden":true,"merged":[[74,0,74,20],[75,26,76,26],[94,27,95,27],[94,28,95,28],[75,28,76,28],[75,21,92,21],[22,22,24,22],[22,23,24,23],[22,24,24,24],[22,25,24,25],[0,0,0,21],[20,0,20,21],[40,0,40,20],[60,0,60,20],[65,0,65,20],[22,21,23,21],[1,0,18,1],[25,0,25,21],[75,29,77,29],[75,22,76,22],[75,23,76,23],[75,24,76,24],[75,25,76,25],[75,27,76,27]]}
[]
["Die Grafiken enthalten größensortierte Daten aus dem unteren Teil des Eingabeblattes (gemessenen Konzentrationen) und dienen ausschließlich der Visualisierung der Werteverteilung"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Mittlere Schadstoffmasse im gesättigten Boden (Einheitsfläche) (MB) [mg/m²]                             "]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Summe \n[kg]"," Mittlere Flächen-Konz. (MB) [mg/m²]"," Standard-abweich. (MB) [mg/m²]","MB + 2 s  [mg/m²]"," Inventar \n(MB-bezogen) [kg]"]
["Sondierung (Bezeichnung)"]
["Flächenrepräsentanz [m²]",5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,50,60,{"$f":"IF(SUM(B25:U25)=Schadstoffbelastung!$K$6,SUM(B25:U25),\"Σ ≠ \"&Schadstoffbelastung!$K$6&\"!\")","v":200}]
["Leichtflüchtige chlorierte Kohlenwasserstoffe (LCKW) ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"kg"]
["Tetrachlorethen",900000,900000,900000,900000,900000,900000,900000,900000,900000,900000,900000,900000,900000,900000,900000,900000,900000,900000,900000,900000,{"$f":"SUMPRODUCT($B$25:$U$25,B27:U27)*10^-6","v":180},{"$f":"IFERROR(AVERAGE($B27:$U27),0)","v":900000},{"$f":"IF(SUM($B27:$U27)>0,_xlfn.STDEV.S(B27:U27),\"\")","v":0},{"$f":"IF(SUM($B27:$U27)>0,W27+X27*2,\"\")","v":900000},{"$f":"IFERROR(Y27*$V$25/1000/1000,0)","v":180}]
["Trichlorethen",null,null,null,null,null,null,null,null,null,null,900000,900000,900000,900000,900000,900000,900000,900000,null,null,{"$f":"SUMPRODUCT($B$25:$U$25,B28:U28)*10^-6","v":36},{"$f":"IFERROR(AVERAGE($B28:$U28),0)","v":900000},{"$f":"IF(SUM($B28:$U28)>0,_xlfn.STDEV.S(B28:U28),\"\")","v":0},{"$f":"IF(SUM($B28:$U28)>0,W28+X28*2,\"\")","v":900000},{"$f":"IFERROR(Y28*$V$25/1000/1000,0)","v":180}]
["cis-1,2-Dichlorethen",null,null,null,null,null,null,null,null,null,null,900000,900000,900000,900000,900000,900000,900000,900000,null,null,36,900000,{"$f":"IF(SUM($B29:$U29)>0,_xlfn.STDEV.S(B29:U29),\"\")","v":0},900000,180]
["trans-1,2-Dichlorethen",null,null,null,null,null,null,null,null,null,null,900000,900000,900000,900000,900000,900000,900000,900000,null,null,36,900000,0,900000,180]
["1,1-Dichlorethen",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"","",0]
["Vinylchlorid",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"","",0]
["Tetrachlormethan",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"","",0]
["Trichlormethan",null,null,null,null,null,null,null,null,null,null,900000,900000,900000,900000,900000,900000,900000,900000,null,null,36,900000,0,900000,180]
["Dichlormethan",null,null,null,null,null,null,null,null,null,null,900000,900000,900000,900000,900000,900000,900000,900000,null,null,36,900000,0,900000,180]
["1,1,1-Trichlorethan",null,null,null,null,null,null,null,null,null,null,900000,900000,900000,900000,900000,900000,900000,900000,null,null,36,900000,0,900000,180]
["1,1,2-Trichlorethan",null,null,null,null,null,null,null,null,null,null,900000,900000,900000,900000,900000,900000,900000,900000,null,null,36,900000,0,900000,180]
["1,1-Dichlorethan",null,null,null,null,null,null,null,null,null,null,900000,900000,900000,900000,900000,900000,900000,900000,null,null,36,900000,0,900000,180]
["1,2-Dichlorethan",null,null,null,null,null,null,null,null,null,null,900000,900000,900000,900000,900000,900000,900000,900000,null,null,36,900000,0,900000,180]
["LCKW",{"$f":"IF(SUM(B27:B39)>0,SUM(B27:B39),\"\")","v":900000},{"$f":"IF(SUM(C27:C39)>0,SUM(C27:C39),\"\")","v":900000},900000,900000,900000,900000,900000,900000,900000,900000,9000000,9000000,9000000,9000000,9000000,9000000,9000000,9000000,900000,900000,{"$f":"SUM(V27:V39)","v":504},4140000,4071259.9885952803,{"$f":"IF(SUM($B40:$U40)>0,W40+X40*2,\"\")","v":12282519.977190562},{"$f":"SUM(Z27:Z39)","v":1800}]
["(Mono)aromatische Kohlenwasserstoffe (AKW) "]
["Benzol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(B42*B$25/$V$25+C42*C$25/$V$25+D42*D$25/$V$25+E42*E$25/$V$25+F42*F$25/$V$25+G42*G$25/$V$25+H42*H$25/$V$25+I42*I$25/$V$25+J42*J$25/$V$25+K42*K$25/$V$25+L42*L$25/$V$25+M42*M$25/$V$25+N42*N$25/$V$25+O42*O$25/$V$25+P42*P$25/$V$25+Q42*Q$25/$V$25+R42*R$25/$V$25+S42*S$25/$V$25+T42*T$25/$V$25+U42*U$25/$V$25)*$V$25/1000/1000","v":0},{"$f":"IF(SUM($B42:$U42)>0,AVERAGE($B42:$U42),\"\")","v":""},{"$f":"IF(SUM($B42:$U42)>0,_xlfn.STDEV.S(B42:U42),\"\")","v":""},{"$f":"IF(SUM($B42:$U42)>0,W42+X42*2,\"\")","v":""},{"$f":"Y42*$V$25/1000/1000","v":{"$error":"#VALUE!"}}]
["Toluol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","",{"$error":"#VALUE!"}]
["Ethylbenzol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","",{"$error":"#VALUE!"}]
["o-Xylol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","",{"$error":"#VALUE!"}]
["m-Xylol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","",{"$error":"#VALUE!"}]
["p-Xylol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","",{"$error":"#VALUE!"}]
["n-Propylbenzol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","",{"$error":"#VALUE!"}]
["Isopropylbenzol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","",{"$error":"#VALUE!"}]
["o-Ethyltoluol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","",{"$error":"#VALUE!"}]
["m-Ethyltoluol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","",{"$error":"#VALUE!"}]
["p-Ethyltoluol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","",{"$error":"#VALUE!"}]
["1,2-Diethylbenzol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","",{"$error":"#VALUE!"}]
["1,3-Diethylbenzol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","",{"$error":"#VALUE!"}]
["1,4-Diethylbenzol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","",{"$error":"#VALUE!"}]
["1,2,3-Trimethylbenzol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","",{"$error":"#VALUE!"}]
["1,2,4-Trimethylbenzol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","",{"$error":"#VALUE!"}]
["1,3,5-Trimethylbenzol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","",{"$error":"#VALUE!"}]
["BTEX",{"$f":"IF(SUM(B42:B47)>0,SUM(B42:B47),\"\")","v":""},{"$f":"IF(SUM(C42:C47)>0,SUM(C42:C47),\"\")","v":""},"","","","","","","","","","","","","","","","","","",{"$f":"SUM(V42:V47)","v":0},"","","",{"$f":"SUM(Z42:Z47)","v":{"$error":"#VALUE!"}}]
["AKW",{"$f":"IF(SUM(B42:B58)>0,SUM(B42:B58),\"\")","v":""},{"$f":"IF(SUM(C42:C58)>0,SUM(C42:C58),\"\")","v":""},"","","","","","","","","","","","","","","","","","",{"$f":"SUM(V42:V58)","v":0},"","","",{"$f":"SUM(Z42:Z58)","v":{"$error":"#VALUE!"}}]
["Oxigenate"]
[" MTBE (Methyl-tert-butylether)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(B62*B$25/$V$25+C62*C$25/$V$25+D62*D$25/$V$25+E62*E$25/$V$25+F62*F$25/$V$25+G62*G$25/$V$25+H62*H$25/$V$25+I62*I$25/$V$25+J62*J$25/$V$25+K62*K$25/$V$25+L62*L$25/$V$25+M62*M$25/$V$25+N62*N$25/$V$25+O62*O$25/$V$25+P62*P$25/$V$25+Q62*Q$25/$V$25+R62*R$25/$V$25+S62*S$25/$V$25+T62*T$25/$V$25+U62*U$25/$V$25)*$V$25/1000/1000","v":0},{"$f":"IF(SUM($B62:$U62)>0,AVERAGE($B62:$U62),\"\")","v":""},{"$f":"IF(SUM($B62:$U62)>0,_xlfn.STDEV.S(B62:U62),\"\")","v":""},{"$f":"IF(SUM($B62:$U62)>0,W62+X62*2,\"\")","v":""},{"$f":"Y62*$V$25/1000/1000","v":{"$error":"#VALUE!"}}]
[" ETBE (Ethyl-tert-butylether)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(B63*B$25/$V$25+C63*C$25/$V$25+D63*D$25/$V$25+E63*E$25/$V$25+F63*F$25/$V$25+G63*G$25/$V$25+H63*H$25/$V$25+I63*I$25/$V$25+J63*J$25/$V$25+K63*K$25/$V$25+L63*L$25/$V$25+M63*M$25/$V$25+N63*N$25/$V$25+O63*O$25/$V$25+P63*P$25/$V$25+Q63*Q$25/$V$25+R63*R$25/$V$25+S63*S$25/$V$25+T63*T$25/$V$25+U63*U$25/$V$25)*$V$25/1000/1000","v":0},{"$f":"IF(SUM($B63:$U63)>0,AVERAGE($B63:$U63),\"\")","v":""},{"$f":"IF(SUM($B63:$U63)>0,_xlfn.STDEV.S(B63:U63),\"\")","v":""},{"$f":"IF(SUM($B63:$U63)>0,W63+X63*2,\"\")","v":""},{"$f":"Y63*$V$25/1000/1000","v":{"$error":"#VALUE!"}}]
[" TBA (tert-Butylalkohol) ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(B64*B$25/$V$25+C64*C$25/$V$25+D64*D$25/$V$25+E64*E$25/$V$25+F64*F$25/$V$25+G64*G$25/$V$25+H64*H$25/$V$25+I64*I$25/$V$25+J64*J$25/$V$25+K64*K$25/$V$25+L64*L$25/$V$25+M64*M$25/$V$25+N64*N$25/$V$25+O64*O$25/$V$25+P64*P$25/$V$25+Q64*Q$25/$V$25+R64*R$25/$V$25+S64*S$25/$V$25+T64*T$25/$V$25+U64*U$25/$V$25)*$V$25/1000/1000","v":0},{"$f":"IF(SUM($B64:$U64)>0,AVERAGE($B64:$U64),\"\")","v":""},{"$f":"IF(SUM($B64:$U64)>0,_xlfn.STDEV.S(B64:U64),\"\")","v":""},{"$f":"IF(SUM($B64:$U64)>0,W64+X64*2,\"\")","v":""},{"$f":"Y64*$V$25/1000/1000","v":{"$error":"#VALUE!"}}]
[" Oxigenate ",{"$f":"IF(SUM(B62:B64)>0,SUM(B62:B64),\"\")","v":""},{"$f":"IF(SUM(C62:C64)>0,SUM(C62:C64),\"\")","v":""},"","","","","","","","","","","","","","","","","","",{"$f":"SUM(V62:V64)","v":0},{"$f":"IF(SUM($B65:$U65)>0,AVERAGE($B65:$U65),\"\")","v":""},{"$f":"IF(SUM($B65:$U65)>0,_xlfn.STDEV.S(B65:U65),\"\")","v":""},{"$f":"IF(SUM($B65:$U65)>0,W65+X65*2,\"\")","v":""},{"$f":"SUM(Z62:Z64)","v":{"$error":"#VALUE!"}}]
["n-Alkane "]
["n-Pentan",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(B67*B$25/$V$25+C67*C$25/$V$25+D67*D$25/$V$25+E67*E$25/$V$25+F67*F$25/$V$25+G67*G$25/$V$25+H67*H$25/$V$25+I67*I$25/$V$25+J67*J$25/$V$25+K67*K$25/$V$25+L67*L$25/$V$25+M67*M$25/$V$25+N67*N$25/$V$25+O67*O$25/$V$25+P67*P$25/$V$25+Q67*Q$25/$V$25+R67*R$25/$V$25+S67*S$25/$V$25+T67*T$25/$V$25+U67*U$25/$V$25)*$V$25/1000/1000","v":0},{"$f":"IF(SUM($B67:$U67)>0,AVERAGE($B67:$U67),\"\")","v":""},{"$f":"IF(SUM($B67:$U67)>0,_xlfn.STDEV.S(B67:U67),\"\")","v":""},{"$f":"IF(SUM($B67:$U67)>0,W67+X67*2,\"\")","v":""},{"$f":"Y67*$V$25/1000/1000","v":{"$error":"#VALUE!"}}]
["n-Hexan",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","",{"$error":"#VALUE!"}]
["n-Heptan",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","",{"$error":"#VALUE!"}]
["n-Octan",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","",{"$f":"Y70*$V$25/1000/1000","v":{"$error":"#VALUE!"}}]
["n-Nonan",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","",{"$error":"#VALUE!"}]
["n-Decan",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","",{"$error":"#VALUE!"}]
["n-Alkane ",{"$f":"IF(SUM(B67:B72)>0,SUM(B67:B72),\"\")","v":""},{"$f":"IF(SUM(C67:C72)>0,SUM(C67:C72),\"\")","v":""},"","","","","","","","","","","","","","","","","","",{"$f":"SUM(V67:V71)","v":0},"","","",{"$f":"SUM(Z67:Z72)","v":{"$error":"#VALUE!"}}]
[]
["Analysierte Schadstoffkonzentrationen im gesättigten Boden  [mg/kg]                             "]
["Probe",1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,null," Minimum [mg/kg OS]"," Maximum [mg/kg OS]"," Median [mg/kg OS]"," Mittlere Konz. (MW) [mg/kg OS]"," Standard-abweich.  [mg/kg OS]","MW + 2 s  [mg/kg OS]"," Inventar \n(Mittelwert-bezogen) [kg]"]
["Bezeichnung"]
[]
["Leichtflüchtige chlorierte Kohlenwasserstoffe (LCKW) "]
["Tetrachlorethen",1000,1000,1000,1000,1000,1000,null,null,null,1000,1000,1000,1000,null,null,null,null,null,null,null,null,{"$f":"MIN(B80:U80)","v":1000},{"$f":"MAX($B80:$U80)","v":1000},{"$f":"IFERROR(MEDIAN($B80:$U80),\"\")","v":1000},{"$f":"IF(SUM($B80:$U80)>0,AVERAGE($B80:$U80),\"\")","v":1000},{"$f":"IF(SUM($B80:$U80)>0,_xlfn.STDEV.S(B80:U80),\"\")","v":0},{"$f":"IF(SUM($B80:$U80)>0,Z80+AA80*2,\"\")","v":1000},{"$f":"IFERROR(AB80*Tonnage/1000,0)","v":1817.9999999999998}]
["Trichlorethen",65.400000000000006,410,2.8,3.2,1.3,0.9,null,null,null,2,3,4,5,null,null,null,null,null,null,null,null,0.9,410,3.1,{"$f":"IF(SUM($B81:$U81)>0,AVERAGE($B81:$U81),\"\")","v":49.76},{"$f":"IF(SUM($B81:$U81)>0,_xlfn.STDEV.S(B81:U81),\"\")","v":128.10202704615307},{"$f":"IF(SUM($B81:$U81)>0,Z81+AA81*2,\"\")","v":305.96405409230613},556.24265033981249]
["cis-1,2-Dichlorethen",25.2,810,350,1.2,0,1.1000000000000001,null,null,null,2,3,4,5,null,null,null,null,null,null,null,null,0,810,3.5,120.15,265.60862289382766,651.36724578765529,1184.1856528419573]
["trans-1,2-Dichlorethen",0,1.5,0,0,0,0,null,null,null,2,3,4,5,null,null,null,null,null,null,null,null,0,5,0.75,1.55,1.8922355972646629,5.3344711945293257,9.6980686316543121]
["1,1-Dichlorethen",5.4,74,22,0,0,0,null,null,null,2,3,4,5,null,null,null,null,null,null,null,null,0,74,3.5,11.540000000000001,22.879986402482359,57.299972804964717,104.17135055942585]
["Vinylchlorid",0,31,0,0,0,0,null,null,null,2,3,4,5,null,null,null,null,null,null,null,null,0,31,1,4.5,9.5014618758261502,23.5029237516523,42.728315380503872]
["Tetrachlormethan",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"","","","",0]
["Trichlormethan",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"","","","",0]
["Dichlormethan",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"","","","",0]
["1,1,1-Trichlorethan",null,null,null,0,0,0,null,null,null,2,3,4,5,null,null,null,null,null,null,null,null,0,5,2,2,2.0816659994661326,6.1633319989322652,11.204937574058857]
["1,1,2-Trichlorethan",null,null,null,null,null,null,null,null,null,2,3,4,5,null,null,null,null,null,null,null,null,2,5,3.5,3.5,1.2909944487358056,6.0819888974716108,11.057055815603388]
["1,1-Dichlorethan",null,null,null,0,1.2,0,null,null,null,2,3,4,5,null,null,null,null,null,null,null,null,0,5,2,2.1714285714285713,1.9336617126704503,6.0387519967694718,10.978451130126897]
["1,2-Dichlorethan",0,110,37,0,0,0,null,null,null,2,3,4,5,null,null,null,null,null,null,null,null,0,110,2.5,16.100000000000001,34.850314839961555,85.800629679923105,155.98554475810019]
["LCKW",{"$f":"IF(SUM(B80:B92)>0,SUM(B80:B92),\"\")","v":1096.0000000000002},{"$f":"IF(SUM(C80:C92)>0,SUM(C80:C92),\"\")","v":2436.5},1411.8,1004.4000000000001,1002.5,1002,"","","",1018,1027,1036,1045,"","","","","","","",null,1002,2436.5,1031.5,1207.92,449.00183568048379,2105.9236713609675,{"$f":"AB93*Tonnage/1000","v":3828.5692345342386}]

{"sheet":"Tabelle1","index":3,"n_rows":7,"n_cols":21,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
[]
[]
[]
[]
[]
[null,{"$f":"'Schadstoffkonzentration Boden'!B93","v":1096.0000000000002},{"$f":"'Schadstoffkonzentration Boden'!C93","v":2436.5},{"$f":"'Schadstoffkonzentration Boden'!D93","v":1411.8},{"$f":"'Schadstoffkonzentration Boden'!E93","v":1004.4000000000001},{"$f":"'Schadstoffkonzentration Boden'!F93","v":1002.5},{"$f":"'Schadstoffkonzentration Boden'!G93","v":1002},{"$f":"'Schadstoffkonzentration Boden'!H93","v":""},{"$f":"'Schadstoffkonzentration Boden'!I93","v":""},{"$f":"'Schadstoffkonzentration Boden'!J93","v":""},{"$f":"'Schadstoffkonzentration Boden'!K93","v":1018},{"$f":"'Schadstoffkonzentration Boden'!L93","v":1027},{"$f":"'Schadstoffkonzentration Boden'!M93","v":1036},{"$f":"'Schadstoffkonzentration Boden'!N93","v":1045},{"$f":"'Schadstoffkonzentration Boden'!O93","v":""},{"$f":"'Schadstoffkonzentration Boden'!P93","v":""},{"$f":"'Schadstoffkonzentration Boden'!Q93","v":""},{"$f":"'Schadstoffkonzentration Boden'!R93","v":""},{"$f":"'Schadstoffkonzentration Boden'!S93","v":""},{"$f":"'Schadstoffkonzentration Boden'!T93","v":""},{"$f":"'Schadstoffkonzentration Boden'!U93","v":""}]
[null,{"$f":"_xlfn.RANK.EQ(B6,$B6:$U6)","v":3},{"$f":"_xlfn.RANK.EQ(C6,$B6:$U6)","v":1},2,8,9,10,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},7,6,5,4,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(SUM(S6)>0,_xlfn.RANK.EQ(S6,$B6:$U6),\"\")","v":""},{"$f":"IF(SUM(T6)>0,_xlfn.RANK.EQ(T6,$B6:$U6),\"\")","v":""},{"$f":"IF(SUM(U6)>0,_xlfn.RANK.EQ(U6,$B6:$U6),\"\")","v":""}]

{"sheet":"Schadstoffbelastung GW","index":4,"n_rows":57,"n_cols":27,"rows_kept":57,"cut":false,"hidden":true,"merged":[[49,0,49,20],[4,22,5,22],[4,23,5,23],[41,0,41,20],[4,25,5,25],[4,24,5,24],[6,0,6,20],[21,0,21,20],[4,21,6,21],[1,8,1,9],[4,30,5,30],[4,31,5,31],[4,27,5,27],[4,29,5,29],[4,28,5,28],[2,8,2,9],[4,26,5,26]]}
[]
[]
["Schadstoffkonzentrationen im Grundwasser (gelöst) [µg/L]",null,null,null,null,null,null,null,"Korrekturfaktor",null,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Fläche*Mächtigkeit*Pges/1000/1000","v":3.9600000000000003E-4},{"$f":"Fläche*Mächtigkeit*Bodencharakterisierung!E11*Bodencharakterisierung!E9/1000/1000","v":1.8179999999999999E-5}]
[]
["Messstelle Nr.",1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,"Summe",null,null," Mittlere Konz. (MW) [µg/L]"," Inventar  (gelöst) [kg]"," Inventar (sorbiert) [kg]"]
["Bezeichnung","A"]
["Leichtflüchtige chlorierte Kohlenwasserstoffe (LCKW) ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"kg"]
["Tetrachlorethen",700,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SUM(B8:U8)>0,(Z8+AA8)*KorFak,\"\")","v":48.585599999999999},null,null,{"$f":"IFERROR(AVERAGE($B8:$U8),0)","v":700},{"$f":"$Z$3*Y8","v":0.2772},{"$f":"$AA$3*Y8*Stoffdatenbank!J5","v":4.5813600000000001}]
["Trichlorethen",680,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.763919999999999,null,null,{"$f":"IFERROR(AVERAGE($B9:$U9),0)","v":680},{"$f":"$Z$3*Y9","v":0.26928000000000002},{"$f":"$AA$3*Y9*Stoffdatenbank!J6","v":1.6071119999999999}]
["cis-1,2-Dichlorethen",1300,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16.965,null,null,1300,0.51480000000000004,{"$f":"$AA$3*Y10*Stoffdatenbank!J7","v":1.1817}]
["trans-1,2-Dichlorethen",1E-8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.4868E-10,null,null,1E-8,3.9600000000000001E-12,{"$f":"$AA$3*Y11*Stoffdatenbank!J8","v":1.0908E-11}]
["1,1-Dichlorethen",1E-8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.6778718000000002E-10,null,null,1E-8,3.9600000000000001E-12,{"$f":"$AA$3*Y12*Stoffdatenbank!J9","v":1.2818718000000001E-11}]
["Vinylchlorid",200,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.9736000000000002,null,null,200,7.9200000000000007E-2,{"$f":"$AA$3*Y13*Stoffdatenbank!J10","v":0.21815999999999999}]
["Tetrachlormethan",1E-8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.5882079999999999E-10,null,null,1E-8,3.9600000000000001E-12,{"$f":"$AA$3*Y14*Stoffdatenbank!J11","v":5.1922080000000005E-11}]
["Trichlormethan",1E-8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.3269977999999999E-10,null,null,1E-8,3.9600000000000001E-12,{"$f":"$AA$3*Y15*Stoffdatenbank!J12","v":9.3099779999999999E-12}]
["Dichlormethan",1E-8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6.1688699999999995E-11,null,null,1E-8,3.9600000000000001E-12,{"$f":"$AA$3*Y16*Stoffdatenbank!J13","v":2.2088699999999997E-12}]
["1,1,1-Trichlorethan",1.0000000000000001E-9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.0139200000000002E-11,null,null,1.0000000000000001E-9,3.9600000000000008E-13,{"$f":"$AA$3*Y17*Stoffdatenbank!J14","v":2.6179200000000002E-12}]
["1,1,2-Trichlorethan",1E-8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1893752E-10,null,null,1E-8,3.9600000000000001E-12,{"$f":"$AA$3*Y18*Stoffdatenbank!J15","v":7.9337519999999997E-12}]
["1,1-Dichlorethan",1E-8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.0457532E-10,null,null,1E-8,3.9600000000000001E-12,{"$f":"$AA$3*Y19*Stoffdatenbank!J16","v":6.4975320000000004E-12}]
["1,2-Dichlorethan",1E-8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.115928E-10,null,null,1E-8,3.9600000000000001E-12,{"$f":"$AA$3*Y20*Stoffdatenbank!J17","v":7.1992799999999996E-12}]
["   LCKW",{"$f":"IF(SUM(B8:B20)>0,SUM(B8:B20),\"\")","v":2880.0000000809991},{"$f":"IF(SUM(C8:C20)>0,SUM(C8:C20),\"\")","v":""},"","","","","","","","","","","","","","","","","","",{"$f":"SUM(V8:V20)","v":87.288120001434933},null,null,2880.0000000809991]
["(Mono)aromatische Kohlenwasserstoffe (AKW) "]
["Benzol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SUM(B23:U23)>0,(Z23+AA23)*$K$3,\"\")","v":""},null,{"$f":"V23","v":""}]
["Toluol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SUM(B24:U24)>0,(Z24+AA24)*$K$3,\"\")","v":""},null,""]
["Ethylbenzol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,""]
["o-Xylol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,""]
["m-Xylol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,""]
["p-Xylol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,""]
["n-Propylbenzol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,""]
["Isopropylbenzol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,""]
["o-Ethyltoluol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,""]
["m-Ethyltoluol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,""]
["p-Ethyltoluol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,""]
["1,2-Diethylbenzol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,""]
["1,3-Diethylbenzol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,""]
["1,4-Diethylbenzol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,""]
["1,2,3-Trimethylbenzol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,""]
["1,2,4-Trimethylbenzol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,""]
["1,3,5-Trimethylbenzol",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,""]
["BTEX",{"$f":"IF(SUM(B23:B28)>0,SUM(B23:B28),\"\")","v":""},{"$f":"IF(SUM(C23:C28)>0,SUM(C23:C28),\"\")","v":""},"","","","","","","","","","","","","","","","","","",{"$f":"SUM(V23:V28)","v":0}]
["AKW",{"$f":"IF(SUM(B23:B39)>0,SUM(B23:B39),\"\")","v":""},{"$f":"IF(SUM(C23:C39)>0,SUM(C23:C39),\"\")","v":""},"","","","","","","","","","","","","","","","","","",{"$f":"SUM(V23:V39)","v":0}]
["n-Alkane "]
["n-Pentan",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SUM(B43:U43)>0,(Z43+AA43)*$K$3,\"\")","v":""},null,{"$f":"V43","v":""}]
["n-Hexan",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,""]
["n-Heptan",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,""]
["n-Octan",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,""]
["n-Nonan",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,""]
["n-Decan",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,""]
["n-Alkane ",{"$f":"IF(SUM(B43:B48)>0,SUM(B43:B48),\"\")","v":""},{"$f":"IF(SUM(C43:C48)>0,SUM(C43:C48),\"\")","v":""},"","","","",{"$f":"IF(SUM(H43:H48)>0,SUM(H43:H48),\"\")","v":""},"","","","","","","","","","","",{"$f":"IF(SUM(T43:T48)>0,SUM(T43:T48),\"\")","v":""},"",{"$f":"SUM(V43:V48)","v":0}]
["Oxigenate"]
[" MTBE (Methyl-tert-butylether)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SUM(B51:U51)>0,(Z51+AA51)*$K$3,\"\")","v":""},null,{"$f":"V51","v":""}]
[" ETBE (Ethyl-tert-butylether)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SUM(B52:U52)>0,(Z52+AA52)*$K$3,\"\")","v":""},null,{"$f":"V52","v":""}]
[" TBA (tert-Butylalkohol) ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SUM(B53:U53)>0,(Z53+AA53)*$K$3,\"\")","v":""},null,{"$f":"V53","v":""}]
[" Oxigenate",{"$f":"IF(SUM(B51:B53)>0,SUM(B51:B53),\"\")","v":""},"","","","","","","","","","","","","","","","","",{"$f":"IF(SUM(T51:T53)>0,SUM(T51:T53),\"\")","v":""},{"$f":"IF(SUM(U51:U53)>0,SUM(U51:U53),\"\")","v":""},{"$f":"SUM(V51:V53)","v":0}]
[]
["[mg/m²]"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"[mg/m²]"]

{"sheet":"Bodencharakterisierung","index":5,"n_rows":18,"n_cols":19,"rows_kept":18,"cut":false,"hidden":true,"merged":[[0,0,0,20],[1,14,1,18],[1,1,2,1],[1,0,2,0],[1,3,2,3],[1,12,2,12],[1,11,2,11],[1,13,2,13]]}
[]
[null,"Parameter",null,"Einheit","Hauptbodenart","Nebenbodenart",null,null,null,null,null,null,"Parameter","Einheit","Datenbank"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Grobsand","Mittelsand","Feinsand","Schluff","Ton"]
[null,"Relativer Anteil (geschätzt)",null,"%",97,{"$f":"100-E4","v":3},null,null,{"$f":"O3","v":"Grobsand"},null,null,null,"Parameter","Einheit","Grobsand","Mittelsand","Feinsand","Schluff","Ton"]
[null,"Wassersättigung (ungesättigter Boden)","SW","-",0.26,0.26,null,null,{"$f":"P3","v":"Mittelsand"},null,null,null,"Wassersättigung (ungesättigter Boden)","-",0.26,0.26,0.26,0.27,0.28999999999999998]
[null,"Durchlässigkeitsbeiwert","kf","m/s",2.7500000000000002E-4,2.7500000000000002E-4,null,{"$f":"F6/E6","v":1},{"$f":"Q3","v":"Feinsand"},null,null,null,"Durchlässigkeitsbeiwert (kf)","m/s",2.0000000000000001E-4,2.7500000000000002E-4,1.0000000000000001E-5,9.9999999999999995E-8,9.9999999999999994E-12]
[null,"Nutzbare Porosität ","neff","-",0.125,0.125,null,null,{"$f":"R3","v":"Schluff"},null,null,null,"Nutzbare Porosität (neff)","-",0.2,0.125,0.1,7.4999999999999997E-2,3.5000000000000003E-2]
[null,"Gesamtporosität (Hohlraumvolumen)","n","-",0.33,0.33,null,null,{"$f":"S3","v":"Ton"},null,null,null,"Gesamtporosität (Hohlraumvolumen)","-",0.33,0.33,0.33,0.34,0.35]
[null,"Organische Kohlenstoffgehalt ","fOC","-",0.01,0.01,null,null,null,null,null,null,"Organische Kohlenstoffgehalt ","-",0.01,0.01,0.01,0.01,0.01]
[null,"Korndichte","ρs","kg/m³",2650,2650,null,null,null,null,null,null,"Korndichte","kg/m³",2650,2650,2650,2690,2700]
[null,"Schüttdichte","d","kg/L",1.5149999999999999,1.5149999999999999,null,null,null,null,null,null,"Schüttdichte","kg/dm³",1.5149999999999999,1.5149999999999999,1.5149999999999999,1.43,1.64]
[null,"Bodendichte (Materialdichte)","nM","kg/m³",1015.0499999999997,1015.0499999999997,null,null,null,null,null,null,"Anteil (Bodenkorn)","kg/m³",{"$f":"1000*(1-O8)*O11","v":1015.0499999999997},{"$f":"1000*(1-P8)*P11","v":1015.0499999999997},{"$f":"1000*(1-Q8)*Q11","v":1015.0499999999997},{"$f":"1000*(1-R8)*R11","v":943.79999999999984},{"$f":"1000*(1-S8)*S11","v":1066}]
[null,"Mittlerer Kornradius ","d50","m",4.15E-4,4.15E-4,null,null,null,null,null,null,"Mittlerer Kornradius (d50)","m",1.315E-3,4.15E-4,1.315E-4,3.2499999999999997E-5,1.9999999999999999E-6]
[null,"Tortouistät in der Wasserphase ","tw","-",8,8,null,null,null,null,null,null,"Tortuoistät in der Wasserphase (τw)","-",{"$f":"1/O7","v":5},{"$f":"1/P7","v":8},{"$f":"1/Q7","v":10},{"$f":"1/R7","v":13.333333333333334},{"$f":"1/S7","v":28.571428571428569}]
[null,"Wärmeleitfähigkeit ","l","W/(m·K)",3.34,3.34,null,null,null,null,null,null,"Wärmeleitfähigkeit (λ)","W/(m·K)",3.72,3.34,2.75,1.5,1.5]
[null,"Temperaturleitfähigkeit","a","m²/s",1.3359999999999999E-3,1.3359999999999999E-3,null,null,null,null,null,null,"Temperaturleitfähigkeit (α)","m²/s",{"$f":"O15/O18","v":1.4880000000000002E-3},{"$f":"P15/P18","v":1.3359999999999999E-3},{"$f":"Q15/Q18","v":1.1000000000000001E-3},{"$f":"R15/R18","v":6.2500000000000001E-4},{"$f":"S15/S18","v":6.2500000000000001E-4}]
[null,"Untergrundtemperatur ","T0","K",283.14999999999998,283.14999999999998,null,null,null,null,null,null,"Untergrundtemperatur (T0)","K",283.14999999999998,283.14999999999998,283.14999999999998,283.14999999999998,283.14999999999998]
[null,"Spezifische Wärmekapazität (Bodenkorn)","cM","kJ/(kg·K)",2500,2500,null,null,null,null,null,null,"Spezifische Wärmekapazität ","kJ/(kg·K)",2500,2500,2500,2400,2400]

{"sheet":"Grundwassercharakterisierung","index":6,"n_rows":15,"n_cols":9,"rows_kept":15,"cut":false,"hidden":true,"merged":[[4,0,4,3]]}
[]
[null,"Parameter","Einheit","Wert"]
[null,"Mittlerer hydraulischer Gradient (I)","%",0.1]
[null,"Grundwasserabstandsgeschwindigkeit (va)","m/d",{"$f":"Bodencharakterisierung!E6*(Grundwassercharakterisierung!D3/100)/Bodencharakterisierung!E7*3600*24","v":0.19008}]
["   Redoxmilieu (charakteristische Mittelwerte)"]
[null,"pH-Wert","--",7,null,null,null,null,7]
[null,"Redoxspannung (korr.)","mV",200,null,null,null,null,200]
[null,"Temperatur","°C",3,null,null,null,null,3]
[null,"Gelöster Sauerstoff","mg/L",20,null,null,null,null,20]
[null,"Nitrat","mg/L",0,null,null,null,null,0]
[null,"Mangan (gelöst)","mg/L",0,null,null,null,null,0]
[null,"Eisen (gelöst)","mg/L",200,null,null,null,null,200]
[null,"Sulfat","mg/L",0,null,null,null,null,0]
[null,"Methan","mg/L",2,null,null,null,null,2]
[null,"DOC","mg/L",2,null,null,null,null,2]

{"sheet":"Heterogenität","index":7,"n_rows":6,"n_cols":7,"rows_kept":6,"cut":false,"hidden":true,"merged":[[2,0,2,1],[3,0,3,1]]}
[]
[]
["Heterogenität (Gini-Koeffizient)",null,"Hoch",0.7]
["Korrekturfaktor",null,null,{"$f":"1/(1-(1-2.45068336614863*(Schadstoffbelastung!$K$4*Schadstoffbelastung!$K$5)^-0.457209937280527)*$D$3)","v":2.2115534486107022}]
[]
[null,null,null,null,null,"Sondierung","Gini-Koeffizient"]

{"sheet":"Stoffdatenbank","index":8,"n_rows":47,"n_cols":23,"rows_kept":47,"cut":false,"hidden":true,"merged":[[3,0,3,18],[17,0,17,18],[35,0,35,18],[42,0,42,18]]}
[]
[null,"Abbaurate (Permang.)","Abbaurate (Sufat-Radikal)","Abbaurate (ERD)","Abbaurate (O2)","Abbaurate (Nitrat)","Abbaurate (Sulfat)"," Ver-dampfungs-enthalpie","Gemisch-siedetemp. mit Wasser","Sorptions-koeffizient","Henry-Koeffizient","Diffusions-koeffizient (in Wasser)","Diffusions-koeffizient (in Luft)","Löslichkeit","Dampf-druck","Siede-punkt","Dichte ","Molekular-gewicht"]
["Verbindung","lPM \n[mol-1 s-1]","lPM \n[mol-1 s-1]","lERD \n[d-1]","lOx \n[d-1]","lNO3 \n[d-1]","lSO4 \n[d-1]"," ΔHv \n[kJ/kg]","\n°C","KOC \n[L/kg]","H (15°C) \n[-]","Dw (15°C) \n[m²/s]","Da (15°C) \n[m²/s]","Lw (20°C) \n[mg/L]","Po (15°C) \n[Pa]","\n°C","\n[kg/L]","Mm \n[g/mol]","Bemerkung"]
["Leichtflüchtige chlorierte Kohlenwasserstoffe (LCKW)"]
["Tetrachlorethen",3.7999999999999999E-2,null,2.8000000000000001E-2,"--","--","--",239.22,88.7,{"$f":"0.36*1000","v":360},0.64,7.49E-10,6.6200000000000001E-6,160,1479,121.075,1.6240000000000001,166,null,null,null,null,2.8000000000000001E-2]
["Trichlorethen",0.67,null,2.7E-2,"--","--","--",263.14999999999998,73.5,130,0.33,8.08E-10,7.1199999999999996E-6,1000,6064,86.974999999999994,1.4641999999999999,131,null,null,null,null,2.7E-2]
["cis-1,2-Dichlorethen",null,null,1.2E-2,"--","--","--",319.07,55.3,50,0.2,8.9500000000000001E-10,7.8800000000000008E-6,3500,17284,60.1875,1.2837000000000001,97,"Lw (cDCE) bei 25 °C",null,null,null,1.2E-2]
["trans-1,2-Dichlorethen",43.6,null,1.2E-2,"--","--","--",306.55,45.3,60,0.19,8.8600000000000004E-10,8.8300000000000002E-6,6300,29294,48.066000000000003,1.2565,97,null,null,null,null,1.2E-2]
["1,1-Dichlorethen",2.3199999999999998,null,1.2E-2,"--","--","--",274.33,{"$f":"I7","v":55.3},70.510000000000005,0.8,1.173E-9,9.8649999999999996E-6,2500,6792.77,31.4,1.218,97,null,null,null,null,1.2E-2]
["Vinylchlorid",null,null,1.7999999999999999E-2,0.03,2E-3,2E-3,364.6,-13,60,6.78,5.7799999999999997E-10,5.9399999999999999E-6,1100,285916,-13.757999999999999,0.91210000000000002,63,null,null,null,null,1.7999999999999999E-2]
["Tetrachlormethan",null,null,0.06,"--","--","--",201.95,66,285.60000000000002,1.153,7.2929999999999995E-10,6.3230000000000003E-6,800,11940,76.760000000000005,1.5940000000000001,154,null,null,null,null,0.06]
["Trichlormethan",null,null,0.06,"--","--","--",273.11,56.1,51.21,0.185,8.245E-10,7.1409999999999999E-6,8200,20900,61.12,1.4850000000000001,119,null,null,null,null,0.06]
["Dichlormethan",null,null,0.03,"--","--","--",343.36,43.5,12.149999999999999,0.1159,9.8300000000000002E-10,8.4409999999999993E-6,17799,39156.78,39.950000000000003,1.3280000000000001,85,null,null,null,null,0.03]
["1,1,1-Trichlorethan",null,null,0.01,"--","--","--",243.62,86,144,1,7.6099999999999996E-10,6.7700000000000004E-6,1300,1369.81,74.05,1.339,133.404,null,null,null,null,0.01]
["1,1,2-Trichlorethan",null,null,0.01,"--","--","--",301.33999999999997,86,43.64,3.7999999999999999E-2,6.8000000000000003E-10,7.6000000000000001E-6,4500,2500,13.65,1.4410000000000001,133.404,"D abgeschätzt",null,null,null,0.01]
["1,1-Dichlorethan",null,null,6.5000000000000006E-3,"--","--","--",310.27999999999997,72.8,35.74,0.25700000000000001,1.14E-9,8.6999999999999997E-6,8690,29100,57.4,1.2350000000000001,98.96,"D abgeschätzt",null,null,null,6.5000000000000006E-3]
["1,2-Dichlorethan",null,null,6.5000000000000006E-3,"--","--","--",354.69,72.844999999999999,39.6,5.0799999999999998E-2,9.2000000000000003E-10,7.8299999999999996E-6,8690,10000,83.6,1.25,98.96,null,null,null,null,6.5000000000000006E-3]
["(Mono)aromatische Kohlenwasserstoffe (AKW)"]
["Benzol",6.9999999999999999E-6,1680000000,"--",0.15,1.5E-3,0.01,434.62,69.3,80,0.15,8.1499999999999998E-10,7.5900000000000002E-6,1770,7941,80.150000000000006,0.877,78]
["Toluol",5.6999999999999998E-4,1870000000,"--",0.23,0.5,0.05,390.22,84.6,300,0.16,7.3400000000000005E-10,6.9E-6,520,2215,110.7,0.87,92]
["Ethylbenzol",7.0699999999999999E-3,1000000000,"--",0.15,0.25,3.0000000000000001E-3,386.76,91.5,1100,0.19,6.7600000000000004E-10,6.3899999999999998E-6,170,728,136.19999999999999,0.86599999999999999,106]
["o-Xylol",1.47E-3,null,"--",7.0000000000000007E-2,2.5000000000000001E-2,0.04,396.23,93.3,830,0.12,6.8000000000000003E-10,6.4200000000000004E-6,180,492,143.9,0.88,106]
["m-Xylol",1E-3,null,"--",0.1,0.1,0.08,386.79,93.3,980,0.16,6.7099999999999996E-10,6.3600000000000001E-6,174,615,139.19999999999999,0.86399999999999999,106]
["p-Xylol",2.2200000000000002E-3,2700000000,"--",0.1,0.05,0.04,396.23,93.3,880,0.15,6.7099999999999996E-10,6.3600000000000001E-6,200,657,138.30000000000001,0.86099999999999999,106]
["n-Propylbenzol",null,null,"--",0.1,0.02,3.0000000000000001E-3,383.33,96.5,980,0.2,6.2000000000000003E-10,6.0000000000000002E-6,60,237,158.9,0.86,120,"LW bei 25 °C"]
["Isopropylbenzol",null,null,"--",0.15,0.02,0.02,366.67,95,940,0.43,6.2000000000000003E-10,6.0000000000000002E-6,50,427,151.9,0.86199999999999999,120,"LW bei 25 °C"]
["o-Ethyltoluol",null,null,"--",0.05,0.02,0.04,395.25,96.5,790,0.11,6.3E-10,6.0000000000000002E-6,93,202,165.2,0.88,120]
["m-Ethyltoluol",null,null,"--",0.15,0.1,0.08,390,96.5,760,0.1,6.2000000000000003E-10,6.0000000000000002E-6,97,202,161.4,0.86399999999999999,120]
["p-Ethyltoluol",null,null,"--",0.15,0.05,0.04,388.92,96.5,900,0.12,6.2000000000000003E-10,6.0000000000000002E-6,95,230,162,0.86099999999999999,120]
["1,2-Diethylbenzol",null,null,"--",7.0000000000000007E-2,1.4999999999999999E-2,0.04,394.03,96.5,500,0.16,5.9000000000000003E-10,5.6999999999999996E-6,24,67,182.9,0.88,134]
["1,3-Diethylbenzol",null,null,"--",7.0000000000000007E-2,0.05,0.08,391.79,96.5,420,0.23,5.7999999999999996E-10,5.5999999999999997E-6,27,109,180.9,0.86,134]
["1,4-Diethylbenzol",null,null,"--",7.0000000000000007E-2,0.03,0.04,391.79,96.5,460,0.23,5.7999999999999996E-10,5.5999999999999997E-6,25,101,183.7,0.86199999999999999,134]
["1,2,3-Trimethylbenzol",null,null,"--",0.12,3.0000000000000001E-3,0.03,408.33,96.5,650,0.08,6.3999999999999996E-10,6.0000000000000002E-6,75,125,176.1,0.89400000000000002,120]
["1,2,4-Trimethylbenzol",null,null,"--",0.17,3.0000000000000001E-3,0.05,391.67,96.5,650,0.12,6.3E-10,6.0000000000000002E-6,60,147,169.3,0.876,120,"LW bei 25 °C"]
["1,3,5-Trimethylbenzol",null,null,"--",0.05,3.0000000000000001E-3,0.05,395.92,96.5,670,0.48,6.3E-10,6.0000000000000002E-6,20,193,164.7,0.86499999999999999,120]
["n-Alkane"]
["n-Pentan",null,125000000,"--",0.06,0.01,5.0000000000000001E-3,368.06,34.6,870,35.69,7.0099999999999996E-10,6.8900000000000001E-6,40,46219,36.049999999999997,0.626,72]
["n-Hexan",null,160000000,"--",0.11,0.01,5.0000000000000001E-3,360.47,61.6,2040,46.48,6.4900000000000003E-10,6.3600000000000001E-6,10,12922,68.75,0.66,86]
["n-Heptan",null,247000000,"--",0.15,0.01,5.0000000000000001E-3,360,79.599999999999994,5250,69.3,6.0499999999999998E-10,5.9200000000000001E-6,2.2000000000000002,3645,98.35,0.68400000000000005,100,"LW bei 25 °C"]
["n-Octan",null,337000000,"--",0.19,0.01,5.0000000000000001E-3,359.65,89.5,17380,70.89,5.69E-10,5.5799999999999999E-6,0.7,1041,125.6,0.70250000000000001,114]
["n-Nonan",null,null,"--",0.22,0.01,5.0000000000000001E-3,363.28,94.8,27540,156.63,5.4099999999999999E-10,5.31E-6,0.12,351,150.69999999999999,0.72,128,"LW bei 25 °C"]
["n-Decan",null,null,"--",0.22,0.01,5.0000000000000001E-3,361.27,97.2,218780,140.30000000000001,5.1299999999999999E-10,5.0499999999999999E-6,0.05,118,174.1,0.73,142]
["Oxigenate"]
["MTBE (Methyl-tert-butylether)",null,31000000,"--",7.0000000000000007E-2,3.0000000000000001E-3,2E-3,340.34,52.4,11,2.7E-2,9.5130000000000001E-10,8.2859999999999999E-6,51259,33300,55.65,0.74,88.147999999999996]
["ETBE (Ethyl-tert-butylether)",null,null,"--",7.0000000000000007E-2,3.0000000000000001E-3,2E-3,323.37,65.2,9,8.1000000000000003E-2,7.3379629629629627E-10,6.9444444444444439E-6,12000,16500,72.825000000000003,0.75,102.1748]
["TBA (tert-Butylalkohol) ",null,740000,"--",7.0000000000000007E-2,1E-3,2E-3,620.6,79.900000000000006,37,6.0999999999999997E-4,6.9999999999999996E-10,{"$f":"M44/(L44/L46)","v":6.0971302428256071E-6},"mischbar",5430,82.35,0.79,74.121600000000001]
["grau = abgeschätzt"]

{"sheet":"Sanierungsdesign","index":9,"n_rows":23,"n_cols":22,"rows_kept":23,"cut":false,"hidden":true,"merged":[[1,14,2,15],[5,0,5,4],[2,0,2,4],[1,11,2,12],[0,0,0,19]]}
[]
[null,"Parameter",null,"Einheit","Wert",null,null,null,null,null,null,"Stöchiometrische Faktoren Bedarf an Wasserstoff",null,null,"Stöchiometrische Faktoren Generierung von Wasserstoff",null,null,null,"Substratauswahl",null,"Anzeigewert","Schadstoff"]
["Sanierungszielwert",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Acetat",null,"Summe LCKW",{"$f":"tblSchadstoffauswahl[[#This Row],[Anzeigewert]]","v":"Summe LCKW"}]
[null,"Sanierungszielwert ",null,"µg/L",200,null,null,null,null,null,null,"Elektronenakzeptor (EA)","g/g EA",null,"Elektronendonator (ED)","ED g/g Wasserstoff",null,null,"Biomasse",null,"Tetrachlorethen",{"$f":"tblSchadstoffauswahl[[#This Row],[Anzeigewert]]","v":"Tetrachlorethen"}]
[null,"Unproduktiver Wasserstoffbedarf des Bodens",null,"g/kg",5.0000000000000001E-3,null,null,null,null,null,null,null,null,null,"Wasserstoff",1,null,null,"Ethanol",null,"Trichlorethen",{"$f":"tblSchadstoffauswahl[[#This Row],[Anzeigewert]]","v":"Trichlorethen"}]
["Design ",null,null,null,null,null,null,null,null,null,null,null,null,null,"Acetat",30.05,null,null,"Glucose",null,"cis-1,2-Dichlorethen",{"$f":"tblSchadstoffauswahl[[#This Row],[Anzeigewert]]","v":"cis-1,2-Dichlorethen"}]
[null,"Sanierungsfläche",null,"m²",{"$f":"Schadstoffbelastung!K6","v":200},null,null,null,null,null,null,null,null,null,"Ethanol",23.05,null,null,"Laktat",null,"trans-1,2-Dichlorethen",{"$f":"tblSchadstoffauswahl[[#This Row],[Anzeigewert]]","v":"trans-1,2-Dichlorethen"}]
[null,"Anzahl der Injektionsbrunnen",null,"-",5,null,null,null,null,null,null,null,null,null,"Laktat",45.05,null,null,"Palmöl",null,"1,1-Dichlorethen",{"$f":"tblSchadstoffauswahl[[#This Row],[Anzeigewert]]","v":"1,1-Dichlorethen"}]
[null,"Radius Injektionsbrunnen inkl. Filterkies ",null,"m ",0.2,null,null,null,null,null,null,null,null,null,"Glucose",90.1,null,null,"Rapsöl",null,"Vinylchlorid",{"$f":"tblSchadstoffauswahl[[#This Row],[Anzeigewert]]","v":"Vinylchlorid"}]
[null,"maximaler Injektionsdruck",null,"Bar",0.2,null,null,null,null,null,null,null,null,null,"Sojaöl",436.55,null,null,"Sojaöl",null,"Tetrachlormethan",{"$f":"tblSchadstoffauswahl[[#This Row],[Anzeigewert]]","v":"Tetrachlormethan"}]
[null,"Elektonendonator (H2)",null,"mg/L",100,null,null,null,null,null,null,"Tetrachlorethen",4.8192771084337345E-2,null,"Palmöl",424.25,null,null,"Wasserstoff",null,"Trichlormethan",{"$f":"tblSchadstoffauswahl[[#This Row],[Anzeigewert]]","v":"Trichlormethan"}]
[null,null,null,null,null,null,null,null,null,null,null,"Trichlorethen",4.5801526717557252E-2,null,"Rapsöl",442.3,null,null,"Andere",null,"Dichlormethan",{"$f":"tblSchadstoffauswahl[[#This Row],[Anzeigewert]]","v":"Dichlormethan"}]
[null,"Betrachteter Schadstoff (zur Auswahl in Zelle clicken)",null,null,"Summe LCKW",null,null,null,null,null,null,"cis-1,2-Dichlorethen",4.1237113402061855E-2,null,"Biomasse",56.55,null,null,null,null,"1,1,1-Trichlorethan",{"$f":"tblSchadstoffauswahl[[#This Row],[Anzeigewert]]","v":"1,1,1-Trichlorethan"}]
[null,null,null,null,null,null,null,null,null,null,null,"t-1,2-Dichlorethen",4.1237113402061855E-2,null,"Andere",0,null,null,null,null,"1,1,2-Trichlorethan",{"$f":"tblSchadstoffauswahl[[#This Row],[Anzeigewert]]","v":"1,1,2-Trichlorethan"}]
[null,null,null,null,null,null,null,null,null,null,null,"1,1-Dichlorethen",4.1237113402061855E-2,null,null,null,null,null,null,null,"1,1-Dichlorethan",{"$f":"tblSchadstoffauswahl[[#This Row],[Anzeigewert]]","v":"1,1-Dichlorethan"}]
[null,"Substrat (zur Auswahl in Zelle clicken)",null,null,"Glucose",null,null,null,null,null,null,"Vinylchlorid",3.1746031746031744E-2,null,null,null,null,null,null,null,"1,2-Dichlorethan",{"$f":"tblSchadstoffauswahl[[#This Row],[Anzeigewert]]","v":"1,2-Dichlorethan"}]
[null,null,null,null,null,null,null,null,null,null,null,"Tetrachlormethan",5.1948051948051951E-2,null,null,null,null,null,null,null,"bewertungsrelevanter Schadstoff",{"$f":"OFFSET(Calculation!$B$49,MATCH(MAX(Calculation!$O$49:$O$62),Calculation!$O$49:$O$62,0)-1,0)","v":"Tetrachlorethen"}]
[null,null,null,null,null,null,null,null,null,null,null,"Trichlormethan",5.0420168067226892E-2]
[null,null,null,null,null,null,null,null,null,null,null,"Dichlormethan",4.7058823529411764E-2]
[null,null,null,null,null,null,null,null,null,null,null,"1,1,1-Trichlorethan",4.4976162633804086E-2]
[null,null,null,null,null,null,null,null,null,null,null,"1,1,2-Trichlorethan",4.4976162633804086E-2]
[null,null,null,null,null,null,null,null,null,null,null,"1,1-Dichlorethan",4.0420371867421187E-2]
[null,null,null,null,null,null,null,null,null,null,null,"1,2-Dichlorethan",4.0420371867421187E-2]

{"sheet":"Calculation","index":10,"n_rows":5017,"n_cols":60,"rows_kept":1125,"cut":true,"hidden":true,"merged":[[14,0,15,0],[14,1,15,1],[14,2,15,2],[14,3,15,3],[28,1,28,3],[14,42,15,42],[14,43,15,43],[14,44,15,44],[14,30,15,30],[14,31,15,31],[14,39,15,39],[14,40,15,40],[14,41,15,41],[45,22,46,22],[45,23,46,23],[30,2,30,3],[31,2,31,3],[45,2,46,2],[45,17,46,17],[45,15,46,15],[45,14,46,14],[45,9,46,9],[45,10,46,10],[45,11,46,11],[45,13,46,13],[45,16,46,16],[14,25,15,25],[14,27,15,27],[14,28,15,28],[14,29,15,29],[14,35,15,35],[17,10,17,15],[80,2,81,2],[14,32,15,32],[67,2,68,2],[67,3,68,3],[67,4,68,4],[80,3,81,3],[80,4,81,4],[80,5,81,5],[80,6,81,6],[45,8,46,8],[45,3,46,3],[45,4,46,4],[45,5,46,5],[45,6,46,6],[45,7,46,7]],"bounds":{"rows_first":500,"rows_last":125,"rows_between":500,"halvings":2}}
[null,"Ergebnisparameter","Einheit","Wert",null,"Sanierungsdauer (d)",{"$f":"COUNT(AT18:AT5017)","v":3374},null,"Eingabeparameter"]
[null,null,null,null,null,"Sanierungsdauer (a)",{"$f":"G1/365.25","v":9.2375085557837107},null,"Reynoldzahl Re'",{"$f":"(Bodencharakterisierung!$E$13*Bodencharakterisierung!$E$6*(IF((Grundwassercharakterisierung!$D$3<0.1),0.1/100,Grundwassercharakterisierung!$D$3/100))/(1.3*10^-6*Bodencharakterisierung!$E$7))","v":7.023076923076924E-4}]
[null,"Dauer der ERD-Sanierung","Tage",{"$f":"G1","v":3374},null,"Auflösung der Residualphase (d)",{"$f":"COUNT(AH18:AH150)","v":133},null,"Diffusionskoeffizient Wasser Daq [m²/s]",{"$f":"VLOOKUP(C30,B44:X62,17,FALSE)","v":7.8838296947049937E-10}]
[null,"Min. erforderliche Substratmenge (LCKW-Abbau)","kg",{"$f":"VLOOKUP($C$30,B83:G96,6,FALSE)","v":359.93855383518786},null,"Desorptionsprozess (d)",{"$f":"G1-G3","v":3241},null,"foc",{"$f":"Bodencharakterisierung!E9","v":0.01}]
[null,"End-Schadstoffkonzentration ","µg/L",{"$f":"(MIN(AX18:AX5017))","v":199.57993256231023},null,"Sanierungsziel kg/m3 Wasser",{"$f":"Sanierungsdesign!E4*10^-6","v":1.9999999999999998E-4},null,"Kd [m³ Wasser/ kg Boden]",{"$f":"$D$24/1000","v":2.0601874130798813E-3}]
[null,null,null,null,null,"Sanierungsziel ug/L",{"$f":"G5*10^6","v":199.99999999999997},null,"λ_Schadstoff [d-1]",{"$f":"$D$25","v":2.2812314698908428E-2}]
[null,"Injektionsvolumen pro Pegel","m3",{"$f":"$G$8","v":30},null,"V(Pegel) (-> Volumen um einen Pegel) [m3 Boden]",{"$f":"Schadstoffbelastung!$K$11/Sanierungsdesign!E8","v":240}]
[null,"Injektionsradius (ROI)","m",{"$f":"$G$9","v":3.5682482323055424},null,"V(Inj) (-> Volumen einer Injektion) [m3 Wasser]",{"$f":"G7*Bodencharakterisierung!$E$7","v":30},null,"Cw (aktuelle Konz.) [kg/m³ Wasser]",{"$f":"$D$18/1000000","v":2.8800000000809988E-3}]
[null,"Dauer eines Injektionszyklus","h",{"$f":"(G8/G18)/3600","v":3.4138042220062674},null,"r(ROI) (-> Radius der Injektion um eine Bohrung) [m]",{"$f":"SQRT(G7/PI()/Schadstoffbelastung!$K$9)","v":3.5682482323055424},null,"Cs (Grenzkonzentration)[kg/kg]",{"$f":"$D$20/1000000","v":4.1740000000612839E-6}]
[null,"Injektionsrate  ","L/s",{"$f":"G18*1000","v":2.4410694906329149},null,"c(inj) (-> Injektionskonz. nach diff. Ausgleich) [kg H2/m3 Wasser]",{"$f":"Sanierungsdesign!$E$11*0.001*(Bodencharakterisierung!$E$7/Bodencharakterisierung!$E$8)","v":3.787878787878788E-2},null,"Cs (Grenzkonzentration) [kg/m3 Boden]",{"$f":"J9*Bodencharakterisierung!$E$11*1000","v":6.3236100000928445E-3}]
[null,"Anzahl Injektionen Nebenreaktanten","Anzahl",{"$f":"G21","v":3.36},null,"maßgeblicher stöchiometrischer Faktor [kgH2/Kg Schadstoff)",{"$f":"$D$28","v":4.3820906330865619E-2},null,"λsw [1/d]",{"$f":"(10^(0.301-0.668*LOG(J5*1000)))*24","v":29.615668923869613},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Abbau im GW",{"$f":"Z17-$Z$17*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3915996627248484E-4},null," [kg/m3 Wasser]"]
[null,"Anzahl Injektionen Schadstoffaustrag","Anzahl",{"$f":"$G$22","v":22.803875992319128},null,"c(gesamtboden;inj) [kg H2/m3 Boden/Injektion]",{"$f":"G10*Bodencharakterisierung!E8","v":1.2500000000000001E-2},null,"c(i) (Sättigungskonz) [kg/m3 Wasser]",{"$f":"VLOOKUP($C$30,$B$49:$X$62,21,FALSE)","v":2.1653329955068661}]
[null,"Anzahl der Gesamtinjektionen","Anzahl",{"$f":"$G$23","v":26.163875992319127},null,"r(0) (-> Radius Injektionsbohrungen) [m]",{"$f":"Sanierungsdesign!$E$9","v":0.2},null,"C(w, Gleichgewicht [kg/m3 Wasser]",{"$f":"VLOOKUP($C$30,$B$49:$X$62,23,FALSE)","v":2.3305291073371062E-2}]
[null,"Min. Substratmenge zur Redoxmilieubildung","kg",{"$f":"(G19+G33)*Schadstoffbelastung!K11*E66","v":908.20799999999997},null,"s (-> Aufhöhung der Wassersäule in Bohrung) [m]",{"$f":"Sanierungsdesign!$E$10*10","v":2},null,"C(w, Berechnung) [kg/m3]",{"$f":"IF(MAX(J13,J8)>J12,J12,MAX(J13,J8))","v":2.3305291073371062E-2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"$J$9*0.05","v":2.087000000030642E-7},null,null,null,null,null,null,"Desorption "]
[null,null,null,null,null,"H (-> Mächtigkeit Grundwasserleiter) [m]",{"$f":"Schadstoffbelastung!$K$9","v":6},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C(w) [kg/m3 Wasser]","Abbau","Volumetrischer Schadstoffanteil θ [m³/m³]","Transferrate J [kg/m3 Wasser*d ]","Zunahme im Wasser dC [kg/m3 Wasser]"," Residualphase C(Res,neu) [kg/m3 Boden]","Residualphase C(Res,neu) [kg/kg Boden]","Wasser C(w,Res,neu) [kg/m3 Wasser]",null,null,"Verbrauch ED [kg H2/m3 Boden]",null,null,null,"Wasser C(w) [kg/m3 Wasser]","Transferrate J [kg/m3 Wasser d]","Zunahme im Wasser dC [kg/m3]","sorbierte Phase C(s,neu-desorp.) [kg/m3 Boden]","sorbierte Phase C(s,neu-desorp.) [kg/kg Boden]","Wasser C(w,neu-desorp.) [kg/m3 Wasser]","Daten für Grafik",null,null,null,null,null,"Daten für Grafik",null,null,null,null,"Daten für Grafik",null,"Daten für Grafik","Daten für Grafik"]
[null,null,null,null,null,"T (-> Transmissivität Grundwasserleiter) [m2/s]",{"$f":"Bodencharakterisierung!$E$6*$G$15","v":1.65E-3},null,"C Residual [kg/kg]",{"$f":"$D$21/1000000","v":4.3839267327460676E-5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tage",null,null,null,null,null,null,null,null,"Tage",null,null,"Injektionen",null,"Tage",null,null,null,null,null,null,"Tage",null,"Verbrauch ED [kg/m3 Boden]","Injektionen","Ausgabe","Tage gesamt","Injektionen gesamt","Injektionen Residual Anzahl","Injektionen Desorption Anzahl","Injektionen zustromender gelöster Stoffe Anzahl",null,"Cboden [mg/kg]","Cboden_sorb [mg/kg]","Cboden_res [mg/kg]","cwasser [µg/L]"]
[null,null,null,null,null,"S (-> Speicherkoeffizient [-]",{"$f":"G15*3.3*10^-6","v":1.9799999999999997E-5},null,"C Residual [kg/m3 Boden]",{"$f":"J16*1000*Bodencharakterisierung!E11","v":6.6416490001102918E-2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"$J$14","v":2.3305291073371062E-2},{"$f":"Z17*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"$J$16*Bodencharakterisierung!$E$11/$J$20","v":4.587723557222869E-5},{"$f":"((150*($J$2^0.87)*(AB17^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z17)*3600*24","v":8.5745592556699085E-2},{"$f":"MIN(AC17,Z17-AA17)","v":2.3915996627248484E-4},{"$f":"$J$17-(AD17*Bodencharakterisierung!$E$8)","v":6.6337567212232995E-2},{"$f":"IF(AE17>$J$18,(AE17/(Bodencharakterisierung!$E$11*1000)),0)","v":4.3787173077381514E-5},{"$f":"AA17+AD17","v":2.3305291073371062E-2},null,null,null,0,null,0,{"$f":"J14","v":2.3305291073371062E-2},null,null,null,null,null,0,null,null,0,null,null,{"$f":"D11","v":3.36},null,null,null,null,{"$f":"J19*10^6","v":4.3827000000643475},{"$f":"MAX(#REF!)*10^6","v":{"$error":"#REF!"}},{"$f":"D21","v":43.839267327460675},{"$f":"AN17*10^6","v":23305.291073371063}]
[null,"Mittlere Konzentration Grundwasser","µg/L",{"$f":"VLOOKUP($C$30,$B$49:$X$62,3,FALSE)*1000000","v":2880.0000000809987},null,"Q(mittel) (-> mittlerer Durchfluss Injektion) [m3/s]",{"$f":"(((G15+G14)^2)-(G15^2))/2*(4*PI()*Bodencharakterisierung!E6/LN(2.25*G16*3600*24/G17/G13^2))","v":2.4410694906329151E-3},null,"C Sorption neu [kg/m3 Boden]",{"$f":"J19*Bodencharakterisierung!$E$11*1000","v":6.6397905000974864E-3},{"$f":"IF(G1>365*5,\"Achtung - Sanierungslaufzeit überschreitet einen Zeitraum von 5 Jahren\",\"\")","v":"Achtung - Sanierungslaufzeit überschreitet einen Zeitraum von 5 Jahren"},null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"AG17","v":2.3305291073371062E-2},{"$f":"Z18*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF17*Bodencharakterisierung!$E$11/$J$20","v":4.5822719602219693E-5},{"$f":"((150*($J$2^0.87)*(AB18^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z18)*3600*24","v":8.5665088157969055E-2},{"$f":"MIN(AC18,Z18-AA18)","v":2.3915996627248484E-4},{"$f":"AE17-AD18*Bodencharakterisierung!$E$8","v":6.6258644423363072E-2},{"$f":"IF(AE18>$J$18,(AE18/(Bodencharakterisierung!$E$11*1000)),0)","v":4.3735078827302359E-5},{"$f":"AA18+AD18","v":2.3305291073371062E-2},{"$f":"IF(AD18>0,Y18,NA())","v":1},null,{"$f":"AD18*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH18>0,(AJ18*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AK17,NA())","v":1.3833872553757791E-3},null,1,{"$f":"IF(AF18<=$J$9*0.05,AN17*EXP((-$J$6*1)/Heterogenität!$D$4),Z18)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF18>=$J$19, J19/$J$5<AN18),0, Bodencharakterisierung!$E$8*$J$11*((J19/$J$5)-AN18))","v":0},{"$f":"MIN(AO18,$AN$17-AN18)","v":0},{"$f":"J18-AP18*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ18/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},{"$f":"AN18+AP18","v":2.3305291073371062E-2},{"$f":"IF(AN18>$G$5,AM18,NA())","v":1},null,{"$f":"(AP18)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF18<=$J$9*1.05,(AV18*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW17,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH18>($G$5*10^6),BH18*0.99,9999)","v":23072.238162637354},{"$f":"AT18+$G$3","v":134},{"$f":"IF(ISNUMBER(AT18),BA18+BB18+BC18+$AZ$17,\"\")","v":3.3676560272553755},{"$f":"IF(ISNUMBER(AK18),AK18,BA17)","v":1.3833872553757791E-3},{"$f":"IF(ISNUMBER(AW18),AW18,0)","v":0},{"$f":"$G$34/$G$12/$G$8","v":6.2726400000000003E-3},null,{"$f":"AR18*10^6","v":4.3827000000643475},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF18*10^6","v":43.73507882730236},23305.291073371063]
[null,"Mittlere Konzentration Boden"," mg/kg",{"$f":"VLOOKUP($C$30,$B$49:$X$62,19,FALSE)*1000000","v":48.01326732752198},null,"Masse unprod. ED-Bedarf im Boden [kg H2/m3 Boden]",{"$f":"Sanierungsdesign!E5*Bodencharakterisierung!$E$11","v":7.5749999999999993E-3},null,"C Sorption neu [kg/kg]",{"$f":"MIN(D19,D20*1.05)*10^-6","v":4.3827000000643478E-6},null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"AG18","v":2.3305291073371062E-2},{"$f":"Z19*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF18*Bodencharakterisierung!$E$11/$J$20","v":4.5768203632210702E-5},{"$f":"((150*($J$2^0.87)*(AB19^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z19)*3600*24","v":8.5584563643492567E-2},{"$f":"MIN(AC19,Z19-AA19)","v":2.3915996627248484E-4},{"$f":"AE18-AD19*Bodencharakterisierung!$E$8","v":6.6179721634493149E-2},{"$f":"IF(AE19>$J$18,(AE19/(Bodencharakterisierung!$E$11*1000)),0)","v":4.3682984577223204E-5},{"$f":"AA19+AD19","v":2.3305291073371062E-2},{"$f":"IF(AD19>0,Y19,NA())","v":2},null,{"$f":"(AD19)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH19>0,(AJ19*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK18,NA())","v":3.5508545107515582E-3},null,2,{"$f":"IF(AF19<=$J$9*0.05,AS18*EXP((-$J$6*1)/Heterogenität!$D$4),Z19)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF19>=$J$19, AR18/$J$5<AN19),0, Bodencharakterisierung!$E$8*$J$11*((AR18/$J$5)-AN19))","v":0},{"$f":"MIN(AO19,AS18-AN19)","v":0},{"$f":"AQ18-AP19*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ19/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},{"$f":"AN19+AP19","v":2.3305291073371062E-2},2,null,{"$f":"(AP19)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF19<=$J$9*1.05,(AV19*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW18,NA())","v":{"$error":"#N/A"}},23072.238162637354,135,{"$f":"IF(ISNUMBER(AT19),BA19+BB19+BC19+$AZ$17,\"\")","v":3.3760961345107514},{"$f":"IF(ISNUMBER(AK19),AK19,BA18)","v":3.5508545107515582E-3},{"$f":"IF(ISNUMBER(AW19),AW19,0)","v":0},{"$f":"$G$34/$G$12/$G$8+BC18","v":1.2545280000000001E-2},null,{"$f":"AR19*10^6","v":4.3827000000643475},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},43.682984577223202,23305.291073371063]
[null,"Grenzkonzentration Boden"," mg/kg",{"$f":"VLOOKUP($C$30,$B$49:$X$62,18,FALSE)*1000000","v":4.1740000000612838},null,null,null,null,"Dichte Schadstoff [kg/L]",{"$f":"$D$27","v":1.4477003501341623},null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,{"$f":"AG19","v":2.3305291073371062E-2},{"$f":"Z20*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF19*Bodencharakterisierung!$E$11/$J$20","v":4.5713687662201705E-5},{"$f":"((150*($J$2^0.87)*(AB20^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z20)*3600*24","v":8.5504018984273622E-2},2.3915996627248484E-4,{"$f":"AE19-AD20*Bodencharakterisierung!$E$8","v":6.6100798845623226E-2},{"$f":"IF(AE20>$J$18,(AE20/(Bodencharakterisierung!$E$11*1000)),0)","v":4.3630890327144042E-5},2.3305291073371062E-2,3,null,{"$f":"(AD20)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH20>0,(AJ20*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK19,NA())","v":5.7183217661273371E-3},null,3,{"$f":"IF(AF20<=$J$9*0.05,AS19*EXP((-$J$6*1)/Heterogenität!$D$4),Z20)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF20>=$J$19, AR19/$J$5<AN20),0, Bodencharakterisierung!$E$8*$J$11*((AR19/$J$5)-AN20))","v":0},{"$f":"MIN(AO20,AS19-AN20)","v":0},{"$f":"AQ19-AP20*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ20/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},{"$f":"AN20+AP20","v":2.3305291073371062E-2},3,null,{"$f":"(AP20)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF20<=$J$9*1.05,(AV20*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW19,NA())","v":{"$error":"#N/A"}},23072.238162637354,136,3.3845362417661273,5.7183217661273371E-3,0,{"$f":"$G$34/$G$12/$G$8+BC19","v":1.8817920000000002E-2},null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},43.630890327144044,23305.291073371063]
[null,"Konzentration Residualphase"," mg/kg",{"$f":"VLOOKUP($C$30,$B$49:$X$62,20,FALSE)*1000000","v":43.839267327460675},null,"Anzahl Injektionen für unprod. ED-Bedarf",{"$f":"($G$19+$G$33)*Schadstoffbelastung!$K$11/($G$12*Calculation!$G$7)","v":3.36},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,2.3305291073371062E-2,{"$f":"Z21*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF20*Bodencharakterisierung!$E$11/$J$20","v":4.5659171692192708E-5},{"$f":"((150*($J$2^0.87)*(AB21^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z21)*3600*24","v":8.542345415124003E-2},2.3915996627248484E-4,{"$f":"AE20-AD21*Bodencharakterisierung!$E$8","v":6.6021876056753304E-2},{"$f":"IF(AE21>$J$18,(AE21/(Bodencharakterisierung!$E$11*1000)),0)","v":4.3578796077064886E-5},2.3305291073371062E-2,4,null,{"$f":"(AD21)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH21>0,(AJ21*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK20,NA())","v":7.8857890215031159E-3},null,4,{"$f":"IF(AF21<=$J$9*0.05,AS20*EXP((-$J$6*1)/Heterogenität!$D$4),Z21)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF21>=$J$19, AR20/$J$5<AN21),0, Bodencharakterisierung!$E$8*$J$11*((AR20/$J$5)-AN21))","v":0},0,{"$f":"AQ20-AP21*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ21/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,4,null,{"$f":"(AP21)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF21<=$J$9*1.05,(AV21*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW20,NA())","v":{"$error":"#N/A"}},23072.238162637354,137,3.3929763490215028,7.8857890215031159E-3,0,2.5090560000000001E-2,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},43.578796077064887,23305.291073371063]
[null,"Konzentration Sorbierte Phase"," mg/kg",{"$f":"$J$19*1000000*1000","v":4382.7000000643475},null,"Anzahl Injektionen Schadstoffaustrag",{"$f":"G23-G21","v":22.803875992319128},null,"Plausibilitätsprüfung",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,2.3305291073371062E-2,{"$f":"Z22*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF21*Bodencharakterisierung!$E$11/$J$20","v":4.5604655722183724E-5},{"$f":"((150*($J$2^0.87)*(AB22^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z22)*3600*24","v":8.5342869115242886E-2},2.3915996627248484E-4,{"$f":"AE21-AD22*Bodencharakterisierung!$E$8","v":6.5942953267883381E-2},{"$f":"IF(AE22>$J$18,(AE22/(Bodencharakterisierung!$E$11*1000)),0)","v":4.3526701826985731E-5},2.3305291073371062E-2,5,null,{"$f":"(AD22)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH22>0,(AJ22*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK21,NA())","v":1.0053256276878895E-2},null,5,{"$f":"IF(AF22<=$J$9*0.05,AS21*EXP((-$J$6*1)/Heterogenität!$D$4),Z22)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF22>=$J$19, AR21/$J$5<AN22),0, Bodencharakterisierung!$E$8*$J$11*((AR21/$J$5)-AN22))","v":0},0,{"$f":"AQ21-AP22*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ22/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,5,null,{"$f":"(AP22)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF22<=$J$9*1.05,(AV22*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW21,NA())","v":{"$error":"#N/A"}},23072.238162637354,138,3.4014164562768787,1.0053256276878895E-2,0,3.1363200000000001E-2,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},43.526701826985729,23305.291073371063]
[null,"Stoffparameter",null,null,null,"Gesamtanzahl der Injektionen",{"$f":"MAX(AZ17:AZ5017)","v":26.163875992319127},null,"Zu entfernende Schadstoffmenge im GW ges. [kg]",{"$f":"(D18-Sanierungsdesign!$E$4)*Schadstoffbelastung!$K$11*Bodencharakterisierung!$E$8*10^-6","v":1.0612800000320755},null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,2.3305291073371062E-2,{"$f":"Z23*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF22*Bodencharakterisierung!$E$11/$J$20","v":4.555013975217472E-5},{"$f":"((150*($J$2^0.87)*(AB23^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z23)*3600*24","v":8.5262263847055875E-2},2.3915996627248484E-4,{"$f":"AE22-AD23*Bodencharakterisierung!$E$8","v":6.5864030479013458E-2},{"$f":"IF(AE23>$J$18,(AE23/(Bodencharakterisierung!$E$11*1000)),0)","v":4.3474607576906576E-5},2.3305291073371062E-2,6,null,{"$f":"(AD23)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH23>0,(AJ23*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK22,NA())","v":1.2220723532254674E-2},null,6,{"$f":"IF(AF23<=$J$9*0.05,AS22*EXP((-$J$6*1)/Heterogenität!$D$4),Z23)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF23>=$J$19, AR22/$J$5<AN23),0, Bodencharakterisierung!$E$8*$J$11*((AR22/$J$5)-AN23))","v":0},0,{"$f":"AQ22-AP23*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ23/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,6,null,{"$f":"(AP23)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF23<=$J$9*1.05,(AV23*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW22,NA())","v":{"$error":"#N/A"}},23072.238162637354,139,3.4098565635322546,1.2220723532254674E-2,0,3.7635840000000004E-2,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},43.474607576906578,23305.291073371063]
[null,"Verteilungskoeffizient Boden-Wasser (kD)","L/kg",{"$f":"VLOOKUP($C$30,$B$49:$X$62,10,FALSE)*1000","v":2.0601874130798814},null,"Gesamtanzahl der Injektionszyklen (Kampagnen)",{"$f":"G23/Sanierungsdesign!$E$8","v":5.2327751984638251},null,"Zu entfernende Schadstoffmenge im Boden ges. [kg]",{"$f":"(D19)*Bodencharakterisierung!E11/1000*Schadstoffbelastung!$K$11","v":87.288120001434947},null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,2.3305291073371062E-2,{"$f":"Z24*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF23*Bodencharakterisierung!$E$11/$J$20","v":4.5495623782165736E-5},{"$f":"((150*($J$2^0.87)*(AB24^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z24)*3600*24","v":8.5181638317375935E-2},2.3915996627248484E-4,{"$f":"AE23-AD24*Bodencharakterisierung!$E$8","v":6.5785107690143535E-2},{"$f":"IF(AE24>$J$18,(AE24/(Bodencharakterisierung!$E$11*1000)),0)","v":4.3422513326827414E-5},2.3305291073371062E-2,7,null,{"$f":"(AD24)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH24>0,(AJ24*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK23,NA())","v":1.4388190787630453E-2},null,7,{"$f":"IF(AF24<=$J$9*0.05,AS23*EXP((-$J$6*1)/Heterogenität!$D$4),Z24)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF24>=$J$19, AR23/$J$5<AN24),0, Bodencharakterisierung!$E$8*$J$11*((AR23/$J$5)-AN24))","v":0},0,{"$f":"AQ23-AP24*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ24/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,7,null,{"$f":"(AP24)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF24<=$J$9*1.05,(AV24*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW23,NA())","v":{"$error":"#N/A"}},23072.238162637354,140,3.4182966707876306,1.4388190787630453E-2,0,4.3908480000000007E-2,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},43.422513326827413,23305.291073371063]
[null,"Abbaurate","d-1",{"$f":"VLOOKUP($C$30,$B$49:$X$62,8,FALSE)","v":2.2812314698908428E-2},null,"Relevante Konzentration DOC im Gesamtboden [kg DOC/m3 Boden]",{"$f":"IF((Grundwassercharakterisierung!D15>2),(Grundwassercharakterisierung!D15*Bodencharakterisierung!E8*0.001*2),0)","v":0},null,"H2 Bedarf zur Entfernung im GW [kg]",{"$f":"$G$11*J23","v":4.6506251472226638E-2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,2.3305291073371062E-2,{"$f":"Z25*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF24*Bodencharakterisierung!$E$11/$J$20","v":4.5441107812156739E-5},{"$f":"((150*($J$2^0.87)*(AB25^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z25)*3600*24","v":8.5100992496822098E-2},2.3915996627248484E-4,{"$f":"AE24-AD25*Bodencharakterisierung!$E$8","v":6.5706184901273612E-2},{"$f":"IF(AE25>$J$18,(AE25/(Bodencharakterisierung!$E$11*1000)),0)","v":4.3370419076748259E-5},2.3305291073371062E-2,8,null,{"$f":"(AD25)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH25>0,(AJ25*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK24,NA())","v":1.6555658043006231E-2},null,8,{"$f":"IF(AF25<=$J$9*0.05,AS24*EXP((-$J$6*1)/Heterogenität!$D$4),Z25)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF25>=$J$19, AR24/$J$5<AN25),0, Bodencharakterisierung!$E$8*$J$11*((AR24/$J$5)-AN25))","v":0},0,{"$f":"AQ24-AP25*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ25/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,8,null,{"$f":"(AP25)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF25<=$J$9*1.05,(AV25*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW24,NA())","v":{"$error":"#N/A"}},23072.238162637354,141,3.426736778043006,1.6555658043006231E-2,0,5.018112000000001E-2,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},43.370419076748256,23305.291073371063]
[null,"Modifizierte Reynoldszahl","-",{"$f":"$J$2","v":7.023076923076924E-4},null,"Stöchio. Faktor Sauerstoff [g H2/gEA]",0.125,null,"H2 Bedarf zur Entfernung im Boden [kg]",{"$f":"$G$11*J24","v":3.8250445303802385},null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,2.3305291073371062E-2,{"$f":"Z26*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF25*Bodencharakterisierung!$E$11/$J$20","v":4.5386591842147748E-5},{"$f":"((150*($J$2^0.87)*(AB26^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z26)*3600*24","v":8.5020326355935177E-2},2.3915996627248484E-4,{"$f":"AE25-AD26*Bodencharakterisierung!$E$8","v":6.5627262112403689E-2},{"$f":"IF(AE26>$J$18,(AE26/(Bodencharakterisierung!$E$11*1000)),0)","v":4.3318324826669104E-5},2.3305291073371062E-2,9,null,{"$f":"(AD26)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH26>0,(AJ26*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK25,NA())","v":1.872312529838201E-2},null,9,{"$f":"IF(AF26<=$J$9*0.05,AS25*EXP((-$J$6*1)/Heterogenität!$D$4),Z26)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF26>=$J$19, AR25/$J$5<AN26),0, Bodencharakterisierung!$E$8*$J$11*((AR25/$J$5)-AN26))","v":0},0,{"$f":"AQ25-AP26*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ26/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,9,null,{"$f":"(AP26)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF26<=$J$9*1.05,(AV26*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW25,NA())","v":{"$error":"#N/A"}},23072.238162637354,142,3.4351768852983819,1.872312529838201E-2,0,5.6453760000000013E-2,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},43.318324826669105,23305.291073371063]
[null,"Dichte des Schadstoffes","kg/L",{"$f":"VLOOKUP($C$30,$B$49:$X$62,16,FALSE)","v":1.4477003501341623},null,"Stöchio. Faktor Nitrat [g H2/gEA]",8.0645161290322578E-2,null,"Erforderliche Injektionen gesamt",{"$f":"(J25+J26)/$G$10/$G$8","v":3.4069646880301692},null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,2.3305291073371062E-2,{"$f":"Z27*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF26*Bodencharakterisierung!$E$11/$J$20","v":4.5332075872138751E-5},{"$f":"((150*($J$2^0.87)*(AB27^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z27)*3600*24","v":8.4939639865178551E-2},2.3915996627248484E-4,{"$f":"AE26-AD27*Bodencharakterisierung!$E$8","v":6.5548339323533766E-2},{"$f":"IF(AE27>$J$18,(AE27/(Bodencharakterisierung!$E$11*1000)),0)","v":4.3266230576589942E-5},2.3305291073371062E-2,10,null,{"$f":"(AD27)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH27>0,(AJ27*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK26,NA())","v":2.0890592553757789E-2},null,10,{"$f":"IF(AF27<=$J$9*0.05,AS26*EXP((-$J$6*1)/Heterogenität!$D$4),Z27)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF27>=$J$19, AR26/$J$5<AN27),0, Bodencharakterisierung!$E$8*$J$11*((AR26/$J$5)-AN27))","v":0},0,{"$f":"AQ26-AP27*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ27/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,10,null,{"$f":"(AP27)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF27<=$J$9*1.05,(AV27*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW26,NA())","v":{"$error":"#N/A"}},23072.238162637354,143,3.4436169925537579,2.0890592553757789E-2,0,6.2726400000000015E-2,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},43.26623057658994,23305.291073371063]
[null,"Stöchiometrischer Abbau-Faktor","g/g",{"$f":"VLOOKUP($C$30,$B$49:$X$62,22,FALSE)","v":4.3820906330865619E-2},null,"Stöchio. Faktor Mangan  [g H2/gEA]",2.2988505747126398E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11,2.3305291073371062E-2,{"$f":"Z28*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF27*Bodencharakterisierung!$E$11/$J$20","v":4.5277559902129753E-5},{"$f":"((150*($J$2^0.87)*(AB28^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z28)*3600*24","v":8.4858932994936381E-2},2.3915996627248484E-4,{"$f":"AE27-AD28*Bodencharakterisierung!$E$8","v":6.5469416534663843E-2},{"$f":"IF(AE28>$J$18,(AE28/(Bodencharakterisierung!$E$11*1000)),0)","v":4.3214136326510786E-5},2.3305291073371062E-2,11,null,{"$f":"(AD28)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH28>0,(AJ28*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK27,NA())","v":2.3058059809133568E-2},null,11,{"$f":"IF(AF28<=$J$9*0.05,AS27*EXP((-$J$6*1)/Heterogenität!$D$4),Z28)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF28>=$J$19, AR27/$J$5<AN28),0, Bodencharakterisierung!$E$8*$J$11*((AR27/$J$5)-AN28))","v":0},0,{"$f":"AQ27-AP28*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ28/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,11,null,{"$f":"(AP28)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF28<=$J$9*1.05,(AV28*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW27,NA())","v":{"$error":"#N/A"}},23072.238162637354,144,3.4520570998091333,2.3058059809133568E-2,0,6.8999040000000011E-2,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},43.214136326510783,23305.291073371063]
[null,null,null,null,null,"Stöchio. Faktor Eisen [g H2/gEA]",1.785714285714286E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,2.3305291073371062E-2,{"$f":"Z29*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF28*Bodencharakterisierung!$E$11/$J$20","v":4.5223043932120763E-5},{"$f":"((150*($J$2^0.87)*(AB29^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z29)*3600*24","v":8.477820571551424E-2},2.3915996627248484E-4,{"$f":"AE28-AD29*Bodencharakterisierung!$E$8","v":6.5390493745793921E-2},{"$f":"IF(AE29>$J$18,(AE29/(Bodencharakterisierung!$E$11*1000)),0)","v":4.3162042076431631E-5},2.3305291073371062E-2,12,null,{"$f":"(AD29)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH29>0,(AJ29*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK28,NA())","v":2.5225527064509347E-2},null,12,{"$f":"IF(AF29<=$J$9*0.05,AS28*EXP((-$J$6*1)/Heterogenität!$D$4),Z29)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF29>=$J$19, AR28/$J$5<AN29),0, Bodencharakterisierung!$E$8*$J$11*((AR28/$J$5)-AN29))","v":0},0,{"$f":"AQ28-AP29*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ29/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,12,null,{"$f":"(AP29)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF29<=$J$9*1.05,(AV29*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW28,NA())","v":{"$error":"#N/A"}},23072.238162637354,145,3.4604972070645093,2.5225527064509347E-2,0,7.5271680000000007E-2,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},43.162042076431632,23305.291073371063]
[null,"Betrachteter Schadstoff",{"$f":"VLOOKUP(Sanierungsdesign!$E$13,tblSchadstoffauswahl[],2,FALSE)","v":"Summe LCKW"},null,null,"Stöchio. Faktor Sulfat  [g H2/gEA]",8.3333333333333329E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,2.3305291073371062E-2,{"$f":"Z30*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF29*Bodencharakterisierung!$E$11/$J$20","v":4.5168527962111779E-5},{"$f":"((150*($J$2^0.87)*(AB30^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z30)*3600*24","v":8.4697457997138847E-2},2.3915996627248484E-4,{"$f":"AE29-AD30*Bodencharakterisierung!$E$8","v":6.5311570956923998E-2},{"$f":"IF(AE30>$J$18,(AE30/(Bodencharakterisierung!$E$11*1000)),0)","v":4.3109947826352476E-5},2.3305291073371062E-2,13,null,{"$f":"(AD30)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH30>0,(AJ30*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK29,NA())","v":2.7392994319885126E-2},null,13,{"$f":"IF(AF30<=$J$9*0.05,AS29*EXP((-$J$6*1)/Heterogenität!$D$4),Z30)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF30>=$J$19, AR29/$J$5<AN30),0, Bodencharakterisierung!$E$8*$J$11*((AR29/$J$5)-AN30))","v":0},0,{"$f":"AQ29-AP30*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ30/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,13,null,{"$f":"(AP30)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF30<=$J$9*1.05,(AV30*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW29,NA())","v":{"$error":"#N/A"}},23072.238162637354,146,3.4689373143198852,2.7392994319885126E-2,0,8.1544320000000003E-2,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},43.109947826352474,23305.291073371063]
[null,"Verwendetes Substrat",{"$f":"Sanierungsdesign!$E$16","v":"Glucose"},null,null,"Stöchio. Faktor CO2  [g H2/gEA]",0.18181818181818182,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14,2.3305291073371062E-2,{"$f":"Z31*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF30*Bodencharakterisierung!$E$11/$J$20","v":4.5114011992102781E-5},{"$f":"((150*($J$2^0.87)*(AB31^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z31)*3600*24","v":8.4616689809957055E-2},2.3915996627248484E-4,{"$f":"AE30-AD31*Bodencharakterisierung!$E$8","v":6.5232648168054075E-2},{"$f":"IF(AE31>$J$18,(AE31/(Bodencharakterisierung!$E$11*1000)),0)","v":4.3057853576273314E-5},2.3305291073371062E-2,14,null,{"$f":"(AD31)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH31>0,(AJ31*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK30,NA())","v":2.9560461575260905E-2},null,14,{"$f":"IF(AF31<=$J$9*0.05,AS30*EXP((-$J$6*1)/Heterogenität!$D$4),Z31)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF31>=$J$19, AR30/$J$5<AN31),0, Bodencharakterisierung!$E$8*$J$11*((AR30/$J$5)-AN31))","v":0},0,{"$f":"AQ30-AP31*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ31/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,14,null,{"$f":"(AP31)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF31<=$J$9*1.05,(AV31*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW30,NA())","v":{"$error":"#N/A"}},23072.238162637354,147,3.4773774215752606,2.9560461575260905E-2,0,8.7816959999999999E-2,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},43.057853576273317,23305.291073371063]
[null,"Gesamtdauer [d] ",{"$f":"D3+((D11*D9)/24)","v":3374.4779325910808},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,2.3305291073371062E-2,{"$f":"Z32*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF31*Bodencharakterisierung!$E$11/$J$20","v":4.5059496022093784E-5},{"$f":"((150*($J$2^0.87)*(AB32^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z32)*3600*24","v":8.4535901124036361E-2},2.3915996627248484E-4,{"$f":"AE31-AD32*Bodencharakterisierung!$E$8","v":6.5153725379184152E-2},{"$f":"IF(AE32>$J$18,(AE32/(Bodencharakterisierung!$E$11*1000)),0)","v":4.3005759326194159E-5},2.3305291073371062E-2,15,null,{"$f":"(AD32)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH32>0,(AJ32*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK31,NA())","v":3.1727928830636687E-2},null,15,{"$f":"IF(AF32<=$J$9*0.05,AS31*EXP((-$J$6*1)/Heterogenität!$D$4),Z32)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF32>=$J$19, AR31/$J$5<AN32),0, Bodencharakterisierung!$E$8*$J$11*((AR31/$J$5)-AN32))","v":0},0,{"$f":"AQ31-AP32*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ32/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,15,null,{"$f":"(AP32)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF32<=$J$9*1.05,(AV32*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW31,NA())","v":{"$error":"#N/A"}},23072.238162637354,148,3.4858175288306366,3.1727928830636687E-2,0,9.4089599999999995E-2,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},43.005759326194159,23305.291073371063]
[null,null,null,null,null,"ED-Verbrauch durch gelöste Stoffe [kg H2/m3 Boden]",{"$f":"(Grundwassercharakterisierung!D9*G26+Grundwassercharakterisierung!$D$10*G27+Grundwassercharakterisierung!$D$13*G30)*0.001*Bodencharakterisierung!$E$8","v":8.250000000000001E-4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,2.3305291073371062E-2,{"$f":"Z33*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF32*Bodencharakterisierung!$E$11/$J$20","v":4.5004980052084793E-5},{"$f":"((150*($J$2^0.87)*(AB33^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z33)*3600*24","v":8.44550919093639E-2},2.3915996627248484E-4,{"$f":"AE32-AD33*Bodencharakterisierung!$E$8","v":6.5074802590314229E-2},{"$f":"IF(AE33>$J$18,(AE33/(Bodencharakterisierung!$E$11*1000)),0)","v":4.2953665076115003E-5},2.3305291073371062E-2,16,null,{"$f":"(AD33)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH33>0,(AJ33*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK32,NA())","v":3.3895396086012469E-2},null,16,{"$f":"IF(AF33<=$J$9*0.05,AS32*EXP((-$J$6*1)/Heterogenität!$D$4),Z33)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF33>=$J$19, AR32/$J$5<AN33),0, Bodencharakterisierung!$E$8*$J$11*((AR32/$J$5)-AN33))","v":0},0,{"$f":"AQ32-AP33*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ33/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,16,null,{"$f":"(AP33)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF33<=$J$9*1.05,(AV33*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW32,NA())","v":{"$error":"#N/A"}},23072.238162637354,149,3.4942576360860125,3.3895396086012469E-2,0,0.10036223999999999,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},42.953665076115001,23305.291073371063]
[null,null,null,null,null,"ED-Verbrauch durch gelöste zuströmende Stoffe [kg H2/d]",{"$f":"Grundwassercharakterisierung!$D$4*Bodencharakterisierung!$E$7*Schadstoffbelastung!$K$5*Schadstoffbelastung!$K$9*G33","v":2.3522400000000002E-3},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17,2.3305291073371062E-2,{"$f":"Z34*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF33*Bodencharakterisierung!$E$11/$J$20","v":4.4950464082075803E-5},{"$f":"((150*($J$2^0.87)*(AB34^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z34)*3600*24","v":8.4374262135846562E-2},2.3915996627248484E-4,{"$f":"AE33-AD34*Bodencharakterisierung!$E$8","v":6.4995879801444306E-2},{"$f":"IF(AE34>$J$18,(AE34/(Bodencharakterisierung!$E$11*1000)),0)","v":4.2901570826035848E-5},2.3305291073371062E-2,17,null,{"$f":"(AD34)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH34>0,(AJ34*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK33,NA())","v":3.6062863341388252E-2},null,17,{"$f":"IF(AF34<=$J$9*0.05,AS33*EXP((-$J$6*1)/Heterogenität!$D$4),Z34)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF34>=$J$19, AR33/$J$5<AN34),0, Bodencharakterisierung!$E$8*$J$11*((AR33/$J$5)-AN34))","v":0},0,{"$f":"AQ33-AP34*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ34/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,17,null,{"$f":"(AP34)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF34<=$J$9*1.05,(AV34*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW33,NA())","v":{"$error":"#N/A"}},23072.238162637354,150,3.5026977433413879,3.6062863341388252E-2,0,0.10663487999999999,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},42.901570826035851,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,2.3305291073371062E-2,{"$f":"Z35*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF34*Bodencharakterisierung!$E$11/$J$20","v":4.4895948112066805E-5},{"$f":"((150*($J$2^0.87)*(AB35^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z35)*3600*24","v":8.4293411773310775E-2},2.3915996627248484E-4,{"$f":"AE34-AD35*Bodencharakterisierung!$E$8","v":6.4916957012574383E-2},{"$f":"IF(AE35>$J$18,(AE35/(Bodencharakterisierung!$E$11*1000)),0)","v":4.2849476575956686E-5},2.3305291073371062E-2,18,null,{"$f":"(AD35)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH35>0,(AJ35*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK34,NA())","v":3.8230330596764034E-2},null,18,{"$f":"IF(AF35<=$J$9*0.05,AS34*EXP((-$J$6*1)/Heterogenität!$D$4),Z35)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF35>=$J$19, AR34/$J$5<AN35),0, Bodencharakterisierung!$E$8*$J$11*((AR34/$J$5)-AN35))","v":0},0,{"$f":"AQ34-AP35*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ35/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,18,null,{"$f":"(AP35)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF35<=$J$9*1.05,(AV35*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW34,NA())","v":{"$error":"#N/A"}},23072.238162637354,151,3.5111378505967639,3.8230330596764034E-2,0,0.11290751999999998,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},42.849476575956686,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,2.3305291073371062E-2,{"$f":"Z36*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF35*Bodencharakterisierung!$E$11/$J$20","v":4.4841432142057808E-5},{"$f":"((150*($J$2^0.87)*(AB36^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z36)*3600*24","v":8.4212540791501769E-2},2.3915996627248484E-4,{"$f":"AE35-AD36*Bodencharakterisierung!$E$8","v":6.483803422370446E-2},{"$f":"IF(AE36>$J$18,(AE36/(Bodencharakterisierung!$E$11*1000)),0)","v":4.2797382325877531E-5},2.3305291073371062E-2,19,null,{"$f":"(AD36)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH36>0,(AJ36*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK35,NA())","v":4.0397797852139816E-2},null,19,{"$f":"IF(AF36<=$J$9*0.05,AS35*EXP((-$J$6*1)/Heterogenität!$D$4),Z36)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF36>=$J$19, AR35/$J$5<AN36),0, Bodencharakterisierung!$E$8*$J$11*((AR35/$J$5)-AN36))","v":0},0,{"$f":"AQ35-AP36*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ36/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,19,null,{"$f":"(AP36)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF36<=$J$9*1.05,(AV36*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW35,NA())","v":{"$error":"#N/A"}},23072.238162637354,152,3.5195779578521398,4.0397797852139816E-2,0,0.11918015999999998,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},42.797382325877528,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,2.3305291073371062E-2,{"$f":"Z37*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF36*Bodencharakterisierung!$E$11/$J$20","v":4.4786916172048824E-5},{"$f":"((150*($J$2^0.87)*(AB37^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z37)*3600*24","v":8.413164916008356E-2},2.3915996627248484E-4,{"$f":"AE36-AD37*Bodencharakterisierung!$E$8","v":6.4759111434834538E-2},{"$f":"IF(AE37>$J$18,(AE37/(Bodencharakterisierung!$E$11*1000)),0)","v":4.2745288075798376E-5},2.3305291073371062E-2,20,null,{"$f":"(AD37)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH37>0,(AJ37*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK36,NA())","v":4.2565265107515599E-2},null,20,{"$f":"IF(AF37<=$J$9*0.05,AS36*EXP((-$J$6*1)/Heterogenität!$D$4),Z37)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF37>=$J$19, AR36/$J$5<AN37),0, Bodencharakterisierung!$E$8*$J$11*((AR36/$J$5)-AN37))","v":0},0,{"$f":"AQ36-AP37*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ37/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,20,null,{"$f":"(AP37)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF37<=$J$9*1.05,(AV37*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW36,NA())","v":{"$error":"#N/A"}},23072.238162637354,153,3.5280180651075153,4.2565265107515599E-2,0,0.12545279999999998,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},42.745288075798378,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21,2.3305291073371062E-2,{"$f":"Z38*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF37*Bodencharakterisierung!$E$11/$J$20","v":4.4732400202039834E-5},{"$f":"((150*($J$2^0.87)*(AB38^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z38)*3600*24","v":8.4050736848638313E-2},2.3915996627248484E-4,{"$f":"AE37-AD38*Bodencharakterisierung!$E$8","v":6.4680188645964615E-2},{"$f":"IF(AE38>$J$18,(AE38/(Bodencharakterisierung!$E$11*1000)),0)","v":4.269319382571922E-5},2.3305291073371062E-2,21,null,{"$f":"(AD38)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH38>0,(AJ38*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK37,NA())","v":4.4732732362891381E-2},null,21,{"$f":"IF(AF38<=$J$9*0.05,AS37*EXP((-$J$6*1)/Heterogenität!$D$4),Z38)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF38>=$J$19, AR37/$J$5<AN38),0, Bodencharakterisierung!$E$8*$J$11*((AR37/$J$5)-AN38))","v":0},0,{"$f":"AQ37-AP38*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ38/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,21,null,{"$f":"(AP38)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF38<=$J$9*1.05,(AV38*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW37,NA())","v":{"$error":"#N/A"}},23072.238162637354,154,3.5364581723628912,4.4732732362891381E-2,0,0.13172543999999997,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},42.69319382571922,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,2.3305291073371062E-2,{"$f":"Z39*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF38*Bodencharakterisierung!$E$11/$J$20","v":4.4677884232030836E-5},{"$f":"((150*($J$2^0.87)*(AB39^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z39)*3600*24","v":8.3969803826666578E-2},2.3915996627248484E-4,{"$f":"AE38-AD39*Bodencharakterisierung!$E$8","v":6.4601265857094692E-2},{"$f":"IF(AE39>$J$18,(AE39/(Bodencharakterisierung!$E$11*1000)),0)","v":4.2641099575640058E-5},2.3305291073371062E-2,22,null,{"$f":"(AD39)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH39>0,(AJ39*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK38,NA())","v":4.6900199618267163E-2},null,22,{"$f":"IF(AF39<=$J$9*0.05,AS38*EXP((-$J$6*1)/Heterogenität!$D$4),Z39)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF39>=$J$19, AR38/$J$5<AN39),0, Bodencharakterisierung!$E$8*$J$11*((AR38/$J$5)-AN39))","v":0},0,{"$f":"AQ38-AP39*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ39/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,22,null,{"$f":"(AP39)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF39<=$J$9*1.05,(AV39*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW38,NA())","v":{"$error":"#N/A"}},23072.238162637354,155,3.5448982796182671,4.6900199618267163E-2,0,0.13799807999999997,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},42.641099575640055,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23,2.3305291073371062E-2,{"$f":"Z40*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF39*Bodencharakterisierung!$E$11/$J$20","v":4.4623368262021839E-5},{"$f":"((150*($J$2^0.87)*(AB40^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z40)*3600*24","v":8.3888850063586554E-2},2.3915996627248484E-4,{"$f":"AE39-AD40*Bodencharakterisierung!$E$8","v":6.4522343068224769E-2},{"$f":"IF(AE40>$J$18,(AE40/(Bodencharakterisierung!$E$11*1000)),0)","v":4.2589005325560903E-5},2.3305291073371062E-2,23,null,{"$f":"(AD40)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH40>0,(AJ40*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK39,NA())","v":4.9067666873642946E-2},null,23,{"$f":"IF(AF40<=$J$9*0.05,AS39*EXP((-$J$6*1)/Heterogenität!$D$4),Z40)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF40>=$J$19, AR39/$J$5<AN40),0, Bodencharakterisierung!$E$8*$J$11*((AR39/$J$5)-AN40))","v":0},0,{"$f":"AQ39-AP40*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ40/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,23,null,{"$f":"(AP40)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF40<=$J$9*1.05,(AV40*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW39,NA())","v":{"$error":"#N/A"}},23072.238162637354,156,3.5533383868736426,4.9067666873642946E-2,0,0.14427071999999996,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},42.589005325560905,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,24,2.3305291073371062E-2,{"$f":"Z41*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF40*Bodencharakterisierung!$E$11/$J$20","v":4.4568852292012848E-5},{"$f":"((150*($J$2^0.87)*(AB41^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z41)*3600*24","v":8.3807875528733769E-2},2.3915996627248484E-4,{"$f":"AE40-AD41*Bodencharakterisierung!$E$8","v":6.4443420279354846E-2},{"$f":"IF(AE41>$J$18,(AE41/(Bodencharakterisierung!$E$11*1000)),0)","v":4.2536911075481748E-5},2.3305291073371062E-2,24,null,{"$f":"(AD41)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH41>0,(AJ41*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK40,NA())","v":5.1235134129018728E-2},null,24,{"$f":"IF(AF41<=$J$9*0.05,AS40*EXP((-$J$6*1)/Heterogenität!$D$4),Z41)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF41>=$J$19, AR40/$J$5<AN41),0, Bodencharakterisierung!$E$8*$J$11*((AR40/$J$5)-AN41))","v":0},0,{"$f":"AQ40-AP41*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ41/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,24,null,{"$f":"(AP41)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF41<=$J$9*1.05,(AV41*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW40,NA())","v":{"$error":"#N/A"}},23072.238162637354,157,3.5617784941290185,5.1235134129018728E-2,0,0.15054335999999996,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},42.536911075481747,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,2.3305291073371062E-2,{"$f":"Z42*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF41*Bodencharakterisierung!$E$11/$J$20","v":4.4514336322003864E-5},{"$f":"((150*($J$2^0.87)*(AB42^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z42)*3600*24","v":8.3726880191360931E-2},2.3915996627248484E-4,{"$f":"AE41-AD42*Bodencharakterisierung!$E$8","v":6.4364497490484923E-2},{"$f":"IF(AE42>$J$18,(AE42/(Bodencharakterisierung!$E$11*1000)),0)","v":4.2484816825402593E-5},2.3305291073371062E-2,25,null,{"$f":"(AD42)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH42>0,(AJ42*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK41,NA())","v":5.340260138439451E-2},null,25,{"$f":"IF(AF42<=$J$9*0.05,AS41*EXP((-$J$6*1)/Heterogenität!$D$4),Z42)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF42>=$J$19, AR41/$J$5<AN42),0, Bodencharakterisierung!$E$8*$J$11*((AR41/$J$5)-AN42))","v":0},0,{"$f":"AQ41-AP42*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ42/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,25,null,{"$f":"(AP42)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF42<=$J$9*1.05,(AV42*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW41,NA())","v":{"$error":"#N/A"}},23072.238162637354,158,3.5702186013843944,5.340260138439451E-2,0,0.15681599999999996,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},42.484816825402589,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,2.3305291073371062E-2,{"$f":"Z43*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF42*Bodencharakterisierung!$E$11/$J$20","v":4.445982035199486E-5},{"$f":"((150*($J$2^0.87)*(AB43^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z43)*3600*24","v":8.3645864020637561E-2},2.3915996627248484E-4,{"$f":"AE42-AD43*Bodencharakterisierung!$E$8","v":6.4285574701615E-2},{"$f":"IF(AE43>$J$18,(AE43/(Bodencharakterisierung!$E$11*1000)),0)","v":4.2432722575323431E-5},2.3305291073371062E-2,26,null,{"$f":"(AD43)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH43>0,(AJ43*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK42,NA())","v":5.5570068639770293E-2},null,26,{"$f":"IF(AF43<=$J$9*0.05,AS42*EXP((-$J$6*1)/Heterogenität!$D$4),Z43)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF43>=$J$19, AR42/$J$5<AN43),0, Bodencharakterisierung!$E$8*$J$11*((AR42/$J$5)-AN43))","v":0},0,{"$f":"AQ42-AP43*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ43/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,26,null,{"$f":"(AP43)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF43<=$J$9*1.05,(AV43*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW42,NA())","v":{"$error":"#N/A"}},23072.238162637354,159,3.5786587086397703,5.5570068639770293E-2,0,0.16308863999999995,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},42.432722575323432,23305.291073371063]
[null,1,{"$f":"B44+1","v":2},{"$f":"C44+1","v":3},{"$f":"D44+1","v":4},{"$f":"E44+1","v":5},{"$f":"F44+1","v":6},{"$f":"G44+1","v":7},{"$f":"H44+1","v":8},{"$f":"I44+1","v":9},{"$f":"J44+1","v":10},{"$f":"K44+1","v":11},{"$f":"L44+1","v":12},{"$f":"M44+1","v":13},{"$f":"N44+1","v":14},{"$f":"O44+1","v":15},{"$f":"P44+1","v":16},{"$f":"Q44+1","v":17},{"$f":"R44+1","v":18},{"$f":"S44+1","v":19},{"$f":"T44+1","v":20},{"$f":"U44+1","v":21},{"$f":"V44+1","v":22},{"$f":"W44+1","v":23},27,2.3305291073371062E-2,{"$f":"Z44*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF43*Bodencharakterisierung!$E$11/$J$20","v":4.4405304381985863E-5},{"$f":"((150*($J$2^0.87)*(AB44^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z44)*3600*24","v":8.3564826985649321E-2},2.3915996627248484E-4,{"$f":"AE43-AD44*Bodencharakterisierung!$E$8","v":6.4206651912745077E-2},{"$f":"IF(AE44>$J$18,(AE44/(Bodencharakterisierung!$E$11*1000)),0)","v":4.2380628325244276E-5},2.3305291073371062E-2,27,null,{"$f":"(AD44)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH44>0,(AJ44*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK43,NA())","v":5.7737535895146075E-2},null,27,{"$f":"IF(AF44<=$J$9*0.05,AS43*EXP((-$J$6*1)/Heterogenität!$D$4),Z44)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF44>=$J$19, AR43/$J$5<AN44),0, Bodencharakterisierung!$E$8*$J$11*((AR43/$J$5)-AN44))","v":0},0,{"$f":"AQ43-AP44*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ44/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,27,null,{"$f":"(AP44)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF44<=$J$9*1.05,(AV44*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW43,NA())","v":{"$error":"#N/A"}},23072.238162637354,160,3.5870988158951458,5.7737535895146075E-2,0,0.16936127999999995,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},42.380628325244274,23305.291073371063]
[null,"betrachteter Schadstoff",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,28,2.3305291073371062E-2,{"$f":"Z45*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF44*Bodencharakterisierung!$E$11/$J$20","v":4.4350788411976879E-5},{"$f":"((150*($J$2^0.87)*(AB45^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z45)*3600*24","v":8.3483769055398643E-2},2.3915996627248484E-4,{"$f":"AE44-AD45*Bodencharakterisierung!$E$8","v":6.4127729123875155E-2},{"$f":"IF(AE45>$J$18,(AE45/(Bodencharakterisierung!$E$11*1000)),0)","v":4.232853407516512E-5},2.3305291073371062E-2,28,null,{"$f":"(AD45)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH45>0,(AJ45*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK44,NA())","v":5.9905003150521857E-2},null,28,{"$f":"IF(AF45<=$J$9*0.05,AS44*EXP((-$J$6*1)/Heterogenität!$D$4),Z45)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF45>=$J$19, AR44/$J$5<AN45),0, Bodencharakterisierung!$E$8*$J$11*((AR44/$J$5)-AN45))","v":0},0,{"$f":"AQ44-AP45*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ45/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,28,null,{"$f":"(AP45)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF45<=$J$9*1.05,(AV45*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW44,NA())","v":{"$error":"#N/A"}},23072.238162637354,161,3.5955389231505217,5.9905003150521857E-2,0,0.17563391999999994,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},42.328534075165123,23305.291073371063]
[null,null,"Inventar [kg]","Konz. Wasser [kg/m3]","Molgewicht [g/Mol]","Stoffmenge [Mol]","Anteile \n[-]","bewertungs-relevant","Abbaurate \n[d-1]","Löslichkeit [kg/m3]","Kd \n[kg/m3]","ZielC \n[kg/m³]","StartC/ZielC","Sanierung erforderlich?","Auswahl","Relevant","Dichte Schadstoff [kg/L]","Diffusionskoeffizient Wasser Daq [m2/s]","Grenzkonzentration","Mittlere Konzentration","Residualphase","Sättigungskonzentration","Stöchiometrischer Faktor ","C(w, Gleich-gewicht) [m³/kg]",29,2.3305291073371062E-2,{"$f":"Z46*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF45*Bodencharakterisierung!$E$11/$J$20","v":4.4296272441967888E-5},{"$f":"((150*($J$2^0.87)*(AB46^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z46)*3600*24","v":8.3402690198802809E-2},2.3915996627248484E-4,{"$f":"AE45-AD46*Bodencharakterisierung!$E$8","v":6.4048806335005232E-2},{"$f":"IF(AE46>$J$18,(AE46/(Bodencharakterisierung!$E$11*1000)),0)","v":4.2276439825085958E-5},2.3305291073371062E-2,29,null,{"$f":"(AD46)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH46>0,(AJ46*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK45,NA())","v":6.207247040589764E-2},null,29,{"$f":"IF(AF46<=$J$9*0.05,AS45*EXP((-$J$6*1)/Heterogenität!$D$4),Z46)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF46>=$J$19, AR45/$J$5<AN46),0, Bodencharakterisierung!$E$8*$J$11*((AR45/$J$5)-AN46))","v":0},0,{"$f":"AQ45-AP46*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ46/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,29,null,{"$f":"(AP46)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF46<=$J$9*1.05,(AV46*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW45,NA())","v":{"$error":"#N/A"}},23072.238162637354,162,3.6039790304058976,6.207247040589764E-2,0,0.18190655999999994,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},42.276439825085959,23305.291073371063]
[null,"LCKW",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Boden [kg/kg]","Boden [kg/kg]","Boden [kg/kg]","ci [kg/m3]",null,null,30,2.3305291073371062E-2,{"$f":"Z47*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF46*Bodencharakterisierung!$E$11/$J$20","v":4.4241756471958891E-5},{"$f":"((150*($J$2^0.87)*(AB47^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z47)*3600*24","v":8.3321590384695499E-2},2.3915996627248484E-4,{"$f":"AE46-AD47*Bodencharakterisierung!$E$8","v":6.3969883546135309E-2},{"$f":"IF(AE47>$J$18,(AE47/(Bodencharakterisierung!$E$11*1000)),0)","v":4.2224345575006803E-5},2.3305291073371062E-2,30,null,{"$f":"(AD47)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH47>0,(AJ47*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK46,NA())","v":6.4239937661273422E-2},null,30,{"$f":"IF(AF47<=$J$9*0.05,AS46*EXP((-$J$6*1)/Heterogenität!$D$4),Z47)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF47>=$J$19, AR46/$J$5<AN47),0, Bodencharakterisierung!$E$8*$J$11*((AR46/$J$5)-AN47))","v":0},0,{"$f":"AQ46-AP47*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ47/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,30,null,{"$f":"(AP47)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF47<=$J$9*1.05,(AV47*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW46,NA())","v":{"$error":"#N/A"}},23072.238162637354,163,3.6124191376612731,6.4239937661273422E-2,0,0.18817919999999994,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},42.224345575006801,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31,2.3305291073371062E-2,{"$f":"Z48*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF47*Bodencharakterisierung!$E$11/$J$20","v":4.4187240501949894E-5},{"$f":"((150*($J$2^0.87)*(AB48^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z48)*3600*24","v":8.3240469581824766E-2},2.3915996627248484E-4,{"$f":"AE47-AD48*Bodencharakterisierung!$E$8","v":6.3890960757265386E-2},{"$f":"IF(AE48>$J$18,(AE48/(Bodencharakterisierung!$E$11*1000)),0)","v":4.2172251324927648E-5},2.3305291073371062E-2,31,null,{"$f":"(AD48)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH48>0,(AJ48*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK47,NA())","v":6.6407404916649204E-2},null,31,{"$f":"IF(AF48<=$J$9*0.05,AS47*EXP((-$J$6*1)/Heterogenität!$D$4),Z48)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF48>=$J$19, AR47/$J$5<AN48),0, Bodencharakterisierung!$E$8*$J$11*((AR47/$J$5)-AN48))","v":0},0,{"$f":"AQ47-AP48*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ48/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,31,null,{"$f":"(AP48)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF48<=$J$9*1.05,(AV48*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW47,NA())","v":{"$error":"#N/A"}},23072.238162637354,164,3.620859244916649,6.6407404916649204E-2,0,0.19445183999999993,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},42.17225132492765,23305.291073371063]
[null,"Tetrachlorethen",{"$f":"Schadstoffbelastung!E4","v":48.585599999999999},{"$f":"Schadstoffbelastung!U4*10^-6","v":6.9999999999999999E-4},{"$f":"Stoffdatenbank!R5","v":166},{"$f":"IFERROR(C49*1000/E49,0)","v":292.68433734939759},{"$f":"(F49/$F$62)","v":0.44479734563117179},{"$f":"G49>0.05","v":true},{"$f":"Stoffdatenbank!D5","v":2.8000000000000001E-2},{"$f":"Stoffdatenbank!N5*10^-3","v":0.16},{"$f":"(Stoffdatenbank!J5*10^-3)*Bodencharakterisierung!$E$9","v":3.5999999999999999E-3},{"$f":"Sanierungsdesign!$E$4*10^-6","v":1.9999999999999998E-4},{"$f":"D49/L49","v":3.5000000000000004},{"$f":"M49>1","v":true},{"$f":"N49*((M49^0.5)*K49)/((I49^1.2)*(J49^0.9))","v":2.5588150766873712},{"$f":"IF(O49=MAX($O$49:$O$61),\"Ja\",0)","v":"Ja"},{"$f":"Stoffdatenbank!Q5","v":1.6240000000000001},{"$f":"Stoffdatenbank!L5","v":7.49E-10},{"$f":"Schadstoffbelastung!X4*10^-6","v":2.5199999999999996E-6},{"$f":"Schadstoffbelastung!Y4*10^-6","v":2.6724752475247528E-5},{"$f":"Schadstoffbelastung!Z4*10^-6","v":2.4204752475247528E-5},{"$f":"Schadstoffbelastung!W4*10^-6","v":2.5965560764859941E-2},{"$f":"Sanierungsdesign!M11","v":4.8192771084337345E-2},{"$f":"T49/K49","v":7.4235423542354248E-3},32,2.3305291073371062E-2,{"$f":"Z49*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF48*Bodencharakterisierung!$E$11/$J$20","v":4.4132724531940903E-5},{"$f":"((150*($J$2^0.87)*(AB49^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z49)*3600*24","v":8.3159327758853915E-2},2.3915996627248484E-4,{"$f":"AE48-AD49*Bodencharakterisierung!$E$8","v":6.3812037968395463E-2},{"$f":"IF(AE49>$J$18,(AE49/(Bodencharakterisierung!$E$11*1000)),0)","v":4.2120157074848493E-5},2.3305291073371062E-2,32,null,{"$f":"(AD49)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH49>0,(AJ49*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK48,NA())","v":6.8574872172024987E-2},null,32,{"$f":"IF(AF49<=$J$9*0.05,AS48*EXP((-$J$6*1)/Heterogenität!$D$4),Z49)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF49>=$J$19, AR48/$J$5<AN49),0, Bodencharakterisierung!$E$8*$J$11*((AR48/$J$5)-AN49))","v":0},0,{"$f":"AQ48-AP49*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ49/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,32,null,{"$f":"(AP49)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF49<=$J$9*1.05,(AV49*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW48,NA())","v":{"$error":"#N/A"}},23072.238162637354,165,3.6292993521720249,6.8574872172024987E-2,0,0.20072447999999993,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},42.120157074848493,23305.291073371063]
[null,"Trichlorethen",{"$f":"Schadstoffbelastung!E5","v":18.763919999999999},{"$f":"Schadstoffbelastung!U5*10^-6","v":6.7999999999999994E-4},{"$f":"Stoffdatenbank!R6","v":131},{"$f":"IFERROR(C50*1000/E50,0)","v":143.23603053435113},{"$f":"(F50/$F$62)","v":0.21767822206477899},{"$f":"G50>0.05","v":true},{"$f":"Stoffdatenbank!D6","v":2.7E-2},{"$f":"Stoffdatenbank!N6*10^-3","v":1},{"$f":"(Stoffdatenbank!J6*10^-3)*Bodencharakterisierung!$E$9","v":1.3000000000000002E-3},{"$f":"Sanierungsdesign!$E$4*10^-6","v":1.9999999999999998E-4},{"$f":"D50/L50","v":3.4},{"$f":"M50>1","v":true},{"$f":"N50*((M50^0.5)*K50)/((I50^1.2)*(J50^0.9))","v":0.18282950937845679},{"$f":"IF(O50=MAX($O$49:$O$61),\"Ja\",0)","v":0},{"$f":"Stoffdatenbank!Q6","v":1.4641999999999999},{"$f":"Stoffdatenbank!L6","v":8.08E-10},{"$f":"Schadstoffbelastung!X5*10^-6","v":8.8400000000000003E-7},{"$f":"Schadstoffbelastung!Y5*10^-6","v":1.0321188118811883E-5},{"$f":"Schadstoffbelastung!Z5*10^-6","v":9.4371881188118823E-6},{"$f":"Schadstoffbelastung!W5*10^-6","v":0.1997677548485135},{"$f":"Sanierungsdesign!M12","v":4.5801526717557252E-2},{"$f":"T50/K50","v":7.9393754760091403E-3},33,2.3305291073371062E-2,{"$f":"Z50*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF49*Bodencharakterisierung!$E$11/$J$20","v":4.4078208561931919E-5},{"$f":"((150*($J$2^0.87)*(AB50^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z50)*3600*24","v":8.3078164884360428E-2},2.3915996627248484E-4,{"$f":"AE49-AD50*Bodencharakterisierung!$E$8","v":6.373311517952554E-2},{"$f":"IF(AE50>$J$18,(AE50/(Bodencharakterisierung!$E$11*1000)),0)","v":4.2068062824769331E-5},2.3305291073371062E-2,33,null,{"$f":"(AD50)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH50>0,(AJ50*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK49,NA())","v":7.0742339427400769E-2},null,33,{"$f":"IF(AF50<=$J$9*0.05,AS49*EXP((-$J$6*1)/Heterogenität!$D$4),Z50)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF50>=$J$19, AR49/$J$5<AN50),0, Bodencharakterisierung!$E$8*$J$11*((AR49/$J$5)-AN50))","v":0},0,{"$f":"AQ49-AP50*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ50/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,33,null,{"$f":"(AP50)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF50<=$J$9*1.05,(AV50*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW49,NA())","v":{"$error":"#N/A"}},23072.238162637354,166,3.6377394594274004,7.0742339427400769E-2,0,0.20699711999999992,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},42.068062824769328,23305.291073371063]
[null,"cis-1,2-Dichlorethen",{"$f":"Schadstoffbelastung!E6","v":16.965},{"$f":"Schadstoffbelastung!U6*10^-6","v":1.2999999999999999E-3},{"$f":"Stoffdatenbank!R7","v":97},174.89690721649484,0.26579379270346992,true,{"$f":"Stoffdatenbank!D7","v":1.2E-2},{"$f":"Stoffdatenbank!N7*10^-3","v":3.5},{"$f":"(Stoffdatenbank!J7*10^-3)*Bodencharakterisierung!$E$9","v":5.0000000000000001E-4},{"$f":"Sanierungsdesign!$E$4*10^-6","v":1.9999999999999998E-4},6.5,true,8.3319747947817088E-2,0,{"$f":"Stoffdatenbank!Q7","v":1.2837000000000001},{"$f":"Stoffdatenbank!L7","v":8.9500000000000001E-10},{"$f":"Schadstoffbelastung!X6*10^-6","v":6.5000000000000002E-7},{"$f":"Schadstoffbelastung!Y6*10^-6","v":9.3316831683168317E-6},{"$f":"Schadstoffbelastung!Z6*10^-6","v":8.6816831683168312E-6},{"$f":"Schadstoffbelastung!W6*10^-6","v":1.8052087670930335},{"$f":"Sanierungsdesign!M13","v":4.1237113402061855E-2},1.8663366336633663E-2,34,2.3305291073371062E-2,{"$f":"Z51*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF50*Bodencharakterisierung!$E$11/$J$20","v":4.4023692591922908E-5},{"$f":"((150*($J$2^0.87)*(AB51^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z51)*3600*24","v":8.2996980926836106E-2},2.3915996627248484E-4,{"$f":"AE50-AD51*Bodencharakterisierung!$E$8","v":6.3654192390655617E-2},{"$f":"IF(AE51>$J$18,(AE51/(Bodencharakterisierung!$E$11*1000)),0)","v":4.2015968574690175E-5},2.3305291073371062E-2,34,null,{"$f":"(AD51)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH51>0,(AJ51*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK50,NA())","v":7.2909806682776551E-2},null,34,{"$f":"IF(AF51<=$J$9*0.05,AS50*EXP((-$J$6*1)/Heterogenität!$D$4),Z51)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF51>=$J$19, AR50/$J$5<AN51),0, Bodencharakterisierung!$E$8*$J$11*((AR50/$J$5)-AN51))","v":0},0,{"$f":"AQ50-AP51*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ51/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,34,null,{"$f":"(AP51)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF51<=$J$9*1.05,(AV51*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW50,NA())","v":{"$error":"#N/A"}},23072.238162637354,167,3.6461795666827763,7.2909806682776551E-2,0,0.21326975999999992,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},42.015968574690177,23305.291073371063]
[null,"trans-1,2-Dichlorethen",{"$f":"Schadstoffbelastung!E7","v":1.4868E-10},{"$f":"Schadstoffbelastung!U7*10^-6","v":1E-14},{"$f":"Stoffdatenbank!R8","v":97},1.5327835051546393E-9,2.3293970586001714E-12,false,{"$f":"Stoffdatenbank!D8","v":1.2E-2},{"$f":"Stoffdatenbank!N8*10^-3","v":6.3},{"$f":"(Stoffdatenbank!J8*10^-3)*Bodencharakterisierung!$E$9","v":5.9999999999999995E-4},{"$f":"Sanierungsdesign!$E$4*10^-6","v":1.9999999999999998E-4},5.0000000000000002E-11,false,0,0,{"$f":"Stoffdatenbank!Q8","v":1.2565},{"$f":"Stoffdatenbank!L8","v":8.8600000000000004E-10},{"$f":"Schadstoffbelastung!X7*10^-6","v":6.0000000000000012E-18},{"$f":"Schadstoffbelastung!Y7*10^-6","v":8.1782178217821796E-17},{"$f":"Schadstoffbelastung!Z7*10^-6","v":7.5782178217821785E-17},{"$f":"Schadstoffbelastung!W7*10^-6","v":2.4995198313595846E-11},{"$f":"Sanierungsdesign!M14","v":4.1237113402061855E-2},1.3630363036303634E-13,35,2.3305291073371062E-2,{"$f":"Z52*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF51*Bodencharakterisierung!$E$11/$J$20","v":4.3969176621913925E-5},{"$f":"((150*($J$2^0.87)*(AB52^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z52)*3600*24","v":8.2915775854686152E-2},2.3915996627248484E-4,{"$f":"AE51-AD52*Bodencharakterisierung!$E$8","v":6.3575269601785694E-2},{"$f":"IF(AE52>$J$18,(AE52/(Bodencharakterisierung!$E$11*1000)),0)","v":4.196387432461102E-5},2.3305291073371062E-2,35,null,{"$f":"(AD52)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH52>0,(AJ52*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK51,NA())","v":7.5077273938152334E-2},null,35,{"$f":"IF(AF52<=$J$9*0.05,AS51*EXP((-$J$6*1)/Heterogenität!$D$4),Z52)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF52>=$J$19, AR51/$J$5<AN52),0, Bodencharakterisierung!$E$8*$J$11*((AR51/$J$5)-AN52))","v":0},0,{"$f":"AQ51-AP52*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ52/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,35,null,{"$f":"(AP52)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF52<=$J$9*1.05,(AV52*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW51,NA())","v":{"$error":"#N/A"}},23072.238162637354,168,3.6546196739381522,7.5077273938152334E-2,0,0.21954239999999992,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},41.96387432461102,23305.291073371063]
[null,"1,1-Dichlorethen",{"$f":"Schadstoffbelastung!E8","v":1.6778718000000002E-10},{"$f":"Schadstoffbelastung!U8*10^-6","v":1E-14},{"$f":"Stoffdatenbank!R9","v":97},1.7297647422680414E-9,2.6287527815632065E-12,false,{"$f":"Stoffdatenbank!D9","v":1.2E-2},{"$f":"Stoffdatenbank!N9*10^-3","v":2.5},{"$f":"(Stoffdatenbank!J9*10^-3)*Bodencharakterisierung!$E$9","v":7.0510000000000006E-4},{"$f":"Sanierungsdesign!$E$4*10^-6","v":1.9999999999999998E-4},5.0000000000000002E-11,false,0,0,{"$f":"Stoffdatenbank!Q9","v":1.218},{"$f":"Stoffdatenbank!L9","v":1.173E-9},{"$f":"Schadstoffbelastung!X8*10^-6","v":7.0510000000000005E-18},{"$f":"Schadstoffbelastung!Y8*10^-6","v":9.2292178217821793E-17},{"$f":"Schadstoffbelastung!Z8*10^-6","v":8.524117821782179E-17},{"$f":"Schadstoffbelastung!W8*10^-6","v":9.9187294895221611E-12},{"$f":"Sanierungsdesign!M15","v":4.1237113402061855E-2},1.3089232480190298E-13,36,2.3305291073371062E-2,{"$f":"Z53*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF52*Bodencharakterisierung!$E$11/$J$20","v":4.3914660651904934E-5},{"$f":"((150*($J$2^0.87)*(AB53^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z53)*3600*24","v":8.2834549636229673E-2},2.3915996627248484E-4,{"$f":"AE52-AD53*Bodencharakterisierung!$E$8","v":6.3496346812915772E-2},{"$f":"IF(AE53>$J$18,(AE53/(Bodencharakterisierung!$E$11*1000)),0)","v":4.1911780074531865E-5},2.3305291073371062E-2,36,null,{"$f":"(AD53)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH53>0,(AJ53*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK52,NA())","v":7.7244741193528116E-2},null,36,{"$f":"IF(AF53<=$J$9*0.05,AS52*EXP((-$J$6*1)/Heterogenität!$D$4),Z53)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF53>=$J$19, AR52/$J$5<AN53),0, Bodencharakterisierung!$E$8*$J$11*((AR52/$J$5)-AN53))","v":0},0,{"$f":"AQ52-AP53*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ53/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,36,null,{"$f":"(AP53)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF53<=$J$9*1.05,(AV53*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW52,NA())","v":{"$error":"#N/A"}},23072.238162637354,169,3.6630597811935282,7.7244741193528116E-2,0,0.22581503999999991,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},41.911780074531862,23305.291073371063]
[null,"Vinylchlorid",{"$f":"Schadstoffbelastung!E9","v":2.9736000000000002},{"$f":"Schadstoffbelastung!U9*10^-6","v":1.9999999999999998E-4},{"$f":"Stoffdatenbank!R10","v":63},47.2,7.1730639582290992E-2,true,{"$f":"Stoffdatenbank!D10","v":1.7999999999999999E-2},{"$f":"Stoffdatenbank!N10*10^-3","v":1.1000000000000001},{"$f":"(Stoffdatenbank!J10*10^-3)*Bodencharakterisierung!$E$9","v":5.9999999999999995E-4},{"$f":"Sanierungsdesign!$E$4*10^-6","v":1.9999999999999998E-4},1,false,0,0,{"$f":"Stoffdatenbank!Q10","v":0.91210000000000002},{"$f":"Stoffdatenbank!L10","v":5.7799999999999997E-10},{"$f":"Schadstoffbelastung!X9*10^-6","v":1.1999999999999999E-7},{"$f":"Schadstoffbelastung!Y9*10^-6","v":1.6356435643564358E-6},{"$f":"Schadstoffbelastung!Z9*10^-6","v":1.5156435643564361E-6},{"$f":"Schadstoffbelastung!W9*10^-6","v":0.13439091257549393},{"$f":"Sanierungsdesign!M16","v":3.1746031746031744E-2},2.7260726072607265E-3,37,2.3305291073371062E-2,{"$f":"Z54*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF53*Bodencharakterisierung!$E$11/$J$20","v":4.3860144681895943E-5},{"$f":"((150*($J$2^0.87)*(AB54^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z54)*3600*24","v":8.2753302239698415E-2},2.3915996627248484E-4,{"$f":"AE53-AD54*Bodencharakterisierung!$E$8","v":6.3417424024045849E-2},{"$f":"IF(AE54>$J$18,(AE54/(Bodencharakterisierung!$E$11*1000)),0)","v":4.1859685824452703E-5},2.3305291073371062E-2,37,null,{"$f":"(AD54)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH54>0,(AJ54*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK53,NA())","v":7.9412208448903898E-2},null,37,{"$f":"IF(AF54<=$J$9*0.05,AS53*EXP((-$J$6*1)/Heterogenität!$D$4),Z54)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF54>=$J$19, AR53/$J$5<AN54),0, Bodencharakterisierung!$E$8*$J$11*((AR53/$J$5)-AN54))","v":0},0,{"$f":"AQ53-AP54*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ54/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,37,null,{"$f":"(AP54)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF54<=$J$9*1.05,(AV54*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW53,NA())","v":{"$error":"#N/A"}},23072.238162637354,170,3.6714998884489036,7.9412208448903898E-2,0,0.23208767999999991,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},41.859685824452704,23305.291073371063]
[null,"Tetrachlormethan",{"$f":"Schadstoffbelastung!E10","v":5.5882079999999999E-10},{"$f":"Schadstoffbelastung!U10*10^-6","v":1E-14},{"$f":"Stoffdatenbank!R11","v":154},3.6287064935064937E-9,5.5146067295685005E-12,false,{"$f":"Stoffdatenbank!D11","v":0.06},{"$f":"Stoffdatenbank!N11*10^-3","v":0.8},{"$f":"(Stoffdatenbank!J11*10^-3)*Bodencharakterisierung!$E$9","v":2.8560000000000005E-3},{"$f":"Sanierungsdesign!$E$4*10^-6","v":1.9999999999999998E-4},5.0000000000000002E-11,false,0,0,{"$f":"Stoffdatenbank!Q11","v":1.5940000000000001},{"$f":"Stoffdatenbank!L11","v":7.2929999999999995E-10},{"$f":"Schadstoffbelastung!X10*10^-6","v":2.8560000000000002E-17},{"$f":"Schadstoffbelastung!Y10*10^-6","v":3.0738217821782179E-16},{"$f":"Schadstoffbelastung!Z10*10^-6","v":2.7882217821782178E-16},{"$f":"Schadstoffbelastung!W10*10^-6","v":1.9992036581478436E-12},{"$f":"Sanierungsdesign!M17","v":5.1948051948051951E-2},1.076268131014782E-13,38,2.3305291073371062E-2,{"$f":"Z55*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF54*Bodencharakterisierung!$E$11/$J$20","v":4.3805628711886939E-5},{"$f":"((150*($J$2^0.87)*(AB55^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z55)*3600*24","v":8.2672033633237094E-2},2.3915996627248484E-4,{"$f":"AE54-AD55*Bodencharakterisierung!$E$8","v":6.3338501235175926E-2},{"$f":"IF(AE55>$J$18,(AE55/(Bodencharakterisierung!$E$11*1000)),0)","v":4.1807591574373548E-5},2.3305291073371062E-2,38,null,{"$f":"(AD55)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH55>0,(AJ55*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK54,NA())","v":8.1579675704279681E-2},null,38,{"$f":"IF(AF55<=$J$9*0.05,AS54*EXP((-$J$6*1)/Heterogenität!$D$4),Z55)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF55>=$J$19, AR54/$J$5<AN55),0, Bodencharakterisierung!$E$8*$J$11*((AR54/$J$5)-AN55))","v":0},0,{"$f":"AQ54-AP55*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ55/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,38,null,{"$f":"(AP55)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF55<=$J$9*1.05,(AV55*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW54,NA())","v":{"$error":"#N/A"}},23072.238162637354,171,3.6799399957042795,8.1579675704279681E-2,0,0.2383603199999999,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},41.807591574373546,23305.291073371063]
[null,"Trichlormethan",{"$f":"Schadstoffbelastung!E11","v":1.3269977999999999E-10},{"$f":"Schadstoffbelastung!U11*10^-6","v":1E-14},{"$f":"Stoffdatenbank!R12","v":119},1.1151242016806723E-9,1.6946731398357261E-12,false,{"$f":"Stoffdatenbank!D12","v":0.06},{"$f":"Stoffdatenbank!N12*10^-3","v":8.1999999999999993},{"$f":"(Stoffdatenbank!J12*10^-3)*Bodencharakterisierung!$E$9","v":5.1210000000000003E-4},{"$f":"Sanierungsdesign!$E$4*10^-6","v":1.9999999999999998E-4},5.0000000000000002E-11,false,0,0,{"$f":"Stoffdatenbank!Q12","v":1.4850000000000001},{"$f":"Stoffdatenbank!L12","v":8.245E-10},{"$f":"Schadstoffbelastung!X11*10^-6","v":5.1209999999999999E-18},{"$f":"Schadstoffbelastung!Y11*10^-6","v":7.299217821782178E-17},{"$f":"Schadstoffbelastung!Z11*10^-6","v":6.7871178217821778E-17},{"$f":"Schadstoffbelastung!W11*10^-6","v":2.6518848524255217E-11},{"$f":"Sanierungsdesign!M18","v":5.0420168067226892E-2},1.4253500921269631E-13,39,2.3305291073371062E-2,{"$f":"Z56*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF55*Bodencharakterisierung!$E$11/$J$20","v":4.3751112741877949E-5},{"$f":"((150*($J$2^0.87)*(AB56^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z56)*3600*24","v":8.2590743784902762E-2},2.3915996627248484E-4,{"$f":"AE55-AD56*Bodencharakterisierung!$E$8","v":6.3259578446306003E-2},{"$f":"IF(AE56>$J$18,(AE56/(Bodencharakterisierung!$E$11*1000)),0)","v":4.1755497324294393E-5},2.3305291073371062E-2,39,null,{"$f":"(AD56)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH56>0,(AJ56*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK55,NA())","v":8.3747142959655463E-2},null,39,{"$f":"IF(AF56<=$J$9*0.05,AS55*EXP((-$J$6*1)/Heterogenität!$D$4),Z56)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF56>=$J$19, AR55/$J$5<AN56),0, Bodencharakterisierung!$E$8*$J$11*((AR55/$J$5)-AN56))","v":0},0,{"$f":"AQ55-AP56*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ56/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,39,null,{"$f":"(AP56)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF56<=$J$9*1.05,(AV56*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW55,NA())","v":{"$error":"#N/A"}},23072.238162637354,172,3.6883801029596555,8.3747142959655463E-2,0,0.2446329599999999,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},41.755497324294396,23305.291073371063]
[null,"Dichlormethan",{"$f":"Schadstoffbelastung!E12","v":6.1688699999999995E-11},{"$f":"Schadstoffbelastung!U12*10^-6","v":1E-14},{"$f":"Stoffdatenbank!R13","v":85},7.2574941176470594E-10,1.1029336754735978E-12,false,{"$f":"Stoffdatenbank!D13","v":0.03},{"$f":"Stoffdatenbank!N13*10^-3","v":17.798999999999999},{"$f":"(Stoffdatenbank!J13*10^-3)*Bodencharakterisierung!$E$9","v":1.215E-4},{"$f":"Sanierungsdesign!$E$4*10^-6","v":1.9999999999999998E-4},5.0000000000000002E-11,false,0,0,{"$f":"Stoffdatenbank!Q13","v":1.3280000000000001},{"$f":"Stoffdatenbank!L13","v":9.8300000000000002E-10},{"$f":"Schadstoffbelastung!X12*10^-6","v":1.2149999999999999E-18},{"$f":"Schadstoffbelastung!Y12*10^-6","v":3.393217821782178E-17},{"$f":"Schadstoffbelastung!Z12*10^-6","v":3.2717178217821782E-17},{"$f":"Schadstoffbelastung!W12*10^-6","v":8.0586899858110501E-11},{"$f":"Sanierungsdesign!M19","v":4.7058823529411764E-2},2.7927718697795704E-13,40,2.3305291073371062E-2,{"$f":"Z57*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF56*Bodencharakterisierung!$E$11/$J$20","v":4.3696596771868965E-5},{"$f":"((150*($J$2^0.87)*(AB57^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z57)*3600*24","v":8.2509432662664334E-2},2.3915996627248484E-4,{"$f":"AE56-AD57*Bodencharakterisierung!$E$8","v":6.318065565743608E-2},{"$f":"IF(AE57>$J$18,(AE57/(Bodencharakterisierung!$E$11*1000)),0)","v":4.1703403074215237E-5},2.3305291073371062E-2,40,null,{"$f":"(AD57)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH57>0,(AJ57*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK56,NA())","v":8.5914610215031245E-2},null,40,{"$f":"IF(AF57<=$J$9*0.05,AS56*EXP((-$J$6*1)/Heterogenität!$D$4),Z57)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF57>=$J$19, AR56/$J$5<AN57),0, Bodencharakterisierung!$E$8*$J$11*((AR56/$J$5)-AN57))","v":0},0,{"$f":"AQ56-AP57*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ57/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,40,null,{"$f":"(AP57)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF57<=$J$9*1.05,(AV57*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW56,NA())","v":{"$error":"#N/A"}},23072.238162637354,173,3.6968202102150309,8.5914610215031245E-2,0,0.2509055999999999,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},41.703403074215238,23305.291073371063]
[null,"1,1,1-Trichlorethan",{"$f":"Schadstoffbelastung!E13","v":3.0139200000000002E-11},{"$f":"Schadstoffbelastung!U13*10^-6","v":1.0000000000000001E-15},{"$f":"Stoffdatenbank!R14","v":133.404},2.2592426014212468E-10,3.4334092536335797E-13,false,{"$f":"Stoffdatenbank!D14","v":0.01},{"$f":"Stoffdatenbank!N14*10^-3","v":1.3},{"$f":"(Stoffdatenbank!J14*10^-3)*Bodencharakterisierung!$E$9","v":1.4400000000000001E-3},{"$f":"Sanierungsdesign!$E$4*10^-6","v":1.9999999999999998E-4},5.0000000000000005E-12,false,0,0,{"$f":"Stoffdatenbank!Q14","v":1.339},{"$f":"Stoffdatenbank!L14","v":7.6099999999999996E-10},{"$f":"Schadstoffbelastung!X13*10^-6","v":1.4399999999999998E-18},{"$f":"Schadstoffbelastung!Y13*10^-6","v":1.6578217821782181E-17},{"$f":"Schadstoffbelastung!Z13*10^-6","v":1.513821782178218E-17},{"$f":"Schadstoffbelastung!W13*10^-6","v":3.7502677239925179E-13},{"$f":"Sanierungsdesign!M20","v":4.4976162633804086E-2},1.1512651265126514E-14,41,2.3305291073371062E-2,{"$f":"Z58*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF57*Bodencharakterisierung!$E$11/$J$20","v":4.3642080801859967E-5},{"$f":"((150*($J$2^0.87)*(AB58^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z58)*3600*24","v":8.2428100234402807E-2},2.3915996627248484E-4,{"$f":"AE57-AD58*Bodencharakterisierung!$E$8","v":6.3101732868566157E-2},{"$f":"IF(AE58>$J$18,(AE58/(Bodencharakterisierung!$E$11*1000)),0)","v":4.1651308824136075E-5},2.3305291073371062E-2,41,null,{"$f":"(AD58)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH58>0,(AJ58*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK57,NA())","v":8.8082077470407028E-2},null,41,{"$f":"IF(AF58<=$J$9*0.05,AS57*EXP((-$J$6*1)/Heterogenität!$D$4),Z58)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF58>=$J$19, AR57/$J$5<AN58),0, Bodencharakterisierung!$E$8*$J$11*((AR57/$J$5)-AN58))","v":0},0,{"$f":"AQ57-AP58*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ58/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,41,null,{"$f":"(AP58)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF58<=$J$9*1.05,(AV58*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW57,NA())","v":{"$error":"#N/A"}},23072.238162637354,174,3.7052603174704069,8.8082077470407028E-2,0,0.25717823999999989,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},41.651308824136073,23305.291073371063]
[null,"1,1,2-Trichlorethan",{"$f":"Schadstoffbelastung!E14","v":1.1893752E-10},{"$f":"Schadstoffbelastung!U14*10^-6","v":1E-14},{"$f":"Stoffdatenbank!R15","v":133.404},8.9155887379688764E-10,1.3549171237863942E-12,false,{"$f":"Stoffdatenbank!D15","v":0.01},{"$f":"Stoffdatenbank!N15*10^-3","v":4.5},{"$f":"(Stoffdatenbank!J15*10^-3)*Bodencharakterisierung!$E$9","v":4.3639999999999998E-4},{"$f":"Sanierungsdesign!$E$4*10^-6","v":1.9999999999999998E-4},5.0000000000000002E-11,false,0,0,{"$f":"Stoffdatenbank!Q15","v":1.4410000000000001},{"$f":"Stoffdatenbank!L15","v":6.8000000000000003E-10},{"$f":"Schadstoffbelastung!X14*10^-6","v":4.364E-18},{"$f":"Schadstoffbelastung!Y14*10^-6","v":6.5422178217821788E-17},{"$f":"Schadstoffbelastung!Z14*10^-6","v":6.1058178217821795E-17},{"$f":"Schadstoffbelastung!W14*10^-6","v":1.298169596766641E-11},{"$f":"Sanierungsdesign!M21","v":4.4976162633804086E-2},1.499133323048162E-13,42,2.3305291073371062E-2,{"$f":"Z59*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF58*Bodencharakterisierung!$E$11/$J$20","v":4.358756483185097E-5},{"$f":"((150*($J$2^0.87)*(AB59^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z59)*3600*24","v":8.2346746467909751E-2},2.3915996627248484E-4,{"$f":"AE58-AD59*Bodencharakterisierung!$E$8","v":6.3022810079696234E-2},{"$f":"IF(AE59>$J$18,(AE59/(Bodencharakterisierung!$E$11*1000)),0)","v":4.159921457405692E-5},2.3305291073371062E-2,42,null,{"$f":"(AD59)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH59>0,(AJ59*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK58,NA())","v":9.024954472578281E-2},null,42,{"$f":"IF(AF59<=$J$9*0.05,AS58*EXP((-$J$6*1)/Heterogenität!$D$4),Z59)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF59>=$J$19, AR58/$J$5<AN59),0, Bodencharakterisierung!$E$8*$J$11*((AR58/$J$5)-AN59))","v":0},0,{"$f":"AQ58-AP59*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ59/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,42,null,{"$f":"(AP59)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF59<=$J$9*1.05,(AV59*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW58,NA())","v":{"$error":"#N/A"}},23072.238162637354,175,3.7137004247257828,9.024954472578281E-2,0,0.26345087999999989,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},41.599214574056923,23305.291073371063]
[null,"1,1-Dichlorethan",{"$f":"Schadstoffbelastung!E15","v":1.0457532E-10},{"$f":"Schadstoffbelastung!U15*10^-6","v":1E-14},{"$f":"Stoffdatenbank!R16","v":98.96},1.0567433306386419E-9,1.6059507411235209E-12,false,{"$f":"Stoffdatenbank!D16","v":6.5000000000000006E-3},{"$f":"Stoffdatenbank!N16*10^-3","v":8.69},{"$f":"(Stoffdatenbank!J16*10^-3)*Bodencharakterisierung!$E$9","v":3.5740000000000001E-4},{"$f":"Sanierungsdesign!$E$4*10^-6","v":1.9999999999999998E-4},5.0000000000000002E-11,false,0,0,{"$f":"Stoffdatenbank!Q16","v":1.2350000000000001},{"$f":"Stoffdatenbank!L16","v":1.14E-9},{"$f":"Schadstoffbelastung!X15*10^-6","v":3.5740000000000004E-18},{"$f":"Schadstoffbelastung!Y15*10^-6","v":5.7522178217821785E-17},{"$f":"Schadstoffbelastung!Z15*10^-6","v":5.3948178217821782E-17},{"$f":"Schadstoffbelastung!W15*10^-6","v":3.3794642880367484E-11},{"$f":"Sanierungsdesign!M22","v":4.0420371867421187E-2},1.6094621773313312E-13,43,2.3305291073371062E-2,{"$f":"Z60*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF59*Bodencharakterisierung!$E$11/$J$20","v":4.3533048861841979E-5},{"$f":"((150*($J$2^0.87)*(AB60^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z60)*3600*24","v":8.2265371330888751E-2},2.3915996627248484E-4,{"$f":"AE59-AD60*Bodencharakterisierung!$E$8","v":6.2943887290826311E-2},{"$f":"IF(AE60>$J$18,(AE60/(Bodencharakterisierung!$E$11*1000)),0)","v":4.1547120323977765E-5},2.3305291073371062E-2,43,null,{"$f":"(AD60)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH60>0,(AJ60*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK59,NA())","v":9.2417011981158592E-2},null,43,{"$f":"IF(AF60<=$J$9*0.05,AS59*EXP((-$J$6*1)/Heterogenität!$D$4),Z60)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF60>=$J$19, AR59/$J$5<AN60),0, Bodencharakterisierung!$E$8*$J$11*((AR59/$J$5)-AN60))","v":0},0,{"$f":"AQ59-AP60*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ60/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,43,null,{"$f":"(AP60)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF60<=$J$9*1.05,(AV60*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW59,NA())","v":{"$error":"#N/A"}},23072.238162637354,176,3.7221405319811582,9.2417011981158592E-2,0,0.26972351999999988,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},41.547120323977765,23305.291073371063]
[null,"1,2-Dichlorethan",{"$f":"Schadstoffbelastung!E16","v":1.115928E-10},{"$f":"Schadstoffbelastung!U16*10^-6","v":1E-14},{"$f":"Stoffdatenbank!R17","v":98.96},1.1276556184316897E-9,1.7137173461582412E-12,false,{"$f":"Stoffdatenbank!D17","v":6.5000000000000006E-3},{"$f":"Stoffdatenbank!N17*10^-3","v":8.69},{"$f":"(Stoffdatenbank!J17*10^-3)*Bodencharakterisierung!$E$9","v":3.9600000000000003E-4},{"$f":"Sanierungsdesign!$E$4*10^-6","v":1.9999999999999998E-4},5.0000000000000002E-11,false,0,0,1.25,{"$f":"Stoffdatenbank!L17","v":9.2000000000000003E-10},{"$f":"Schadstoffbelastung!X16*10^-6","v":3.9600000000000005E-18},{"$f":"Schadstoffbelastung!Y16*10^-6","v":6.1382178217821788E-17},{"$f":"Schadstoffbelastung!Z16*10^-6","v":5.7422178217821793E-17},{"$f":"Schadstoffbelastung!W16*10^-6","v":3.3794642880367484E-11},{"$f":"Sanierungsdesign!M23","v":4.0420371867421187E-2},1.55005500550055E-13,44,2.3305291073371062E-2,{"$f":"Z61*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF60*Bodencharakterisierung!$E$11/$J$20","v":4.3478532891832989E-5},{"$f":"((150*($J$2^0.87)*(AB61^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z61)*3600*24","v":8.2183974790952852E-2},2.3915996627248484E-4,{"$f":"AE60-AD61*Bodencharakterisierung!$E$8","v":6.2864964501956389E-2},{"$f":"IF(AE61>$J$18,(AE61/(Bodencharakterisierung!$E$11*1000)),0)","v":4.149502607389861E-5},2.3305291073371062E-2,44,null,{"$f":"(AD61)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH61>0,(AJ61*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK60,NA())","v":9.4584479236534375E-2},null,44,{"$f":"IF(AF61<=$J$9*0.05,AS60*EXP((-$J$6*1)/Heterogenität!$D$4),Z61)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF61>=$J$19, AR60/$J$5<AN61),0, Bodencharakterisierung!$E$8*$J$11*((AR60/$J$5)-AN61))","v":0},0,{"$f":"AQ60-AP61*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ61/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,44,null,{"$f":"(AP61)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF61<=$J$9*1.05,(AV61*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW60,NA())","v":{"$error":"#N/A"}},23072.238162637354,177,3.7305806392365342,9.4584479236534375E-2,0,0.27599615999999988,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},41.495026073898607,23305.291073371063]
[null,"Summe LCKW",null,{"$f":"SUM(D49:D61)","v":2.8800000000809988E-3},null,{"$f":"SUM(F49:F61)","v":658.01727511227762},{"$f":"SUM(G49:G61)","v":1},true,{"$f":"(I49*G49)+(I50*G50)+(I51*G51)+(I52*G52)+(I53*G53)+(I54*G54)+(I55*G55)+(I56*G56)+(I57*G57)+(I58*G58)+(I59*G59)+(I60*G60)+(I61*G61)","v":2.2812314698908428E-2},{"$f":"(J49*G49)+(J50*G50)+(J51*G51)+(J52*G52)+(J53*G53)+(J54*G54)+(J55*G55)+(J56*G56)+(J57*G57)+(J58*G58)+(J59*G59)+(J60*G60)+(J61*G61)","v":1.2980277754630087},{"$f":"(K49*G49)+(K50*G50)+(K51*G51)+(K52*G52)+(K53*G53)+(K54*G54)+(K55*G55)+(K56*G56)+(K57*G57)+(K58*G58)+(K59*G59)+(K60*G60)+(K61*G61)","v":2.0601874130798813E-3},{"$f":"Sanierungsdesign!$E$4*10^-6","v":1.9999999999999998E-4},14.400000000404996,true,null,0,{"$f":"(Q49*$G$49)+(Q50*$G$50)+(Q51*$G$51)+(Q52*$G$52)+(Q53*$G$53)+(Q54*$G$54)+(Q55*$G$55)+(Q56*$G$56)+(Q57*$G$57)+(Q58*$G$58)+(Q59*$G$59)+(Q60*$G$60)+(Q61*$G$61)","v":1.4477003501341623},{"$f":"(R49*$G$49)+(R50*$G$50)+(R51*$G$51)+(R52*$G$52)+(R53*$G$53)+(R54*$G$54)+(R55*$G$55)+(R56*$G$56)+(R57*$G$57)+(R58*$G$58)+(R59*$G$59)+(R60*$G$60)+(R61*$G$61)","v":7.8838296947049937E-10},{"$f":"SUM(S49:S61)","v":4.1740000000612839E-6},{"$f":"SUM(T49:T61)","v":4.8013267327521979E-5},{"$f":"SUM(U49:U61)","v":4.3839267327460676E-5},{"$f":"SUM(V49:V61)","v":2.1653329955068661},{"$f":"AVERAGE(W49:W61)","v":4.3820906330865619E-2},{"$f":"T62/K62","v":2.3305291073371062E-2},45,2.3305291073371062E-2,{"$f":"Z62*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF61*Bodencharakterisierung!$E$11/$J$20","v":4.3424016921823991E-5},{"$f":"((150*($J$2^0.87)*(AB62^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z62)*3600*24","v":8.2102556815626365E-2},2.3915996627248484E-4,{"$f":"AE61-AD62*Bodencharakterisierung!$E$8","v":6.2786041713086466E-2},{"$f":"IF(AE62>$J$18,(AE62/(Bodencharakterisierung!$E$11*1000)),0)","v":4.1442931823819448E-5},2.3305291073371062E-2,45,null,{"$f":"(AD62)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH62>0,(AJ62*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK61,NA())","v":9.6751946491910157E-2},null,45,{"$f":"IF(AF62<=$J$9*0.05,AS61*EXP((-$J$6*1)/Heterogenität!$D$4),Z62)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF62>=$J$19, AR61/$J$5<AN62),0, Bodencharakterisierung!$E$8*$J$11*((AR61/$J$5)-AN62))","v":0},0,{"$f":"AQ61-AP62*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ62/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,45,null,{"$f":"(AP62)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF62<=$J$9*1.05,(AV62*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW61,NA())","v":{"$error":"#N/A"}},23072.238162637354,178,3.7390207464919101,9.6751946491910157E-2,0,0.28226879999999988,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},41.44293182381945,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,46,2.3305291073371062E-2,{"$f":"Z63*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF62*Bodencharakterisierung!$E$11/$J$20","v":4.3369500951814994E-5},{"$f":"((150*($J$2^0.87)*(AB63^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z63)*3600*24","v":8.2021117372342689E-2},2.3915996627248484E-4,{"$f":"AE62-AD63*Bodencharakterisierung!$E$8","v":6.2707118924216543E-2},{"$f":"IF(AE63>$J$18,(AE63/(Bodencharakterisierung!$E$11*1000)),0)","v":4.1390837573740292E-5},2.3305291073371062E-2,46,null,{"$f":"(AD63)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH63>0,(AJ63*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK62,NA())","v":9.8919413747285939E-2},null,46,{"$f":"IF(AF63<=$J$9*0.05,AS62*EXP((-$J$6*1)/Heterogenität!$D$4),Z63)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF63>=$J$19, AR62/$J$5<AN63),0, Bodencharakterisierung!$E$8*$J$11*((AR62/$J$5)-AN63))","v":0},0,{"$f":"AQ62-AP63*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ63/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,46,null,{"$f":"(AP63)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF63<=$J$9*1.05,(AV63*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW62,NA())","v":{"$error":"#N/A"}},23072.238162637354,179,3.7474608537472855,9.8919413747285939E-2,0,0.28854143999999987,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},41.390837573740292,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,47,2.3305291073371062E-2,{"$f":"Z64*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF63*Bodencharakterisierung!$E$11/$J$20","v":4.3314984981806003E-5},{"$f":"((150*($J$2^0.87)*(AB64^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z64)*3600*24","v":8.1939656428445223E-2},2.3915996627248484E-4,{"$f":"AE63-AD64*Bodencharakterisierung!$E$8","v":6.262819613534662E-2},{"$f":"IF(AE64>$J$18,(AE64/(Bodencharakterisierung!$E$11*1000)),0)","v":4.1338743323661137E-5},2.3305291073371062E-2,47,null,{"$f":"(AD64)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH64>0,(AJ64*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK63,NA())","v":0.10108688100266172},null,47,{"$f":"IF(AF64<=$J$9*0.05,AS63*EXP((-$J$6*1)/Heterogenität!$D$4),Z64)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF64>=$J$19, AR63/$J$5<AN64),0, Bodencharakterisierung!$E$8*$J$11*((AR63/$J$5)-AN64))","v":0},0,{"$f":"AQ63-AP64*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ64/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,47,null,{"$f":"(AP64)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF64<=$J$9*1.05,(AV64*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW63,NA())","v":{"$error":"#N/A"}},23072.238162637354,180,3.7559009610026615,0.10108688100266172,0,0.29481407999999987,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},41.338743323661134,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,48,2.3305291073371062E-2,{"$f":"Z65*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF64*Bodencharakterisierung!$E$11/$J$20","v":4.326046901179702E-5},{"$f":"((150*($J$2^0.87)*(AB65^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z65)*3600*24","v":8.1858173951186275E-2},2.3915996627248484E-4,{"$f":"AE64-AD65*Bodencharakterisierung!$E$8","v":6.2549273346476697E-2},{"$f":"IF(AE65>$J$18,(AE65/(Bodencharakterisierung!$E$11*1000)),0)","v":4.1286649073581975E-5},2.3305291073371062E-2,48,null,{"$f":"(AD65)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH65>0,(AJ65*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK64,NA())","v":0.1032543482580375},null,48,{"$f":"IF(AF65<=$J$9*0.05,AS64*EXP((-$J$6*1)/Heterogenität!$D$4),Z65)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF65>=$J$19, AR64/$J$5<AN65),0, Bodencharakterisierung!$E$8*$J$11*((AR64/$J$5)-AN65))","v":0},0,{"$f":"AQ64-AP65*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ65/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,48,null,{"$f":"(AP65)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF65<=$J$9*1.05,(AV65*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW64,NA())","v":{"$error":"#N/A"}},23072.238162637354,181,3.7643410682580374,0.1032543482580375,0,0.30108671999999986,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},41.286649073581977,23305.291073371063]
[null,"Verwendetes Substrat",null,"Stöch. Faktor",{"$f":"VLOOKUP($C$31,$B$70:$E$79,4,FALSE)","v":90.1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,49,2.3305291073371062E-2,{"$f":"Z66*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF65*Bodencharakterisierung!$E$11/$J$20","v":4.3205953041788022E-5},{"$f":"((150*($J$2^0.87)*(AB66^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z66)*3600*24","v":8.1776669907727251E-2},2.3915996627248484E-4,{"$f":"AE65-AD66*Bodencharakterisierung!$E$8","v":6.2470350557606774E-2},{"$f":"IF(AE66>$J$18,(AE66/(Bodencharakterisierung!$E$11*1000)),0)","v":4.123455482350282E-5},2.3305291073371062E-2,49,null,{"$f":"(AD66)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH66>0,(AJ66*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK65,NA())","v":0.10542181551341329},null,49,{"$f":"IF(AF66<=$J$9*0.05,AS65*EXP((-$J$6*1)/Heterogenität!$D$4),Z66)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF66>=$J$19, AR65/$J$5<AN66),0, Bodencharakterisierung!$E$8*$J$11*((AR65/$J$5)-AN66))","v":0},0,{"$f":"AQ65-AP66*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ66/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,49,null,{"$f":"(AP66)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF66<=$J$9*1.05,(AV66*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW65,NA())","v":{"$error":"#N/A"}},23072.238162637354,182,3.7727811755134129,0.10542181551341329,0,0.30735935999999986,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},41.234554823502819,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50,2.3305291073371062E-2,{"$f":"Z67*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF66*Bodencharakterisierung!$E$11/$J$20","v":4.3151437071779025E-5},{"$f":"((150*($J$2^0.87)*(AB67^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z67)*3600*24","v":8.1695144265137576E-2},2.3915996627248484E-4,{"$f":"AE66-AD67*Bodencharakterisierung!$E$8","v":6.2391427768736851E-2},{"$f":"IF(AE67>$J$18,(AE67/(Bodencharakterisierung!$E$11*1000)),0)","v":4.1182460573423665E-5},2.3305291073371062E-2,50,null,{"$f":"(AD67)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH67>0,(AJ67*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK66,NA())","v":0.10758928276878907},null,50,{"$f":"IF(AF67<=$J$9*0.05,AS66*EXP((-$J$6*1)/Heterogenität!$D$4),Z67)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF67>=$J$19, AR66/$J$5<AN67),0, Bodencharakterisierung!$E$8*$J$11*((AR66/$J$5)-AN67))","v":0},0,{"$f":"AQ66-AP67*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ67/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,50,null,{"$f":"(AP67)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF67<=$J$9*1.05,(AV67*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW66,NA())","v":{"$error":"#N/A"}},23072.238162637354,183,3.7812212827687888,0.10758928276878907,0,0.31363199999999986,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},41.182460573423661,23305.291073371063]
[null,null,"Molmasse Substrat g/mol ","H2 Bildung mol / mol Substrat","Gramm Substrat / 1 Gramm H2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,51,2.3305291073371062E-2,{"$f":"Z68*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF67*Bodencharakterisierung!$E$11/$J$20","v":4.3096921101770034E-5},{"$f":"((150*($J$2^0.87)*(AB68^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z68)*3600*24","v":8.1613596990394888E-2},2.3915996627248484E-4,{"$f":"AE67-AD68*Bodencharakterisierung!$E$8","v":6.2312504979866928E-2},{"$f":"IF(AE68>$J$18,(AE68/(Bodencharakterisierung!$E$11*1000)),0)","v":4.1130366323344509E-5},2.3305291073371062E-2,51,null,{"$f":"(AD68)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH68>0,(AJ68*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK67,NA())","v":0.10975675002416485},null,51,{"$f":"IF(AF68<=$J$9*0.05,AS67*EXP((-$J$6*1)/Heterogenität!$D$4),Z68)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF68>=$J$19, AR67/$J$5<AN68),0, Bodencharakterisierung!$E$8*$J$11*((AR67/$J$5)-AN68))","v":0},0,{"$f":"AQ67-AP68*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ68/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,51,null,{"$f":"(AP68)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF68<=$J$9*1.05,(AV68*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW67,NA())","v":{"$error":"#N/A"}},23072.238162637354,184,3.7896613900241647,0.10975675002416485,0,0.31990463999999985,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},41.130366323344511,23305.291073371063]
[null,"Elektronendonator (ED)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,52,2.3305291073371062E-2,{"$f":"Z69*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF68*Bodencharakterisierung!$E$11/$J$20","v":4.3042405131761044E-5},{"$f":"((150*($J$2^0.87)*(AB69^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z69)*3600*24","v":8.153202805038455E-2},2.3915996627248484E-4,{"$f":"AE68-AD69*Bodencharakterisierung!$E$8","v":6.2233582190997006E-2},{"$f":"IF(AE69>$J$18,(AE69/(Bodencharakterisierung!$E$11*1000)),0)","v":4.1078272073265347E-5},2.3305291073371062E-2,52,null,{"$f":"(AD69)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH69>0,(AJ69*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK68,NA())","v":0.11192421727954063},null,52,{"$f":"IF(AF69<=$J$9*0.05,AS68*EXP((-$J$6*1)/Heterogenität!$D$4),Z69)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF69>=$J$19, AR68/$J$5<AN69),0, Bodencharakterisierung!$E$8*$J$11*((AR68/$J$5)-AN69))","v":0},0,{"$f":"AQ68-AP69*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ69/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,52,null,{"$f":"(AP69)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF69<=$J$9*1.05,(AV69*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW68,NA())","v":{"$error":"#N/A"}},23072.238162637354,185,3.7981014972795402,0.11192421727954063,0,0.32617727999999985,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},41.078272073265346,23305.291073371063]
[null,"Wasserstoff",2,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,53,2.3305291073371062E-2,{"$f":"Z70*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF69*Bodencharakterisierung!$E$11/$J$20","v":4.2987889161752046E-5},{"$f":"((150*($J$2^0.87)*(AB70^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z70)*3600*24","v":8.1450437411899182E-2},2.3915996627248484E-4,{"$f":"AE69-AD70*Bodencharakterisierung!$E$8","v":6.2154659402127083E-2},{"$f":"IF(AE70>$J$18,(AE70/(Bodencharakterisierung!$E$11*1000)),0)","v":4.1026177823186192E-5},2.3305291073371062E-2,53,null,{"$f":"(AD70)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH70>0,(AJ70*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK69,NA())","v":0.11409168453491642},null,53,{"$f":"IF(AF70<=$J$9*0.05,AS69*EXP((-$J$6*1)/Heterogenität!$D$4),Z70)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF70>=$J$19, AR69/$J$5<AN70),0, Bodencharakterisierung!$E$8*$J$11*((AR69/$J$5)-AN70))","v":0},0,{"$f":"AQ69-AP70*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ70/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,53,null,{"$f":"(AP70)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF70<=$J$9*1.05,(AV70*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW69,NA())","v":{"$error":"#N/A"}},23072.238162637354,186,3.8065416045349161,0.11409168453491642,0,0.33244991999999984,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},41.026177823186195,23305.291073371063]
[null,"Acetat",60.1,4,30.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,54,2.3305291073371062E-2,{"$f":"Z71*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF70*Bodencharakterisierung!$E$11/$J$20","v":4.2933373191743049E-5},{"$f":"((150*($J$2^0.87)*(AB71^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z71)*3600*24","v":8.1368825041638462E-2},2.3915996627248484E-4,{"$f":"AE70-AD71*Bodencharakterisierung!$E$8","v":6.207573661325716E-2},{"$f":"IF(AE71>$J$18,(AE71/(Bodencharakterisierung!$E$11*1000)),0)","v":4.0974083573107037E-5},2.3305291073371062E-2,54,null,{"$f":"(AD71)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH71>0,(AJ71*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK70,NA())","v":0.1162591517902922},null,54,{"$f":"IF(AF71<=$J$9*0.05,AS70*EXP((-$J$6*1)/Heterogenität!$D$4),Z71)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF71>=$J$19, AR70/$J$5<AN71),0, Bodencharakterisierung!$E$8*$J$11*((AR70/$J$5)-AN71))","v":0},0,{"$f":"AQ70-AP71*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ71/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,54,null,{"$f":"(AP71)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF71<=$J$9*1.05,(AV71*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW70,NA())","v":{"$error":"#N/A"}},23072.238162637354,187,3.814981711790292,0.1162591517902922,0,0.33872255999999984,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},40.974083573107038,23305.291073371063]
[null,"Ethanol",46.1,6,23.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,2.3305291073371062E-2,{"$f":"Z72*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF71*Bodencharakterisierung!$E$11/$J$20","v":4.2878857221734065E-5},{"$f":"((150*($J$2^0.87)*(AB72^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z72)*3600*24","v":8.1287190906208229E-2},2.3915996627248484E-4,{"$f":"AE71-AD72*Bodencharakterisierung!$E$8","v":6.1996813824387237E-2},{"$f":"IF(AE72>$J$18,(AE72/(Bodencharakterisierung!$E$11*1000)),0)","v":4.0921989323027882E-5},2.3305291073371062E-2,55,null,{"$f":"(AD72)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH72>0,(AJ72*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK71,NA())","v":0.11842661904566798},null,55,{"$f":"IF(AF72<=$J$9*0.05,AS71*EXP((-$J$6*1)/Heterogenität!$D$4),Z72)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF72>=$J$19, AR71/$J$5<AN72),0, Bodencharakterisierung!$E$8*$J$11*((AR71/$J$5)-AN72))","v":0},0,{"$f":"AQ71-AP72*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ72/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,55,null,{"$f":"(AP72)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF72<=$J$9*1.05,(AV72*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW71,NA())","v":{"$error":"#N/A"}},23072.238162637354,188,3.8234218190456675,0.11842661904566798,0,0.34499519999999984,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},40.92198932302788,23305.291073371063]
[null,"Laktat",90.1,6,45.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56,2.3305291073371062E-2,{"$f":"Z73*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF72*Bodencharakterisierung!$E$11/$J$20","v":4.2824341251725075E-5},{"$f":"((150*($J$2^0.87)*(AB73^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z73)*3600*24","v":8.1205534972120838E-2},2.3915996627248484E-4,{"$f":"AE72-AD73*Bodencharakterisierung!$E$8","v":6.1917891035517314E-2},{"$f":"IF(AE73>$J$18,(AE73/(Bodencharakterisierung!$E$11*1000)),0)","v":4.086989507294872E-5},2.3305291073371062E-2,56,null,{"$f":"(AD73)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH73>0,(AJ73*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK72,NA())","v":0.12059408630104376},null,56,{"$f":"IF(AF73<=$J$9*0.05,AS72*EXP((-$J$6*1)/Heterogenität!$D$4),Z73)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF73>=$J$19, AR72/$J$5<AN73),0, Bodencharakterisierung!$E$8*$J$11*((AR72/$J$5)-AN73))","v":0},0,{"$f":"AQ72-AP73*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ73/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,56,null,{"$f":"(AP73)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF73<=$J$9*1.05,(AV73*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW72,NA())","v":{"$error":"#N/A"}},23072.238162637354,189,3.8318619263010434,0.12059408630104376,0,0.35126783999999983,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},40.869895072948722,23305.291073371063]
[null,"Glucose",180.2,12,90.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57,2.3305291073371062E-2,{"$f":"Z74*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF73*Bodencharakterisierung!$E$11/$J$20","v":4.2769825281716077E-5},{"$f":"((150*($J$2^0.87)*(AB74^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z74)*3600*24","v":8.1123857205794236E-2},2.3915996627248484E-4,{"$f":"AE73-AD74*Bodencharakterisierung!$E$8","v":6.1838968246647391E-2},{"$f":"IF(AE74>$J$18,(AE74/(Bodencharakterisierung!$E$11*1000)),0)","v":4.0817800822869565E-5},2.3305291073371062E-2,57,null,{"$f":"(AD74)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH74>0,(AJ74*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK73,NA())","v":0.12276155355641954},null,57,{"$f":"IF(AF74<=$J$9*0.05,AS73*EXP((-$J$6*1)/Heterogenität!$D$4),Z74)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF74>=$J$19, AR73/$J$5<AN74),0, Bodencharakterisierung!$E$8*$J$11*((AR73/$J$5)-AN74))","v":0},0,{"$f":"AQ73-AP74*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ74/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,57,null,{"$f":"(AP74)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF74<=$J$9*1.05,(AV74*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW73,NA())","v":{"$error":"#N/A"}},23072.238162637354,190,3.8403020335564193,0.12276155355641954,0,0.35754047999999983,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},40.817800822869565,23305.291073371063]
[null,"Sojaöl",873.1,165.5,436.55,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58,2.3305291073371062E-2,{"$f":"Z75*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF74*Bodencharakterisierung!$E$11/$J$20","v":4.271530931170708E-5},{"$f":"((150*($J$2^0.87)*(AB75^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z75)*3600*24","v":8.1042157573551835E-2},2.3915996627248484E-4,{"$f":"AE74-AD75*Bodencharakterisierung!$E$8","v":6.1760045457777468E-2},{"$f":"IF(AE75>$J$18,(AE75/(Bodencharakterisierung!$E$11*1000)),0)","v":4.0765706572790409E-5},2.3305291073371062E-2,58,null,{"$f":"(AD75)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH75>0,(AJ75*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK74,NA())","v":0.12492902081179533},null,58,{"$f":"IF(AF75<=$J$9*0.05,AS74*EXP((-$J$6*1)/Heterogenität!$D$4),Z75)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF75>=$J$19, AR74/$J$5<AN75),0, Bodencharakterisierung!$E$8*$J$11*((AR74/$J$5)-AN75))","v":0},0,{"$f":"AQ74-AP75*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ75/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,58,null,{"$f":"(AP75)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF75<=$J$9*1.05,(AV75*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW74,NA())","v":{"$error":"#N/A"}},23072.238162637354,191,3.8487421408117948,0.12492902081179533,0,0.36381311999999982,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},40.765706572790407,23305.291073371063]
[null,"Palmöl",848.5,152.80000000000001,424.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59,2.3305291073371062E-2,{"$f":"Z76*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF75*Bodencharakterisierung!$E$11/$J$20","v":4.2660793341698089E-5},{"$f":"((150*($J$2^0.87)*(AB76^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z76)*3600*24","v":8.0960436041622216E-2},2.3915996627248484E-4,{"$f":"AE75-AD76*Bodencharakterisierung!$E$8","v":6.1681122668907545E-2},{"$f":"IF(AE76>$J$18,(AE76/(Bodencharakterisierung!$E$11*1000)),0)","v":4.0713612322711254E-5},2.3305291073371062E-2,59,null,{"$f":"(AD76)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH76>0,(AJ76*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK75,NA())","v":0.12709648806717111},null,59,{"$f":"IF(AF76<=$J$9*0.05,AS75*EXP((-$J$6*1)/Heterogenität!$D$4),Z76)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF76>=$J$19, AR75/$J$5<AN76),0, Bodencharakterisierung!$E$8*$J$11*((AR75/$J$5)-AN76))","v":0},0,{"$f":"AQ75-AP76*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ76/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,59,null,{"$f":"(AP76)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF76<=$J$9*1.05,(AV76*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW75,NA())","v":{"$error":"#N/A"}},23072.238162637354,192,3.8571822480671707,0.12709648806717111,0,0.37008575999999982,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},40.713612322711256,23305.291073371063]
[null,"Rapsöl",884.6,159.30000000000001,442.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60,2.3305291073371062E-2,{"$f":"Z77*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF76*Bodencharakterisierung!$E$11/$J$20","v":4.2606277371689105E-5},{"$f":"((150*($J$2^0.87)*(AB77^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z77)*3600*24","v":8.087869257613807E-2},2.3915996627248484E-4,{"$f":"AE76-AD77*Bodencharakterisierung!$E$8","v":6.1602199880037622E-2},{"$f":"IF(AE77>$J$18,(AE77/(Bodencharakterisierung!$E$11*1000)),0)","v":4.0661518072632092E-5},2.3305291073371062E-2,60,null,{"$f":"(AD77)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH77>0,(AJ77*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK76,NA())","v":0.12926395532254689},null,60,{"$f":"IF(AF77<=$J$9*0.05,AS76*EXP((-$J$6*1)/Heterogenität!$D$4),Z77)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF77>=$J$19, AR76/$J$5<AN77),0, Bodencharakterisierung!$E$8*$J$11*((AR76/$J$5)-AN77))","v":0},0,{"$f":"AQ76-AP77*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ77/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,60,null,{"$f":"(AP77)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF77<=$J$9*1.05,(AV77*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW76,NA())","v":{"$error":"#N/A"}},23072.238162637354,193,3.8656223553225466,0.12926395532254689,0,0.37635839999999982,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},40.661518072632092,23305.291073371063]
[null,"Biomasse",113.1,10,56.55,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,61,2.3305291073371062E-2,{"$f":"Z78*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF77*Bodencharakterisierung!$E$11/$J$20","v":4.2551761401680108E-5},{"$f":"((150*($J$2^0.87)*(AB78^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z78)*3600*24","v":8.0796927143136951E-2},2.3915996627248484E-4,{"$f":"AE77-AD78*Bodencharakterisierung!$E$8","v":6.15232770911677E-2},{"$f":"IF(AE78>$J$18,(AE78/(Bodencharakterisierung!$E$11*1000)),0)","v":4.0609423822552937E-5},2.3305291073371062E-2,61,null,{"$f":"(AD78)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH78>0,(AJ78*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK77,NA())","v":0.13143142257792267},null,61,{"$f":"IF(AF78<=$J$9*0.05,AS77*EXP((-$J$6*1)/Heterogenität!$D$4),Z78)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF78>=$J$19, AR77/$J$5<AN78),0, Bodencharakterisierung!$E$8*$J$11*((AR77/$J$5)-AN78))","v":0},0,{"$f":"AQ77-AP78*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ78/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,61,null,{"$f":"(AP78)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF78<=$J$9*1.05,(AV78*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW77,NA())","v":{"$error":"#N/A"}},23072.238162637354,194,3.8740624625779221,0.13143142257792267,0,0.38263103999999981,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},40.609423822552934,23305.291073371063]
[null,"Andere",0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,62,2.3305291073371062E-2,{"$f":"Z79*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF78*Bodencharakterisierung!$E$11/$J$20","v":4.2497245431671111E-5},{"$f":"((150*($J$2^0.87)*(AB79^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z79)*3600*24","v":8.0715139708559577E-2},2.3915996627248484E-4,{"$f":"AE78-AD79*Bodencharakterisierung!$E$8","v":6.1444354302297777E-2},{"$f":"IF(AE79>$J$18,(AE79/(Bodencharakterisierung!$E$11*1000)),0)","v":4.0557329572473782E-5},2.3305291073371062E-2,62,null,{"$f":"(AD79)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH79>0,(AJ79*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK78,NA())","v":0.13359888983329846},null,62,{"$f":"IF(AF79<=$J$9*0.05,AS78*EXP((-$J$6*1)/Heterogenität!$D$4),Z79)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF79>=$J$19, AR78/$J$5<AN79),0, Bodencharakterisierung!$E$8*$J$11*((AR78/$J$5)-AN79))","v":0},0,{"$f":"AQ78-AP79*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ79/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,62,null,{"$f":"(AP79)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF79<=$J$9*1.05,(AV79*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW78,NA())","v":{"$error":"#N/A"}},23072.238162637354,195,3.882502569833298,0.13359888983329846,0,0.38890367999999981,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},40.557329572473783,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63,2.3305291073371062E-2,{"$f":"Z80*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF79*Bodencharakterisierung!$E$11/$J$20","v":4.244272946166212E-5},{"$f":"((150*($J$2^0.87)*(AB80^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z80)*3600*24","v":8.0633330238250783E-2},2.3915996627248484E-4,{"$f":"AE79-AD80*Bodencharakterisierung!$E$8","v":6.1365431513427854E-2},{"$f":"IF(AE80>$J$18,(AE80/(Bodencharakterisierung!$E$11*1000)),0)","v":4.050523532239462E-5},2.3305291073371062E-2,63,null,{"$f":"(AD80)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH80>0,(AJ80*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK79,NA())","v":0.13576635708867424},null,63,{"$f":"IF(AF80<=$J$9*0.05,AS79*EXP((-$J$6*1)/Heterogenität!$D$4),Z80)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF80>=$J$19, AR79/$J$5<AN80),0, Bodencharakterisierung!$E$8*$J$11*((AR79/$J$5)-AN80))","v":0},0,{"$f":"AQ79-AP80*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ80/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,63,null,{"$f":"(AP80)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF80<=$J$9*1.05,(AV80*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW79,NA())","v":{"$error":"#N/A"}},23072.238162637354,196,3.8909426770886739,0.13576635708867424,0,0.3951763199999998,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},40.505235322394618,23305.291073371063]
[null,"LCKW","Inventar kg","Inventar g","benötigte H2-Menge g","Substrat-menge g","Substrat-menge kg",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,64,2.3305291073371062E-2,{"$f":"Z81*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF80*Bodencharakterisierung!$E$11/$J$20","v":4.2388213491653123E-5},{"$f":"((150*($J$2^0.87)*(AB81^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z81)*3600*24","v":8.0551498697957746E-2},2.3915996627248484E-4,{"$f":"AE80-AD81*Bodencharakterisierung!$E$8","v":6.1286508724557931E-2},{"$f":"IF(AE81>$J$18,(AE81/(Bodencharakterisierung!$E$11*1000)),0)","v":4.0453141072315464E-5},2.3305291073371062E-2,64,null,{"$f":"(AD81)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH81>0,(AJ81*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK80,NA())","v":0.13793382434405002},null,64,{"$f":"IF(AF81<=$J$9*0.05,AS80*EXP((-$J$6*1)/Heterogenität!$D$4),Z81)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF81>=$J$19, AR80/$J$5<AN81),0, Bodencharakterisierung!$E$8*$J$11*((AR80/$J$5)-AN81))","v":0},0,{"$f":"AQ80-AP81*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ81/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,64,null,{"$f":"(AP81)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF81<=$J$9*1.05,(AV81*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW80,NA())","v":{"$error":"#N/A"}},23072.238162637354,197,3.8993827843440498,0.13793382434405002,0,0.4014489599999998,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},40.453141072315468,{"$f":"AN81*10^6","v":23305.291073371063}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,65,2.3305291073371062E-2,{"$f":"Z82*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF81*Bodencharakterisierung!$E$11/$J$20","v":4.2333697521644132E-5},{"$f":"((150*($J$2^0.87)*(AB82^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z82)*3600*24","v":8.0469645053330902E-2},2.3915996627248484E-4,{"$f":"AE81-AD82*Bodencharakterisierung!$E$8","v":6.1207585935688008E-2},{"$f":"IF(AE82>$J$18,(AE82/(Bodencharakterisierung!$E$11*1000)),0)","v":4.0401046822236309E-5},2.3305291073371062E-2,65,null,{"$f":"(AD82)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH82>0,(AJ82*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK81,NA())","v":0.1401012915994258},null,65,{"$f":"IF(AF82<=$J$9*0.05,AS81*EXP((-$J$6*1)/Heterogenität!$D$4),Z82)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF82>=$J$19, AR81/$J$5<AN82),0, Bodencharakterisierung!$E$8*$J$11*((AR81/$J$5)-AN82))","v":0},0,{"$f":"AQ81-AP82*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ82/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,{"$f":"IF(AN82>$G$5,AM82,NA())","v":65},null,{"$f":"(AP82)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF82<=$J$9*1.05,(AV82*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW81,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH82>($G$5*10^6),BH82*0.99,9999)","v":23072.238162637354},{"$f":"AT82+$G$3","v":198},3.9078228915994258,0.1401012915994258,0,0.4077215999999998,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF82*10^6","v":40.40104682223631},23305.291073371063]
[null,"Tetrachlorethen",{"$f":"IFERROR(Schadstoffbelastung!E4,0)","v":48.585599999999999},{"$f":"C83*1000","v":48585.599999999999},{"$f":"D83*Sanierungsdesign!M11","v":2341.4746987951803},{"$f":"E83*$E$66","v":210966.87036144573},{"$f":"F83/1000","v":210.96687036144573},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,66,{"$f":"AG82","v":2.3305291073371062E-2},{"$f":"Z83*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF82*Bodencharakterisierung!$E$11/$J$20","v":4.2279181551635135E-5},{"$f":"((150*($J$2^0.87)*(AB83^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z83)*3600*24","v":8.0387769269922443E-2},{"$f":"MIN(AC83,Z83-AA83)","v":2.3915996627248484E-4},{"$f":"AE82-AD83*Bodencharakterisierung!$E$8","v":6.1128663146818085E-2},{"$f":"IF(AE83>$J$18,(AE83/(Bodencharakterisierung!$E$11*1000)),0)","v":4.0348952572157154E-5},{"$f":"AA83+AD83","v":2.3305291073371062E-2},{"$f":"IF(AD83>0,Y83,NA())","v":66},null,{"$f":"(AD83)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH83>0,(AJ83*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK82,NA())","v":0.14226875885480159},null,66,{"$f":"IF(AF83<=$J$9*0.05,AS82*EXP((-$J$6*1)/Heterogenität!$D$4),Z83)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF83>=$J$19, AR82/$J$5<AN83),0, Bodencharakterisierung!$E$8*$J$11*((AR82/$J$5)-AN83))","v":0},0,{"$f":"AQ82-AP83*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ83/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},{"$f":"AN83+AP83","v":2.3305291073371062E-2},66,null,{"$f":"(AP83)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF83<=$J$9*1.05,(AV83*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW82,NA())","v":{"$error":"#N/A"}},23072.238162637354,199,{"$f":"IF(ISNUMBER(AT83),BA83+BB83+BC83+$AZ$17,\"\")","v":3.9162629988548012},{"$f":"IF(ISNUMBER(AK83),AK83,BA82)","v":0.14226875885480159},{"$f":"IF(ISNUMBER(AW83),AW83,0)","v":0},0.41399423999999979,null,{"$f":"AR83*10^6","v":4.3827000000643475},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},40.348952572157152,23305.291073371063]
[null,"Trichlorethen",{"$f":"IFERROR(Schadstoffbelastung!E5,0)","v":18.763919999999999},18763.919999999998,{"$f":"D84*Sanierungsdesign!M12","v":859.41618320610678},{"$f":"E84*$E$66","v":77433.398106870212},{"$f":"F84/1000","v":77.433398106870214},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,67,2.3305291073371062E-2,{"$f":"Z84*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF83*Bodencharakterisierung!$E$11/$J$20","v":4.2224665581626144E-5},{"$f":"((150*($J$2^0.87)*(AB84^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z84)*3600*24","v":8.0305871313186561E-2},2.3915996627248484E-4,{"$f":"AE83-AD84*Bodencharakterisierung!$E$8","v":6.1049740357948162E-2},{"$f":"IF(AE84>$J$18,(AE84/(Bodencharakterisierung!$E$11*1000)),0)","v":4.0296858322077992E-5},2.3305291073371062E-2,67,null,{"$f":"(AD84)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH84>0,(AJ84*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK83,NA())","v":0.14443622611017737},null,67,{"$f":"IF(AF84<=$J$9*0.05,AS83*EXP((-$J$6*1)/Heterogenität!$D$4),Z84)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF84>=$J$19, AR83/$J$5<AN84),0, Bodencharakterisierung!$E$8*$J$11*((AR83/$J$5)-AN84))","v":0},{"$f":"MIN(AO84,AS83-AN84)","v":0},{"$f":"AQ83-AP84*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ84/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,67,null,{"$f":"(AP84)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF84<=$J$9*1.05,(AV84*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW83,NA())","v":{"$error":"#N/A"}},23072.238162637354,200,3.9247031061101771,0.14443622611017737,0,{"$f":"$G$34/$G$12/$G$8+BC83","v":0.42026687999999979},null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},40.296858322077995,23305.291073371063]
[null,"cis-1,2-Dichlorethen",{"$f":"IFERROR(Schadstoffbelastung!E6,0)","v":16.965},16965,{"$f":"D85*Sanierungsdesign!M13","v":699.58762886597935},63032.845360824736,63.032845360824737,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,68,2.3305291073371062E-2,{"$f":"Z85*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF84*Bodencharakterisierung!$E$11/$J$20","v":4.2170149611617147E-5},{"$f":"((150*($J$2^0.87)*(AB85^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z85)*3600*24","v":8.0223951148479022E-2},2.3915996627248484E-4,{"$f":"AE84-AD85*Bodencharakterisierung!$E$8","v":6.0970817569078239E-2},{"$f":"IF(AE85>$J$18,(AE85/(Bodencharakterisierung!$E$11*1000)),0)","v":4.0244764071998837E-5},2.3305291073371062E-2,68,null,{"$f":"(AD85)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH85>0,(AJ85*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK84,NA())","v":0.14660369336555315},null,68,{"$f":"IF(AF85<=$J$9*0.05,AS84*EXP((-$J$6*1)/Heterogenität!$D$4),Z85)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF85>=$J$19, AR84/$J$5<AN85),0, Bodencharakterisierung!$E$8*$J$11*((AR84/$J$5)-AN85))","v":0},0,{"$f":"AQ84-AP85*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ85/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,68,null,{"$f":"(AP85)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF85<=$J$9*1.05,(AV85*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW84,NA())","v":{"$error":"#N/A"}},23072.238162637354,201,3.9331432133655531,0.14660369336555315,0,0.42653951999999978,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},40.244764071998837,23305.291073371063]
[null,"trans-1,2-Dichlorethen",{"$f":"IFERROR(Schadstoffbelastung!E7,0)","v":1.4868E-10},1.4868000000000001E-7,{"$f":"D86*Sanierungsdesign!M14","v":6.1311340206185572E-9},5.52415175257732E-7,5.5241517525773196E-10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,69,2.3305291073371062E-2,{"$f":"Z86*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF85*Bodencharakterisierung!$E$11/$J$20","v":4.2115633641608156E-5},{"$f":"((150*($J$2^0.87)*(AB86^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z86)*3600*24","v":8.0142008741056203E-2},2.3915996627248484E-4,{"$f":"AE85-AD86*Bodencharakterisierung!$E$8","v":6.0891894780208317E-2},{"$f":"IF(AE86>$J$18,(AE86/(Bodencharakterisierung!$E$11*1000)),0)","v":4.0192669821919682E-5},2.3305291073371062E-2,69,null,{"$f":"(AD86)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH86>0,(AJ86*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK85,NA())","v":0.14877116062092893},null,69,{"$f":"IF(AF86<=$J$9*0.05,AS85*EXP((-$J$6*1)/Heterogenität!$D$4),Z86)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF86>=$J$19, AR85/$J$5<AN86),0, Bodencharakterisierung!$E$8*$J$11*((AR85/$J$5)-AN86))","v":0},0,{"$f":"AQ85-AP86*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ86/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,69,null,{"$f":"(AP86)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF86<=$J$9*1.05,(AV86*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW85,NA())","v":{"$error":"#N/A"}},23072.238162637354,202,3.9415833206209285,0.14877116062092893,0,0.43281215999999978,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},40.192669821919679,23305.291073371063]
[null,"1,1-Dichlorethen",{"$f":"IFERROR(Schadstoffbelastung!E8,0)","v":1.6778718000000002E-10},1.6778718000000001E-7,{"$f":"D87*Sanierungsdesign!M15","v":6.9190589690721656E-9},6.2340721311340209E-7,6.2340721311340205E-10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70,2.3305291073371062E-2,{"$f":"Z87*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF86*Bodencharakterisierung!$E$11/$J$20","v":4.2061117671599165E-5},{"$f":"((150*($J$2^0.87)*(AB87^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z87)*3600*24","v":8.0060044056075544E-2},2.3915996627248484E-4,{"$f":"AE86-AD87*Bodencharakterisierung!$E$8","v":6.0812971991338394E-2},{"$f":"IF(AE87>$J$18,(AE87/(Bodencharakterisierung!$E$11*1000)),0)","v":4.0140575571840526E-5},2.3305291073371062E-2,70,null,{"$f":"(AD87)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH87>0,(AJ87*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK86,NA())","v":0.15093862787630472},null,70,{"$f":"IF(AF87<=$J$9*0.05,AS86*EXP((-$J$6*1)/Heterogenität!$D$4),Z87)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF87>=$J$19, AR86/$J$5<AN87),0, Bodencharakterisierung!$E$8*$J$11*((AR86/$J$5)-AN87))","v":0},0,{"$f":"AQ86-AP87*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ87/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,70,null,{"$f":"(AP87)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF87<=$J$9*1.05,(AV87*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW86,NA())","v":{"$error":"#N/A"}},23072.238162637354,203,3.9500234278763044,0.15093862787630472,0,0.43908479999999978,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},40.140575571840529,23305.291073371063]
[null,"Vinylchlorid",{"$f":"IFERROR(Schadstoffbelastung!E9,0)","v":2.9736000000000002},2973.6000000000004,{"$f":"D88*Sanierungsdesign!M16","v":94.4},8505.44,8.5054400000000001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,71,2.3305291073371062E-2,{"$f":"Z88*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF87*Bodencharakterisierung!$E$11/$J$20","v":4.2006601701590175E-5},{"$f":"((150*($J$2^0.87)*(AB88^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z88)*3600*24","v":7.9978057058594426E-2},2.3915996627248484E-4,{"$f":"AE87-AD88*Bodencharakterisierung!$E$8","v":6.0734049202468471E-2},{"$f":"IF(AE88>$J$18,(AE88/(Bodencharakterisierung!$E$11*1000)),0)","v":4.0088481321761364E-5},2.3305291073371062E-2,71,null,{"$f":"(AD88)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH88>0,(AJ88*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK87,NA())","v":0.1531060951316805},null,71,{"$f":"IF(AF88<=$J$9*0.05,AS87*EXP((-$J$6*1)/Heterogenität!$D$4),Z88)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF88>=$J$19, AR87/$J$5<AN88),0, Bodencharakterisierung!$E$8*$J$11*((AR87/$J$5)-AN88))","v":0},0,{"$f":"AQ87-AP88*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ88/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,71,null,{"$f":"(AP88)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF88<=$J$9*1.05,(AV88*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW87,NA())","v":{"$error":"#N/A"}},23072.238162637354,204,3.9584635351316804,0.1531060951316805,0,0.44535743999999977,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},40.088481321761364,23305.291073371063]
[null,"Tetrachlormethan",{"$f":"IFERROR(Schadstoffbelastung!E10,0)","v":5.5882079999999999E-10},5.5882080000000001E-7,{"$f":"D89*Sanierungsdesign!M17","v":2.902965194805195E-8},2.6155716405194807E-6,2.6155716405194808E-9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,72,2.3305291073371062E-2,{"$f":"Z89*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF88*Bodencharakterisierung!$E$11/$J$20","v":4.1952085731581177E-5},{"$f":"((150*($J$2^0.87)*(AB89^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z89)*3600*24","v":7.9896047713569965E-2},2.3915996627248484E-4,{"$f":"AE88-AD89*Bodencharakterisierung!$E$8","v":6.0655126413598548E-2},{"$f":"IF(AE89>$J$18,(AE89/(Bodencharakterisierung!$E$11*1000)),0)","v":4.0036387071682209E-5},2.3305291073371062E-2,72,null,{"$f":"(AD89)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH89>0,(AJ89*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK88,NA())","v":0.15527356238705628},null,72,{"$f":"IF(AF89<=$J$9*0.05,AS88*EXP((-$J$6*1)/Heterogenität!$D$4),Z89)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF89>=$J$19, AR88/$J$5<AN89),0, Bodencharakterisierung!$E$8*$J$11*((AR88/$J$5)-AN89))","v":0},0,{"$f":"AQ88-AP89*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ89/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,72,null,{"$f":"(AP89)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF89<=$J$9*1.05,(AV89*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW88,NA())","v":{"$error":"#N/A"}},23072.238162637354,205,3.9669036423870558,0.15527356238705628,0,0.45163007999999977,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},40.036387071682206,23305.291073371063]
[null,"Trichlormethan",{"$f":"IFERROR(Schadstoffbelastung!E11,0)","v":1.3269977999999999E-10},1.3269977999999999E-7,{"$f":"D90*Sanierungsdesign!M18","v":6.6907452100840331E-9},6.0283614342857136E-7,6.0283614342857133E-10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,73,2.3305291073371062E-2,{"$f":"Z90*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF89*Bodencharakterisierung!$E$11/$J$20","v":4.1897569761572187E-5},{"$f":"((150*($J$2^0.87)*(AB90^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z90)*3600*24","v":7.9814015985858522E-2},2.3915996627248484E-4,{"$f":"AE89-AD90*Bodencharakterisierung!$E$8","v":6.0576203624728625E-2},{"$f":"IF(AE90>$J$18,(AE90/(Bodencharakterisierung!$E$11*1000)),0)","v":3.9984292821603054E-5},2.3305291073371062E-2,73,null,{"$f":"(AD90)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH90>0,(AJ90*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK89,NA())","v":0.15744102964243206},null,73,{"$f":"IF(AF90<=$J$9*0.05,AS89*EXP((-$J$6*1)/Heterogenität!$D$4),Z90)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF90>=$J$19, AR89/$J$5<AN90),0, Bodencharakterisierung!$E$8*$J$11*((AR89/$J$5)-AN90))","v":0},0,{"$f":"AQ89-AP90*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ90/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,73,null,{"$f":"(AP90)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF90<=$J$9*1.05,(AV90*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW89,NA())","v":{"$error":"#N/A"}},23072.238162637354,206,3.9753437496424318,0.15744102964243206,0,0.45790271999999976,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},39.984292821603056,23305.291073371063]
[null,"Dichlormethan",{"$f":"IFERROR(Schadstoffbelastung!E12,0)","v":6.1688699999999995E-11},6.1688700000000001E-8,{"$f":"D91*Sanierungsdesign!M19","v":2.9029976470588233E-9},2.6156008799999997E-7,2.6156008799999997E-10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74,2.3305291073371062E-2,{"$f":"Z91*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF90*Bodencharakterisierung!$E$11/$J$20","v":4.184305379156319E-5},{"$f":"((150*($J$2^0.87)*(AB91^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z91)*3600*24","v":7.9731961840215734E-2},2.3915996627248484E-4,{"$f":"AE90-AD91*Bodencharakterisierung!$E$8","v":6.0497280835858702E-2},{"$f":"IF(AE91>$J$18,(AE91/(Bodencharakterisierung!$E$11*1000)),0)","v":3.9932198571523899E-5},2.3305291073371062E-2,74,null,{"$f":"(AD91)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH91>0,(AJ91*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK90,NA())","v":0.15960849689780784},null,74,{"$f":"IF(AF91<=$J$9*0.05,AS90*EXP((-$J$6*1)/Heterogenität!$D$4),Z91)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF91>=$J$19, AR90/$J$5<AN91),0, Bodencharakterisierung!$E$8*$J$11*((AR90/$J$5)-AN91))","v":0},0,{"$f":"AQ90-AP91*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ91/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,74,null,{"$f":"(AP91)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF91<=$J$9*1.05,(AV91*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW90,NA())","v":{"$error":"#N/A"}},23072.238162637354,207,3.9837838568978077,0.15960849689780784,0,0.46417535999999976,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},39.932198571523898,23305.291073371063]
[null,"1,1,1-Trichlorethan",{"$f":"IFERROR(Schadstoffbelastung!E13,0)","v":3.0139200000000002E-11},3.01392E-8,{"$f":"D92*Sanierungsdesign!M20","v":1.3555455608527482E-9},1.2213465503283261E-7,1.2213465503283261E-10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,75,2.3305291073371062E-2,{"$f":"Z92*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF91*Bodencharakterisierung!$E$11/$J$20","v":4.1788537821554206E-5},{"$f":"((150*($J$2^0.87)*(AB92^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z92)*3600*24","v":7.9649885241295432E-2},2.3915996627248484E-4,{"$f":"AE91-AD92*Bodencharakterisierung!$E$8","v":6.0418358046988779E-2},{"$f":"IF(AE92>$J$18,(AE92/(Bodencharakterisierung!$E$11*1000)),0)","v":3.9880104321444737E-5},2.3305291073371062E-2,75,null,{"$f":"(AD92)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH92>0,(AJ92*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK91,NA())","v":0.16177596415318363},null,75,{"$f":"IF(AF92<=$J$9*0.05,AS91*EXP((-$J$6*1)/Heterogenität!$D$4),Z92)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF92>=$J$19, AR91/$J$5<AN92),0, Bodencharakterisierung!$E$8*$J$11*((AR91/$J$5)-AN92))","v":0},0,{"$f":"AQ91-AP92*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ92/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,75,null,{"$f":"(AP92)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF92<=$J$9*1.05,(AV92*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW91,NA())","v":{"$error":"#N/A"}},23072.238162637354,208,3.9922239641531831,0.16177596415318363,0,0.47044799999999976,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},39.880104321444733,23305.291073371063]
[null,"1,1,2-Trichlorethan",{"$f":"IFERROR(Schadstoffbelastung!E14,0)","v":1.1893752E-10},1.1893752E-7,{"$f":"D93*Sanierungsdesign!M21","v":5.349353242781326E-9},4.8197672717459749E-7,4.8197672717459746E-10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,76,2.3305291073371062E-2,{"$f":"Z93*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF92*Bodencharakterisierung!$E$11/$J$20","v":4.1734021851545202E-5},{"$f":"((150*($J$2^0.87)*(AB93^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z93)*3600*24","v":7.9567786153649886E-2},2.3915996627248484E-4,{"$f":"AE92-AD93*Bodencharakterisierung!$E$8","v":6.0339435258118856E-2},{"$f":"IF(AE93>$J$18,(AE93/(Bodencharakterisierung!$E$11*1000)),0)","v":3.9828010071365581E-5},2.3305291073371062E-2,76,null,{"$f":"(AD93)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH93>0,(AJ93*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK92,NA())","v":0.16394343140855941},null,76,{"$f":"IF(AF93<=$J$9*0.05,AS92*EXP((-$J$6*1)/Heterogenität!$D$4),Z93)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF93>=$J$19, AR92/$J$5<AN93),0, Bodencharakterisierung!$E$8*$J$11*((AR92/$J$5)-AN93))","v":0},0,{"$f":"AQ92-AP93*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ93/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,76,null,{"$f":"(AP93)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF93<=$J$9*1.05,(AV93*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW92,NA())","v":{"$error":"#N/A"}},23072.238162637354,209,4.0006640714085595,0.16394343140855941,0,0.47672063999999975,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},39.828010071365583,23305.291073371063]
[null,"1,1-Dichlorethan",{"$f":"IFERROR(Schadstoffbelastung!E15,0)","v":1.0457532E-10},1.0457532E-7,{"$f":"D94*Sanierungsdesign!M22","v":4.2269733225545685E-9},3.8085029636216661E-7,3.8085029636216661E-10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,77,2.3305291073371062E-2,{"$f":"Z94*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF93*Bodencharakterisierung!$E$11/$J$20","v":4.1679505881536211E-5},{"$f":"((150*($J$2^0.87)*(AB94^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z94)*3600*24","v":7.9485664541728465E-2},2.3915996627248484E-4,{"$f":"AE93-AD94*Bodencharakterisierung!$E$8","v":6.0260512469248934E-2},{"$f":"IF(AE94>$J$18,(AE94/(Bodencharakterisierung!$E$11*1000)),0)","v":3.9775915821286426E-5},2.3305291073371062E-2,77,null,{"$f":"(AD94)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH94>0,(AJ94*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK93,NA())","v":0.16611089866393519},null,77,{"$f":"IF(AF94<=$J$9*0.05,AS93*EXP((-$J$6*1)/Heterogenität!$D$4),Z94)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF94>=$J$19, AR93/$J$5<AN94),0, Bodencharakterisierung!$E$8*$J$11*((AR93/$J$5)-AN94))","v":0},0,{"$f":"AQ93-AP94*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ94/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,77,null,{"$f":"(AP94)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF94<=$J$9*1.05,(AV94*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW93,NA())","v":{"$error":"#N/A"}},23072.238162637354,210,4.009104178663935,0.16611089866393519,0,0.48299327999999975,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},39.775915821286425,23305.291073371063]
[null,"1,2-Dichlorethan",{"$f":"IFERROR(Schadstoffbelastung!E16,0)","v":1.115928E-10},1.115928E-7,{"$f":"D95*Sanierungsdesign!M23","v":4.5106224737267588E-9},4.0640708488278092E-7,4.0640708488278095E-10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,78,2.3305291073371062E-2,{"$f":"Z95*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF94*Bodencharakterisierung!$E$11/$J$20","v":4.162498991152722E-5},{"$f":"((150*($J$2^0.87)*(AB95^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z95)*3600*24","v":7.9403520369878161E-2},2.3915996627248484E-4,{"$f":"AE94-AD95*Bodencharakterisierung!$E$8","v":6.0181589680379011E-2},{"$f":"IF(AE95>$J$18,(AE95/(Bodencharakterisierung!$E$11*1000)),0)","v":3.9723821571207271E-5},2.3305291073371062E-2,78,null,{"$f":"(AD95)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH95>0,(AJ95*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK94,NA())","v":0.16827836591931097},null,78,{"$f":"IF(AF95<=$J$9*0.05,AS94*EXP((-$J$6*1)/Heterogenität!$D$4),Z95)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF95>=$J$19, AR94/$J$5<AN95),0, Bodencharakterisierung!$E$8*$J$11*((AR94/$J$5)-AN95))","v":0},0,{"$f":"AQ94-AP95*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ95/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,78,null,{"$f":"(AP95)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF95<=$J$9*1.05,(AV95*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW94,NA())","v":{"$error":"#N/A"}},23072.238162637354,211,4.0175442859193105,0.16827836591931097,0,0.48926591999999974,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},39.723821571207274,23305.291073371063]
[null,"Summe LCKW",{"$f":"SUM(C83:C95)","v":87.288120001434933},{"$f":"C96*1000","v":87288.120001434931},{"$f":"SUM(E83:E95)","v":3994.8785109343826},{"$f":"E96*$E$66","v":359938.55383518786},359.93855383518786,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,79,2.3305291073371062E-2,{"$f":"Z96*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF95*Bodencharakterisierung!$E$11/$J$20","v":4.157047394151823E-5},{"$f":"((150*($J$2^0.87)*(AB96^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z96)*3600*24","v":7.9321353602342687E-2},2.3915996627248484E-4,{"$f":"AE95-AD96*Bodencharakterisierung!$E$8","v":6.0102666891509088E-2},{"$f":"IF(AE96>$J$18,(AE96/(Bodencharakterisierung!$E$11*1000)),0)","v":3.9671727321128109E-5},2.3305291073371062E-2,79,null,{"$f":"(AD96)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH96>0,(AJ96*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK95,NA())","v":0.17044583317468676},null,79,{"$f":"IF(AF96<=$J$9*0.05,AS95*EXP((-$J$6*1)/Heterogenität!$D$4),Z96)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF96>=$J$19, AR95/$J$5<AN96),0, Bodencharakterisierung!$E$8*$J$11*((AR95/$J$5)-AN96))","v":0},0,{"$f":"AQ95-AP96*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ96/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,79,null,{"$f":"(AP96)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF96<=$J$9*1.05,(AV96*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW95,NA())","v":{"$error":"#N/A"}},23072.238162637354,212,4.0259843931746868,0.17044583317468676,0,0.49553855999999974,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},39.67172732112811,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,80,2.3305291073371062E-2,{"$f":"Z97*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF96*Bodencharakterisierung!$E$11/$J$20","v":4.1515957971509232E-5},{"$f":"((150*($J$2^0.87)*(AB97^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z97)*3600*24","v":7.9239164203262158E-2},2.3915996627248484E-4,{"$f":"AE96-AD97*Bodencharakterisierung!$E$8","v":6.0023744102639165E-2},{"$f":"IF(AE97>$J$18,(AE97/(Bodencharakterisierung!$E$11*1000)),0)","v":3.9619633071048954E-5},2.3305291073371062E-2,80,null,{"$f":"(AD97)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH97>0,(AJ97*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK96,NA())","v":0.17261330043006254},null,80,{"$f":"IF(AF97<=$J$9*0.05,AS96*EXP((-$J$6*1)/Heterogenität!$D$4),Z97)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF97>=$J$19, AR96/$J$5<AN97),0, Bodencharakterisierung!$E$8*$J$11*((AR96/$J$5)-AN97))","v":0},0,{"$f":"AQ96-AP97*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ97/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,80,null,{"$f":"(AP97)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF97<=$J$9*1.05,(AV97*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW96,NA())","v":{"$error":"#N/A"}},23072.238162637354,213,4.0344245004300623,0.17261330043006254,0,0.50181119999999979,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},39.619633071048952,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,81,2.3305291073371062E-2,{"$f":"Z98*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF97*Bodencharakterisierung!$E$11/$J$20","v":4.1461442001500242E-5},{"$f":"((150*($J$2^0.87)*(AB98^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z98)*3600*24","v":7.9156952136672509E-2},2.3915996627248484E-4,{"$f":"AE97-AD98*Bodencharakterisierung!$E$8","v":5.9944821313769242E-2},{"$f":"IF(AE98>$J$18,(AE98/(Bodencharakterisierung!$E$11*1000)),0)","v":3.9567538820969799E-5},2.3305291073371062E-2,81,null,{"$f":"(AD98)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH98>0,(AJ98*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK97,NA())","v":0.17478076768543832},null,81,{"$f":"IF(AF98<=$J$9*0.05,AS97*EXP((-$J$6*1)/Heterogenität!$D$4),Z98)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF98>=$J$19, AR97/$J$5<AN98),0, Bodencharakterisierung!$E$8*$J$11*((AR97/$J$5)-AN98))","v":0},0,{"$f":"AQ97-AP98*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ98/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,81,null,{"$f":"(AP98)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF98<=$J$9*1.05,(AV98*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW97,NA())","v":{"$error":"#N/A"}},23072.238162637354,214,4.0428646076854378,0.17478076768543832,0,0.50808383999999984,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},39.567538820969801,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,82,2.3305291073371062E-2,{"$f":"Z99*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF98*Bodencharakterisierung!$E$11/$J$20","v":4.1406926031491251E-5},{"$f":"((150*($J$2^0.87)*(AB99^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z99)*3600*24","v":7.9074717366505107E-2},2.3915996627248484E-4,{"$f":"AE98-AD99*Bodencharakterisierung!$E$8","v":5.9865898524899319E-2},{"$f":"IF(AE99>$J$18,(AE99/(Bodencharakterisierung!$E$11*1000)),0)","v":3.9515444570890637E-5},2.3305291073371062E-2,82,null,{"$f":"(AD99)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH99>0,(AJ99*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK98,NA())","v":0.1769482349408141},null,82,{"$f":"IF(AF99<=$J$9*0.05,AS98*EXP((-$J$6*1)/Heterogenität!$D$4),Z99)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF99>=$J$19, AR98/$J$5<AN99),0, Bodencharakterisierung!$E$8*$J$11*((AR98/$J$5)-AN99))","v":0},0,{"$f":"AQ98-AP99*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ99/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,82,null,{"$f":"(AP99)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF99<=$J$9*1.05,(AV99*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW98,NA())","v":{"$error":"#N/A"}},23072.238162637354,215,4.0513047149408141,0.1769482349408141,0,0.51435647999999989,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},39.515444570890637,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,83,2.3305291073371062E-2,{"$f":"Z100*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF99*Bodencharakterisierung!$E$11/$J$20","v":4.1352410061482254E-5},{"$f":"((150*($J$2^0.87)*(AB100^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z100)*3600*24","v":7.8992459856586594E-2},2.3915996627248484E-4,{"$f":"AE99-AD100*Bodencharakterisierung!$E$8","v":5.9786975736029396E-2},{"$f":"IF(AE100>$J$18,(AE100/(Bodencharakterisierung!$E$11*1000)),0)","v":3.9463350320811481E-5},2.3305291073371062E-2,83,null,{"$f":"(AD100)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH100>0,(AJ100*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK99,NA())","v":0.17911570219618989},null,83,{"$f":"IF(AF100<=$J$9*0.05,AS99*EXP((-$J$6*1)/Heterogenität!$D$4),Z100)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF100>=$J$19, AR99/$J$5<AN100),0, Bodencharakterisierung!$E$8*$J$11*((AR99/$J$5)-AN100))","v":0},0,{"$f":"AQ99-AP100*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ100/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,83,null,{"$f":"(AP100)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF100<=$J$9*1.05,(AV100*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW99,NA())","v":{"$error":"#N/A"}},23072.238162637354,216,4.0597448221961896,0.17911570219618989,0,0.52062911999999995,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},39.463350320811479,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,84,2.3305291073371062E-2,{"$f":"Z101*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF100*Bodencharakterisierung!$E$11/$J$20","v":4.1297894091473256E-5},{"$f":"((150*($J$2^0.87)*(AB101^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z101)*3600*24","v":7.8910179570637798E-2},2.3915996627248484E-4,{"$f":"AE100-AD101*Bodencharakterisierung!$E$8","v":5.9708052947159473E-2},{"$f":"IF(AE101>$J$18,(AE101/(Bodencharakterisierung!$E$11*1000)),0)","v":3.9411256070732326E-5},2.3305291073371062E-2,84,null,{"$f":"(AD101)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH101>0,(AJ101*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK100,NA())","v":0.18128316945156567},null,84,{"$f":"IF(AF101<=$J$9*0.05,AS100*EXP((-$J$6*1)/Heterogenität!$D$4),Z101)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF101>=$J$19, AR100/$J$5<AN101),0, Bodencharakterisierung!$E$8*$J$11*((AR100/$J$5)-AN101))","v":0},0,{"$f":"AQ100-AP101*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ101/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,84,null,{"$f":"(AP101)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF101<=$J$9*1.05,(AV101*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW100,NA())","v":{"$error":"#N/A"}},23072.238162637354,217,4.0681849294515651,0.18128316945156567,0,0.52690176,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},39.411256070732328,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,85,2.3305291073371062E-2,{"$f":"Z102*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF101*Bodencharakterisierung!$E$11/$J$20","v":4.1243378121464273E-5},{"$f":"((150*($J$2^0.87)*(AB102^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z102)*3600*24","v":7.8827876472274197E-2},2.3915996627248484E-4,{"$f":"AE101-AD102*Bodencharakterisierung!$E$8","v":5.9629130158289551E-2},{"$f":"IF(AE102>$J$18,(AE102/(Bodencharakterisierung!$E$11*1000)),0)","v":3.9359161820653171E-5},2.3305291073371062E-2,85,null,{"$f":"(AD102)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH102>0,(AJ102*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK101,NA())","v":0.18345063670694145},null,85,{"$f":"IF(AF102<=$J$9*0.05,AS101*EXP((-$J$6*1)/Heterogenität!$D$4),Z102)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF102>=$J$19, AR101/$J$5<AN102),0, Bodencharakterisierung!$E$8*$J$11*((AR101/$J$5)-AN102))","v":0},0,{"$f":"AQ101-AP102*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ102/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,85,null,{"$f":"(AP102)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF102<=$J$9*1.05,(AV102*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW101,NA())","v":{"$error":"#N/A"}},23072.238162637354,218,4.0766250367069414,0.18345063670694145,0,0.53317440000000005,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},39.359161820653171,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,86,2.3305291073371062E-2,{"$f":"Z103*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF102*Bodencharakterisierung!$E$11/$J$20","v":4.1188862151455275E-5},{"$f":"((150*($J$2^0.87)*(AB103^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z103)*3600*24","v":7.8745550525004523E-2},2.3915996627248484E-4,{"$f":"AE102-AD103*Bodencharakterisierung!$E$8","v":5.9550207369419628E-2},{"$f":"IF(AE103>$J$18,(AE103/(Bodencharakterisierung!$E$11*1000)),0)","v":3.9307067570574009E-5},2.3305291073371062E-2,86,null,{"$f":"(AD103)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH103>0,(AJ103*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK102,NA())","v":0.18561810396231723},null,86,{"$f":"IF(AF103<=$J$9*0.05,AS102*EXP((-$J$6*1)/Heterogenität!$D$4),Z103)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF103>=$J$19, AR102/$J$5<AN103),0, Bodencharakterisierung!$E$8*$J$11*((AR102/$J$5)-AN103))","v":0},0,{"$f":"AQ102-AP103*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ103/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,86,null,{"$f":"(AP103)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF103<=$J$9*1.05,(AV103*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW102,NA())","v":{"$error":"#N/A"}},23072.238162637354,219,4.0850651439623169,0.18561810396231723,0,0.5394470400000001,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},39.307067570574006,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,87,2.3305291073371062E-2,{"$f":"Z104*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF103*Bodencharakterisierung!$E$11/$J$20","v":4.1134346181446278E-5},{"$f":"((150*($J$2^0.87)*(AB104^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z104)*3600*24","v":7.8663201692231177E-2},2.3915996627248484E-4,{"$f":"AE103-AD104*Bodencharakterisierung!$E$8","v":5.9471284580549705E-2},{"$f":"IF(AE104>$J$18,(AE104/(Bodencharakterisierung!$E$11*1000)),0)","v":3.9254973320494854E-5},2.3305291073371062E-2,87,null,{"$f":"(AD104)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH104>0,(AJ104*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK103,NA())","v":0.18778557121769301},null,87,{"$f":"IF(AF104<=$J$9*0.05,AS103*EXP((-$J$6*1)/Heterogenität!$D$4),Z104)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF104>=$J$19, AR103/$J$5<AN104),0, Bodencharakterisierung!$E$8*$J$11*((AR103/$J$5)-AN104))","v":0},0,{"$f":"AQ103-AP104*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ104/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,87,null,{"$f":"(AP104)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF104<=$J$9*1.05,(AV104*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW103,NA())","v":{"$error":"#N/A"}},23072.238162637354,220,4.0935052512176933,0.18778557121769301,0,0.54571968000000015,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},39.254973320494855,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,88,2.3305291073371062E-2,{"$f":"Z105*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF104*Bodencharakterisierung!$E$11/$J$20","v":4.1079830211437287E-5},{"$f":"((150*($J$2^0.87)*(AB105^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z105)*3600*24","v":7.8580829937248853E-2},2.3915996627248484E-4,{"$f":"AE104-AD105*Bodencharakterisierung!$E$8","v":5.9392361791679782E-2},{"$f":"IF(AE105>$J$18,(AE105/(Bodencharakterisierung!$E$11*1000)),0)","v":3.9202879070415698E-5},2.3305291073371062E-2,88,null,{"$f":"(AD105)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH105>0,(AJ105*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK104,NA())","v":0.1899530384730688},null,88,{"$f":"IF(AF105<=$J$9*0.05,AS104*EXP((-$J$6*1)/Heterogenität!$D$4),Z105)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF105>=$J$19, AR104/$J$5<AN105),0, Bodencharakterisierung!$E$8*$J$11*((AR104/$J$5)-AN105))","v":0},0,{"$f":"AQ104-AP105*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ105/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,88,null,{"$f":"(AP105)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF105<=$J$9*1.05,(AV105*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW104,NA())","v":{"$error":"#N/A"}},23072.238162637354,221,4.1019453584730687,0.1899530384730688,0,0.5519923200000002,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},39.202879070415698,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,89,2.3305291073371062E-2,{"$f":"Z106*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF105*Bodencharakterisierung!$E$11/$J$20","v":4.1025314241428297E-5},{"$f":"((150*($J$2^0.87)*(AB106^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z106)*3600*24","v":7.8498435223244983E-2},2.3915996627248484E-4,{"$f":"AE105-AD106*Bodencharakterisierung!$E$8","v":5.9313439002809859E-2},{"$f":"IF(AE106>$J$18,(AE106/(Bodencharakterisierung!$E$11*1000)),0)","v":3.9150784820336543E-5},2.3305291073371062E-2,89,null,{"$f":"(AD106)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH106>0,(AJ106*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK105,NA())","v":0.19212050572844458},null,89,{"$f":"IF(AF106<=$J$9*0.05,AS105*EXP((-$J$6*1)/Heterogenität!$D$4),Z106)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF106>=$J$19, AR105/$J$5<AN106),0, Bodencharakterisierung!$E$8*$J$11*((AR105/$J$5)-AN106))","v":0},0,{"$f":"AQ105-AP106*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ106/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,89,null,{"$f":"(AP106)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF106<=$J$9*1.05,(AV106*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW105,NA())","v":{"$error":"#N/A"}},23072.238162637354,222,4.1103854657284451,0.19212050572844458,0,0.55826496000000025,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},39.15078482033654,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,90,2.3305291073371062E-2,{"$f":"Z107*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF106*Bodencharakterisierung!$E$11/$J$20","v":4.0970798271419306E-5},{"$f":"((150*($J$2^0.87)*(AB107^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z107)*3600*24","v":7.8416017513298769E-2},2.3915996627248484E-4,{"$f":"AE106-AD107*Bodencharakterisierung!$E$8","v":5.9234516213939936E-2},{"$f":"IF(AE107>$J$18,(AE107/(Bodencharakterisierung!$E$11*1000)),0)","v":3.9098690570257381E-5},2.3305291073371062E-2,90,null,{"$f":"(AD107)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH107>0,(AJ107*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK106,NA())","v":0.19428797298382036},null,90,{"$f":"IF(AF107<=$J$9*0.05,AS106*EXP((-$J$6*1)/Heterogenität!$D$4),Z107)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF107>=$J$19, AR106/$J$5<AN107),0, Bodencharakterisierung!$E$8*$J$11*((AR106/$J$5)-AN107))","v":0},0,{"$f":"AQ106-AP107*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ107/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,90,null,{"$f":"(AP107)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF107<=$J$9*1.05,(AV107*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW106,NA())","v":{"$error":"#N/A"}},23072.238162637354,223,4.1188255729838206,0.19428797298382036,0,0.56453760000000031,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},39.098690570257382,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,91,2.3305291073371062E-2,{"$f":"Z108*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF107*Bodencharakterisierung!$E$11/$J$20","v":4.0916282301410309E-5},{"$f":"((150*($J$2^0.87)*(AB108^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z108)*3600*24","v":7.8333576770380789E-2},2.3915996627248484E-4,{"$f":"AE107-AD108*Bodencharakterisierung!$E$8","v":5.9155593425070013E-2},{"$f":"IF(AE108>$J$18,(AE108/(Bodencharakterisierung!$E$11*1000)),0)","v":3.9046596320178226E-5},2.3305291073371062E-2,91,null,{"$f":"(AD108)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH108>0,(AJ108*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK107,NA())","v":0.19645544023919614},null,91,{"$f":"IF(AF108<=$J$9*0.05,AS107*EXP((-$J$6*1)/Heterogenität!$D$4),Z108)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF108>=$J$19, AR107/$J$5<AN108),0, Bodencharakterisierung!$E$8*$J$11*((AR107/$J$5)-AN108))","v":0},0,{"$f":"AQ107-AP108*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ108/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,91,null,{"$f":"(AP108)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF108<=$J$9*1.05,(AV108*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW107,NA())","v":{"$error":"#N/A"}},23072.238162637354,224,4.127265680239196,0.19645544023919614,0,0.57081024000000036,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},39.046596320178224,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,92,2.3305291073371062E-2,{"$f":"Z109*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF108*Bodencharakterisierung!$E$11/$J$20","v":4.0861766331401311E-5},{"$f":"((150*($J$2^0.87)*(AB109^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z109)*3600*24","v":7.8251112957352445E-2},2.3915996627248484E-4,{"$f":"AE108-AD109*Bodencharakterisierung!$E$8","v":5.907667063620009E-2},{"$f":"IF(AE109>$J$18,(AE109/(Bodencharakterisierung!$E$11*1000)),0)","v":3.8994502070099071E-5},2.3305291073371062E-2,92,null,{"$f":"(AD109)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH109>0,(AJ109*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK108,NA())","v":0.19862290749457193},null,92,{"$f":"IF(AF109<=$J$9*0.05,AS108*EXP((-$J$6*1)/Heterogenität!$D$4),Z109)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF109>=$J$19, AR108/$J$5<AN109),0, Bodencharakterisierung!$E$8*$J$11*((AR108/$J$5)-AN109))","v":0},0,{"$f":"AQ108-AP109*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ109/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,92,null,{"$f":"(AP109)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF109<=$J$9*1.05,(AV109*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW108,NA())","v":{"$error":"#N/A"}},23072.238162637354,225,4.1357057874945724,0.19862290749457193,0,0.57708288000000041,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},38.994502070099074,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,93,2.3305291073371062E-2,{"$f":"Z110*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF109*Bodencharakterisierung!$E$11/$J$20","v":4.0807250361392327E-5},{"$f":"((150*($J$2^0.87)*(AB110^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z110)*3600*24","v":7.8168626036965963E-2},2.3915996627248484E-4,{"$f":"AE109-AD110*Bodencharakterisierung!$E$8","v":5.8997747847330168E-2},{"$f":"IF(AE110>$J$18,(AE110/(Bodencharakterisierung!$E$11*1000)),0)","v":3.8942407820019915E-5},2.3305291073371062E-2,93,null,{"$f":"(AD110)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH110>0,(AJ110*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK109,NA())","v":0.20079037474994771},null,93,{"$f":"IF(AF110<=$J$9*0.05,AS109*EXP((-$J$6*1)/Heterogenität!$D$4),Z110)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF110>=$J$19, AR109/$J$5<AN110),0, Bodencharakterisierung!$E$8*$J$11*((AR109/$J$5)-AN110))","v":0},0,{"$f":"AQ109-AP110*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ110/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,93,null,{"$f":"(AP110)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF110<=$J$9*1.05,(AV110*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW109,NA())","v":{"$error":"#N/A"}},23072.238162637354,226,4.1441458947499479,0.20079037474994771,0,0.58335552000000046,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},38.942407820019916,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94,2.3305291073371062E-2,{"$f":"Z111*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF110*Bodencharakterisierung!$E$11/$J$20","v":4.075273439138333E-5},{"$f":"((150*($J$2^0.87)*(AB111^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z111)*3600*24","v":7.8086115971863268E-2},2.3915996627248484E-4,{"$f":"AE110-AD111*Bodencharakterisierung!$E$8","v":5.8918825058460245E-2},{"$f":"IF(AE111>$J$18,(AE111/(Bodencharakterisierung!$E$11*1000)),0)","v":3.8890313569940753E-5},2.3305291073371062E-2,94,null,{"$f":"(AD111)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH111>0,(AJ111*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK110,NA())","v":0.20295784200532349},null,94,{"$f":"IF(AF111<=$J$9*0.05,AS110*EXP((-$J$6*1)/Heterogenität!$D$4),Z111)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF111>=$J$19, AR110/$J$5<AN111),0, Bodencharakterisierung!$E$8*$J$11*((AR110/$J$5)-AN111))","v":0},0,{"$f":"AQ110-AP111*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ111/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,94,null,{"$f":"(AP111)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF111<=$J$9*1.05,(AV111*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW110,NA())","v":{"$error":"#N/A"}},23072.238162637354,227,4.1525860020053242,0.20295784200532349,0,0.58962816000000051,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},38.890313569940751,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,95,2.3305291073371062E-2,{"$f":"Z112*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF111*Bodencharakterisierung!$E$11/$J$20","v":4.0698218421374333E-5},{"$f":"((150*($J$2^0.87)*(AB112^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z112)*3600*24","v":7.8003582724575804E-2},2.3915996627248484E-4,{"$f":"AE111-AD112*Bodencharakterisierung!$E$8","v":5.8839902269590322E-2},{"$f":"IF(AE112>$J$18,(AE112/(Bodencharakterisierung!$E$11*1000)),0)","v":3.8838219319861598E-5},2.3305291073371062E-2,95,null,{"$f":"(AD112)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH112>0,(AJ112*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK111,NA())","v":0.20512530926069927},null,95,{"$f":"IF(AF112<=$J$9*0.05,AS111*EXP((-$J$6*1)/Heterogenität!$D$4),Z112)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF112>=$J$19, AR111/$J$5<AN112),0, Bodencharakterisierung!$E$8*$J$11*((AR111/$J$5)-AN112))","v":0},0,{"$f":"AQ111-AP112*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ112/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,95,null,{"$f":"(AP112)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF112<=$J$9*1.05,(AV112*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW111,NA())","v":{"$error":"#N/A"}},23072.238162637354,228,4.1610261092606997,0.20512530926069927,0,0.59590080000000056,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},38.838219319861601,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,96,2.3305291073371062E-2,{"$f":"Z113*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF112*Bodencharakterisierung!$E$11/$J$20","v":4.0643702451365342E-5},{"$f":"((150*($J$2^0.87)*(AB113^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z113)*3600*24","v":7.7921026257524437E-2},2.3915996627248484E-4,{"$f":"AE112-AD113*Bodencharakterisierung!$E$8","v":5.8760979480720399E-2},{"$f":"IF(AE113>$J$18,(AE113/(Bodencharakterisierung!$E$11*1000)),0)","v":3.8786125069782443E-5},2.3305291073371062E-2,96,null,{"$f":"(AD113)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH113>0,(AJ113*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK112,NA())","v":0.20729277651607506},null,96,{"$f":"IF(AF113<=$J$9*0.05,AS112*EXP((-$J$6*1)/Heterogenität!$D$4),Z113)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF113>=$J$19, AR112/$J$5<AN113),0, Bodencharakterisierung!$E$8*$J$11*((AR112/$J$5)-AN113))","v":0},0,{"$f":"AQ112-AP113*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ113/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,96,null,{"$f":"(AP113)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF113<=$J$9*1.05,(AV113*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW112,NA())","v":{"$error":"#N/A"}},23072.238162637354,229,4.1694662165160752,0.20729277651607506,0,0.60217344000000061,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},38.786125069782443,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,97,2.3305291073371062E-2,{"$f":"Z114*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF113*Bodencharakterisierung!$E$11/$J$20","v":4.0589186481356352E-5},{"$f":"((150*($J$2^0.87)*(AB114^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z114)*3600*24","v":7.7838446533018232E-2},2.3915996627248484E-4,{"$f":"AE113-AD114*Bodencharakterisierung!$E$8","v":5.8682056691850476E-2},{"$f":"IF(AE114>$J$18,(AE114/(Bodencharakterisierung!$E$11*1000)),0)","v":3.8734030819703288E-5},2.3305291073371062E-2,97,null,{"$f":"(AD114)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH114>0,(AJ114*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK113,NA())","v":0.20946024377145084},null,97,{"$f":"IF(AF114<=$J$9*0.05,AS113*EXP((-$J$6*1)/Heterogenität!$D$4),Z114)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF114>=$J$19, AR113/$J$5<AN114),0, Bodencharakterisierung!$E$8*$J$11*((AR113/$J$5)-AN114))","v":0},0,{"$f":"AQ113-AP114*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ114/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,97,null,{"$f":"(AP114)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF114<=$J$9*1.05,(AV114*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW113,NA())","v":{"$error":"#N/A"}},23072.238162637354,230,4.1779063237714515,0.20946024377145084,0,0.60844608000000067,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},38.734030819703285,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,98,2.3305291073371062E-2,{"$f":"Z115*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF114*Bodencharakterisierung!$E$11/$J$20","v":4.0534670511347361E-5},{"$f":"((150*($J$2^0.87)*(AB115^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z115)*3600*24","v":7.7755843513254652E-2},2.3915996627248484E-4,{"$f":"AE114-AD115*Bodencharakterisierung!$E$8","v":5.8603133902980553E-2},{"$f":"IF(AE115>$J$18,(AE115/(Bodencharakterisierung!$E$11*1000)),0)","v":3.8681936569624126E-5},2.3305291073371062E-2,98,null,{"$f":"(AD115)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH115>0,(AJ115*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK114,NA())","v":0.21162771102682662},null,98,{"$f":"IF(AF115<=$J$9*0.05,AS114*EXP((-$J$6*1)/Heterogenität!$D$4),Z115)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF115>=$J$19, AR114/$J$5<AN115),0, Bodencharakterisierung!$E$8*$J$11*((AR114/$J$5)-AN115))","v":0},0,{"$f":"AQ114-AP115*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ115/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,98,null,{"$f":"(AP115)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF115<=$J$9*1.05,(AV115*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW114,NA())","v":{"$error":"#N/A"}},23072.238162637354,231,4.186346431026827,0.21162771102682662,0,0.61471872000000072,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},38.681936569624128,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,99,2.3305291073371062E-2,{"$f":"Z116*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF115*Bodencharakterisierung!$E$11/$J$20","v":4.0480154541338364E-5},{"$f":"((150*($J$2^0.87)*(AB116^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z116)*3600*24","v":7.7673217160318525E-2},2.3915996627248484E-4,{"$f":"AE115-AD116*Bodencharakterisierung!$E$8","v":5.852421111411063E-2},{"$f":"IF(AE116>$J$18,(AE116/(Bodencharakterisierung!$E$11*1000)),0)","v":3.8629842319544971E-5},2.3305291073371062E-2,99,null,{"$f":"(AD116)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH116>0,(AJ116*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK115,NA())","v":0.2137951782822024},null,99,{"$f":"IF(AF116<=$J$9*0.05,AS115*EXP((-$J$6*1)/Heterogenität!$D$4),Z116)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF116>=$J$19, AR115/$J$5<AN116),0, Bodencharakterisierung!$E$8*$J$11*((AR115/$J$5)-AN116))","v":0},0,{"$f":"AQ115-AP116*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ116/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,99,null,{"$f":"(AP116)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF116<=$J$9*1.05,(AV116*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW115,NA())","v":{"$error":"#N/A"}},23072.238162637354,232,4.1947865382822034,0.2137951782822024,0,0.62099136000000077,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},38.62984231954497,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100,2.3305291073371062E-2,{"$f":"Z117*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF116*Bodencharakterisierung!$E$11/$J$20","v":4.0425638571329373E-5},{"$f":"((150*($J$2^0.87)*(AB117^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z117)*3600*24","v":7.7590567436182006E-2},2.3915996627248484E-4,{"$f":"AE116-AD117*Bodencharakterisierung!$E$8","v":5.8445288325240707E-2},{"$f":"IF(AE117>$J$18,(AE117/(Bodencharakterisierung!$E$11*1000)),0)","v":3.8577748069465815E-5},2.3305291073371062E-2,100,null,{"$f":"(AD117)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH117>0,(AJ117*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK116,NA())","v":0.21596264553757819},null,100,{"$f":"IF(AF117<=$J$9*0.05,AS116*EXP((-$J$6*1)/Heterogenität!$D$4),Z117)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF117>=$J$19, AR116/$J$5<AN117),0, Bodencharakterisierung!$E$8*$J$11*((AR116/$J$5)-AN117))","v":0},0,{"$f":"AQ116-AP117*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ117/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,100,null,{"$f":"(AP117)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF117<=$J$9*1.05,(AV117*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW116,NA())","v":{"$error":"#N/A"}},23072.238162637354,233,4.2032266455375789,0.21596264553757819,0,0.62726400000000082,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},38.577748069465812,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,101,2.3305291073371062E-2,{"$f":"Z118*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF117*Bodencharakterisierung!$E$11/$J$20","v":4.0371122601320376E-5},{"$f":"((150*($J$2^0.87)*(AB118^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z118)*3600*24","v":7.7507894302703814E-2},2.3915996627248484E-4,{"$f":"AE117-AD118*Bodencharakterisierung!$E$8","v":5.8366365536370785E-2},{"$f":"IF(AE118>$J$18,(AE118/(Bodencharakterisierung!$E$11*1000)),0)","v":3.8525653819386653E-5},2.3305291073371062E-2,101,null,{"$f":"(AD118)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH118>0,(AJ118*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK117,NA())","v":0.21813011279295397},null,101,{"$f":"IF(AF118<=$J$9*0.05,AS117*EXP((-$J$6*1)/Heterogenität!$D$4),Z118)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF118>=$J$19, AR117/$J$5<AN118),0, Bodencharakterisierung!$E$8*$J$11*((AR117/$J$5)-AN118))","v":0},0,{"$f":"AQ117-AP118*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ118/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,101,null,{"$f":"(AP118)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF118<=$J$9*1.05,(AV118*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW117,NA())","v":{"$error":"#N/A"}},23072.238162637354,234,4.2116667527929543,0.21813011279295397,0,0.63353664000000087,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},38.525653819386655,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,102,2.3305291073371062E-2,{"$f":"Z119*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF118*Bodencharakterisierung!$E$11/$J$20","v":4.0316606631311378E-5},{"$f":"((150*($J$2^0.87)*(AB119^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z119)*3600*24","v":7.7425197721628883E-2},2.3915996627248484E-4,{"$f":"AE118-AD119*Bodencharakterisierung!$E$8","v":5.8287442747500862E-2},{"$f":"IF(AE119>$J$18,(AE119/(Bodencharakterisierung!$E$11*1000)),0)","v":3.8473559569307498E-5},2.3305291073371062E-2,102,null,{"$f":"(AD119)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH119>0,(AJ119*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK118,NA())","v":0.22029758004832975},null,102,{"$f":"IF(AF119<=$J$9*0.05,AS118*EXP((-$J$6*1)/Heterogenität!$D$4),Z119)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF119>=$J$19, AR118/$J$5<AN119),0, Bodencharakterisierung!$E$8*$J$11*((AR118/$J$5)-AN119))","v":0},0,{"$f":"AQ118-AP119*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ119/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,102,null,{"$f":"(AP119)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF119<=$J$9*1.05,(AV119*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW118,NA())","v":{"$error":"#N/A"}},23072.238162637354,235,4.2201068600483307,0.22029758004832975,0,0.63980928000000092,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},38.473559569307497,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,103,2.3305291073371062E-2,{"$f":"Z120*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF119*Bodencharakterisierung!$E$11/$J$20","v":4.0262090661302394E-5},{"$f":"((150*($J$2^0.87)*(AB120^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z120)*3600*24","v":7.7342477654587807E-2},2.3915996627248484E-4,{"$f":"AE119-AD120*Bodencharakterisierung!$E$8","v":5.8208519958630939E-2},{"$f":"IF(AE120>$J$18,(AE120/(Bodencharakterisierung!$E$11*1000)),0)","v":3.8421465319228343E-5},2.3305291073371062E-2,103,null,{"$f":"(AD120)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH120>0,(AJ120*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK119,NA())","v":0.22246504730370553},null,103,{"$f":"IF(AF120<=$J$9*0.05,AS119*EXP((-$J$6*1)/Heterogenität!$D$4),Z120)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF120>=$J$19, AR119/$J$5<AN120),0, Bodencharakterisierung!$E$8*$J$11*((AR119/$J$5)-AN120))","v":0},0,{"$f":"AQ119-AP120*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ120/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,103,null,{"$f":"(AP120)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF120<=$J$9*1.05,(AV120*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW119,NA())","v":{"$error":"#N/A"}},23072.238162637354,236,4.2285469673037062,0.22246504730370553,0,0.64608192000000098,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},38.421465319228346,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,104,2.3305291073371062E-2,{"$f":"Z121*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF120*Bodencharakterisierung!$E$11/$J$20","v":4.0207574691293397E-5},{"$f":"((150*($J$2^0.87)*(AB121^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z121)*3600*24","v":7.7259734063096108E-2},2.3915996627248484E-4,{"$f":"AE120-AD121*Bodencharakterisierung!$E$8","v":5.8129597169761016E-2},{"$f":"IF(AE121>$J$18,(AE121/(Bodencharakterisierung!$E$11*1000)),0)","v":3.8369371069149188E-5},2.3305291073371062E-2,104,null,{"$f":"(AD121)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH121>0,(AJ121*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK120,NA())","v":0.22463251455908131},null,104,{"$f":"IF(AF121<=$J$9*0.05,AS120*EXP((-$J$6*1)/Heterogenität!$D$4),Z121)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF121>=$J$19, AR120/$J$5<AN121),0, Bodencharakterisierung!$E$8*$J$11*((AR120/$J$5)-AN121))","v":0},0,{"$f":"AQ120-AP121*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ121/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,104,null,{"$f":"(AP121)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF121<=$J$9*1.05,(AV121*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW120,NA())","v":{"$error":"#N/A"}},23072.238162637354,237,4.2369870745590825,0.22463251455908131,0,0.65235456000000103,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},38.369371069149189,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,105,2.3305291073371062E-2,{"$f":"Z122*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF121*Bodencharakterisierung!$E$11/$J$20","v":4.0153058721284406E-5},{"$f":"((150*($J$2^0.87)*(AB122^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z122)*3600*24","v":7.7176966908554467E-2},2.3915996627248484E-4,{"$f":"AE121-AD122*Bodencharakterisierung!$E$8","v":5.8050674380891093E-2},{"$f":"IF(AE122>$J$18,(AE122/(Bodencharakterisierung!$E$11*1000)),0)","v":3.8317276819070026E-5},2.3305291073371062E-2,105,null,{"$f":"(AD122)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH122>0,(AJ122*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK121,NA())","v":0.2267999818144571},null,105,{"$f":"IF(AF122<=$J$9*0.05,AS121*EXP((-$J$6*1)/Heterogenität!$D$4),Z122)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF122>=$J$19, AR121/$J$5<AN122),0, Bodencharakterisierung!$E$8*$J$11*((AR121/$J$5)-AN122))","v":0},0,{"$f":"AQ121-AP122*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ122/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,105,null,{"$f":"(AP122)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF122<=$J$9*1.05,(AV122*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW121,NA())","v":{"$error":"#N/A"}},23072.238162637354,238,4.245427181814458,0.2267999818144571,0,0.65862720000000108,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},38.317276819070024,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,106,2.3305291073371062E-2,{"$f":"Z123*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF122*Bodencharakterisierung!$E$11/$J$20","v":4.0098542751275409E-5},{"$f":"((150*($J$2^0.87)*(AB123^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z123)*3600*24","v":7.7094176152247257E-2},2.3915996627248484E-4,{"$f":"AE122-AD123*Bodencharakterisierung!$E$8","v":5.797175159202117E-2},{"$f":"IF(AE123>$J$18,(AE123/(Bodencharakterisierung!$E$11*1000)),0)","v":3.826518256899087E-5},2.3305291073371062E-2,106,null,{"$f":"(AD123)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH123>0,(AJ123*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK122,NA())","v":0.22896744906983288},null,106,{"$f":"IF(AF123<=$J$9*0.05,AS122*EXP((-$J$6*1)/Heterogenität!$D$4),Z123)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF123>=$J$19, AR122/$J$5<AN123),0, Bodencharakterisierung!$E$8*$J$11*((AR122/$J$5)-AN123))","v":0},0,{"$f":"AQ122-AP123*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ123/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,106,null,{"$f":"(AP123)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF123<=$J$9*1.05,(AV123*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW122,NA())","v":{"$error":"#N/A"}},23072.238162637354,239,4.2538672890698344,0.22896744906983288,0,0.66489984000000113,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},38.265182568990873,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,107,2.3305291073371062E-2,{"$f":"Z124*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF123*Bodencharakterisierung!$E$11/$J$20","v":4.0044026781266418E-5},{"$f":"((150*($J$2^0.87)*(AB124^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z124)*3600*24","v":7.7011361755342927E-2},2.3915996627248484E-4,{"$f":"AE123-AD124*Bodencharakterisierung!$E$8","v":5.7892828803151247E-2},{"$f":"IF(AE124>$J$18,(AE124/(Bodencharakterisierung!$E$11*1000)),0)","v":3.8213088318911715E-5},2.3305291073371062E-2,107,null,{"$f":"(AD124)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH124>0,(AJ124*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK123,NA())","v":0.23113491632520866},null,107,{"$f":"IF(AF124<=$J$9*0.05,AS123*EXP((-$J$6*1)/Heterogenität!$D$4),Z124)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF124>=$J$19, AR123/$J$5<AN124),0, Bodencharakterisierung!$E$8*$J$11*((AR123/$J$5)-AN124))","v":0},0,{"$f":"AQ123-AP124*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ124/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,107,null,{"$f":"(AP124)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF124<=$J$9*1.05,(AV124*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW123,NA())","v":{"$error":"#N/A"}},23072.238162637354,240,4.2623073963252098,0.23113491632520866,0,0.67117248000000118,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},38.213088318911716,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,108,2.3305291073371062E-2,{"$f":"Z125*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF124*Bodencharakterisierung!$E$11/$J$20","v":3.9989510811257428E-5},{"$f":"((150*($J$2^0.87)*(AB125^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z125)*3600*24","v":7.6928523678892524E-2},2.3915996627248484E-4,{"$f":"AE124-AD125*Bodencharakterisierung!$E$8","v":5.7813906014281324E-2},{"$f":"IF(AE125>$J$18,(AE125/(Bodencharakterisierung!$E$11*1000)),0)","v":3.816099406883256E-5},2.3305291073371062E-2,108,null,{"$f":"(AD125)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH125>0,(AJ125*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK124,NA())","v":0.23330238358058444},null,108,{"$f":"IF(AF125<=$J$9*0.05,AS124*EXP((-$J$6*1)/Heterogenität!$D$4),Z125)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF125>=$J$19, AR124/$J$5<AN125),0, Bodencharakterisierung!$E$8*$J$11*((AR124/$J$5)-AN125))","v":0},0,{"$f":"AQ124-AP125*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ125/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,108,null,{"$f":"(AP125)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF125<=$J$9*1.05,(AV125*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW124,NA())","v":{"$error":"#N/A"}},23072.238162637354,241,4.2707475035805853,0.23330238358058444,0,0.67744512000000123,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},38.160994068832558,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,109,2.3305291073371062E-2,{"$f":"Z126*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF125*Bodencharakterisierung!$E$11/$J$20","v":3.993499484124843E-5},{"$f":"((150*($J$2^0.87)*(AB126^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z126)*3600*24","v":7.6845661883830241E-2},2.3915996627248484E-4,{"$f":"AE125-AD126*Bodencharakterisierung!$E$8","v":5.7734983225411401E-2},{"$f":"IF(AE126>$J$18,(AE126/(Bodencharakterisierung!$E$11*1000)),0)","v":3.8108899818753398E-5},2.3305291073371062E-2,109,null,{"$f":"(AD126)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH126>0,(AJ126*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK125,NA())","v":0.23546985083596023},null,109,{"$f":"IF(AF126<=$J$9*0.05,AS125*EXP((-$J$6*1)/Heterogenität!$D$4),Z126)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF126>=$J$19, AR125/$J$5<AN126),0, Bodencharakterisierung!$E$8*$J$11*((AR125/$J$5)-AN126))","v":0},0,{"$f":"AQ125-AP126*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ126/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,109,null,{"$f":"(AP126)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF126<=$J$9*1.05,(AV126*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW125,NA())","v":{"$error":"#N/A"}},23072.238162637354,242,4.2791876108359617,0.23546985083596023,0,0.68371776000000128,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},38.1088998187534,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,110,2.3305291073371062E-2,{"$f":"Z127*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF126*Bodencharakterisierung!$E$11/$J$20","v":3.9880478871239433E-5},{"$f":"((150*($J$2^0.87)*(AB127^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z127)*3600*24","v":7.6762776330972185E-2},2.3915996627248484E-4,{"$f":"AE126-AD127*Bodencharakterisierung!$E$8","v":5.7656060436541479E-2},{"$f":"IF(AE127>$J$18,(AE127/(Bodencharakterisierung!$E$11*1000)),0)","v":3.8056805568674243E-5},2.3305291073371062E-2,110,null,{"$f":"(AD127)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH127>0,(AJ127*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK126,NA())","v":0.23763731809133601},null,110,{"$f":"IF(AF127<=$J$9*0.05,AS126*EXP((-$J$6*1)/Heterogenität!$D$4),Z127)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF127>=$J$19, AR126/$J$5<AN127),0, Bodencharakterisierung!$E$8*$J$11*((AR126/$J$5)-AN127))","v":0},0,{"$f":"AQ126-AP127*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ127/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,110,null,{"$f":"(AP127)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF127<=$J$9*1.05,(AV127*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW126,NA())","v":{"$error":"#N/A"}},23072.238162637354,243,4.2876277180913371,0.23763731809133601,0,0.68999040000000134,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},38.056805568674243,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,111,2.3305291073371062E-2,{"$f":"Z128*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF127*Bodencharakterisierung!$E$11/$J$20","v":3.9825962901230442E-5},{"$f":"((150*($J$2^0.87)*(AB128^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z128)*3600*24","v":7.6679866981016226E-2},2.3915996627248484E-4,{"$f":"AE127-AD128*Bodencharakterisierung!$E$8","v":5.7577137647671556E-2},{"$f":"IF(AE128>$J$18,(AE128/(Bodencharakterisierung!$E$11*1000)),0)","v":3.8004711318595088E-5},2.3305291073371062E-2,111,null,{"$f":"(AD128)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH128>0,(AJ128*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK127,NA())","v":0.23980478534671179},null,111,{"$f":"IF(AF128<=$J$9*0.05,AS127*EXP((-$J$6*1)/Heterogenität!$D$4),Z128)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF128>=$J$19, AR127/$J$5<AN128),0, Bodencharakterisierung!$E$8*$J$11*((AR127/$J$5)-AN128))","v":0},0,{"$f":"AQ127-AP128*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ128/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,111,null,{"$f":"(AP128)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF128<=$J$9*1.05,(AV128*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW127,NA())","v":{"$error":"#N/A"}},23072.238162637354,244,4.2960678253467126,0.23980478534671179,0,0.69626304000000139,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},38.004711318595085,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,112,2.3305291073371062E-2,{"$f":"Z129*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF128*Bodencharakterisierung!$E$11/$J$20","v":3.9771446931221452E-5},{"$f":"((150*($J$2^0.87)*(AB129^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z129)*3600*24","v":7.6596933794540967E-2},2.3915996627248484E-4,{"$f":"AE128-AD129*Bodencharakterisierung!$E$8","v":5.7498214858801633E-2},{"$f":"IF(AE129>$J$18,(AE129/(Bodencharakterisierung!$E$11*1000)),0)","v":3.7952617068515932E-5},2.3305291073371062E-2,112,null,{"$f":"(AD129)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH129>0,(AJ129*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK128,NA())","v":0.24197225260208757},null,112,{"$f":"IF(AF129<=$J$9*0.05,AS128*EXP((-$J$6*1)/Heterogenität!$D$4),Z129)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF129>=$J$19, AR128/$J$5<AN129),0, Bodencharakterisierung!$E$8*$J$11*((AR128/$J$5)-AN129))","v":0},0,{"$f":"AQ128-AP129*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ129/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,112,null,{"$f":"(AP129)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF129<=$J$9*1.05,(AV129*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW128,NA())","v":{"$error":"#N/A"}},23072.238162637354,245,4.304507932602089,0.24197225260208757,0,0.70253568000000144,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},37.952617068515934,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,113,2.3305291073371062E-2,{"$f":"Z130*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF129*Bodencharakterisierung!$E$11/$J$20","v":3.9716930961212461E-5},{"$f":"((150*($J$2^0.87)*(AB130^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z130)*3600*24","v":7.6513976732005995E-2},2.3915996627248484E-4,{"$f":"AE129-AD130*Bodencharakterisierung!$E$8","v":5.741929206993171E-2},{"$f":"IF(AE130>$J$18,(AE130/(Bodencharakterisierung!$E$11*1000)),0)","v":3.790052281843677E-5},2.3305291073371062E-2,113,null,{"$f":"(AD130)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH130>0,(AJ130*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK129,NA())","v":0.24413971985746336},null,113,{"$f":"IF(AF130<=$J$9*0.05,AS129*EXP((-$J$6*1)/Heterogenität!$D$4),Z130)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF130>=$J$19, AR129/$J$5<AN130),0, Bodencharakterisierung!$E$8*$J$11*((AR129/$J$5)-AN130))","v":0},0,{"$f":"AQ129-AP130*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ130/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,113,null,{"$f":"(AP130)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF130<=$J$9*1.05,(AV130*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW129,NA())","v":{"$error":"#N/A"}},23072.238162637354,246,4.3129480398574644,0.24413971985746336,0,0.70880832000000149,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},37.90052281843677,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,114,2.3305291073371062E-2,{"$f":"Z131*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF130*Bodencharakterisierung!$E$11/$J$20","v":3.9662414991203464E-5},{"$f":"((150*($J$2^0.87)*(AB131^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z131)*3600*24","v":7.6430995753750619E-2},2.3915996627248484E-4,{"$f":"AE130-AD131*Bodencharakterisierung!$E$8","v":5.7340369281061787E-2},{"$f":"IF(AE131>$J$18,(AE131/(Bodencharakterisierung!$E$11*1000)),0)","v":3.7848428568357615E-5},2.3305291073371062E-2,114,null,{"$f":"(AD131)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH131>0,(AJ131*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK130,NA())","v":0.24630718711283914},null,114,{"$f":"IF(AF131<=$J$9*0.05,AS130*EXP((-$J$6*1)/Heterogenität!$D$4),Z131)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF131>=$J$19, AR130/$J$5<AN131),0, Bodencharakterisierung!$E$8*$J$11*((AR130/$J$5)-AN131))","v":0},0,{"$f":"AQ130-AP131*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ131/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,114,null,{"$f":"(AP131)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF131<=$J$9*1.05,(AV131*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW130,NA())","v":{"$error":"#N/A"}},23072.238162637354,247,4.3213881471128408,0.24630718711283914,0,0.71508096000000154,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},37.848428568357612,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115,2.3305291073371062E-2,{"$f":"Z132*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF131*Bodencharakterisierung!$E$11/$J$20","v":3.9607899021194473E-5},{"$f":"((150*($J$2^0.87)*(AB132^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z132)*3600*24","v":7.6347990819993869E-2},2.3915996627248484E-4,{"$f":"AE131-AD132*Bodencharakterisierung!$E$8","v":5.7261446492191864E-2},{"$f":"IF(AE132>$J$18,(AE132/(Bodencharakterisierung!$E$11*1000)),0)","v":3.779633431827846E-5},2.3305291073371062E-2,115,null,{"$f":"(AD132)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH132>0,(AJ132*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK131,NA())","v":0.24847465436821492},null,115,{"$f":"IF(AF132<=$J$9*0.05,AS131*EXP((-$J$6*1)/Heterogenität!$D$4),Z132)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF132>=$J$19, AR131/$J$5<AN132),0, Bodencharakterisierung!$E$8*$J$11*((AR131/$J$5)-AN132))","v":0},0,{"$f":"AQ131-AP132*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ132/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,115,null,{"$f":"(AP132)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF132<=$J$9*1.05,(AV132*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW131,NA())","v":{"$error":"#N/A"}},23072.238162637354,248,4.3298282543682163,0.24847465436821492,0,0.72135360000000159,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},37.796334318278461,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,116,2.3305291073371062E-2,{"$f":"Z133*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF132*Bodencharakterisierung!$E$11/$J$20","v":3.9553383051185483E-5},{"$f":"((150*($J$2^0.87)*(AB133^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z133)*3600*24","v":7.6264961890833427E-2},2.3915996627248484E-4,{"$f":"AE132-AD133*Bodencharakterisierung!$E$8","v":5.7182523703321941E-2},{"$f":"IF(AE133>$J$18,(AE133/(Bodencharakterisierung!$E$11*1000)),0)","v":3.7744240068199298E-5},2.3305291073371062E-2,116,null,{"$f":"(AD133)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH133>0,(AJ133*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK132,NA())","v":0.25064212162359067},null,116,{"$f":"IF(AF133<=$J$9*0.05,AS132*EXP((-$J$6*1)/Heterogenität!$D$4),Z133)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF133>=$J$19, AR132/$J$5<AN133),0, Bodencharakterisierung!$E$8*$J$11*((AR132/$J$5)-AN133))","v":0},0,{"$f":"AQ132-AP133*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ133/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,116,null,{"$f":"(AP133)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF133<=$J$9*1.05,(AV133*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW132,NA())","v":{"$error":"#N/A"}},23072.238162637354,249,4.3382683616235926,0.25064212162359067,0,0.72762624000000165,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},37.744240068199296,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,117,2.3305291073371062E-2,{"$f":"Z134*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF133*Bodencharakterisierung!$E$11/$J$20","v":3.9498867081176485E-5},{"$f":"((150*($J$2^0.87)*(AB134^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z134)*3600*24","v":7.6181908926245934E-2},2.3915996627248484E-4,{"$f":"AE133-AD134*Bodencharakterisierung!$E$8","v":5.7103600914452018E-2},{"$f":"IF(AE134>$J$18,(AE134/(Bodencharakterisierung!$E$11*1000)),0)","v":3.7692145818120143E-5},2.3305291073371062E-2,117,null,{"$f":"(AD134)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH134>0,(AJ134*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK133,NA())","v":0.25280958887896643},null,117,{"$f":"IF(AF134<=$J$9*0.05,AS133*EXP((-$J$6*1)/Heterogenität!$D$4),Z134)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF134>=$J$19, AR133/$J$5<AN134),0, Bodencharakterisierung!$E$8*$J$11*((AR133/$J$5)-AN134))","v":0},0,{"$f":"AQ133-AP134*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ134/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,117,null,{"$f":"(AP134)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF134<=$J$9*1.05,(AV134*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW133,NA())","v":{"$error":"#N/A"}},23072.238162637354,250,4.3467084688789681,0.25280958887896643,0,0.7338988800000017,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},37.692145818120146,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,118,2.3305291073371062E-2,{"$f":"Z135*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF134*Bodencharakterisierung!$E$11/$J$20","v":3.9444351111167495E-5},{"$f":"((150*($J$2^0.87)*(AB135^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z135)*3600*24","v":7.6098831886085558E-2},2.3915996627248484E-4,{"$f":"AE134-AD135*Bodencharakterisierung!$E$8","v":5.7024678125582096E-2},{"$f":"IF(AE135>$J$18,(AE135/(Bodencharakterisierung!$E$11*1000)),0)","v":3.7640051568040987E-5},2.3305291073371062E-2,118,null,{"$f":"(AD135)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH135>0,(AJ135*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK134,NA())","v":0.25497705613434218},null,118,{"$f":"IF(AF135<=$J$9*0.05,AS134*EXP((-$J$6*1)/Heterogenität!$D$4),Z135)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF135>=$J$19, AR134/$J$5<AN135),0, Bodencharakterisierung!$E$8*$J$11*((AR134/$J$5)-AN135))","v":0},0,{"$f":"AQ134-AP135*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ135/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,118,null,{"$f":"(AP135)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF135<=$J$9*1.05,(AV135*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW134,NA())","v":{"$error":"#N/A"}},23072.238162637354,251,4.3551485761343436,0.25497705613434218,0,0.74017152000000175,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},37.640051568040988,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,119,2.3305291073371062E-2,{"$f":"Z136*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF135*Bodencharakterisierung!$E$11/$J$20","v":3.9389835141158497E-5},{"$f":"((150*($J$2^0.87)*(AB136^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z136)*3600*24","v":7.601573073008383E-2},2.3915996627248484E-4,{"$f":"AE135-AD136*Bodencharakterisierung!$E$8","v":5.6945755336712173E-2},{"$f":"IF(AE136>$J$18,(AE136/(Bodencharakterisierung!$E$11*1000)),0)","v":3.7587957317961832E-5},2.3305291073371062E-2,119,null,{"$f":"(AD136)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH136>0,(AJ136*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK135,NA())","v":0.25714452338971794},null,119,{"$f":"IF(AF136<=$J$9*0.05,AS135*EXP((-$J$6*1)/Heterogenität!$D$4),Z136)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF136>=$J$19, AR135/$J$5<AN136),0, Bodencharakterisierung!$E$8*$J$11*((AR135/$J$5)-AN136))","v":0},0,{"$f":"AQ135-AP136*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ136/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,119,null,{"$f":"(AP136)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF136<=$J$9*1.05,(AV136*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW135,NA())","v":{"$error":"#N/A"}},23072.238162637354,252,4.3635886833897199,0.25714452338971794,0,0.7464441600000018,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},37.58795731796183,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,120,2.3305291073371062E-2,{"$f":"Z137*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF136*Bodencharakterisierung!$E$11/$J$20","v":3.9335319171149513E-5},{"$f":"((150*($J$2^0.87)*(AB137^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z137)*3600*24","v":7.5932605417849242E-2},2.3915996627248484E-4,{"$f":"AE136-AD137*Bodencharakterisierung!$E$8","v":5.686683254784225E-2},{"$f":"IF(AE137>$J$18,(AE137/(Bodencharakterisierung!$E$11*1000)),0)","v":3.753586306788267E-5},2.3305291073371062E-2,120,null,{"$f":"(AD137)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH137>0,(AJ137*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK136,NA())","v":0.25931199064509369},null,120,{"$f":"IF(AF137<=$J$9*0.05,AS136*EXP((-$J$6*1)/Heterogenität!$D$4),Z137)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF137>=$J$19, AR136/$J$5<AN137),0, Bodencharakterisierung!$E$8*$J$11*((AR136/$J$5)-AN137))","v":0},0,{"$f":"AQ136-AP137*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ137/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,120,null,{"$f":"(AP137)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF137<=$J$9*1.05,(AV137*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW136,NA())","v":{"$error":"#N/A"}},23072.238162637354,253,4.3720287906450954,0.25931199064509369,0,0.75271680000000185,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},37.535863067882673,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,121,2.3305291073371062E-2,{"$f":"Z138*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF137*Bodencharakterisierung!$E$11/$J$20","v":3.9280803201140516E-5},{"$f":"((150*($J$2^0.87)*(AB138^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z138)*3600*24","v":7.5849455908866548E-2},2.3915996627248484E-4,{"$f":"AE137-AD138*Bodencharakterisierung!$E$8","v":5.6787909758972327E-2},{"$f":"IF(AE138>$J$18,(AE138/(Bodencharakterisierung!$E$11*1000)),0)","v":3.7483768817803515E-5},2.3305291073371062E-2,121,null,{"$f":"(AD138)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH138>0,(AJ138*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK137,NA())","v":0.26147945790046945},null,121,{"$f":"IF(AF138<=$J$9*0.05,AS137*EXP((-$J$6*1)/Heterogenität!$D$4),Z138)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF138>=$J$19, AR137/$J$5<AN138),0, Bodencharakterisierung!$E$8*$J$11*((AR137/$J$5)-AN138))","v":0},0,{"$f":"AQ137-AP138*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ138/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,121,null,{"$f":"(AP138)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF138<=$J$9*1.05,(AV138*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW137,NA())","v":{"$error":"#N/A"}},23072.238162637354,254,4.3804688979004709,0.26147945790046945,0,0.7589894400000019,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},37.483768817803515,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,122,2.3305291073371062E-2,{"$f":"Z139*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF138*Bodencharakterisierung!$E$11/$J$20","v":3.9226287231131519E-5},{"$f":"((150*($J$2^0.87)*(AB139^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z139)*3600*24","v":7.5766282162495993E-2},2.3915996627248484E-4,{"$f":"AE138-AD139*Bodencharakterisierung!$E$8","v":5.6708986970102404E-2},{"$f":"IF(AE139>$J$18,(AE139/(Bodencharakterisierung!$E$11*1000)),0)","v":3.743167456772436E-5},2.3305291073371062E-2,122,null,{"$f":"(AD139)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH139>0,(AJ139*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK138,NA())","v":0.2636469251558452},null,122,{"$f":"IF(AF139<=$J$9*0.05,AS138*EXP((-$J$6*1)/Heterogenität!$D$4),Z139)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF139>=$J$19, AR138/$J$5<AN139),0, Bodencharakterisierung!$E$8*$J$11*((AR138/$J$5)-AN139))","v":0},0,{"$f":"AQ138-AP139*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ139/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,122,null,{"$f":"(AP139)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF139<=$J$9*1.05,(AV139*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW138,NA())","v":{"$error":"#N/A"}},23072.238162637354,255,4.3889090051558473,0.2636469251558452,0,0.76526208000000195,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},37.431674567724357,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,123,2.3305291073371062E-2,{"$f":"Z140*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF139*Bodencharakterisierung!$E$11/$J$20","v":3.9171771261122528E-5},{"$f":"((150*($J$2^0.87)*(AB140^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z140)*3600*24","v":7.5683084137973214E-2},2.3915996627248484E-4,{"$f":"AE139-AD140*Bodencharakterisierung!$E$8","v":5.6630064181232481E-2},{"$f":"IF(AE140>$J$18,(AE140/(Bodencharakterisierung!$E$11*1000)),0)","v":3.7379580317645204E-5},2.3305291073371062E-2,123,null,{"$f":"(AD140)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH140>0,(AJ140*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK139,NA())","v":0.26581439241122096},null,123,{"$f":"IF(AF140<=$J$9*0.05,AS139*EXP((-$J$6*1)/Heterogenität!$D$4),Z140)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF140>=$J$19, AR139/$J$5<AN140),0, Bodencharakterisierung!$E$8*$J$11*((AR139/$J$5)-AN140))","v":0},0,{"$f":"AQ139-AP140*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ140/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,123,null,{"$f":"(AP140)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF140<=$J$9*1.05,(AV140*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW139,NA())","v":{"$error":"#N/A"}},23072.238162637354,256,4.3973491124112227,0.26581439241122096,0,0.77153472000000201,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},37.379580317645207,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,124,2.3305291073371062E-2,{"$f":"Z141*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF140*Bodencharakterisierung!$E$11/$J$20","v":3.9117255291113538E-5},{"$f":"((150*($J$2^0.87)*(AB141^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z141)*3600*24","v":7.5599861794408529E-2},2.3915996627248484E-4,{"$f":"AE140-AD141*Bodencharakterisierung!$E$8","v":5.6551141392362558E-2},{"$f":"IF(AE141>$J$18,(AE141/(Bodencharakterisierung!$E$11*1000)),0)","v":3.7327486067566042E-5},2.3305291073371062E-2,124,null,{"$f":"(AD141)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH141>0,(AJ141*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK140,NA())","v":0.26798185966659671},null,124,{"$f":"IF(AF141<=$J$9*0.05,AS140*EXP((-$J$6*1)/Heterogenität!$D$4),Z141)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF141>=$J$19, AR140/$J$5<AN141),0, Bodencharakterisierung!$E$8*$J$11*((AR140/$J$5)-AN141))","v":0},0,{"$f":"AQ140-AP141*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ141/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,124,null,{"$f":"(AP141)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF141<=$J$9*1.05,(AV141*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW140,NA())","v":{"$error":"#N/A"}},23072.238162637354,257,4.4057892196665982,0.26798185966659671,0,0.77780736000000206,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},37.327486067566042,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,125,2.3305291073371062E-2,{"$f":"Z142*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF141*Bodencharakterisierung!$E$11/$J$20","v":3.9062739321104533E-5},{"$f":"((150*($J$2^0.87)*(AB142^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z142)*3600*24","v":7.5516615090785916E-2},2.3915996627248484E-4,{"$f":"AE141-AD142*Bodencharakterisierung!$E$8","v":5.6472218603492635E-2},{"$f":"IF(AE142>$J$18,(AE142/(Bodencharakterisierung!$E$11*1000)),0)","v":3.7275391817486887E-5},2.3305291073371062E-2,125,null,{"$f":"(AD142)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH142>0,(AJ142*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK141,NA())","v":0.27014932692197247},null,125,{"$f":"IF(AF142<=$J$9*0.05,AS141*EXP((-$J$6*1)/Heterogenität!$D$4),Z142)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF142>=$J$19, AR141/$J$5<AN142),0, Bodencharakterisierung!$E$8*$J$11*((AR141/$J$5)-AN142))","v":0},0,{"$f":"AQ141-AP142*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ142/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,125,null,{"$f":"(AP142)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF142<=$J$9*1.05,(AV142*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW141,NA())","v":{"$error":"#N/A"}},23072.238162637354,258,4.4142293269219746,0.27014932692197247,0,0.78408000000000211,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},37.275391817486884,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,126,2.3305291073371062E-2,{"$f":"Z143*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF142*Bodencharakterisierung!$E$11/$J$20","v":3.900822335109555E-5},{"$f":"((150*($J$2^0.87)*(AB143^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z143)*3600*24","v":7.5433343985963144E-2},2.3915996627248484E-4,{"$f":"AE142-AD143*Bodencharakterisierung!$E$8","v":5.6393295814622713E-2},{"$f":"IF(AE143>$J$18,(AE143/(Bodencharakterisierung!$E$11*1000)),0)","v":3.7223297567407732E-5},2.3305291073371062E-2,126,null,{"$f":"(AD143)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH143>0,(AJ143*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK142,NA())","v":0.27231679417734822},null,126,{"$f":"IF(AF143<=$J$9*0.05,AS142*EXP((-$J$6*1)/Heterogenität!$D$4),Z143)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF143>=$J$19, AR142/$J$5<AN143),0, Bodencharakterisierung!$E$8*$J$11*((AR142/$J$5)-AN143))","v":0},0,{"$f":"AQ142-AP143*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ143/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,126,null,{"$f":"(AP143)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF143<=$J$9*1.05,(AV143*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW142,NA())","v":{"$error":"#N/A"}},23072.238162637354,259,4.42266943417735,0.27231679417734822,0,0.79035264000000216,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},37.223297567407734,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,127,2.3305291073371062E-2,{"$f":"Z144*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF143*Bodencharakterisierung!$E$11/$J$20","v":3.8953707381086552E-5},{"$f":"((150*($J$2^0.87)*(AB144^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z144)*3600*24","v":7.5350048438671019E-2},2.3915996627248484E-4,{"$f":"AE143-AD144*Bodencharakterisierung!$E$8","v":5.631437302575279E-2},{"$f":"IF(AE144>$J$18,(AE144/(Bodencharakterisierung!$E$11*1000)),0)","v":3.7171203317328577E-5},2.3305291073371062E-2,127,null,{"$f":"(AD144)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH144>0,(AJ144*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK143,NA())","v":0.27448426143272397},null,127,{"$f":"IF(AF144<=$J$9*0.05,AS143*EXP((-$J$6*1)/Heterogenität!$D$4),Z144)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF144>=$J$19, AR143/$J$5<AN144),0, Bodencharakterisierung!$E$8*$J$11*((AR143/$J$5)-AN144))","v":0},0,{"$f":"AQ143-AP144*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ144/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,127,null,{"$f":"(AP144)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF144<=$J$9*1.05,(AV144*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW143,NA())","v":{"$error":"#N/A"}},23072.238162637354,260,4.4311095414327255,0.27448426143272397,0,0.79662528000000221,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},37.171203317328576,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,128,2.3305291073371062E-2,{"$f":"Z145*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF144*Bodencharakterisierung!$E$11/$J$20","v":3.8899191411077568E-5},{"$f":"((150*($J$2^0.87)*(AB145^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z145)*3600*24","v":7.5266728407512168E-2},2.3915996627248484E-4,{"$f":"AE144-AD145*Bodencharakterisierung!$E$8","v":5.6235450236882867E-2},{"$f":"IF(AE145>$J$18,(AE145/(Bodencharakterisierung!$E$11*1000)),0)","v":3.7119109067249415E-5},2.3305291073371062E-2,128,null,{"$f":"(AD145)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH145>0,(AJ145*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK144,NA())","v":0.27665172868809973},null,128,{"$f":"IF(AF145<=$J$9*0.05,AS144*EXP((-$J$6*1)/Heterogenität!$D$4),Z145)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF145>=$J$19, AR144/$J$5<AN145),0, Bodencharakterisierung!$E$8*$J$11*((AR144/$J$5)-AN145))","v":0},0,{"$f":"AQ144-AP145*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ145/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,128,null,{"$f":"(AP145)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF145<=$J$9*1.05,(AV145*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW144,NA())","v":{"$error":"#N/A"}},23072.238162637354,261,4.4395496486881019,0.27665172868809973,0,0.80289792000000226,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},37.119109067249411,{"$f":"AN145*10^6","v":23305.291073371063}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,129,2.3305291073371062E-2,{"$f":"Z146*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF145*Bodencharakterisierung!$E$11/$J$20","v":3.8844675441068564E-5},{"$f":"((150*($J$2^0.87)*(AB146^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z146)*3600*24","v":7.5183383850961544E-2},2.3915996627248484E-4,{"$f":"AE145-AD146*Bodencharakterisierung!$E$8","v":5.6156527448012944E-2},{"$f":"IF(AE146>$J$18,(AE146/(Bodencharakterisierung!$E$11*1000)),0)","v":3.706701481717026E-5},2.3305291073371062E-2,129,null,{"$f":"(AD146)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH146>0,(AJ146*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK145,NA())","v":0.27881919594347548},null,129,{"$f":"IF(AF146<=$J$9*0.05,AS145*EXP((-$J$6*1)/Heterogenität!$D$4),Z146)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF146>=$J$19, AR145/$J$5<AN146),0, Bodencharakterisierung!$E$8*$J$11*((AR145/$J$5)-AN146))","v":0},0,{"$f":"AQ145-AP146*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ146/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,{"$f":"IF(AN146>$G$5,AM146,NA())","v":129},null,{"$f":"(AP146)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF146<=$J$9*1.05,(AV146*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW145,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH146>($G$5*10^6),BH146*0.99,9999)","v":23072.238162637354},{"$f":"AT146+$G$3","v":262},4.4479897559434782,0.27881919594347548,0,0.80917056000000231,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF146*10^6","v":37.067014817170261},23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,130,{"$f":"AG146","v":2.3305291073371062E-2},{"$f":"Z147*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF146*Bodencharakterisierung!$E$11/$J$20","v":3.8790159471059574E-5},{"$f":"((150*($J$2^0.87)*(AB147^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z147)*3600*24","v":7.5100014727364856E-2},{"$f":"MIN(AC147,Z147-AA147)","v":2.3915996627248484E-4},{"$f":"AE146-AD147*Bodencharakterisierung!$E$8","v":5.6077604659143021E-2},{"$f":"IF(AE147>$J$18,(AE147/(Bodencharakterisierung!$E$11*1000)),0)","v":3.7014920567091104E-5},{"$f":"AA147+AD147","v":2.3305291073371062E-2},{"$f":"IF(AD147>0,Y147,NA())","v":130},null,{"$f":"(AD147)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH147>0,(AJ147*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK146,NA())","v":0.28098666319885124},null,130,{"$f":"IF(AF147<=$J$9*0.05,AS146*EXP((-$J$6*1)/Heterogenität!$D$4),Z147)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF147>=$J$19, AR146/$J$5<AN147),0, Bodencharakterisierung!$E$8*$J$11*((AR146/$J$5)-AN147))","v":0},0,{"$f":"AQ146-AP147*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ147/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},{"$f":"AN147+AP147","v":2.3305291073371062E-2},130,null,{"$f":"(AP147)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF147<=$J$9*1.05,(AV147*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW146,NA())","v":{"$error":"#N/A"}},23072.238162637354,263,{"$f":"IF(ISNUMBER(AT147),BA147+BB147+BC147+$AZ$17,\"\")","v":4.4564298631988537},{"$f":"IF(ISNUMBER(AK147),AK147,BA146)","v":0.28098666319885124},{"$f":"IF(ISNUMBER(AW147),AW147,0)","v":0},0.81544320000000237,null,{"$f":"AR147*10^6","v":4.3827000000643475},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},37.014920567091103,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,131,2.3305291073371062E-2,{"$f":"Z148*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF147*Bodencharakterisierung!$E$11/$J$20","v":3.8735643501050583E-5},{"$f":"((150*($J$2^0.87)*(AB148^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z148)*3600*24","v":7.5016620994938832E-2},2.3915996627248484E-4,{"$f":"AE147-AD148*Bodencharakterisierung!$E$8","v":5.5998681870273098E-2},{"$f":"IF(AE148>$J$18,(AE148/(Bodencharakterisierung!$E$11*1000)),0)","v":3.6962826317011949E-5},2.3305291073371062E-2,131,null,{"$f":"(AD148)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH148>0,(AJ148*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK147,NA())","v":0.28315413045422699},null,131,{"$f":"IF(AF148<=$J$9*0.05,AS147*EXP((-$J$6*1)/Heterogenität!$D$4),Z148)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF148>=$J$19, AR147/$J$5<AN148),0, Bodencharakterisierung!$E$8*$J$11*((AR147/$J$5)-AN148))","v":0},{"$f":"MIN(AO148,AS147-AN148)","v":0},{"$f":"AQ147-AP148*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ148/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,131,null,{"$f":"(AP148)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF148<=$J$9*1.05,(AV148*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW147,NA())","v":{"$error":"#N/A"}},23072.238162637354,264,4.4648699704542292,0.28315413045422699,0,{"$f":"$G$34/$G$12/$G$8+BC147","v":0.82171584000000242},null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},36.962826317011952,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,132,2.3305291073371062E-2,{"$f":"Z149*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF148*Bodencharakterisierung!$E$11/$J$20","v":3.8681127531041592E-5},{"$f":"((150*($J$2^0.87)*(AB149^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z149)*3600*24","v":7.4933202611769653E-2},2.3915996627248484E-4,{"$f":"AE148-AD149*Bodencharakterisierung!$E$8","v":5.5919759081403175E-2},{"$f":"IF(AE149>$J$18,(AE149/(Bodencharakterisierung!$E$11*1000)),0)","v":3.6910732066932787E-5},2.3305291073371062E-2,132,null,{"$f":"(AD149)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH149>0,(AJ149*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK148,NA())","v":0.28532159770960275},null,132,{"$f":"IF(AF149<=$J$9*0.05,AS148*EXP((-$J$6*1)/Heterogenität!$D$4),Z149)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF149>=$J$19, AR148/$J$5<AN149),0, Bodencharakterisierung!$E$8*$J$11*((AR148/$J$5)-AN149))","v":0},0,{"$f":"AQ148-AP149*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ149/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,132,null,{"$f":"(AP149)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF149<=$J$9*1.05,(AV149*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW148,NA())","v":{"$error":"#N/A"}},23072.238162637354,265,4.4733100777096055,0.28532159770960275,0,0.82798848000000247,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},36.910732066932788,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133,2.3305291073371062E-2,{"$f":"Z150*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF149*Bodencharakterisierung!$E$11/$J$20","v":3.8626611561032595E-5},{"$f":"((150*($J$2^0.87)*(AB150^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z150)*3600*24","v":7.4849759535813534E-2},2.3915996627248484E-4,{"$f":"AE149-AD150*Bodencharakterisierung!$E$8","v":5.5840836292533252E-2},{"$f":"IF(AE150>$J$18,(AE150/(Bodencharakterisierung!$E$11*1000)),0)","v":3.6858637816853632E-5},2.3305291073371062E-2,133,null,{"$f":"(AD150)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH150>0,(AJ150*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK149,NA())","v":0.2874890649649785},null,133,{"$f":"IF(AF150<=$J$9*0.05,AS149*EXP((-$J$6*1)/Heterogenität!$D$4),Z150)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF150>=$J$19, AR149/$J$5<AN150),0, Bodencharakterisierung!$E$8*$J$11*((AR149/$J$5)-AN150))","v":0},0,{"$f":"AQ149-AP150*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ150/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,133,null,{"$f":"(AP150)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF150<=$J$9*1.05,(AV150*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW149,NA())","v":{"$error":"#N/A"}},23072.238162637354,266,4.481750184964981,0.2874890649649785,0,0.83426112000000252,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},36.85863781685363,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,134,{"$f":"AG150","v":2.3305291073371062E-2},{"$f":"Z151*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF150*Bodencharakterisierung!$E$11/$J$20","v":3.8572095591023604E-5},{"$f":"((150*($J$2^0.87)*(AB151^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z151)*3600*24","v":7.4766291724895073E-2},{"$f":"MIN(AC151,Z151-AA151)","v":2.3915996627248484E-4},{"$f":"AE150-AD151*Bodencharakterisierung!$E$8","v":5.576191350366333E-2},{"$f":"IF(AE151>$J$18,(AE151/(Bodencharakterisierung!$E$11*1000)),0)","v":3.6806543566774477E-5},{"$f":"AA151+AD151","v":2.3305291073371062E-2},{"$f":"IF(AD151>0,Y151,NA())","v":134},null,{"$f":"(AD151)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH151>0,(AJ151*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK150,NA())","v":0.28965653222035426},null,134,{"$f":"IF(AF151<=$J$9*0.05,AS150*EXP((-$J$6*1)/Heterogenität!$D$4),Z151)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF151>=$J$19, AR150/$J$5<AN151),0, Bodencharakterisierung!$E$8*$J$11*((AR150/$J$5)-AN151))","v":0},{"$f":"MIN(AO151,AS150-AN151)","v":0},{"$f":"AQ150-AP151*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ151/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},{"$f":"AN151+AP151","v":2.3305291073371062E-2},{"$f":"IF(AN151>$G$5,AM151,NA())","v":134},null,{"$f":"(AP151)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF151<=$J$9*1.05,(AV151*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW150,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH151>($G$5*10^6),BH151*0.99,9999)","v":23072.238162637354},{"$f":"AT151+$G$3","v":267},{"$f":"IF(ISNUMBER(AT151),BA151+BB151+BC151+$AZ$17,\"\")","v":4.4901902922203565},{"$f":"IF(ISNUMBER(AK151),AK151,BA150)","v":0.28965653222035426},{"$f":"IF(ISNUMBER(AW151),AW151,0)","v":0},0.84053376000000257,null,{"$f":"AR151*10^6","v":4.3827000000643475},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF151*10^6","v":36.806543566774479},{"$f":"AN151*10^6","v":23305.291073371063}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,135,2.3305291073371062E-2,{"$f":"Z152*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF151*Bodencharakterisierung!$E$11/$J$20","v":3.8517579621014614E-5},{"$f":"((150*($J$2^0.87)*(AB152^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z152)*3600*24","v":7.4682799136707528E-2},2.3915996627248484E-4,{"$f":"AE151-AD152*Bodencharakterisierung!$E$8","v":5.5682990714793407E-2},{"$f":"IF(AE152>$J$18,(AE152/(Bodencharakterisierung!$E$11*1000)),0)","v":3.6754449316695315E-5},2.3305291073371062E-2,135,null,{"$f":"(AD152)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH152>0,(AJ152*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK151,NA())","v":0.29182399947573001},null,135,{"$f":"IF(AF152<=$J$9*0.05,AS151*EXP((-$J$6*1)/Heterogenität!$D$4),Z152)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF152>=$J$19, AR151/$J$5<AN152),0, Bodencharakterisierung!$E$8*$J$11*((AR151/$J$5)-AN152))","v":0},0,{"$f":"AQ151-AP152*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ152/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,135,null,{"$f":"(AP152)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF152<=$J$9*1.05,(AV152*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW151,NA())","v":{"$error":"#N/A"}},23072.238162637354,268,4.4986303994757328,0.29182399947573001,0,0.84680640000000262,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},36.754449316695315,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,136,2.3305291073371062E-2,{"$f":"Z153*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF152*Bodencharakterisierung!$E$11/$J$20","v":3.8463063651005616E-5},{"$f":"((150*($J$2^0.87)*(AB153^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z153)*3600*24","v":7.4599281728811445E-2},2.3915996627248484E-4,{"$f":"AE152-AD153*Bodencharakterisierung!$E$8","v":5.5604067925923484E-2},{"$f":"IF(AE153>$J$18,(AE153/(Bodencharakterisierung!$E$11*1000)),0)","v":3.6702355066616159E-5},2.3305291073371062E-2,136,null,{"$f":"(AD153)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH153>0,(AJ153*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK152,NA())","v":0.29399146673110577},null,136,{"$f":"IF(AF153<=$J$9*0.05,AS152*EXP((-$J$6*1)/Heterogenität!$D$4),Z153)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF153>=$J$19, AR152/$J$5<AN153),0, Bodencharakterisierung!$E$8*$J$11*((AR152/$J$5)-AN153))","v":0},0,{"$f":"AQ152-AP153*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ153/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,136,null,{"$f":"(AP153)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF153<=$J$9*1.05,(AV153*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW152,NA())","v":{"$error":"#N/A"}},23072.238162637354,269,4.5070705067311083,0.29399146673110577,0,0.85307904000000268,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},36.702355066616157,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,137,2.3305291073371062E-2,{"$f":"Z154*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF153*Bodencharakterisierung!$E$11/$J$20","v":3.8408547680996619E-5},{"$f":"((150*($J$2^0.87)*(AB154^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z154)*3600*24","v":7.4515739458634447E-2},2.3915996627248484E-4,{"$f":"AE153-AD154*Bodencharakterisierung!$E$8","v":5.5525145137053561E-2},{"$f":"IF(AE154>$J$18,(AE154/(Bodencharakterisierung!$E$11*1000)),0)","v":3.6650260816537004E-5},2.3305291073371062E-2,137,null,{"$f":"(AD154)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH154>0,(AJ154*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK153,NA())","v":0.29615893398648152},null,137,{"$f":"IF(AF154<=$J$9*0.05,AS153*EXP((-$J$6*1)/Heterogenität!$D$4),Z154)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF154>=$J$19, AR153/$J$5<AN154),0, Bodencharakterisierung!$E$8*$J$11*((AR153/$J$5)-AN154))","v":0},0,{"$f":"AQ153-AP154*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ154/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,137,null,{"$f":"(AP154)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF154<=$J$9*1.05,(AV154*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW153,NA())","v":{"$error":"#N/A"}},23072.238162637354,270,4.5155106139864838,0.29615893398648152,0,0.85935168000000273,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},36.650260816537006,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,138,2.3305291073371062E-2,{"$f":"Z155*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF154*Bodencharakterisierung!$E$11/$J$20","v":3.8354031710987635E-5},{"$f":"((150*($J$2^0.87)*(AB155^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z155)*3600*24","v":7.4432172283470974E-2},2.3915996627248484E-4,{"$f":"AE154-AD155*Bodencharakterisierung!$E$8","v":5.5446222348183638E-2},{"$f":"IF(AE155>$J$18,(AE155/(Bodencharakterisierung!$E$11*1000)),0)","v":3.6598166566457849E-5},2.3305291073371062E-2,138,null,{"$f":"(AD155)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH155>0,(AJ155*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK154,NA())","v":0.29832640124185728},null,138,{"$f":"IF(AF155<=$J$9*0.05,AS154*EXP((-$J$6*1)/Heterogenität!$D$4),Z155)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF155>=$J$19, AR154/$J$5<AN155),0, Bodencharakterisierung!$E$8*$J$11*((AR154/$J$5)-AN155))","v":0},0,{"$f":"AQ154-AP155*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ155/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,138,null,{"$f":"(AP155)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF155<=$J$9*1.05,(AV155*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW154,NA())","v":{"$error":"#N/A"}},23072.238162637354,271,4.5239507212418602,0.29832640124185728,0,0.86562432000000278,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},36.598166566457849,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,139,2.3305291073371062E-2,{"$f":"Z156*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF155*Bodencharakterisierung!$E$11/$J$20","v":3.8299515740978638E-5},{"$f":"((150*($J$2^0.87)*(AB156^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z156)*3600*24","v":7.4348580160480751E-2},2.3915996627248484E-4,{"$f":"AE155-AD156*Bodencharakterisierung!$E$8","v":5.5367299559313715E-2},{"$f":"IF(AE156>$J$18,(AE156/(Bodencharakterisierung!$E$11*1000)),0)","v":3.6546072316378687E-5},2.3305291073371062E-2,139,null,{"$f":"(AD156)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH156>0,(AJ156*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK155,NA())","v":0.30049386849723303},null,139,{"$f":"IF(AF156<=$J$9*0.05,AS155*EXP((-$J$6*1)/Heterogenität!$D$4),Z156)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF156>=$J$19, AR155/$J$5<AN156),0, Bodencharakterisierung!$E$8*$J$11*((AR155/$J$5)-AN156))","v":0},0,{"$f":"AQ155-AP156*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ156/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,139,null,{"$f":"(AP156)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF156<=$J$9*1.05,(AV156*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW155,NA())","v":{"$error":"#N/A"}},23072.238162637354,272,4.5323908284972356,0.30049386849723303,0,0.87189696000000283,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},36.546072316378684,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,140,2.3305291073371062E-2,{"$f":"Z157*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF156*Bodencharakterisierung!$E$11/$J$20","v":3.8244999770969641E-5},{"$f":"((150*($J$2^0.87)*(AB157^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z157)*3600*24","v":7.426496304668917E-2},2.3915996627248484E-4,{"$f":"AE156-AD157*Bodencharakterisierung!$E$8","v":5.5288376770443792E-2},{"$f":"IF(AE157>$J$18,(AE157/(Bodencharakterisierung!$E$11*1000)),0)","v":3.6493978066299532E-5},2.3305291073371062E-2,140,null,{"$f":"(AD157)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH157>0,(AJ157*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK156,NA())","v":0.30266133575260878},null,140,{"$f":"IF(AF157<=$J$9*0.05,AS156*EXP((-$J$6*1)/Heterogenität!$D$4),Z157)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF157>=$J$19, AR156/$J$5<AN157),0, Bodencharakterisierung!$E$8*$J$11*((AR156/$J$5)-AN157))","v":0},0,{"$f":"AQ156-AP157*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ157/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,140,null,{"$f":"(AP157)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF157<=$J$9*1.05,(AV157*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW156,NA())","v":{"$error":"#N/A"}},23072.238162637354,273,4.5408309357526111,0.30266133575260878,0,0.87816960000000288,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},36.493978066299533,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,141,2.3305291073371062E-2,{"$f":"Z158*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF157*Bodencharakterisierung!$E$11/$J$20","v":3.819048380096065E-5},{"$f":"((150*($J$2^0.87)*(AB158^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z158)*3600*24","v":7.4181320898986006E-2},2.3915996627248484E-4,{"$f":"AE157-AD158*Bodencharakterisierung!$E$8","v":5.5209453981573869E-2},{"$f":"IF(AE158>$J$18,(AE158/(Bodencharakterisierung!$E$11*1000)),0)","v":3.6441883816220377E-5},2.3305291073371062E-2,141,null,{"$f":"(AD158)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH158>0,(AJ158*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK157,NA())","v":0.30482880300798454},null,141,{"$f":"IF(AF158<=$J$9*0.05,AS157*EXP((-$J$6*1)/Heterogenität!$D$4),Z158)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF158>=$J$19, AR157/$J$5<AN158),0, Bodencharakterisierung!$E$8*$J$11*((AR157/$J$5)-AN158))","v":0},0,{"$f":"AQ157-AP158*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ158/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,141,null,{"$f":"(AP158)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF158<=$J$9*1.05,(AV158*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW157,NA())","v":{"$error":"#N/A"}},23072.238162637354,274,4.5492710430079875,0.30482880300798454,0,0.88444224000000293,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},36.441883816220376,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,142,2.3305291073371062E-2,{"$f":"Z159*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF158*Bodencharakterisierung!$E$11/$J$20","v":3.8135967830951659E-5},{"$f":"((150*($J$2^0.87)*(AB159^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z159)*3600*24","v":7.4097653674125005E-2},2.3915996627248484E-4,{"$f":"AE158-AD159*Bodencharakterisierung!$E$8","v":5.5130531192703947E-2},{"$f":"IF(AE159>$J$18,(AE159/(Bodencharakterisierung!$E$11*1000)),0)","v":3.6389789566141221E-5},2.3305291073371062E-2,142,null,{"$f":"(AD159)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH159>0,(AJ159*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK158,NA())","v":0.30699627026336029},null,142,{"$f":"IF(AF159<=$J$9*0.05,AS158*EXP((-$J$6*1)/Heterogenität!$D$4),Z159)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF159>=$J$19, AR158/$J$5<AN159),0, Bodencharakterisierung!$E$8*$J$11*((AR158/$J$5)-AN159))","v":0},0,{"$f":"AQ158-AP159*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ159/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,142,null,{"$f":"(AP159)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF159<=$J$9*1.05,(AV159*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW158,NA())","v":{"$error":"#N/A"}},23072.238162637354,275,4.5577111502633629,0.30699627026336029,0,0.89071488000000298,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},36.389789566141218,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,143,2.3305291073371062E-2,{"$f":"Z160*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF159*Bodencharakterisierung!$E$11/$J$20","v":3.8081451860942669E-5},{"$f":"((150*($J$2^0.87)*(AB160^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z160)*3600*24","v":7.4013961328723329E-2},2.3915996627248484E-4,{"$f":"AE159-AD160*Bodencharakterisierung!$E$8","v":5.5051608403834024E-2},{"$f":"IF(AE160>$J$18,(AE160/(Bodencharakterisierung!$E$11*1000)),0)","v":3.6337695316062059E-5},2.3305291073371062E-2,143,null,{"$f":"(AD160)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH160>0,(AJ160*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK159,NA())","v":0.30916373751873605},null,143,{"$f":"IF(AF160<=$J$9*0.05,AS159*EXP((-$J$6*1)/Heterogenität!$D$4),Z160)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF160>=$J$19, AR159/$J$5<AN160),0, Bodencharakterisierung!$E$8*$J$11*((AR159/$J$5)-AN160))","v":0},0,{"$f":"AQ159-AP160*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ160/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,143,null,{"$f":"(AP160)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF160<=$J$9*1.05,(AV160*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW159,NA())","v":{"$error":"#N/A"}},23072.238162637354,276,4.5661512575187384,0.30916373751873605,0,0.89698752000000304,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},36.33769531606206,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,144,2.3305291073371062E-2,{"$f":"Z161*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF160*Bodencharakterisierung!$E$11/$J$20","v":3.8026935890933671E-5},{"$f":"((150*($J$2^0.87)*(AB161^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z161)*3600*24","v":7.3930243819260832E-2},2.3915996627248484E-4,{"$f":"AE160-AD161*Bodencharakterisierung!$E$8","v":5.4972685614964101E-2},{"$f":"IF(AE161>$J$18,(AE161/(Bodencharakterisierung!$E$11*1000)),0)","v":3.6285601065982904E-5},2.3305291073371062E-2,144,null,{"$f":"(AD161)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH161>0,(AJ161*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK160,NA())","v":0.3113312047741118},null,144,{"$f":"IF(AF161<=$J$9*0.05,AS160*EXP((-$J$6*1)/Heterogenität!$D$4),Z161)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF161>=$J$19, AR160/$J$5<AN161),0, Bodencharakterisierung!$E$8*$J$11*((AR160/$J$5)-AN161))","v":0},0,{"$f":"AQ160-AP161*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ161/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,144,null,{"$f":"(AP161)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF161<=$J$9*1.05,(AV161*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW160,NA())","v":{"$error":"#N/A"}},23072.238162637354,277,4.5745913647741148,0.3113312047741118,0,0.90326016000000309,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},36.285601065982902,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,145,2.3305291073371062E-2,{"$f":"Z162*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF161*Bodencharakterisierung!$E$11/$J$20","v":3.7972419920924681E-5},{"$f":"((150*($J$2^0.87)*(AB162^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z162)*3600*24","v":7.3846501102079479E-2},2.3915996627248484E-4,{"$f":"AE161-AD162*Bodencharakterisierung!$E$8","v":5.4893762826094178E-2},{"$f":"IF(AE162>$J$18,(AE162/(Bodencharakterisierung!$E$11*1000)),0)","v":3.6233506815903749E-5},2.3305291073371062E-2,145,null,{"$f":"(AD162)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH162>0,(AJ162*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK161,NA())","v":0.31349867202948756},null,145,{"$f":"IF(AF162<=$J$9*0.05,AS161*EXP((-$J$6*1)/Heterogenität!$D$4),Z162)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF162>=$J$19, AR161/$J$5<AN162),0, Bodencharakterisierung!$E$8*$J$11*((AR161/$J$5)-AN162))","v":0},0,{"$f":"AQ161-AP162*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ162/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,145,null,{"$f":"(AP162)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF162<=$J$9*1.05,(AV162*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW161,NA())","v":{"$error":"#N/A"}},23072.238162637354,278,4.5830314720294911,0.31349867202948756,0,0.90953280000000314,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},36.233506815903752,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,146,2.3305291073371062E-2,{"$f":"Z163*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF162*Bodencharakterisierung!$E$11/$J$20","v":3.7917903950915683E-5},{"$f":"((150*($J$2^0.87)*(AB163^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z163)*3600*24","v":7.3762733133382691E-2},2.3915996627248484E-4,{"$f":"AE162-AD163*Bodencharakterisierung!$E$8","v":5.4814840037224255E-2},{"$f":"IF(AE163>$J$18,(AE163/(Bodencharakterisierung!$E$11*1000)),0)","v":3.6181412565824594E-5},2.3305291073371062E-2,146,null,{"$f":"(AD163)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH163>0,(AJ163*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK162,NA())","v":0.31566613928486331},null,146,{"$f":"IF(AF163<=$J$9*0.05,AS162*EXP((-$J$6*1)/Heterogenität!$D$4),Z163)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF163>=$J$19, AR162/$J$5<AN163),0, Bodencharakterisierung!$E$8*$J$11*((AR162/$J$5)-AN163))","v":0},0,{"$f":"AQ162-AP163*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ163/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,146,null,{"$f":"(AP163)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF163<=$J$9*1.05,(AV163*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW162,NA())","v":{"$error":"#N/A"}},23072.238162637354,279,4.5914715792848666,0.31566613928486331,0,0.91580544000000319,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},36.181412565824594,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,147,2.3305291073371062E-2,{"$f":"Z164*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF163*Bodencharakterisierung!$E$11/$J$20","v":3.78633879809067E-5},{"$f":"((150*($J$2^0.87)*(AB164^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z164)*3600*24","v":7.3678939869234655E-2},2.3915996627248484E-4,{"$f":"AE163-AD164*Bodencharakterisierung!$E$8","v":5.4735917248354332E-2},{"$f":"IF(AE164>$J$18,(AE164/(Bodencharakterisierung!$E$11*1000)),0)","v":3.6129318315745432E-5},2.3305291073371062E-2,147,null,{"$f":"(AD164)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH164>0,(AJ164*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK163,NA())","v":0.31783360654023907},null,147,{"$f":"IF(AF164<=$J$9*0.05,AS163*EXP((-$J$6*1)/Heterogenität!$D$4),Z164)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF164>=$J$19, AR163/$J$5<AN164),0, Bodencharakterisierung!$E$8*$J$11*((AR163/$J$5)-AN164))","v":0},0,{"$f":"AQ163-AP164*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ164/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,147,null,{"$f":"(AP164)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF164<=$J$9*1.05,(AV164*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW163,NA())","v":{"$error":"#N/A"}},23072.238162637354,280,4.5999116865402421,0.31783360654023907,0,0.92207808000000324,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},36.129318315745429,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,148,2.3305291073371062E-2,{"$f":"Z165*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF164*Bodencharakterisierung!$E$11/$J$20","v":3.7808872010897695E-5},{"$f":"((150*($J$2^0.87)*(AB165^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z165)*3600*24","v":7.3595121265560004E-2},2.3915996627248484E-4,{"$f":"AE164-AD165*Bodencharakterisierung!$E$8","v":5.4656994459484409E-2},{"$f":"IF(AE165>$J$18,(AE165/(Bodencharakterisierung!$E$11*1000)),0)","v":3.6077224065666276E-5},2.3305291073371062E-2,148,null,{"$f":"(AD165)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH165>0,(AJ165*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK164,NA())","v":0.32000107379561482},null,148,{"$f":"IF(AF165<=$J$9*0.05,AS164*EXP((-$J$6*1)/Heterogenität!$D$4),Z165)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF165>=$J$19, AR164/$J$5<AN165),0, Bodencharakterisierung!$E$8*$J$11*((AR164/$J$5)-AN165))","v":0},0,{"$f":"AQ164-AP165*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ165/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,148,null,{"$f":"(AP165)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF165<=$J$9*1.05,(AV165*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW164,NA())","v":{"$error":"#N/A"}},23072.238162637354,281,4.6083517937956184,0.32000107379561482,0,0.92835072000000329,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},36.077224065666279,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,149,2.3305291073371062E-2,{"$f":"Z166*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF165*Bodencharakterisierung!$E$11/$J$20","v":3.7754356040888705E-5},{"$f":"((150*($J$2^0.87)*(AB166^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z166)*3600*24","v":7.3511277278142495E-2},2.3915996627248484E-4,{"$f":"AE165-AD166*Bodencharakterisierung!$E$8","v":5.4578071670614486E-2},{"$f":"IF(AE166>$J$18,(AE166/(Bodencharakterisierung!$E$11*1000)),0)","v":3.6025129815587121E-5},2.3305291073371062E-2,149,null,{"$f":"(AD166)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH166>0,(AJ166*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK165,NA())","v":0.32216854105099058},null,149,{"$f":"IF(AF166<=$J$9*0.05,AS165*EXP((-$J$6*1)/Heterogenität!$D$4),Z166)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF166>=$J$19, AR165/$J$5<AN166),0, Bodencharakterisierung!$E$8*$J$11*((AR165/$J$5)-AN166))","v":0},0,{"$f":"AQ165-AP166*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ166/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,149,null,{"$f":"(AP166)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF166<=$J$9*1.05,(AV166*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW165,NA())","v":{"$error":"#N/A"}},23072.238162637354,282,4.6167919010509939,0.32216854105099058,0,0.93462336000000334,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},36.025129815587121,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,2.3305291073371062E-2,{"$f":"Z167*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF166*Bodencharakterisierung!$E$11/$J$20","v":3.7699840070879714E-5},{"$f":"((150*($J$2^0.87)*(AB167^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z167)*3600*24","v":7.3427407862624999E-2},2.3915996627248484E-4,{"$f":"AE166-AD167*Bodencharakterisierung!$E$8","v":5.4499148881744564E-2},{"$f":"IF(AE167>$J$18,(AE167/(Bodencharakterisierung!$E$11*1000)),0)","v":3.5973035565507966E-5},2.3305291073371062E-2,150,null,{"$f":"(AD167)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH167>0,(AJ167*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK166,NA())","v":0.32433600830636633},null,150,{"$f":"IF(AF167<=$J$9*0.05,AS166*EXP((-$J$6*1)/Heterogenität!$D$4),Z167)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF167>=$J$19, AR166/$J$5<AN167),0, Bodencharakterisierung!$E$8*$J$11*((AR166/$J$5)-AN167))","v":0},0,{"$f":"AQ166-AP167*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ167/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,150,null,{"$f":"(AP167)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF167<=$J$9*1.05,(AV167*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW166,NA())","v":{"$error":"#N/A"}},23072.238162637354,283,4.6252320083063694,0.32433600830636633,0,0.9408960000000034,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},35.973035565507963,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,151,2.3305291073371062E-2,{"$f":"Z168*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF167*Bodencharakterisierung!$E$11/$J$20","v":3.7645324100870724E-5},{"$f":"((150*($J$2^0.87)*(AB168^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z168)*3600*24","v":7.3343512974508668E-2},2.3915996627248484E-4,{"$f":"AE167-AD168*Bodencharakterisierung!$E$8","v":5.4420226092874641E-2},{"$f":"IF(AE168>$J$18,(AE168/(Bodencharakterisierung!$E$11*1000)),0)","v":3.5920941315428804E-5},2.3305291073371062E-2,151,null,{"$f":"(AD168)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH168>0,(AJ168*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK167,NA())","v":0.32650347556174208},null,151,{"$f":"IF(AF168<=$J$9*0.05,AS167*EXP((-$J$6*1)/Heterogenität!$D$4),Z168)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF168>=$J$19, AR167/$J$5<AN168),0, Bodencharakterisierung!$E$8*$J$11*((AR167/$J$5)-AN168))","v":0},0,{"$f":"AQ167-AP168*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ168/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,151,null,{"$f":"(AP168)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF168<=$J$9*1.05,(AV168*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW167,NA())","v":{"$error":"#N/A"}},23072.238162637354,284,4.6336721155617457,0.32650347556174208,0,0.94716864000000345,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},35.920941315428806,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,152,2.3305291073371062E-2,{"$f":"Z169*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF168*Bodencharakterisierung!$E$11/$J$20","v":3.7590808130861726E-5},{"$f":"((150*($J$2^0.87)*(AB169^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z169)*3600*24","v":7.3259592569151905E-2},2.3915996627248484E-4,{"$f":"AE168-AD169*Bodencharakterisierung!$E$8","v":5.4341303304004718E-2},{"$f":"IF(AE169>$J$18,(AE169/(Bodencharakterisierung!$E$11*1000)),0)","v":3.5868847065349649E-5},2.3305291073371062E-2,152,null,{"$f":"(AD169)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH169>0,(AJ169*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK168,NA())","v":0.32867094281711784},null,152,{"$f":"IF(AF169<=$J$9*0.05,AS168*EXP((-$J$6*1)/Heterogenität!$D$4),Z169)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF169>=$J$19, AR168/$J$5<AN169),0, Bodencharakterisierung!$E$8*$J$11*((AR168/$J$5)-AN169))","v":0},0,{"$f":"AQ168-AP169*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ169/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,152,null,{"$f":"(AP169)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF169<=$J$9*1.05,(AV169*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW168,NA())","v":{"$error":"#N/A"}},23072.238162637354,285,4.6421122228171212,0.32867094281711784,0,0.9534412800000035,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},35.868847065349648,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,153,2.3305291073371062E-2,{"$f":"Z170*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF169*Bodencharakterisierung!$E$11/$J$20","v":3.7536292160852736E-5},{"$f":"((150*($J$2^0.87)*(AB170^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z170)*3600*24","v":7.3175646601770492E-2},2.3915996627248484E-4,{"$f":"AE169-AD170*Bodencharakterisierung!$E$8","v":5.4262380515134795E-2},{"$f":"IF(AE170>$J$18,(AE170/(Bodencharakterisierung!$E$11*1000)),0)","v":3.5816752815270494E-5},2.3305291073371062E-2,153,null,{"$f":"(AD170)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH170>0,(AJ170*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK169,NA())","v":0.33083841007249359},null,153,{"$f":"IF(AF170<=$J$9*0.05,AS169*EXP((-$J$6*1)/Heterogenität!$D$4),Z170)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF170>=$J$19, AR169/$J$5<AN170),0, Bodencharakterisierung!$E$8*$J$11*((AR169/$J$5)-AN170))","v":0},0,{"$f":"AQ169-AP170*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ170/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,153,null,{"$f":"(AP170)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF170<=$J$9*1.05,(AV170*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW169,NA())","v":{"$error":"#N/A"}},23072.238162637354,286,4.6505523300724967,0.33083841007249359,0,0.95971392000000355,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},35.81675281527049,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,154,2.3305291073371062E-2,{"$f":"Z171*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF170*Bodencharakterisierung!$E$11/$J$20","v":3.7481776190843738E-5},{"$f":"((150*($J$2^0.87)*(AB171^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z171)*3600*24","v":7.309167502743584E-2},2.3915996627248484E-4,{"$f":"AE170-AD171*Bodencharakterisierung!$E$8","v":5.4183457726264872E-2},{"$f":"IF(AE171>$J$18,(AE171/(Bodencharakterisierung!$E$11*1000)),0)","v":3.5764658565191332E-5},2.3305291073371062E-2,154,null,{"$f":"(AD171)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH171>0,(AJ171*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK170,NA())","v":0.33300587732786935},null,154,{"$f":"IF(AF171<=$J$9*0.05,AS170*EXP((-$J$6*1)/Heterogenität!$D$4),Z171)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF171>=$J$19, AR170/$J$5<AN171),0, Bodencharakterisierung!$E$8*$J$11*((AR170/$J$5)-AN171))","v":0},0,{"$f":"AQ170-AP171*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ171/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,154,null,{"$f":"(AP171)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF171<=$J$9*1.05,(AV171*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW170,NA())","v":{"$error":"#N/A"}},23072.238162637354,287,4.658992437327873,0.33300587732786935,0,0.9659865600000036,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},35.764658565191333,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,155,2.3305291073371062E-2,{"$f":"Z172*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF171*Bodencharakterisierung!$E$11/$J$20","v":3.7427260220834741E-5},{"$f":"((150*($J$2^0.87)*(AB172^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z172)*3600*24","v":7.3007677801075505E-2},2.3915996627248484E-4,{"$f":"AE171-AD172*Bodencharakterisierung!$E$8","v":5.4104534937394949E-2},{"$f":"IF(AE172>$J$18,(AE172/(Bodencharakterisierung!$E$11*1000)),0)","v":3.5712564315112176E-5},2.3305291073371062E-2,155,null,{"$f":"(AD172)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH172>0,(AJ172*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK171,NA())","v":0.3351733445832451},null,155,{"$f":"IF(AF172<=$J$9*0.05,AS171*EXP((-$J$6*1)/Heterogenität!$D$4),Z172)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF172>=$J$19, AR171/$J$5<AN172),0, Bodencharakterisierung!$E$8*$J$11*((AR171/$J$5)-AN172))","v":0},0,{"$f":"AQ171-AP172*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ172/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,155,null,{"$f":"(AP172)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF172<=$J$9*1.05,(AV172*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW171,NA())","v":{"$error":"#N/A"}},23072.238162637354,288,4.6674325445832485,0.3351733445832451,0,0.97225920000000365,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},35.712564315112175,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,156,2.3305291073371062E-2,{"$f":"Z173*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF172*Bodencharakterisierung!$E$11/$J$20","v":3.737274425082575E-5},{"$f":"((150*($J$2^0.87)*(AB173^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z173)*3600*24","v":7.2923654877471572E-2},2.3915996627248484E-4,{"$f":"AE172-AD173*Bodencharakterisierung!$E$8","v":5.4025612148525026E-2},{"$f":"IF(AE173>$J$18,(AE173/(Bodencharakterisierung!$E$11*1000)),0)","v":3.5660470065033021E-5},2.3305291073371062E-2,156,null,{"$f":"(AD173)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH173>0,(AJ173*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK172,NA())","v":0.33734081183862086},null,156,{"$f":"IF(AF173<=$J$9*0.05,AS172*EXP((-$J$6*1)/Heterogenität!$D$4),Z173)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF173>=$J$19, AR172/$J$5<AN173),0, Bodencharakterisierung!$E$8*$J$11*((AR172/$J$5)-AN173))","v":0},0,{"$f":"AQ172-AP173*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ173/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,156,null,{"$f":"(AP173)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF173<=$J$9*1.05,(AV173*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW172,NA())","v":{"$error":"#N/A"}},23072.238162637354,289,4.675872651838624,0.33734081183862086,0,0.97853184000000371,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},35.660470065033024,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,157,2.3305291073371062E-2,{"$f":"Z174*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF173*Bodencharakterisierung!$E$11/$J$20","v":3.731822828081676E-5},{"$f":"((150*($J$2^0.87)*(AB174^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z174)*3600*24","v":7.2839606211260594E-2},2.3915996627248484E-4,{"$f":"AE173-AD174*Bodencharakterisierung!$E$8","v":5.3946689359655103E-2},{"$f":"IF(AE174>$J$18,(AE174/(Bodencharakterisierung!$E$11*1000)),0)","v":3.5608375814953866E-5},2.3305291073371062E-2,157,null,{"$f":"(AD174)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH174>0,(AJ174*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK173,NA())","v":0.33950827909399661},null,157,{"$f":"IF(AF174<=$J$9*0.05,AS173*EXP((-$J$6*1)/Heterogenität!$D$4),Z174)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF174>=$J$19, AR173/$J$5<AN174),0, Bodencharakterisierung!$E$8*$J$11*((AR173/$J$5)-AN174))","v":0},0,{"$f":"AQ173-AP174*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ174/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,157,null,{"$f":"(AP174)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF174<=$J$9*1.05,(AV174*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW173,NA())","v":{"$error":"#N/A"}},23072.238162637354,290,4.6843127590940004,0.33950827909399661,0,0.98480448000000376,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},35.608375814953867,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,158,2.3305291073371062E-2,{"$f":"Z175*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF174*Bodencharakterisierung!$E$11/$J$20","v":3.7263712310807769E-5},{"$f":"((150*($J$2^0.87)*(AB175^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z175)*3600*24","v":7.2755531756932404E-2},2.3915996627248484E-4,{"$f":"AE174-AD175*Bodencharakterisierung!$E$8","v":5.386776657078518E-2},{"$f":"IF(AE175>$J$18,(AE175/(Bodencharakterisierung!$E$11*1000)),0)","v":3.5556281564874704E-5},2.3305291073371062E-2,158,null,{"$f":"(AD175)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH175>0,(AJ175*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK174,NA())","v":0.34167574634937237},null,158,{"$f":"IF(AF175<=$J$9*0.05,AS174*EXP((-$J$6*1)/Heterogenität!$D$4),Z175)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF175>=$J$19, AR174/$J$5<AN175),0, Bodencharakterisierung!$E$8*$J$11*((AR174/$J$5)-AN175))","v":0},0,{"$f":"AQ174-AP175*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ175/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,158,null,{"$f":"(AP175)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF175<=$J$9*1.05,(AV175*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW174,NA())","v":{"$error":"#N/A"}},23072.238162637354,291,4.6927528663493758,0.34167574634937237,0,0.99107712000000381,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},35.556281564874702,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,159,2.3305291073371062E-2,{"$f":"Z176*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF175*Bodencharakterisierung!$E$11/$J$20","v":3.7209196340798772E-5},{"$f":"((150*($J$2^0.87)*(AB176^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z176)*3600*24","v":7.2671431468829706E-2},2.3915996627248484E-4,{"$f":"AE175-AD176*Bodencharakterisierung!$E$8","v":5.3788843781915258E-2},{"$f":"IF(AE176>$J$18,(AE176/(Bodencharakterisierung!$E$11*1000)),0)","v":3.5504187314795549E-5},2.3305291073371062E-2,159,null,{"$f":"(AD176)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH176>0,(AJ176*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK175,NA())","v":0.34384321360474812},null,159,{"$f":"IF(AF176<=$J$9*0.05,AS175*EXP((-$J$6*1)/Heterogenität!$D$4),Z176)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF176>=$J$19, AR175/$J$5<AN176),0, Bodencharakterisierung!$E$8*$J$11*((AR175/$J$5)-AN176))","v":0},0,{"$f":"AQ175-AP176*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ176/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,159,null,{"$f":"(AP176)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF176<=$J$9*1.05,(AV176*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW175,NA())","v":{"$error":"#N/A"}},23072.238162637354,292,4.7011929736047513,0.34384321360474812,0,0.99734976000000386,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},35.504187314795551,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,160,2.3305291073371062E-2,{"$f":"Z177*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF176*Bodencharakterisierung!$E$11/$J$20","v":3.7154680370789781E-5},{"$f":"((150*($J$2^0.87)*(AB177^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z177)*3600*24","v":7.2587305301147431E-2},2.3915996627248484E-4,{"$f":"AE176-AD177*Bodencharakterisierung!$E$8","v":5.3709920993045335E-2},{"$f":"IF(AE177>$J$18,(AE177/(Bodencharakterisierung!$E$11*1000)),0)","v":3.5452093064716393E-5},2.3305291073371062E-2,160,null,{"$f":"(AD177)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH177>0,(AJ177*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK176,NA())","v":0.34601068086012388},null,160,{"$f":"IF(AF177<=$J$9*0.05,AS176*EXP((-$J$6*1)/Heterogenität!$D$4),Z177)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF177>=$J$19, AR176/$J$5<AN177),0, Bodencharakterisierung!$E$8*$J$11*((AR176/$J$5)-AN177))","v":0},0,{"$f":"AQ176-AP177*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ177/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,160,null,{"$f":"(AP177)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF177<=$J$9*1.05,(AV177*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW176,NA())","v":{"$error":"#N/A"}},23072.238162637354,293,4.7096330808601277,0.34601068086012388,0,1.0036224000000038,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},35.452093064716394,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,161,2.3305291073371062E-2,{"$f":"Z178*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF177*Bodencharakterisierung!$E$11/$J$20","v":3.710016440078079E-5},{"$f":"((150*($J$2^0.87)*(AB178^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z178)*3600*24","v":7.2503153207931936E-2},2.3915996627248484E-4,{"$f":"AE177-AD178*Bodencharakterisierung!$E$8","v":5.3630998204175412E-2},{"$f":"IF(AE178>$J$18,(AE178/(Bodencharakterisierung!$E$11*1000)),0)","v":3.5399998814637238E-5},2.3305291073371062E-2,161,null,{"$f":"(AD178)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH178>0,(AJ178*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK177,NA())","v":0.34817814811549963},null,161,{"$f":"IF(AF178<=$J$9*0.05,AS177*EXP((-$J$6*1)/Heterogenität!$D$4),Z178)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF178>=$J$19, AR177/$J$5<AN178),0, Bodencharakterisierung!$E$8*$J$11*((AR177/$J$5)-AN178))","v":0},0,{"$f":"AQ177-AP178*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ178/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,161,null,{"$f":"(AP178)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF178<=$J$9*1.05,(AV178*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW177,NA())","v":{"$error":"#N/A"}},23072.238162637354,294,4.7180731881155031,0.34817814811549963,0,1.0098950400000037,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},35.399998814637236,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,162,2.3305291073371062E-2,{"$f":"Z179*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF178*Bodencharakterisierung!$E$11/$J$20","v":3.70456484307718E-5},{"$f":"((150*($J$2^0.87)*(AB179^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z179)*3600*24","v":7.2418975143080405E-2},2.3915996627248484E-4,{"$f":"AE178-AD179*Bodencharakterisierung!$E$8","v":5.3552075415305489E-2},{"$f":"IF(AE179>$J$18,(AE179/(Bodencharakterisierung!$E$11*1000)),0)","v":3.5347904564558076E-5},2.3305291073371062E-2,162,null,{"$f":"(AD179)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH179>0,(AJ179*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK178,NA())","v":0.35034561537087539},null,162,{"$f":"IF(AF179<=$J$9*0.05,AS178*EXP((-$J$6*1)/Heterogenität!$D$4),Z179)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF179>=$J$19, AR178/$J$5<AN179),0, Bodencharakterisierung!$E$8*$J$11*((AR178/$J$5)-AN179))","v":0},0,{"$f":"AQ178-AP179*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ179/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,162,null,{"$f":"(AP179)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF179<=$J$9*1.05,(AV179*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW178,NA())","v":{"$error":"#N/A"}},23072.238162637354,295,4.7265132953708786,0.35034561537087539,0,1.0161676800000037,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},35.347904564558078,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,163,2.3305291073371062E-2,{"$f":"Z180*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF179*Bodencharakterisierung!$E$11/$J$20","v":3.6991132460762803E-5},{"$f":"((150*($J$2^0.87)*(AB180^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z180)*3600*24","v":7.2334771060339823E-2},2.3915996627248484E-4,{"$f":"AE179-AD180*Bodencharakterisierung!$E$8","v":5.3473152626435566E-2},{"$f":"IF(AE180>$J$18,(AE180/(Bodencharakterisierung!$E$11*1000)),0)","v":3.5295810314478921E-5},2.3305291073371062E-2,163,null,{"$f":"(AD180)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH180>0,(AJ180*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK179,NA())","v":0.35251308262625114},null,163,{"$f":"IF(AF180<=$J$9*0.05,AS179*EXP((-$J$6*1)/Heterogenität!$D$4),Z180)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF180>=$J$19, AR179/$J$5<AN180),0, Bodencharakterisierung!$E$8*$J$11*((AR179/$J$5)-AN180))","v":0},0,{"$f":"AQ179-AP180*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ180/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,163,null,{"$f":"(AP180)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF180<=$J$9*1.05,(AV180*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW179,NA())","v":{"$error":"#N/A"}},23072.238162637354,296,4.734953402626255,0.35251308262625114,0,1.0224403200000036,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},35.295810314478921,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,164,2.3305291073371062E-2,{"$f":"Z181*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF180*Bodencharakterisierung!$E$11/$J$20","v":3.6936616490753805E-5},{"$f":"((150*($J$2^0.87)*(AB181^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z181)*3600*24","v":7.2250540913306904E-2},2.3915996627248484E-4,{"$f":"AE180-AD181*Bodencharakterisierung!$E$8","v":5.3394229837565643E-2},{"$f":"IF(AE181>$J$18,(AE181/(Bodencharakterisierung!$E$11*1000)),0)","v":3.5243716064399766E-5},2.3305291073371062E-2,164,null,{"$f":"(AD181)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH181>0,(AJ181*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK180,NA())","v":0.35468054988162689},null,164,{"$f":"IF(AF181<=$J$9*0.05,AS180*EXP((-$J$6*1)/Heterogenität!$D$4),Z181)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF181>=$J$19, AR180/$J$5<AN181),0, Bodencharakterisierung!$E$8*$J$11*((AR180/$J$5)-AN181))","v":0},0,{"$f":"AQ180-AP181*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ181/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,164,null,{"$f":"(AP181)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF181<=$J$9*1.05,(AV181*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW180,NA())","v":{"$error":"#N/A"}},23072.238162637354,297,4.7433935098816304,0.35468054988162689,0,1.0287129600000036,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},35.243716064399763,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,165,2.3305291073371062E-2,{"$f":"Z182*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF181*Bodencharakterisierung!$E$11/$J$20","v":3.6882100520744821E-5},{"$f":"((150*($J$2^0.87)*(AB182^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z182)*3600*24","v":7.2166284655426335E-2},2.3915996627248484E-4,{"$f":"AE181-AD182*Bodencharakterisierung!$E$8","v":5.331530704869572E-2},{"$f":"IF(AE182>$J$18,(AE182/(Bodencharakterisierung!$E$11*1000)),0)","v":3.519162181432061E-5},2.3305291073371062E-2,165,null,{"$f":"(AD182)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH182>0,(AJ182*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK181,NA())","v":0.35684801713700265},null,165,{"$f":"IF(AF182<=$J$9*0.05,AS181*EXP((-$J$6*1)/Heterogenität!$D$4),Z182)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF182>=$J$19, AR181/$J$5<AN182),0, Bodencharakterisierung!$E$8*$J$11*((AR181/$J$5)-AN182))","v":0},0,{"$f":"AQ181-AP182*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ182/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,165,null,{"$f":"(AP182)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF182<=$J$9*1.05,(AV182*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW181,NA())","v":{"$error":"#N/A"}},23072.238162637354,298,4.7518336171370059,0.35684801713700265,0,1.0349856000000035,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},35.191621814320612,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,166,2.3305291073371062E-2,{"$f":"Z183*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF182*Bodencharakterisierung!$E$11/$J$20","v":3.6827584550735824E-5},{"$f":"((150*($J$2^0.87)*(AB183^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z183)*3600*24","v":7.2082002239991436E-2},2.3915996627248484E-4,{"$f":"AE182-AD183*Bodencharakterisierung!$E$8","v":5.3236384259825797E-2},{"$f":"IF(AE183>$J$18,(AE183/(Bodencharakterisierung!$E$11*1000)),0)","v":3.5139527564241448E-5},2.3305291073371062E-2,166,null,{"$f":"(AD183)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH183>0,(AJ183*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK182,NA())","v":0.3590154843923784},null,166,{"$f":"IF(AF183<=$J$9*0.05,AS182*EXP((-$J$6*1)/Heterogenität!$D$4),Z183)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF183>=$J$19, AR182/$J$5<AN183),0, Bodencharakterisierung!$E$8*$J$11*((AR182/$J$5)-AN183))","v":0},0,{"$f":"AQ182-AP183*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ183/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,166,null,{"$f":"(AP183)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF183<=$J$9*1.05,(AV183*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW182,NA())","v":{"$error":"#N/A"}},23072.238162637354,299,4.7602737243923823,0.3590154843923784,0,1.0412582400000034,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},35.139527564241448,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,167,2.3305291073371062E-2,{"$f":"Z184*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF183*Bodencharakterisierung!$E$11/$J$20","v":3.6773068580726827E-5},{"$f":"((150*($J$2^0.87)*(AB184^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z184)*3600*24","v":7.1997693620142161E-2},2.3915996627248484E-4,{"$f":"AE183-AD184*Bodencharakterisierung!$E$8","v":5.3157461470955875E-2},{"$f":"IF(AE184>$J$18,(AE184/(Bodencharakterisierung!$E$11*1000)),0)","v":3.5087433314162293E-5},2.3305291073371062E-2,167,null,{"$f":"(AD184)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH184>0,(AJ184*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK183,NA())","v":0.36118295164775416},null,167,{"$f":"IF(AF184<=$J$9*0.05,AS183*EXP((-$J$6*1)/Heterogenität!$D$4),Z184)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF184>=$J$19, AR183/$J$5<AN184),0, Bodencharakterisierung!$E$8*$J$11*((AR183/$J$5)-AN184))","v":0},0,{"$f":"AQ183-AP184*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ184/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,167,null,{"$f":"(AP184)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF184<=$J$9*1.05,(AV184*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW183,NA())","v":{"$error":"#N/A"}},23072.238162637354,300,4.7687138316477569,0.36118295164775416,0,1.0475308800000034,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},35.08743331416229,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,168,2.3305291073371062E-2,{"$f":"Z185*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF184*Bodencharakterisierung!$E$11/$J$20","v":3.6718552610717836E-5},{"$f":"((150*($J$2^0.87)*(AB185^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z185)*3600*24","v":7.1913358748865175E-2},2.3915996627248484E-4,{"$f":"AE184-AD185*Bodencharakterisierung!$E$8","v":5.3078538682085952E-2},{"$f":"IF(AE185>$J$18,(AE185/(Bodencharakterisierung!$E$11*1000)),0)","v":3.5035339064083138E-5},2.3305291073371062E-2,168,null,{"$f":"(AD185)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH185>0,(AJ185*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK184,NA())","v":0.36335041890312991},null,168,{"$f":"IF(AF185<=$J$9*0.05,AS184*EXP((-$J$6*1)/Heterogenität!$D$4),Z185)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF185>=$J$19, AR184/$J$5<AN185),0, Bodencharakterisierung!$E$8*$J$11*((AR184/$J$5)-AN185))","v":0},0,{"$f":"AQ184-AP185*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ185/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,168,null,{"$f":"(AP185)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF185<=$J$9*1.05,(AV185*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW184,NA())","v":{"$error":"#N/A"}},23072.238162637354,301,4.7771539389031332,0.36335041890312991,0,1.0538035200000033,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},35.035339064083139,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,169,2.3305291073371062E-2,{"$f":"Z186*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF185*Bodencharakterisierung!$E$11/$J$20","v":3.6664036640708845E-5},{"$f":"((150*($J$2^0.87)*(AB186^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z186)*3600*24","v":7.1828997578992887E-2},2.3915996627248484E-4,{"$f":"AE185-AD186*Bodencharakterisierung!$E$8","v":5.2999615893216029E-2},{"$f":"IF(AE186>$J$18,(AE186/(Bodencharakterisierung!$E$11*1000)),0)","v":3.4983244814003983E-5},2.3305291073371062E-2,169,null,{"$f":"(AD186)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH186>0,(AJ186*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK185,NA())","v":0.36551788615850567},null,169,{"$f":"IF(AF186<=$J$9*0.05,AS185*EXP((-$J$6*1)/Heterogenität!$D$4),Z186)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF186>=$J$19, AR185/$J$5<AN186),0, Bodencharakterisierung!$E$8*$J$11*((AR185/$J$5)-AN186))","v":0},0,{"$f":"AQ185-AP186*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ186/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,169,null,{"$f":"(AP186)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF186<=$J$9*1.05,(AV186*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW185,NA())","v":{"$error":"#N/A"}},23072.238162637354,302,4.7855940461585087,0.36551788615850567,0,1.0600761600000033,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},34.983244814003982,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,170,2.3305291073371062E-2,{"$f":"Z187*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF186*Bodencharakterisierung!$E$11/$J$20","v":3.6609520670699855E-5},{"$f":"((150*($J$2^0.87)*(AB187^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z187)*3600*24","v":7.1744610063202527E-2},2.3915996627248484E-4,{"$f":"AE186-AD187*Bodencharakterisierung!$E$8","v":5.2920693104346106E-2},{"$f":"IF(AE187>$J$18,(AE187/(Bodencharakterisierung!$E$11*1000)),0)","v":3.4931150563924821E-5},2.3305291073371062E-2,170,null,{"$f":"(AD187)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH187>0,(AJ187*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK186,NA())","v":0.36768535341388142},null,170,{"$f":"IF(AF187<=$J$9*0.05,AS186*EXP((-$J$6*1)/Heterogenität!$D$4),Z187)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF187>=$J$19, AR186/$J$5<AN187),0, Bodencharakterisierung!$E$8*$J$11*((AR186/$J$5)-AN187))","v":0},0,{"$f":"AQ186-AP187*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ187/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,170,null,{"$f":"(AP187)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF187<=$J$9*1.05,(AV187*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW186,NA())","v":{"$error":"#N/A"}},23072.238162637354,303,4.7940341534138842,0.36768535341388142,0,1.0663488000000032,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},34.931150563924824,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,171,2.3305291073371062E-2,{"$f":"Z188*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF187*Bodencharakterisierung!$E$11/$J$20","v":3.6555004700690857E-5},{"$f":"((150*($J$2^0.87)*(AB188^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z188)*3600*24","v":7.1660196154015518E-2},2.3915996627248484E-4,{"$f":"AE187-AD188*Bodencharakterisierung!$E$8","v":5.2841770315476183E-2},{"$f":"IF(AE188>$J$18,(AE188/(Bodencharakterisierung!$E$11*1000)),0)","v":3.4879056313845666E-5},2.3305291073371062E-2,171,null,{"$f":"(AD188)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH188>0,(AJ188*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK187,NA())","v":0.36985282066925718},null,171,{"$f":"IF(AF188<=$J$9*0.05,AS187*EXP((-$J$6*1)/Heterogenität!$D$4),Z188)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF188>=$J$19, AR187/$J$5<AN188),0, Bodencharakterisierung!$E$8*$J$11*((AR187/$J$5)-AN188))","v":0},0,{"$f":"AQ187-AP188*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ188/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,171,null,{"$f":"(AP188)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF188<=$J$9*1.05,(AV188*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW187,NA())","v":{"$error":"#N/A"}},23072.238162637354,304,4.8024742606692605,0.36985282066925718,0,1.0726214400000031,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},34.879056313845666,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,172,2.3305291073371062E-2,{"$f":"Z189*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF188*Bodencharakterisierung!$E$11/$J$20","v":3.650048873068186E-5},{"$f":"((150*($J$2^0.87)*(AB189^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z189)*3600*24","v":7.157575580379702E-2},2.3915996627248484E-4,{"$f":"AE188-AD189*Bodencharakterisierung!$E$8","v":5.276284752660626E-2},{"$f":"IF(AE189>$J$18,(AE189/(Bodencharakterisierung!$E$11*1000)),0)","v":3.482696206376651E-5},2.3305291073371062E-2,172,null,{"$f":"(AD189)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH189>0,(AJ189*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK188,NA())","v":0.37202028792463293},null,172,{"$f":"IF(AF189<=$J$9*0.05,AS188*EXP((-$J$6*1)/Heterogenität!$D$4),Z189)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF189>=$J$19, AR188/$J$5<AN189),0, Bodencharakterisierung!$E$8*$J$11*((AR188/$J$5)-AN189))","v":0},0,{"$f":"AQ188-AP189*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ189/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,172,null,{"$f":"(AP189)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF189<=$J$9*1.05,(AV189*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW188,NA())","v":{"$error":"#N/A"}},23072.238162637354,305,4.810914367924636,0.37202028792463293,0,1.0788940800000031,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},34.826962063766508,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,173,2.3305291073371062E-2,{"$f":"Z190*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF189*Bodencharakterisierung!$E$11/$J$20","v":3.6445972760672876E-5},{"$f":"((150*($J$2^0.87)*(AB190^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z190)*3600*24","v":7.149128896475497E-2},2.3915996627248484E-4,{"$f":"AE189-AD190*Bodencharakterisierung!$E$8","v":5.2683924737736337E-2},{"$f":"IF(AE190>$J$18,(AE190/(Bodencharakterisierung!$E$11*1000)),0)","v":3.4774867813687348E-5},2.3305291073371062E-2,173,null,{"$f":"(AD190)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH190>0,(AJ190*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK189,NA())","v":0.37418775518000869},null,173,{"$f":"IF(AF190<=$J$9*0.05,AS189*EXP((-$J$6*1)/Heterogenität!$D$4),Z190)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF190>=$J$19, AR189/$J$5<AN190),0, Bodencharakterisierung!$E$8*$J$11*((AR189/$J$5)-AN190))","v":0},0,{"$f":"AQ189-AP190*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ190/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,173,null,{"$f":"(AP190)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF190<=$J$9*1.05,(AV190*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW189,NA())","v":{"$error":"#N/A"}},23072.238162637354,306,4.8193544751800115,0.37418775518000869,0,1.085166720000003,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},34.774867813687351,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,174,2.3305291073371062E-2,{"$f":"Z191*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF190*Bodencharakterisierung!$E$11/$J$20","v":3.6391456790663872E-5},{"$f":"((150*($J$2^0.87)*(AB191^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z191)*3600*24","v":7.1406795588938754E-2},2.3915996627248484E-4,{"$f":"AE190-AD191*Bodencharakterisierung!$E$8","v":5.2605001948866414E-2},{"$f":"IF(AE191>$J$18,(AE191/(Bodencharakterisierung!$E$11*1000)),0)","v":3.4722773563608193E-5},2.3305291073371062E-2,174,null,{"$f":"(AD191)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH191>0,(AJ191*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK190,NA())","v":0.37635522243538444},null,174,{"$f":"IF(AF191<=$J$9*0.05,AS190*EXP((-$J$6*1)/Heterogenität!$D$4),Z191)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF191>=$J$19, AR190/$J$5<AN191),0, Bodencharakterisierung!$E$8*$J$11*((AR190/$J$5)-AN191))","v":0},0,{"$f":"AQ190-AP191*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ191/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,174,null,{"$f":"(AP191)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF191<=$J$9*1.05,(AV191*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW190,NA())","v":{"$error":"#N/A"}},23072.238162637354,307,4.8277945824353878,0.37635522243538444,0,1.091439360000003,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},34.722773563608193,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,175,2.3305291073371062E-2,{"$f":"Z192*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF191*Bodencharakterisierung!$E$11/$J$20","v":3.6336940820654881E-5},{"$f":"((150*($J$2^0.87)*(AB192^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z192)*3600*24","v":7.1322275628239673E-2},2.3915996627248484E-4,{"$f":"AE191-AD192*Bodencharakterisierung!$E$8","v":5.2526079159996492E-2},{"$f":"IF(AE192>$J$18,(AE192/(Bodencharakterisierung!$E$11*1000)),0)","v":3.4670679313529038E-5},2.3305291073371062E-2,175,null,{"$f":"(AD192)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH192>0,(AJ192*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK191,NA())","v":0.37852268969076019},null,175,{"$f":"IF(AF192<=$J$9*0.05,AS191*EXP((-$J$6*1)/Heterogenität!$D$4),Z192)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF192>=$J$19, AR191/$J$5<AN192),0, Bodencharakterisierung!$E$8*$J$11*((AR191/$J$5)-AN192))","v":0},0,{"$f":"AQ191-AP192*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ192/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,175,null,{"$f":"(AP192)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF192<=$J$9*1.05,(AV192*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW191,NA())","v":{"$error":"#N/A"}},23072.238162637354,308,4.8362346896907624,0.37852268969076019,0,1.0977120000000029,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},34.670679313529035,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,176,2.3305291073371062E-2,{"$f":"Z193*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF192*Bodencharakterisierung!$E$11/$J$20","v":3.6282424850645891E-5},{"$f":"((150*($J$2^0.87)*(AB193^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z193)*3600*24","v":7.1237729034389144E-2},2.3915996627248484E-4,{"$f":"AE192-AD193*Bodencharakterisierung!$E$8","v":5.2447156371126569E-2},{"$f":"IF(AE193>$J$18,(AE193/(Bodencharakterisierung!$E$11*1000)),0)","v":3.4618585063449883E-5},2.3305291073371062E-2,176,null,{"$f":"(AD193)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH193>0,(AJ193*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK192,NA())","v":0.38069015694613595},null,176,{"$f":"IF(AF193<=$J$9*0.05,AS192*EXP((-$J$6*1)/Heterogenität!$D$4),Z193)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF193>=$J$19, AR192/$J$5<AN193),0, Bodencharakterisierung!$E$8*$J$11*((AR192/$J$5)-AN193))","v":0},0,{"$f":"AQ192-AP193*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ193/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,176,null,{"$f":"(AP193)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF193<=$J$9*1.05,(AV193*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW192,NA())","v":{"$error":"#N/A"}},23072.238162637354,309,4.8446747969461388,0.38069015694613595,0,1.1039846400000028,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},34.618585063449885,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,177,2.3305291073371062E-2,{"$f":"Z194*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF193*Bodencharakterisierung!$E$11/$J$20","v":3.62279088806369E-5},{"$f":"((150*($J$2^0.87)*(AB194^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z194)*3600*24","v":7.1153155758958073E-2},2.3915996627248484E-4,{"$f":"AE193-AD194*Bodencharakterisierung!$E$8","v":5.2368233582256646E-2},{"$f":"IF(AE194>$J$18,(AE194/(Bodencharakterisierung!$E$11*1000)),0)","v":3.4566490813370721E-5},2.3305291073371062E-2,177,null,{"$f":"(AD194)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH194>0,(AJ194*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK193,NA())","v":0.3828576242015117},null,177,{"$f":"IF(AF194<=$J$9*0.05,AS193*EXP((-$J$6*1)/Heterogenität!$D$4),Z194)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF194>=$J$19, AR193/$J$5<AN194),0, Bodencharakterisierung!$E$8*$J$11*((AR193/$J$5)-AN194))","v":0},0,{"$f":"AQ193-AP194*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ194/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,177,null,{"$f":"(AP194)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF194<=$J$9*1.05,(AV194*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW193,NA())","v":{"$error":"#N/A"}},23072.238162637354,310,4.8531149042015143,0.3828576242015117,0,1.1102572800000028,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},34.56649081337072,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,178,2.3305291073371062E-2,{"$f":"Z195*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF194*Bodencharakterisierung!$E$11/$J$20","v":3.6173392910627903E-5},{"$f":"((150*($J$2^0.87)*(AB195^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z195)*3600*24","v":7.1068555753356633E-2},2.3915996627248484E-4,{"$f":"AE194-AD195*Bodencharakterisierung!$E$8","v":5.2289310793386723E-2},{"$f":"IF(AE195>$J$18,(AE195/(Bodencharakterisierung!$E$11*1000)),0)","v":3.4514396563291565E-5},2.3305291073371062E-2,178,null,{"$f":"(AD195)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH195>0,(AJ195*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK194,NA())","v":0.38502509145688746},null,178,{"$f":"IF(AF195<=$J$9*0.05,AS194*EXP((-$J$6*1)/Heterogenität!$D$4),Z195)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF195>=$J$19, AR194/$J$5<AN195),0, Bodencharakterisierung!$E$8*$J$11*((AR194/$J$5)-AN195))","v":0},0,{"$f":"AQ194-AP195*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ195/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,178,null,{"$f":"(AP195)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF195<=$J$9*1.05,(AV195*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW194,NA())","v":{"$error":"#N/A"}},23072.238162637354,311,4.8615550114568897,0.38502509145688746,0,1.1165299200000027,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},34.514396563291562,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,179,2.3305291073371062E-2,{"$f":"Z196*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF195*Bodencharakterisierung!$E$11/$J$20","v":3.6118876940618912E-5},{"$f":"((150*($J$2^0.87)*(AB196^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z196)*3600*24","v":7.098392896883321E-2},2.3915996627248484E-4,{"$f":"AE195-AD196*Bodencharakterisierung!$E$8","v":5.22103880045168E-2},{"$f":"IF(AE196>$J$18,(AE196/(Bodencharakterisierung!$E$11*1000)),0)","v":3.446230231321241E-5},2.3305291073371062E-2,179,null,{"$f":"(AD196)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH196>0,(AJ196*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK195,NA())","v":0.38719255871226321},null,179,{"$f":"IF(AF196<=$J$9*0.05,AS195*EXP((-$J$6*1)/Heterogenität!$D$4),Z196)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF196>=$J$19, AR195/$J$5<AN196),0, Bodencharakterisierung!$E$8*$J$11*((AR195/$J$5)-AN196))","v":0},0,{"$f":"AQ195-AP196*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ196/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,179,null,{"$f":"(AP196)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF196<=$J$9*1.05,(AV196*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW195,NA())","v":{"$error":"#N/A"}},23072.238162637354,312,4.8699951187122661,0.38719255871226321,0,1.1228025600000027,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},34.462302313212412,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,180,2.3305291073371062E-2,{"$f":"Z197*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF196*Bodencharakterisierung!$E$11/$J$20","v":3.6064360970609922E-5},{"$f":"((150*($J$2^0.87)*(AB197^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z197)*3600*24","v":7.0899275356473238E-2},2.3915996627248484E-4,{"$f":"AE196-AD197*Bodencharakterisierung!$E$8","v":5.2131465215646877E-2},{"$f":"IF(AE197>$J$18,(AE197/(Bodencharakterisierung!$E$11*1000)),0)","v":3.4410208063133255E-5},2.3305291073371062E-2,180,null,{"$f":"(AD197)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH197>0,(AJ197*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK196,NA())","v":0.38936002596763897},null,180,{"$f":"IF(AF197<=$J$9*0.05,AS196*EXP((-$J$6*1)/Heterogenität!$D$4),Z197)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF197>=$J$19, AR196/$J$5<AN197),0, Bodencharakterisierung!$E$8*$J$11*((AR196/$J$5)-AN197))","v":0},0,{"$f":"AQ196-AP197*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ197/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,180,null,{"$f":"(AP197)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF197<=$J$9*1.05,(AV197*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW196,NA())","v":{"$error":"#N/A"}},23072.238162637354,313,4.8784352259676416,0.38936002596763897,0,1.1290752000000026,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},34.410208063133254,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,181,2.3305291073371062E-2,{"$f":"Z198*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF197*Bodencharakterisierung!$E$11/$J$20","v":3.6009845000600924E-5},{"$f":"((150*($J$2^0.87)*(AB198^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z198)*3600*24","v":7.0814594867198738E-2},2.3915996627248484E-4,{"$f":"AE197-AD198*Bodencharakterisierung!$E$8","v":5.2052542426776954E-2},{"$f":"IF(AE198>$J$18,(AE198/(Bodencharakterisierung!$E$11*1000)),0)","v":3.4358113813054093E-5},2.3305291073371062E-2,181,null,{"$f":"(AD198)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH198>0,(AJ198*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK197,NA())","v":0.39152749322301472},null,181,{"$f":"IF(AF198<=$J$9*0.05,AS197*EXP((-$J$6*1)/Heterogenität!$D$4),Z198)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF198>=$J$19, AR197/$J$5<AN198),0, Bodencharakterisierung!$E$8*$J$11*((AR197/$J$5)-AN198))","v":0},0,{"$f":"AQ197-AP198*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ198/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,181,null,{"$f":"(AP198)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF198<=$J$9*1.05,(AV198*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW197,NA())","v":{"$error":"#N/A"}},23072.238162637354,314,4.886875333223017,0.39152749322301472,0,1.1353478400000026,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},34.358113813054096,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,182,2.3305291073371062E-2,{"$f":"Z199*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF198*Bodencharakterisierung!$E$11/$J$20","v":3.5955329030591927E-5},{"$f":"((150*($J$2^0.87)*(AB199^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z199)*3600*24","v":7.0729887451767698E-2},2.3915996627248484E-4,{"$f":"AE198-AD199*Bodencharakterisierung!$E$8","v":5.1973619637907031E-2},{"$f":"IF(AE199>$J$18,(AE199/(Bodencharakterisierung!$E$11*1000)),0)","v":3.4306019562974938E-5},2.3305291073371062E-2,182,null,{"$f":"(AD199)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH199>0,(AJ199*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK198,NA())","v":0.39369496047839048},null,182,{"$f":"IF(AF199<=$J$9*0.05,AS198*EXP((-$J$6*1)/Heterogenität!$D$4),Z199)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF199>=$J$19, AR198/$J$5<AN199),0, Bodencharakterisierung!$E$8*$J$11*((AR198/$J$5)-AN199))","v":0},0,{"$f":"AQ198-AP199*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ199/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,182,null,{"$f":"(AP199)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF199<=$J$9*1.05,(AV199*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW198,NA())","v":{"$error":"#N/A"}},23072.238162637354,315,4.8953154404783934,0.39369496047839048,0,1.1416204800000025,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},34.306019562974939,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,183,2.3305291073371062E-2,{"$f":"Z200*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF199*Bodencharakterisierung!$E$11/$J$20","v":3.5900813060582943E-5},{"$f":"((150*($J$2^0.87)*(AB200^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z200)*3600*24","v":7.0645153060772903E-2},2.3915996627248484E-4,{"$f":"AE199-AD200*Bodencharakterisierung!$E$8","v":5.1894696849037109E-2},{"$f":"IF(AE200>$J$18,(AE200/(Bodencharakterisierung!$E$11*1000)),0)","v":3.4253925312895783E-5},2.3305291073371062E-2,183,null,{"$f":"(AD200)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH200>0,(AJ200*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK199,NA())","v":0.39586242773376623},null,183,{"$f":"IF(AF200<=$J$9*0.05,AS199*EXP((-$J$6*1)/Heterogenität!$D$4),Z200)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF200>=$J$19, AR199/$J$5<AN200),0, Bodencharakterisierung!$E$8*$J$11*((AR199/$J$5)-AN200))","v":0},0,{"$f":"AQ199-AP200*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ200/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,183,null,{"$f":"(AP200)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF200<=$J$9*1.05,(AV200*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW199,NA())","v":{"$error":"#N/A"}},23072.238162637354,316,4.903755547733768,0.39586242773376623,0,1.1478931200000024,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},34.253925312895781,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,184,2.3305291073371062E-2,{"$f":"Z201*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF200*Bodencharakterisierung!$E$11/$J$20","v":3.5846297090573946E-5},{"$f":"((150*($J$2^0.87)*(AB201^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z201)*3600*24","v":7.0560391644641521E-2},2.3915996627248484E-4,{"$f":"AE200-AD201*Bodencharakterisierung!$E$8","v":5.1815774060167186E-2},{"$f":"IF(AE201>$J$18,(AE201/(Bodencharakterisierung!$E$11*1000)),0)","v":3.4201831062816627E-5},2.3305291073371062E-2,184,null,{"$f":"(AD201)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH201>0,(AJ201*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK200,NA())","v":0.39802989498914199},null,184,{"$f":"IF(AF201<=$J$9*0.05,AS200*EXP((-$J$6*1)/Heterogenität!$D$4),Z201)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF201>=$J$19, AR200/$J$5<AN201),0, Bodencharakterisierung!$E$8*$J$11*((AR200/$J$5)-AN201))","v":0},0,{"$f":"AQ200-AP201*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ201/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,184,null,{"$f":"(AP201)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF201<=$J$9*1.05,(AV201*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW200,NA())","v":{"$error":"#N/A"}},23072.238162637354,317,4.9121956549891443,0.39802989498914199,0,1.1541657600000024,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},34.20183106281663,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,185,2.3305291073371062E-2,{"$f":"Z202*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF201*Bodencharakterisierung!$E$11/$J$20","v":3.5791781120564955E-5},{"$f":"((150*($J$2^0.87)*(AB202^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z202)*3600*24","v":7.0475603153633798E-2},2.3915996627248484E-4,{"$f":"AE201-AD202*Bodencharakterisierung!$E$8","v":5.1736851271297263E-2},{"$f":"IF(AE202>$J$18,(AE202/(Bodencharakterisierung!$E$11*1000)),0)","v":3.4149736812737465E-5},2.3305291073371062E-2,185,null,{"$f":"(AD202)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH202>0,(AJ202*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK201,NA())","v":0.40019736224451774},null,185,{"$f":"IF(AF202<=$J$9*0.05,AS201*EXP((-$J$6*1)/Heterogenität!$D$4),Z202)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF202>=$J$19, AR201/$J$5<AN202),0, Bodencharakterisierung!$E$8*$J$11*((AR201/$J$5)-AN202))","v":0},0,{"$f":"AQ201-AP202*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ202/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,185,null,{"$f":"(AP202)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF202<=$J$9*1.05,(AV202*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW201,NA())","v":{"$error":"#N/A"}},23072.238162637354,318,4.9206357622445198,0.40019736224451774,0,1.1604384000000023,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},34.149736812737466,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,186,2.3305291073371062E-2,{"$f":"Z203*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF202*Bodencharakterisierung!$E$11/$J$20","v":3.5737265150555958E-5},{"$f":"((150*($J$2^0.87)*(AB203^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z203)*3600*24","v":7.0390787537842836E-2},2.3915996627248484E-4,{"$f":"AE202-AD203*Bodencharakterisierung!$E$8","v":5.165792848242734E-2},{"$f":"IF(AE203>$J$18,(AE203/(Bodencharakterisierung!$E$11*1000)),0)","v":3.409764256265831E-5},2.3305291073371062E-2,186,null,{"$f":"(AD203)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH203>0,(AJ203*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK202,NA())","v":0.40236482949989349},null,186,{"$f":"IF(AF203<=$J$9*0.05,AS202*EXP((-$J$6*1)/Heterogenität!$D$4),Z203)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF203>=$J$19, AR202/$J$5<AN203),0, Bodencharakterisierung!$E$8*$J$11*((AR202/$J$5)-AN203))","v":0},0,{"$f":"AQ202-AP203*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ203/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,186,null,{"$f":"(AP203)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF203<=$J$9*1.05,(AV203*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW202,NA())","v":{"$error":"#N/A"}},23072.238162637354,319,4.9290758694998953,0.40236482949989349,0,1.1667110400000023,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},34.097642562658308,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,187,2.3305291073371062E-2,{"$f":"Z204*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF203*Bodencharakterisierung!$E$11/$J$20","v":3.5682749180546967E-5},{"$f":"((150*($J$2^0.87)*(AB204^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z204)*3600*24","v":7.0305944747193164E-2},2.3915996627248484E-4,{"$f":"AE203-AD204*Bodencharakterisierung!$E$8","v":5.1579005693557417E-2},{"$f":"IF(AE204>$J$18,(AE204/(Bodencharakterisierung!$E$11*1000)),0)","v":3.4045548312579155E-5},2.3305291073371062E-2,187,null,{"$f":"(AD204)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH204>0,(AJ204*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK203,NA())","v":0.40453229675526925},null,187,{"$f":"IF(AF204<=$J$9*0.05,AS203*EXP((-$J$6*1)/Heterogenität!$D$4),Z204)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF204>=$J$19, AR203/$J$5<AN204),0, Bodencharakterisierung!$E$8*$J$11*((AR203/$J$5)-AN204))","v":0},0,{"$f":"AQ203-AP204*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ204/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,187,null,{"$f":"(AP204)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF204<=$J$9*1.05,(AV204*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW203,NA())","v":{"$error":"#N/A"}},23072.238162637354,320,4.9375159767552717,0.40453229675526925,0,1.1729836800000022,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},34.045548312579157,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,188,2.3305291073371062E-2,{"$f":"Z205*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF204*Bodencharakterisierung!$E$11/$J$20","v":3.5628233210537977E-5},{"$f":"((150*($J$2^0.87)*(AB205^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z205)*3600*24","v":7.0221074731440264E-2},2.3915996627248484E-4,{"$f":"AE204-AD205*Bodencharakterisierung!$E$8","v":5.1500082904687494E-2},{"$f":"IF(AE205>$J$18,(AE205/(Bodencharakterisierung!$E$11*1000)),0)","v":3.3993454062499993E-5},2.3305291073371062E-2,188,null,{"$f":"(AD205)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH205>0,(AJ205*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK204,NA())","v":0.406699764010645},null,188,{"$f":"IF(AF205<=$J$9*0.05,AS204*EXP((-$J$6*1)/Heterogenität!$D$4),Z205)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF205>=$J$19, AR204/$J$5<AN205),0, Bodencharakterisierung!$E$8*$J$11*((AR204/$J$5)-AN205))","v":0},0,{"$f":"AQ204-AP205*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ205/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,188,null,{"$f":"(AP205)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF205<=$J$9*1.05,(AV205*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW204,NA())","v":{"$error":"#N/A"}},23072.238162637354,321,4.9459560840106471,0.406699764010645,0,1.1792563200000021,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},33.993454062499993,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,189,2.3305291073371062E-2,{"$f":"Z206*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF205*Bodencharakterisierung!$E$11/$J$20","v":3.5573717240528979E-5},{"$f":"((150*($J$2^0.87)*(AB206^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z206)*3600*24","v":7.0136177440169811E-2},2.3915996627248484E-4,{"$f":"AE205-AD206*Bodencharakterisierung!$E$8","v":5.1421160115817571E-2},{"$f":"IF(AE206>$J$18,(AE206/(Bodencharakterisierung!$E$11*1000)),0)","v":3.3941359812420838E-5},2.3305291073371062E-2,189,null,{"$f":"(AD206)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH206>0,(AJ206*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK205,NA())","v":0.40886723126602076},null,189,{"$f":"IF(AF206<=$J$9*0.05,AS205*EXP((-$J$6*1)/Heterogenität!$D$4),Z206)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF206>=$J$19, AR205/$J$5<AN206),0, Bodencharakterisierung!$E$8*$J$11*((AR205/$J$5)-AN206))","v":0},0,{"$f":"AQ205-AP206*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ206/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,189,null,{"$f":"(AP206)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF206<=$J$9*1.05,(AV206*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW205,NA())","v":{"$error":"#N/A"}},23072.238162637354,322,4.9543961912660226,0.40886723126602076,0,1.1855289600000021,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},33.941359812420835,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,190,2.3305291073371062E-2,{"$f":"Z207*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF206*Bodencharakterisierung!$E$11/$J$20","v":3.5519201270519982E-5},{"$f":"((150*($J$2^0.87)*(AB207^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z207)*3600*24","v":7.0051252822796756E-2},2.3915996627248484E-4,{"$f":"AE206-AD207*Bodencharakterisierung!$E$8","v":5.1342237326947648E-2},{"$f":"IF(AE207>$J$18,(AE207/(Bodencharakterisierung!$E$11*1000)),0)","v":3.3889265562341682E-5},2.3305291073371062E-2,190,null,{"$f":"(AD207)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH207>0,(AJ207*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK206,NA())","v":0.41103469852139651},null,190,{"$f":"IF(AF207<=$J$9*0.05,AS206*EXP((-$J$6*1)/Heterogenität!$D$4),Z207)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF207>=$J$19, AR206/$J$5<AN207),0, Bodencharakterisierung!$E$8*$J$11*((AR206/$J$5)-AN207))","v":0},0,{"$f":"AQ206-AP207*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ207/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,190,null,{"$f":"(AP207)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF207<=$J$9*1.05,(AV207*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW206,NA())","v":{"$error":"#N/A"}},23072.238162637354,323,4.962836298521399,0.41103469852139651,0,1.191801600000002,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},33.889265562341684,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,191,2.3305291073371062E-2,{"$f":"Z208*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF207*Bodencharakterisierung!$E$11/$J$20","v":3.5464685300510991E-5},{"$f":"((150*($J$2^0.87)*(AB208^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z208)*3600*24","v":6.9966300828564226E-2},2.3915996627248484E-4,{"$f":"AE207-AD208*Bodencharakterisierung!$E$8","v":5.1263314538077726E-2},{"$f":"IF(AE208>$J$18,(AE208/(Bodencharakterisierung!$E$11*1000)),0)","v":3.3837171312262527E-5},2.3305291073371062E-2,191,null,{"$f":"(AD208)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH208>0,(AJ208*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK207,NA())","v":0.41320216577677227},null,191,{"$f":"IF(AF208<=$J$9*0.05,AS207*EXP((-$J$6*1)/Heterogenität!$D$4),Z208)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF208>=$J$19, AR207/$J$5<AN208),0, Bodencharakterisierung!$E$8*$J$11*((AR207/$J$5)-AN208))","v":0},0,{"$f":"AQ207-AP208*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ208/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,191,null,{"$f":"(AP208)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF208<=$J$9*1.05,(AV208*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW207,NA())","v":{"$error":"#N/A"}},23072.238162637354,324,4.9712764057767735,0.41320216577677227,0,1.198074240000002,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},33.837171312262527,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,192,2.3305291073371062E-2,{"$f":"Z209*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF208*Bodencharakterisierung!$E$11/$J$20","v":3.5410169330502001E-5},{"$f":"((150*($J$2^0.87)*(AB209^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z209)*3600*24","v":6.9881321406543129E-2},2.3915996627248484E-4,{"$f":"AE208-AD209*Bodencharakterisierung!$E$8","v":5.1184391749207803E-2},{"$f":"IF(AE209>$J$18,(AE209/(Bodencharakterisierung!$E$11*1000)),0)","v":3.3785077062183365E-5},2.3305291073371062E-2,192,null,{"$f":"(AD209)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH209>0,(AJ209*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK208,NA())","v":0.41536963303214802},null,192,{"$f":"IF(AF209<=$J$9*0.05,AS208*EXP((-$J$6*1)/Heterogenität!$D$4),Z209)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF209>=$J$19, AR208/$J$5<AN209),0, Bodencharakterisierung!$E$8*$J$11*((AR208/$J$5)-AN209))","v":0},0,{"$f":"AQ208-AP209*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ209/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,192,null,{"$f":"(AP209)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF209<=$J$9*1.05,(AV209*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW208,NA())","v":{"$error":"#N/A"}},23072.238162637354,325,4.9797165130321499,0.41536963303214802,0,1.2043468800000019,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},33.785077062183362,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,193,2.3305291073371062E-2,{"$f":"Z210*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF209*Bodencharakterisierung!$E$11/$J$20","v":3.5355653360493003E-5},{"$f":"((150*($J$2^0.87)*(AB210^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z210)*3600*24","v":6.9796314505630605E-2},2.3915996627248484E-4,{"$f":"AE209-AD210*Bodencharakterisierung!$E$8","v":5.110546896033788E-2},{"$f":"IF(AE210>$J$18,(AE210/(Bodencharakterisierung!$E$11*1000)),0)","v":3.373298281210421E-5},2.3305291073371062E-2,193,null,{"$f":"(AD210)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH210>0,(AJ210*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK209,NA())","v":0.41753710028752378},null,193,{"$f":"IF(AF210<=$J$9*0.05,AS209*EXP((-$J$6*1)/Heterogenität!$D$4),Z210)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF210>=$J$19, AR209/$J$5<AN210),0, Bodencharakterisierung!$E$8*$J$11*((AR209/$J$5)-AN210))","v":0},0,{"$f":"AQ209-AP210*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ210/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,193,null,{"$f":"(AP210)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF210<=$J$9*1.05,(AV210*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW209,NA())","v":{"$error":"#N/A"}},23072.238162637354,326,4.9881566202875254,0.41753710028752378,0,1.2106195200000018,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},33.732982812104211,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,194,2.3305291073371062E-2,{"$f":"Z211*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF210*Bodencharakterisierung!$E$11/$J$20","v":3.5301137390484013E-5},{"$f":"((150*($J$2^0.87)*(AB211^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z211)*3600*24","v":6.9711280074550241E-2},2.3915996627248484E-4,{"$f":"AE210-AD211*Bodencharakterisierung!$E$8","v":5.1026546171467957E-2},{"$f":"IF(AE211>$J$18,(AE211/(Bodencharakterisierung!$E$11*1000)),0)","v":3.3680888562025055E-5},2.3305291073371062E-2,194,null,{"$f":"(AD211)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH211>0,(AJ211*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK210,NA())","v":0.41970456754289953},null,194,{"$f":"IF(AF211<=$J$9*0.05,AS210*EXP((-$J$6*1)/Heterogenität!$D$4),Z211)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF211>=$J$19, AR210/$J$5<AN211),0, Bodencharakterisierung!$E$8*$J$11*((AR210/$J$5)-AN211))","v":0},0,{"$f":"AQ210-AP211*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ211/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,194,null,{"$f":"(AP211)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF211<=$J$9*1.05,(AV211*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW210,NA())","v":{"$error":"#N/A"}},23072.238162637354,327,4.9965967275429009,0.41970456754289953,0,1.2168921600000018,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},33.680888562025054,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,195,2.3305291073371062E-2,{"$f":"Z212*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF211*Bodencharakterisierung!$E$11/$J$20","v":3.5246621420475022E-5},{"$f":"((150*($J$2^0.87)*(AB212^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z212)*3600*24","v":6.9626218061850292E-2},2.3915996627248484E-4,{"$f":"AE211-AD212*Bodencharakterisierung!$E$8","v":5.0947623382598034E-2},{"$f":"IF(AE212>$J$18,(AE212/(Bodencharakterisierung!$E$11*1000)),0)","v":3.3628794311945899E-5},2.3305291073371062E-2,195,null,{"$f":"(AD212)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH212>0,(AJ212*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK211,NA())","v":0.42187203479827529},null,195,{"$f":"IF(AF212<=$J$9*0.05,AS211*EXP((-$J$6*1)/Heterogenität!$D$4),Z212)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF212>=$J$19, AR211/$J$5<AN212),0, Bodencharakterisierung!$E$8*$J$11*((AR211/$J$5)-AN212))","v":0},0,{"$f":"AQ211-AP212*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ212/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,195,null,{"$f":"(AP212)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF212<=$J$9*1.05,(AV212*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW211,NA())","v":{"$error":"#N/A"}},23072.238162637354,328,5.0050368347982772,0.42187203479827529,0,{"$f":"$G$34/$G$12/$G$8+BC211","v":1.2231648000000017},null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},33.628794311945903,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,196,2.3305291073371062E-2,{"$f":"Z213*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF212*Bodencharakterisierung!$E$11/$J$20","v":3.5192105450466031E-5},{"$f":"((150*($J$2^0.87)*(AB213^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z213)*3600*24","v":6.9541128415902972E-2},2.3915996627248484E-4,{"$f":"AE212-AD213*Bodencharakterisierung!$E$8","v":5.0868700593728111E-2},{"$f":"IF(AE213>$J$18,(AE213/(Bodencharakterisierung!$E$11*1000)),0)","v":3.3576700061866737E-5},2.3305291073371062E-2,196,null,{"$f":"(AD213)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH213>0,(AJ213*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK212,NA())","v":0.42403950205365104},null,196,{"$f":"IF(AF213<=$J$9*0.05,AS212*EXP((-$J$6*1)/Heterogenität!$D$4),Z213)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF213>=$J$19, AR212/$J$5<AN213),0, Bodencharakterisierung!$E$8*$J$11*((AR212/$J$5)-AN213))","v":0},0,{"$f":"AQ212-AP213*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ213/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,196,null,{"$f":"(AP213)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF213<=$J$9*1.05,(AV213*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW212,NA())","v":{"$error":"#N/A"}},23072.238162637354,329,5.0134769420536527,0.42403950205365104,0,1.2294374400000017,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},33.576700061866738,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,197,2.3305291073371062E-2,{"$f":"Z214*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF213*Bodencharakterisierung!$E$11/$J$20","v":3.5137589480457034E-5},{"$f":"((150*($J$2^0.87)*(AB214^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z214)*3600*24","v":6.9456011084903943E-2},2.3915996627248484E-4,{"$f":"AE213-AD214*Bodencharakterisierung!$E$8","v":5.0789777804858188E-2},{"$f":"IF(AE214>$J$18,(AE214/(Bodencharakterisierung!$E$11*1000)),0)","v":3.3524605811787582E-5},2.3305291073371062E-2,197,null,{"$f":"(AD214)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH214>0,(AJ214*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK213,NA())","v":0.4262069693090268},null,197,{"$f":"IF(AF214<=$J$9*0.05,AS213*EXP((-$J$6*1)/Heterogenität!$D$4),Z214)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF214>=$J$19, AR213/$J$5<AN214),0, Bodencharakterisierung!$E$8*$J$11*((AR213/$J$5)-AN214))","v":0},0,{"$f":"AQ213-AP214*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ214/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,197,null,{"$f":"(AP214)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF214<=$J$9*1.05,(AV214*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW213,NA())","v":{"$error":"#N/A"}},23072.238162637354,330,5.0219170493090282,0.4262069693090268,0,1.2357100800000016,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},33.52460581178758,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,198,{"$f":"AG214","v":2.3305291073371062E-2},{"$f":"Z215*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF214*Bodencharakterisierung!$E$11/$J$20","v":3.5083073510448043E-5},{"$f":"((150*($J$2^0.87)*(AB215^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z215)*3600*24","v":6.9370866016871091E-2},{"$f":"MIN(AC215,Z215-AA215)","v":2.3915996627248484E-4},{"$f":"AE214-AD215*Bodencharakterisierung!$E$8","v":5.0710855015988265E-2},{"$f":"IF(AE215>$J$18,(AE215/(Bodencharakterisierung!$E$11*1000)),0)","v":3.3472511561708427E-5},{"$f":"AA215+AD215","v":2.3305291073371062E-2},{"$f":"IF(AD215>0,Y215,NA())","v":198},null,{"$f":"(AD215)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH215>0,(AJ215*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK214,NA())","v":0.42837443656440255},null,198,{"$f":"IF(AF215<=$J$9*0.05,AS214*EXP((-$J$6*1)/Heterogenität!$D$4),Z215)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF215>=$J$19, AR214/$J$5<AN215),0, Bodencharakterisierung!$E$8*$J$11*((AR214/$J$5)-AN215))","v":0},{"$f":"MIN(AO215,AS214-AN215)","v":0},{"$f":"AQ214-AP215*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ215/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},{"$f":"AN215+AP215","v":2.3305291073371062E-2},{"$f":"IF(AN215>$G$5,AM215,NA())","v":198},null,{"$f":"(AP215)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF215<=$J$9*1.05,(AV215*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW214,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH215>($G$5*10^6),BH215*0.99,9999)","v":23072.238162637354},{"$f":"AT215+$G$3","v":331},{"$f":"IF(ISNUMBER(AT215),BA215+BB215+BC215+$AZ$17,\"\")","v":5.0303571565644045},{"$f":"IF(ISNUMBER(AK215),AK215,BA214)","v":0.42837443656440255},{"$f":"IF(ISNUMBER(AW215),AW215,0)","v":0},1.2419827200000015,null,{"$f":"AR215*10^6","v":4.3827000000643475},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF215*10^6","v":33.47251156170843},{"$f":"AN215*10^6","v":23305.291073371063}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,199,2.3305291073371062E-2,{"$f":"Z216*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF215*Bodencharakterisierung!$E$11/$J$20","v":3.5028557540439046E-5},{"$f":"((150*($J$2^0.87)*(AB216^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z216)*3600*24","v":6.9285693159643905E-2},2.3915996627248484E-4,{"$f":"AE215-AD216*Bodencharakterisierung!$E$8","v":5.0631932227118343E-2},{"$f":"IF(AE216>$J$18,(AE216/(Bodencharakterisierung!$E$11*1000)),0)","v":3.3420417311629272E-5},2.3305291073371062E-2,199,null,{"$f":"(AD216)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH216>0,(AJ216*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK215,NA())","v":0.4305419038197783},null,199,{"$f":"IF(AF216<=$J$9*0.05,AS215*EXP((-$J$6*1)/Heterogenität!$D$4),Z216)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF216>=$J$19, AR215/$J$5<AN216),0, Bodencharakterisierung!$E$8*$J$11*((AR215/$J$5)-AN216))","v":0},0,{"$f":"AQ215-AP216*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ216/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,199,null,{"$f":"(AP216)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF216<=$J$9*1.05,(AV216*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW215,NA())","v":{"$error":"#N/A"}},23072.238162637354,332,5.0387972638197791,0.4305419038197783,0,1.2482553600000015,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},33.420417311629272,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,200,2.3305291073371062E-2,{"$f":"Z217*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF216*Bodencharakterisierung!$E$11/$J$20","v":3.4974041570430062E-5},{"$f":"((150*($J$2^0.87)*(AB217^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z217)*3600*24","v":6.9200492460882182E-2},2.3915996627248484E-4,{"$f":"AE216-AD217*Bodencharakterisierung!$E$8","v":5.055300943824842E-2},{"$f":"IF(AE217>$J$18,(AE217/(Bodencharakterisierung!$E$11*1000)),0)","v":3.336832306155011E-5},2.3305291073371062E-2,200,null,{"$f":"(AD217)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH217>0,(AJ217*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK216,NA())","v":0.43270937107515406},null,200,{"$f":"IF(AF217<=$J$9*0.05,AS216*EXP((-$J$6*1)/Heterogenität!$D$4),Z217)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF217>=$J$19, AR216/$J$5<AN217),0, Bodencharakterisierung!$E$8*$J$11*((AR216/$J$5)-AN217))","v":0},0,{"$f":"AQ216-AP217*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ217/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,200,null,{"$f":"(AP217)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF217<=$J$9*1.05,(AV217*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW216,NA())","v":{"$error":"#N/A"}},23072.238162637354,333,5.0472373710751555,0.43270937107515406,0,1.2545280000000014,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},33.368323061550107,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,201,2.3305291073371062E-2,{"$f":"Z218*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF217*Bodencharakterisierung!$E$11/$J$20","v":3.4919525600421065E-5},{"$f":"((150*($J$2^0.87)*(AB218^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z218)*3600*24","v":6.9115263868065782E-2},2.3915996627248484E-4,{"$f":"AE217-AD218*Bodencharakterisierung!$E$8","v":5.0474086649378497E-2},{"$f":"IF(AE218>$J$18,(AE218/(Bodencharakterisierung!$E$11*1000)),0)","v":3.3316228811470955E-5},2.3305291073371062E-2,201,null,{"$f":"(AD218)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH218>0,(AJ218*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK217,NA())","v":0.43487683833052981},null,201,{"$f":"IF(AF218<=$J$9*0.05,AS217*EXP((-$J$6*1)/Heterogenität!$D$4),Z218)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF218>=$J$19, AR217/$J$5<AN218),0, Bodencharakterisierung!$E$8*$J$11*((AR217/$J$5)-AN218))","v":0},0,{"$f":"AQ217-AP218*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ218/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,201,null,{"$f":"(AP218)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF218<=$J$9*1.05,(AV218*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW217,NA())","v":{"$error":"#N/A"}},23072.238162637354,334,5.0556774783305309,0.43487683833052981,0,1.2608006400000014,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},33.316228811470957,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,202,2.3305291073371062E-2,{"$f":"Z219*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF218*Bodencharakterisierung!$E$11/$J$20","v":3.4865009630412067E-5},{"$f":"((150*($J$2^0.87)*(AB219^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z219)*3600*24","v":6.9030007328492793E-2},2.3915996627248484E-4,{"$f":"AE218-AD219*Bodencharakterisierung!$E$8","v":5.0395163860508574E-2},{"$f":"IF(AE219>$J$18,(AE219/(Bodencharakterisierung!$E$11*1000)),0)","v":3.3264134561391799E-5},2.3305291073371062E-2,202,null,{"$f":"(AD219)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH219>0,(AJ219*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK218,NA())","v":0.43704430558590557},null,202,{"$f":"IF(AF219<=$J$9*0.05,AS218*EXP((-$J$6*1)/Heterogenität!$D$4),Z219)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF219>=$J$19, AR218/$J$5<AN219),0, Bodencharakterisierung!$E$8*$J$11*((AR218/$J$5)-AN219))","v":0},0,{"$f":"AQ218-AP219*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ219/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,202,null,{"$f":"(AP219)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF219<=$J$9*1.05,(AV219*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW218,NA())","v":{"$error":"#N/A"}},23072.238162637354,335,5.0641175855859064,0.43704430558590557,0,1.2670732800000013,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},33.264134561391799,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,203,2.3305291073371062E-2,{"$f":"Z220*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF219*Bodencharakterisierung!$E$11/$J$20","v":3.4810493660403077E-5},{"$f":"((150*($J$2^0.87)*(AB220^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z220)*3600*24","v":6.8944722789279517E-2},2.3915996627248484E-4,{"$f":"AE219-AD220*Bodencharakterisierung!$E$8","v":5.0316241071638651E-2},{"$f":"IF(AE220>$J$18,(AE220/(Bodencharakterisierung!$E$11*1000)),0)","v":3.3212040311312644E-5},2.3305291073371062E-2,203,null,{"$f":"(AD220)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH220>0,(AJ220*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK219,NA())","v":0.43921177284128132},null,203,{"$f":"IF(AF220<=$J$9*0.05,AS219*EXP((-$J$6*1)/Heterogenität!$D$4),Z220)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF220>=$J$19, AR219/$J$5<AN220),0, Bodencharakterisierung!$E$8*$J$11*((AR219/$J$5)-AN220))","v":0},0,{"$f":"AQ219-AP220*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ220/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,203,null,{"$f":"(AP220)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF220<=$J$9*1.05,(AV220*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW219,NA())","v":{"$error":"#N/A"}},23072.238162637354,336,5.0725576928412828,0.43921177284128132,0,1.2733459200000012,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},33.212040311312641,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,204,2.3305291073371062E-2,{"$f":"Z221*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF220*Bodencharakterisierung!$E$11/$J$20","v":3.4755977690394086E-5},{"$f":"((150*($J$2^0.87)*(AB221^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z221)*3600*24","v":6.8859410197359319E-2},2.3915996627248484E-4,{"$f":"AE220-AD221*Bodencharakterisierung!$E$8","v":5.0237318282768728E-2},{"$f":"IF(AE221>$J$18,(AE221/(Bodencharakterisierung!$E$11*1000)),0)","v":3.3159946061233482E-5},2.3305291073371062E-2,204,null,{"$f":"(AD221)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH221>0,(AJ221*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK220,NA())","v":0.44137924009665708},null,204,{"$f":"IF(AF221<=$J$9*0.05,AS220*EXP((-$J$6*1)/Heterogenität!$D$4),Z221)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF221>=$J$19, AR220/$J$5<AN221),0, Bodencharakterisierung!$E$8*$J$11*((AR220/$J$5)-AN221))","v":0},0,{"$f":"AQ220-AP221*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ221/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,204,null,{"$f":"(AP221)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF221<=$J$9*1.05,(AV221*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW220,NA())","v":{"$error":"#N/A"}},23072.238162637354,337,5.0809978000966582,0.44137924009665708,0,1.2796185600000012,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},33.159946061233484,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,205,2.3305291073371062E-2,{"$f":"Z222*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF221*Bodencharakterisierung!$E$11/$J$20","v":3.4701461720385089E-5},{"$f":"((150*($J$2^0.87)*(AB222^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z222)*3600*24","v":6.8774069499481325E-2},2.3915996627248484E-4,{"$f":"AE221-AD222*Bodencharakterisierung!$E$8","v":5.0158395493898805E-2},{"$f":"IF(AE222>$J$18,(AE222/(Bodencharakterisierung!$E$11*1000)),0)","v":3.3107851811154327E-5},2.3305291073371062E-2,205,null,{"$f":"(AD222)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH222>0,(AJ222*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK221,NA())","v":0.44354670735203283},null,205,{"$f":"IF(AF222<=$J$9*0.05,AS221*EXP((-$J$6*1)/Heterogenität!$D$4),Z222)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF222>=$J$19, AR221/$J$5<AN222),0, Bodencharakterisierung!$E$8*$J$11*((AR221/$J$5)-AN222))","v":0},0,{"$f":"AQ221-AP222*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ222/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,205,null,{"$f":"(AP222)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF222<=$J$9*1.05,(AV222*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW221,NA())","v":{"$error":"#N/A"}},23072.238162637354,338,5.0894379073520337,0.44354670735203283,0,1.2858912000000011,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},33.107851811154326,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,206,2.3305291073371062E-2,{"$f":"Z223*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF222*Bodencharakterisierung!$E$11/$J$20","v":3.4646945750376098E-5},{"$f":"((150*($J$2^0.87)*(AB223^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z223)*3600*24","v":6.8688700642209541E-2},2.3915996627248484E-4,{"$f":"AE222-AD223*Bodencharakterisierung!$E$8","v":5.0079472705028882E-2},{"$f":"IF(AE223>$J$18,(AE223/(Bodencharakterisierung!$E$11*1000)),0)","v":3.3055757561075172E-5},2.3305291073371062E-2,206,null,{"$f":"(AD223)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH223>0,(AJ223*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK222,NA())","v":0.44571417460740859},null,206,{"$f":"IF(AF223<=$J$9*0.05,AS222*EXP((-$J$6*1)/Heterogenität!$D$4),Z223)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF223>=$J$19, AR222/$J$5<AN223),0, Bodencharakterisierung!$E$8*$J$11*((AR222/$J$5)-AN223))","v":0},0,{"$f":"AQ222-AP223*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ223/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,206,null,{"$f":"(AP223)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF223<=$J$9*1.05,(AV223*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW222,NA())","v":{"$error":"#N/A"}},23072.238162637354,339,5.0978780146074101,0.44571417460740859,0,1.2921638400000011,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},33.055757561075168,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,207,2.3305291073371062E-2,{"$f":"Z224*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF223*Bodencharakterisierung!$E$11/$J$20","v":3.4592429780367101E-5},{"$f":"((150*($J$2^0.87)*(AB224^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z224)*3600*24","v":6.8603303571922569E-2},2.3915996627248484E-4,{"$f":"AE223-AD224*Bodencharakterisierung!$E$8","v":5.0000549916158959E-2},{"$f":"IF(AE224>$J$18,(AE224/(Bodencharakterisierung!$E$11*1000)),0)","v":3.300366331099601E-5},2.3305291073371062E-2,207,null,{"$f":"(AD224)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH224>0,(AJ224*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK223,NA())","v":0.44788164186278434},null,207,{"$f":"IF(AF224<=$J$9*0.05,AS223*EXP((-$J$6*1)/Heterogenität!$D$4),Z224)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF224>=$J$19, AR223/$J$5<AN224),0, Bodencharakterisierung!$E$8*$J$11*((AR223/$J$5)-AN224))","v":0},0,{"$f":"AQ223-AP224*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ224/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,207,null,{"$f":"(AP224)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF224<=$J$9*1.05,(AV224*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW223,NA())","v":{"$error":"#N/A"}},23072.238162637354,340,5.1063181218627847,0.44788164186278434,0,1.298436480000001,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},33.003663310996011,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,208,2.3305291073371062E-2,{"$f":"Z225*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF224*Bodencharakterisierung!$E$11/$J$20","v":3.4537913810358104E-5},{"$f":"((150*($J$2^0.87)*(AB225^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z225)*3600*24","v":6.8517878234812174E-2},2.3915996627248484E-4,{"$f":"AE224-AD225*Bodencharakterisierung!$E$8","v":4.9921627127289037E-2},{"$f":"IF(AE225>$J$18,(AE225/(Bodencharakterisierung!$E$11*1000)),0)","v":3.2951569060916854E-5},2.3305291073371062E-2,208,null,{"$f":"(AD225)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH225>0,(AJ225*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK224,NA())","v":0.4500491091181601},null,208,{"$f":"IF(AF225<=$J$9*0.05,AS224*EXP((-$J$6*1)/Heterogenität!$D$4),Z225)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF225>=$J$19, AR224/$J$5<AN225),0, Bodencharakterisierung!$E$8*$J$11*((AR224/$J$5)-AN225))","v":0},0,{"$f":"AQ224-AP225*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ225/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,208,null,{"$f":"(AP225)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF225<=$J$9*1.05,(AV225*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW224,NA())","v":{"$error":"#N/A"}},23072.238162637354,341,5.114758229118161,0.4500491091181601,0,1.3047091200000009,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},32.951569060916853,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,209,2.3305291073371062E-2,{"$f":"Z226*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF225*Bodencharakterisierung!$E$11/$J$20","v":3.4483397840349113E-5},{"$f":"((150*($J$2^0.87)*(AB226^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z226)*3600*24","v":6.8432424576882103E-2},2.3915996627248484E-4,{"$f":"AE225-AD226*Bodencharakterisierung!$E$8","v":4.9842704338419114E-2},{"$f":"IF(AE226>$J$18,(AE226/(Bodencharakterisierung!$E$11*1000)),0)","v":3.2899474810837699E-5},2.3305291073371062E-2,209,null,{"$f":"(AD226)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH226>0,(AJ226*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK225,NA())","v":0.45221657637353585},null,209,{"$f":"IF(AF226<=$J$9*0.05,AS225*EXP((-$J$6*1)/Heterogenität!$D$4),Z226)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF226>=$J$19, AR225/$J$5<AN226),0, Bodencharakterisierung!$E$8*$J$11*((AR225/$J$5)-AN226))","v":0},0,{"$f":"AQ225-AP226*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ226/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,209,null,{"$f":"(AP226)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF226<=$J$9*1.05,(AV226*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW225,NA())","v":{"$error":"#N/A"}},23072.238162637354,342,5.1231983363735365,0.45221657637353585,0,1.3109817600000009,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},32.899474810837702,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,210,2.3305291073371062E-2,{"$f":"Z227*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF226*Bodencharakterisierung!$E$11/$J$20","v":3.4428881870340122E-5},{"$f":"((150*($J$2^0.87)*(AB227^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z227)*3600*24","v":6.8346942543947714E-2},2.3915996627248484E-4,{"$f":"AE226-AD227*Bodencharakterisierung!$E$8","v":4.9763781549549191E-2},{"$f":"IF(AE227>$J$18,(AE227/(Bodencharakterisierung!$E$11*1000)),0)","v":3.2847380560758544E-5},2.3305291073371062E-2,210,null,{"$f":"(AD227)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH227>0,(AJ227*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK226,NA())","v":0.4543840436289116},null,210,{"$f":"IF(AF227<=$J$9*0.05,AS226*EXP((-$J$6*1)/Heterogenität!$D$4),Z227)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF227>=$J$19, AR226/$J$5<AN227),0, Bodencharakterisierung!$E$8*$J$11*((AR226/$J$5)-AN227))","v":0},0,{"$f":"AQ226-AP227*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ227/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,210,null,{"$f":"(AP227)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF227<=$J$9*1.05,(AV227*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW226,NA())","v":{"$error":"#N/A"}},23072.238162637354,343,5.131638443628912,0.4543840436289116,0,1.3172544000000008,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},32.847380560758545,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,211,2.3305291073371062E-2,{"$f":"Z228*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF227*Bodencharakterisierung!$E$11/$J$20","v":3.4374365900331132E-5},{"$f":"((150*($J$2^0.87)*(AB228^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z228)*3600*24","v":6.8261432081634293E-2},2.3915996627248484E-4,{"$f":"AE227-AD228*Bodencharakterisierung!$E$8","v":4.9684858760679268E-2},{"$f":"IF(AE228>$J$18,(AE228/(Bodencharakterisierung!$E$11*1000)),0)","v":3.2795286310679382E-5},2.3305291073371062E-2,211,null,{"$f":"(AD228)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH228>0,(AJ228*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK227,NA())","v":0.45655151088428736},null,211,{"$f":"IF(AF228<=$J$9*0.05,AS227*EXP((-$J$6*1)/Heterogenität!$D$4),Z228)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF228>=$J$19, AR227/$J$5<AN228),0, Bodencharakterisierung!$E$8*$J$11*((AR227/$J$5)-AN228))","v":0},0,{"$f":"AQ227-AP228*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ228/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,211,null,{"$f":"(AP228)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF228<=$J$9*1.05,(AV228*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW227,NA())","v":{"$error":"#N/A"}},23072.238162637354,344,5.1400785508842883,0.45655151088428736,0,1.3235270400000008,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},32.79528631067938,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,212,2.3305291073371062E-2,{"$f":"Z229*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF228*Bodencharakterisierung!$E$11/$J$20","v":3.4319849930322134E-5},{"$f":"((150*($J$2^0.87)*(AB229^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z229)*3600*24","v":6.8175893135377169E-2},2.3915996627248484E-4,{"$f":"AE228-AD229*Bodencharakterisierung!$E$8","v":4.9605935971809345E-2},{"$f":"IF(AE229>$J$18,(AE229/(Bodencharakterisierung!$E$11*1000)),0)","v":3.2743192060600227E-5},2.3305291073371062E-2,212,null,{"$f":"(AD229)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH229>0,(AJ229*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK228,NA())","v":0.45871897813966311},null,212,{"$f":"IF(AF229<=$J$9*0.05,AS228*EXP((-$J$6*1)/Heterogenität!$D$4),Z229)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF229>=$J$19, AR228/$J$5<AN229),0, Bodencharakterisierung!$E$8*$J$11*((AR228/$J$5)-AN229))","v":0},0,{"$f":"AQ228-AP229*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ229/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,212,null,{"$f":"(AP229)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF229<=$J$9*1.05,(AV229*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW228,NA())","v":{"$error":"#N/A"}},23072.238162637354,345,5.1485186581396638,0.45871897813966311,0,1.3297996800000007,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},32.743192060600229,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,213,2.3305291073371062E-2,{"$f":"Z230*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF229*Bodencharakterisierung!$E$11/$J$20","v":3.4265333960313144E-5},{"$f":"((150*($J$2^0.87)*(AB230^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z230)*3600*24","v":6.809032565041942E-2},2.3915996627248484E-4,{"$f":"AE229-AD230*Bodencharakterisierung!$E$8","v":4.9527013182939422E-2},{"$f":"IF(AE230>$J$18,(AE230/(Bodencharakterisierung!$E$11*1000)),0)","v":3.2691097810521072E-5},2.3305291073371062E-2,213,null,{"$f":"(AD230)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH230>0,(AJ230*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK229,NA())","v":0.46088644539503887},null,213,{"$f":"IF(AF230<=$J$9*0.05,AS229*EXP((-$J$6*1)/Heterogenität!$D$4),Z230)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF230>=$J$19, AR229/$J$5<AN230),0, Bodencharakterisierung!$E$8*$J$11*((AR229/$J$5)-AN230))","v":0},0,{"$f":"AQ229-AP230*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ230/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,213,null,{"$f":"(AP230)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF230<=$J$9*1.05,(AV230*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW229,NA())","v":{"$error":"#N/A"}},23072.238162637354,346,5.1569587653950393,0.46088644539503887,0,1.3360723200000006,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},32.691097810521072,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,214,2.3305291073371062E-2,{"$f":"Z231*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF230*Bodencharakterisierung!$E$11/$J$20","v":3.4210817990304153E-5},{"$f":"((150*($J$2^0.87)*(AB231^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z231)*3600*24","v":6.8004729571811931E-2},2.3915996627248484E-4,{"$f":"AE230-AD231*Bodencharakterisierung!$E$8","v":4.9448090394069499E-2},{"$f":"IF(AE231>$J$18,(AE231/(Bodencharakterisierung!$E$11*1000)),0)","v":3.2639003560441916E-5},2.3305291073371062E-2,214,null,{"$f":"(AD231)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH231>0,(AJ231*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK230,NA())","v":0.46305391265041462},null,214,{"$f":"IF(AF231<=$J$9*0.05,AS230*EXP((-$J$6*1)/Heterogenität!$D$4),Z231)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF231>=$J$19, AR230/$J$5<AN231),0, Bodencharakterisierung!$E$8*$J$11*((AR230/$J$5)-AN231))","v":0},0,{"$f":"AQ230-AP231*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ231/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,214,null,{"$f":"(AP231)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF231<=$J$9*1.05,(AV231*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW230,NA())","v":{"$error":"#N/A"}},23072.238162637354,347,5.1653988726504156,0.46305391265041462,0,1.3423449600000006,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},32.639003560441914,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,215,2.3305291073371062E-2,{"$f":"Z232*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF231*Bodencharakterisierung!$E$11/$J$20","v":3.4156302020295163E-5},{"$f":"((150*($J$2^0.87)*(AB232^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z232)*3600*24","v":6.7919104844412131E-2},2.3915996627248484E-4,{"$f":"AE231-AD232*Bodencharakterisierung!$E$8","v":4.9369167605199576E-2},{"$f":"IF(AE232>$J$18,(AE232/(Bodencharakterisierung!$E$11*1000)),0)","v":3.2586909310362754E-5},2.3305291073371062E-2,215,null,{"$f":"(AD232)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH232>0,(AJ232*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK231,NA())","v":0.46522137990579038},null,215,{"$f":"IF(AF232<=$J$9*0.05,AS231*EXP((-$J$6*1)/Heterogenität!$D$4),Z232)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF232>=$J$19, AR231/$J$5<AN232),0, Bodencharakterisierung!$E$8*$J$11*((AR231/$J$5)-AN232))","v":0},0,{"$f":"AQ231-AP232*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ232/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,215,null,{"$f":"(AP232)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF232<=$J$9*1.05,(AV232*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW231,NA())","v":{"$error":"#N/A"}},23072.238162637354,348,5.1738389799057902,0.46522137990579038,0,1.3486176000000005,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},32.586909310362756,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,216,2.3305291073371062E-2,{"$f":"Z233*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF232*Bodencharakterisierung!$E$11/$J$20","v":3.4101786050286165E-5},{"$f":"((150*($J$2^0.87)*(AB233^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z233)*3600*24","v":6.7833451412882564E-2},2.3915996627248484E-4,{"$f":"AE232-AD233*Bodencharakterisierung!$E$8","v":4.9290244816329654E-2},{"$f":"IF(AE233>$J$18,(AE233/(Bodencharakterisierung!$E$11*1000)),0)","v":3.2534815060283599E-5},2.3305291073371062E-2,216,null,{"$f":"(AD233)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH233>0,(AJ233*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK232,NA())","v":0.46738884716116613},null,216,{"$f":"IF(AF233<=$J$9*0.05,AS232*EXP((-$J$6*1)/Heterogenität!$D$4),Z233)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF233>=$J$19, AR232/$J$5<AN233),0, Bodencharakterisierung!$E$8*$J$11*((AR232/$J$5)-AN233))","v":0},0,{"$f":"AQ232-AP233*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ233/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,216,null,{"$f":"(AP233)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF233<=$J$9*1.05,(AV233*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW232,NA())","v":{"$error":"#N/A"}},23072.238162637354,349,5.1822790871611666,0.46738884716116613,0,1.3548902400000005,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},32.534815060283599,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,217,2.3305291073371062E-2,{"$f":"Z234*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF233*Bodencharakterisierung!$E$11/$J$20","v":3.4047270080277168E-5},{"$f":"((150*($J$2^0.87)*(AB234^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z234)*3600*24","v":6.7747769221690499E-2},2.3915996627248484E-4,{"$f":"AE233-AD234*Bodencharakterisierung!$E$8","v":4.9211322027459731E-2},{"$f":"IF(AE234>$J$18,(AE234/(Bodencharakterisierung!$E$11*1000)),0)","v":3.2482720810204444E-5},2.3305291073371062E-2,217,null,{"$f":"(AD234)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH234>0,(AJ234*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK233,NA())","v":0.46955631441654189},null,217,{"$f":"IF(AF234<=$J$9*0.05,AS233*EXP((-$J$6*1)/Heterogenität!$D$4),Z234)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF234>=$J$19, AR233/$J$5<AN234),0, Bodencharakterisierung!$E$8*$J$11*((AR233/$J$5)-AN234))","v":0},0,{"$f":"AQ233-AP234*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ234/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,217,null,{"$f":"(AP234)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF234<=$J$9*1.05,(AV234*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW233,NA())","v":{"$error":"#N/A"}},23072.238162637354,350,5.1907191944165421,0.46955631441654189,0,1.3611628800000004,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},32.482720810204441,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,218,2.3305291073371062E-2,{"$f":"Z235*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF234*Bodencharakterisierung!$E$11/$J$20","v":3.3992754110268184E-5},{"$f":"((150*($J$2^0.87)*(AB235^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z235)*3600*24","v":6.7662058215106735E-2},2.3915996627248484E-4,{"$f":"AE234-AD235*Bodencharakterisierung!$E$8","v":4.9132399238589808E-2},{"$f":"IF(AE235>$J$18,(AE235/(Bodencharakterisierung!$E$11*1000)),0)","v":3.2430626560125289E-5},2.3305291073371062E-2,218,null,{"$f":"(AD235)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH235>0,(AJ235*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK234,NA())","v":0.47172378167191764},null,218,{"$f":"IF(AF235<=$J$9*0.05,AS234*EXP((-$J$6*1)/Heterogenität!$D$4),Z235)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF235>=$J$19, AR234/$J$5<AN235),0, Bodencharakterisierung!$E$8*$J$11*((AR234/$J$5)-AN235))","v":0},0,{"$f":"AQ234-AP235*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ235/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,218,null,{"$f":"(AP235)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF235<=$J$9*1.05,(AV235*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW234,NA())","v":{"$error":"#N/A"}},23072.238162637354,351,5.1991593016719175,0.47172378167191764,0,1.3674355200000003,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},32.43062656012529,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,219,2.3305291073371062E-2,{"$f":"Z236*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF235*Bodencharakterisierung!$E$11/$J$20","v":3.3938238140259187E-5},{"$f":"((150*($J$2^0.87)*(AB236^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z236)*3600*24","v":6.7576318337203928E-2},2.3915996627248484E-4,{"$f":"AE235-AD236*Bodencharakterisierung!$E$8","v":4.9053476449719885E-2},{"$f":"IF(AE236>$J$18,(AE236/(Bodencharakterisierung!$E$11*1000)),0)","v":3.2378532310046127E-5},2.3305291073371062E-2,219,null,{"$f":"(AD236)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH236>0,(AJ236*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK235,NA())","v":0.4738912489272934},null,219,{"$f":"IF(AF236<=$J$9*0.05,AS235*EXP((-$J$6*1)/Heterogenität!$D$4),Z236)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF236>=$J$19, AR235/$J$5<AN236),0, Bodencharakterisierung!$E$8*$J$11*((AR235/$J$5)-AN236))","v":0},0,{"$f":"AQ235-AP236*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ236/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,219,null,{"$f":"(AP236)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF236<=$J$9*1.05,(AV236*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW235,NA())","v":{"$error":"#N/A"}},23072.238162637354,352,5.2075994089272939,0.4738912489272934,0,1.3737081600000003,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},32.378532310046126,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,220,2.3305291073371062E-2,{"$f":"Z237*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF236*Bodencharakterisierung!$E$11/$J$20","v":3.3883722170250189E-5},{"$f":"((150*($J$2^0.87)*(AB237^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z237)*3600*24","v":6.7490549531857097E-2},2.3915996627248484E-4,{"$f":"AE236-AD237*Bodencharakterisierung!$E$8","v":4.8974553660849962E-2},{"$f":"IF(AE237>$J$18,(AE237/(Bodencharakterisierung!$E$11*1000)),0)","v":3.2326438059966971E-5},2.3305291073371062E-2,220,null,{"$f":"(AD237)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH237>0,(AJ237*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK236,NA())","v":0.47605871618266915},null,220,{"$f":"IF(AF237<=$J$9*0.05,AS236*EXP((-$J$6*1)/Heterogenität!$D$4),Z237)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF237>=$J$19, AR236/$J$5<AN237),0, Bodencharakterisierung!$E$8*$J$11*((AR236/$J$5)-AN237))","v":0},0,{"$f":"AQ236-AP237*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ237/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,220,null,{"$f":"(AP237)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF237<=$J$9*1.05,(AV237*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW236,NA())","v":{"$error":"#N/A"}},23072.238162637354,353,5.2160395161826694,0.47605871618266915,0,1.3799808000000002,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},32.326438059966975,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,221,2.3305291073371062E-2,{"$f":"Z238*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF237*Bodencharakterisierung!$E$11/$J$20","v":3.3829206200241199E-5},{"$f":"((150*($J$2^0.87)*(AB238^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z238)*3600*24","v":6.7404751742740826E-2},2.3915996627248484E-4,{"$f":"AE237-AD238*Bodencharakterisierung!$E$8","v":4.8895630871980039E-2},{"$f":"IF(AE238>$J$18,(AE238/(Bodencharakterisierung!$E$11*1000)),0)","v":3.2274343809887816E-5},2.3305291073371062E-2,221,null,{"$f":"(AD238)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH238>0,(AJ238*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK237,NA())","v":0.47822618343804491},null,221,{"$f":"IF(AF238<=$J$9*0.05,AS237*EXP((-$J$6*1)/Heterogenität!$D$4),Z238)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF238>=$J$19, AR237/$J$5<AN238),0, Bodencharakterisierung!$E$8*$J$11*((AR237/$J$5)-AN238))","v":0},0,{"$f":"AQ237-AP238*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ238/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,221,null,{"$f":"(AP238)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF238<=$J$9*1.05,(AV238*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW237,NA())","v":{"$error":"#N/A"}},23072.238162637354,354,5.2244796234380448,0.47822618343804491,0,1.3862534400000002,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},32.274343809887817,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,222,2.3305291073371062E-2,{"$f":"Z239*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF238*Bodencharakterisierung!$E$11/$J$20","v":3.3774690230232208E-5},{"$f":"((150*($J$2^0.87)*(AB239^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z239)*3600*24","v":6.7318924913329511E-2},2.3915996627248484E-4,{"$f":"AE238-AD239*Bodencharakterisierung!$E$8","v":4.8816708083110116E-2},{"$f":"IF(AE239>$J$18,(AE239/(Bodencharakterisierung!$E$11*1000)),0)","v":3.2222249559808661E-5},2.3305291073371062E-2,222,null,{"$f":"(AD239)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH239>0,(AJ239*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK238,NA())","v":0.48039365069342066},null,222,{"$f":"IF(AF239<=$J$9*0.05,AS238*EXP((-$J$6*1)/Heterogenität!$D$4),Z239)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF239>=$J$19, AR238/$J$5<AN239),0, Bodencharakterisierung!$E$8*$J$11*((AR238/$J$5)-AN239))","v":0},0,{"$f":"AQ238-AP239*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ239/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,222,null,{"$f":"(AP239)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF239<=$J$9*1.05,(AV239*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW238,NA())","v":{"$error":"#N/A"}},23072.238162637354,355,5.2329197306934212,0.48039365069342066,0,1.3925260800000001,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},32.22224955980866,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,223,2.3305291073371062E-2,{"$f":"Z240*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF239*Bodencharakterisierung!$E$11/$J$20","v":3.3720174260223217E-5},{"$f":"((150*($J$2^0.87)*(AB240^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z240)*3600*24","v":6.7233068986895878E-2},2.3915996627248484E-4,{"$f":"AE239-AD240*Bodencharakterisierung!$E$8","v":4.8737785294240193E-2},{"$f":"IF(AE240>$J$18,(AE240/(Bodencharakterisierung!$E$11*1000)),0)","v":3.2170155309729499E-5},2.3305291073371062E-2,223,null,{"$f":"(AD240)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH240>0,(AJ240*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK239,NA())","v":0.48256111794879641},null,223,{"$f":"IF(AF240<=$J$9*0.05,AS239*EXP((-$J$6*1)/Heterogenität!$D$4),Z240)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF240>=$J$19, AR239/$J$5<AN240),0, Bodencharakterisierung!$E$8*$J$11*((AR239/$J$5)-AN240))","v":0},0,{"$f":"AQ239-AP240*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ240/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,223,null,{"$f":"(AP240)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF240<=$J$9*1.05,(AV240*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW239,NA())","v":{"$error":"#N/A"}},23072.238162637354,356,5.2413598379487958,0.48256111794879641,0,1.3987987200000001,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},32.170155309729502,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,224,2.3305291073371062E-2,{"$f":"Z241*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF240*Bodencharakterisierung!$E$11/$J$20","v":3.366565829021422E-5},{"$f":"((150*($J$2^0.87)*(AB241^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z241)*3600*24","v":6.7147183906509617E-2},2.3915996627248484E-4,{"$f":"AE240-AD241*Bodencharakterisierung!$E$8","v":4.8658862505370271E-2},{"$f":"IF(AE241>$J$18,(AE241/(Bodencharakterisierung!$E$11*1000)),0)","v":3.2118061059650344E-5},2.3305291073371062E-2,224,null,{"$f":"(AD241)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH241>0,(AJ241*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK240,NA())","v":0.48472858520417217},null,224,{"$f":"IF(AF241<=$J$9*0.05,AS240*EXP((-$J$6*1)/Heterogenität!$D$4),Z241)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF241>=$J$19, AR240/$J$5<AN241),0, Bodencharakterisierung!$E$8*$J$11*((AR240/$J$5)-AN241))","v":0},0,{"$f":"AQ240-AP241*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ241/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,224,null,{"$f":"(AP241)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF241<=$J$9*1.05,(AV241*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW240,NA())","v":{"$error":"#N/A"}},23072.238162637354,357,5.2497999452041721,0.48472858520417217,0,1.40507136,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},32.118061059650344,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,225,2.3305291073371062E-2,{"$f":"Z242*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF241*Bodencharakterisierung!$E$11/$J$20","v":3.3611142320205229E-5},{"$f":"((150*($J$2^0.87)*(AB242^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z242)*3600*24","v":6.706126961503707E-2},2.3915996627248484E-4,{"$f":"AE241-AD242*Bodencharakterisierung!$E$8","v":4.8579939716500348E-2},{"$f":"IF(AE242>$J$18,(AE242/(Bodencharakterisierung!$E$11*1000)),0)","v":3.2065966809571189E-5},2.3305291073371062E-2,225,null,{"$f":"(AD242)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH242>0,(AJ242*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK241,NA())","v":0.48689605245954792},null,225,{"$f":"IF(AF242<=$J$9*0.05,AS241*EXP((-$J$6*1)/Heterogenität!$D$4),Z242)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF242>=$J$19, AR241/$J$5<AN242),0, Bodencharakterisierung!$E$8*$J$11*((AR241/$J$5)-AN242))","v":0},0,{"$f":"AQ241-AP242*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ242/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,225,null,{"$f":"(AP242)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF242<=$J$9*1.05,(AV242*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW241,NA())","v":{"$error":"#N/A"}},23072.238162637354,358,5.2582400524595476,0.48689605245954792,0,1.4113439999999999,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},32.065966809571187,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,226,2.3305291073371062E-2,{"$f":"Z243*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF242*Bodencharakterisierung!$E$11/$J$20","v":3.3556626350196232E-5},{"$f":"((150*($J$2^0.87)*(AB243^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z243)*3600*24","v":6.697532605513927E-2},2.3915996627248484E-4,{"$f":"AE242-AD243*Bodencharakterisierung!$E$8","v":4.8501016927630425E-2},{"$f":"IF(AE243>$J$18,(AE243/(Bodencharakterisierung!$E$11*1000)),0)","v":3.2013872559492027E-5},2.3305291073371062E-2,226,null,{"$f":"(AD243)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH243>0,(AJ243*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK242,NA())","v":0.48906351971492368},null,226,{"$f":"IF(AF243<=$J$9*0.05,AS242*EXP((-$J$6*1)/Heterogenität!$D$4),Z243)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF243>=$J$19, AR242/$J$5<AN243),0, Bodencharakterisierung!$E$8*$J$11*((AR242/$J$5)-AN243))","v":0},0,{"$f":"AQ242-AP243*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ243/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,226,null,{"$f":"(AP243)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF243<=$J$9*1.05,(AV243*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW242,NA())","v":{"$error":"#N/A"}},23072.238162637354,359,5.2666801597149231,0.48906351971492368,0,1.4176166399999999,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},32.013872559492029,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,227,2.3305291073371062E-2,{"$f":"Z244*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF243*Bodencharakterisierung!$E$11/$J$20","v":3.3502110380187235E-5},{"$f":"((150*($J$2^0.87)*(AB244^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z244)*3600*24","v":6.6889353169271901E-2},2.3915996627248484E-4,{"$f":"AE243-AD244*Bodencharakterisierung!$E$8","v":4.8422094138760502E-2},{"$f":"IF(AE244>$J$18,(AE244/(Bodencharakterisierung!$E$11*1000)),0)","v":3.1961778309412871E-5},2.3305291073371062E-2,227,null,{"$f":"(AD244)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH244>0,(AJ244*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK243,NA())","v":0.49123098697029943},null,227,{"$f":"IF(AF244<=$J$9*0.05,AS243*EXP((-$J$6*1)/Heterogenität!$D$4),Z244)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF244>=$J$19, AR243/$J$5<AN244),0, Bodencharakterisierung!$E$8*$J$11*((AR243/$J$5)-AN244))","v":0},0,{"$f":"AQ243-AP244*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ244/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,227,null,{"$f":"(AP244)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF244<=$J$9*1.05,(AV244*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW243,NA())","v":{"$error":"#N/A"}},23072.238162637354,360,5.2751202669702995,0.49123098697029943,0,1.4238892799999998,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},31.961778309412871,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,228,2.3305291073371062E-2,{"$f":"Z245*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF244*Bodencharakterisierung!$E$11/$J$20","v":3.3447594410178244E-5},{"$f":"((150*($J$2^0.87)*(AB245^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z245)*3600*24","v":6.6803350899683145E-2},2.3915996627248484E-4,{"$f":"AE244-AD245*Bodencharakterisierung!$E$8","v":4.8343171349890579E-2},{"$f":"IF(AE245>$J$18,(AE245/(Bodencharakterisierung!$E$11*1000)),0)","v":3.1909684059333716E-5},2.3305291073371062E-2,228,null,{"$f":"(AD245)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH245>0,(AJ245*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK244,NA())","v":0.49339845422567519},null,228,{"$f":"IF(AF245<=$J$9*0.05,AS244*EXP((-$J$6*1)/Heterogenität!$D$4),Z245)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF245>=$J$19, AR244/$J$5<AN245),0, Bodencharakterisierung!$E$8*$J$11*((AR244/$J$5)-AN245))","v":0},0,{"$f":"AQ244-AP245*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ245/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,228,null,{"$f":"(AP245)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF245<=$J$9*1.05,(AV245*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW244,NA())","v":{"$error":"#N/A"}},23072.238162637354,361,5.2835603742256749,0.49339845422567519,0,1.4301619199999998,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},31.909684059333717,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,229,2.3305291073371062E-2,{"$f":"Z246*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF245*Bodencharakterisierung!$E$11/$J$20","v":3.3393078440169254E-5},{"$f":"((150*($J$2^0.87)*(AB246^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z246)*3600*24","v":6.6717319188413504E-2},2.3915996627248484E-4,{"$f":"AE245-AD246*Bodencharakterisierung!$E$8","v":4.8264248561020656E-2},{"$f":"IF(AE246>$J$18,(AE246/(Bodencharakterisierung!$E$11*1000)),0)","v":3.1857589809254561E-5},2.3305291073371062E-2,229,null,{"$f":"(AD246)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH246>0,(AJ246*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK245,NA())","v":0.49556592148105094},null,229,{"$f":"IF(AF246<=$J$9*0.05,AS245*EXP((-$J$6*1)/Heterogenität!$D$4),Z246)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF246>=$J$19, AR245/$J$5<AN246),0, Bodencharakterisierung!$E$8*$J$11*((AR245/$J$5)-AN246))","v":0},0,{"$f":"AQ245-AP246*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ246/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,229,null,{"$f":"(AP246)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF246<=$J$9*1.05,(AV246*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW245,NA())","v":{"$error":"#N/A"}},23072.238162637354,362,5.2920004814810504,0.49556592148105094,0,1.4364345599999997,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},31.857589809254559,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,230,2.3305291073371062E-2,{"$f":"Z247*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF246*Bodencharakterisierung!$E$11/$J$20","v":3.3338562470160263E-5},{"$f":"((150*($J$2^0.87)*(AB247^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z247)*3600*24","v":6.6631257977294037E-2},2.3915996627248484E-4,{"$f":"AE246-AD247*Bodencharakterisierung!$E$8","v":4.8185325772150733E-2},{"$f":"IF(AE247>$J$18,(AE247/(Bodencharakterisierung!$E$11*1000)),0)","v":3.1805495559175399E-5},2.3305291073371062E-2,230,null,{"$f":"(AD247)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH247>0,(AJ247*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK246,NA())","v":0.4977333887364267},null,230,{"$f":"IF(AF247<=$J$9*0.05,AS246*EXP((-$J$6*1)/Heterogenität!$D$4),Z247)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF247>=$J$19, AR246/$J$5<AN247),0, Bodencharakterisierung!$E$8*$J$11*((AR246/$J$5)-AN247))","v":0},0,{"$f":"AQ246-AP247*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ247/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,230,null,{"$f":"(AP247)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF247<=$J$9*1.05,(AV247*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW246,NA())","v":{"$error":"#N/A"}},23072.238162637354,363,5.3004405887364268,0.4977333887364267,0,1.4427071999999996,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},31.805495559175398,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,231,2.3305291073371062E-2,{"$f":"Z248*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF247*Bodencharakterisierung!$E$11/$J$20","v":3.3284046500151266E-5},{"$f":"((150*($J$2^0.87)*(AB248^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z248)*3600*24","v":6.6545167207945885E-2},2.3915996627248484E-4,{"$f":"AE247-AD248*Bodencharakterisierung!$E$8","v":4.810640298328081E-2},{"$f":"IF(AE248>$J$18,(AE248/(Bodencharakterisierung!$E$11*1000)),0)","v":3.1753401309096244E-5},2.3305291073371062E-2,231,null,{"$f":"(AD248)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH248>0,(AJ248*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK247,NA())","v":0.49990085599180245},null,231,{"$f":"IF(AF248<=$J$9*0.05,AS247*EXP((-$J$6*1)/Heterogenität!$D$4),Z248)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF248>=$J$19, AR247/$J$5<AN248),0, Bodencharakterisierung!$E$8*$J$11*((AR247/$J$5)-AN248))","v":0},0,{"$f":"AQ247-AP248*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ248/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,231,null,{"$f":"(AP248)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF248<=$J$9*1.05,(AV248*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW247,NA())","v":{"$error":"#N/A"}},23072.238162637354,364,5.3088806959918013,0.49990085599180245,0,1.4489798399999996,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},31.753401309096244,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,232,2.3305291073371062E-2,{"$f":"Z249*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF248*Bodencharakterisierung!$E$11/$J$20","v":3.3229530530142275E-5},{"$f":"((150*($J$2^0.87)*(AB249^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z249)*3600*24","v":6.6459046821778528E-2},2.3915996627248484E-4,{"$f":"AE248-AD249*Bodencharakterisierung!$E$8","v":4.8027480194410888E-2},{"$f":"IF(AE249>$J$18,(AE249/(Bodencharakterisierung!$E$11*1000)),0)","v":3.1701307059017088E-5},2.3305291073371062E-2,232,null,{"$f":"(AD249)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH249>0,(AJ249*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK248,NA())","v":0.50206832324717821},null,232,{"$f":"IF(AF249<=$J$9*0.05,AS248*EXP((-$J$6*1)/Heterogenität!$D$4),Z249)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF249>=$J$19, AR248/$J$5<AN249),0, Bodencharakterisierung!$E$8*$J$11*((AR248/$J$5)-AN249))","v":0},0,{"$f":"AQ248-AP249*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ249/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,232,null,{"$f":"(AP249)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF249<=$J$9*1.05,(AV249*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW248,NA())","v":{"$error":"#N/A"}},23072.238162637354,365,5.3173208032471777,0.50206832324717821,0,1.4552524799999995,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},31.70130705901709,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,233,2.3305291073371062E-2,{"$f":"Z250*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF249*Bodencharakterisierung!$E$11/$J$20","v":3.3175014560133284E-5},{"$f":"((150*($J$2^0.87)*(AB250^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z250)*3600*24","v":6.6372896759988934E-2},2.3915996627248484E-4,{"$f":"AE249-AD250*Bodencharakterisierung!$E$8","v":4.7948557405540965E-2},{"$f":"IF(AE250>$J$18,(AE250/(Bodencharakterisierung!$E$11*1000)),0)","v":3.1649212808937933E-5},2.3305291073371062E-2,233,null,{"$f":"(AD250)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH250>0,(AJ250*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK249,NA())","v":0.50423579050255396},null,233,{"$f":"IF(AF250<=$J$9*0.05,AS249*EXP((-$J$6*1)/Heterogenität!$D$4),Z250)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF250>=$J$19, AR249/$J$5<AN250),0, Bodencharakterisierung!$E$8*$J$11*((AR249/$J$5)-AN250))","v":0},0,{"$f":"AQ249-AP250*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ250/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,233,null,{"$f":"(AP250)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF250<=$J$9*1.05,(AV250*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW249,NA())","v":{"$error":"#N/A"}},23072.238162637354,366,5.3257609105025532,0.50423579050255396,0,1.4615251199999995,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},31.649212808937932,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,234,2.3305291073371062E-2,{"$f":"Z251*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF250*Bodencharakterisierung!$E$11/$J$20","v":3.3120498590124287E-5},{"$f":"((150*($J$2^0.87)*(AB251^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z251)*3600*24","v":6.6286716963560977E-2},2.3915996627248484E-4,{"$f":"AE250-AD251*Bodencharakterisierung!$E$8","v":4.7869634616671042E-2},{"$f":"IF(AE251>$J$18,(AE251/(Bodencharakterisierung!$E$11*1000)),0)","v":3.1597118558858771E-5},2.3305291073371062E-2,234,null,{"$f":"(AD251)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH251>0,(AJ251*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK250,NA())","v":0.50640325775792971},null,234,{"$f":"IF(AF251<=$J$9*0.05,AS250*EXP((-$J$6*1)/Heterogenität!$D$4),Z251)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF251>=$J$19, AR250/$J$5<AN251),0, Bodencharakterisierung!$E$8*$J$11*((AR250/$J$5)-AN251))","v":0},0,{"$f":"AQ250-AP251*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ251/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,234,null,{"$f":"(AP251)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF251<=$J$9*1.05,(AV251*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW250,NA())","v":{"$error":"#N/A"}},23072.238162637354,367,5.3342010177579287,0.50640325775792971,0,1.4677977599999994,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},31.597118558858771,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,235,2.3305291073371062E-2,{"$f":"Z252*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF251*Bodencharakterisierung!$E$11/$J$20","v":3.306598262011529E-5},{"$f":"((150*($J$2^0.87)*(AB252^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z252)*3600*24","v":6.6200507373263287E-2},2.3915996627248484E-4,{"$f":"AE251-AD252*Bodencharakterisierung!$E$8","v":4.7790711827801119E-2},{"$f":"IF(AE252>$J$18,(AE252/(Bodencharakterisierung!$E$11*1000)),0)","v":3.1545024308779616E-5},2.3305291073371062E-2,235,null,{"$f":"(AD252)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH252>0,(AJ252*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK251,NA())","v":0.50857072501330547},null,235,{"$f":"IF(AF252<=$J$9*0.05,AS251*EXP((-$J$6*1)/Heterogenität!$D$4),Z252)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF252>=$J$19, AR251/$J$5<AN252),0, Bodencharakterisierung!$E$8*$J$11*((AR251/$J$5)-AN252))","v":0},0,{"$f":"AQ251-AP252*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ252/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,235,null,{"$f":"(AP252)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF252<=$J$9*1.05,(AV252*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW251,NA())","v":{"$error":"#N/A"}},23072.238162637354,368,5.342641125013305,0.50857072501330547,0,1.4740703999999993,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},31.545024308779617,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,236,2.3305291073371062E-2,{"$f":"Z253*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF252*Bodencharakterisierung!$E$11/$J$20","v":3.3011466650106306E-5},{"$f":"((150*($J$2^0.87)*(AB253^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z253)*3600*24","v":6.6114267929648862E-2},2.3915996627248484E-4,{"$f":"AE252-AD253*Bodencharakterisierung!$E$8","v":4.7711789038931196E-2},{"$f":"IF(AE253>$J$18,(AE253/(Bodencharakterisierung!$E$11*1000)),0)","v":3.1492930058700461E-5},2.3305291073371062E-2,236,null,{"$f":"(AD253)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH253>0,(AJ253*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK252,NA())","v":0.51073819226868122},null,236,{"$f":"IF(AF253<=$J$9*0.05,AS252*EXP((-$J$6*1)/Heterogenität!$D$4),Z253)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF253>=$J$19, AR252/$J$5<AN253),0, Bodencharakterisierung!$E$8*$J$11*((AR252/$J$5)-AN253))","v":0},0,{"$f":"AQ252-AP253*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ253/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,236,null,{"$f":"(AP253)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF253<=$J$9*1.05,(AV253*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW252,NA())","v":{"$error":"#N/A"}},23072.238162637354,369,5.3510812322686805,0.51073819226868122,0,1.4803430399999993,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},31.492930058700459,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,237,2.3305291073371062E-2,{"$f":"Z254*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF253*Bodencharakterisierung!$E$11/$J$20","v":3.2956950680097308E-5},{"$f":"((150*($J$2^0.87)*(AB254^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z254)*3600*24","v":6.6027998573053803E-2},2.3915996627248484E-4,{"$f":"AE253-AD254*Bodencharakterisierung!$E$8","v":4.7632866250061273E-2},{"$f":"IF(AE254>$J$18,(AE254/(Bodencharakterisierung!$E$11*1000)),0)","v":3.1440835808621305E-5},2.3305291073371062E-2,237,null,{"$f":"(AD254)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH254>0,(AJ254*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK253,NA())","v":0.51290565952405698},null,237,{"$f":"IF(AF254<=$J$9*0.05,AS253*EXP((-$J$6*1)/Heterogenität!$D$4),Z254)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF254>=$J$19, AR253/$J$5<AN254),0, Bodencharakterisierung!$E$8*$J$11*((AR253/$J$5)-AN254))","v":0},0,{"$f":"AQ253-AP254*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ254/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,237,null,{"$f":"(AP254)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF254<=$J$9*1.05,(AV254*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW253,NA())","v":{"$error":"#N/A"}},23072.238162637354,370,5.359521339524056,0.51290565952405698,0,1.4866156799999992,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},31.440835808621305,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,238,2.3305291073371062E-2,{"$f":"Z255*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF254*Bodencharakterisierung!$E$11/$J$20","v":3.2902434710088318E-5},{"$f":"((150*($J$2^0.87)*(AB255^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z255)*3600*24","v":6.5941699243595636E-2},2.3915996627248484E-4,{"$f":"AE254-AD255*Bodencharakterisierung!$E$8","v":4.755394346119135E-2},{"$f":"IF(AE255>$J$18,(AE255/(Bodencharakterisierung!$E$11*1000)),0)","v":3.1388741558542143E-5},2.3305291073371062E-2,238,null,{"$f":"(AD255)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH255>0,(AJ255*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK254,NA())","v":0.51507312677943273},null,238,{"$f":"IF(AF255<=$J$9*0.05,AS254*EXP((-$J$6*1)/Heterogenität!$D$4),Z255)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF255>=$J$19, AR254/$J$5<AN255),0, Bodencharakterisierung!$E$8*$J$11*((AR254/$J$5)-AN255))","v":0},0,{"$f":"AQ254-AP255*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ255/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,238,null,{"$f":"(AP255)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF255<=$J$9*1.05,(AV255*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW254,NA())","v":{"$error":"#N/A"}},23072.238162637354,371,5.3679614467794323,0.51507312677943273,0,1.4928883199999992,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},31.388741558542144,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,239,2.3305291073371062E-2,{"$f":"Z256*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF255*Bodencharakterisierung!$E$11/$J$20","v":3.284791874007932E-5},{"$f":"((150*($J$2^0.87)*(AB256^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z256)*3600*24","v":6.5855369881173048E-2},2.3915996627248484E-4,{"$f":"AE255-AD256*Bodencharakterisierung!$E$8","v":4.7475020672321427E-2},{"$f":"IF(AE256>$J$18,(AE256/(Bodencharakterisierung!$E$11*1000)),0)","v":3.1336647308462988E-5},2.3305291073371062E-2,239,null,{"$f":"(AD256)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH256>0,(AJ256*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK255,NA())","v":0.51724059403480849},null,239,{"$f":"IF(AF256<=$J$9*0.05,AS255*EXP((-$J$6*1)/Heterogenität!$D$4),Z256)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF256>=$J$19, AR255/$J$5<AN256),0, Bodencharakterisierung!$E$8*$J$11*((AR255/$J$5)-AN256))","v":0},0,{"$f":"AQ255-AP256*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ256/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,239,null,{"$f":"(AP256)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF256<=$J$9*1.05,(AV256*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW255,NA())","v":{"$error":"#N/A"}},23072.238162637354,372,5.3764015540348069,0.51724059403480849,0,1.4991609599999991,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},31.33664730846299,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,240,2.3305291073371062E-2,{"$f":"Z257*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF256*Bodencharakterisierung!$E$11/$J$20","v":3.279340277007033E-5},{"$f":"((150*($J$2^0.87)*(AB257^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z257)*3600*24","v":6.5769010425464125E-2},2.3915996627248484E-4,{"$f":"AE256-AD257*Bodencharakterisierung!$E$8","v":4.7396097883451505E-2},{"$f":"IF(AE257>$J$18,(AE257/(Bodencharakterisierung!$E$11*1000)),0)","v":3.1284553058383833E-5},2.3305291073371062E-2,240,null,{"$f":"(AD257)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH257>0,(AJ257*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK256,NA())","v":0.51940806129018424},null,240,{"$f":"IF(AF257<=$J$9*0.05,AS256*EXP((-$J$6*1)/Heterogenität!$D$4),Z257)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF257>=$J$19, AR256/$J$5<AN257),0, Bodencharakterisierung!$E$8*$J$11*((AR256/$J$5)-AN257))","v":0},0,{"$f":"AQ256-AP257*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ257/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,240,null,{"$f":"(AP257)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF257<=$J$9*1.05,(AV257*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW256,NA())","v":{"$error":"#N/A"}},23072.238162637354,373,5.3848416612901833,0.51940806129018424,0,1.505433599999999,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},31.284553058383832,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,241,2.3305291073371062E-2,{"$f":"Z258*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF257*Bodencharakterisierung!$E$11/$J$20","v":3.2738886800061339E-5},{"$f":"((150*($J$2^0.87)*(AB258^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z258)*3600*24","v":6.568262081592513E-2},2.3915996627248484E-4,{"$f":"AE257-AD258*Bodencharakterisierung!$E$8","v":4.7317175094581582E-2},{"$f":"IF(AE258>$J$18,(AE258/(Bodencharakterisierung!$E$11*1000)),0)","v":3.1232458808304671E-5},2.3305291073371062E-2,241,null,{"$f":"(AD258)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH258>0,(AJ258*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK257,NA())","v":0.52157552854556},null,241,{"$f":"IF(AF258<=$J$9*0.05,AS257*EXP((-$J$6*1)/Heterogenität!$D$4),Z258)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF258>=$J$19, AR257/$J$5<AN258),0, Bodencharakterisierung!$E$8*$J$11*((AR257/$J$5)-AN258))","v":0},0,{"$f":"AQ257-AP258*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ258/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,241,null,{"$f":"(AP258)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF258<=$J$9*1.05,(AV258*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW257,NA())","v":{"$error":"#N/A"}},23072.238162637354,374,5.3932817685455587,0.52157552854556,0,1.511706239999999,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},31.232458808304671,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,242,2.3305291073371062E-2,{"$f":"Z259*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF258*Bodencharakterisierung!$E$11/$J$20","v":3.2684370830052342E-5},{"$f":"((150*($J$2^0.87)*(AB259^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z259)*3600*24","v":6.5596200991789602E-2},2.3915996627248484E-4,{"$f":"AE258-AD259*Bodencharakterisierung!$E$8","v":4.7238252305711659E-2},{"$f":"IF(AE259>$J$18,(AE259/(Bodencharakterisierung!$E$11*1000)),0)","v":3.1180364558225516E-5},2.3305291073371062E-2,242,null,{"$f":"(AD259)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH259>0,(AJ259*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK258,NA())","v":0.52374299580093575},null,242,{"$f":"IF(AF259<=$J$9*0.05,AS258*EXP((-$J$6*1)/Heterogenität!$D$4),Z259)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF259>=$J$19, AR258/$J$5<AN259),0, Bodencharakterisierung!$E$8*$J$11*((AR258/$J$5)-AN259))","v":0},0,{"$f":"AQ258-AP259*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ259/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,242,null,{"$f":"(AP259)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF259<=$J$9*1.05,(AV259*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW258,NA())","v":{"$error":"#N/A"}},23072.238162637354,375,5.4017218758009342,0.52374299580093575,0,1.5179788799999989,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},31.180364558225516,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243,2.3305291073371062E-2,{"$f":"Z260*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF259*Bodencharakterisierung!$E$11/$J$20","v":3.2629854860043351E-5},{"$f":"((150*($J$2^0.87)*(AB260^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z260)*3600*24","v":6.5509750892067037E-2},2.3915996627248484E-4,{"$f":"AE259-AD260*Bodencharakterisierung!$E$8","v":4.7159329516841736E-2},{"$f":"IF(AE260>$J$18,(AE260/(Bodencharakterisierung!$E$11*1000)),0)","v":3.1128270308146361E-5},2.3305291073371062E-2,243,null,{"$f":"(AD260)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH260>0,(AJ260*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK259,NA())","v":0.52591046305631151},null,243,{"$f":"IF(AF260<=$J$9*0.05,AS259*EXP((-$J$6*1)/Heterogenität!$D$4),Z260)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF260>=$J$19, AR259/$J$5<AN260),0, Bodencharakterisierung!$E$8*$J$11*((AR259/$J$5)-AN260))","v":0},0,{"$f":"AQ259-AP260*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ260/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,243,null,{"$f":"(AP260)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF260<=$J$9*1.05,(AV260*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW259,NA())","v":{"$error":"#N/A"}},23072.238162637354,376,5.4101619830563106,0.52591046305631151,0,1.5242515199999989,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},31.128270308146362,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,244,2.3305291073371062E-2,{"$f":"Z261*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF260*Bodencharakterisierung!$E$11/$J$20","v":3.2575338890034354E-5},{"$f":"((150*($J$2^0.87)*(AB261^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z261)*3600*24","v":6.5423270455541832E-2},2.3915996627248484E-4,{"$f":"AE260-AD261*Bodencharakterisierung!$E$8","v":4.7080406727971813E-2},{"$f":"IF(AE261>$J$18,(AE261/(Bodencharakterisierung!$E$11*1000)),0)","v":3.1076176058067205E-5},2.3305291073371062E-2,244,null,{"$f":"(AD261)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH261>0,(AJ261*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK260,NA())","v":0.52807793031168726},null,244,{"$f":"IF(AF261<=$J$9*0.05,AS260*EXP((-$J$6*1)/Heterogenität!$D$4),Z261)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF261>=$J$19, AR260/$J$5<AN261),0, Bodencharakterisierung!$E$8*$J$11*((AR260/$J$5)-AN261))","v":0},0,{"$f":"AQ260-AP261*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ261/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,244,null,{"$f":"(AP261)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF261<=$J$9*1.05,(AV261*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW260,NA())","v":{"$error":"#N/A"}},23072.238162637354,377,5.418602090311686,0.52807793031168726,0,1.5305241599999988,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},31.076176058067205,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,245,2.3305291073371062E-2,{"$f":"Z262*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF261*Bodencharakterisierung!$E$11/$J$20","v":3.252082292002537E-5},{"$f":"((150*($J$2^0.87)*(AB262^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z262)*3600*24","v":6.5336759620771512E-2},2.3915996627248484E-4,{"$f":"AE261-AD262*Bodencharakterisierung!$E$8","v":4.700148393910189E-2},{"$f":"IF(AE262>$J$18,(AE262/(Bodencharakterisierung!$E$11*1000)),0)","v":3.1024081807988043E-5},2.3305291073371062E-2,245,null,{"$f":"(AD262)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH262>0,(AJ262*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK261,NA())","v":0.53024539756706301},null,245,{"$f":"IF(AF262<=$J$9*0.05,AS261*EXP((-$J$6*1)/Heterogenität!$D$4),Z262)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF262>=$J$19, AR261/$J$5<AN262),0, Bodencharakterisierung!$E$8*$J$11*((AR261/$J$5)-AN262))","v":0},0,{"$f":"AQ261-AP262*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ262/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,245,null,{"$f":"(AP262)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF262<=$J$9*1.05,(AV262*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW261,NA())","v":{"$error":"#N/A"}},23072.238162637354,378,5.4270421975670615,0.53024539756706301,0,1.5367967999999987,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},31.024081807988043,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,246,2.3305291073371062E-2,{"$f":"Z263*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF262*Bodencharakterisierung!$E$11/$J$20","v":3.2466306950016373E-5},{"$f":"((150*($J$2^0.87)*(AB263^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z263)*3600*24","v":6.5250218326086379E-2},2.3915996627248484E-4,{"$f":"AE262-AD263*Bodencharakterisierung!$E$8","v":4.6922561150231967E-2},{"$f":"IF(AE263>$J$18,(AE263/(Bodencharakterisierung!$E$11*1000)),0)","v":3.0971987557908888E-5},2.3305291073371062E-2,246,null,{"$f":"(AD263)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH263>0,(AJ263*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK262,NA())","v":0.53241286482243877},null,246,{"$f":"IF(AF263<=$J$9*0.05,AS262*EXP((-$J$6*1)/Heterogenität!$D$4),Z263)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF263>=$J$19, AR262/$J$5<AN263),0, Bodencharakterisierung!$E$8*$J$11*((AR262/$J$5)-AN263))","v":0},0,{"$f":"AQ262-AP263*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ263/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,246,null,{"$f":"(AP263)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF263<=$J$9*1.05,(AV263*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW262,NA())","v":{"$error":"#N/A"}},23072.238162637354,379,5.4354823048224379,0.53241286482243877,0,1.5430694399999987,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},30.971987557908889,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,247,2.3305291073371062E-2,{"$f":"Z264*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF263*Bodencharakterisierung!$E$11/$J$20","v":3.2411790980007375E-5},{"$f":"((150*($J$2^0.87)*(AB264^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z264)*3600*24","v":6.516364650958778E-2},2.3915996627248484E-4,{"$f":"AE263-AD264*Bodencharakterisierung!$E$8","v":4.6843638361362044E-2},{"$f":"IF(AE264>$J$18,(AE264/(Bodencharakterisierung!$E$11*1000)),0)","v":3.0919893307829733E-5},2.3305291073371062E-2,247,null,{"$f":"(AD264)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH264>0,(AJ264*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK263,NA())","v":0.53458033207781452},null,247,{"$f":"IF(AF264<=$J$9*0.05,AS263*EXP((-$J$6*1)/Heterogenität!$D$4),Z264)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF264>=$J$19, AR263/$J$5<AN264),0, Bodencharakterisierung!$E$8*$J$11*((AR263/$J$5)-AN264))","v":0},0,{"$f":"AQ263-AP264*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ264/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,247,null,{"$f":"(AP264)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF264<=$J$9*1.05,(AV264*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW263,NA())","v":{"$error":"#N/A"}},23072.238162637354,380,5.4439224120778125,0.53458033207781452,0,1.5493420799999986,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},30.919893307829732,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,248,2.3305291073371062E-2,{"$f":"Z265*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF264*Bodencharakterisierung!$E$11/$J$20","v":3.2357275009998385E-5},{"$f":"((150*($J$2^0.87)*(AB265^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z265)*3600*24","v":6.5077044109146678E-2},2.3915996627248484E-4,{"$f":"AE264-AD265*Bodencharakterisierung!$E$8","v":4.6764715572492122E-2},{"$f":"IF(AE265>$J$18,(AE265/(Bodencharakterisierung!$E$11*1000)),0)","v":3.0867799057750578E-5},2.3305291073371062E-2,248,null,{"$f":"(AD265)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH265>0,(AJ265*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK264,NA())","v":0.53674779933319028},null,248,{"$f":"IF(AF265<=$J$9*0.05,AS264*EXP((-$J$6*1)/Heterogenität!$D$4),Z265)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF265>=$J$19, AR264/$J$5<AN265),0, Bodencharakterisierung!$E$8*$J$11*((AR264/$J$5)-AN265))","v":0},0,{"$f":"AQ264-AP265*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ265/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,248,null,{"$f":"(AP265)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF265<=$J$9*1.05,(AV265*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW264,NA())","v":{"$error":"#N/A"}},23072.238162637354,381,5.4523625193331888,0.53674779933319028,0,1.5556147199999986,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},30.867799057750577,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,249,2.3305291073371062E-2,{"$f":"Z266*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF265*Bodencharakterisierung!$E$11/$J$20","v":3.2302759039989394E-5},{"$f":"((150*($J$2^0.87)*(AB266^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z266)*3600*24","v":6.4990411062402942E-2},2.3915996627248484E-4,{"$f":"AE265-AD266*Bodencharakterisierung!$E$8","v":4.6685792783622199E-2},{"$f":"IF(AE266>$J$18,(AE266/(Bodencharakterisierung!$E$11*1000)),0)","v":3.0815704807671416E-5},2.3305291073371062E-2,249,null,{"$f":"(AD266)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH266>0,(AJ266*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK265,NA())","v":0.53891526658856603},null,249,{"$f":"IF(AF266<=$J$9*0.05,AS265*EXP((-$J$6*1)/Heterogenität!$D$4),Z266)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF266>=$J$19, AR265/$J$5<AN266),0, Bodencharakterisierung!$E$8*$J$11*((AR265/$J$5)-AN266))","v":0},0,{"$f":"AQ265-AP266*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ266/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,249,null,{"$f":"(AP266)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF266<=$J$9*1.05,(AV266*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW265,NA())","v":{"$error":"#N/A"}},23072.238162637354,382,5.4608026265885643,0.53891526658856603,0,1.5618873599999985,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},30.815704807671416,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250,2.3305291073371062E-2,{"$f":"Z267*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF266*Bodencharakterisierung!$E$11/$J$20","v":3.2248243069980397E-5},{"$f":"((150*($J$2^0.87)*(AB267^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z267)*3600*24","v":6.4903747306763598E-2},2.3915996627248484E-4,{"$f":"AE266-AD267*Bodencharakterisierung!$E$8","v":4.6606869994752276E-2},{"$f":"IF(AE267>$J$18,(AE267/(Bodencharakterisierung!$E$11*1000)),0)","v":3.076361055759226E-5},2.3305291073371062E-2,250,null,{"$f":"(AD267)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH267>0,(AJ267*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK266,NA())","v":0.54108273384394179},null,250,{"$f":"IF(AF267<=$J$9*0.05,AS266*EXP((-$J$6*1)/Heterogenität!$D$4),Z267)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF267>=$J$19, AR266/$J$5<AN267),0, Bodencharakterisierung!$E$8*$J$11*((AR266/$J$5)-AN267))","v":0},0,{"$f":"AQ266-AP267*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ267/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,250,null,{"$f":"(AP267)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF267<=$J$9*1.05,(AV267*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW266,NA())","v":{"$error":"#N/A"}},23072.238162637354,383,5.4692427338439398,0.54108273384394179,0,1.5681599999999984,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},30.763610557592262,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,251,2.3305291073371062E-2,{"$f":"Z268*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF267*Bodencharakterisierung!$E$11/$J$20","v":3.2193727099971406E-5},{"$f":"((150*($J$2^0.87)*(AB268^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z268)*3600*24","v":6.4817052779401807E-2},2.3915996627248484E-4,{"$f":"AE267-AD268*Bodencharakterisierung!$E$8","v":4.6527947205882353E-2},{"$f":"IF(AE268>$J$18,(AE268/(Bodencharakterisierung!$E$11*1000)),0)","v":3.0711516307513105E-5},2.3305291073371062E-2,251,null,{"$f":"(AD268)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH268>0,(AJ268*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK267,NA())","v":0.54325020109931754},null,251,{"$f":"IF(AF268<=$J$9*0.05,AS267*EXP((-$J$6*1)/Heterogenität!$D$4),Z268)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF268>=$J$19, AR267/$J$5<AN268),0, Bodencharakterisierung!$E$8*$J$11*((AR267/$J$5)-AN268))","v":0},0,{"$f":"AQ267-AP268*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ268/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,251,null,{"$f":"(AP268)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF268<=$J$9*1.05,(AV268*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW267,NA())","v":{"$error":"#N/A"}},23072.238162637354,384,5.4776828410993161,0.54325020109931754,0,1.5744326399999984,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},30.711516307513104,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,252,2.3305291073371062E-2,{"$f":"Z269*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF268*Bodencharakterisierung!$E$11/$J$20","v":3.2139211129962409E-5},{"$f":"((150*($J$2^0.87)*(AB269^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z269)*3600*24","v":6.4730327417255845E-2},2.3915996627248484E-4,{"$f":"AE268-AD269*Bodencharakterisierung!$E$8","v":4.644902441701243E-2},{"$f":"IF(AE269>$J$18,(AE269/(Bodencharakterisierung!$E$11*1000)),0)","v":3.065942205743395E-5},2.3305291073371062E-2,252,null,{"$f":"(AD269)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH269>0,(AJ269*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK268,NA())","v":0.5454176683546933},null,252,{"$f":"IF(AF269<=$J$9*0.05,AS268*EXP((-$J$6*1)/Heterogenität!$D$4),Z269)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF269>=$J$19, AR268/$J$5<AN269),0, Bodencharakterisierung!$E$8*$J$11*((AR268/$J$5)-AN269))","v":0},0,{"$f":"AQ268-AP269*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ269/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,252,null,{"$f":"(AP269)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF269<=$J$9*1.05,(AV269*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW268,NA())","v":{"$error":"#N/A"}},23072.238162637354,385,5.4861229483546916,0.5454176683546933,0,1.5807052799999983,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},30.65942205743395,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,253,2.3305291073371062E-2,{"$f":"Z270*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF269*Bodencharakterisierung!$E$11/$J$20","v":3.2084695159953425E-5},{"$f":"((150*($J$2^0.87)*(AB270^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z270)*3600*24","v":6.4643571157027124E-2},2.3915996627248484E-4,{"$f":"AE269-AD270*Bodencharakterisierung!$E$8","v":4.6370101628142507E-2},{"$f":"IF(AE270>$J$18,(AE270/(Bodencharakterisierung!$E$11*1000)),0)","v":3.0607327807354788E-5},2.3305291073371062E-2,253,null,{"$f":"(AD270)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH270>0,(AJ270*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK269,NA())","v":0.54758513561006905},null,253,{"$f":"IF(AF270<=$J$9*0.05,AS269*EXP((-$J$6*1)/Heterogenität!$D$4),Z270)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF270>=$J$19, AR269/$J$5<AN270),0, Bodencharakterisierung!$E$8*$J$11*((AR269/$J$5)-AN270))","v":0},0,{"$f":"AQ269-AP270*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ270/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,253,null,{"$f":"(AP270)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF270<=$J$9*1.05,(AV270*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW269,NA())","v":{"$error":"#N/A"}},23072.238162637354,386,5.4945630556100671,0.54758513561006905,0,1.5869779199999983,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},30.607327807354789,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,254,2.3305291073371062E-2,{"$f":"Z271*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF270*Bodencharakterisierung!$E$11/$J$20","v":3.2030179189944421E-5},{"$f":"((150*($J$2^0.87)*(AB271^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z271)*3600*24","v":6.4556783935179635E-2},2.3915996627248484E-4,{"$f":"AE270-AD271*Bodencharakterisierung!$E$8","v":4.6291178839272584E-2},{"$f":"IF(AE271>$J$18,(AE271/(Bodencharakterisierung!$E$11*1000)),0)","v":3.0555233557275633E-5},2.3305291073371062E-2,254,null,{"$f":"(AD271)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH271>0,(AJ271*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK270,NA())","v":0.54975260286544481},null,254,{"$f":"IF(AF271<=$J$9*0.05,AS270*EXP((-$J$6*1)/Heterogenität!$D$4),Z271)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF271>=$J$19, AR270/$J$5<AN271),0, Bodencharakterisierung!$E$8*$J$11*((AR270/$J$5)-AN271))","v":0},0,{"$f":"AQ270-AP271*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ271/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,254,null,{"$f":"(AP271)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF271<=$J$9*1.05,(AV271*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW270,NA())","v":{"$error":"#N/A"}},23072.238162637354,387,5.5030031628654434,0.54975260286544481,0,1.5932505599999982,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},30.555233557275631,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,255,2.3305291073371062E-2,{"$f":"Z272*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF271*Bodencharakterisierung!$E$11/$J$20","v":3.197566321993543E-5},{"$f":"((150*($J$2^0.87)*(AB272^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z272)*3600*24","v":6.4469965687938197E-2},2.3915996627248484E-4,{"$f":"AE271-AD272*Bodencharakterisierung!$E$8","v":4.6212256050402661E-2},{"$f":"IF(AE272>$J$18,(AE272/(Bodencharakterisierung!$E$11*1000)),0)","v":3.0503139307196478E-5},2.3305291073371062E-2,255,null,{"$f":"(AD272)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH272>0,(AJ272*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK271,NA())","v":0.55192007012082056},null,255,{"$f":"IF(AF272<=$J$9*0.05,AS271*EXP((-$J$6*1)/Heterogenität!$D$4),Z272)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF272>=$J$19, AR271/$J$5<AN272),0, Bodencharakterisierung!$E$8*$J$11*((AR271/$J$5)-AN272))","v":0},0,{"$f":"AQ271-AP272*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ272/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,255,null,{"$f":"(AP272)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF272<=$J$9*1.05,(AV272*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW271,NA())","v":{"$error":"#N/A"}},23072.238162637354,388,5.511443270120818,0.55192007012082056,0,1.5995231999999981,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},30.503139307196477,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,256,2.3305291073371062E-2,{"$f":"Z273*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF272*Bodencharakterisierung!$E$11/$J$20","v":3.192114724992644E-5},{"$f":"((150*($J$2^0.87)*(AB273^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z273)*3600*24","v":6.4383116351287351E-2},2.3915996627248484E-4,{"$f":"AE272-AD273*Bodencharakterisierung!$E$8","v":4.6133333261532739E-2},{"$f":"IF(AE273>$J$18,(AE273/(Bodencharakterisierung!$E$11*1000)),0)","v":3.0451045057117319E-5},2.3305291073371062E-2,256,null,{"$f":"(AD273)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH273>0,(AJ273*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK272,NA())","v":0.55408753737619632},null,256,{"$f":"IF(AF273<=$J$9*0.05,AS272*EXP((-$J$6*1)/Heterogenität!$D$4),Z273)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF273>=$J$19, AR272/$J$5<AN273),0, Bodencharakterisierung!$E$8*$J$11*((AR272/$J$5)-AN273))","v":0},0,{"$f":"AQ272-AP273*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ273/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,256,null,{"$f":"(AP273)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF273<=$J$9*1.05,(AV273*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW272,NA())","v":{"$error":"#N/A"}},23072.238162637354,389,5.5198833773761944,0.55408753737619632,0,1.6057958399999981,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},30.451045057117319,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,257,2.3305291073371062E-2,{"$f":"Z274*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF273*Bodencharakterisierung!$E$11/$J$20","v":3.1866631279917449E-5},{"$f":"((150*($J$2^0.87)*(AB274^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z274)*3600*24","v":6.429623586097008E-2},2.3915996627248484E-4,{"$f":"AE273-AD274*Bodencharakterisierung!$E$8","v":4.6054410472662816E-2},{"$f":"IF(AE274>$J$18,(AE274/(Bodencharakterisierung!$E$11*1000)),0)","v":3.0398950807038164E-5},2.3305291073371062E-2,257,null,{"$f":"(AD274)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH274>0,(AJ274*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK273,NA())","v":0.55625500463157207},null,257,{"$f":"IF(AF274<=$J$9*0.05,AS273*EXP((-$J$6*1)/Heterogenität!$D$4),Z274)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF274>=$J$19, AR273/$J$5<AN274),0, Bodencharakterisierung!$E$8*$J$11*((AR273/$J$5)-AN274))","v":0},0,{"$f":"AQ273-AP274*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ274/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,257,null,{"$f":"(AP274)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF274<=$J$9*1.05,(AV274*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW273,NA())","v":{"$error":"#N/A"}},23072.238162637354,390,5.5283234846315699,0.55625500463157207,0,1.612068479999998,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},30.398950807038165,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,258,2.3305291073371062E-2,{"$f":"Z275*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF274*Bodencharakterisierung!$E$11/$J$20","v":3.1812115309908452E-5},{"$f":"((150*($J$2^0.87)*(AB275^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z275)*3600*24","v":6.4209324152485953E-2},2.3915996627248484E-4,{"$f":"AE274-AD275*Bodencharakterisierung!$E$8","v":4.5975487683792893E-2},{"$f":"IF(AE275>$J$18,(AE275/(Bodencharakterisierung!$E$11*1000)),0)","v":3.0346856556959005E-5},2.3305291073371062E-2,258,null,{"$f":"(AD275)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH275>0,(AJ275*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK274,NA())","v":0.55842247188694782},null,258,{"$f":"IF(AF275<=$J$9*0.05,AS274*EXP((-$J$6*1)/Heterogenität!$D$4),Z275)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF275>=$J$19, AR274/$J$5<AN275),0, Bodencharakterisierung!$E$8*$J$11*((AR274/$J$5)-AN275))","v":0},0,{"$f":"AQ274-AP275*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ275/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,258,null,{"$f":"(AP275)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF275<=$J$9*1.05,(AV275*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW274,NA())","v":{"$error":"#N/A"}},23072.238162637354,391,5.5367635918869453,0.55842247188694782,0,1.618341119999998,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},30.346856556959004,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,259,2.3305291073371062E-2,{"$f":"Z276*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF275*Bodencharakterisierung!$E$11/$J$20","v":3.1757599339899461E-5},{"$f":"((150*($J$2^0.87)*(AB276^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z276)*3600*24","v":6.4122381161090758E-2},2.3915996627248484E-4,{"$f":"AE275-AD276*Bodencharakterisierung!$E$8","v":4.589656489492297E-2},{"$f":"IF(AE276>$J$18,(AE276/(Bodencharakterisierung!$E$11*1000)),0)","v":3.0294762306879846E-5},2.3305291073371062E-2,259,null,{"$f":"(AD276)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH276>0,(AJ276*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK275,NA())","v":0.56058993914232358},null,259,{"$f":"IF(AF276<=$J$9*0.05,AS275*EXP((-$J$6*1)/Heterogenität!$D$4),Z276)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF276>=$J$19, AR275/$J$5<AN276),0, Bodencharakterisierung!$E$8*$J$11*((AR275/$J$5)-AN276))","v":0},0,{"$f":"AQ275-AP276*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ276/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,259,null,{"$f":"(AP276)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF276<=$J$9*1.05,(AV276*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW275,NA())","v":{"$error":"#N/A"}},23072.238162637354,392,5.5452036991423217,0.56058993914232358,0,{"$f":"$G$34/$G$12/$G$8+BC275","v":1.6246137599999979},null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},30.294762306879846,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,260,2.3305291073371062E-2,{"$f":"Z277*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF276*Bodencharakterisierung!$E$11/$J$20","v":3.1703083369890464E-5},{"$f":"((150*($J$2^0.87)*(AB277^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z277)*3600*24","v":6.4035406821794302E-2},2.3915996627248484E-4,{"$f":"AE276-AD277*Bodencharakterisierung!$E$8","v":4.5817642106053047E-2},{"$f":"IF(AE277>$J$18,(AE277/(Bodencharakterisierung!$E$11*1000)),0)","v":3.0242668056800691E-5},2.3305291073371062E-2,260,null,{"$f":"(AD277)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH277>0,(AJ277*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK276,NA())","v":0.56275740639769933},null,260,{"$f":"IF(AF277<=$J$9*0.05,AS276*EXP((-$J$6*1)/Heterogenität!$D$4),Z277)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF277>=$J$19, AR276/$J$5<AN277),0, Bodencharakterisierung!$E$8*$J$11*((AR276/$J$5)-AN277))","v":0},0,{"$f":"AQ276-AP277*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ277/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,260,null,{"$f":"(AP277)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF277<=$J$9*1.05,(AV277*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW276,NA())","v":{"$error":"#N/A"}},23072.238162637354,393,5.5536438063976972,0.56275740639769933,0,1.6308863999999978,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},30.242668056800692,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,261,2.3305291073371062E-2,{"$f":"Z278*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF277*Bodencharakterisierung!$E$11/$J$20","v":3.1648567399881473E-5},{"$f":"((150*($J$2^0.87)*(AB278^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z278)*3600*24","v":6.3948401069359548E-2},2.3915996627248484E-4,{"$f":"AE277-AD278*Bodencharakterisierung!$E$8","v":4.5738719317183124E-2},{"$f":"IF(AE278>$J$18,(AE278/(Bodencharakterisierung!$E$11*1000)),0)","v":3.0190573806721533E-5},2.3305291073371062E-2,261,null,{"$f":"(AD278)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH278>0,(AJ278*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK277,NA())","v":0.56492487365307509},null,261,{"$f":"IF(AF278<=$J$9*0.05,AS277*EXP((-$J$6*1)/Heterogenität!$D$4),Z278)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF278>=$J$19, AR277/$J$5<AN278),0, Bodencharakterisierung!$E$8*$J$11*((AR277/$J$5)-AN278))","v":0},0,{"$f":"AQ277-AP278*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ278/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,261,null,{"$f":"(AP278)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF278<=$J$9*1.05,(AV278*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW277,NA())","v":{"$error":"#N/A"}},23072.238162637354,394,5.5620839136530726,0.56492487365307509,0,1.6371590399999978,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},30.190573806721531,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,262,{"$f":"AG278","v":2.3305291073371062E-2},{"$f":"Z279*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF278*Bodencharakterisierung!$E$11/$J$20","v":3.1594051429872476E-5},{"$f":"((150*($J$2^0.87)*(AB279^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z279)*3600*24","v":6.3861363838300711E-2},{"$f":"MIN(AC279,Z279-AA279)","v":2.3915996627248484E-4},{"$f":"AE278-AD279*Bodencharakterisierung!$E$8","v":4.5659796528313201E-2},{"$f":"IF(AE279>$J$18,(AE279/(Bodencharakterisierung!$E$11*1000)),0)","v":3.0138479556642377E-5},{"$f":"AA279+AD279","v":2.3305291073371062E-2},{"$f":"IF(AD279>0,Y279,NA())","v":262},null,{"$f":"(AD279)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH279>0,(AJ279*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK278,NA())","v":0.56709234090845084},null,262,{"$f":"IF(AF279<=$J$9*0.05,AS278*EXP((-$J$6*1)/Heterogenität!$D$4),Z279)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF279>=$J$19, AR278/$J$5<AN279),0, Bodencharakterisierung!$E$8*$J$11*((AR278/$J$5)-AN279))","v":0},{"$f":"MIN(AO279,AS278-AN279)","v":0},{"$f":"AQ278-AP279*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ279/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},{"$f":"AN279+AP279","v":2.3305291073371062E-2},{"$f":"IF(AN279>$G$5,AM279,NA())","v":262},null,{"$f":"(AP279)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF279<=$J$9*1.05,(AV279*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW278,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH279>($G$5*10^6),BH279*0.99,9999)","v":23072.238162637354},{"$f":"AT279+$G$3","v":395},{"$f":"IF(ISNUMBER(AT279),BA279+BB279+BC279+$AZ$17,\"\")","v":5.570524020908449},{"$f":"IF(ISNUMBER(AK279),AK279,BA278)","v":0.56709234090845084},{"$f":"IF(ISNUMBER(AW279),AW279,0)","v":0},1.6434316799999977,null,{"$f":"AR279*10^6","v":4.3827000000643475},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF279*10^6","v":30.138479556642377},{"$f":"AN279*10^6","v":23305.291073371063}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,263,2.3305291073371062E-2,{"$f":"Z280*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF279*Bodencharakterisierung!$E$11/$J$20","v":3.1539535459863492E-5},{"$f":"((150*($J$2^0.87)*(AB280^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z280)*3600*24","v":6.3774295062882791E-2},2.3915996627248484E-4,{"$f":"AE279-AD280*Bodencharakterisierung!$E$8","v":4.5580873739443278E-2},{"$f":"IF(AE280>$J$18,(AE280/(Bodencharakterisierung!$E$11*1000)),0)","v":3.0086385306563219E-5},2.3305291073371062E-2,263,null,{"$f":"(AD280)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH280>0,(AJ280*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK279,NA())","v":0.5692598081638266},null,263,{"$f":"IF(AF280<=$J$9*0.05,AS279*EXP((-$J$6*1)/Heterogenität!$D$4),Z280)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF280>=$J$19, AR279/$J$5<AN280),0, Bodencharakterisierung!$E$8*$J$11*((AR279/$J$5)-AN280))","v":0},0,{"$f":"AQ279-AP280*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ280/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,263,null,{"$f":"(AP280)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF280<=$J$9*1.05,(AV280*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW279,NA())","v":{"$error":"#N/A"}},23072.238162637354,396,5.5789641281638236,0.5692598081638266,0,1.6497043199999977,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},30.086385306563219,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,264,2.3305291073371062E-2,{"$f":"Z281*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF280*Bodencharakterisierung!$E$11/$J$20","v":3.1485019489854494E-5},{"$f":"((150*($J$2^0.87)*(AB281^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z281)*3600*24","v":6.368719467711928E-2},2.3915996627248484E-4,{"$f":"AE280-AD281*Bodencharakterisierung!$E$8","v":4.5501950950573355E-2},{"$f":"IF(AE281>$J$18,(AE281/(Bodencharakterisierung!$E$11*1000)),0)","v":3.0034291056484064E-5},2.3305291073371062E-2,264,null,{"$f":"(AD281)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH281>0,(AJ281*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK280,NA())","v":0.57142727541920235},null,264,{"$f":"IF(AF281<=$J$9*0.05,AS280*EXP((-$J$6*1)/Heterogenität!$D$4),Z281)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF281>=$J$19, AR280/$J$5<AN281),0, Bodencharakterisierung!$E$8*$J$11*((AR280/$J$5)-AN281))","v":0},0,{"$f":"AQ280-AP281*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ281/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,264,null,{"$f":"(AP281)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF281<=$J$9*1.05,(AV281*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW280,NA())","v":{"$error":"#N/A"}},23072.238162637354,397,5.5874042354191999,0.57142727541920235,0,1.6559769599999976,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},30.034291056484065,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,265,2.3305291073371062E-2,{"$f":"Z282*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF281*Bodencharakterisierung!$E$11/$J$20","v":3.1430503519845504E-5},{"$f":"((150*($J$2^0.87)*(AB282^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z282)*3600*24","v":6.3600062614770969E-2},2.3915996627248484E-4,{"$f":"AE281-AD282*Bodencharakterisierung!$E$8","v":4.5423028161703433E-2},{"$f":"IF(AE282>$J$18,(AE282/(Bodencharakterisierung!$E$11*1000)),0)","v":2.9982196806404905E-5},2.3305291073371062E-2,265,null,{"$f":"(AD282)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH282>0,(AJ282*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK281,NA())","v":0.57359474267457811},null,265,{"$f":"IF(AF282<=$J$9*0.05,AS281*EXP((-$J$6*1)/Heterogenität!$D$4),Z282)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF282>=$J$19, AR281/$J$5<AN282),0, Bodencharakterisierung!$E$8*$J$11*((AR281/$J$5)-AN282))","v":0},0,{"$f":"AQ281-AP282*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ282/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,265,null,{"$f":"(AP282)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF282<=$J$9*1.05,(AV282*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW281,NA())","v":{"$error":"#N/A"}},23072.238162637354,398,5.5958443426745754,0.57359474267457811,0,1.6622495999999976,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},29.982196806404904,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,266,2.3305291073371062E-2,{"$f":"Z283*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF282*Bodencharakterisierung!$E$11/$J$20","v":3.1375987549836506E-5},{"$f":"((150*($J$2^0.87)*(AB283^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z283)*3600*24","v":6.351289880934502E-2},2.3915996627248484E-4,{"$f":"AE282-AD283*Bodencharakterisierung!$E$8","v":4.534410537283351E-2},{"$f":"IF(AE283>$J$18,(AE283/(Bodencharakterisierung!$E$11*1000)),0)","v":2.993010255632575E-5},2.3305291073371062E-2,266,null,{"$f":"(AD283)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH283>0,(AJ283*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK282,NA())","v":0.57576220992995386},null,266,{"$f":"IF(AF283<=$J$9*0.05,AS282*EXP((-$J$6*1)/Heterogenität!$D$4),Z283)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF283>=$J$19, AR282/$J$5<AN283),0, Bodencharakterisierung!$E$8*$J$11*((AR282/$J$5)-AN283))","v":0},0,{"$f":"AQ282-AP283*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ283/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,266,null,{"$f":"(AP283)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF283<=$J$9*1.05,(AV283*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW282,NA())","v":{"$error":"#N/A"}},23072.238162637354,399,5.6042844499299509,0.57576220992995386,0,1.6685222399999975,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},29.93010255632575,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,267,2.3305291073371062E-2,{"$f":"Z284*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF283*Bodencharakterisierung!$E$11/$J$20","v":3.1321471579827516E-5},{"$f":"((150*($J$2^0.87)*(AB284^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z284)*3600*24","v":6.3425703194093103E-2},2.3915996627248484E-4,{"$f":"AE283-AD284*Bodencharakterisierung!$E$8","v":4.5265182583963587E-2},{"$f":"IF(AE284>$J$18,(AE284/(Bodencharakterisierung!$E$11*1000)),0)","v":2.9878008306246591E-5},2.3305291073371062E-2,267,null,{"$f":"(AD284)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH284>0,(AJ284*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK283,NA())","v":0.57792967718532962},null,267,{"$f":"IF(AF284<=$J$9*0.05,AS283*EXP((-$J$6*1)/Heterogenität!$D$4),Z284)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF284>=$J$19, AR283/$J$5<AN284),0, Bodencharakterisierung!$E$8*$J$11*((AR283/$J$5)-AN284))","v":0},0,{"$f":"AQ283-AP284*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ284/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,267,null,{"$f":"(AP284)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF284<=$J$9*1.05,(AV284*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW283,NA())","v":{"$error":"#N/A"}},23072.238162637354,400,5.6127245571853273,0.57792967718532962,0,1.6747948799999974,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},29.878008306246592,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,268,2.3305291073371062E-2,{"$f":"Z285*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF284*Bodencharakterisierung!$E$11/$J$20","v":3.1266955609818518E-5},{"$f":"((150*($J$2^0.87)*(AB285^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z285)*3600*24","v":6.3338475702010177E-2},2.3915996627248484E-4,{"$f":"AE284-AD285*Bodencharakterisierung!$E$8","v":4.5186259795093664E-2},{"$f":"IF(AE285>$J$18,(AE285/(Bodencharakterisierung!$E$11*1000)),0)","v":2.9825914056167436E-5},2.3305291073371062E-2,268,null,{"$f":"(AD285)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH285>0,(AJ285*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK284,NA())","v":0.58009714444070537},null,268,{"$f":"IF(AF285<=$J$9*0.05,AS284*EXP((-$J$6*1)/Heterogenität!$D$4),Z285)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF285>=$J$19, AR284/$J$5<AN285),0, Bodencharakterisierung!$E$8*$J$11*((AR284/$J$5)-AN285))","v":0},0,{"$f":"AQ284-AP285*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ285/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,268,null,{"$f":"(AP285)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF285<=$J$9*1.05,(AV285*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW284,NA())","v":{"$error":"#N/A"}},23072.238162637354,401,5.6211646644407027,0.58009714444070537,0,1.6810675199999974,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},29.825914056167434,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,269,2.3305291073371062E-2,{"$f":"Z286*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF285*Bodencharakterisierung!$E$11/$J$20","v":3.1212439639809528E-5},{"$f":"((150*($J$2^0.87)*(AB286^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z286)*3600*24","v":6.325121626583266E-2},2.3915996627248484E-4,{"$f":"AE285-AD286*Bodencharakterisierung!$E$8","v":4.5107337006223741E-2},{"$f":"IF(AE286>$J$18,(AE286/(Bodencharakterisierung!$E$11*1000)),0)","v":2.9773819806088277E-5},2.3305291073371062E-2,269,null,{"$f":"(AD286)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH286>0,(AJ286*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK285,NA())","v":0.58226461169608112},null,269,{"$f":"IF(AF286<=$J$9*0.05,AS285*EXP((-$J$6*1)/Heterogenität!$D$4),Z286)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF286>=$J$19, AR285/$J$5<AN286),0, Bodencharakterisierung!$E$8*$J$11*((AR285/$J$5)-AN286))","v":0},0,{"$f":"AQ285-AP286*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ286/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,269,null,{"$f":"(AP286)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF286<=$J$9*1.05,(AV286*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW285,NA())","v":{"$error":"#N/A"}},23072.238162637354,402,5.6296047716960782,0.58226461169608112,0,1.6873401599999973,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},29.773819806088277,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,270,2.3305291073371062E-2,{"$f":"Z287*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF286*Bodencharakterisierung!$E$11/$J$20","v":3.115792366980053E-5},{"$f":"((150*($J$2^0.87)*(AB287^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z287)*3600*24","v":6.3163924818037731E-2},2.3915996627248484E-4,{"$f":"AE286-AD287*Bodencharakterisierung!$E$8","v":4.5028414217353818E-2},{"$f":"IF(AE287>$J$18,(AE287/(Bodencharakterisierung!$E$11*1000)),0)","v":2.9721725556009122E-5},2.3305291073371062E-2,270,null,{"$f":"(AD287)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH287>0,(AJ287*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK286,NA())","v":0.58443207895145688},null,270,{"$f":"IF(AF287<=$J$9*0.05,AS286*EXP((-$J$6*1)/Heterogenität!$D$4),Z287)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF287>=$J$19, AR286/$J$5<AN287),0, Bodencharakterisierung!$E$8*$J$11*((AR286/$J$5)-AN287))","v":0},0,{"$f":"AQ286-AP287*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ287/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,270,null,{"$f":"(AP287)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF287<=$J$9*1.05,(AV287*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW286,NA())","v":{"$error":"#N/A"}},23072.238162637354,403,5.6380448789514546,0.58443207895145688,0,1.6936127999999973,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},29.721725556009122,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,271,2.3305291073371062E-2,{"$f":"Z288*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF287*Bodencharakterisierung!$E$11/$J$20","v":3.1103407699791547E-5},{"$f":"((150*($J$2^0.87)*(AB288^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z288)*3600*24","v":6.3076601290841167E-2},2.3915996627248484E-4,{"$f":"AE287-AD288*Bodencharakterisierung!$E$8","v":4.4949491428483895E-2},{"$f":"IF(AE288>$J$18,(AE288/(Bodencharakterisierung!$E$11*1000)),0)","v":2.9669631305929963E-5},2.3305291073371062E-2,271,null,{"$f":"(AD288)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH288>0,(AJ288*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK287,NA())","v":0.58659954620683263},null,271,{"$f":"IF(AF288<=$J$9*0.05,AS287*EXP((-$J$6*1)/Heterogenität!$D$4),Z288)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF288>=$J$19, AR287/$J$5<AN288),0, Bodencharakterisierung!$E$8*$J$11*((AR287/$J$5)-AN288))","v":0},0,{"$f":"AQ287-AP288*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ288/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,271,null,{"$f":"(AP288)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF288<=$J$9*1.05,(AV288*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW287,NA())","v":{"$error":"#N/A"}},23072.238162637354,404,5.6464849862068291,0.58659954620683263,0,1.6998854399999972,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},29.669631305929965,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,272,2.3305291073371062E-2,{"$f":"Z289*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF288*Bodencharakterisierung!$E$11/$J$20","v":3.1048891729782549E-5},{"$f":"((150*($J$2^0.87)*(AB289^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z289)*3600*24","v":6.2989245616195857E-2},2.3915996627248484E-4,{"$f":"AE288-AD289*Bodencharakterisierung!$E$8","v":4.4870568639613972E-2},{"$f":"IF(AE289>$J$18,(AE289/(Bodencharakterisierung!$E$11*1000)),0)","v":2.9617537055850808E-5},2.3305291073371062E-2,272,null,{"$f":"(AD289)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH289>0,(AJ289*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK288,NA())","v":0.58876701346220839},null,272,{"$f":"IF(AF289<=$J$9*0.05,AS288*EXP((-$J$6*1)/Heterogenität!$D$4),Z289)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF289>=$J$19, AR288/$J$5<AN289),0, Bodencharakterisierung!$E$8*$J$11*((AR288/$J$5)-AN289))","v":0},0,{"$f":"AQ288-AP289*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ289/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,272,null,{"$f":"(AP289)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF289<=$J$9*1.05,(AV289*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW288,NA())","v":{"$error":"#N/A"}},23072.238162637354,405,5.6549250934622055,0.58876701346220839,0,1.7061580799999971,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},29.617537055850807,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,273,2.3305291073371062E-2,{"$f":"Z290*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF289*Bodencharakterisierung!$E$11/$J$20","v":3.0994375759773552E-5},{"$f":"((150*($J$2^0.87)*(AB290^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z290)*3600*24","v":6.2901857725791127E-2},2.3915996627248484E-4,{"$f":"AE289-AD290*Bodencharakterisierung!$E$8","v":4.479164585074405E-2},{"$f":"IF(AE290>$J$18,(AE290/(Bodencharakterisierung!$E$11*1000)),0)","v":2.956544280577165E-5},2.3305291073371062E-2,273,null,{"$f":"(AD290)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH290>0,(AJ290*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK289,NA())","v":0.59093448071758414},null,273,{"$f":"IF(AF290<=$J$9*0.05,AS289*EXP((-$J$6*1)/Heterogenität!$D$4),Z290)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF290>=$J$19, AR289/$J$5<AN290),0, Bodencharakterisierung!$E$8*$J$11*((AR289/$J$5)-AN290))","v":0},0,{"$f":"AQ289-AP290*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ290/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,273,null,{"$f":"(AP290)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF290<=$J$9*1.05,(AV290*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW289,NA())","v":{"$error":"#N/A"}},23072.238162637354,406,5.663365200717581,0.59093448071758414,0,1.7124307199999971,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},29.565442805771649,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,274,2.3305291073371062E-2,{"$f":"Z291*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF290*Bodencharakterisierung!$E$11/$J$20","v":3.0939859789764561E-5},{"$f":"((150*($J$2^0.87)*(AB291^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z291)*3600*24","v":6.2814437551050623E-2},2.3915996627248484E-4,{"$f":"AE290-AD291*Bodencharakterisierung!$E$8","v":4.4712723061874127E-2},{"$f":"IF(AE291>$J$18,(AE291/(Bodencharakterisierung!$E$11*1000)),0)","v":2.9513348555692494E-5},2.3305291073371062E-2,274,null,{"$f":"(AD291)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH291>0,(AJ291*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK290,NA())","v":0.5931019479729599},null,274,{"$f":"IF(AF291<=$J$9*0.05,AS290*EXP((-$J$6*1)/Heterogenität!$D$4),Z291)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF291>=$J$19, AR290/$J$5<AN291),0, Bodencharakterisierung!$E$8*$J$11*((AR290/$J$5)-AN291))","v":0},0,{"$f":"AQ290-AP291*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ291/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,274,null,{"$f":"(AP291)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF291<=$J$9*1.05,(AV291*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW290,NA())","v":{"$error":"#N/A"}},23072.238162637354,407,5.6718053079729565,0.5931019479729599,0,1.718703359999997,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},29.513348555692495,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,275,2.3305291073371062E-2,{"$f":"Z292*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF291*Bodencharakterisierung!$E$11/$J$20","v":3.0885343819755571E-5},{"$f":"((150*($J$2^0.87)*(AB292^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z292)*3600*24","v":6.2726985023130677E-2},2.3915996627248484E-4,{"$f":"AE291-AD292*Bodencharakterisierung!$E$8","v":4.4633800273004204E-2},{"$f":"IF(AE292>$J$18,(AE292/(Bodencharakterisierung!$E$11*1000)),0)","v":2.9461254305613336E-5},2.3305291073371062E-2,275,null,{"$f":"(AD292)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH292>0,(AJ292*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK291,NA())","v":0.59526941522833565},null,275,{"$f":"IF(AF292<=$J$9*0.05,AS291*EXP((-$J$6*1)/Heterogenität!$D$4),Z292)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF292>=$J$19, AR291/$J$5<AN292),0, Bodencharakterisierung!$E$8*$J$11*((AR291/$J$5)-AN292))","v":0},0,{"$f":"AQ291-AP292*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ292/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,275,null,{"$f":"(AP292)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF292<=$J$9*1.05,(AV292*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW291,NA())","v":{"$error":"#N/A"}},23072.238162637354,408,5.6802454152283328,0.59526941522833565,0,1.724975999999997,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},29.461254305613334,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,276,2.3305291073371062E-2,{"$f":"Z293*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF292*Bodencharakterisierung!$E$11/$J$20","v":3.0830827849746573E-5},{"$f":"((150*($J$2^0.87)*(AB293^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z293)*3600*24","v":6.2639500072918866E-2},2.3915996627248484E-4,{"$f":"AE292-AD293*Bodencharakterisierung!$E$8","v":4.4554877484134281E-2},{"$f":"IF(AE293>$J$18,(AE293/(Bodencharakterisierung!$E$11*1000)),0)","v":2.9409160055534181E-5},2.3305291073371062E-2,276,null,{"$f":"(AD293)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH293>0,(AJ293*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK292,NA())","v":0.59743688248371141},null,276,{"$f":"IF(AF293<=$J$9*0.05,AS292*EXP((-$J$6*1)/Heterogenität!$D$4),Z293)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF293>=$J$19, AR292/$J$5<AN293),0, Bodencharakterisierung!$E$8*$J$11*((AR292/$J$5)-AN293))","v":0},0,{"$f":"AQ292-AP293*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ293/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,276,null,{"$f":"(AP293)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF293<=$J$9*1.05,(AV293*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW292,NA())","v":{"$error":"#N/A"}},23072.238162637354,409,5.6886855224837083,0.59743688248371141,0,1.7312486399999969,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},29.40916005553418,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,277,2.3305291073371062E-2,{"$f":"Z294*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF293*Bodencharakterisierung!$E$11/$J$20","v":3.0776311879737583E-5},{"$f":"((150*($J$2^0.87)*(AB294^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z294)*3600*24","v":6.2551982631033232E-2},2.3915996627248484E-4,{"$f":"AE293-AD294*Bodencharakterisierung!$E$8","v":4.4475954695264358E-2},{"$f":"IF(AE294>$J$18,(AE294/(Bodencharakterisierung!$E$11*1000)),0)","v":2.9357065805455022E-5},2.3305291073371062E-2,277,null,{"$f":"(AD294)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH294>0,(AJ294*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK293,NA())","v":0.59960434973908716},null,277,{"$f":"IF(AF294<=$J$9*0.05,AS293*EXP((-$J$6*1)/Heterogenität!$D$4),Z294)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF294>=$J$19, AR293/$J$5<AN294),0, Bodencharakterisierung!$E$8*$J$11*((AR293/$J$5)-AN294))","v":0},0,{"$f":"AQ293-AP294*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ294/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,277,null,{"$f":"(AP294)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF294<=$J$9*1.05,(AV294*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW293,NA())","v":{"$error":"#N/A"}},23072.238162637354,410,5.6971256297390838,0.59960434973908716,0,1.7375212799999968,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},29.357065805455022,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,278,2.3305291073371062E-2,{"$f":"Z295*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF294*Bodencharakterisierung!$E$11/$J$20","v":3.0721795909728592E-5},{"$f":"((150*($J$2^0.87)*(AB295^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z295)*3600*24","v":6.2464432627819574E-2},2.3915996627248484E-4,{"$f":"AE294-AD295*Bodencharakterisierung!$E$8","v":4.4397031906394435E-2},{"$f":"IF(AE295>$J$18,(AE295/(Bodencharakterisierung!$E$11*1000)),0)","v":2.9304971555375863E-5},2.3305291073371062E-2,278,null,{"$f":"(AD295)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH295>0,(AJ295*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK294,NA())","v":0.60177181699446292},null,278,{"$f":"IF(AF295<=$J$9*0.05,AS294*EXP((-$J$6*1)/Heterogenität!$D$4),Z295)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF295>=$J$19, AR294/$J$5<AN295),0, Bodencharakterisierung!$E$8*$J$11*((AR294/$J$5)-AN295))","v":0},0,{"$f":"AQ294-AP295*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ295/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,278,null,{"$f":"(AP295)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF295<=$J$9*1.05,(AV295*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW294,NA())","v":{"$error":"#N/A"}},23072.238162637354,411,5.7055657369944601,0.60177181699446292,0,1.7437939199999968,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},29.304971555375865,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,279,2.3305291073371062E-2,{"$f":"Z296*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF295*Bodencharakterisierung!$E$11/$J$20","v":3.0667279939719595E-5},{"$f":"((150*($J$2^0.87)*(AB296^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z296)*3600*24","v":6.2376849993350733E-2},2.3915996627248484E-4,{"$f":"AE295-AD296*Bodencharakterisierung!$E$8","v":4.4318109117524512E-2},{"$f":"IF(AE296>$J$18,(AE296/(Bodencharakterisierung!$E$11*1000)),0)","v":2.9252877305296708E-5},2.3305291073371062E-2,279,null,{"$f":"(AD296)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH296>0,(AJ296*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK295,NA())","v":0.60393928424983867},null,279,{"$f":"IF(AF296<=$J$9*0.05,AS295*EXP((-$J$6*1)/Heterogenität!$D$4),Z296)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF296>=$J$19, AR295/$J$5<AN296),0, Bodencharakterisierung!$E$8*$J$11*((AR295/$J$5)-AN296))","v":0},0,{"$f":"AQ295-AP296*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ296/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,279,null,{"$f":"(AP296)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF296<=$J$9*1.05,(AV296*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW295,NA())","v":{"$error":"#N/A"}},23072.238162637354,412,5.7140058442498347,0.60393928424983867,0,1.7500665599999967,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},29.252877305296707,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,280,2.3305291073371062E-2,{"$f":"Z297*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF296*Bodencharakterisierung!$E$11/$J$20","v":3.0612763969710604E-5},{"$f":"((150*($J$2^0.87)*(AB297^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z297)*3600*24","v":6.2289234657424974E-2},2.3915996627248484E-4,{"$f":"AE296-AD297*Bodencharakterisierung!$E$8","v":4.4239186328654589E-2},{"$f":"IF(AE297>$J$18,(AE297/(Bodencharakterisierung!$E$11*1000)),0)","v":2.9200783055217549E-5},2.3305291073371062E-2,280,null,{"$f":"(AD297)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH297>0,(AJ297*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK296,NA())","v":0.60610675150521443},null,280,{"$f":"IF(AF297<=$J$9*0.05,AS296*EXP((-$J$6*1)/Heterogenität!$D$4),Z297)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF297>=$J$19, AR296/$J$5<AN297),0, Bodencharakterisierung!$E$8*$J$11*((AR296/$J$5)-AN297))","v":0},0,{"$f":"AQ296-AP297*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ297/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,280,null,{"$f":"(AP297)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF297<=$J$9*1.05,(AV297*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW296,NA())","v":{"$error":"#N/A"}},23072.238162637354,413,5.7224459515052111,0.60610675150521443,0,1.7563391999999967,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},29.200783055217549,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,281,2.3305291073371062E-2,{"$f":"Z298*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF297*Bodencharakterisierung!$E$11/$J$20","v":3.0558247999701614E-5},{"$f":"((150*($J$2^0.87)*(AB298^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z298)*3600*24","v":6.2201586549563675E-2},2.3915996627248484E-4,{"$f":"AE297-AD298*Bodencharakterisierung!$E$8","v":4.4160263539784667E-2},{"$f":"IF(AE298>$J$18,(AE298/(Bodencharakterisierung!$E$11*1000)),0)","v":2.9148688805138394E-5},2.3305291073371062E-2,281,null,{"$f":"(AD298)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH298>0,(AJ298*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK297,NA())","v":0.60827421876059018},null,281,{"$f":"IF(AF298<=$J$9*0.05,AS297*EXP((-$J$6*1)/Heterogenität!$D$4),Z298)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF298>=$J$19, AR297/$J$5<AN298),0, Bodencharakterisierung!$E$8*$J$11*((AR297/$J$5)-AN298))","v":0},0,{"$f":"AQ297-AP298*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ298/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,281,null,{"$f":"(AP298)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF298<=$J$9*1.05,(AV298*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW297,NA())","v":{"$error":"#N/A"}},23072.238162637354,414,5.7308860587605865,0.60827421876059018,0,1.7626118399999966,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},29.148688805138395,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,282,2.3305291073371062E-2,{"$f":"Z299*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF298*Bodencharakterisierung!$E$11/$J$20","v":3.050373202969262E-5},{"$f":"((150*($J$2^0.87)*(AB299^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z299)*3600*24","v":6.2113905599010977E-2},2.3915996627248484E-4,{"$f":"AE298-AD299*Bodencharakterisierung!$E$8","v":4.4081340750914744E-2},{"$f":"IF(AE299>$J$18,(AE299/(Bodencharakterisierung!$E$11*1000)),0)","v":2.9096594555059236E-5},2.3305291073371062E-2,282,null,{"$f":"(AD299)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH299>0,(AJ299*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK298,NA())","v":0.61044168601596593},null,282,{"$f":"IF(AF299<=$J$9*0.05,AS298*EXP((-$J$6*1)/Heterogenität!$D$4),Z299)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF299>=$J$19, AR298/$J$5<AN299),0, Bodencharakterisierung!$E$8*$J$11*((AR298/$J$5)-AN299))","v":0},0,{"$f":"AQ298-AP299*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ299/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,282,null,{"$f":"(AP299)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF299<=$J$9*1.05,(AV299*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW298,NA())","v":{"$error":"#N/A"}},23072.238162637354,415,5.739326166015962,0.61044168601596593,0,1.7688844799999965,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},29.096594555059237,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,283,2.3305291073371062E-2,{"$f":"Z300*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF299*Bodencharakterisierung!$E$11/$J$20","v":3.0449216059683626E-5},{"$f":"((150*($J$2^0.87)*(AB300^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z300)*3600*24","v":6.2026191734730868E-2},2.3915996627248484E-4,{"$f":"AE299-AD300*Bodencharakterisierung!$E$8","v":4.4002417962044821E-2},{"$f":"IF(AE300>$J$18,(AE300/(Bodencharakterisierung!$E$11*1000)),0)","v":2.904450030498008E-5},2.3305291073371062E-2,283,null,{"$f":"(AD300)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH300>0,(AJ300*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK299,NA())","v":0.61260915327134169},null,283,{"$f":"IF(AF300<=$J$9*0.05,AS299*EXP((-$J$6*1)/Heterogenität!$D$4),Z300)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF300>=$J$19, AR299/$J$5<AN300),0, Bodencharakterisierung!$E$8*$J$11*((AR299/$J$5)-AN300))","v":0},0,{"$f":"AQ299-AP300*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ300/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,283,null,{"$f":"(AP300)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF300<=$J$9*1.05,(AV300*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW299,NA())","v":{"$error":"#N/A"}},23072.238162637354,416,5.7477662732713384,0.61260915327134169,0,1.7751571199999965,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},29.04450030498008,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,284,2.3305291073371062E-2,{"$f":"Z301*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF300*Bodencharakterisierung!$E$11/$J$20","v":3.0394700089674632E-5},{"$f":"((150*($J$2^0.87)*(AB301^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z301)*3600*24","v":6.1938444885406604E-2},2.3915996627248484E-4,{"$f":"AE300-AD301*Bodencharakterisierung!$E$8","v":4.3923495173174898E-2},{"$f":"IF(AE301>$J$18,(AE301/(Bodencharakterisierung!$E$11*1000)),0)","v":2.8992406054900922E-5},2.3305291073371062E-2,284,null,{"$f":"(AD301)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH301>0,(AJ301*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK300,NA())","v":0.61477662052671744},null,284,{"$f":"IF(AF301<=$J$9*0.05,AS300*EXP((-$J$6*1)/Heterogenität!$D$4),Z301)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF301>=$J$19, AR300/$J$5<AN301),0, Bodencharakterisierung!$E$8*$J$11*((AR300/$J$5)-AN301))","v":0},0,{"$f":"AQ300-AP301*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ301/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,284,null,{"$f":"(AP301)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF301<=$J$9*1.05,(AV301*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW300,NA())","v":{"$error":"#N/A"}},23072.238162637354,417,5.7562063805267139,0.61477662052671744,0,1.7814297599999964,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},28.992406054900922,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,285,2.3305291073371062E-2,{"$f":"Z302*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF301*Bodencharakterisierung!$E$11/$J$20","v":3.0340184119665638E-5},{"$f":"((150*($J$2^0.87)*(AB302^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z302)*3600*24","v":6.1850664979438738E-2},2.3915996627248484E-4,{"$f":"AE301-AD302*Bodencharakterisierung!$E$8","v":4.3844572384304975E-2},{"$f":"IF(AE302>$J$18,(AE302/(Bodencharakterisierung!$E$11*1000)),0)","v":2.8940311804821767E-5},2.3305291073371062E-2,285,null,{"$f":"(AD302)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH302>0,(AJ302*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK301,NA())","v":0.6169440877820932},null,285,{"$f":"IF(AF302<=$J$9*0.05,AS301*EXP((-$J$6*1)/Heterogenität!$D$4),Z302)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF302>=$J$19, AR301/$J$5<AN302),0, Bodencharakterisierung!$E$8*$J$11*((AR301/$J$5)-AN302))","v":0},0,{"$f":"AQ301-AP302*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ302/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,285,null,{"$f":"(AP302)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF302<=$J$9*1.05,(AV302*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW301,NA())","v":{"$error":"#N/A"}},23072.238162637354,418,5.7646464877820893,0.6169440877820932,0,1.7877023999999964,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},28.940311804821768,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,286,2.3305291073371062E-2,{"$f":"Z303*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF302*Bodencharakterisierung!$E$11/$J$20","v":3.0285668149656647E-5},{"$f":"((150*($J$2^0.87)*(AB303^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z303)*3600*24","v":6.1762851944942986E-2},2.3915996627248484E-4,{"$f":"AE302-AD303*Bodencharakterisierung!$E$8","v":4.3765649595435052E-2},{"$f":"IF(AE303>$J$18,(AE303/(Bodencharakterisierung!$E$11*1000)),0)","v":2.8888217554742608E-5},2.3305291073371062E-2,286,null,{"$f":"(AD303)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH303>0,(AJ303*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK302,NA())","v":0.61911155503746895},null,286,{"$f":"IF(AF303<=$J$9*0.05,AS302*EXP((-$J$6*1)/Heterogenität!$D$4),Z303)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF303>=$J$19, AR302/$J$5<AN303),0, Bodencharakterisierung!$E$8*$J$11*((AR302/$J$5)-AN303))","v":0},0,{"$f":"AQ302-AP303*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ303/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,286,null,{"$f":"(AP303)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF303<=$J$9*1.05,(AV303*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW302,NA())","v":{"$error":"#N/A"}},23072.238162637354,419,5.7730865950374657,0.61911155503746895,0,1.7939750399999963,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},28.888217554742607,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,287,2.3305291073371062E-2,{"$f":"Z304*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF303*Bodencharakterisierung!$E$11/$J$20","v":3.023115217964765E-5},{"$f":"((150*($J$2^0.87)*(AB304^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z304)*3600*24","v":6.1675005709749528E-2},2.3915996627248484E-4,{"$f":"AE303-AD304*Bodencharakterisierung!$E$8","v":4.3686726806565129E-2},{"$f":"IF(AE304>$J$18,(AE304/(Bodencharakterisierung!$E$11*1000)),0)","v":2.8836123304663453E-5},2.3305291073371062E-2,287,null,{"$f":"(AD304)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH304>0,(AJ304*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK303,NA())","v":0.62127902229284471},null,287,{"$f":"IF(AF304<=$J$9*0.05,AS303*EXP((-$J$6*1)/Heterogenität!$D$4),Z304)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF304>=$J$19, AR303/$J$5<AN304),0, Bodencharakterisierung!$E$8*$J$11*((AR303/$J$5)-AN304))","v":0},0,{"$f":"AQ303-AP304*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ304/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,287,null,{"$f":"(AP304)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF304<=$J$9*1.05,(AV304*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW303,NA())","v":{"$error":"#N/A"}},23072.238162637354,420,5.7815267022928403,0.62127902229284471,0,1.8002476799999962,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},28.836123304663452,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,288,2.3305291073371062E-2,{"$f":"Z305*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF304*Bodencharakterisierung!$E$11/$J$20","v":3.0176636209638659E-5},{"$f":"((150*($J$2^0.87)*(AB305^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z305)*3600*24","v":6.1587126201400805E-2},2.3915996627248484E-4,{"$f":"AE304-AD305*Bodencharakterisierung!$E$8","v":4.3607804017695206E-2},{"$f":"IF(AE305>$J$18,(AE305/(Bodencharakterisierung!$E$11*1000)),0)","v":2.8784029054584294E-5},2.3305291073371062E-2,288,null,{"$f":"(AD305)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH305>0,(AJ305*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK304,NA())","v":0.62344648954822046},null,288,{"$f":"IF(AF305<=$J$9*0.05,AS304*EXP((-$J$6*1)/Heterogenität!$D$4),Z305)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF305>=$J$19, AR304/$J$5<AN305),0, Bodencharakterisierung!$E$8*$J$11*((AR304/$J$5)-AN305))","v":0},0,{"$f":"AQ304-AP305*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ305/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,288,null,{"$f":"(AP305)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF305<=$J$9*1.05,(AV305*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW304,NA())","v":{"$error":"#N/A"}},23072.238162637354,421,5.7899668095482166,0.62344648954822046,0,1.8065203199999962,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},28.784029054584295,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,289,2.3305291073371062E-2,{"$f":"Z306*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF305*Bodencharakterisierung!$E$11/$J$20","v":3.0122120239629662E-5},{"$f":"((150*($J$2^0.87)*(AB306^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z306)*3600*24","v":6.1499213347149681E-2},2.3915996627248484E-4,{"$f":"AE305-AD306*Bodencharakterisierung!$E$8","v":4.3528881228825284E-2},{"$f":"IF(AE306>$J$18,(AE306/(Bodencharakterisierung!$E$11*1000)),0)","v":2.8731934804505139E-5},2.3305291073371062E-2,289,null,{"$f":"(AD306)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH306>0,(AJ306*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK305,NA())","v":0.62561395680359622},null,289,{"$f":"IF(AF306<=$J$9*0.05,AS305*EXP((-$J$6*1)/Heterogenität!$D$4),Z306)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF306>=$J$19, AR305/$J$5<AN306),0, Bodencharakterisierung!$E$8*$J$11*((AR305/$J$5)-AN306))","v":0},0,{"$f":"AQ305-AP306*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ306/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,289,null,{"$f":"(AP306)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF306<=$J$9*1.05,(AV306*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW305,NA())","v":{"$error":"#N/A"}},23072.238162637354,422,5.7984069168035921,0.62561395680359622,0,1.8127929599999961,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},28.731934804505141,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,290,2.3305291073371062E-2,{"$f":"Z307*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF306*Bodencharakterisierung!$E$11/$J$20","v":3.0067604269620674E-5},{"$f":"((150*($J$2^0.87)*(AB307^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z307)*3600*24","v":6.1411267073958109E-2},2.3915996627248484E-4,{"$f":"AE306-AD307*Bodencharakterisierung!$E$8","v":4.3449958439955361E-2},{"$f":"IF(AE307>$J$18,(AE307/(Bodencharakterisierung!$E$11*1000)),0)","v":2.867984055442598E-5},2.3305291073371062E-2,290,null,{"$f":"(AD307)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH307>0,(AJ307*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK306,NA())","v":0.62778142405897197},null,290,{"$f":"IF(AF307<=$J$9*0.05,AS306*EXP((-$J$6*1)/Heterogenität!$D$4),Z307)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF307>=$J$19, AR306/$J$5<AN307),0, Bodencharakterisierung!$E$8*$J$11*((AR306/$J$5)-AN307))","v":0},0,{"$f":"AQ306-AP307*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ307/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,290,null,{"$f":"(AP307)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF307<=$J$9*1.05,(AV307*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW306,NA())","v":{"$error":"#N/A"}},23072.238162637354,423,5.8068470240589676,0.62778142405897197,0,1.8190655999999961,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},28.679840554425979,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,291,2.3305291073371062E-2,{"$f":"Z308*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF307*Bodencharakterisierung!$E$11/$J$20","v":3.0013088299611677E-5},{"$f":"((150*($J$2^0.87)*(AB308^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z308)*3600*24","v":6.1323287308495289E-2},2.3915996627248484E-4,{"$f":"AE307-AD308*Bodencharakterisierung!$E$8","v":4.3371035651085438E-2},{"$f":"IF(AE308>$J$18,(AE308/(Bodencharakterisierung!$E$11*1000)),0)","v":2.8627746304346825E-5},2.3305291073371062E-2,291,null,{"$f":"(AD308)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH308>0,(AJ308*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK307,NA())","v":0.62994889131434773},null,291,{"$f":"IF(AF308<=$J$9*0.05,AS307*EXP((-$J$6*1)/Heterogenität!$D$4),Z308)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF308>=$J$19, AR307/$J$5<AN308),0, Bodencharakterisierung!$E$8*$J$11*((AR307/$J$5)-AN308))","v":0},0,{"$f":"AQ307-AP308*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ308/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,291,null,{"$f":"(AP308)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF308<=$J$9*1.05,(AV308*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW307,NA())","v":{"$error":"#N/A"}},23072.238162637354,424,5.8152871313143439,0.62994889131434773,0,1.825338239999996,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},28.627746304346825,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,292,2.3305291073371062E-2,{"$f":"Z309*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF308*Bodencharakterisierung!$E$11/$J$20","v":2.995857232960269E-5},{"$f":"((150*($J$2^0.87)*(AB309^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z309)*3600*24","v":6.1235273977136233E-2},2.3915996627248484E-4,{"$f":"AE308-AD309*Bodencharakterisierung!$E$8","v":4.3292112862215515E-2},{"$f":"IF(AE309>$J$18,(AE309/(Bodencharakterisierung!$E$11*1000)),0)","v":2.8575652054267666E-5},2.3305291073371062E-2,292,null,{"$f":"(AD309)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH309>0,(AJ309*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK308,NA())","v":0.63211635856972348},null,292,{"$f":"IF(AF309<=$J$9*0.05,AS308*EXP((-$J$6*1)/Heterogenität!$D$4),Z309)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF309>=$J$19, AR308/$J$5<AN309),0, Bodencharakterisierung!$E$8*$J$11*((AR308/$J$5)-AN309))","v":0},0,{"$f":"AQ308-AP309*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ309/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,292,null,{"$f":"(AP309)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF309<=$J$9*1.05,(AV309*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW308,NA())","v":{"$error":"#N/A"}},23072.238162637354,425,5.8237272385697194,0.63211635856972348,0,1.8316108799999959,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},28.575652054267668,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,293,2.3305291073371062E-2,{"$f":"Z310*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF309*Bodencharakterisierung!$E$11/$J$20","v":2.9904056359593689E-5},{"$f":"((150*($J$2^0.87)*(AB310^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z310)*3600*24","v":6.1147227005959426E-2},2.3915996627248484E-4,{"$f":"AE309-AD310*Bodencharakterisierung!$E$8","v":4.3213190073345592E-2},{"$f":"IF(AE310>$J$18,(AE310/(Bodencharakterisierung!$E$11*1000)),0)","v":2.8523557804188511E-5},2.3305291073371062E-2,293,null,{"$f":"(AD310)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH310>0,(AJ310*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK309,NA())","v":0.63428382582509923},null,293,{"$f":"IF(AF310<=$J$9*0.05,AS309*EXP((-$J$6*1)/Heterogenität!$D$4),Z310)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF310>=$J$19, AR309/$J$5<AN310),0, Bodencharakterisierung!$E$8*$J$11*((AR309/$J$5)-AN310))","v":0},0,{"$f":"AQ309-AP310*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ310/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,293,null,{"$f":"(AP310)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF310<=$J$9*1.05,(AV310*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW309,NA())","v":{"$error":"#N/A"}},23072.238162637354,426,5.8321673458250949,0.63428382582509923,0,1.8378835199999959,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},28.52355780418851,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,294,2.3305291073371062E-2,{"$f":"Z311*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF310*Bodencharakterisierung!$E$11/$J$20","v":2.9849540389584702E-5},{"$f":"((150*($J$2^0.87)*(AB311^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z311)*3600*24","v":6.1059146320745841E-2},2.3915996627248484E-4,{"$f":"AE310-AD311*Bodencharakterisierung!$E$8","v":4.3134267284475669E-2},{"$f":"IF(AE311>$J$18,(AE311/(Bodencharakterisierung!$E$11*1000)),0)","v":2.8471463554109353E-5},2.3305291073371062E-2,294,null,{"$f":"(AD311)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH311>0,(AJ311*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK310,NA())","v":0.63645129308047499},null,294,{"$f":"IF(AF311<=$J$9*0.05,AS310*EXP((-$J$6*1)/Heterogenität!$D$4),Z311)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF311>=$J$19, AR310/$J$5<AN311),0, Bodencharakterisierung!$E$8*$J$11*((AR310/$J$5)-AN311))","v":0},0,{"$f":"AQ310-AP311*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ311/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,294,null,{"$f":"(AP311)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF311<=$J$9*1.05,(AV311*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW310,NA())","v":{"$error":"#N/A"}},23072.238162637354,427,5.8406074530804712,0.63645129308047499,0,1.8441561599999958,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},28.471463554109352,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,295,2.3305291073371062E-2,{"$f":"Z312*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF311*Bodencharakterisierung!$E$11/$J$20","v":2.9795024419575705E-5},{"$f":"((150*($J$2^0.87)*(AB312^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z312)*3600*24","v":6.0971031846976553E-2},2.3915996627248484E-4,{"$f":"AE311-AD312*Bodencharakterisierung!$E$8","v":4.3055344495605746E-2},{"$f":"IF(AE312>$J$18,(AE312/(Bodencharakterisierung!$E$11*1000)),0)","v":2.8419369304030194E-5},2.3305291073371062E-2,295,null,{"$f":"(AD312)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH312>0,(AJ312*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK311,NA())","v":0.63861876033585074},null,295,{"$f":"IF(AF312<=$J$9*0.05,AS311*EXP((-$J$6*1)/Heterogenität!$D$4),Z312)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF312>=$J$19, AR311/$J$5<AN312),0, Bodencharakterisierung!$E$8*$J$11*((AR311/$J$5)-AN312))","v":0},0,{"$f":"AQ311-AP312*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ312/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,295,null,{"$f":"(AP312)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF312<=$J$9*1.05,(AV312*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW311,NA())","v":{"$error":"#N/A"}},23072.238162637354,428,5.8490475603358458,0.63861876033585074,0,1.8504287999999958,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},28.419369304030194,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,296,2.3305291073371062E-2,{"$f":"Z313*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF312*Bodencharakterisierung!$E$11/$J$20","v":2.9740508449566711E-5},{"$f":"((150*($J$2^0.87)*(AB313^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z313)*3600*24","v":6.088288350983137E-2},2.3915996627248484E-4,{"$f":"AE312-AD313*Bodencharakterisierung!$E$8","v":4.2976421706735823E-2},{"$f":"IF(AE313>$J$18,(AE313/(Bodencharakterisierung!$E$11*1000)),0)","v":2.8367275053951039E-5},2.3305291073371062E-2,296,null,{"$f":"(AD313)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH313>0,(AJ313*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK312,NA())","v":0.6407862275912265},null,296,{"$f":"IF(AF313<=$J$9*0.05,AS312*EXP((-$J$6*1)/Heterogenität!$D$4),Z313)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF313>=$J$19, AR312/$J$5<AN313),0, Bodencharakterisierung!$E$8*$J$11*((AR312/$J$5)-AN313))","v":0},0,{"$f":"AQ312-AP313*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ313/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,296,null,{"$f":"(AP313)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF313<=$J$9*1.05,(AV313*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW312,NA())","v":{"$error":"#N/A"}},23072.238162637354,429,5.8574876675912222,0.6407862275912265,0,1.8567014399999957,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},28.36727505395104,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,297,2.3305291073371062E-2,{"$f":"Z314*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF313*Bodencharakterisierung!$E$11/$J$20","v":2.968599247955772E-5},{"$f":"((150*($J$2^0.87)*(AB314^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z314)*3600*24","v":6.0794701234186968E-2},2.3915996627248484E-4,{"$f":"AE313-AD314*Bodencharakterisierung!$E$8","v":4.2897498917865901E-2},{"$f":"IF(AE314>$J$18,(AE314/(Bodencharakterisierung!$E$11*1000)),0)","v":2.831518080387188E-5},2.3305291073371062E-2,297,null,{"$f":"(AD314)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH314>0,(AJ314*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK313,NA())","v":0.64295369484660225},null,297,{"$f":"IF(AF314<=$J$9*0.05,AS313*EXP((-$J$6*1)/Heterogenität!$D$4),Z314)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF314>=$J$19, AR313/$J$5<AN314),0, Bodencharakterisierung!$E$8*$J$11*((AR313/$J$5)-AN314))","v":0},0,{"$f":"AQ313-AP314*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ314/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,297,null,{"$f":"(AP314)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF314<=$J$9*1.05,(AV314*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW313,NA())","v":{"$error":"#N/A"}},23072.238162637354,430,5.8659277748465977,0.64295369484660225,0,1.8629740799999956,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},28.315180803871879,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,298,2.3305291073371062E-2,{"$f":"Z315*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF314*Bodencharakterisierung!$E$11/$J$20","v":2.9631476509548726E-5},{"$f":"((150*($J$2^0.87)*(AB315^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z315)*3600*24","v":6.0706484944614891E-2},2.3915996627248484E-4,{"$f":"AE314-AD315*Bodencharakterisierung!$E$8","v":4.2818576128995978E-2},{"$f":"IF(AE315>$J$18,(AE315/(Bodencharakterisierung!$E$11*1000)),0)","v":2.8263086553792725E-5},2.3305291073371062E-2,298,null,{"$f":"(AD315)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH315>0,(AJ315*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK314,NA())","v":0.64512116210197801},null,298,{"$f":"IF(AF315<=$J$9*0.05,AS314*EXP((-$J$6*1)/Heterogenität!$D$4),Z315)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF315>=$J$19, AR314/$J$5<AN315),0, Bodencharakterisierung!$E$8*$J$11*((AR314/$J$5)-AN315))","v":0},0,{"$f":"AQ314-AP315*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ315/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,298,null,{"$f":"(AP315)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF315<=$J$9*1.05,(AV315*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW314,NA())","v":{"$error":"#N/A"}},23072.238162637354,431,5.8743678821019731,0.64512116210197801,0,1.8692467199999956,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},28.263086553792725,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,299,2.3305291073371062E-2,{"$f":"Z316*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF315*Bodencharakterisierung!$E$11/$J$20","v":2.9576960539539732E-5},{"$f":"((150*($J$2^0.87)*(AB316^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z316)*3600*24","v":6.0618234565380229E-2},2.3915996627248484E-4,{"$f":"AE315-AD316*Bodencharakterisierung!$E$8","v":4.2739653340126055E-2},{"$f":"IF(AE316>$J$18,(AE316/(Bodencharakterisierung!$E$11*1000)),0)","v":2.8210992303713566E-5},2.3305291073371062E-2,299,null,{"$f":"(AD316)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH316>0,(AJ316*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK315,NA())","v":0.64728862935735376},null,299,{"$f":"IF(AF316<=$J$9*0.05,AS315*EXP((-$J$6*1)/Heterogenität!$D$4),Z316)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF316>=$J$19, AR315/$J$5<AN316),0, Bodencharakterisierung!$E$8*$J$11*((AR315/$J$5)-AN316))","v":0},0,{"$f":"AQ315-AP316*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ316/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,299,null,{"$f":"(AP316)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF316<=$J$9*1.05,(AV316*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW315,NA())","v":{"$error":"#N/A"}},23072.238162637354,432,5.8828079893573495,0.64728862935735376,0,1.8755193599999955,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},28.210992303713567,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,2.3305291073371062E-2,{"$f":"Z317*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF316*Bodencharakterisierung!$E$11/$J$20","v":2.9522444569530741E-5},{"$f":"((150*($J$2^0.87)*(AB317^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z317)*3600*24","v":6.0529950020439371E-2},2.3915996627248484E-4,{"$f":"AE316-AD317*Bodencharakterisierung!$E$8","v":4.2660730551256132E-2},{"$f":"IF(AE317>$J$18,(AE317/(Bodencharakterisierung!$E$11*1000)),0)","v":2.8158898053634411E-5},2.3305291073371062E-2,300,null,{"$f":"(AD317)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH317>0,(AJ317*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK316,NA())","v":0.64945609661272952},null,300,{"$f":"IF(AF317<=$J$9*0.05,AS316*EXP((-$J$6*1)/Heterogenität!$D$4),Z317)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF317>=$J$19, AR316/$J$5<AN317),0, Bodencharakterisierung!$E$8*$J$11*((AR316/$J$5)-AN317))","v":0},0,{"$f":"AQ316-AP317*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ317/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,300,null,{"$f":"(AP317)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF317<=$J$9*1.05,(AV317*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW316,NA())","v":{"$error":"#N/A"}},23072.238162637354,433,5.891248096612725,0.64945609661272952,0,1.8817919999999955,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},28.15889805363441,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,301,2.3305291073371062E-2,{"$f":"Z318*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF317*Bodencharakterisierung!$E$11/$J$20","v":2.9467928599521747E-5},{"$f":"((150*($J$2^0.87)*(AB318^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z318)*3600*24","v":6.0441631233438167E-2},2.3915996627248484E-4,{"$f":"AE317-AD318*Bodencharakterisierung!$E$8","v":4.2581807762386209E-2},{"$f":"IF(AE318>$J$18,(AE318/(Bodencharakterisierung!$E$11*1000)),0)","v":2.8106803803555252E-5},2.3305291073371062E-2,301,null,{"$f":"(AD318)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH318>0,(AJ318*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK317,NA())","v":0.65162356386810527},null,301,{"$f":"IF(AF318<=$J$9*0.05,AS317*EXP((-$J$6*1)/Heterogenität!$D$4),Z318)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF318>=$J$19, AR317/$J$5<AN318),0, Bodencharakterisierung!$E$8*$J$11*((AR317/$J$5)-AN318))","v":0},0,{"$f":"AQ317-AP318*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ318/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,301,null,{"$f":"(AP318)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF318<=$J$9*1.05,(AV318*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW317,NA())","v":{"$error":"#N/A"}},23072.238162637354,434,5.8996882038681004,0.65162356386810527,0,1.8880646399999954,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},28.106803803555252,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,302,2.3305291073371062E-2,{"$f":"Z319*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF318*Bodencharakterisierung!$E$11/$J$20","v":2.9413412629512753E-5},{"$f":"((150*($J$2^0.87)*(AB319^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z319)*3600*24","v":6.0353278127710394E-2},2.3915996627248484E-4,{"$f":"AE318-AD319*Bodencharakterisierung!$E$8","v":4.2502884973516286E-2},{"$f":"IF(AE319>$J$18,(AE319/(Bodencharakterisierung!$E$11*1000)),0)","v":2.8054709553476097E-5},2.3305291073371062E-2,302,null,{"$f":"(AD319)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH319>0,(AJ319*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK318,NA())","v":0.65379103112348103},null,302,{"$f":"IF(AF319<=$J$9*0.05,AS318*EXP((-$J$6*1)/Heterogenität!$D$4),Z319)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF319>=$J$19, AR318/$J$5<AN319),0, Bodencharakterisierung!$E$8*$J$11*((AR318/$J$5)-AN319))","v":0},0,{"$f":"AQ318-AP319*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ319/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,302,null,{"$f":"(AP319)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF319<=$J$9*1.05,(AV319*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW318,NA())","v":{"$error":"#N/A"}},23072.238162637354,435,5.9081283111234768,0.65379103112348103,0,1.8943372799999953,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},28.054709553476098,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,303,2.3305291073371062E-2,{"$f":"Z320*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF319*Bodencharakterisierung!$E$11/$J$20","v":2.9358896659503759E-5},{"$f":"((150*($J$2^0.87)*(AB320^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z320)*3600*24","v":6.0264890626275755E-2},2.3915996627248484E-4,{"$f":"AE319-AD320*Bodencharakterisierung!$E$8","v":4.2423962184646363E-2},{"$f":"IF(AE320>$J$18,(AE320/(Bodencharakterisierung!$E$11*1000)),0)","v":2.8002615303396939E-5},2.3305291073371062E-2,303,null,{"$f":"(AD320)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH320>0,(AJ320*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK319,NA())","v":0.65595849837885678},null,303,{"$f":"IF(AF320<=$J$9*0.05,AS319*EXP((-$J$6*1)/Heterogenität!$D$4),Z320)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF320>=$J$19, AR319/$J$5<AN320),0, Bodencharakterisierung!$E$8*$J$11*((AR319/$J$5)-AN320))","v":0},0,{"$f":"AQ319-AP320*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ320/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,303,null,{"$f":"(AP320)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF320<=$J$9*1.05,(AV320*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW319,NA())","v":{"$error":"#N/A"}},23072.238162637354,436,5.9165684183788514,0.65595849837885678,0,1.9006099199999953,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},28.00261530339694,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,304,2.3305291073371062E-2,{"$f":"Z321*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF320*Bodencharakterisierung!$E$11/$J$20","v":2.9304380689494769E-5},{"$f":"((150*($J$2^0.87)*(AB321^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z321)*3600*24","v":6.0176468651837969E-2},2.3915996627248484E-4,{"$f":"AE320-AD321*Bodencharakterisierung!$E$8","v":4.234503939577644E-2},{"$f":"IF(AE321>$J$18,(AE321/(Bodencharakterisierung!$E$11*1000)),0)","v":2.7950521053317783E-5},2.3305291073371062E-2,304,null,{"$f":"(AD321)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH321>0,(AJ321*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK320,NA())","v":0.65812596563423253},null,304,{"$f":"IF(AF321<=$J$9*0.05,AS320*EXP((-$J$6*1)/Heterogenität!$D$4),Z321)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF321>=$J$19, AR320/$J$5<AN321),0, Bodencharakterisierung!$E$8*$J$11*((AR320/$J$5)-AN321))","v":0},0,{"$f":"AQ320-AP321*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ321/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,304,null,{"$f":"(AP321)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF321<=$J$9*1.05,(AV321*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW320,NA())","v":{"$error":"#N/A"}},23072.238162637354,437,5.9250085256342278,0.65812596563423253,0,1.9068825599999952,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},27.950521053317782,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,305,2.3305291073371062E-2,{"$f":"Z322*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF321*Bodencharakterisierung!$E$11/$J$20","v":2.9249864719485775E-5},{"$f":"((150*($J$2^0.87)*(AB322^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z322)*3600*24","v":6.0088012126782761E-2},2.3915996627248484E-4,{"$f":"AE321-AD322*Bodencharakterisierung!$E$8","v":4.2266116606906518E-2},{"$f":"IF(AE322>$J$18,(AE322/(Bodencharakterisierung!$E$11*1000)),0)","v":2.7898426803238625E-5},2.3305291073371062E-2,305,null,{"$f":"(AD322)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH322>0,(AJ322*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK321,NA())","v":0.66029343288960829},null,305,{"$f":"IF(AF322<=$J$9*0.05,AS321*EXP((-$J$6*1)/Heterogenität!$D$4),Z322)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF322>=$J$19, AR321/$J$5<AN322),0, Bodencharakterisierung!$E$8*$J$11*((AR321/$J$5)-AN322))","v":0},0,{"$f":"AQ321-AP322*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ322/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,305,null,{"$f":"(AP322)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF322<=$J$9*1.05,(AV322*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW321,NA())","v":{"$error":"#N/A"}},23072.238162637354,438,5.9334486328896032,0.66029343288960829,0,1.9131551999999952,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},27.898426803238625,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,306,2.3305291073371062E-2,{"$f":"Z323*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF322*Bodencharakterisierung!$E$11/$J$20","v":2.9195348749476781E-5},{"$f":"((150*($J$2^0.87)*(AB323^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z323)*3600*24","v":5.9999520973176318E-2},2.3915996627248484E-4,{"$f":"AE322-AD323*Bodencharakterisierung!$E$8","v":4.2187193818036595E-2},{"$f":"IF(AE323>$J$18,(AE323/(Bodencharakterisierung!$E$11*1000)),0)","v":2.784633255315947E-5},2.3305291073371062E-2,306,null,{"$f":"(AD323)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH323>0,(AJ323*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK322,NA())","v":0.66246090014498404},null,306,{"$f":"IF(AF323<=$J$9*0.05,AS322*EXP((-$J$6*1)/Heterogenität!$D$4),Z323)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF323>=$J$19, AR322/$J$5<AN323),0, Bodencharakterisierung!$E$8*$J$11*((AR322/$J$5)-AN323))","v":0},0,{"$f":"AQ322-AP323*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ323/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,306,null,{"$f":"(AP323)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF323<=$J$9*1.05,(AV323*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW322,NA())","v":{"$error":"#N/A"}},23072.238162637354,439,5.9418887401449787,0.66246090014498404,0,1.9194278399999951,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},27.846332553159471,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,307,2.3305291073371062E-2,{"$f":"Z324*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF323*Bodencharakterisierung!$E$11/$J$20","v":2.914083277946779E-5},{"$f":"((150*($J$2^0.87)*(AB324^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z324)*3600*24","v":5.9910995112762822E-2},2.3915996627248484E-4,{"$f":"AE323-AD324*Bodencharakterisierung!$E$8","v":4.2108271029166672E-2},{"$f":"IF(AE324>$J$18,(AE324/(Bodencharakterisierung!$E$11*1000)),0)","v":2.7794238303080311E-5},2.3305291073371062E-2,307,null,{"$f":"(AD324)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH324>0,(AJ324*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK323,NA())","v":0.6646283674003598},null,307,{"$f":"IF(AF324<=$J$9*0.05,AS323*EXP((-$J$6*1)/Heterogenität!$D$4),Z324)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF324>=$J$19, AR323/$J$5<AN324),0, Bodencharakterisierung!$E$8*$J$11*((AR323/$J$5)-AN324))","v":0},0,{"$f":"AQ323-AP324*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ324/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,307,null,{"$f":"(AP324)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF324<=$J$9*1.05,(AV324*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW323,NA())","v":{"$error":"#N/A"}},23072.238162637354,440,5.9503288474003551,0.6646283674003598,0,1.9257004799999951,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},27.794238303080309,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,308,2.3305291073371062E-2,{"$f":"Z325*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF324*Bodencharakterisierung!$E$11/$J$20","v":2.9086316809458796E-5},{"$f":"((150*($J$2^0.87)*(AB325^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z325)*3600*24","v":5.982243446696324E-2},2.3915996627248484E-4,{"$f":"AE324-AD325*Bodencharakterisierung!$E$8","v":4.2029348240296749E-2},{"$f":"IF(AE325>$J$18,(AE325/(Bodencharakterisierung!$E$11*1000)),0)","v":2.7742144053001156E-5},2.3305291073371062E-2,308,null,{"$f":"(AD325)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH325>0,(AJ325*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK324,NA())","v":0.66679583465573555},null,308,{"$f":"IF(AF325<=$J$9*0.05,AS324*EXP((-$J$6*1)/Heterogenität!$D$4),Z325)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF325>=$J$19, AR324/$J$5<AN325),0, Bodencharakterisierung!$E$8*$J$11*((AR324/$J$5)-AN325))","v":0},0,{"$f":"AQ324-AP325*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ325/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,308,null,{"$f":"(AP325)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF325<=$J$9*1.05,(AV325*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW324,NA())","v":{"$error":"#N/A"}},23072.238162637354,441,5.9587689546557305,0.66679583465573555,0,1.931973119999995,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},27.742144053001155,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,309,2.3305291073371062E-2,{"$f":"Z326*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF325*Bodencharakterisierung!$E$11/$J$20","v":2.9031800839449802E-5},{"$f":"((150*($J$2^0.87)*(AB326^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z326)*3600*24","v":5.9733838956872926E-2},2.3915996627248484E-4,{"$f":"AE325-AD326*Bodencharakterisierung!$E$8","v":4.1950425451426826E-2},{"$f":"IF(AE326>$J$18,(AE326/(Bodencharakterisierung!$E$11*1000)),0)","v":2.7690049802921997E-5},2.3305291073371062E-2,309,null,{"$f":"(AD326)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH326>0,(AJ326*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK325,NA())","v":0.66896330191111131},null,309,{"$f":"IF(AF326<=$J$9*0.05,AS325*EXP((-$J$6*1)/Heterogenität!$D$4),Z326)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF326>=$J$19, AR325/$J$5<AN326),0, Bodencharakterisierung!$E$8*$J$11*((AR325/$J$5)-AN326))","v":0},0,{"$f":"AQ325-AP326*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ326/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,309,null,{"$f":"(AP326)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF326<=$J$9*1.05,(AV326*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW325,NA())","v":{"$error":"#N/A"}},23072.238162637354,442,5.967209061911106,0.66896330191111131,0,1.9382457599999949,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},27.690049802921997,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,310,2.3305291073371062E-2,{"$f":"Z327*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF326*Bodencharakterisierung!$E$11/$J$20","v":2.8977284869440812E-5},{"$f":"((150*($J$2^0.87)*(AB327^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z327)*3600*24","v":5.96452085032593E-2},2.3915996627248484E-4,{"$f":"AE326-AD327*Bodencharakterisierung!$E$8","v":4.1871502662556903E-2},{"$f":"IF(AE327>$J$18,(AE327/(Bodencharakterisierung!$E$11*1000)),0)","v":2.7637955552842842E-5},2.3305291073371062E-2,310,null,{"$f":"(AD327)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH327>0,(AJ327*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK326,NA())","v":0.67113076916648706},null,310,{"$f":"IF(AF327<=$J$9*0.05,AS326*EXP((-$J$6*1)/Heterogenität!$D$4),Z327)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF327>=$J$19, AR326/$J$5<AN327),0, Bodencharakterisierung!$E$8*$J$11*((AR326/$J$5)-AN327))","v":0},0,{"$f":"AQ326-AP327*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ327/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,310,null,{"$f":"(AP327)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF327<=$J$9*1.05,(AV327*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW326,NA())","v":{"$error":"#N/A"}},23072.238162637354,443,5.9756491691664824,0.67113076916648706,0,1.9445183999999949,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},27.637955552842843,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,311,2.3305291073371062E-2,{"$f":"Z328*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF327*Bodencharakterisierung!$E$11/$J$20","v":2.8922768899431818E-5},{"$f":"((150*($J$2^0.87)*(AB328^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z328)*3600*24","v":5.9556543026560924E-2},2.3915996627248484E-4,{"$f":"AE327-AD328*Bodencharakterisierung!$E$8","v":4.179257987368698E-2},{"$f":"IF(AE328>$J$18,(AE328/(Bodencharakterisierung!$E$11*1000)),0)","v":2.7585861302763683E-5},2.3305291073371062E-2,311,null,{"$f":"(AD328)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH328>0,(AJ328*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK327,NA())","v":0.67329823642186282},null,311,{"$f":"IF(AF328<=$J$9*0.05,AS327*EXP((-$J$6*1)/Heterogenität!$D$4),Z328)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF328>=$J$19, AR327/$J$5<AN328),0, Bodencharakterisierung!$E$8*$J$11*((AR327/$J$5)-AN328))","v":0},0,{"$f":"AQ327-AP328*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ328/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,311,null,{"$f":"(AP328)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF328<=$J$9*1.05,(AV328*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW327,NA())","v":{"$error":"#N/A"}},23072.238162637354,444,5.984089276421857,0.67329823642186282,0,1.9507910399999948,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},27.585861302763682,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,312,2.3305291073371062E-2,{"$f":"Z329*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF328*Bodencharakterisierung!$E$11/$J$20","v":2.8868252929422824E-5},{"$f":"((150*($J$2^0.87)*(AB329^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z329)*3600*24","v":5.9467842446884224E-2},2.3915996627248484E-4,{"$f":"AE328-AD329*Bodencharakterisierung!$E$8","v":4.1713657084817057E-2},{"$f":"IF(AE329>$J$18,(AE329/(Bodencharakterisierung!$E$11*1000)),0)","v":2.7533767052684525E-5},2.3305291073371062E-2,312,null,{"$f":"(AD329)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH329>0,(AJ329*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK328,NA())","v":0.67546570367723857},null,312,{"$f":"IF(AF329<=$J$9*0.05,AS328*EXP((-$J$6*1)/Heterogenität!$D$4),Z329)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF329>=$J$19, AR328/$J$5<AN329),0, Bodencharakterisierung!$E$8*$J$11*((AR328/$J$5)-AN329))","v":0},0,{"$f":"AQ328-AP329*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ329/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,312,null,{"$f":"(AP329)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF329<=$J$9*1.05,(AV329*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW328,NA())","v":{"$error":"#N/A"}},23072.238162637354,445,5.9925293836772333,0.67546570367723857,0,1.9570636799999948,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},27.533767052684524,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,313,2.3305291073371062E-2,{"$f":"Z330*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF329*Bodencharakterisierung!$E$11/$J$20","v":2.8813736959413826E-5},{"$f":"((150*($J$2^0.87)*(AB330^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z330)*3600*24","v":5.9379106684002744E-2},2.3915996627248484E-4,{"$f":"AE329-AD330*Bodencharakterisierung!$E$8","v":4.1634734295947134E-2},{"$f":"IF(AE330>$J$18,(AE330/(Bodencharakterisierung!$E$11*1000)),0)","v":2.7481672802605369E-5},2.3305291073371062E-2,313,null,{"$f":"(AD330)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH330>0,(AJ330*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK329,NA())","v":0.67763317093261433},null,313,{"$f":"IF(AF330<=$J$9*0.05,AS329*EXP((-$J$6*1)/Heterogenität!$D$4),Z330)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF330>=$J$19, AR329/$J$5<AN330),0, Bodencharakterisierung!$E$8*$J$11*((AR329/$J$5)-AN330))","v":0},0,{"$f":"AQ329-AP330*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ330/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,313,null,{"$f":"(AP330)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF330<=$J$9*1.05,(AV330*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW329,NA())","v":{"$error":"#N/A"}},23072.238162637354,446,6.0009694909326088,0.67763317093261433,0,1.9633363199999947,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},27.48167280260537,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,314,2.3305291073371062E-2,{"$f":"Z331*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF330*Bodencharakterisierung!$E$11/$J$20","v":2.8759220989404839E-5},{"$f":"((150*($J$2^0.87)*(AB331^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z331)*3600*24","v":5.9290335657354046E-2},2.3915996627248484E-4,{"$f":"AE330-AD331*Bodencharakterisierung!$E$8","v":4.1555811507077212E-2},{"$f":"IF(AE331>$J$18,(AE331/(Bodencharakterisierung!$E$11*1000)),0)","v":2.7429578552526211E-5},2.3305291073371062E-2,314,null,{"$f":"(AD331)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH331>0,(AJ331*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK330,NA())","v":0.67980063818799008},null,314,{"$f":"IF(AF331<=$J$9*0.05,AS330*EXP((-$J$6*1)/Heterogenität!$D$4),Z331)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF331>=$J$19, AR330/$J$5<AN331),0, Bodencharakterisierung!$E$8*$J$11*((AR330/$J$5)-AN331))","v":0},0,{"$f":"AQ330-AP331*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ331/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,314,null,{"$f":"(AP331)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF331<=$J$9*1.05,(AV331*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW330,NA())","v":{"$error":"#N/A"}},23072.238162637354,447,6.0094095981879843,0.67980063818799008,0,1.9696089599999946,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},27.429578552526209,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,315,2.3305291073371062E-2,{"$f":"Z332*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF331*Bodencharakterisierung!$E$11/$J$20","v":2.8704705019395842E-5},{"$f":"((150*($J$2^0.87)*(AB332^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z332)*3600*24","v":5.92015292860383E-2},2.3915996627248484E-4,{"$f":"AE331-AD332*Bodencharakterisierung!$E$8","v":4.1476888718207289E-2},{"$f":"IF(AE332>$J$18,(AE332/(Bodencharakterisierung!$E$11*1000)),0)","v":2.7377484302447056E-5},2.3305291073371062E-2,315,null,{"$f":"(AD332)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH332>0,(AJ332*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK331,NA())","v":0.68196810544336584},null,315,{"$f":"IF(AF332<=$J$9*0.05,AS331*EXP((-$J$6*1)/Heterogenität!$D$4),Z332)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF332>=$J$19, AR331/$J$5<AN332),0, Bodencharakterisierung!$E$8*$J$11*((AR331/$J$5)-AN332))","v":0},0,{"$f":"AQ331-AP332*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ332/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,315,null,{"$f":"(AP332)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF332<=$J$9*1.05,(AV332*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW331,NA())","v":{"$error":"#N/A"}},23072.238162637354,448,6.0178497054433606,0.68196810544336584,0,1.9758815999999946,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},27.377484302447055,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,316,2.3305291073371062E-2,{"$f":"Z333*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF332*Bodencharakterisierung!$E$11/$J$20","v":2.8650189049386851E-5},{"$f":"((150*($J$2^0.87)*(AB333^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z333)*3600*24","v":5.9112687488816068E-2},2.3915996627248484E-4,{"$f":"AE332-AD333*Bodencharakterisierung!$E$8","v":4.1397965929337366E-2},{"$f":"IF(AE333>$J$18,(AE333/(Bodencharakterisierung!$E$11*1000)),0)","v":2.7325390052367897E-5},2.3305291073371062E-2,316,null,{"$f":"(AD333)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH333>0,(AJ333*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK332,NA())","v":0.68413557269874159},null,316,{"$f":"IF(AF333<=$J$9*0.05,AS332*EXP((-$J$6*1)/Heterogenität!$D$4),Z333)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF333>=$J$19, AR332/$J$5<AN333),0, Bodencharakterisierung!$E$8*$J$11*((AR332/$J$5)-AN333))","v":0},0,{"$f":"AQ332-AP333*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ333/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,316,null,{"$f":"(AP333)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF333<=$J$9*1.05,(AV333*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW332,NA())","v":{"$error":"#N/A"}},23072.238162637354,449,6.0262898126987361,0.68413557269874159,0,1.9821542399999945,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},27.325390052367897,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,317,2.3305291073371062E-2,{"$f":"Z334*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF333*Bodencharakterisierung!$E$11/$J$20","v":2.8595673079377854E-5},{"$f":"((150*($J$2^0.87)*(AB334^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z334)*3600*24","v":5.9023810184106143E-2},2.3915996627248484E-4,{"$f":"AE333-AD334*Bodencharakterisierung!$E$8","v":4.1319043140467443E-2},{"$f":"IF(AE334>$J$18,(AE334/(Bodencharakterisierung!$E$11*1000)),0)","v":2.7273295802288742E-5},2.3305291073371062E-2,317,null,{"$f":"(AD334)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH334>0,(AJ334*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK333,NA())","v":0.68630303995411734},null,317,{"$f":"IF(AF334<=$J$9*0.05,AS333*EXP((-$J$6*1)/Heterogenität!$D$4),Z334)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF334>=$J$19, AR333/$J$5<AN334),0, Bodencharakterisierung!$E$8*$J$11*((AR333/$J$5)-AN334))","v":0},0,{"$f":"AQ333-AP334*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ334/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,317,null,{"$f":"(AP334)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF334<=$J$9*1.05,(AV334*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW333,NA())","v":{"$error":"#N/A"}},23072.238162637354,450,6.0347299199541116,0.68630303995411734,0,1.9884268799999945,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},27.273295802288743,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,318,2.3305291073371062E-2,{"$f":"Z335*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF334*Bodencharakterisierung!$E$11/$J$20","v":2.8541157109368866E-5},{"$f":"((150*($J$2^0.87)*(AB335^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z335)*3600*24","v":5.8934897289983704E-2},2.3915996627248484E-4,{"$f":"AE334-AD335*Bodencharakterisierung!$E$8","v":4.124012035159752E-2},{"$f":"IF(AE335>$J$18,(AE335/(Bodencharakterisierung!$E$11*1000)),0)","v":2.7221201552209583E-5},2.3305291073371062E-2,318,null,{"$f":"(AD335)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH335>0,(AJ335*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK334,NA())","v":0.6884705072094931},null,318,{"$f":"IF(AF335<=$J$9*0.05,AS334*EXP((-$J$6*1)/Heterogenität!$D$4),Z335)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF335>=$J$19, AR334/$J$5<AN335),0, Bodencharakterisierung!$E$8*$J$11*((AR334/$J$5)-AN335))","v":0},0,{"$f":"AQ334-AP335*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ335/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,318,null,{"$f":"(AP335)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF335<=$J$9*1.05,(AV335*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW334,NA())","v":{"$error":"#N/A"}},23072.238162637354,451,6.0431700272094879,0.6884705072094931,0,1.9946995199999944,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},27.221201552209582,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,319,2.3305291073371062E-2,{"$f":"Z336*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF335*Bodencharakterisierung!$E$11/$J$20","v":2.8486641139359869E-5},{"$f":"((150*($J$2^0.87)*(AB336^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z336)*3600*24","v":5.8845948724177699E-2},2.3915996627248484E-4,{"$f":"AE335-AD336*Bodencharakterisierung!$E$8","v":4.1161197562727597E-2},{"$f":"IF(AE336>$J$18,(AE336/(Bodencharakterisierung!$E$11*1000)),0)","v":2.7169107302130428E-5},2.3305291073371062E-2,319,null,{"$f":"(AD336)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH336>0,(AJ336*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK335,NA())","v":0.69063797446486885},null,319,{"$f":"IF(AF336<=$J$9*0.05,AS335*EXP((-$J$6*1)/Heterogenität!$D$4),Z336)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF336>=$J$19, AR335/$J$5<AN336),0, Bodencharakterisierung!$E$8*$J$11*((AR335/$J$5)-AN336))","v":0},0,{"$f":"AQ335-AP336*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ336/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,319,null,{"$f":"(AP336)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF336<=$J$9*1.05,(AV336*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW335,NA())","v":{"$error":"#N/A"}},23072.238162637354,452,6.0516101344648634,0.69063797446486885,0,2.0009721599999946,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},27.169107302130428,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,320,2.3305291073371062E-2,{"$f":"Z337*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF336*Bodencharakterisierung!$E$11/$J$20","v":2.8432125169350882E-5},{"$f":"((150*($J$2^0.87)*(AB337^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z337)*3600*24","v":5.8756964404069412E-2},2.3915996627248484E-4,{"$f":"AE336-AD337*Bodencharakterisierung!$E$8","v":4.1082274773857674E-2},{"$f":"IF(AE337>$J$18,(AE337/(Bodencharakterisierung!$E$11*1000)),0)","v":2.7117013052051269E-5},2.3305291073371062E-2,320,null,{"$f":"(AD337)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH337>0,(AJ337*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK336,NA())","v":0.69280544172024461},null,320,{"$f":"IF(AF337<=$J$9*0.05,AS336*EXP((-$J$6*1)/Heterogenität!$D$4),Z337)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF337>=$J$19, AR336/$J$5<AN337),0, Bodencharakterisierung!$E$8*$J$11*((AR336/$J$5)-AN337))","v":0},0,{"$f":"AQ336-AP337*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ337/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,320,null,{"$f":"(AP337)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF337<=$J$9*1.05,(AV337*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW336,NA())","v":{"$error":"#N/A"}},23072.238162637354,453,6.0600502417202389,0.69280544172024461,0,2.0072447999999947,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},27.11701305205127,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,321,2.3305291073371062E-2,{"$f":"Z338*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF337*Bodencharakterisierung!$E$11/$J$20","v":2.8377609199341885E-5},{"$f":"((150*($J$2^0.87)*(AB338^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z338)*3600*24","v":5.8667944246689696E-2},2.3915996627248484E-4,{"$f":"AE337-AD338*Bodencharakterisierung!$E$8","v":4.1003351984987751E-2},{"$f":"IF(AE338>$J$18,(AE338/(Bodencharakterisierung!$E$11*1000)),0)","v":2.7064918801972114E-5},2.3305291073371062E-2,321,null,{"$f":"(AD338)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH338>0,(AJ338*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK337,NA())","v":0.69497290897562036},null,321,{"$f":"IF(AF338<=$J$9*0.05,AS337*EXP((-$J$6*1)/Heterogenität!$D$4),Z338)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF338>=$J$19, AR337/$J$5<AN338),0, Bodencharakterisierung!$E$8*$J$11*((AR337/$J$5)-AN338))","v":0},0,{"$f":"AQ337-AP338*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ338/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,321,null,{"$f":"(AP338)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF338<=$J$9*1.05,(AV338*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW337,NA())","v":{"$error":"#N/A"}},23072.238162637354,454,6.0684903489756152,0.69497290897562036,0,2.0135174399999949,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},27.064918801972112,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,322,2.3305291073371062E-2,{"$f":"Z339*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF338*Bodencharakterisierung!$E$11/$J$20","v":2.8323093229332891E-5},{"$f":"((150*($J$2^0.87)*(AB339^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z339)*3600*24","v":5.8578888168717216E-2},2.3915996627248484E-4,{"$f":"AE338-AD339*Bodencharakterisierung!$E$8","v":4.0924429196117829E-2},{"$f":"IF(AE339>$J$18,(AE339/(Bodencharakterisierung!$E$11*1000)),0)","v":2.7012824551892955E-5},2.3305291073371062E-2,322,null,{"$f":"(AD339)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH339>0,(AJ339*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK338,NA())","v":0.69714037623099612},null,322,{"$f":"IF(AF339<=$J$9*0.05,AS338*EXP((-$J$6*1)/Heterogenität!$D$4),Z339)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF339>=$J$19, AR338/$J$5<AN339),0, Bodencharakterisierung!$E$8*$J$11*((AR338/$J$5)-AN339))","v":0},0,{"$f":"AQ338-AP339*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ339/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,322,null,{"$f":"(AP339)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF339<=$J$9*1.05,(AV339*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW338,NA())","v":{"$error":"#N/A"}},23072.238162637354,455,6.0769304562309916,0.69714037623099612,0,2.019790079999995,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},27.012824551892955,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,323,2.3305291073371062E-2,{"$f":"Z340*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF339*Bodencharakterisierung!$E$11/$J$20","v":2.8268577259323897E-5},{"$f":"((150*($J$2^0.87)*(AB340^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z340)*3600*24","v":5.8489796086476233E-2},2.3915996627248484E-4,{"$f":"AE339-AD340*Bodencharakterisierung!$E$8","v":4.0845506407247906E-2},{"$f":"IF(AE340>$J$18,(AE340/(Bodencharakterisierung!$E$11*1000)),0)","v":2.69607303018138E-5},2.3305291073371062E-2,323,null,{"$f":"(AD340)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH340>0,(AJ340*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK339,NA())","v":0.69930784348637187},null,323,{"$f":"IF(AF340<=$J$9*0.05,AS339*EXP((-$J$6*1)/Heterogenität!$D$4),Z340)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF340>=$J$19, AR339/$J$5<AN340),0, Bodencharakterisierung!$E$8*$J$11*((AR339/$J$5)-AN340))","v":0},0,{"$f":"AQ339-AP340*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ340/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,323,null,{"$f":"(AP340)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF340<=$J$9*1.05,(AV340*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW339,NA())","v":{"$error":"#N/A"}},23072.238162637354,456,6.0853705634863671,0.69930784348637187,0,{"$f":"$G$34/$G$12/$G$8+BC339","v":2.0260627199999952},null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},26.9607303018138,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,324,2.3305291073371062E-2,{"$f":"Z341*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF340*Bodencharakterisierung!$E$11/$J$20","v":2.8214061289314903E-5},{"$f":"((150*($J$2^0.87)*(AB341^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z341)*3600*24","v":5.8400667915934054E-2},2.3915996627248484E-4,{"$f":"AE340-AD341*Bodencharakterisierung!$E$8","v":4.0766583618377983E-2},{"$f":"IF(AE341>$J$18,(AE341/(Bodencharakterisierung!$E$11*1000)),0)","v":2.6908636051734642E-5},2.3305291073371062E-2,324,null,{"$f":"(AD341)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH341>0,(AJ341*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK340,NA())","v":0.70147531074174763},null,324,{"$f":"IF(AF341<=$J$9*0.05,AS340*EXP((-$J$6*1)/Heterogenität!$D$4),Z341)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF341>=$J$19, AR340/$J$5<AN341),0, Bodencharakterisierung!$E$8*$J$11*((AR340/$J$5)-AN341))","v":0},0,{"$f":"AQ340-AP341*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ341/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,324,null,{"$f":"(AP341)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF341<=$J$9*1.05,(AV341*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW340,NA())","v":{"$error":"#N/A"}},23072.238162637354,457,6.0938106707417425,0.70147531074174763,0,2.0323353599999954,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},26.908636051734643,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,325,2.3305291073371062E-2,{"$f":"Z342*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF341*Bodencharakterisierung!$E$11/$J$20","v":2.8159545319305912E-5},{"$f":"((150*($J$2^0.87)*(AB342^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z342)*3600*24","v":5.8311503572699111E-2},2.3915996627248484E-4,{"$f":"AE341-AD342*Bodencharakterisierung!$E$8","v":4.068766082950806E-2},{"$f":"IF(AE342>$J$18,(AE342/(Bodencharakterisierung!$E$11*1000)),0)","v":2.6856541801655486E-5},2.3305291073371062E-2,325,null,{"$f":"(AD342)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH342>0,(AJ342*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK341,NA())","v":0.70364277799712338},null,325,{"$f":"IF(AF342<=$J$9*0.05,AS341*EXP((-$J$6*1)/Heterogenität!$D$4),Z342)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF342>=$J$19, AR341/$J$5<AN342),0, Bodencharakterisierung!$E$8*$J$11*((AR341/$J$5)-AN342))","v":0},0,{"$f":"AQ341-AP342*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ342/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,325,null,{"$f":"(AP342)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF342<=$J$9*1.05,(AV342*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW341,NA())","v":{"$error":"#N/A"}},23072.238162637354,458,6.1022507779971189,0.70364277799712338,0,2.0386079999999955,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},26.856541801655485,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,326,{"$f":"AG342","v":2.3305291073371062E-2},{"$f":"Z343*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF342*Bodencharakterisierung!$E$11/$J$20","v":2.8105029349296918E-5},{"$f":"((150*($J$2^0.87)*(AB343^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z343)*3600*24","v":5.8222302972018899E-2},{"$f":"MIN(AC343,Z343-AA343)","v":2.3915996627248484E-4},{"$f":"AE342-AD343*Bodencharakterisierung!$E$8","v":4.0608738040638137E-2},{"$f":"IF(AE343>$J$18,(AE343/(Bodencharakterisierung!$E$11*1000)),0)","v":2.6804447551576328E-5},{"$f":"AA343+AD343","v":2.3305291073371062E-2},{"$f":"IF(AD343>0,Y343,NA())","v":326},null,{"$f":"(AD343)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH343>0,(AJ343*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK342,NA())","v":0.70581024525249914},null,326,{"$f":"IF(AF343<=$J$9*0.05,AS342*EXP((-$J$6*1)/Heterogenität!$D$4),Z343)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF343>=$J$19, AR342/$J$5<AN343),0, Bodencharakterisierung!$E$8*$J$11*((AR342/$J$5)-AN343))","v":0},{"$f":"MIN(AO343,AS342-AN343)","v":0},{"$f":"AQ342-AP343*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ343/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},{"$f":"AN343+AP343","v":2.3305291073371062E-2},{"$f":"IF(AN343>$G$5,AM343,NA())","v":326},null,{"$f":"(AP343)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF343<=$J$9*1.05,(AV343*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW342,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH343>($G$5*10^6),BH343*0.99,9999)","v":23072.238162637354},{"$f":"AT343+$G$3","v":459},{"$f":"IF(ISNUMBER(AT343),BA343+BB343+BC343+$AZ$17,\"\")","v":6.1106908852524953},{"$f":"IF(ISNUMBER(AK343),AK343,BA342)","v":0.70581024525249914},{"$f":"IF(ISNUMBER(AW343),AW343,0)","v":0},2.0448806399999957,null,{"$f":"AR343*10^6","v":4.3827000000643475},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF343*10^6","v":26.804447551576327},{"$f":"AN343*10^6","v":23305.291073371063}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,327,2.3305291073371062E-2,{"$f":"Z344*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF343*Bodencharakterisierung!$E$11/$J$20","v":2.8050513379287924E-5},{"$f":"((150*($J$2^0.87)*(AB344^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z344)*3600*24","v":5.8133066028777491E-2},2.3915996627248484E-4,{"$f":"AE343-AD344*Bodencharakterisierung!$E$8","v":4.0529815251768214E-2},{"$f":"IF(AE344>$J$18,(AE344/(Bodencharakterisierung!$E$11*1000)),0)","v":2.6752353301497173E-5},2.3305291073371062E-2,327,null,{"$f":"(AD344)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH344>0,(AJ344*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK343,NA())","v":0.70797771250787489},null,327,{"$f":"IF(AF344<=$J$9*0.05,AS343*EXP((-$J$6*1)/Heterogenität!$D$4),Z344)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF344>=$J$19, AR343/$J$5<AN344),0, Bodencharakterisierung!$E$8*$J$11*((AR343/$J$5)-AN344))","v":0},0,{"$f":"AQ343-AP344*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ344/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,327,null,{"$f":"(AP344)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF344<=$J$9*1.05,(AV344*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW343,NA())","v":{"$error":"#N/A"}},23072.238162637354,460,6.1191309925078707,0.70797771250787489,0,2.0511532799999959,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},26.752353301497173,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,328,2.3305291073371062E-2,{"$f":"Z345*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF344*Bodencharakterisierung!$E$11/$J$20","v":2.7995997409278933E-5},{"$f":"((150*($J$2^0.87)*(AB345^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z345)*3600*24","v":5.8043792657493036E-2},2.3915996627248484E-4,{"$f":"AE344-AD345*Bodencharakterisierung!$E$8","v":4.0450892462898291E-2},{"$f":"IF(AE345>$J$18,(AE345/(Bodencharakterisierung!$E$11*1000)),0)","v":2.6700259051418014E-5},2.3305291073371062E-2,328,null,{"$f":"(AD345)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH345>0,(AJ345*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK344,NA())","v":0.71014517976325064},null,328,{"$f":"IF(AF345<=$J$9*0.05,AS344*EXP((-$J$6*1)/Heterogenität!$D$4),Z345)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF345>=$J$19, AR344/$J$5<AN345),0, Bodencharakterisierung!$E$8*$J$11*((AR344/$J$5)-AN345))","v":0},0,{"$f":"AQ344-AP345*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ345/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,328,null,{"$f":"(AP345)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF345<=$J$9*1.05,(AV345*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW344,NA())","v":{"$error":"#N/A"}},23072.238162637354,461,6.1275710997632462,0.71014517976325064,0,2.057425919999996,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},26.700259051418016,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,329,2.3305291073371062E-2,{"$f":"Z346*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF345*Bodencharakterisierung!$E$11/$J$20","v":2.7941481439269939E-5},{"$f":"((150*($J$2^0.87)*(AB346^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z346)*3600*24","v":5.7954482772315977E-2},2.3915996627248484E-4,{"$f":"AE345-AD346*Bodencharakterisierung!$E$8","v":4.0371969674028368E-2},{"$f":"IF(AE346>$J$18,(AE346/(Bodencharakterisierung!$E$11*1000)),0)","v":2.6648164801338859E-5},2.3305291073371062E-2,329,null,{"$f":"(AD346)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH346>0,(AJ346*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK345,NA())","v":0.7123126470186264},null,329,{"$f":"IF(AF346<=$J$9*0.05,AS345*EXP((-$J$6*1)/Heterogenität!$D$4),Z346)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF346>=$J$19, AR345/$J$5<AN346),0, Bodencharakterisierung!$E$8*$J$11*((AR345/$J$5)-AN346))","v":0},0,{"$f":"AQ345-AP346*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ346/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,329,null,{"$f":"(AP346)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF346<=$J$9*1.05,(AV346*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW345,NA())","v":{"$error":"#N/A"}},23072.238162637354,462,6.1360112070186226,0.7123126470186264,0,2.0636985599999962,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},26.648164801338858,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,330,2.3305291073371062E-2,{"$f":"Z347*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF346*Bodencharakterisierung!$E$11/$J$20","v":2.7886965469260945E-5},{"$f":"((150*($J$2^0.87)*(AB347^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z347)*3600*24","v":5.7865136287026532E-2},2.3915996627248484E-4,{"$f":"AE346-AD347*Bodencharakterisierung!$E$8","v":4.0293046885158446E-2},{"$f":"IF(AE347>$J$18,(AE347/(Bodencharakterisierung!$E$11*1000)),0)","v":2.65960705512597E-5},2.3305291073371062E-2,330,null,{"$f":"(AD347)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH347>0,(AJ347*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK346,NA())","v":0.71448011427400215},null,330,{"$f":"IF(AF347<=$J$9*0.05,AS346*EXP((-$J$6*1)/Heterogenität!$D$4),Z347)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF347>=$J$19, AR346/$J$5<AN347),0, Bodencharakterisierung!$E$8*$J$11*((AR346/$J$5)-AN347))","v":0},0,{"$f":"AQ346-AP347*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ347/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,330,null,{"$f":"(AP347)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF347<=$J$9*1.05,(AV347*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW346,NA())","v":{"$error":"#N/A"}},23072.238162637354,463,6.1444513142739989,0.71448011427400215,0,2.0699711999999963,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},26.5960705512597,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,331,2.3305291073371062E-2,{"$f":"Z348*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF347*Bodencharakterisierung!$E$11/$J$20","v":2.7832449499251955E-5},{"$f":"((150*($J$2^0.87)*(AB348^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z348)*3600*24","v":5.7775753115032122E-2},2.3915996627248484E-4,{"$f":"AE347-AD348*Bodencharakterisierung!$E$8","v":4.0214124096288523E-2},{"$f":"IF(AE348>$J$18,(AE348/(Bodencharakterisierung!$E$11*1000)),0)","v":2.6543976301180541E-5},2.3305291073371062E-2,331,null,{"$f":"(AD348)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH348>0,(AJ348*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK347,NA())","v":0.71664758152937791},null,331,{"$f":"IF(AF348<=$J$9*0.05,AS347*EXP((-$J$6*1)/Heterogenität!$D$4),Z348)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF348>=$J$19, AR347/$J$5<AN348),0, Bodencharakterisierung!$E$8*$J$11*((AR347/$J$5)-AN348))","v":0},0,{"$f":"AQ347-AP348*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ348/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,331,null,{"$f":"(AP348)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF348<=$J$9*1.05,(AV348*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW347,NA())","v":{"$error":"#N/A"}},23072.238162637354,464,6.1528914215293744,0.71664758152937791,0,2.0762438399999965,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},26.543976301180543,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,332,2.3305291073371062E-2,{"$f":"Z349*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF348*Bodencharakterisierung!$E$11/$J$20","v":2.7777933529242961E-5},{"$f":"((150*($J$2^0.87)*(AB349^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z349)*3600*24","v":5.7686333169365542E-2},2.3915996627248484E-4,{"$f":"AE348-AD349*Bodencharakterisierung!$E$8","v":4.01352013074186E-2},{"$f":"IF(AE349>$J$18,(AE349/(Bodencharakterisierung!$E$11*1000)),0)","v":2.6491882051101386E-5},2.3305291073371062E-2,332,null,{"$f":"(AD349)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH349>0,(AJ349*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK348,NA())","v":0.71881504878475366},null,332,{"$f":"IF(AF349<=$J$9*0.05,AS348*EXP((-$J$6*1)/Heterogenität!$D$4),Z349)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF349>=$J$19, AR348/$J$5<AN349),0, Bodencharakterisierung!$E$8*$J$11*((AR348/$J$5)-AN349))","v":0},0,{"$f":"AQ348-AP349*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ349/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,332,null,{"$f":"(AP349)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF349<=$J$9*1.05,(AV349*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW348,NA())","v":{"$error":"#N/A"}},23072.238162637354,465,6.1613315287847499,0.71881504878475366,0,2.0825164799999967,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},26.491882051101385,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,333,2.3305291073371062E-2,{"$f":"Z350*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF349*Bodencharakterisierung!$E$11/$J$20","v":2.7723417559233967E-5},{"$f":"((150*($J$2^0.87)*(AB350^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z350)*3600*24","v":5.7596876362682001E-2},2.3915996627248484E-4,{"$f":"AE349-AD350*Bodencharakterisierung!$E$8","v":4.0056278518548677E-2},{"$f":"IF(AE350>$J$18,(AE350/(Bodencharakterisierung!$E$11*1000)),0)","v":2.6439787801022228E-5},2.3305291073371062E-2,333,null,{"$f":"(AD350)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH350>0,(AJ350*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK349,NA())","v":0.72098251604012942},null,333,{"$f":"IF(AF350<=$J$9*0.05,AS349*EXP((-$J$6*1)/Heterogenität!$D$4),Z350)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF350>=$J$19, AR349/$J$5<AN350),0, Bodencharakterisierung!$E$8*$J$11*((AR349/$J$5)-AN350))","v":0},0,{"$f":"AQ349-AP350*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ350/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,333,null,{"$f":"(AP350)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF350<=$J$9*1.05,(AV350*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW349,NA())","v":{"$error":"#N/A"}},23072.238162637354,466,6.1697716360401262,0.72098251604012942,0,2.0887891199999968,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},26.439787801022227,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,334,2.3305291073371062E-2,{"$f":"Z351*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF350*Bodencharakterisierung!$E$11/$J$20","v":2.7668901589224973E-5},{"$f":"((150*($J$2^0.87)*(AB351^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z351)*3600*24","v":5.7507382607257268E-2},2.3915996627248484E-4,{"$f":"AE350-AD351*Bodencharakterisierung!$E$8","v":3.9977355729678754E-2},{"$f":"IF(AE351>$J$18,(AE351/(Bodencharakterisierung!$E$11*1000)),0)","v":2.6387693550943072E-5},2.3305291073371062E-2,334,null,{"$f":"(AD351)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH351>0,(AJ351*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK350,NA())","v":0.72314998329550517},null,334,{"$f":"IF(AF351<=$J$9*0.05,AS350*EXP((-$J$6*1)/Heterogenität!$D$4),Z351)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF351>=$J$19, AR350/$J$5<AN351),0, Bodencharakterisierung!$E$8*$J$11*((AR350/$J$5)-AN351))","v":0},0,{"$f":"AQ350-AP351*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ351/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,334,null,{"$f":"(AP351)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF351<=$J$9*1.05,(AV351*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW350,NA())","v":{"$error":"#N/A"}},23072.238162637354,467,6.1782117432955026,0.72314998329550517,0,2.095061759999997,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},26.387693550943073,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,335,2.3305291073371062E-2,{"$f":"Z352*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF351*Bodencharakterisierung!$E$11/$J$20","v":2.7614385619215982E-5},{"$f":"((150*($J$2^0.87)*(AB352^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z352)*3600*24","v":5.7417851814985182E-2},2.3915996627248484E-4,{"$f":"AE351-AD352*Bodencharakterisierung!$E$8","v":3.9898432940808831E-2},{"$f":"IF(AE352>$J$18,(AE352/(Bodencharakterisierung!$E$11*1000)),0)","v":2.6335599300863914E-5},2.3305291073371062E-2,335,null,{"$f":"(AD352)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH352>0,(AJ352*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK351,NA())","v":0.72531745055088093},null,335,{"$f":"IF(AF352<=$J$9*0.05,AS351*EXP((-$J$6*1)/Heterogenität!$D$4),Z352)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF352>=$J$19, AR351/$J$5<AN352),0, Bodencharakterisierung!$E$8*$J$11*((AR351/$J$5)-AN352))","v":0},0,{"$f":"AQ351-AP352*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ352/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,335,null,{"$f":"(AP352)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF352<=$J$9*1.05,(AV352*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW351,NA())","v":{"$error":"#N/A"}},23072.238162637354,468,6.1866518505508781,0.72531745055088093,0,2.1013343999999972,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},26.335599300863915,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,336,2.3305291073371062E-2,{"$f":"Z353*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF352*Bodencharakterisierung!$E$11/$J$20","v":2.7559869649206985E-5},{"$f":"((150*($J$2^0.87)*(AB353^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z353)*3600*24","v":5.7328283897374481E-2},2.3915996627248484E-4,{"$f":"AE352-AD353*Bodencharakterisierung!$E$8","v":3.9819510151938908E-2},{"$f":"IF(AE353>$J$18,(AE353/(Bodencharakterisierung!$E$11*1000)),0)","v":2.6283505050784759E-5},2.3305291073371062E-2,336,null,{"$f":"(AD353)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH353>0,(AJ353*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK352,NA())","v":0.72748491780625668},null,336,{"$f":"IF(AF353<=$J$9*0.05,AS352*EXP((-$J$6*1)/Heterogenität!$D$4),Z353)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF353>=$J$19, AR352/$J$5<AN353),0, Bodencharakterisierung!$E$8*$J$11*((AR352/$J$5)-AN353))","v":0},0,{"$f":"AQ352-AP353*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ353/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,336,null,{"$f":"(AP353)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF353<=$J$9*1.05,(AV353*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW352,NA())","v":{"$error":"#N/A"}},23072.238162637354,469,6.1950919578062535,0.72748491780625668,0,2.1076070399999973,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},26.283505050784758,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,337,2.3305291073371062E-2,{"$f":"Z354*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF353*Bodencharakterisierung!$E$11/$J$20","v":2.7505353679197994E-5},{"$f":"((150*($J$2^0.87)*(AB354^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z354)*3600*24","v":5.7238678765547737E-2},2.3915996627248484E-4,{"$f":"AE353-AD354*Bodencharakterisierung!$E$8","v":3.9740587363068985E-2},{"$f":"IF(AE354>$J$18,(AE354/(Bodencharakterisierung!$E$11*1000)),0)","v":2.62314108007056E-5},2.3305291073371062E-2,337,null,{"$f":"(AD354)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH354>0,(AJ354*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK353,NA())","v":0.72965238506163244},null,337,{"$f":"IF(AF354<=$J$9*0.05,AS353*EXP((-$J$6*1)/Heterogenität!$D$4),Z354)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF354>=$J$19, AR353/$J$5<AN354),0, Bodencharakterisierung!$E$8*$J$11*((AR353/$J$5)-AN354))","v":0},0,{"$f":"AQ353-AP354*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ354/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,337,null,{"$f":"(AP354)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF354<=$J$9*1.05,(AV354*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW353,NA())","v":{"$error":"#N/A"}},23072.238162637354,470,6.2035320650616299,0.72965238506163244,0,2.1138796799999975,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},26.2314108007056,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,338,2.3305291073371062E-2,{"$f":"Z355*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF354*Bodencharakterisierung!$E$11/$J$20","v":2.7450837709188997E-5},{"$f":"((150*($J$2^0.87)*(AB355^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z355)*3600*24","v":5.7149036330237712E-2},2.3915996627248484E-4,{"$f":"AE354-AD355*Bodencharakterisierung!$E$8","v":3.9661664574199063E-2},{"$f":"IF(AE355>$J$18,(AE355/(Bodencharakterisierung!$E$11*1000)),0)","v":2.6179316550626445E-5},2.3305291073371062E-2,338,null,{"$f":"(AD355)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH355>0,(AJ355*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK354,NA())","v":0.73181985231700819},null,338,{"$f":"IF(AF355<=$J$9*0.05,AS354*EXP((-$J$6*1)/Heterogenität!$D$4),Z355)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF355>=$J$19, AR354/$J$5<AN355),0, Bodencharakterisierung!$E$8*$J$11*((AR354/$J$5)-AN355))","v":0},0,{"$f":"AQ354-AP355*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ355/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,338,null,{"$f":"(AP355)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF355<=$J$9*1.05,(AV355*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW354,NA())","v":{"$error":"#N/A"}},23072.238162637354,471,6.2119721723170063,0.73181985231700819,0,2.1201523199999976,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},26.179316550626446,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,339,2.3305291073371062E-2,{"$f":"Z356*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF355*Bodencharakterisierung!$E$11/$J$20","v":2.739632173918001E-5},{"$f":"((150*($J$2^0.87)*(AB356^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z356)*3600*24","v":5.7059356501785286E-2},2.3915996627248484E-4,{"$f":"AE355-AD356*Bodencharakterisierung!$E$8","v":3.958274178532914E-2},{"$f":"IF(AE356>$J$18,(AE356/(Bodencharakterisierung!$E$11*1000)),0)","v":2.6127222300547286E-5},2.3305291073371062E-2,339,null,{"$f":"(AD356)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH356>0,(AJ356*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK355,NA())","v":0.73398731957238394},null,339,{"$f":"IF(AF356<=$J$9*0.05,AS355*EXP((-$J$6*1)/Heterogenität!$D$4),Z356)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF356>=$J$19, AR355/$J$5<AN356),0, Bodencharakterisierung!$E$8*$J$11*((AR355/$J$5)-AN356))","v":0},0,{"$f":"AQ355-AP356*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ356/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,339,null,{"$f":"(AP356)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF356<=$J$9*1.05,(AV356*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW355,NA())","v":{"$error":"#N/A"}},23072.238162637354,472,6.2204122795723817,0.73398731957238394,0,2.1264249599999978,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},26.127222300547285,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,340,2.3305291073371062E-2,{"$f":"Z357*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF356*Bodencharakterisierung!$E$11/$J$20","v":2.7341805769171012E-5},{"$f":"((150*($J$2^0.87)*(AB357^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z357)*3600*24","v":5.6969639190137158E-2},2.3915996627248484E-4,{"$f":"AE356-AD357*Bodencharakterisierung!$E$8","v":3.9503818996459217E-2},{"$f":"IF(AE357>$J$18,(AE357/(Bodencharakterisierung!$E$11*1000)),0)","v":2.6075128050468131E-5},2.3305291073371062E-2,340,null,{"$f":"(AD357)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH357>0,(AJ357*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK356,NA())","v":0.7361547868277597},null,340,{"$f":"IF(AF357<=$J$9*0.05,AS356*EXP((-$J$6*1)/Heterogenität!$D$4),Z357)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF357>=$J$19, AR356/$J$5<AN357),0, Bodencharakterisierung!$E$8*$J$11*((AR356/$J$5)-AN357))","v":0},0,{"$f":"AQ356-AP357*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ357/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,340,null,{"$f":"(AP357)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF357<=$J$9*1.05,(AV357*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW356,NA())","v":{"$error":"#N/A"}},23072.238162637354,473,6.2288523868277572,0.7361547868277597,0,2.132697599999998,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},26.07512805046813,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,341,2.3305291073371062E-2,{"$f":"Z358*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF357*Bodencharakterisierung!$E$11/$J$20","v":2.7287289799162025E-5},{"$f":"((150*($J$2^0.87)*(AB358^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z358)*3600*24","v":5.6879884304842906E-2},2.3915996627248484E-4,{"$f":"AE357-AD358*Bodencharakterisierung!$E$8","v":3.9424896207589294E-2},{"$f":"IF(AE358>$J$18,(AE358/(Bodencharakterisierung!$E$11*1000)),0)","v":2.6023033800388972E-5},2.3305291073371062E-2,341,null,{"$f":"(AD358)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH358>0,(AJ358*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK357,NA())","v":0.73832225408313545},null,341,{"$f":"IF(AF358<=$J$9*0.05,AS357*EXP((-$J$6*1)/Heterogenität!$D$4),Z358)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF358>=$J$19, AR357/$J$5<AN358),0, Bodencharakterisierung!$E$8*$J$11*((AR357/$J$5)-AN358))","v":0},0,{"$f":"AQ357-AP358*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ358/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,341,null,{"$f":"(AP358)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF358<=$J$9*1.05,(AV358*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW357,NA())","v":{"$error":"#N/A"}},23072.238162637354,474,6.2372924940831336,0.73832225408313545,0,2.1389702399999981,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},26.023033800388973,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,342,2.3305291073371062E-2,{"$f":"Z359*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF358*Bodencharakterisierung!$E$11/$J$20","v":2.7232773829153024E-5},{"$f":"((150*($J$2^0.87)*(AB359^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z359)*3600*24","v":5.6790091755052938E-2},2.3915996627248484E-4,{"$f":"AE358-AD359*Bodencharakterisierung!$E$8","v":3.9345973418719371E-2},{"$f":"IF(AE359>$J$18,(AE359/(Bodencharakterisierung!$E$11*1000)),0)","v":2.5970939550309817E-5},2.3305291073371062E-2,342,null,{"$f":"(AD359)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH359>0,(AJ359*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK358,NA())","v":0.74048972133851121},null,342,{"$f":"IF(AF359<=$J$9*0.05,AS358*EXP((-$J$6*1)/Heterogenität!$D$4),Z359)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF359>=$J$19, AR358/$J$5<AN359),0, Bodencharakterisierung!$E$8*$J$11*((AR358/$J$5)-AN359))","v":0},0,{"$f":"AQ358-AP359*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ359/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,342,null,{"$f":"(AP359)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF359<=$J$9*1.05,(AV359*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW358,NA())","v":{"$error":"#N/A"}},23072.238162637354,475,6.2457326013385099,0.74048972133851121,0,2.1452428799999983,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},25.970939550309819,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,343,2.3305291073371062E-2,{"$f":"Z360*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF359*Bodencharakterisierung!$E$11/$J$20","v":2.7178257859144037E-5},{"$f":"((150*($J$2^0.87)*(AB360^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z360)*3600*24","v":5.670026144951551E-2},2.3915996627248484E-4,{"$f":"AE359-AD360*Bodencharakterisierung!$E$8","v":3.9267050629849448E-2},{"$f":"IF(AE360>$J$18,(AE360/(Bodencharakterisierung!$E$11*1000)),0)","v":2.5918845300230658E-5},2.3305291073371062E-2,343,null,{"$f":"(AD360)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH360>0,(AJ360*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK359,NA())","v":0.74265718859388696},null,343,{"$f":"IF(AF360<=$J$9*0.05,AS359*EXP((-$J$6*1)/Heterogenität!$D$4),Z360)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF360>=$J$19, AR359/$J$5<AN360),0, Bodencharakterisierung!$E$8*$J$11*((AR359/$J$5)-AN360))","v":0},0,{"$f":"AQ359-AP360*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ360/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,343,null,{"$f":"(AP360)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF360<=$J$9*1.05,(AV360*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW359,NA())","v":{"$error":"#N/A"}},23072.238162637354,476,6.2541727085938854,0.74265718859388696,0,2.1515155199999985,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},25.918845300230657,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,344,2.3305291073371062E-2,{"$f":"Z361*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF360*Bodencharakterisierung!$E$11/$J$20","v":2.712374188913504E-5},{"$f":"((150*($J$2^0.87)*(AB361^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z361)*3600*24","v":5.6610393296573983E-2},2.3915996627248484E-4,{"$f":"AE360-AD361*Bodencharakterisierung!$E$8","v":3.9188127840979525E-2},{"$f":"IF(AE361>$J$18,(AE361/(Bodencharakterisierung!$E$11*1000)),0)","v":2.5866751050151503E-5},2.3305291073371062E-2,344,null,{"$f":"(AD361)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH361>0,(AJ361*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK360,NA())","v":0.74482465584926272},null,344,{"$f":"IF(AF361<=$J$9*0.05,AS360*EXP((-$J$6*1)/Heterogenität!$D$4),Z361)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF361>=$J$19, AR360/$J$5<AN361),0, Bodencharakterisierung!$E$8*$J$11*((AR360/$J$5)-AN361))","v":0},0,{"$f":"AQ360-AP361*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ361/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,344,null,{"$f":"(AP361)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF361<=$J$9*1.05,(AV361*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW360,NA())","v":{"$error":"#N/A"}},23072.238162637354,477,6.2626128158492609,0.74482465584926272,0,2.1577881599999986,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},25.866751050151503,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,345,2.3305291073371062E-2,{"$f":"Z362*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF361*Bodencharakterisierung!$E$11/$J$20","v":2.7069225919126053E-5},{"$f":"((150*($J$2^0.87)*(AB362^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z362)*3600*24","v":5.6520487204164936E-2},2.3915996627248484E-4,{"$f":"AE361-AD362*Bodencharakterisierung!$E$8","v":3.9109205052109602E-2},{"$f":"IF(AE362>$J$18,(AE362/(Bodencharakterisierung!$E$11*1000)),0)","v":2.5814656800072345E-5},2.3305291073371062E-2,345,null,{"$f":"(AD362)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH362>0,(AJ362*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK361,NA())","v":0.74699212310463847},null,345,{"$f":"IF(AF362<=$J$9*0.05,AS361*EXP((-$J$6*1)/Heterogenität!$D$4),Z362)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF362>=$J$19, AR361/$J$5<AN362),0, Bodencharakterisierung!$E$8*$J$11*((AR361/$J$5)-AN362))","v":0},0,{"$f":"AQ361-AP362*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ362/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,345,null,{"$f":"(AP362)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF362<=$J$9*1.05,(AV362*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW361,NA())","v":{"$error":"#N/A"}},23072.238162637354,478,6.2710529231046372,0.74699212310463847,0,2.1640607999999988,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},25.814656800072346,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,346,2.3305291073371062E-2,{"$f":"Z363*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF362*Bodencharakterisierung!$E$11/$J$20","v":2.7014709949117055E-5},{"$f":"((150*($J$2^0.87)*(AB363^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z363)*3600*24","v":5.6430543079815015E-2},2.3915996627248484E-4,{"$f":"AE362-AD363*Bodencharakterisierung!$E$8","v":3.903028226323968E-2},{"$f":"IF(AE363>$J$18,(AE363/(Bodencharakterisierung!$E$11*1000)),0)","v":2.5762562549993189E-5},2.3305291073371062E-2,346,null,{"$f":"(AD363)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH363>0,(AJ363*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK362,NA())","v":0.74915959036001423},null,346,{"$f":"IF(AF363<=$J$9*0.05,AS362*EXP((-$J$6*1)/Heterogenität!$D$4),Z363)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF363>=$J$19, AR362/$J$5<AN363),0, Bodencharakterisierung!$E$8*$J$11*((AR362/$J$5)-AN363))","v":0},0,{"$f":"AQ362-AP363*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ363/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,346,null,{"$f":"(AP363)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF363<=$J$9*1.05,(AV363*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW362,NA())","v":{"$error":"#N/A"}},23072.238162637354,479,6.2794930303600136,0.74915959036001423,0,2.1703334399999989,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},25.762562549993188,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,347,2.3305291073371062E-2,{"$f":"Z364*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF363*Bodencharakterisierung!$E$11/$J$20","v":2.6960193979108065E-5},{"$f":"((150*($J$2^0.87)*(AB364^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z364)*3600*24","v":5.6340560830638306E-2},2.3915996627248484E-4,{"$f":"AE363-AD364*Bodencharakterisierung!$E$8","v":3.8951359474369757E-2},{"$f":"IF(AE364>$J$18,(AE364/(Bodencharakterisierung!$E$11*1000)),0)","v":2.5710468299914031E-5},2.3305291073371062E-2,347,null,{"$f":"(AD364)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH364>0,(AJ364*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK363,NA())","v":0.75132705761538998},null,347,{"$f":"IF(AF364<=$J$9*0.05,AS363*EXP((-$J$6*1)/Heterogenität!$D$4),Z364)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF364>=$J$19, AR363/$J$5<AN364),0, Bodencharakterisierung!$E$8*$J$11*((AR363/$J$5)-AN364))","v":0},0,{"$f":"AQ363-AP364*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ364/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,347,null,{"$f":"(AP364)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF364<=$J$9*1.05,(AV364*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW363,NA())","v":{"$error":"#N/A"}},23072.238162637354,480,6.2879331376153891,0.75132705761538998,0,2.1766060799999991,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},25.71046829991403,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,348,2.3305291073371062E-2,{"$f":"Z365*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF364*Bodencharakterisierung!$E$11/$J$20","v":2.6905678009099067E-5},{"$f":"((150*($J$2^0.87)*(AB365^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z365)*3600*24","v":5.625054036333365E-2},2.3915996627248484E-4,{"$f":"AE364-AD365*Bodencharakterisierung!$E$8","v":3.8872436685499834E-2},{"$f":"IF(AE365>$J$18,(AE365/(Bodencharakterisierung!$E$11*1000)),0)","v":2.5658374049834872E-5},2.3305291073371062E-2,348,null,{"$f":"(AD365)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH365>0,(AJ365*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK364,NA())","v":0.75349452487076574},null,348,{"$f":"IF(AF365<=$J$9*0.05,AS364*EXP((-$J$6*1)/Heterogenität!$D$4),Z365)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF365>=$J$19, AR364/$J$5<AN365),0, Bodencharakterisierung!$E$8*$J$11*((AR364/$J$5)-AN365))","v":0},0,{"$f":"AQ364-AP365*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ365/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,348,null,{"$f":"(AP365)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF365<=$J$9*1.05,(AV365*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW364,NA())","v":{"$error":"#N/A"}},23072.238162637354,481,6.2963732448707646,0.75349452487076574,0,2.1828787199999993,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},25.658374049834872,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,349,2.3305291073371062E-2,{"$f":"Z366*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF365*Bodencharakterisierung!$E$11/$J$20","v":2.6851162039090077E-5},{"$f":"((150*($J$2^0.87)*(AB366^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z366)*3600*24","v":5.6160481584181923E-2},2.3915996627248484E-4,{"$f":"AE365-AD366*Bodencharakterisierung!$E$8","v":3.8793513896629911E-2},{"$f":"IF(AE366>$J$18,(AE366/(Bodencharakterisierung!$E$11*1000)),0)","v":2.5606279799755717E-5},2.3305291073371062E-2,349,null,{"$f":"(AD366)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH366>0,(AJ366*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK365,NA())","v":0.75566199212614149},null,349,{"$f":"IF(AF366<=$J$9*0.05,AS365*EXP((-$J$6*1)/Heterogenität!$D$4),Z366)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF366>=$J$19, AR365/$J$5<AN366),0, Bodencharakterisierung!$E$8*$J$11*((AR365/$J$5)-AN366))","v":0},0,{"$f":"AQ365-AP366*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ366/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,349,null,{"$f":"(AP366)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF366<=$J$9*1.05,(AV366*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW365,NA())","v":{"$error":"#N/A"}},23072.238162637354,482,6.3048133521261409,0.75566199212614149,0,2.1891513599999994,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},25.606279799755718,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,350,2.3305291073371062E-2,{"$f":"Z367*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF366*Bodencharakterisierung!$E$11/$J$20","v":2.6796646069081083E-5},{"$f":"((150*($J$2^0.87)*(AB367^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z367)*3600*24","v":5.6070384399043785E-2},2.3915996627248484E-4,{"$f":"AE366-AD367*Bodencharakterisierung!$E$8","v":3.8714591107759988E-2},{"$f":"IF(AE367>$J$18,(AE367/(Bodencharakterisierung!$E$11*1000)),0)","v":2.5554185549676558E-5},2.3305291073371062E-2,350,null,{"$f":"(AD367)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH367>0,(AJ367*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK366,NA())","v":0.75782945938151725},null,350,{"$f":"IF(AF367<=$J$9*0.05,AS366*EXP((-$J$6*1)/Heterogenität!$D$4),Z367)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF367>=$J$19, AR366/$J$5<AN367),0, Bodencharakterisierung!$E$8*$J$11*((AR366/$J$5)-AN367))","v":0},0,{"$f":"AQ366-AP367*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ367/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,350,null,{"$f":"(AP367)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF367<=$J$9*1.05,(AV367*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW366,NA())","v":{"$error":"#N/A"}},23072.238162637354,483,6.3132534593815173,0.75782945938151725,0,2.1954239999999996,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},25.554185549676557,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,351,2.3305291073371062E-2,{"$f":"Z368*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF367*Bodencharakterisierung!$E$11/$J$20","v":2.6742130099072089E-5},{"$f":"((150*($J$2^0.87)*(AB368^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z368)*3600*24","v":5.5980248713356086E-2},2.3915996627248484E-4,{"$f":"AE367-AD368*Bodencharakterisierung!$E$8","v":3.8635668318890065E-2},{"$f":"IF(AE368>$J$18,(AE368/(Bodencharakterisierung!$E$11*1000)),0)","v":2.5502091299597403E-5},2.3305291073371062E-2,351,null,{"$f":"(AD368)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH368>0,(AJ368*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK367,NA())","v":0.759996926636893},null,351,{"$f":"IF(AF368<=$J$9*0.05,AS367*EXP((-$J$6*1)/Heterogenität!$D$4),Z368)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF368>=$J$19, AR367/$J$5<AN368),0, Bodencharakterisierung!$E$8*$J$11*((AR367/$J$5)-AN368))","v":0},0,{"$f":"AQ367-AP368*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ368/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,351,null,{"$f":"(AP368)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF368<=$J$9*1.05,(AV368*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW367,NA())","v":{"$error":"#N/A"}},23072.238162637354,484,6.3216935666368927,0.759996926636893,0,2.2016966399999998,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},25.502091299597403,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,352,2.3305291073371062E-2,{"$f":"Z369*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF368*Bodencharakterisierung!$E$11/$J$20","v":2.6687614129063098E-5},{"$f":"((150*($J$2^0.87)*(AB369^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z369)*3600*24","v":5.5890074432129858E-2},2.3915996627248484E-4,{"$f":"AE368-AD369*Bodencharakterisierung!$E$8","v":3.8556745530020142E-2},{"$f":"IF(AE369>$J$18,(AE369/(Bodencharakterisierung!$E$11*1000)),0)","v":2.5449997049518244E-5},2.3305291073371062E-2,352,null,{"$f":"(AD369)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH369>0,(AJ369*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK368,NA())","v":0.76216439389226875},null,352,{"$f":"IF(AF369<=$J$9*0.05,AS368*EXP((-$J$6*1)/Heterogenität!$D$4),Z369)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF369>=$J$19, AR368/$J$5<AN369),0, Bodencharakterisierung!$E$8*$J$11*((AR368/$J$5)-AN369))","v":0},0,{"$f":"AQ368-AP369*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ369/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,352,null,{"$f":"(AP369)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF369<=$J$9*1.05,(AV369*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW368,NA())","v":{"$error":"#N/A"}},23072.238162637354,485,6.3301336738922682,0.76216439389226875,0,2.2079692799999999,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},25.449997049518245,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,353,2.3305291073371062E-2,{"$f":"Z370*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF369*Bodencharakterisierung!$E$11/$J$20","v":2.6633098159054104E-5},{"$f":"((150*($J$2^0.87)*(AB370^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z370)*3600*24","v":5.5799861459947191E-2},2.3915996627248484E-4,{"$f":"AE369-AD370*Bodencharakterisierung!$E$8","v":3.8477822741150219E-2},{"$f":"IF(AE370>$J$18,(AE370/(Bodencharakterisierung!$E$11*1000)),0)","v":2.5397902799439089E-5},2.3305291073371062E-2,353,null,{"$f":"(AD370)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH370>0,(AJ370*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK369,NA())","v":0.76433186114764451},null,353,{"$f":"IF(AF370<=$J$9*0.05,AS369*EXP((-$J$6*1)/Heterogenität!$D$4),Z370)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF370>=$J$19, AR369/$J$5<AN370),0, Bodencharakterisierung!$E$8*$J$11*((AR369/$J$5)-AN370))","v":0},0,{"$f":"AQ369-AP370*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ370/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,353,null,{"$f":"(AP370)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF370<=$J$9*1.05,(AV370*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW369,NA())","v":{"$error":"#N/A"}},23072.238162637354,486,6.3385737811476446,0.76433186114764451,0,2.2142419200000001,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},25.397902799439088,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,354,2.3305291073371062E-2,{"$f":"Z371*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF370*Bodencharakterisierung!$E$11/$J$20","v":2.657858218904511E-5},{"$f":"((150*($J$2^0.87)*(AB371^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z371)*3600*24","v":5.5709609700958278E-2},2.3915996627248484E-4,{"$f":"AE370-AD371*Bodencharakterisierung!$E$8","v":3.8398899952280297E-2},{"$f":"IF(AE371>$J$18,(AE371/(Bodencharakterisierung!$E$11*1000)),0)","v":2.5345808549359931E-5},2.3305291073371062E-2,354,null,{"$f":"(AD371)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH371>0,(AJ371*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK370,NA())","v":0.76649932840302026},null,354,{"$f":"IF(AF371<=$J$9*0.05,AS370*EXP((-$J$6*1)/Heterogenität!$D$4),Z371)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF371>=$J$19, AR370/$J$5<AN371),0, Bodencharakterisierung!$E$8*$J$11*((AR370/$J$5)-AN371))","v":0},0,{"$f":"AQ370-AP371*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ371/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,354,null,{"$f":"(AP371)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF371<=$J$9*1.05,(AV371*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW370,NA())","v":{"$error":"#N/A"}},23072.238162637354,487,6.3470138884030209,0.76649932840302026,0,2.2205145600000002,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},25.34580854935993,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,355,2.3305291073371062E-2,{"$f":"Z372*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF371*Bodencharakterisierung!$E$11/$J$20","v":2.6524066219036116E-5},{"$f":"((150*($J$2^0.87)*(AB372^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z372)*3600*24","v":5.5619319058878722E-2},2.3915996627248484E-4,{"$f":"AE371-AD372*Bodencharakterisierung!$E$8","v":3.8319977163410374E-2},{"$f":"IF(AE372>$J$18,(AE372/(Bodencharakterisierung!$E$11*1000)),0)","v":2.5293714299280775E-5},2.3305291073371062E-2,355,null,{"$f":"(AD372)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH372>0,(AJ372*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK371,NA())","v":0.76866679565839602},null,355,{"$f":"IF(AF372<=$J$9*0.05,AS371*EXP((-$J$6*1)/Heterogenität!$D$4),Z372)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF372>=$J$19, AR371/$J$5<AN372),0, Bodencharakterisierung!$E$8*$J$11*((AR371/$J$5)-AN372))","v":0},0,{"$f":"AQ371-AP372*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ372/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,355,null,{"$f":"(AP372)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF372<=$J$9*1.05,(AV372*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW371,NA())","v":{"$error":"#N/A"}},23072.238162637354,488,6.3554539956583964,0.76866679565839602,0,2.2267872000000004,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},25.293714299280776,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,356,2.3305291073371062E-2,{"$f":"Z373*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF372*Bodencharakterisierung!$E$11/$J$20","v":2.6469550249027125E-5},{"$f":"((150*($J$2^0.87)*(AB373^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z373)*3600*24","v":5.5528989436986996E-2},2.3915996627248484E-4,{"$f":"AE372-AD373*Bodencharakterisierung!$E$8","v":3.8241054374540451E-2},{"$f":"IF(AE373>$J$18,(AE373/(Bodencharakterisierung!$E$11*1000)),0)","v":2.5241620049201617E-5},2.3305291073371062E-2,356,null,{"$f":"(AD373)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH373>0,(AJ373*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK372,NA())","v":0.77083426291377177},null,356,{"$f":"IF(AF373<=$J$9*0.05,AS372*EXP((-$J$6*1)/Heterogenität!$D$4),Z373)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF373>=$J$19, AR372/$J$5<AN373),0, Bodencharakterisierung!$E$8*$J$11*((AR372/$J$5)-AN373))","v":0},0,{"$f":"AQ372-AP373*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ373/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,356,null,{"$f":"(AP373)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF373<=$J$9*1.05,(AV373*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW372,NA())","v":{"$error":"#N/A"}},23072.238162637354,489,6.3638941029137719,0.77083426291377177,0,2.2330598400000006,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},25.241620049201618,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,357,2.3305291073371062E-2,{"$f":"Z374*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF373*Bodencharakterisierung!$E$11/$J$20","v":2.6415034279018131E-5},{"$f":"((150*($J$2^0.87)*(AB374^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z374)*3600*24","v":5.5438620738120864E-2},2.3915996627248484E-4,{"$f":"AE373-AD374*Bodencharakterisierung!$E$8","v":3.8162131585670528E-2},{"$f":"IF(AE374>$J$18,(AE374/(Bodencharakterisierung!$E$11*1000)),0)","v":2.5189525799122462E-5},2.3305291073371062E-2,357,null,{"$f":"(AD374)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH374>0,(AJ374*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK373,NA())","v":0.77300173016914753},null,357,{"$f":"IF(AF374<=$J$9*0.05,AS373*EXP((-$J$6*1)/Heterogenität!$D$4),Z374)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF374>=$J$19, AR373/$J$5<AN374),0, Bodencharakterisierung!$E$8*$J$11*((AR373/$J$5)-AN374))","v":0},0,{"$f":"AQ373-AP374*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ374/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,357,null,{"$f":"(AP374)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF374<=$J$9*1.05,(AV374*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW373,NA())","v":{"$error":"#N/A"}},23072.238162637354,490,6.3723342101691482,0.77300173016914753,0,2.2393324800000007,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},25.18952579912246,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,358,2.3305291073371062E-2,{"$f":"Z375*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF374*Bodencharakterisierung!$E$11/$J$20","v":2.6360518309009137E-5},{"$f":"((150*($J$2^0.87)*(AB375^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z375)*3600*24","v":5.5348212864674944E-2},2.3915996627248484E-4,{"$f":"AE374-AD375*Bodencharakterisierung!$E$8","v":3.8083208796800605E-2},{"$f":"IF(AE375>$J$18,(AE375/(Bodencharakterisierung!$E$11*1000)),0)","v":2.5137431549043303E-5},2.3305291073371062E-2,358,null,{"$f":"(AD375)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH375>0,(AJ375*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK374,NA())","v":0.77516919742452328},null,358,{"$f":"IF(AF375<=$J$9*0.05,AS374*EXP((-$J$6*1)/Heterogenität!$D$4),Z375)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF375>=$J$19, AR374/$J$5<AN375),0, Bodencharakterisierung!$E$8*$J$11*((AR374/$J$5)-AN375))","v":0},0,{"$f":"AQ374-AP375*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ375/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,358,null,{"$f":"(AP375)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF375<=$J$9*1.05,(AV375*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW374,NA())","v":{"$error":"#N/A"}},23072.238162637354,491,6.3807743174245246,0.77516919742452328,0,2.2456051200000009,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},25.137431549043303,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,359,2.3305291073371062E-2,{"$f":"Z376*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF375*Bodencharakterisierung!$E$11/$J$20","v":2.6306002339000147E-5},{"$f":"((150*($J$2^0.87)*(AB376^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z376)*3600*24","v":5.5257765718597897E-2},2.3915996627248484E-4,{"$f":"AE375-AD376*Bodencharakterisierung!$E$8","v":3.8004286007930682E-2},{"$f":"IF(AE376>$J$18,(AE376/(Bodencharakterisierung!$E$11*1000)),0)","v":2.5085337298964148E-5},2.3305291073371062E-2,359,null,{"$f":"(AD376)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH376>0,(AJ376*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK375,NA())","v":0.77733666467989904},null,359,{"$f":"IF(AF376<=$J$9*0.05,AS375*EXP((-$J$6*1)/Heterogenität!$D$4),Z376)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF376>=$J$19, AR375/$J$5<AN376),0, Bodencharakterisierung!$E$8*$J$11*((AR375/$J$5)-AN376))","v":0},0,{"$f":"AQ375-AP376*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ376/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,359,null,{"$f":"(AP376)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF376<=$J$9*1.05,(AV376*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW375,NA())","v":{"$error":"#N/A"}},23072.238162637354,492,6.3892144246799001,0.77733666467989904,0,2.2518777600000011,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},25.085337298964149,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,360,2.3305291073371062E-2,{"$f":"Z377*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF376*Bodencharakterisierung!$E$11/$J$20","v":2.6251486368991153E-5},{"$f":"((150*($J$2^0.87)*(AB377^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z377)*3600*24","v":5.516727920138887E-2},2.3915996627248484E-4,{"$f":"AE376-AD377*Bodencharakterisierung!$E$8","v":3.7925363219060759E-2},{"$f":"IF(AE377>$J$18,(AE377/(Bodencharakterisierung!$E$11*1000)),0)","v":2.5033243048884989E-5},2.3305291073371062E-2,360,null,{"$f":"(AD377)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH377>0,(AJ377*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK376,NA())","v":0.77950413193527479},null,360,{"$f":"IF(AF377<=$J$9*0.05,AS376*EXP((-$J$6*1)/Heterogenität!$D$4),Z377)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF377>=$J$19, AR376/$J$5<AN377),0, Bodencharakterisierung!$E$8*$J$11*((AR376/$J$5)-AN377))","v":0},0,{"$f":"AQ376-AP377*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ377/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,360,null,{"$f":"(AP377)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF377<=$J$9*1.05,(AV377*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW376,NA())","v":{"$error":"#N/A"}},23072.238162637354,493,6.3976545319352756,0.77950413193527479,0,2.2581504000000012,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},25.033243048884991,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,361,2.3305291073371062E-2,{"$f":"Z378*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF377*Bodencharakterisierung!$E$11/$J$20","v":2.6196970398982159E-5},{"$f":"((150*($J$2^0.87)*(AB378^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z378)*3600*24","v":5.5076753214094894E-2},2.3915996627248484E-4,{"$f":"AE377-AD378*Bodencharakterisierung!$E$8","v":3.7846440430190836E-2},{"$f":"IF(AE378>$J$18,(AE378/(Bodencharakterisierung!$E$11*1000)),0)","v":2.4981148798805834E-5},2.3305291073371062E-2,361,null,{"$f":"(AD378)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH378>0,(AJ378*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK377,NA())","v":0.78167159919065055},null,361,{"$f":"IF(AF378<=$J$9*0.05,AS377*EXP((-$J$6*1)/Heterogenität!$D$4),Z378)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF378>=$J$19, AR377/$J$5<AN378),0, Bodencharakterisierung!$E$8*$J$11*((AR377/$J$5)-AN378))","v":0},0,{"$f":"AQ377-AP378*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ378/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,361,null,{"$f":"(AP378)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF378<=$J$9*1.05,(AV378*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW377,NA())","v":{"$error":"#N/A"}},23072.238162637354,494,6.4060946391906519,0.78167159919065055,0,2.2644230400000014,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},24.981148798805833,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,362,2.3305291073371062E-2,{"$f":"Z379*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF378*Bodencharakterisierung!$E$11/$J$20","v":2.6142454428973168E-5},{"$f":"((150*($J$2^0.87)*(AB379^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z379)*3600*24","v":5.4986187657308006E-2},2.3915996627248484E-4,{"$f":"AE378-AD379*Bodencharakterisierung!$E$8","v":3.7767517641320913E-2},{"$f":"IF(AE379>$J$18,(AE379/(Bodencharakterisierung!$E$11*1000)),0)","v":2.4929054548726675E-5},2.3305291073371062E-2,362,null,{"$f":"(AD379)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH379>0,(AJ379*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK378,NA())","v":0.7838390664460263},null,362,{"$f":"IF(AF379<=$J$9*0.05,AS378*EXP((-$J$6*1)/Heterogenität!$D$4),Z379)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF379>=$J$19, AR378/$J$5<AN379),0, Bodencharakterisierung!$E$8*$J$11*((AR378/$J$5)-AN379))","v":0},0,{"$f":"AQ378-AP379*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ379/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,362,null,{"$f":"(AP379)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF379<=$J$9*1.05,(AV379*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW378,NA())","v":{"$error":"#N/A"}},23072.238162637354,495,6.4145347464460283,0.7838390664460263,0,2.2706956800000015,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},24.929054548726675,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,363,2.3305291073371062E-2,{"$f":"Z380*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF379*Bodencharakterisierung!$E$11/$J$20","v":2.6087938458964174E-5},{"$f":"((150*($J$2^0.87)*(AB380^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z380)*3600*24","v":5.4895582431161945E-2},2.3915996627248484E-4,{"$f":"AE379-AD380*Bodencharakterisierung!$E$8","v":3.7688594852450991E-2},{"$f":"IF(AE380>$J$18,(AE380/(Bodencharakterisierung!$E$11*1000)),0)","v":2.487696029864752E-5},2.3305291073371062E-2,363,null,{"$f":"(AD380)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH380>0,(AJ380*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK379,NA())","v":0.78600653370140205},null,363,{"$f":"IF(AF380<=$J$9*0.05,AS379*EXP((-$J$6*1)/Heterogenität!$D$4),Z380)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF380>=$J$19, AR379/$J$5<AN380),0, Bodencharakterisierung!$E$8*$J$11*((AR379/$J$5)-AN380))","v":0},0,{"$f":"AQ379-AP380*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ380/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,363,null,{"$f":"(AP380)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF380<=$J$9*1.05,(AV380*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW379,NA())","v":{"$error":"#N/A"}},23072.238162637354,496,6.4229748537014038,0.78600653370140205,0,2.2769683200000017,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},24.876960298647521,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,364,2.3305291073371062E-2,{"$f":"Z381*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF380*Bodencharakterisierung!$E$11/$J$20","v":2.603342248895518E-5},{"$f":"((150*($J$2^0.87)*(AB381^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z381)*3600*24","v":5.4804937435329035E-2},2.3915996627248484E-4,{"$f":"AE380-AD381*Bodencharakterisierung!$E$8","v":3.7609672063581068E-2},{"$f":"IF(AE381>$J$18,(AE381/(Bodencharakterisierung!$E$11*1000)),0)","v":2.4824866048568361E-5},2.3305291073371062E-2,364,null,{"$f":"(AD381)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH381>0,(AJ381*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK380,NA())","v":0.78817400095677781},null,364,{"$f":"IF(AF381<=$J$9*0.05,AS380*EXP((-$J$6*1)/Heterogenität!$D$4),Z381)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF381>=$J$19, AR380/$J$5<AN381),0, Bodencharakterisierung!$E$8*$J$11*((AR380/$J$5)-AN381))","v":0},0,{"$f":"AQ380-AP381*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ381/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,364,null,{"$f":"(AP381)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF381<=$J$9*1.05,(AV381*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW380,NA())","v":{"$error":"#N/A"}},23072.238162637354,497,6.4314149609567792,0.78817400095677781,0,2.2832409600000019,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},24.82486604856836,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,365,2.3305291073371062E-2,{"$f":"Z382*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF381*Bodencharakterisierung!$E$11/$J$20","v":2.5978906518946186E-5},{"$f":"((150*($J$2^0.87)*(AB382^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z382)*3600*24","v":5.4714252569017283E-2},2.3915996627248484E-4,{"$f":"AE381-AD382*Bodencharakterisierung!$E$8","v":3.7530749274711145E-2},{"$f":"IF(AE382>$J$18,(AE382/(Bodencharakterisierung!$E$11*1000)),0)","v":2.4772771798489206E-5},2.3305291073371062E-2,365,null,{"$f":"(AD382)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH382>0,(AJ382*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK381,NA())","v":0.79034146821215356},null,365,{"$f":"IF(AF382<=$J$9*0.05,AS381*EXP((-$J$6*1)/Heterogenität!$D$4),Z382)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF382>=$J$19, AR381/$J$5<AN382),0, Bodencharakterisierung!$E$8*$J$11*((AR381/$J$5)-AN382))","v":0},0,{"$f":"AQ381-AP382*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ382/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,365,null,{"$f":"(AP382)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF382<=$J$9*1.05,(AV382*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW381,NA())","v":{"$error":"#N/A"}},23072.238162637354,498,6.4398550682121556,0.79034146821215356,0,2.289513600000002,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},24.772771798489206,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,366,2.3305291073371062E-2,{"$f":"Z383*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF382*Bodencharakterisierung!$E$11/$J$20","v":2.5924390548937196E-5},{"$f":"((150*($J$2^0.87)*(AB383^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z383)*3600*24","v":5.4623527730967111E-2},2.3915996627248484E-4,{"$f":"AE382-AD383*Bodencharakterisierung!$E$8","v":3.7451826485841222E-2},{"$f":"IF(AE383>$J$18,(AE383/(Bodencharakterisierung!$E$11*1000)),0)","v":2.4720677548410048E-5},2.3305291073371062E-2,366,null,{"$f":"(AD383)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH383>0,(AJ383*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK382,NA())","v":0.79250893546752932},null,366,{"$f":"IF(AF383<=$J$9*0.05,AS382*EXP((-$J$6*1)/Heterogenität!$D$4),Z383)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF383>=$J$19, AR382/$J$5<AN383),0, Bodencharakterisierung!$E$8*$J$11*((AR382/$J$5)-AN383))","v":0},0,{"$f":"AQ382-AP383*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ383/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,366,null,{"$f":"(AP383)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF383<=$J$9*1.05,(AV383*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW382,NA())","v":{"$error":"#N/A"}},23072.238162637354,499,6.4482951754675319,0.79250893546752932,0,2.2957862400000022,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},24.720677548410048,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,367,2.3305291073371062E-2,{"$f":"Z384*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF383*Bodencharakterisierung!$E$11/$J$20","v":2.5869874578928202E-5},{"$f":"((150*($J$2^0.87)*(AB384^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z384)*3600*24","v":5.4532762819448265E-2},2.3915996627248484E-4,{"$f":"AE383-AD384*Bodencharakterisierung!$E$8","v":3.7372903696971299E-2},{"$f":"IF(AE384>$J$18,(AE384/(Bodencharakterisierung!$E$11*1000)),0)","v":2.4668583298330889E-5},2.3305291073371062E-2,367,null,{"$f":"(AD384)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH384>0,(AJ384*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK383,NA())","v":0.79467640272290507},null,367,{"$f":"IF(AF384<=$J$9*0.05,AS383*EXP((-$J$6*1)/Heterogenität!$D$4),Z384)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF384>=$J$19, AR383/$J$5<AN384),0, Bodencharakterisierung!$E$8*$J$11*((AR383/$J$5)-AN384))","v":0},0,{"$f":"AQ383-AP384*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ384/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,367,null,{"$f":"(AP384)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF384<=$J$9*1.05,(AV384*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW383,NA())","v":{"$error":"#N/A"}},23072.238162637354,500,6.4567352827229074,0.79467640272290507,0,2.3020588800000024,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},24.668583298330891,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,368,2.3305291073371062E-2,{"$f":"Z385*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF384*Bodencharakterisierung!$E$11/$J$20","v":2.5815358608919204E-5},{"$f":"((150*($J$2^0.87)*(AB385^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z385)*3600*24","v":5.4441957732256657E-2},2.3915996627248484E-4,{"$f":"AE384-AD385*Bodencharakterisierung!$E$8","v":3.7293980908101376E-2},{"$f":"IF(AE385>$J$18,(AE385/(Bodencharakterisierung!$E$11*1000)),0)","v":2.4616489048251734E-5},2.3305291073371062E-2,368,null,{"$f":"(AD385)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH385>0,(AJ385*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK384,NA())","v":0.79684386997828083},null,368,{"$f":"IF(AF385<=$J$9*0.05,AS384*EXP((-$J$6*1)/Heterogenität!$D$4),Z385)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF385>=$J$19, AR384/$J$5<AN385),0, Bodencharakterisierung!$E$8*$J$11*((AR384/$J$5)-AN385))","v":0},0,{"$f":"AQ384-AP385*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ385/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,368,null,{"$f":"(AP385)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF385<=$J$9*1.05,(AV385*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW384,NA())","v":{"$error":"#N/A"}},23072.238162637354,501,6.4651753899782829,0.79684386997828083,0,2.3083315200000025,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},24.616489048251733,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,369,2.3305291073371062E-2,{"$f":"Z386*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF385*Bodencharakterisierung!$E$11/$J$20","v":2.576084263891021E-5},{"$f":"((150*($J$2^0.87)*(AB386^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z386)*3600*24","v":5.4351112366710974E-2},2.3915996627248484E-4,{"$f":"AE385-AD386*Bodencharakterisierung!$E$8","v":3.7215058119231453E-2},{"$f":"IF(AE386>$J$18,(AE386/(Bodencharakterisierung!$E$11*1000)),0)","v":2.4564394798172575E-5},2.3305291073371062E-2,369,null,{"$f":"(AD386)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH386>0,(AJ386*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK385,NA())","v":0.79901133723365658},null,369,{"$f":"IF(AF386<=$J$9*0.05,AS385*EXP((-$J$6*1)/Heterogenität!$D$4),Z386)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF386>=$J$19, AR385/$J$5<AN386),0, Bodencharakterisierung!$E$8*$J$11*((AR385/$J$5)-AN386))","v":0},0,{"$f":"AQ385-AP386*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ386/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,369,null,{"$f":"(AP386)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF386<=$J$9*1.05,(AV386*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW385,NA())","v":{"$error":"#N/A"}},23072.238162637354,502,6.4736154972336593,0.79901133723365658,0,2.3146041600000027,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},24.564394798172575,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,370,2.3305291073371062E-2,{"$f":"Z387*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF386*Bodencharakterisierung!$E$11/$J$20","v":2.570632666890122E-5},{"$f":"((150*($J$2^0.87)*(AB387^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z387)*3600*24","v":5.4260226619649632E-2},2.3915996627248484E-4,{"$f":"AE386-AD387*Bodencharakterisierung!$E$8","v":3.713613533036153E-2},{"$f":"IF(AE387>$J$18,(AE387/(Bodencharakterisierung!$E$11*1000)),0)","v":2.451230054809342E-5},2.3305291073371062E-2,370,null,{"$f":"(AD387)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH387>0,(AJ387*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK386,NA())","v":0.80117880448903234},null,370,{"$f":"IF(AF387<=$J$9*0.05,AS386*EXP((-$J$6*1)/Heterogenität!$D$4),Z387)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF387>=$J$19, AR386/$J$5<AN387),0, Bodencharakterisierung!$E$8*$J$11*((AR386/$J$5)-AN387))","v":0},0,{"$f":"AQ386-AP387*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ387/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,370,null,{"$f":"(AP387)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF387<=$J$9*1.05,(AV387*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW386,NA())","v":{"$error":"#N/A"}},23072.238162637354,503,6.4820556044890356,0.80117880448903234,0,2.3208768000000028,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},24.512300548093421,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,371,2.3305291073371062E-2,{"$f":"Z388*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF387*Bodencharakterisierung!$E$11/$J$20","v":2.5651810698892226E-5},{"$f":"((150*($J$2^0.87)*(AB388^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z388)*3600*24","v":5.4169300387427705E-2},2.3915996627248484E-4,{"$f":"AE387-AD388*Bodencharakterisierung!$E$8","v":3.7057212541491608E-2},{"$f":"IF(AE388>$J$18,(AE388/(Bodencharakterisierung!$E$11*1000)),0)","v":2.4460206298014261E-5},2.3305291073371062E-2,371,null,{"$f":"(AD388)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH388>0,(AJ388*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK387,NA())","v":0.80334627174440809},null,371,{"$f":"IF(AF388<=$J$9*0.05,AS387*EXP((-$J$6*1)/Heterogenität!$D$4),Z388)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF388>=$J$19, AR387/$J$5<AN388),0, Bodencharakterisierung!$E$8*$J$11*((AR387/$J$5)-AN388))","v":0},0,{"$f":"AQ387-AP388*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ388/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,371,null,{"$f":"(AP388)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF388<=$J$9*1.05,(AV388*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW387,NA())","v":{"$error":"#N/A"}},23072.238162637354,504,6.4904957117444111,0.80334627174440809,0,2.327149440000003,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},24.46020629801426,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,372,2.3305291073371062E-2,{"$f":"Z389*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF388*Bodencharakterisierung!$E$11/$J$20","v":2.5597294728883232E-5},{"$f":"((150*($J$2^0.87)*(AB389^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z389)*3600*24","v":5.4078333565912795E-2},2.3915996627248484E-4,{"$f":"AE388-AD389*Bodencharakterisierung!$E$8","v":3.6978289752621685E-2},{"$f":"IF(AE389>$J$18,(AE389/(Bodencharakterisierung!$E$11*1000)),0)","v":2.4408112047935106E-5},2.3305291073371062E-2,372,null,{"$f":"(AD389)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH389>0,(AJ389*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK388,NA())","v":0.80551373899978385},null,372,{"$f":"IF(AF389<=$J$9*0.05,AS388*EXP((-$J$6*1)/Heterogenität!$D$4),Z389)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF389>=$J$19, AR388/$J$5<AN389),0, Bodencharakterisierung!$E$8*$J$11*((AR388/$J$5)-AN389))","v":0},0,{"$f":"AQ388-AP389*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ389/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,372,null,{"$f":"(AP389)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF389<=$J$9*1.05,(AV389*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW388,NA())","v":{"$error":"#N/A"}},23072.238162637354,505,6.4989358189997866,0.80551373899978385,0,2.3334220800000032,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},24.408112047935106,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,373,2.3305291073371062E-2,{"$f":"Z390*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF389*Bodencharakterisierung!$E$11/$J$20","v":2.5542778758874238E-5},{"$f":"((150*($J$2^0.87)*(AB390^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z390)*3600*24","v":5.398732605048278E-2},2.3915996627248484E-4,{"$f":"AE389-AD390*Bodencharakterisierung!$E$8","v":3.6899366963751762E-2},{"$f":"IF(AE390>$J$18,(AE390/(Bodencharakterisierung!$E$11*1000)),0)","v":2.4356017797855947E-5},2.3305291073371062E-2,373,null,{"$f":"(AD390)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH390>0,(AJ390*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK389,NA())","v":0.8076812062551596},null,373,{"$f":"IF(AF390<=$J$9*0.05,AS389*EXP((-$J$6*1)/Heterogenität!$D$4),Z390)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF390>=$J$19, AR389/$J$5<AN390),0, Bodencharakterisierung!$E$8*$J$11*((AR389/$J$5)-AN390))","v":0},0,{"$f":"AQ389-AP390*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ390/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,373,null,{"$f":"(AP390)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF390<=$J$9*1.05,(AV390*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW389,NA())","v":{"$error":"#N/A"}},23072.238162637354,506,6.5073759262551629,0.8076812062551596,0,2.3396947200000033,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},24.356017797855948,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,374,2.3305291073371062E-2,{"$f":"Z391*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF390*Bodencharakterisierung!$E$11/$J$20","v":2.5488262788865247E-5},{"$f":"((150*($J$2^0.87)*(AB391^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z391)*3600*24","v":5.3896277736021743E-2},2.3915996627248484E-4,{"$f":"AE390-AD391*Bodencharakterisierung!$E$8","v":3.6820444174881839E-2},{"$f":"IF(AE391>$J$18,(AE391/(Bodencharakterisierung!$E$11*1000)),0)","v":2.4303923547776792E-5},2.3305291073371062E-2,374,null,{"$f":"(AD391)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH391>0,(AJ391*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK390,NA())","v":0.80984867351053536},null,374,{"$f":"IF(AF391<=$J$9*0.05,AS390*EXP((-$J$6*1)/Heterogenität!$D$4),Z391)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF391>=$J$19, AR390/$J$5<AN391),0, Bodencharakterisierung!$E$8*$J$11*((AR390/$J$5)-AN391))","v":0},0,{"$f":"AQ390-AP391*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ391/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,374,null,{"$f":"(AP391)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF391<=$J$9*1.05,(AV391*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW390,NA())","v":{"$error":"#N/A"}},23072.238162637354,507,6.5158160335105393,0.80984867351053536,0,2.3459673600000035,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},24.303923547776794,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,375,2.3305291073371062E-2,{"$f":"Z392*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF391*Bodencharakterisierung!$E$11/$J$20","v":2.5433746818856253E-5},{"$f":"((150*($J$2^0.87)*(AB392^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z392)*3600*24","v":5.3805188516916742E-2},2.3915996627248484E-4,{"$f":"AE391-AD392*Bodencharakterisierung!$E$8","v":3.6741521386011916E-2},{"$f":"IF(AE392>$J$18,(AE392/(Bodencharakterisierung!$E$11*1000)),0)","v":2.4251829297697634E-5},2.3305291073371062E-2,375,null,{"$f":"(AD392)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH392>0,(AJ392*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK391,NA())","v":0.81201614076591111},null,375,{"$f":"IF(AF392<=$J$9*0.05,AS391*EXP((-$J$6*1)/Heterogenität!$D$4),Z392)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF392>=$J$19, AR391/$J$5<AN392),0, Bodencharakterisierung!$E$8*$J$11*((AR391/$J$5)-AN392))","v":0},0,{"$f":"AQ391-AP392*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ392/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,375,null,{"$f":"(AP392)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF392<=$J$9*1.05,(AV392*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW391,NA())","v":{"$error":"#N/A"}},23072.238162637354,508,6.5242561407659148,0.81201614076591111,0,2.3522400000000037,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},24.251829297697633,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,376,2.3305291073371062E-2,{"$f":"Z393*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF392*Bodencharakterisierung!$E$11/$J$20","v":2.5379230848847259E-5},{"$f":"((150*($J$2^0.87)*(AB393^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z393)*3600*24","v":5.3714058287054445E-2},2.3915996627248484E-4,{"$f":"AE392-AD393*Bodencharakterisierung!$E$8","v":3.6662598597141993E-2},{"$f":"IF(AE393>$J$18,(AE393/(Bodencharakterisierung!$E$11*1000)),0)","v":2.4199735047618478E-5},2.3305291073371062E-2,376,null,{"$f":"(AD393)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH393>0,(AJ393*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK392,NA())","v":0.81418360802128686},null,376,{"$f":"IF(AF393<=$J$9*0.05,AS392*EXP((-$J$6*1)/Heterogenität!$D$4),Z393)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF393>=$J$19, AR392/$J$5<AN393),0, Bodencharakterisierung!$E$8*$J$11*((AR392/$J$5)-AN393))","v":0},0,{"$f":"AQ392-AP393*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ393/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,376,null,{"$f":"(AP393)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF393<=$J$9*1.05,(AV393*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW392,NA())","v":{"$error":"#N/A"}},23072.238162637354,509,6.5326962480212902,0.81418360802128686,0,2.3585126400000038,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},24.199735047618478,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,377,2.3305291073371062E-2,{"$f":"Z394*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF393*Bodencharakterisierung!$E$11/$J$20","v":2.5324714878838269E-5},{"$f":"((150*($J$2^0.87)*(AB394^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z394)*3600*24","v":5.362288693981776E-2},2.3915996627248484E-4,{"$f":"AE393-AD394*Bodencharakterisierung!$E$8","v":3.658367580827207E-2},{"$f":"IF(AE394>$J$18,(AE394/(Bodencharakterisierung!$E$11*1000)),0)","v":2.414764079753932E-5},2.3305291073371062E-2,377,null,{"$f":"(AD394)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH394>0,(AJ394*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK393,NA())","v":0.81635107527666262},null,377,{"$f":"IF(AF394<=$J$9*0.05,AS393*EXP((-$J$6*1)/Heterogenität!$D$4),Z394)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF394>=$J$19, AR393/$J$5<AN394),0, Bodencharakterisierung!$E$8*$J$11*((AR393/$J$5)-AN394))","v":0},0,{"$f":"AQ393-AP394*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ394/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,377,null,{"$f":"(AP394)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF394<=$J$9*1.05,(AV394*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW393,NA())","v":{"$error":"#N/A"}},23072.238162637354,510,6.5411363552766666,0.81635107527666262,0,2.364785280000004,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},24.147640797539321,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,378,2.3305291073371062E-2,{"$f":"Z395*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF394*Bodencharakterisierung!$E$11/$J$20","v":2.5270198908829275E-5},{"$f":"((150*($J$2^0.87)*(AB395^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z395)*3600*24","v":5.3531674368082177E-2},2.3915996627248484E-4,{"$f":"AE394-AD395*Bodencharakterisierung!$E$8","v":3.6504753019402147E-2},{"$f":"IF(AE395>$J$18,(AE395/(Bodencharakterisierung!$E$11*1000)),0)","v":2.4095546547460165E-5},2.3305291073371062E-2,378,null,{"$f":"(AD395)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH395>0,(AJ395*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK394,NA())","v":0.81851854253203837},null,378,{"$f":"IF(AF395<=$J$9*0.05,AS394*EXP((-$J$6*1)/Heterogenität!$D$4),Z395)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF395>=$J$19, AR394/$J$5<AN395),0, Bodencharakterisierung!$E$8*$J$11*((AR394/$J$5)-AN395))","v":0},0,{"$f":"AQ394-AP395*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ395/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,378,null,{"$f":"(AP395)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF395<=$J$9*1.05,(AV395*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW394,NA())","v":{"$error":"#N/A"}},23072.238162637354,511,6.549576462532043,0.81851854253203837,0,2.3710579200000041,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},24.095546547460163,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,379,2.3305291073371062E-2,{"$f":"Z396*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF395*Bodencharakterisierung!$E$11/$J$20","v":2.5215682938820281E-5},{"$f":"((150*($J$2^0.87)*(AB396^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z396)*3600*24","v":5.344042046421249E-2},2.3915996627248484E-4,{"$f":"AE395-AD396*Bodencharakterisierung!$E$8","v":3.6425830230532225E-2},{"$f":"IF(AE396>$J$18,(AE396/(Bodencharakterisierung!$E$11*1000)),0)","v":2.4043452297381006E-5},2.3305291073371062E-2,379,null,{"$f":"(AD396)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH396>0,(AJ396*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK395,NA())","v":0.82068600978741413},null,379,{"$f":"IF(AF396<=$J$9*0.05,AS395*EXP((-$J$6*1)/Heterogenität!$D$4),Z396)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF396>=$J$19, AR395/$J$5<AN396),0, Bodencharakterisierung!$E$8*$J$11*((AR395/$J$5)-AN396))","v":0},0,{"$f":"AQ395-AP396*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ396/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,379,null,{"$f":"(AP396)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF396<=$J$9*1.05,(AV396*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW395,NA())","v":{"$error":"#N/A"}},23072.238162637354,512,6.5580165697874184,0.82068600978741413,0,2.3773305600000043,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},24.043452297381005,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,380,2.3305291073371062E-2,{"$f":"Z397*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF396*Bodencharakterisierung!$E$11/$J$20","v":2.516116696881129E-5},{"$f":"((150*($J$2^0.87)*(AB397^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z397)*3600*24","v":5.3349125120058696E-2},2.3915996627248484E-4,{"$f":"AE396-AD397*Bodencharakterisierung!$E$8","v":3.6346907441662302E-2},{"$f":"IF(AE397>$J$18,(AE397/(Bodencharakterisierung!$E$11*1000)),0)","v":2.3991358047301851E-5},2.3305291073371062E-2,380,null,{"$f":"(AD397)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH397>0,(AJ397*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK396,NA())","v":0.82285347704278988},null,380,{"$f":"IF(AF397<=$J$9*0.05,AS396*EXP((-$J$6*1)/Heterogenität!$D$4),Z397)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF397>=$J$19, AR396/$J$5<AN397),0, Bodencharakterisierung!$E$8*$J$11*((AR396/$J$5)-AN397))","v":0},0,{"$f":"AQ396-AP397*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ397/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,380,null,{"$f":"(AP397)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF397<=$J$9*1.05,(AV397*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW396,NA())","v":{"$error":"#N/A"}},23072.238162637354,513,6.5664566770427939,0.82285347704278988,0,2.3836032000000045,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},23.991358047301851,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,381,2.3305291073371062E-2,{"$f":"Z398*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF397*Bodencharakterisierung!$E$11/$J$20","v":2.5106650998802296E-5},{"$f":"((150*($J$2^0.87)*(AB398^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z398)*3600*24","v":5.325778822695329E-2},2.3915996627248484E-4,{"$f":"AE397-AD398*Bodencharakterisierung!$E$8","v":3.6267984652792379E-2},{"$f":"IF(AE398>$J$18,(AE398/(Bodencharakterisierung!$E$11*1000)),0)","v":2.3939263797222692E-5},2.3305291073371062E-2,381,null,{"$f":"(AD398)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH398>0,(AJ398*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK397,NA())","v":0.82502094429816564},null,381,{"$f":"IF(AF398<=$J$9*0.05,AS397*EXP((-$J$6*1)/Heterogenität!$D$4),Z398)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF398>=$J$19, AR397/$J$5<AN398),0, Bodencharakterisierung!$E$8*$J$11*((AR397/$J$5)-AN398))","v":0},0,{"$f":"AQ397-AP398*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ398/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,381,null,{"$f":"(AP398)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF398<=$J$9*1.05,(AV398*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW397,NA())","v":{"$error":"#N/A"}},23072.238162637354,514,6.5748967842981703,0.82502094429816564,0,2.3898758400000046,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},23.939263797222694,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,382,2.3305291073371062E-2,{"$f":"Z399*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF398*Bodencharakterisierung!$E$11/$J$20","v":2.5052135028793302E-5},{"$f":"((150*($J$2^0.87)*(AB399^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z399)*3600*24","v":5.3166409675706947E-2},2.3915996627248484E-4,{"$f":"AE398-AD399*Bodencharakterisierung!$E$8","v":3.6189061863922456E-2},{"$f":"IF(AE399>$J$18,(AE399/(Bodencharakterisierung!$E$11*1000)),0)","v":2.3887169547143537E-5},2.3305291073371062E-2,382,null,{"$f":"(AD399)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH399>0,(AJ399*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK398,NA())","v":0.82718841155354139},null,382,{"$f":"IF(AF399<=$J$9*0.05,AS398*EXP((-$J$6*1)/Heterogenität!$D$4),Z399)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF399>=$J$19, AR398/$J$5<AN399),0, Bodencharakterisierung!$E$8*$J$11*((AR398/$J$5)-AN399))","v":0},0,{"$f":"AQ398-AP399*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ399/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,382,null,{"$f":"(AP399)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF399<=$J$9*1.05,(AV399*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW398,NA())","v":{"$error":"#N/A"}},23072.238162637354,515,6.5833368915535466,0.82718841155354139,0,2.3961484800000048,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},23.887169547143536,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,383,2.3305291073371062E-2,{"$f":"Z400*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF399*Bodencharakterisierung!$E$11/$J$20","v":2.4997619058784311E-5},{"$f":"((150*($J$2^0.87)*(AB400^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z400)*3600*24","v":5.3074989356605096E-2},2.3915996627248484E-4,{"$f":"AE399-AD400*Bodencharakterisierung!$E$8","v":3.6110139075052533E-2},{"$f":"IF(AE400>$J$18,(AE400/(Bodencharakterisierung!$E$11*1000)),0)","v":2.3835075297064378E-5},2.3305291073371062E-2,383,null,{"$f":"(AD400)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH400>0,(AJ400*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK399,NA())","v":0.82935587880891715},null,383,{"$f":"IF(AF400<=$J$9*0.05,AS399*EXP((-$J$6*1)/Heterogenität!$D$4),Z400)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF400>=$J$19, AR399/$J$5<AN400),0, Bodencharakterisierung!$E$8*$J$11*((AR399/$J$5)-AN400))","v":0},0,{"$f":"AQ399-AP400*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ400/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,383,null,{"$f":"(AP400)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF400<=$J$9*1.05,(AV400*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW399,NA())","v":{"$error":"#N/A"}},23072.238162637354,516,6.5917769988089221,0.82935587880891715,0,2.402421120000005,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},23.835075297064378,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,384,2.3305291073371062E-2,{"$f":"Z401*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF400*Bodencharakterisierung!$E$11/$J$20","v":2.4943103088775317E-5},{"$f":"((150*($J$2^0.87)*(AB401^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z401)*3600*24","v":5.2983527159404173E-2},2.3915996627248484E-4,{"$f":"AE400-AD401*Bodencharakterisierung!$E$8","v":3.603121628618261E-2},{"$f":"IF(AE401>$J$18,(AE401/(Bodencharakterisierung!$E$11*1000)),0)","v":2.378298104698522E-5},2.3305291073371062E-2,384,null,{"$f":"(AD401)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH401>0,(AJ401*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK400,NA())","v":0.8315233460642929},null,384,{"$f":"IF(AF401<=$J$9*0.05,AS400*EXP((-$J$6*1)/Heterogenität!$D$4),Z401)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF401>=$J$19, AR400/$J$5<AN401),0, Bodencharakterisierung!$E$8*$J$11*((AR400/$J$5)-AN401))","v":0},0,{"$f":"AQ400-AP401*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ401/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,384,null,{"$f":"(AP401)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF401<=$J$9*1.05,(AV401*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW400,NA())","v":{"$error":"#N/A"}},23072.238162637354,517,6.6002171060642976,0.8315233460642929,0,2.4086937600000051,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},23.782981046985221,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,385,2.3305291073371062E-2,{"$f":"Z402*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF401*Bodencharakterisierung!$E$11/$J$20","v":2.488858711876632E-5},{"$f":"((150*($J$2^0.87)*(AB402^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z402)*3600*24","v":5.2892022973328304E-2},2.3915996627248484E-4,{"$f":"AE401-AD402*Bodencharakterisierung!$E$8","v":3.5952293497312687E-2},{"$f":"IF(AE402>$J$18,(AE402/(Bodencharakterisierung!$E$11*1000)),0)","v":2.3730886796906064E-5},2.3305291073371062E-2,385,null,{"$f":"(AD402)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH402>0,(AJ402*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK401,NA())","v":0.83369081331966866},null,385,{"$f":"IF(AF402<=$J$9*0.05,AS401*EXP((-$J$6*1)/Heterogenität!$D$4),Z402)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF402>=$J$19, AR401/$J$5<AN402),0, Bodencharakterisierung!$E$8*$J$11*((AR401/$J$5)-AN402))","v":0},0,{"$f":"AQ401-AP402*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ402/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,385,null,{"$f":"(AP402)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF402<=$J$9*1.05,(AV402*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW401,NA())","v":{"$error":"#N/A"}},23072.238162637354,518,6.6086572133196739,0.83369081331966866,0,2.4149664000000053,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},23.730886796906063,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,386,2.3305291073371062E-2,{"$f":"Z403*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF402*Bodencharakterisierung!$E$11/$J$20","v":2.483407114875733E-5},{"$f":"((150*($J$2^0.87)*(AB403^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z403)*3600*24","v":5.2800476687064939E-2},2.3915996627248484E-4,{"$f":"AE402-AD403*Bodencharakterisierung!$E$8","v":3.5873370708442764E-2},{"$f":"IF(AE403>$J$18,(AE403/(Bodencharakterisierung!$E$11*1000)),0)","v":2.3678792546826906E-5},2.3305291073371062E-2,386,null,{"$f":"(AD403)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH403>0,(AJ403*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK402,NA())","v":0.83585828057504441},null,386,{"$f":"IF(AF403<=$J$9*0.05,AS402*EXP((-$J$6*1)/Heterogenität!$D$4),Z403)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF403>=$J$19, AR402/$J$5<AN403),0, Bodencharakterisierung!$E$8*$J$11*((AR402/$J$5)-AN403))","v":0},0,{"$f":"AQ402-AP403*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ403/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,386,null,{"$f":"(AP403)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF403<=$J$9*1.05,(AV403*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW402,NA())","v":{"$error":"#N/A"}},23072.238162637354,519,6.6170973205750503,0.83585828057504441,0,2.4212390400000054,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},23.678792546826905,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,387,2.3305291073371062E-2,{"$f":"Z404*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF403*Bodencharakterisierung!$E$11/$J$20","v":2.4779555178748332E-5},{"$f":"((150*($J$2^0.87)*(AB404^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z404)*3600*24","v":5.270888818876153E-2},2.3915996627248484E-4,{"$f":"AE403-AD404*Bodencharakterisierung!$E$8","v":3.5794447919572842E-2},{"$f":"IF(AE404>$J$18,(AE404/(Bodencharakterisierung!$E$11*1000)),0)","v":2.3626698296747751E-5},2.3305291073371062E-2,387,null,{"$f":"(AD404)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH404>0,(AJ404*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK403,NA())","v":0.83802574783042016},null,387,{"$f":"IF(AF404<=$J$9*0.05,AS403*EXP((-$J$6*1)/Heterogenität!$D$4),Z404)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF404>=$J$19, AR403/$J$5<AN404),0, Bodencharakterisierung!$E$8*$J$11*((AR403/$J$5)-AN404))","v":0},0,{"$f":"AQ403-AP404*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ404/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,387,null,{"$f":"(AP404)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF404<=$J$9*1.05,(AV404*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW403,NA())","v":{"$error":"#N/A"}},23072.238162637354,520,6.6255374278304258,0.83802574783042016,0,{"$f":"$G$34/$G$12/$G$8+BC403","v":2.4275116800000056},null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},23.626698296747751,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,388,2.3305291073371062E-2,{"$f":"Z405*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF404*Bodencharakterisierung!$E$11/$J$20","v":2.4725039208739345E-5},{"$f":"((150*($J$2^0.87)*(AB405^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z405)*3600*24","v":5.2617257366021408E-2},2.3915996627248484E-4,{"$f":"AE404-AD405*Bodencharakterisierung!$E$8","v":3.5715525130702919E-2},{"$f":"IF(AE405>$J$18,(AE405/(Bodencharakterisierung!$E$11*1000)),0)","v":2.3574604046668592E-5},2.3305291073371062E-2,388,null,{"$f":"(AD405)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH405>0,(AJ405*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK404,NA())","v":0.84019321508579592},null,388,{"$f":"IF(AF405<=$J$9*0.05,AS404*EXP((-$J$6*1)/Heterogenität!$D$4),Z405)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF405>=$J$19, AR404/$J$5<AN405),0, Bodencharakterisierung!$E$8*$J$11*((AR404/$J$5)-AN405))","v":0},0,{"$f":"AQ404-AP405*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ405/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,388,null,{"$f":"(AP405)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF405<=$J$9*1.05,(AV405*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW404,NA())","v":{"$error":"#N/A"}},23072.238162637354,521,6.6339775350858012,0.84019321508579592,0,2.4337843200000058,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},23.574604046668593,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,389,2.3305291073371062E-2,{"$f":"Z406*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF405*Bodencharakterisierung!$E$11/$J$20","v":2.4670523238730348E-5},{"$f":"((150*($J$2^0.87)*(AB406^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z406)*3600*24","v":5.2525584105900337E-2},2.3915996627248484E-4,{"$f":"AE405-AD406*Bodencharakterisierung!$E$8","v":3.5636602341832996E-2},{"$f":"IF(AE406>$J$18,(AE406/(Bodencharakterisierung!$E$11*1000)),0)","v":2.3522509796589437E-5},2.3305291073371062E-2,389,null,{"$f":"(AD406)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH406>0,(AJ406*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK405,NA())","v":0.84236068234117167},null,389,{"$f":"IF(AF406<=$J$9*0.05,AS405*EXP((-$J$6*1)/Heterogenität!$D$4),Z406)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF406>=$J$19, AR405/$J$5<AN406),0, Bodencharakterisierung!$E$8*$J$11*((AR405/$J$5)-AN406))","v":0},0,{"$f":"AQ405-AP406*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ406/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,389,null,{"$f":"(AP406)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF406<=$J$9*1.05,(AV406*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW405,NA())","v":{"$error":"#N/A"}},23072.238162637354,522,6.6424176423411776,0.84236068234117167,0,2.4400569600000059,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},23.522509796589436,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,390,{"$f":"AG406","v":2.3305291073371062E-2},{"$f":"Z407*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF406*Bodencharakterisierung!$E$11/$J$20","v":2.461600726872136E-5},{"$f":"((150*($J$2^0.87)*(AB407^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z407)*3600*24","v":5.2433868294902361E-2},{"$f":"MIN(AC407,Z407-AA407)","v":2.3915996627248484E-4},{"$f":"AE406-AD407*Bodencharakterisierung!$E$8","v":3.5557679552963073E-2},{"$f":"IF(AE407>$J$18,(AE407/(Bodencharakterisierung!$E$11*1000)),0)","v":2.3470415546510278E-5},{"$f":"AA407+AD407","v":2.3305291073371062E-2},{"$f":"IF(AD407>0,Y407,NA())","v":390},null,{"$f":"(AD407)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH407>0,(AJ407*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK406,NA())","v":0.84452814959654743},null,390,{"$f":"IF(AF407<=$J$9*0.05,AS406*EXP((-$J$6*1)/Heterogenität!$D$4),Z407)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF407>=$J$19, AR406/$J$5<AN407),0, Bodencharakterisierung!$E$8*$J$11*((AR406/$J$5)-AN407))","v":0},{"$f":"MIN(AO407,AS406-AN407)","v":0},{"$f":"AQ406-AP407*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ407/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},{"$f":"AN407+AP407","v":2.3305291073371062E-2},{"$f":"IF(AN407>$G$5,AM407,NA())","v":390},null,{"$f":"(AP407)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF407<=$J$9*1.05,(AV407*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW406,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH407>($G$5*10^6),BH407*0.99,9999)","v":23072.238162637354},{"$f":"AT407+$G$3","v":523},{"$f":"IF(ISNUMBER(AT407),BA407+BB407+BC407+$AZ$17,\"\")","v":6.650857749596554},{"$f":"IF(ISNUMBER(AK407),AK407,BA406)","v":0.84452814959654743},{"$f":"IF(ISNUMBER(AW407),AW407,0)","v":0},2.4463296000000061,null,{"$f":"AR407*10^6","v":4.3827000000643475},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF407*10^6","v":23.470415546510278},{"$f":"AN407*10^6","v":23305.291073371063}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,391,2.3305291073371062E-2,{"$f":"Z408*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF407*Bodencharakterisierung!$E$11/$J$20","v":2.4561491298712363E-5},{"$f":"((150*($J$2^0.87)*(AB408^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z408)*3600*24","v":5.2342109818975469E-2},2.3915996627248484E-4,{"$f":"AE407-AD408*Bodencharakterisierung!$E$8","v":3.547875676409315E-2},{"$f":"IF(AE408>$J$18,(AE408/(Bodencharakterisierung!$E$11*1000)),0)","v":2.3418321296431123E-5},2.3305291073371062E-2,391,null,{"$f":"(AD408)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH408>0,(AJ408*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK407,NA())","v":0.84669561685192318},null,391,{"$f":"IF(AF408<=$J$9*0.05,AS407*EXP((-$J$6*1)/Heterogenität!$D$4),Z408)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF408>=$J$19, AR407/$J$5<AN408),0, Bodencharakterisierung!$E$8*$J$11*((AR407/$J$5)-AN408))","v":0},0,{"$f":"AQ407-AP408*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ408/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,391,null,{"$f":"(AP408)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF408<=$J$9*1.05,(AV408*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW407,NA())","v":{"$error":"#N/A"}},23072.238162637354,524,6.6592978568519294,0.84669561685192318,0,2.4526022400000063,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},23.418321296431124,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,392,2.3305291073371062E-2,{"$f":"Z409*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF408*Bodencharakterisierung!$E$11/$J$20","v":2.4506975328703372E-5},{"$f":"((150*($J$2^0.87)*(AB409^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z409)*3600*24","v":5.2250308563508756E-2},2.3915996627248484E-4,{"$f":"AE408-AD409*Bodencharakterisierung!$E$8","v":3.5399833975223227E-2},{"$f":"IF(AE409>$J$18,(AE409/(Bodencharakterisierung!$E$11*1000)),0)","v":2.3366227046351964E-5},2.3305291073371062E-2,392,null,{"$f":"(AD409)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH409>0,(AJ409*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK408,NA())","v":0.84886308410729894},null,392,{"$f":"IF(AF409<=$J$9*0.05,AS408*EXP((-$J$6*1)/Heterogenität!$D$4),Z409)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF409>=$J$19, AR408/$J$5<AN409),0, Bodencharakterisierung!$E$8*$J$11*((AR408/$J$5)-AN409))","v":0},0,{"$f":"AQ408-AP409*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ409/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,392,null,{"$f":"(AP409)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF409<=$J$9*1.05,(AV409*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW408,NA())","v":{"$error":"#N/A"}},23072.238162637354,525,6.6677379641073049,0.84886308410729894,0,2.4588748800000064,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},23.366227046351963,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,393,2.3305291073371062E-2,{"$f":"Z410*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF409*Bodencharakterisierung!$E$11/$J$20","v":2.4452459358694375E-5},{"$f":"((150*($J$2^0.87)*(AB410^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z410)*3600*24","v":5.215846441332702E-2},2.3915996627248484E-4,{"$f":"AE409-AD410*Bodencharakterisierung!$E$8","v":3.5320911186353304E-2},{"$f":"IF(AE410>$J$18,(AE410/(Bodencharakterisierung!$E$11*1000)),0)","v":2.3314132796272809E-5},2.3305291073371062E-2,393,null,{"$f":"(AD410)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH410>0,(AJ410*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK409,NA())","v":0.85103055136267469},null,393,{"$f":"IF(AF410<=$J$9*0.05,AS409*EXP((-$J$6*1)/Heterogenität!$D$4),Z410)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF410>=$J$19, AR409/$J$5<AN410),0, Bodencharakterisierung!$E$8*$J$11*((AR409/$J$5)-AN410))","v":0},0,{"$f":"AQ409-AP410*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ410/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,393,null,{"$f":"(AP410)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF410<=$J$9*1.05,(AV410*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW409,NA())","v":{"$error":"#N/A"}},23072.238162637354,526,6.6761780713626813,0.85103055136267469,0,2.4651475200000066,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},23.314132796272808,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,394,2.3305291073371062E-2,{"$f":"Z411*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF410*Bodencharakterisierung!$E$11/$J$20","v":2.4397943388685388E-5},{"$f":"((150*($J$2^0.87)*(AB411^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z411)*3600*24","v":5.2066577252688151E-2},2.3915996627248484E-4,{"$f":"AE410-AD411*Bodencharakterisierung!$E$8","v":3.5241988397483381E-2},{"$f":"IF(AE411>$J$18,(AE411/(Bodencharakterisierung!$E$11*1000)),0)","v":2.326203854619365E-5},2.3305291073371062E-2,394,null,{"$f":"(AD411)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH411>0,(AJ411*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK410,NA())","v":0.85319801861805045},null,394,{"$f":"IF(AF411<=$J$9*0.05,AS410*EXP((-$J$6*1)/Heterogenität!$D$4),Z411)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF411>=$J$19, AR410/$J$5<AN411),0, Bodencharakterisierung!$E$8*$J$11*((AR410/$J$5)-AN411))","v":0},0,{"$f":"AQ410-AP411*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ411/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,394,null,{"$f":"(AP411)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF411<=$J$9*1.05,(AV411*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW410,NA())","v":{"$error":"#N/A"}},23072.238162637354,527,6.6846181786180576,0.85319801861805045,0,2.4714201600000067,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},23.262038546193651,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,395,2.3305291073371062E-2,{"$f":"Z412*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF411*Bodencharakterisierung!$E$11/$J$20","v":2.434342741867639E-5},{"$f":"((150*($J$2^0.87)*(AB412^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z412)*3600*24","v":5.197464696527767E-2},2.3915996627248484E-4,{"$f":"AE411-AD412*Bodencharakterisierung!$E$8","v":3.5163065608613459E-2},{"$f":"IF(AE412>$J$18,(AE412/(Bodencharakterisierung!$E$11*1000)),0)","v":2.3209944296114495E-5},2.3305291073371062E-2,395,null,{"$f":"(AD412)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH412>0,(AJ412*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK411,NA())","v":0.8553654858734262},null,395,{"$f":"IF(AF412<=$J$9*0.05,AS411*EXP((-$J$6*1)/Heterogenität!$D$4),Z412)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF412>=$J$19, AR411/$J$5<AN412),0, Bodencharakterisierung!$E$8*$J$11*((AR411/$J$5)-AN412))","v":0},0,{"$f":"AQ411-AP412*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ412/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,395,null,{"$f":"(AP412)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF412<=$J$9*1.05,(AV412*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW411,NA())","v":{"$error":"#N/A"}},23072.238162637354,528,6.6930582858734331,0.8553654858734262,0,2.4776928000000069,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},23.209944296114497,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,396,2.3305291073371062E-2,{"$f":"Z413*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF412*Bodencharakterisierung!$E$11/$J$20","v":2.42889114486674E-5},{"$f":"((150*($J$2^0.87)*(AB413^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z413)*3600*24","v":5.1882673434205724E-2},2.3915996627248484E-4,{"$f":"AE412-AD413*Bodencharakterisierung!$E$8","v":3.5084142819743536E-2},{"$f":"IF(AE413>$J$18,(AE413/(Bodencharakterisierung!$E$11*1000)),0)","v":2.3157850046035337E-5},2.3305291073371062E-2,396,null,{"$f":"(AD413)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH413>0,(AJ413*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK412,NA())","v":0.85753295312880196},null,396,{"$f":"IF(AF413<=$J$9*0.05,AS412*EXP((-$J$6*1)/Heterogenität!$D$4),Z413)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF413>=$J$19, AR412/$J$5<AN413),0, Bodencharakterisierung!$E$8*$J$11*((AR412/$J$5)-AN413))","v":0},0,{"$f":"AQ412-AP413*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ413/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,396,null,{"$f":"(AP413)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF413<=$J$9*1.05,(AV413*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW412,NA())","v":{"$error":"#N/A"}},23072.238162637354,529,6.7014983931288086,0.85753295312880196,0,2.4839654400000071,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},23.157850046035335,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,397,2.3305291073371062E-2,{"$f":"Z414*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF413*Bodencharakterisierung!$E$11/$J$20","v":2.4234395478658402E-5},{"$f":"((150*($J$2^0.87)*(AB414^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z414)*3600*24","v":5.1790656542002517E-2},2.3915996627248484E-4,{"$f":"AE413-AD414*Bodencharakterisierung!$E$8","v":3.5005220030873613E-2},{"$f":"IF(AE414>$J$18,(AE414/(Bodencharakterisierung!$E$11*1000)),0)","v":2.3105755795956181E-5},2.3305291073371062E-2,397,null,{"$f":"(AD414)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH414>0,(AJ414*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK413,NA())","v":0.85970042038417771},null,397,{"$f":"IF(AF414<=$J$9*0.05,AS413*EXP((-$J$6*1)/Heterogenität!$D$4),Z414)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF414>=$J$19, AR413/$J$5<AN414),0, Bodencharakterisierung!$E$8*$J$11*((AR413/$J$5)-AN414))","v":0},0,{"$f":"AQ413-AP414*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ414/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,397,null,{"$f":"(AP414)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF414<=$J$9*1.05,(AV414*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW413,NA())","v":{"$error":"#N/A"}},23072.238162637354,530,6.7099385003841849,0.85970042038417771,0,2.4902380800000072,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},23.105755795956181,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,398,2.3305291073371062E-2,{"$f":"Z415*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF414*Bodencharakterisierung!$E$11/$J$20","v":2.4179879508649415E-5},{"$f":"((150*($J$2^0.87)*(AB415^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z415)*3600*24","v":5.1698596170613884E-2},2.3915996627248484E-4,{"$f":"AE414-AD415*Bodencharakterisierung!$E$8","v":3.492629724200369E-2},{"$f":"IF(AE415>$J$18,(AE415/(Bodencharakterisierung!$E$11*1000)),0)","v":2.3053661545877023E-5},2.3305291073371062E-2,398,null,{"$f":"(AD415)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH415>0,(AJ415*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK414,NA())","v":0.86186788763955346},null,398,{"$f":"IF(AF415<=$J$9*0.05,AS414*EXP((-$J$6*1)/Heterogenität!$D$4),Z415)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF415>=$J$19, AR414/$J$5<AN415),0, Bodencharakterisierung!$E$8*$J$11*((AR414/$J$5)-AN415))","v":0},0,{"$f":"AQ414-AP415*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ415/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,398,null,{"$f":"(AP415)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF415<=$J$9*1.05,(AV415*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW414,NA())","v":{"$error":"#N/A"}},23072.238162637354,531,6.7183786076395613,0.86186788763955346,0,2.4965107200000074,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},23.053661545877024,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,399,2.3305291073371062E-2,{"$f":"Z416*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF415*Bodencharakterisierung!$E$11/$J$20","v":2.4125363538640418E-5},{"$f":"((150*($J$2^0.87)*(AB416^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z416)*3600*24","v":5.1606492201397514E-2},2.3915996627248484E-4,{"$f":"AE415-AD416*Bodencharakterisierung!$E$8","v":3.4847374453133767E-2},{"$f":"IF(AE416>$J$18,(AE416/(Bodencharakterisierung!$E$11*1000)),0)","v":2.3001567295797868E-5},2.3305291073371062E-2,399,null,{"$f":"(AD416)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH416>0,(AJ416*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK415,NA())","v":0.86403535489492922},null,399,{"$f":"IF(AF416<=$J$9*0.05,AS415*EXP((-$J$6*1)/Heterogenität!$D$4),Z416)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF416>=$J$19, AR415/$J$5<AN416),0, Bodencharakterisierung!$E$8*$J$11*((AR415/$J$5)-AN416))","v":0},0,{"$f":"AQ415-AP416*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ416/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,399,null,{"$f":"(AP416)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF416<=$J$9*1.05,(AV416*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW415,NA())","v":{"$error":"#N/A"}},23072.238162637354,532,6.7268187148949368,0.86403535489492922,0,2.5027833600000076,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},23.001567295797866,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,2.3305291073371062E-2,{"$f":"Z417*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF416*Bodencharakterisierung!$E$11/$J$20","v":2.4070847568631431E-5},{"$f":"((150*($J$2^0.87)*(AB417^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z417)*3600*24","v":5.1514344515118368E-2},2.3915996627248484E-4,{"$f":"AE416-AD417*Bodencharakterisierung!$E$8","v":3.4768451664263844E-2},{"$f":"IF(AE417>$J$18,(AE417/(Bodencharakterisierung!$E$11*1000)),0)","v":2.2949473045718709E-5},2.3305291073371062E-2,400,null,{"$f":"(AD417)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH417>0,(AJ417*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK416,NA())","v":0.86620282215030497},null,400,{"$f":"IF(AF417<=$J$9*0.05,AS416*EXP((-$J$6*1)/Heterogenität!$D$4),Z417)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF417>=$J$19, AR416/$J$5<AN417),0, Bodencharakterisierung!$E$8*$J$11*((AR416/$J$5)-AN417))","v":0},0,{"$f":"AQ416-AP417*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ417/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,400,null,{"$f":"(AP417)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF417<=$J$9*1.05,(AV417*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW416,NA())","v":{"$error":"#N/A"}},23072.238162637354,533,6.7352588221503122,0.86620282215030497,0,2.5090560000000077,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},22.949473045718708,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,401,2.3305291073371062E-2,{"$f":"Z418*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF417*Bodencharakterisierung!$E$11/$J$20","v":2.4016331598622433E-5},{"$f":"((150*($J$2^0.87)*(AB418^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z418)*3600*24","v":5.1422152991944331E-2},2.3915996627248484E-4,{"$f":"AE417-AD418*Bodencharakterisierung!$E$8","v":3.4689528875393921E-2},{"$f":"IF(AE418>$J$18,(AE418/(Bodencharakterisierung!$E$11*1000)),0)","v":2.289737879563955E-5},2.3305291073371062E-2,401,null,{"$f":"(AD418)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH418>0,(AJ418*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK417,NA())","v":0.86837028940568073},null,401,{"$f":"IF(AF418<=$J$9*0.05,AS417*EXP((-$J$6*1)/Heterogenität!$D$4),Z418)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF418>=$J$19, AR417/$J$5<AN418),0, Bodencharakterisierung!$E$8*$J$11*((AR417/$J$5)-AN418))","v":0},0,{"$f":"AQ417-AP418*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ418/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,401,null,{"$f":"(AP418)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF418<=$J$9*1.05,(AV418*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW417,NA())","v":{"$error":"#N/A"}},23072.238162637354,534,6.7436989294056886,0.86837028940568073,0,2.5153286400000079,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},22.89737879563955,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,402,2.3305291073371062E-2,{"$f":"Z419*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF418*Bodencharakterisierung!$E$11/$J$20","v":2.3961815628613439E-5},{"$f":"((150*($J$2^0.87)*(AB419^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z419)*3600*24","v":5.1329917511442308E-2},2.3915996627248484E-4,{"$f":"AE418-AD419*Bodencharakterisierung!$E$8","v":3.4610606086523998E-2},{"$f":"IF(AE419>$J$18,(AE419/(Bodencharakterisierung!$E$11*1000)),0)","v":2.2845284545560395E-5},2.3305291073371062E-2,402,null,{"$f":"(AD419)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH419>0,(AJ419*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK418,NA())","v":0.87053775666105648},null,402,{"$f":"IF(AF419<=$J$9*0.05,AS418*EXP((-$J$6*1)/Heterogenität!$D$4),Z419)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF419>=$J$19, AR418/$J$5<AN419),0, Bodencharakterisierung!$E$8*$J$11*((AR418/$J$5)-AN419))","v":0},0,{"$f":"AQ418-AP419*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ419/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,402,null,{"$f":"(AP419)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF419<=$J$9*1.05,(AV419*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW418,NA())","v":{"$error":"#N/A"}},23072.238162637354,535,6.752139036661065,0.87053775666105648,0,2.521601280000008,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},22.845284545560396,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,403,2.3305291073371062E-2,{"$f":"Z420*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF419*Bodencharakterisierung!$E$11/$J$20","v":2.3907299658604445E-5},{"$f":"((150*($J$2^0.87)*(AB420^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z420)*3600*24","v":5.1237637952573314E-2},2.3915996627248484E-4,{"$f":"AE419-AD420*Bodencharakterisierung!$E$8","v":3.4531683297654076E-2},{"$f":"IF(AE420>$J$18,(AE420/(Bodencharakterisierung!$E$11*1000)),0)","v":2.2793190295481236E-5},2.3305291073371062E-2,403,null,{"$f":"(AD420)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH420>0,(AJ420*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK419,NA())","v":0.87270522391643224},null,403,{"$f":"IF(AF420<=$J$9*0.05,AS419*EXP((-$J$6*1)/Heterogenität!$D$4),Z420)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF420>=$J$19, AR419/$J$5<AN420),0, Bodencharakterisierung!$E$8*$J$11*((AR419/$J$5)-AN420))","v":0},0,{"$f":"AQ419-AP420*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ420/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,403,null,{"$f":"(AP420)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF420<=$J$9*1.05,(AV420*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW419,NA())","v":{"$error":"#N/A"}},23072.238162637354,536,6.7605791439164404,0.87270522391643224,0,2.5278739200000082,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},22.793190295481235,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,404,2.3305291073371062E-2,{"$f":"Z421*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF420*Bodencharakterisierung!$E$11/$J$20","v":2.3852783688595451E-5},{"$f":"((150*($J$2^0.87)*(AB421^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z421)*3600*24","v":5.1145314193688042E-2},2.3915996627248484E-4,{"$f":"AE420-AD421*Bodencharakterisierung!$E$8","v":3.4452760508784153E-2},{"$f":"IF(AE421>$J$18,(AE421/(Bodencharakterisierung!$E$11*1000)),0)","v":2.2741096045402081E-5},2.3305291073371062E-2,404,null,{"$f":"(AD421)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH421>0,(AJ421*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK420,NA())","v":0.87487269117180799},null,404,{"$f":"IF(AF421<=$J$9*0.05,AS420*EXP((-$J$6*1)/Heterogenität!$D$4),Z421)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF421>=$J$19, AR420/$J$5<AN421),0, Bodencharakterisierung!$E$8*$J$11*((AR420/$J$5)-AN421))","v":0},0,{"$f":"AQ420-AP421*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ421/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,404,null,{"$f":"(AP421)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF421<=$J$9*1.05,(AV421*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW420,NA())","v":{"$error":"#N/A"}},23072.238162637354,537,6.7690192511718159,0.87487269117180799,0,2.5341465600000084,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},22.741096045402081,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,405,2.3305291073371062E-2,{"$f":"Z422*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF421*Bodencharakterisierung!$E$11/$J$20","v":2.3798267718586461E-5},{"$f":"((150*($J$2^0.87)*(AB422^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z422)*3600*24","v":5.1052946112523132E-2},2.3915996627248484E-4,{"$f":"AE421-AD422*Bodencharakterisierung!$E$8","v":3.437383771991423E-2},{"$f":"IF(AE422>$J$18,(AE422/(Bodencharakterisierung!$E$11*1000)),0)","v":2.2689001795322923E-5},2.3305291073371062E-2,405,null,{"$f":"(AD422)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH422>0,(AJ422*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK421,NA())","v":0.87704015842718375},null,405,{"$f":"IF(AF422<=$J$9*0.05,AS421*EXP((-$J$6*1)/Heterogenität!$D$4),Z422)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF422>=$J$19, AR421/$J$5<AN422),0, Bodencharakterisierung!$E$8*$J$11*((AR421/$J$5)-AN422))","v":0},0,{"$f":"AQ421-AP422*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ422/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,405,null,{"$f":"(AP422)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF422<=$J$9*1.05,(AV422*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW421,NA())","v":{"$error":"#N/A"}},23072.238162637354,538,6.7774593584271923,0.87704015842718375,0,2.5404192000000085,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},22.689001795322923,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,406,2.3305291073371062E-2,{"$f":"Z423*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF422*Bodencharakterisierung!$E$11/$J$20","v":2.3743751748577467E-5},{"$f":"((150*($J$2^0.87)*(AB423^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z423)*3600*24","v":5.0960533586195594E-2},2.3915996627248484E-4,{"$f":"AE422-AD423*Bodencharakterisierung!$E$8","v":3.4294914931044307E-2},{"$f":"IF(AE423>$J$18,(AE423/(Bodencharakterisierung!$E$11*1000)),0)","v":2.2636907545243767E-5},2.3305291073371062E-2,406,null,{"$f":"(AD423)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH423>0,(AJ423*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK422,NA())","v":0.8792076256825595},null,406,{"$f":"IF(AF423<=$J$9*0.05,AS422*EXP((-$J$6*1)/Heterogenität!$D$4),Z423)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF423>=$J$19, AR422/$J$5<AN423),0, Bodencharakterisierung!$E$8*$J$11*((AR422/$J$5)-AN423))","v":0},0,{"$f":"AQ422-AP423*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ423/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,406,null,{"$f":"(AP423)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF423<=$J$9*1.05,(AV423*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW422,NA())","v":{"$error":"#N/A"}},23072.238162637354,539,6.7858994656825686,0.8792076256825595,0,2.5466918400000087,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},22.636907545243769,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,407,2.3305291073371062E-2,{"$f":"Z424*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF423*Bodencharakterisierung!$E$11/$J$20","v":2.3689235778568473E-5},{"$f":"((150*($J$2^0.87)*(AB424^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z424)*3600*24","v":5.0868076491199052E-2},2.3915996627248484E-4,{"$f":"AE423-AD424*Bodencharakterisierung!$E$8","v":3.4215992142174384E-2},{"$f":"IF(AE424>$J$18,(AE424/(Bodencharakterisierung!$E$11*1000)),0)","v":2.2584813295164609E-5},2.3305291073371062E-2,407,null,{"$f":"(AD424)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH424>0,(AJ424*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK423,NA())","v":0.88137509293793526},null,407,{"$f":"IF(AF424<=$J$9*0.05,AS423*EXP((-$J$6*1)/Heterogenität!$D$4),Z424)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF424>=$J$19, AR423/$J$5<AN424),0, Bodencharakterisierung!$E$8*$J$11*((AR423/$J$5)-AN424))","v":0},0,{"$f":"AQ423-AP424*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ424/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,407,null,{"$f":"(AP424)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF424<=$J$9*1.05,(AV424*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW423,NA())","v":{"$error":"#N/A"}},23072.238162637354,540,6.7943395729379441,0.88137509293793526,0,2.5529644800000089,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},22.584813295164608,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,408,2.3305291073371062E-2,{"$f":"Z425*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF424*Bodencharakterisierung!$E$11/$J$20","v":2.3634719808559482E-5},{"$f":"((150*($J$2^0.87)*(AB425^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z425)*3600*24","v":5.0775574703398718E-2},2.3915996627248484E-4,{"$f":"AE424-AD425*Bodencharakterisierung!$E$8","v":3.4137069353304461E-2},{"$f":"IF(AE425>$J$18,(AE425/(Bodencharakterisierung!$E$11*1000)),0)","v":2.2532719045085454E-5},2.3305291073371062E-2,408,null,{"$f":"(AD425)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH425>0,(AJ425*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK424,NA())","v":0.88354256019331101},null,408,{"$f":"IF(AF425<=$J$9*0.05,AS424*EXP((-$J$6*1)/Heterogenität!$D$4),Z425)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF425>=$J$19, AR424/$J$5<AN425),0, Bodencharakterisierung!$E$8*$J$11*((AR424/$J$5)-AN425))","v":0},0,{"$f":"AQ424-AP425*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ425/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,408,null,{"$f":"(AP425)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF425<=$J$9*1.05,(AV425*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW424,NA())","v":{"$error":"#N/A"}},23072.238162637354,541,6.8027796801933196,0.88354256019331101,0,2.559237120000009,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},22.532719045085454,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,409,2.3305291073371062E-2,{"$f":"Z426*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF425*Bodencharakterisierung!$E$11/$J$20","v":2.3580203838550488E-5},{"$f":"((150*($J$2^0.87)*(AB426^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z426)*3600*24","v":5.0683028098026758E-2},2.3915996627248484E-4,{"$f":"AE425-AD426*Bodencharakterisierung!$E$8","v":3.4058146564434538E-2},{"$f":"IF(AE426>$J$18,(AE426/(Bodencharakterisierung!$E$11*1000)),0)","v":2.2480624795006295E-5},2.3305291073371062E-2,409,null,{"$f":"(AD426)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH426>0,(AJ426*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK425,NA())","v":0.88571002744868677},null,409,{"$f":"IF(AF426<=$J$9*0.05,AS425*EXP((-$J$6*1)/Heterogenität!$D$4),Z426)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF426>=$J$19, AR425/$J$5<AN426),0, Bodencharakterisierung!$E$8*$J$11*((AR425/$J$5)-AN426))","v":0},0,{"$f":"AQ425-AP426*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ426/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,409,null,{"$f":"(AP426)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF426<=$J$9*1.05,(AV426*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW425,NA())","v":{"$error":"#N/A"}},23072.238162637354,542,6.8112197874486959,0.88571002744868677,0,2.5655097600000092,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},22.480624795006296,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,410,2.3305291073371062E-2,{"$f":"Z427*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF426*Bodencharakterisierung!$E$11/$J$20","v":2.3525687868541494E-5},{"$f":"((150*($J$2^0.87)*(AB427^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z427)*3600*24","v":5.0590436549677952E-2},2.3915996627248484E-4,{"$f":"AE426-AD427*Bodencharakterisierung!$E$8","v":3.3979223775564615E-2},{"$f":"IF(AE427>$J$18,(AE427/(Bodencharakterisierung!$E$11*1000)),0)","v":2.242853054492714E-5},2.3305291073371062E-2,410,null,{"$f":"(AD427)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH427>0,(AJ427*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK426,NA())","v":0.88787749470406252},null,410,{"$f":"IF(AF427<=$J$9*0.05,AS426*EXP((-$J$6*1)/Heterogenität!$D$4),Z427)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF427>=$J$19, AR426/$J$5<AN427),0, Bodencharakterisierung!$E$8*$J$11*((AR426/$J$5)-AN427))","v":0},0,{"$f":"AQ426-AP427*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ427/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,410,null,{"$f":"(AP427)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF427<=$J$9*1.05,(AV427*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW426,NA())","v":{"$error":"#N/A"}},23072.238162637354,543,6.8196598947040723,0.88787749470406252,0,2.5717824000000093,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},22.428530544927138,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,411,2.3305291073371062E-2,{"$f":"Z428*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF427*Bodencharakterisierung!$E$11/$J$20","v":2.3471171898532504E-5},{"$f":"((150*($J$2^0.87)*(AB428^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z428)*3600*24","v":5.0497799932304535E-2},2.3915996627248484E-4,{"$f":"AE427-AD428*Bodencharakterisierung!$E$8","v":3.3900300986694692E-2},{"$f":"IF(AE428>$J$18,(AE428/(Bodencharakterisierung!$E$11*1000)),0)","v":2.2376436294847981E-5},2.3305291073371062E-2,411,null,{"$f":"(AD428)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH428>0,(AJ428*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK427,NA())","v":0.89004496195943827},null,411,{"$f":"IF(AF428<=$J$9*0.05,AS427*EXP((-$J$6*1)/Heterogenität!$D$4),Z428)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF428>=$J$19, AR427/$J$5<AN428),0, Bodencharakterisierung!$E$8*$J$11*((AR427/$J$5)-AN428))","v":0},0,{"$f":"AQ427-AP428*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ428/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,411,null,{"$f":"(AP428)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF428<=$J$9*1.05,(AV428*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW427,NA())","v":{"$error":"#N/A"}},23072.238162637354,544,6.8281000019594478,0.89004496195943827,0,2.5780550400000095,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},22.376436294847981,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,412,2.3305291073371062E-2,{"$f":"Z429*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF428*Bodencharakterisierung!$E$11/$J$20","v":2.341665592852351E-5},{"$f":"((150*($J$2^0.87)*(AB429^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z429)*3600*24","v":5.0405118119211494E-2},2.3915996627248484E-4,{"$f":"AE428-AD429*Bodencharakterisierung!$E$8","v":3.382137819782477E-2},{"$f":"IF(AE429>$J$18,(AE429/(Bodencharakterisierung!$E$11*1000)),0)","v":2.2324342044768826E-5},2.3305291073371062E-2,412,null,{"$f":"(AD429)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH429>0,(AJ429*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK428,NA())","v":0.89221242921481403},null,412,{"$f":"IF(AF429<=$J$9*0.05,AS428*EXP((-$J$6*1)/Heterogenität!$D$4),Z429)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF429>=$J$19, AR428/$J$5<AN429),0, Bodencharakterisierung!$E$8*$J$11*((AR428/$J$5)-AN429))","v":0},0,{"$f":"AQ428-AP429*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ429/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,412,null,{"$f":"(AP429)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF429<=$J$9*1.05,(AV429*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW428,NA())","v":{"$error":"#N/A"}},23072.238162637354,545,6.8365401092148232,0.89221242921481403,0,2.5843276800000097,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},22.324342044768827,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,413,2.3305291073371062E-2,{"$f":"Z430*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF429*Bodencharakterisierung!$E$11/$J$20","v":2.3362139958514516E-5},{"$f":"((150*($J$2^0.87)*(AB430^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z430)*3600*24","v":5.0312390983052041E-2},2.3915996627248484E-4,{"$f":"AE429-AD430*Bodencharakterisierung!$E$8","v":3.3742455408954847E-2},{"$f":"IF(AE430>$J$18,(AE430/(Bodencharakterisierung!$E$11*1000)),0)","v":2.2272247794689667E-5},2.3305291073371062E-2,413,null,{"$f":"(AD430)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH430>0,(AJ430*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK429,NA())","v":0.89437989647018978},null,413,{"$f":"IF(AF430<=$J$9*0.05,AS429*EXP((-$J$6*1)/Heterogenität!$D$4),Z430)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF430>=$J$19, AR429/$J$5<AN430),0, Bodencharakterisierung!$E$8*$J$11*((AR429/$J$5)-AN430))","v":0},0,{"$f":"AQ429-AP430*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ430/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,413,null,{"$f":"(AP430)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF430<=$J$9*1.05,(AV430*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW429,NA())","v":{"$error":"#N/A"}},23072.238162637354,546,6.8449802164701996,0.89437989647018978,0,2.5906003200000098,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},22.272247794689669,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,414,2.3305291073371062E-2,{"$f":"Z431*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF430*Bodencharakterisierung!$E$11/$J$20","v":2.3307623988505522E-5},{"$f":"((150*($J$2^0.87)*(AB431^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z431)*3600*24","v":5.0219618395822216E-2},2.3915996627248484E-4,{"$f":"AE430-AD431*Bodencharakterisierung!$E$8","v":3.3663532620084924E-2},{"$f":"IF(AE431>$J$18,(AE431/(Bodencharakterisierung!$E$11*1000)),0)","v":2.2220153544610512E-5},2.3305291073371062E-2,414,null,{"$f":"(AD431)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH431>0,(AJ431*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK430,NA())","v":0.89654736372556554},null,414,{"$f":"IF(AF431<=$J$9*0.05,AS430*EXP((-$J$6*1)/Heterogenität!$D$4),Z431)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF431>=$J$19, AR430/$J$5<AN431),0, Bodencharakterisierung!$E$8*$J$11*((AR430/$J$5)-AN431))","v":0},0,{"$f":"AQ430-AP431*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ431/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,414,null,{"$f":"(AP431)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF431<=$J$9*1.05,(AV431*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW430,NA())","v":{"$error":"#N/A"}},23072.238162637354,547,6.853420323725576,0.89654736372556554,0,2.59687296000001,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},22.220153544610511,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,415,2.3305291073371062E-2,{"$f":"Z432*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF431*Bodencharakterisierung!$E$11/$J$20","v":2.3253108018496531E-5},{"$f":"((150*($J$2^0.87)*(AB432^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z432)*3600*24","v":5.0126800228856502E-2},2.3915996627248484E-4,{"$f":"AE431-AD432*Bodencharakterisierung!$E$8","v":3.3584609831215001E-2},{"$f":"IF(AE432>$J$18,(AE432/(Bodencharakterisierung!$E$11*1000)),0)","v":2.2168059294531353E-5},2.3305291073371062E-2,415,null,{"$f":"(AD432)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH432>0,(AJ432*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK431,NA())","v":0.89871483098094129},null,415,{"$f":"IF(AF432<=$J$9*0.05,AS431*EXP((-$J$6*1)/Heterogenität!$D$4),Z432)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF432>=$J$19, AR431/$J$5<AN432),0, Bodencharakterisierung!$E$8*$J$11*((AR431/$J$5)-AN432))","v":0},0,{"$f":"AQ431-AP432*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ432/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,415,null,{"$f":"(AP432)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF432<=$J$9*1.05,(AV432*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW431,NA())","v":{"$error":"#N/A"}},23072.238162637354,548,6.8618604309809514,0.89871483098094129,0,2.6031456000000102,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},22.168059294531353,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,416,2.3305291073371062E-2,{"$f":"Z433*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF432*Bodencharakterisierung!$E$11/$J$20","v":2.3198592048487537E-5},{"$f":"((150*($J$2^0.87)*(AB433^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z433)*3600*24","v":5.0033936352822238E-2},2.3915996627248484E-4,{"$f":"AE432-AD433*Bodencharakterisierung!$E$8","v":3.3505687042345078E-2},{"$f":"IF(AE433>$J$18,(AE433/(Bodencharakterisierung!$E$11*1000)),0)","v":2.2115965044452198E-5},2.3305291073371062E-2,416,null,{"$f":"(AD433)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH433>0,(AJ433*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK432,NA())","v":0.90088229823631705},null,416,{"$f":"IF(AF433<=$J$9*0.05,AS432*EXP((-$J$6*1)/Heterogenität!$D$4),Z433)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF433>=$J$19, AR432/$J$5<AN433),0, Bodencharakterisierung!$E$8*$J$11*((AR432/$J$5)-AN433))","v":0},0,{"$f":"AQ432-AP433*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ433/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,416,null,{"$f":"(AP433)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF433<=$J$9*1.05,(AV433*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW432,NA())","v":{"$error":"#N/A"}},23072.238162637354,549,6.8703005382363269,0.90088229823631705,0,2.6094182400000103,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},22.115965044452199,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,417,2.3305291073371062E-2,{"$f":"Z434*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF433*Bodencharakterisierung!$E$11/$J$20","v":2.3144076078478543E-5},{"$f":"((150*($J$2^0.87)*(AB434^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z434)*3600*24","v":4.9941026637715158E-2},2.3915996627248484E-4,{"$f":"AE433-AD434*Bodencharakterisierung!$E$8","v":3.3426764253475155E-2},{"$f":"IF(AE434>$J$18,(AE434/(Bodencharakterisierung!$E$11*1000)),0)","v":2.206387079437304E-5},2.3305291073371062E-2,417,null,{"$f":"(AD434)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH434>0,(AJ434*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK433,NA())","v":0.9030497654916928},null,417,{"$f":"IF(AF434<=$J$9*0.05,AS433*EXP((-$J$6*1)/Heterogenität!$D$4),Z434)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF434>=$J$19, AR433/$J$5<AN434),0, Bodencharakterisierung!$E$8*$J$11*((AR433/$J$5)-AN434))","v":0},0,{"$f":"AQ433-AP434*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ434/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,417,null,{"$f":"(AP434)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF434<=$J$9*1.05,(AV434*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW433,NA())","v":{"$error":"#N/A"}},23072.238162637354,550,6.8787406454917033,0.9030497654916928,0,2.6156908800000105,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},22.063870794373038,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,418,2.3305291073371062E-2,{"$f":"Z435*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF434*Bodencharakterisierung!$E$11/$J$20","v":2.3089560108469546E-5},{"$f":"((150*($J$2^0.87)*(AB435^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z435)*3600*24","v":4.9848070952853984E-2},2.3915996627248484E-4,{"$f":"AE434-AD435*Bodencharakterisierung!$E$8","v":3.3347841464605232E-2},{"$f":"IF(AE435>$J$18,(AE435/(Bodencharakterisierung!$E$11*1000)),0)","v":2.2011776544293884E-5},2.3305291073371062E-2,418,null,{"$f":"(AD435)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH435>0,(AJ435*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK434,NA())","v":0.90521723274706856},null,418,{"$f":"IF(AF435<=$J$9*0.05,AS434*EXP((-$J$6*1)/Heterogenität!$D$4),Z435)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF435>=$J$19, AR434/$J$5<AN435),0, Bodencharakterisierung!$E$8*$J$11*((AR434/$J$5)-AN435))","v":0},0,{"$f":"AQ434-AP435*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ435/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,418,null,{"$f":"(AP435)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF435<=$J$9*1.05,(AV435*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW434,NA())","v":{"$error":"#N/A"}},23072.238162637354,551,6.8871807527470796,0.90521723274706856,0,2.6219635200000107,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},22.011776544293884,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,419,2.3305291073371062E-2,{"$f":"Z436*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF435*Bodencharakterisierung!$E$11/$J$20","v":2.3035044138460558E-5},{"$f":"((150*($J$2^0.87)*(AB436^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z436)*3600*24","v":4.9755069166875526E-2},2.3915996627248484E-4,{"$f":"AE435-AD436*Bodencharakterisierung!$E$8","v":3.3268918675735309E-2},{"$f":"IF(AE436>$J$18,(AE436/(Bodencharakterisierung!$E$11*1000)),0)","v":2.1959682294214726E-5},2.3305291073371062E-2,419,null,{"$f":"(AD436)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH436>0,(AJ436*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK435,NA())","v":0.90738470000244431},null,419,{"$f":"IF(AF436<=$J$9*0.05,AS435*EXP((-$J$6*1)/Heterogenität!$D$4),Z436)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF436>=$J$19, AR435/$J$5<AN436),0, Bodencharakterisierung!$E$8*$J$11*((AR435/$J$5)-AN436))","v":0},0,{"$f":"AQ435-AP436*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ436/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,419,null,{"$f":"(AP436)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF436<=$J$9*1.05,(AV436*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW435,NA())","v":{"$error":"#N/A"}},23072.238162637354,552,6.8956208600024551,0.90738470000244431,0,2.6282361600000108,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},21.959682294214726,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,420,2.3305291073371062E-2,{"$f":"Z437*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF436*Bodencharakterisierung!$E$11/$J$20","v":2.2980528168451561E-5},{"$f":"((150*($J$2^0.87)*(AB437^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z437)*3600*24","v":4.9662021147729052E-2},2.3915996627248484E-4,{"$f":"AE436-AD437*Bodencharakterisierung!$E$8","v":3.3189995886865387E-2},{"$f":"IF(AE437>$J$18,(AE437/(Bodencharakterisierung!$E$11*1000)),0)","v":2.1907588044135567E-5},2.3305291073371062E-2,420,null,{"$f":"(AD437)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH437>0,(AJ437*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK436,NA())","v":0.90955216725782007},null,420,{"$f":"IF(AF437<=$J$9*0.05,AS436*EXP((-$J$6*1)/Heterogenität!$D$4),Z437)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF437>=$J$19, AR436/$J$5<AN437),0, Bodencharakterisierung!$E$8*$J$11*((AR436/$J$5)-AN437))","v":0},0,{"$f":"AQ436-AP437*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ437/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,420,null,{"$f":"(AP437)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF437<=$J$9*1.05,(AV437*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW436,NA())","v":{"$error":"#N/A"}},23072.238162637354,553,6.9040609672578306,0.90955216725782007,0,2.634508800000011,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},21.907588044135569,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,421,2.3305291073371062E-2,{"$f":"Z438*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF437*Bodencharakterisierung!$E$11/$J$20","v":2.2926012198442567E-5},{"$f":"((150*($J$2^0.87)*(AB438^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z438)*3600*24","v":4.9568926762671578E-2},2.3915996627248484E-4,{"$f":"AE437-AD438*Bodencharakterisierung!$E$8","v":3.3111073097995464E-2},{"$f":"IF(AE438>$J$18,(AE438/(Bodencharakterisierung!$E$11*1000)),0)","v":2.1855493794056412E-5},2.3305291073371062E-2,421,null,{"$f":"(AD438)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH438>0,(AJ438*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK437,NA())","v":0.91171963451319582},null,421,{"$f":"IF(AF438<=$J$9*0.05,AS437*EXP((-$J$6*1)/Heterogenität!$D$4),Z438)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF438>=$J$19, AR437/$J$5<AN438),0, Bodencharakterisierung!$E$8*$J$11*((AR437/$J$5)-AN438))","v":0},0,{"$f":"AQ437-AP438*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ438/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,421,null,{"$f":"(AP438)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF438<=$J$9*1.05,(AV438*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW437,NA())","v":{"$error":"#N/A"}},23072.238162637354,554,6.9125010745132069,0.91171963451319582,0,2.6407814400000111,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},21.855493794056411,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,422,2.3305291073371062E-2,{"$f":"Z439*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF438*Bodencharakterisierung!$E$11/$J$20","v":2.2871496228433576E-5},{"$f":"((150*($J$2^0.87)*(AB439^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z439)*3600*24","v":4.9475785878262409E-2},2.3915996627248484E-4,{"$f":"AE438-AD439*Bodencharakterisierung!$E$8","v":3.3032150309125541E-2},{"$f":"IF(AE439>$J$18,(AE439/(Bodencharakterisierung!$E$11*1000)),0)","v":2.1803399543977253E-5},2.3305291073371062E-2,422,null,{"$f":"(AD439)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH439>0,(AJ439*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK438,NA())","v":0.91388710176857157},null,422,{"$f":"IF(AF439<=$J$9*0.05,AS438*EXP((-$J$6*1)/Heterogenität!$D$4),Z439)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF439>=$J$19, AR438/$J$5<AN439),0, Bodencharakterisierung!$E$8*$J$11*((AR438/$J$5)-AN439))","v":0},0,{"$f":"AQ438-AP439*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ439/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,422,null,{"$f":"(AP439)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF439<=$J$9*1.05,(AV439*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW438,NA())","v":{"$error":"#N/A"}},23072.238162637354,555,6.9209411817685833,0.91388710176857157,0,2.6470540800000113,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},21.803399543977253,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,423,2.3305291073371062E-2,{"$f":"Z440*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF439*Bodencharakterisierung!$E$11/$J$20","v":2.2816980258424582E-5},{"$f":"((150*($J$2^0.87)*(AB440^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z440)*3600*24","v":4.9382598360357487E-2},2.3915996627248484E-4,{"$f":"AE439-AD440*Bodencharakterisierung!$E$8","v":3.2953227520255618E-2},{"$f":"IF(AE440>$J$18,(AE440/(Bodencharakterisierung!$E$11*1000)),0)","v":2.1751305293898098E-5},2.3305291073371062E-2,423,null,{"$f":"(AD440)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH440>0,(AJ440*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK439,NA())","v":0.91605456902394733},null,423,{"$f":"IF(AF440<=$J$9*0.05,AS439*EXP((-$J$6*1)/Heterogenität!$D$4),Z440)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF440>=$J$19, AR439/$J$5<AN440),0, Bodencharakterisierung!$E$8*$J$11*((AR439/$J$5)-AN440))","v":0},0,{"$f":"AQ439-AP440*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ440/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,423,null,{"$f":"(AP440)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF440<=$J$9*1.05,(AV440*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW439,NA())","v":{"$error":"#N/A"}},23072.238162637354,556,6.9293812890239588,0.91605456902394733,0,2.6533267200000115,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},21.751305293898099,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,424,2.3305291073371062E-2,{"$f":"Z441*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF440*Bodencharakterisierung!$E$11/$J$20","v":2.2762464288415588E-5},{"$f":"((150*($J$2^0.87)*(AB441^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z441)*3600*24","v":4.9289364074104419E-2},2.3915996627248484E-4,{"$f":"AE440-AD441*Bodencharakterisierung!$E$8","v":3.2874304731385695E-2},{"$f":"IF(AE441>$J$18,(AE441/(Bodencharakterisierung!$E$11*1000)),0)","v":2.1699211043818939E-5},2.3305291073371062E-2,424,null,{"$f":"(AD441)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH441>0,(AJ441*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK440,NA())","v":0.91822203627932308},null,424,{"$f":"IF(AF441<=$J$9*0.05,AS440*EXP((-$J$6*1)/Heterogenität!$D$4),Z441)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF441>=$J$19, AR440/$J$5<AN441),0, Bodencharakterisierung!$E$8*$J$11*((AR440/$J$5)-AN441))","v":0},0,{"$f":"AQ440-AP441*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ441/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,424,null,{"$f":"(AP441)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF441<=$J$9*1.05,(AV441*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW440,NA())","v":{"$error":"#N/A"}},23072.238162637354,557,6.9378213962793343,0.91822203627932308,0,2.6595993600000116,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},21.699211043818938,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,425,2.3305291073371062E-2,{"$f":"Z442*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF441*Bodencharakterisierung!$E$11/$J$20","v":2.2707948318406594E-5},{"$f":"((150*($J$2^0.87)*(AB442^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z442)*3600*24","v":4.9196082883936954E-2},2.3915996627248484E-4,{"$f":"AE441-AD442*Bodencharakterisierung!$E$8","v":3.2795381942515772E-2},{"$f":"IF(AE442>$J$18,(AE442/(Bodencharakterisierung!$E$11*1000)),0)","v":2.1647116793739784E-5},2.3305291073371062E-2,425,null,{"$f":"(AD442)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH442>0,(AJ442*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK441,NA())","v":0.92038950353469884},null,425,{"$f":"IF(AF442<=$J$9*0.05,AS441*EXP((-$J$6*1)/Heterogenität!$D$4),Z442)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF442>=$J$19, AR441/$J$5<AN442),0, Bodencharakterisierung!$E$8*$J$11*((AR441/$J$5)-AN442))","v":0},0,{"$f":"AQ441-AP442*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ442/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,425,null,{"$f":"(AP442)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF442<=$J$9*1.05,(AV442*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW441,NA())","v":{"$error":"#N/A"}},23072.238162637354,558,6.9462615035347106,0.92038950353469884,0,2.6658720000000118,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},21.647116793739784,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,426,2.3305291073371062E-2,{"$f":"Z443*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF442*Bodencharakterisierung!$E$11/$J$20","v":2.2653432348397604E-5},{"$f":"((150*($J$2^0.87)*(AB443^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z443)*3600*24","v":4.910275465356928E-2},2.3915996627248484E-4,{"$f":"AE442-AD443*Bodencharakterisierung!$E$8","v":3.2716459153645849E-2},{"$f":"IF(AE443>$J$18,(AE443/(Bodencharakterisierung!$E$11*1000)),0)","v":2.1595022543660626E-5},2.3305291073371062E-2,426,null,{"$f":"(AD443)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH443>0,(AJ443*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK442,NA())","v":0.92255697079007459},null,426,{"$f":"IF(AF443<=$J$9*0.05,AS442*EXP((-$J$6*1)/Heterogenität!$D$4),Z443)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF443>=$J$19, AR442/$J$5<AN443),0, Bodencharakterisierung!$E$8*$J$11*((AR442/$J$5)-AN443))","v":0},0,{"$f":"AQ442-AP443*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ443/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,426,null,{"$f":"(AP443)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF443<=$J$9*1.05,(AV443*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW442,NA())","v":{"$error":"#N/A"}},23072.238162637354,559,6.954701610790087,0.92255697079007459,0,2.672144640000012,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},21.595022543660626,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,427,2.3305291073371062E-2,{"$f":"Z444*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF443*Bodencharakterisierung!$E$11/$J$20","v":2.259891637838861E-5},{"$f":"((150*($J$2^0.87)*(AB444^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z444)*3600*24","v":4.9009379245990387E-2},2.3915996627248484E-4,{"$f":"AE443-AD444*Bodencharakterisierung!$E$8","v":3.2637536364775926E-2},{"$f":"IF(AE444>$J$18,(AE444/(Bodencharakterisierung!$E$11*1000)),0)","v":2.154292829358147E-5},2.3305291073371062E-2,427,null,{"$f":"(AD444)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH444>0,(AJ444*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK443,NA())","v":0.92472443804545035},null,427,{"$f":"IF(AF444<=$J$9*0.05,AS443*EXP((-$J$6*1)/Heterogenität!$D$4),Z444)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF444>=$J$19, AR443/$J$5<AN444),0, Bodencharakterisierung!$E$8*$J$11*((AR443/$J$5)-AN444))","v":0},0,{"$f":"AQ443-AP444*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ444/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,427,null,{"$f":"(AP444)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF444<=$J$9*1.05,(AV444*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW443,NA())","v":{"$error":"#N/A"}},23072.238162637354,560,6.9631417180454624,0.92472443804545035,0,2.6784172800000121,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},21.542928293581472,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,428,2.3305291073371062E-2,{"$f":"Z445*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF444*Bodencharakterisierung!$E$11/$J$20","v":2.2544400408379616E-5},{"$f":"((150*($J$2^0.87)*(AB445^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z445)*3600*24","v":4.8915956523459064E-2},2.3915996627248484E-4,{"$f":"AE444-AD445*Bodencharakterisierung!$E$8","v":3.2558613575906004E-2},{"$f":"IF(AE445>$J$18,(AE445/(Bodencharakterisierung!$E$11*1000)),0)","v":2.1490834043502312E-5},2.3305291073371062E-2,428,null,{"$f":"(AD445)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH445>0,(AJ445*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK444,NA())","v":0.9268919053008261},null,428,{"$f":"IF(AF445<=$J$9*0.05,AS444*EXP((-$J$6*1)/Heterogenität!$D$4),Z445)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF445>=$J$19, AR444/$J$5<AN445),0, Bodencharakterisierung!$E$8*$J$11*((AR444/$J$5)-AN445))","v":0},0,{"$f":"AQ444-AP445*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ445/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,428,null,{"$f":"(AP445)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF445<=$J$9*1.05,(AV445*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW444,NA())","v":{"$error":"#N/A"}},23072.238162637354,561,6.9715818253008379,0.9268919053008261,0,2.6846899200000123,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},21.490834043502311,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,429,2.3305291073371062E-2,{"$f":"Z446*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF445*Bodencharakterisierung!$E$11/$J$20","v":2.2489884438370625E-5},{"$f":"((150*($J$2^0.87)*(AB446^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z446)*3600*24","v":4.8822486347497446E-2},2.3915996627248484E-4,{"$f":"AE445-AD446*Bodencharakterisierung!$E$8","v":3.2479690787036081E-2},{"$f":"IF(AE446>$J$18,(AE446/(Bodencharakterisierung!$E$11*1000)),0)","v":2.1438739793423157E-5},2.3305291073371062E-2,429,null,{"$f":"(AD446)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH446>0,(AJ446*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK445,NA())","v":0.92905937255620186},null,429,{"$f":"IF(AF446<=$J$9*0.05,AS445*EXP((-$J$6*1)/Heterogenität!$D$4),Z446)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF446>=$J$19, AR445/$J$5<AN446),0, Bodencharakterisierung!$E$8*$J$11*((AR445/$J$5)-AN446))","v":0},0,{"$f":"AQ445-AP446*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ446/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,429,null,{"$f":"(AP446)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF446<=$J$9*1.05,(AV446*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW445,NA())","v":{"$error":"#N/A"}},23072.238162637354,562,6.9800219325562143,0.92905937255620186,0,2.6909625600000124,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},21.438739793423156,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,430,2.3305291073371062E-2,{"$f":"Z447*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF446*Bodencharakterisierung!$E$11/$J$20","v":2.2435368468361631E-5},{"$f":"((150*($J$2^0.87)*(AB447^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z447)*3600*24","v":4.8728968578885909E-2},2.3915996627248484E-4,{"$f":"AE446-AD447*Bodencharakterisierung!$E$8","v":3.2400767998166158E-2},{"$f":"IF(AE447>$J$18,(AE447/(Bodencharakterisierung!$E$11*1000)),0)","v":2.1386645543343998E-5},2.3305291073371062E-2,430,null,{"$f":"(AD447)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH447>0,(AJ447*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK446,NA())","v":0.93122683981157761},null,430,{"$f":"IF(AF447<=$J$9*0.05,AS446*EXP((-$J$6*1)/Heterogenität!$D$4),Z447)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF447>=$J$19, AR446/$J$5<AN447),0, Bodencharakterisierung!$E$8*$J$11*((AR446/$J$5)-AN447))","v":0},0,{"$f":"AQ446-AP447*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ447/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,430,null,{"$f":"(AP447)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF447<=$J$9*1.05,(AV447*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW446,NA())","v":{"$error":"#N/A"}},23072.238162637354,563,6.9884620398115906,0.93122683981157761,0,2.6972352000000126,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},21.386645543343999,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,431,2.3305291073371062E-2,{"$f":"Z448*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF447*Bodencharakterisierung!$E$11/$J$20","v":2.2380852498352637E-5},{"$f":"((150*($J$2^0.87)*(AB448^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z448)*3600*24","v":4.8635403077656722E-2},2.3915996627248484E-4,{"$f":"AE447-AD448*Bodencharakterisierung!$E$8","v":3.2321845209296235E-2},{"$f":"IF(AE448>$J$18,(AE448/(Bodencharakterisierung!$E$11*1000)),0)","v":2.1334551293264843E-5},2.3305291073371062E-2,431,null,{"$f":"(AD448)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH448>0,(AJ448*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK447,NA())","v":0.93339430706695337},null,431,{"$f":"IF(AF448<=$J$9*0.05,AS447*EXP((-$J$6*1)/Heterogenität!$D$4),Z448)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF448>=$J$19, AR447/$J$5<AN448),0, Bodencharakterisierung!$E$8*$J$11*((AR447/$J$5)-AN448))","v":0},0,{"$f":"AQ447-AP448*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ448/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,431,null,{"$f":"(AP448)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF448<=$J$9*1.05,(AV448*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW447,NA())","v":{"$error":"#N/A"}},23072.238162637354,564,6.9969021470669661,0.93339430706695337,0,2.7035078400000128,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},21.334551293264841,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,432,2.3305291073371062E-2,{"$f":"Z449*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF448*Bodencharakterisierung!$E$11/$J$20","v":2.2326336528343647E-5},{"$f":"((150*($J$2^0.87)*(AB449^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z449)*3600*24","v":4.854178970308877E-2},2.3915996627248484E-4,{"$f":"AE448-AD449*Bodencharakterisierung!$E$8","v":3.2242922420426312E-2},{"$f":"IF(AE449>$J$18,(AE449/(Bodencharakterisierung!$E$11*1000)),0)","v":2.1282457043185684E-5},2.3305291073371062E-2,432,null,{"$f":"(AD449)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH449>0,(AJ449*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK448,NA())","v":0.93556177432232912},null,432,{"$f":"IF(AF449<=$J$9*0.05,AS448*EXP((-$J$6*1)/Heterogenität!$D$4),Z449)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF449>=$J$19, AR448/$J$5<AN449),0, Bodencharakterisierung!$E$8*$J$11*((AR448/$J$5)-AN449))","v":0},0,{"$f":"AQ448-AP449*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ449/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,432,null,{"$f":"(AP449)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF449<=$J$9*1.05,(AV449*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW448,NA())","v":{"$error":"#N/A"}},23072.238162637354,565,7.0053422543223416,0.93556177432232912,0,2.7097804800000129,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},21.282457043185683,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,433,2.3305291073371062E-2,{"$f":"Z450*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF449*Bodencharakterisierung!$E$11/$J$20","v":2.2271820558334653E-5},{"$f":"((150*($J$2^0.87)*(AB450^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z450)*3600*24","v":4.8448128313701024E-2},2.3915996627248484E-4,{"$f":"AE449-AD450*Bodencharakterisierung!$E$8","v":3.2163999631556389E-2},{"$f":"IF(AE450>$J$18,(AE450/(Bodencharakterisierung!$E$11*1000)),0)","v":2.1230362793106529E-5},2.3305291073371062E-2,433,null,{"$f":"(AD450)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH450>0,(AJ450*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK449,NA())","v":0.93772924157770488},null,433,{"$f":"IF(AF450<=$J$9*0.05,AS449*EXP((-$J$6*1)/Heterogenität!$D$4),Z450)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF450>=$J$19, AR449/$J$5<AN450),0, Bodencharakterisierung!$E$8*$J$11*((AR449/$J$5)-AN450))","v":0},0,{"$f":"AQ449-AP450*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ450/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,433,null,{"$f":"(AP450)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF450<=$J$9*1.05,(AV450*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW449,NA())","v":{"$error":"#N/A"}},23072.238162637354,566,7.0137823615777179,0.93772924157770488,0,2.7160531200000131,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},21.230362793106529,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,434,2.3305291073371062E-2,{"$f":"Z451*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF450*Bodencharakterisierung!$E$11/$J$20","v":2.2217304588325659E-5},{"$f":"((150*($J$2^0.87)*(AB451^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z451)*3600*24","v":4.8354418767247304E-2},2.3915996627248484E-4,{"$f":"AE450-AD451*Bodencharakterisierung!$E$8","v":3.2085076842686466E-2},{"$f":"IF(AE451>$J$18,(AE451/(Bodencharakterisierung!$E$11*1000)),0)","v":2.117826854302737E-5},2.3305291073371062E-2,434,null,{"$f":"(AD451)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH451>0,(AJ451*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK450,NA())","v":0.93989670883308063},null,434,{"$f":"IF(AF451<=$J$9*0.05,AS450*EXP((-$J$6*1)/Heterogenität!$D$4),Z451)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF451>=$J$19, AR450/$J$5<AN451),0, Bodencharakterisierung!$E$8*$J$11*((AR450/$J$5)-AN451))","v":0},0,{"$f":"AQ450-AP451*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ451/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,434,null,{"$f":"(AP451)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF451<=$J$9*1.05,(AV451*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW450,NA())","v":{"$error":"#N/A"}},23072.238162637354,567,7.0222224688330943,0.93989670883308063,0,2.7223257600000133,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},21.178268543027372,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,435,2.3305291073371062E-2,{"$f":"Z452*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF451*Bodencharakterisierung!$E$11/$J$20","v":2.2162788618316665E-5},{"$f":"((150*($J$2^0.87)*(AB452^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z452)*3600*24","v":4.8260660920709554E-2},2.3915996627248484E-4,{"$f":"AE451-AD452*Bodencharakterisierung!$E$8","v":3.2006154053816543E-2},{"$f":"IF(AE452>$J$18,(AE452/(Bodencharakterisierung!$E$11*1000)),0)","v":2.1126174292948215E-5},2.3305291073371062E-2,435,null,{"$f":"(AD452)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH452>0,(AJ452*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK451,NA())","v":0.94206417608845638},null,435,{"$f":"IF(AF452<=$J$9*0.05,AS451*EXP((-$J$6*1)/Heterogenität!$D$4),Z452)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF452>=$J$19, AR451/$J$5<AN452),0, Bodencharakterisierung!$E$8*$J$11*((AR451/$J$5)-AN452))","v":0},0,{"$f":"AQ451-AP452*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ452/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,435,null,{"$f":"(AP452)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF452<=$J$9*1.05,(AV452*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW451,NA())","v":{"$error":"#N/A"}},23072.238162637354,568,7.0306625760884698,0.94206417608845638,0,2.7285984000000134,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},21.126174292948214,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,436,2.3305291073371062E-2,{"$f":"Z453*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF452*Bodencharakterisierung!$E$11/$J$20","v":2.2108272648307674E-5},{"$f":"((150*($J$2^0.87)*(AB453^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z453)*3600*24","v":4.8166854630292286E-2},2.3915996627248484E-4,{"$f":"AE452-AD453*Bodencharakterisierung!$E$8","v":3.1927231264946621E-2},{"$f":"IF(AE453>$J$18,(AE453/(Bodencharakterisierung!$E$11*1000)),0)","v":2.1074080042869056E-5},2.3305291073371062E-2,436,null,{"$f":"(AD453)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH453>0,(AJ453*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK452,NA())","v":0.94423164334383214},null,436,{"$f":"IF(AF453<=$J$9*0.05,AS452*EXP((-$J$6*1)/Heterogenität!$D$4),Z453)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF453>=$J$19, AR452/$J$5<AN453),0, Bodencharakterisierung!$E$8*$J$11*((AR452/$J$5)-AN453))","v":0},0,{"$f":"AQ452-AP453*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ453/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,436,null,{"$f":"(AP453)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF453<=$J$9*1.05,(AV453*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW452,NA())","v":{"$error":"#N/A"}},23072.238162637354,569,7.0391026833438453,0.94423164334383214,0,2.7348710400000136,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},21.074080042869056,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,437,2.3305291073371062E-2,{"$f":"Z454*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF453*Bodencharakterisierung!$E$11/$J$20","v":2.205375667829868E-5},{"$f":"((150*($J$2^0.87)*(AB454^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z454)*3600*24","v":4.8072999751415865E-2},2.3915996627248484E-4,{"$f":"AE453-AD454*Bodencharakterisierung!$E$8","v":3.1848308476076698E-2},{"$f":"IF(AE454>$J$18,(AE454/(Bodencharakterisierung!$E$11*1000)),0)","v":2.1021985792789898E-5},2.3305291073371062E-2,437,null,{"$f":"(AD454)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH454>0,(AJ454*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK453,NA())","v":0.94639911059920789},null,437,{"$f":"IF(AF454<=$J$9*0.05,AS453*EXP((-$J$6*1)/Heterogenität!$D$4),Z454)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF454>=$J$19, AR453/$J$5<AN454),0, Bodencharakterisierung!$E$8*$J$11*((AR453/$J$5)-AN454))","v":0},0,{"$f":"AQ453-AP454*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ454/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,437,null,{"$f":"(AP454)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF454<=$J$9*1.05,(AV454*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW453,NA())","v":{"$error":"#N/A"}},23072.238162637354,570,7.0475427905992216,0.94639911059920789,0,2.7411436800000137,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},21.021985792789899,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,438,2.3305291073371062E-2,{"$f":"Z455*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF454*Bodencharakterisierung!$E$11/$J$20","v":2.1999240708289683E-5},{"$f":"((150*($J$2^0.87)*(AB455^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z455)*3600*24","v":4.7979096138711083E-2},2.3915996627248484E-4,{"$f":"AE454-AD455*Bodencharakterisierung!$E$8","v":3.1769385687206775E-2},{"$f":"IF(AE455>$J$18,(AE455/(Bodencharakterisierung!$E$11*1000)),0)","v":2.0969891542710743E-5},2.3305291073371062E-2,438,null,{"$f":"(AD455)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH455>0,(AJ455*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK454,NA())","v":0.94856657785458365},null,438,{"$f":"IF(AF455<=$J$9*0.05,AS454*EXP((-$J$6*1)/Heterogenität!$D$4),Z455)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF455>=$J$19, AR454/$J$5<AN455),0, Bodencharakterisierung!$E$8*$J$11*((AR454/$J$5)-AN455))","v":0},0,{"$f":"AQ454-AP455*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ455/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,438,null,{"$f":"(AP455)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF455<=$J$9*1.05,(AV455*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW454,NA())","v":{"$error":"#N/A"}},23072.238162637354,571,7.055982897854598,0.94856657785458365,0,2.7474163200000139,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},20.969891542710741,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,439,2.3305291073371062E-2,{"$f":"Z456*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF455*Bodencharakterisierung!$E$11/$J$20","v":2.1944724738280696E-5},{"$f":"((150*($J$2^0.87)*(AB456^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z456)*3600*24","v":4.7885143646011846E-2},2.3915996627248484E-4,{"$f":"AE455-AD456*Bodencharakterisierung!$E$8","v":3.1690462898336852E-2},{"$f":"IF(AE456>$J$18,(AE456/(Bodencharakterisierung!$E$11*1000)),0)","v":2.0917797292631584E-5},2.3305291073371062E-2,439,null,{"$f":"(AD456)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH456>0,(AJ456*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK455,NA())","v":0.9507340451099594},null,439,{"$f":"IF(AF456<=$J$9*0.05,AS455*EXP((-$J$6*1)/Heterogenität!$D$4),Z456)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF456>=$J$19, AR455/$J$5<AN456),0, Bodencharakterisierung!$E$8*$J$11*((AR455/$J$5)-AN456))","v":0},0,{"$f":"AQ455-AP456*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ456/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,439,null,{"$f":"(AP456)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF456<=$J$9*1.05,(AV456*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW455,NA())","v":{"$error":"#N/A"}},23072.238162637354,572,7.0644230051099735,0.9507340451099594,0,2.7536889600000141,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},20.917797292631583,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,440,2.3305291073371062E-2,{"$f":"Z457*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF456*Bodencharakterisierung!$E$11/$J$20","v":2.1890208768271698E-5},{"$f":"((150*($J$2^0.87)*(AB457^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z457)*3600*24","v":4.7791142126349724E-2},2.3915996627248484E-4,{"$f":"AE456-AD457*Bodencharakterisierung!$E$8","v":3.1611540109466929E-2},{"$f":"IF(AE457>$J$18,(AE457/(Bodencharakterisierung!$E$11*1000)),0)","v":2.0865703042552429E-5},2.3305291073371062E-2,440,null,{"$f":"(AD457)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH457>0,(AJ457*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK456,NA())","v":0.95290151236533516},null,440,{"$f":"IF(AF457<=$J$9*0.05,AS456*EXP((-$J$6*1)/Heterogenität!$D$4),Z457)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF457>=$J$19, AR456/$J$5<AN457),0, Bodencharakterisierung!$E$8*$J$11*((AR456/$J$5)-AN457))","v":0},0,{"$f":"AQ456-AP457*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ457/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,440,null,{"$f":"(AP457)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF457<=$J$9*1.05,(AV457*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW456,NA())","v":{"$error":"#N/A"}},23072.238162637354,573,7.0728631123653489,0.95290151236533516,0,2.7599616000000142,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},20.865703042552429,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,441,2.3305291073371062E-2,{"$f":"Z458*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF457*Bodencharakterisierung!$E$11/$J$20","v":2.1835692798262708E-5},{"$f":"((150*($J$2^0.87)*(AB458^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z458)*3600*24","v":4.7697091431947128E-2},2.3915996627248484E-4,{"$f":"AE457-AD458*Bodencharakterisierung!$E$8","v":3.1532617320597006E-2},{"$f":"IF(AE458>$J$18,(AE458/(Bodencharakterisierung!$E$11*1000)),0)","v":2.081360879247327E-5},2.3305291073371062E-2,441,null,{"$f":"(AD458)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH458>0,(AJ458*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK457,NA())","v":0.95506897962071091},null,441,{"$f":"IF(AF458<=$J$9*0.05,AS457*EXP((-$J$6*1)/Heterogenität!$D$4),Z458)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF458>=$J$19, AR457/$J$5<AN458),0, Bodencharakterisierung!$E$8*$J$11*((AR457/$J$5)-AN458))","v":0},0,{"$f":"AQ457-AP458*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ458/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,441,null,{"$f":"(AP458)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF458<=$J$9*1.05,(AV458*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW457,NA())","v":{"$error":"#N/A"}},23072.238162637354,574,7.0813032196207253,0.95506897962071091,0,2.7662342400000144,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},20.813608792473271,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,442,2.3305291073371062E-2,{"$f":"Z459*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF458*Bodencharakterisierung!$E$11/$J$20","v":2.178117682825371E-5},{"$f":"((150*($J$2^0.87)*(AB459^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z459)*3600*24","v":4.7602991414210788E-2},2.3915996627248484E-4,{"$f":"AE458-AD459*Bodencharakterisierung!$E$8","v":3.1453694531727083E-2},{"$f":"IF(AE459>$J$18,(AE459/(Bodencharakterisierung!$E$11*1000)),0)","v":2.0761514542394115E-5},2.3305291073371062E-2,442,null,{"$f":"(AD459)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH459>0,(AJ459*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK458,NA())","v":0.95723644687608667},null,442,{"$f":"IF(AF459<=$J$9*0.05,AS458*EXP((-$J$6*1)/Heterogenität!$D$4),Z459)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF459>=$J$19, AR458/$J$5<AN459),0, Bodencharakterisierung!$E$8*$J$11*((AR458/$J$5)-AN459))","v":0},0,{"$f":"AQ458-AP459*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ459/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,442,null,{"$f":"(AP459)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF459<=$J$9*1.05,(AV459*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW458,NA())","v":{"$error":"#N/A"}},23072.238162637354,575,7.0897433268761016,0.95723644687608667,0,2.7725068800000146,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},20.761514542394114,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,443,2.3305291073371062E-2,{"$f":"Z460*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF459*Bodencharakterisierung!$E$11/$J$20","v":2.1726660858244723E-5},{"$f":"((150*($J$2^0.87)*(AB460^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z460)*3600*24","v":4.7508841923725509E-2},2.3915996627248484E-4,{"$f":"AE459-AD460*Bodencharakterisierung!$E$8","v":3.137477174285716E-2},{"$f":"IF(AE460>$J$18,(AE460/(Bodencharakterisierung!$E$11*1000)),0)","v":2.0709420292314956E-5},2.3305291073371062E-2,443,null,{"$f":"(AD460)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH460>0,(AJ460*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK459,NA())","v":0.95940391413146242},null,443,{"$f":"IF(AF460<=$J$9*0.05,AS459*EXP((-$J$6*1)/Heterogenität!$D$4),Z460)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF460>=$J$19, AR459/$J$5<AN460),0, Bodencharakterisierung!$E$8*$J$11*((AR459/$J$5)-AN460))","v":0},0,{"$f":"AQ459-AP460*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ460/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,443,null,{"$f":"(AP460)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF460<=$J$9*1.05,(AV460*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW459,NA())","v":{"$error":"#N/A"}},23072.238162637354,576,7.0981834341314771,0.95940391413146242,0,2.7787795200000147,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},20.709420292314956,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,444,2.3305291073371062E-2,{"$f":"Z461*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF460*Bodencharakterisierung!$E$11/$J$20","v":2.1672144888235726E-5},{"$f":"((150*($J$2^0.87)*(AB461^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z461)*3600*24","v":4.7414642810246849E-2},2.3915996627248484E-4,{"$f":"AE460-AD461*Bodencharakterisierung!$E$8","v":3.1295848953987238E-2},{"$f":"IF(AE461>$J$18,(AE461/(Bodencharakterisierung!$E$11*1000)),0)","v":2.0657326042235801E-5},2.3305291073371062E-2,444,null,{"$f":"(AD461)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH461>0,(AJ461*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK460,NA())","v":0.96157138138683818},null,444,{"$f":"IF(AF461<=$J$9*0.05,AS460*EXP((-$J$6*1)/Heterogenität!$D$4),Z461)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF461>=$J$19, AR460/$J$5<AN461),0, Bodencharakterisierung!$E$8*$J$11*((AR460/$J$5)-AN461))","v":0},0,{"$f":"AQ460-AP461*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ461/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,444,null,{"$f":"(AP461)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF461<=$J$9*1.05,(AV461*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW460,NA())","v":{"$error":"#N/A"}},23072.238162637354,577,7.1066235413868526,0.96157138138683818,0,2.7850521600000149,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},20.657326042235802,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,445,2.3305291073371062E-2,{"$f":"Z462*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF461*Bodencharakterisierung!$E$11/$J$20","v":2.1617628918226735E-5},{"$f":"((150*($J$2^0.87)*(AB462^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z462)*3600*24","v":4.7320393922695519E-2},2.3915996627248484E-4,{"$f":"AE461-AD462*Bodencharakterisierung!$E$8","v":3.1216926165117318E-2},{"$f":"IF(AE462>$J$18,(AE462/(Bodencharakterisierung!$E$11*1000)),0)","v":2.0605231792156646E-5},2.3305291073371062E-2,445,null,{"$f":"(AD462)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH462>0,(AJ462*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK461,NA())","v":0.96373884864221393},null,445,{"$f":"IF(AF462<=$J$9*0.05,AS461*EXP((-$J$6*1)/Heterogenität!$D$4),Z462)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF462>=$J$19, AR461/$J$5<AN462),0, Bodencharakterisierung!$E$8*$J$11*((AR461/$J$5)-AN462))","v":0},0,{"$f":"AQ461-AP462*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ462/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,445,null,{"$f":"(AP462)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF462<=$J$9*1.05,(AV462*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW461,NA())","v":{"$error":"#N/A"}},23072.238162637354,578,7.115063648642229,0.96373884864221393,0,2.791324800000015,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},20.605231792156644,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,446,2.3305291073371062E-2,{"$f":"Z463*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF462*Bodencharakterisierung!$E$11/$J$20","v":2.1563112948217744E-5},{"$f":"((150*($J$2^0.87)*(AB463^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z463)*3600*24","v":4.7226095109149491E-2},2.3915996627248484E-4,{"$f":"AE462-AD463*Bodencharakterisierung!$E$8","v":3.1138003376247399E-2},{"$f":"IF(AE463>$J$18,(AE463/(Bodencharakterisierung!$E$11*1000)),0)","v":2.0553137542077491E-5},2.3305291073371062E-2,446,null,{"$f":"(AD463)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH463>0,(AJ463*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK462,NA())","v":0.96590631589758968},null,446,{"$f":"IF(AF463<=$J$9*0.05,AS462*EXP((-$J$6*1)/Heterogenität!$D$4),Z463)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF463>=$J$19, AR462/$J$5<AN463),0, Bodencharakterisierung!$E$8*$J$11*((AR462/$J$5)-AN463))","v":0},0,{"$f":"AQ462-AP463*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ463/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,446,null,{"$f":"(AP463)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF463<=$J$9*1.05,(AV463*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW462,NA())","v":{"$error":"#N/A"}},23072.238162637354,579,7.1235037558976053,0.96590631589758968,0,2.7975974400000152,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},20.55313754207749,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,447,2.3305291073371062E-2,{"$f":"Z464*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF463*Bodencharakterisierung!$E$11/$J$20","v":2.150859697820875E-5},{"$f":"((150*($J$2^0.87)*(AB464^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z464)*3600*24","v":4.7131746216838154E-2},2.3915996627248484E-4,{"$f":"AE463-AD464*Bodencharakterisierung!$E$8","v":3.1059080587377479E-2},{"$f":"IF(AE464>$J$18,(AE464/(Bodencharakterisierung!$E$11*1000)),0)","v":2.0501043291998335E-5},2.3305291073371062E-2,447,null,{"$f":"(AD464)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH464>0,(AJ464*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK463,NA())","v":0.96807378315296544},null,447,{"$f":"IF(AF464<=$J$9*0.05,AS463*EXP((-$J$6*1)/Heterogenität!$D$4),Z464)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF464>=$J$19, AR463/$J$5<AN464),0, Bodencharakterisierung!$E$8*$J$11*((AR463/$J$5)-AN464))","v":0},0,{"$f":"AQ463-AP464*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ464/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,447,null,{"$f":"(AP464)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF464<=$J$9*1.05,(AV464*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW463,NA())","v":{"$error":"#N/A"}},23072.238162637354,580,7.1319438631529808,0.96807378315296544,0,2.8038700800000154,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},20.501043291998336,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,448,2.3305291073371062E-2,{"$f":"Z465*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF464*Bodencharakterisierung!$E$11/$J$20","v":2.1454081008199763E-5},{"$f":"((150*($J$2^0.87)*(AB465^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z465)*3600*24","v":4.7037347092134259E-2},2.3915996627248484E-4,{"$f":"AE464-AD465*Bodencharakterisierung!$E$8","v":3.098015779850756E-2},{"$f":"IF(AE465>$J$18,(AE465/(Bodencharakterisierung!$E$11*1000)),0)","v":2.044894904191918E-5},2.3305291073371062E-2,448,null,{"$f":"(AD465)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH465>0,(AJ465*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK464,NA())","v":0.97024125040834119},null,448,{"$f":"IF(AF465<=$J$9*0.05,AS464*EXP((-$J$6*1)/Heterogenität!$D$4),Z465)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF465>=$J$19, AR464/$J$5<AN465),0, Bodencharakterisierung!$E$8*$J$11*((AR464/$J$5)-AN465))","v":0},0,{"$f":"AQ464-AP465*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ465/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,448,null,{"$f":"(AP465)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF465<=$J$9*1.05,(AV465*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW464,NA())","v":{"$error":"#N/A"}},23072.238162637354,581,7.1403839704083563,0.97024125040834119,0,2.8101427200000155,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},20.448949041919182,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,449,2.3305291073371062E-2,{"$f":"Z466*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF465*Bodencharakterisierung!$E$11/$J$20","v":2.1399565038190769E-5},{"$f":"((150*($J$2^0.87)*(AB466^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z466)*3600*24","v":4.6942897580548329E-2},2.3915996627248484E-4,{"$f":"AE465-AD466*Bodencharakterisierung!$E$8","v":3.090123500963764E-2},{"$f":"IF(AE466>$J$18,(AE466/(Bodencharakterisierung!$E$11*1000)),0)","v":2.0396854791840028E-5},2.3305291073371062E-2,449,null,{"$f":"(AD466)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH466>0,(AJ466*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK465,NA())","v":0.97240871766371695},null,449,{"$f":"IF(AF466<=$J$9*0.05,AS465*EXP((-$J$6*1)/Heterogenität!$D$4),Z466)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF466>=$J$19, AR465/$J$5<AN466),0, Bodencharakterisierung!$E$8*$J$11*((AR465/$J$5)-AN466))","v":0},0,{"$f":"AQ465-AP466*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ466/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,449,null,{"$f":"(AP466)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF466<=$J$9*1.05,(AV466*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW465,NA())","v":{"$error":"#N/A"}},23072.238162637354,582,7.1488240776637326,0.97240871766371695,0,2.8164153600000157,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},20.396854791840028,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,450,2.3305291073371062E-2,{"$f":"Z467*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF466*Bodencharakterisierung!$E$11/$J$20","v":2.1345049068181782E-5},{"$f":"((150*($J$2^0.87)*(AB467^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z467)*3600*24","v":4.6848397526720292E-2},2.3915996627248484E-4,{"$f":"AE466-AD467*Bodencharakterisierung!$E$8","v":3.0822312220767721E-2},{"$f":"IF(AE467>$J$18,(AE467/(Bodencharakterisierung!$E$11*1000)),0)","v":2.0344760541760873E-5},2.3305291073371062E-2,450,null,{"$f":"(AD467)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH467>0,(AJ467*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK466,NA())","v":0.9745761849190927},null,450,{"$f":"IF(AF467<=$J$9*0.05,AS466*EXP((-$J$6*1)/Heterogenität!$D$4),Z467)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF467>=$J$19, AR466/$J$5<AN467),0, Bodencharakterisierung!$E$8*$J$11*((AR466/$J$5)-AN467))","v":0},0,{"$f":"AQ466-AP467*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ467/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,450,null,{"$f":"(AP467)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF467<=$J$9*1.05,(AV467*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW466,NA())","v":{"$error":"#N/A"}},23072.238162637354,583,7.157264184919109,0.9745761849190927,0,2.8226880000000159,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},20.344760541760873,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,451,2.3305291073371062E-2,{"$f":"Z468*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF467*Bodencharakterisierung!$E$11/$J$20","v":2.1290533098172791E-5},{"$f":"((150*($J$2^0.87)*(AB468^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z468)*3600*24","v":4.6753846774413278E-2},2.3915996627248484E-4,{"$f":"AE467-AD468*Bodencharakterisierung!$E$8","v":3.0743389431897802E-2},{"$f":"IF(AE468>$J$18,(AE468/(Bodencharakterisierung!$E$11*1000)),0)","v":2.0292666291681718E-5},2.3305291073371062E-2,451,null,{"$f":"(AD468)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH468>0,(AJ468*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK467,NA())","v":0.97674365217446846},null,451,{"$f":"IF(AF468<=$J$9*0.05,AS467*EXP((-$J$6*1)/Heterogenität!$D$4),Z468)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF468>=$J$19, AR467/$J$5<AN468),0, Bodencharakterisierung!$E$8*$J$11*((AR467/$J$5)-AN468))","v":0},0,{"$f":"AQ467-AP468*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ468/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,451,null,{"$f":"(AP468)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF468<=$J$9*1.05,(AV468*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW467,NA())","v":{"$error":"#N/A"}},23072.238162637354,584,7.1657042921744845,0.97674365217446846,0,{"$f":"$G$34/$G$12/$G$8+BC467","v":2.828960640000016},null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},20.292666291681719,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,452,2.3305291073371062E-2,{"$f":"Z469*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF468*Bodencharakterisierung!$E$11/$J$20","v":2.1236017128163801E-5},{"$f":"((150*($J$2^0.87)*(AB469^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z469)*3600*24","v":4.665924516650586E-2},2.3915996627248484E-4,{"$f":"AE468-AD469*Bodencharakterisierung!$E$8","v":3.0664466643027882E-2},{"$f":"IF(AE469>$J$18,(AE469/(Bodencharakterisierung!$E$11*1000)),0)","v":2.0240572041602563E-5},2.3305291073371062E-2,452,null,{"$f":"(AD469)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH469>0,(AJ469*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK468,NA())","v":0.97891111942984421},null,452,{"$f":"IF(AF469<=$J$9*0.05,AS468*EXP((-$J$6*1)/Heterogenität!$D$4),Z469)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF469>=$J$19, AR468/$J$5<AN469),0, Bodencharakterisierung!$E$8*$J$11*((AR468/$J$5)-AN469))","v":0},0,{"$f":"AQ468-AP469*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ469/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,452,null,{"$f":"(AP469)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF469<=$J$9*1.05,(AV469*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW468,NA())","v":{"$error":"#N/A"}},23072.238162637354,585,7.1741443994298599,0.97891111942984421,0,2.8352332800000162,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},20.240572041602562,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,453,2.3305291073371062E-2,{"$f":"Z470*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF469*Bodencharakterisierung!$E$11/$J$20","v":2.1181501158154807E-5},{"$f":"((150*($J$2^0.87)*(AB470^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z470)*3600*24","v":4.6564592544985059E-2},2.3915996627248484E-4,{"$f":"AE469-AD470*Bodencharakterisierung!$E$8","v":3.0585543854157963E-2},{"$f":"IF(AE470>$J$18,(AE470/(Bodencharakterisierung!$E$11*1000)),0)","v":2.0188477791523407E-5},2.3305291073371062E-2,453,null,{"$f":"(AD470)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH470>0,(AJ470*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK469,NA())","v":0.98107858668521997},null,453,{"$f":"IF(AF470<=$J$9*0.05,AS469*EXP((-$J$6*1)/Heterogenität!$D$4),Z470)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF470>=$J$19, AR469/$J$5<AN470),0, Bodencharakterisierung!$E$8*$J$11*((AR469/$J$5)-AN470))","v":0},0,{"$f":"AQ469-AP470*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ470/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,453,null,{"$f":"(AP470)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF470<=$J$9*1.05,(AV470*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW469,NA())","v":{"$error":"#N/A"}},23072.238162637354,586,7.1825845066852363,0.98107858668521997,0,2.8415059200000163,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},20.188477791523407,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,454,{"$f":"AG470","v":2.3305291073371062E-2},{"$f":"Z471*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF470*Bodencharakterisierung!$E$11/$J$20","v":2.112698518814582E-5},{"$f":"((150*($J$2^0.87)*(AB471^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z471)*3600*24","v":4.6469888750938944E-2},{"$f":"MIN(AC471,Z471-AA471)","v":2.3915996627248484E-4},{"$f":"AE470-AD471*Bodencharakterisierung!$E$8","v":3.0506621065288043E-2},{"$f":"IF(AE471>$J$18,(AE471/(Bodencharakterisierung!$E$11*1000)),0)","v":2.0136383541444252E-5},{"$f":"AA471+AD471","v":2.3305291073371062E-2},{"$f":"IF(AD471>0,Y471,NA())","v":454},null,{"$f":"(AD471)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH471>0,(AJ471*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK470,NA())","v":0.98324605394059572},null,454,{"$f":"IF(AF471<=$J$9*0.05,AS470*EXP((-$J$6*1)/Heterogenität!$D$4),Z471)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF471>=$J$19, AR470/$J$5<AN471),0, Bodencharakterisierung!$E$8*$J$11*((AR470/$J$5)-AN471))","v":0},{"$f":"MIN(AO471,AS470-AN471)","v":0},{"$f":"AQ470-AP471*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ471/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},{"$f":"AN471+AP471","v":2.3305291073371062E-2},{"$f":"IF(AN471>$G$5,AM471,NA())","v":454},null,{"$f":"(AP471)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF471<=$J$9*1.05,(AV471*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW470,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH471>($G$5*10^6),BH471*0.99,9999)","v":23072.238162637354},{"$f":"AT471+$G$3","v":587},{"$f":"IF(ISNUMBER(AT471),BA471+BB471+BC471+$AZ$17,\"\")","v":7.1910246139406127},{"$f":"IF(ISNUMBER(AK471),AK471,BA470)","v":0.98324605394059572},{"$f":"IF(ISNUMBER(AW471),AW471,0)","v":0},2.8477785600000165,null,{"$f":"AR471*10^6","v":4.3827000000643475},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF471*10^6","v":20.136383541444253},{"$f":"AN471*10^6","v":23305.291073371063}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,455,2.3305291073371062E-2,{"$f":"Z472*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF471*Bodencharakterisierung!$E$11/$J$20","v":2.1072469218136826E-5},{"$f":"((150*($J$2^0.87)*(AB472^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z472)*3600*24","v":4.6375133624548794E-2},2.3915996627248484E-4,{"$f":"AE471-AD472*Bodencharakterisierung!$E$8","v":3.0427698276418124E-2},{"$f":"IF(AE472>$J$18,(AE472/(Bodencharakterisierung!$E$11*1000)),0)","v":2.0084289291365097E-5},2.3305291073371062E-2,455,null,{"$f":"(AD472)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH472>0,(AJ472*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK471,NA())","v":0.98541352119597148},null,455,{"$f":"IF(AF472<=$J$9*0.05,AS471*EXP((-$J$6*1)/Heterogenität!$D$4),Z472)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF472>=$J$19, AR471/$J$5<AN472),0, Bodencharakterisierung!$E$8*$J$11*((AR471/$J$5)-AN472))","v":0},0,{"$f":"AQ471-AP472*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ472/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,455,null,{"$f":"(AP472)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF472<=$J$9*1.05,(AV472*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW471,NA())","v":{"$error":"#N/A"}},23072.238162637354,588,7.1994647211959881,0.98541352119597148,0,2.8540512000000167,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},20.084289291365096,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,456,2.3305291073371062E-2,{"$f":"Z473*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF472*Bodencharakterisierung!$E$11/$J$20","v":2.1017953248127835E-5},{"$f":"((150*($J$2^0.87)*(AB473^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z473)*3600*24","v":4.6280327005082202E-2},2.3915996627248484E-4,{"$f":"AE472-AD473*Bodencharakterisierung!$E$8","v":3.0348775487548205E-2},{"$f":"IF(AE473>$J$18,(AE473/(Bodencharakterisierung!$E$11*1000)),0)","v":2.0032195041285945E-5},2.3305291073371062E-2,456,null,{"$f":"(AD473)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH473>0,(AJ473*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK472,NA())","v":0.98758098845134723},null,456,{"$f":"IF(AF473<=$J$9*0.05,AS472*EXP((-$J$6*1)/Heterogenität!$D$4),Z473)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF473>=$J$19, AR472/$J$5<AN473),0, Bodencharakterisierung!$E$8*$J$11*((AR472/$J$5)-AN473))","v":0},0,{"$f":"AQ472-AP473*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ473/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,456,null,{"$f":"(AP473)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF473<=$J$9*1.05,(AV473*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW472,NA())","v":{"$error":"#N/A"}},23072.238162637354,589,7.2079048284513636,0.98758098845134723,0,2.8603238400000168,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},20.032195041285945,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,457,2.3305291073371062E-2,{"$f":"Z474*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF473*Bodencharakterisierung!$E$11/$J$20","v":2.0963437278118848E-5},{"$f":"((150*($J$2^0.87)*(AB474^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z474)*3600*24","v":4.618546873088504E-2},2.3915996627248484E-4,{"$f":"AE473-AD474*Bodencharakterisierung!$E$8","v":3.0269852698678285E-2},{"$f":"IF(AE474>$J$18,(AE474/(Bodencharakterisierung!$E$11*1000)),0)","v":1.998010079120679E-5},2.3305291073371062E-2,457,null,{"$f":"(AD474)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH474>0,(AJ474*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK473,NA())","v":0.98974845570672298},null,457,{"$f":"IF(AF474<=$J$9*0.05,AS473*EXP((-$J$6*1)/Heterogenität!$D$4),Z474)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF474>=$J$19, AR473/$J$5<AN474),0, Bodencharakterisierung!$E$8*$J$11*((AR473/$J$5)-AN474))","v":0},0,{"$f":"AQ473-AP474*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ474/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,457,null,{"$f":"(AP474)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF474<=$J$9*1.05,(AV474*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW473,NA())","v":{"$error":"#N/A"}},23072.238162637354,590,7.21634493570674,0.98974845570672298,0,2.866596480000017,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},19.980100791206791,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,458,2.3305291073371062E-2,{"$f":"Z475*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF474*Bodencharakterisierung!$E$11/$J$20","v":2.0908921308109857E-5},{"$f":"((150*($J$2^0.87)*(AB475^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z475)*3600*24","v":4.6090558639373877E-2},2.3915996627248484E-4,{"$f":"AE474-AD475*Bodencharakterisierung!$E$8","v":3.0190929909808366E-2},{"$f":"IF(AE475>$J$18,(AE475/(Bodencharakterisierung!$E$11*1000)),0)","v":1.9928006541127635E-5},2.3305291073371062E-2,458,null,{"$f":"(AD475)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH475>0,(AJ475*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK474,NA())","v":0.99191592296209874},null,458,{"$f":"IF(AF475<=$J$9*0.05,AS474*EXP((-$J$6*1)/Heterogenität!$D$4),Z475)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF475>=$J$19, AR474/$J$5<AN475),0, Bodencharakterisierung!$E$8*$J$11*((AR474/$J$5)-AN475))","v":0},0,{"$f":"AQ474-AP475*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ475/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,458,null,{"$f":"(AP475)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF475<=$J$9*1.05,(AV475*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW474,NA())","v":{"$error":"#N/A"}},23072.238162637354,591,7.2247850429621163,0.99191592296209874,0,2.8728691200000172,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},19.928006541127633,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,459,2.3305291073371062E-2,{"$f":"Z476*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF475*Bodencharakterisierung!$E$11/$J$20","v":2.0854405338100863E-5},{"$f":"((150*($J$2^0.87)*(AB476^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z476)*3600*24","v":4.5995596567028285E-2},2.3915996627248484E-4,{"$f":"AE475-AD476*Bodencharakterisierung!$E$8","v":3.0112007120938446E-2},{"$f":"IF(AE476>$J$18,(AE476/(Bodencharakterisierung!$E$11*1000)),0)","v":1.9875912291048479E-5},2.3305291073371062E-2,459,null,{"$f":"(AD476)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH476>0,(AJ476*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK475,NA())","v":0.99408339021747449},null,459,{"$f":"IF(AF476<=$J$9*0.05,AS475*EXP((-$J$6*1)/Heterogenität!$D$4),Z476)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF476>=$J$19, AR475/$J$5<AN476),0, Bodencharakterisierung!$E$8*$J$11*((AR475/$J$5)-AN476))","v":0},0,{"$f":"AQ475-AP476*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ476/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,459,null,{"$f":"(AP476)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF476<=$J$9*1.05,(AV476*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW475,NA())","v":{"$error":"#N/A"}},23072.238162637354,592,7.2332251502174918,0.99408339021747449,0,2.8791417600000173,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},19.875912291048479,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,460,2.3305291073371062E-2,{"$f":"Z477*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF476*Bodencharakterisierung!$E$11/$J$20","v":2.0799889368091873E-5},{"$f":"((150*($J$2^0.87)*(AB477^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z477)*3600*24","v":4.5900582349382581E-2},2.3915996627248484E-4,{"$f":"AE476-AD477*Bodencharakterisierung!$E$8","v":3.0033084332068527E-2},{"$f":"IF(AE477>$J$18,(AE477/(Bodencharakterisierung!$E$11*1000)),0)","v":1.9823818040969324E-5},2.3305291073371062E-2,460,null,{"$f":"(AD477)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH477>0,(AJ477*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK476,NA())","v":0.99625085747285025},null,460,{"$f":"IF(AF477<=$J$9*0.05,AS476*EXP((-$J$6*1)/Heterogenität!$D$4),Z477)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF477>=$J$19, AR476/$J$5<AN477),0, Bodencharakterisierung!$E$8*$J$11*((AR476/$J$5)-AN477))","v":0},0,{"$f":"AQ476-AP477*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ477/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,460,null,{"$f":"(AP477)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF477<=$J$9*1.05,(AV477*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW476,NA())","v":{"$error":"#N/A"}},23072.238162637354,593,7.2416652574728673,0.99625085747285025,0,2.8854144000000175,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},19.823818040969325,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,461,2.3305291073371062E-2,{"$f":"Z478*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF477*Bodencharakterisierung!$E$11/$J$20","v":2.0745373398082882E-5},{"$f":"((150*($J$2^0.87)*(AB478^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z478)*3600*24","v":4.5805515821018571E-2},2.3915996627248484E-4,{"$f":"AE477-AD478*Bodencharakterisierung!$E$8","v":2.9954161543198608E-2},{"$f":"IF(AE478>$J$18,(AE478/(Bodencharakterisierung!$E$11*1000)),0)","v":1.9771723790890169E-5},2.3305291073371062E-2,461,null,{"$f":"(AD478)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH478>0,(AJ478*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK477,NA())","v":0.998418324728226},null,461,{"$f":"IF(AF478<=$J$9*0.05,AS477*EXP((-$J$6*1)/Heterogenität!$D$4),Z478)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF478>=$J$19, AR477/$J$5<AN478),0, Bodencharakterisierung!$E$8*$J$11*((AR477/$J$5)-AN478))","v":0},0,{"$f":"AQ477-AP478*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ478/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,461,null,{"$f":"(AP478)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF478<=$J$9*1.05,(AV478*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW477,NA())","v":{"$error":"#N/A"}},23072.238162637354,594,7.2501053647282436,0.998418324728226,0,2.8916870400000176,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},19.771723790890167,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,462,2.3305291073371062E-2,{"$f":"Z479*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF478*Bodencharakterisierung!$E$11/$J$20","v":2.0690857428073891E-5},{"$f":"((150*($J$2^0.87)*(AB479^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z479)*3600*24","v":4.5710396815556831E-2},2.3915996627248484E-4,{"$f":"AE478-AD479*Bodencharakterisierung!$E$8","v":2.9875238754328688E-2},{"$f":"IF(AE479>$J$18,(AE479/(Bodencharakterisierung!$E$11*1000)),0)","v":1.9719629540811014E-5},2.3305291073371062E-2,462,null,{"$f":"(AD479)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH479>0,(AJ479*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK478,NA())","v":1.0005857919836019},null,462,{"$f":"IF(AF479<=$J$9*0.05,AS478*EXP((-$J$6*1)/Heterogenität!$D$4),Z479)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF479>=$J$19, AR478/$J$5<AN479),0, Bodencharakterisierung!$E$8*$J$11*((AR478/$J$5)-AN479))","v":0},0,{"$f":"AQ478-AP479*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ479/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,462,null,{"$f":"(AP479)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF479<=$J$9*1.05,(AV479*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW478,NA())","v":{"$error":"#N/A"}},23072.238162637354,595,7.25854547198362,1.0005857919836019,0,2.8979596800000178,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},19.719629540811013,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,463,2.3305291073371062E-2,{"$f":"Z480*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF479*Bodencharakterisierung!$E$11/$J$20","v":2.0636341458064897E-5},{"$f":"((150*($J$2^0.87)*(AB480^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z480)*3600*24","v":4.5615225165648941E-2},2.3915996627248484E-4,{"$f":"AE479-AD480*Bodencharakterisierung!$E$8","v":2.9796315965458769E-2},{"$f":"IF(AE480>$J$18,(AE480/(Bodencharakterisierung!$E$11*1000)),0)","v":1.9667535290731862E-5},2.3305291073371062E-2,463,null,{"$f":"(AD480)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH480>0,(AJ480*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK479,NA())","v":1.0027532592389776},null,463,{"$f":"IF(AF480<=$J$9*0.05,AS479*EXP((-$J$6*1)/Heterogenität!$D$4),Z480)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF480>=$J$19, AR479/$J$5<AN480),0, Bodencharakterisierung!$E$8*$J$11*((AR479/$J$5)-AN480))","v":0},0,{"$f":"AQ479-AP480*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ480/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,463,null,{"$f":"(AP480)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF480<=$J$9*1.05,(AV480*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW479,NA())","v":{"$error":"#N/A"}},23072.238162637354,596,7.2669855792389955,1.0027532592389776,0,2.904232320000018,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},19.667535290731863,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,464,2.3305291073371062E-2,{"$f":"Z481*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF480*Bodencharakterisierung!$E$11/$J$20","v":2.058182548805591E-5},{"$f":"((150*($J$2^0.87)*(AB481^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z481)*3600*24","v":4.5520000702969167E-2},2.3915996627248484E-4,{"$f":"AE480-AD481*Bodencharakterisierung!$E$8","v":2.9717393176588849E-2},{"$f":"IF(AE481>$J$18,(AE481/(Bodencharakterisierung!$E$11*1000)),0)","v":1.9615441040652707E-5},2.3305291073371062E-2,464,null,{"$f":"(AD481)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH481>0,(AJ481*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK480,NA())","v":1.0049207264943534},null,464,{"$f":"IF(AF481<=$J$9*0.05,AS480*EXP((-$J$6*1)/Heterogenität!$D$4),Z481)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF481>=$J$19, AR480/$J$5<AN481),0, Bodencharakterisierung!$E$8*$J$11*((AR480/$J$5)-AN481))","v":0},0,{"$f":"AQ480-AP481*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ481/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,464,null,{"$f":"(AP481)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF481<=$J$9*1.05,(AV481*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW480,NA())","v":{"$error":"#N/A"}},23072.238162637354,597,7.2754256864943709,1.0049207264943534,0,2.9105049600000181,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},19.615441040652708,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,465,2.3305291073371062E-2,{"$f":"Z482*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF481*Bodencharakterisierung!$E$11/$J$20","v":2.052730951804692E-5},{"$f":"((150*($J$2^0.87)*(AB482^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z482)*3600*24","v":4.5424723258206262E-2},2.3915996627248484E-4,{"$f":"AE481-AD482*Bodencharakterisierung!$E$8","v":2.963847038771893E-2},{"$f":"IF(AE482>$J$18,(AE482/(Bodencharakterisierung!$E$11*1000)),0)","v":1.9563346790573551E-5},2.3305291073371062E-2,465,null,{"$f":"(AD482)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH482>0,(AJ482*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK481,NA())","v":1.0070881937497291},null,465,{"$f":"IF(AF482<=$J$9*0.05,AS481*EXP((-$J$6*1)/Heterogenität!$D$4),Z482)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF482>=$J$19, AR481/$J$5<AN482),0, Bodencharakterisierung!$E$8*$J$11*((AR481/$J$5)-AN482))","v":0},0,{"$f":"AQ481-AP482*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ482/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,465,null,{"$f":"(AP482)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF482<=$J$9*1.05,(AV482*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW481,NA())","v":{"$error":"#N/A"}},23072.238162637354,598,7.2838657937497473,1.0070881937497291,0,2.9167776000000183,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},19.563346790573551,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,466,2.3305291073371062E-2,{"$f":"Z483*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF482*Bodencharakterisierung!$E$11/$J$20","v":2.0472793548037929E-5},{"$f":"((150*($J$2^0.87)*(AB483^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z483)*3600*24","v":4.5329392661054929E-2},2.3915996627248484E-4,{"$f":"AE482-AD483*Bodencharakterisierung!$E$8","v":2.9559547598849011E-2},{"$f":"IF(AE483>$J$18,(AE483/(Bodencharakterisierung!$E$11*1000)),0)","v":1.9511252540494396E-5},2.3305291073371062E-2,466,null,{"$f":"(AD483)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH483>0,(AJ483*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK482,NA())","v":1.0092556610051049},null,466,{"$f":"IF(AF483<=$J$9*0.05,AS482*EXP((-$J$6*1)/Heterogenität!$D$4),Z483)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF483>=$J$19, AR482/$J$5<AN483),0, Bodencharakterisierung!$E$8*$J$11*((AR482/$J$5)-AN483))","v":0},0,{"$f":"AQ482-AP483*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ483/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,466,null,{"$f":"(AP483)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF483<=$J$9*1.05,(AV483*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW482,NA())","v":{"$error":"#N/A"}},23072.238162637354,599,7.2923059010051237,1.0092556610051049,0,2.9230502400000185,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},19.511252540494397,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,467,2.3305291073371062E-2,{"$f":"Z484*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF483*Bodencharakterisierung!$E$11/$J$20","v":2.0418277578028938E-5},{"$f":"((150*($J$2^0.87)*(AB484^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z484)*3600*24","v":4.52340087402072E-2},2.3915996627248484E-4,{"$f":"AE483-AD484*Bodencharakterisierung!$E$8","v":2.9480624809979091E-2},{"$f":"IF(AE484>$J$18,(AE484/(Bodencharakterisierung!$E$11*1000)),0)","v":1.9459158290415241E-5},2.3305291073371062E-2,467,null,{"$f":"(AD484)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH484>0,(AJ484*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK483,NA())","v":1.0114231282604806},null,467,{"$f":"IF(AF484<=$J$9*0.05,AS483*EXP((-$J$6*1)/Heterogenität!$D$4),Z484)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF484>=$J$19, AR483/$J$5<AN484),0, Bodencharakterisierung!$E$8*$J$11*((AR483/$J$5)-AN484))","v":0},0,{"$f":"AQ483-AP484*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ484/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,467,null,{"$f":"(AP484)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF484<=$J$9*1.05,(AV484*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW483,NA())","v":{"$error":"#N/A"}},23072.238162637354,600,7.3007460082604991,1.0114231282604806,0,2.9293228800000186,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},19.459158290415242,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,468,2.3305291073371062E-2,{"$f":"Z485*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF484*Bodencharakterisierung!$E$11/$J$20","v":2.0363761608019944E-5},{"$f":"((150*($J$2^0.87)*(AB485^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z485)*3600*24","v":4.5138571323344222E-2},2.3915996627248484E-4,{"$f":"AE484-AD485*Bodencharakterisierung!$E$8","v":2.9401702021109172E-2},{"$f":"IF(AE485>$J$18,(AE485/(Bodencharakterisierung!$E$11*1000)),0)","v":1.9407064040336086E-5},2.3305291073371062E-2,468,null,{"$f":"(AD485)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH485>0,(AJ485*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK484,NA())","v":1.0135905955158564},null,468,{"$f":"IF(AF485<=$J$9*0.05,AS484*EXP((-$J$6*1)/Heterogenität!$D$4),Z485)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF485>=$J$19, AR484/$J$5<AN485),0, Bodencharakterisierung!$E$8*$J$11*((AR484/$J$5)-AN485))","v":0},0,{"$f":"AQ484-AP485*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ485/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,468,null,{"$f":"(AP485)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF485<=$J$9*1.05,(AV485*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW484,NA())","v":{"$error":"#N/A"}},23072.238162637354,601,7.3091861155158746,1.0135905955158564,0,2.9355955200000188,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},19.407064040336085,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,469,2.3305291073371062E-2,{"$f":"Z486*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF485*Bodencharakterisierung!$E$11/$J$20","v":2.0309245638010954E-5},{"$f":"((150*($J$2^0.87)*(AB486^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z486)*3600*24","v":4.504308023712715E-2},2.3915996627248484E-4,{"$f":"AE485-AD486*Bodencharakterisierung!$E$8","v":2.9322779232239252E-2},{"$f":"IF(AE486>$J$18,(AE486/(Bodencharakterisierung!$E$11*1000)),0)","v":1.9354969790256931E-5},2.3305291073371062E-2,469,null,{"$f":"(AD486)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH486>0,(AJ486*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK485,NA())","v":1.0157580627712322},null,469,{"$f":"IF(AF486<=$J$9*0.05,AS485*EXP((-$J$6*1)/Heterogenität!$D$4),Z486)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF486>=$J$19, AR485/$J$5<AN486),0, Bodencharakterisierung!$E$8*$J$11*((AR485/$J$5)-AN486))","v":0},0,{"$f":"AQ485-AP486*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ486/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,469,null,{"$f":"(AP486)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF486<=$J$9*1.05,(AV486*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW485,NA())","v":{"$error":"#N/A"}},23072.238162637354,602,7.317626222771251,1.0157580627712322,0,2.9418681600000189,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},19.354969790256931,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,470,2.3305291073371062E-2,{"$f":"Z487*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF486*Bodencharakterisierung!$E$11/$J$20","v":2.0254729668001963E-5},{"$f":"((150*($J$2^0.87)*(AB487^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z487)*3600*24","v":4.4947535307188757E-2},2.3915996627248484E-4,{"$f":"AE486-AD487*Bodencharakterisierung!$E$8","v":2.9243856443369333E-2},{"$f":"IF(AE487>$J$18,(AE487/(Bodencharakterisierung!$E$11*1000)),0)","v":1.9302875540177779E-5},2.3305291073371062E-2,470,null,{"$f":"(AD487)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH487>0,(AJ487*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK486,NA())","v":1.0179255300266079},null,470,{"$f":"IF(AF487<=$J$9*0.05,AS486*EXP((-$J$6*1)/Heterogenität!$D$4),Z487)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF487>=$J$19, AR486/$J$5<AN487),0, Bodencharakterisierung!$E$8*$J$11*((AR486/$J$5)-AN487))","v":0},0,{"$f":"AQ486-AP487*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ487/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,470,null,{"$f":"(AP487)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF487<=$J$9*1.05,(AV487*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW486,NA())","v":{"$error":"#N/A"}},23072.238162637354,603,7.3260663300266273,1.0179255300266079,0,2.9481408000000191,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},19.30287554017778,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,471,2.3305291073371062E-2,{"$f":"Z488*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF487*Bodencharakterisierung!$E$11/$J$20","v":2.0200213697992976E-5},{"$f":"((150*($J$2^0.87)*(AB488^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z488)*3600*24","v":4.4851936358124123E-2},2.3915996627248484E-4,{"$f":"AE487-AD488*Bodencharakterisierung!$E$8","v":2.9164933654499414E-2},{"$f":"IF(AE488>$J$18,(AE488/(Bodencharakterisierung!$E$11*1000)),0)","v":1.9250781290098624E-5},2.3305291073371062E-2,471,null,{"$f":"(AD488)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH488>0,(AJ488*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK487,NA())","v":1.0200929972819837},null,471,{"$f":"IF(AF488<=$J$9*0.05,AS487*EXP((-$J$6*1)/Heterogenität!$D$4),Z488)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF488>=$J$19, AR487/$J$5<AN488),0, Bodencharakterisierung!$E$8*$J$11*((AR487/$J$5)-AN488))","v":0},0,{"$f":"AQ487-AP488*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ488/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,471,null,{"$f":"(AP488)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF488<=$J$9*1.05,(AV488*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW487,NA())","v":{"$error":"#N/A"}},23072.238162637354,604,7.3345064372820028,1.0200929972819837,0,2.9544134400000193,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},19.250781290098622,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,472,2.3305291073371062E-2,{"$f":"Z489*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF488*Bodencharakterisierung!$E$11/$J$20","v":2.0145697727983985E-5},{"$f":"((150*($J$2^0.87)*(AB489^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z489)*3600*24","v":4.4756283213482018E-2},2.3915996627248484E-4,{"$f":"AE488-AD489*Bodencharakterisierung!$E$8","v":2.9086010865629494E-2},{"$f":"IF(AE489>$J$18,(AE489/(Bodencharakterisierung!$E$11*1000)),0)","v":1.9198687040019468E-5},2.3305291073371062E-2,472,null,{"$f":"(AD489)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH489>0,(AJ489*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK488,NA())","v":1.0222604645373594},null,472,{"$f":"IF(AF489<=$J$9*0.05,AS488*EXP((-$J$6*1)/Heterogenität!$D$4),Z489)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF489>=$J$19, AR488/$J$5<AN489),0, Bodencharakterisierung!$E$8*$J$11*((AR488/$J$5)-AN489))","v":0},0,{"$f":"AQ488-AP489*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ489/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,472,null,{"$f":"(AP489)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF489<=$J$9*1.05,(AV489*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW488,NA())","v":{"$error":"#N/A"}},23072.238162637354,605,7.3429465445373783,1.0222604645373594,0,2.9606860800000194,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},19.198687040019468,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,473,2.3305291073371062E-2,{"$f":"Z490*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF489*Bodencharakterisierung!$E$11/$J$20","v":2.0091181757974991E-5},{"$f":"((150*($J$2^0.87)*(AB490^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z490)*3600*24","v":4.4660575695755614E-2},2.3915996627248484E-4,{"$f":"AE489-AD490*Bodencharakterisierung!$E$8","v":2.9007088076759575E-2},{"$f":"IF(AE490>$J$18,(AE490/(Bodencharakterisierung!$E$11*1000)),0)","v":1.9146592789940313E-5},2.3305291073371062E-2,473,null,{"$f":"(AD490)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH490>0,(AJ490*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK489,NA())","v":1.0244279317927352},null,473,{"$f":"IF(AF490<=$J$9*0.05,AS489*EXP((-$J$6*1)/Heterogenität!$D$4),Z490)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF490>=$J$19, AR489/$J$5<AN490),0, Bodencharakterisierung!$E$8*$J$11*((AR489/$J$5)-AN490))","v":0},0,{"$f":"AQ489-AP490*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ490/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,473,null,{"$f":"(AP490)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF490<=$J$9*1.05,(AV490*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW489,NA())","v":{"$error":"#N/A"}},23072.238162637354,606,7.3513866517927546,1.0244279317927352,0,2.9669587200000196,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},19.146592789940314,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,474,2.3305291073371062E-2,{"$f":"Z491*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF490*Bodencharakterisierung!$E$11/$J$20","v":2.0036665787966001E-5},{"$f":"((150*($J$2^0.87)*(AB491^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z491)*3600*24","v":4.4564813626373254E-2},2.3915996627248484E-4,{"$f":"AE490-AD491*Bodencharakterisierung!$E$8","v":2.8928165287889655E-2},{"$f":"IF(AE491>$J$18,(AE491/(Bodencharakterisierung!$E$11*1000)),0)","v":1.9094498539861158E-5},2.3305291073371062E-2,474,null,{"$f":"(AD491)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH491>0,(AJ491*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK490,NA())","v":1.0265953990481109},null,474,{"$f":"IF(AF491<=$J$9*0.05,AS490*EXP((-$J$6*1)/Heterogenität!$D$4),Z491)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF491>=$J$19, AR490/$J$5<AN491),0, Bodencharakterisierung!$E$8*$J$11*((AR490/$J$5)-AN491))","v":0},0,{"$f":"AQ490-AP491*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ491/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,474,null,{"$f":"(AP491)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF491<=$J$9*1.05,(AV491*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW490,NA())","v":{"$error":"#N/A"}},23072.238162637354,607,7.359826759048131,1.0265953990481109,0,2.9732313600000198,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},19.094498539861156,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,475,2.3305291073371062E-2,{"$f":"Z492*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF491*Bodencharakterisierung!$E$11/$J$20","v":1.998214981795701E-5},{"$f":"((150*($J$2^0.87)*(AB492^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z492)*3600*24","v":4.4468996825689312E-2},2.3915996627248484E-4,{"$f":"AE491-AD492*Bodencharakterisierung!$E$8","v":2.8849242499019736E-2},{"$f":"IF(AE492>$J$18,(AE492/(Bodencharakterisierung!$E$11*1000)),0)","v":1.9042404289782003E-5},2.3305291073371062E-2,475,null,{"$f":"(AD492)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH492>0,(AJ492*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK491,NA())","v":1.0287628663034867},null,475,{"$f":"IF(AF492<=$J$9*0.05,AS491*EXP((-$J$6*1)/Heterogenität!$D$4),Z492)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF492>=$J$19, AR491/$J$5<AN492),0, Bodencharakterisierung!$E$8*$J$11*((AR491/$J$5)-AN492))","v":0},0,{"$f":"AQ491-AP492*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ492/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,475,null,{"$f":"(AP492)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF492<=$J$9*1.05,(AV492*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW491,NA())","v":{"$error":"#N/A"}},23072.238162637354,608,7.3682668663035056,1.0287628663034867,0,2.9795040000000199,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},19.042404289782002,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,476,2.3305291073371062E-2,{"$f":"Z493*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF492*Bodencharakterisierung!$E$11/$J$20","v":1.992763384794802E-5},{"$f":"((150*($J$2^0.87)*(AB493^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z493)*3600*24","v":4.4373125112974504E-2},2.3915996627248484E-4,{"$f":"AE492-AD493*Bodencharakterisierung!$E$8","v":2.8770319710149816E-2},{"$f":"IF(AE493>$J$18,(AE493/(Bodencharakterisierung!$E$11*1000)),0)","v":1.8990310039702851E-5},2.3305291073371062E-2,476,null,{"$f":"(AD493)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH493>0,(AJ493*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK492,NA())","v":1.0309303335588624},null,476,{"$f":"IF(AF493<=$J$9*0.05,AS492*EXP((-$J$6*1)/Heterogenität!$D$4),Z493)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF493>=$J$19, AR492/$J$5<AN493),0, Bodencharakterisierung!$E$8*$J$11*((AR492/$J$5)-AN493))","v":0},0,{"$f":"AQ492-AP493*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ493/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,476,null,{"$f":"(AP493)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF493<=$J$9*1.05,(AV493*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW492,NA())","v":{"$error":"#N/A"}},23072.238162637354,609,7.3767069735588819,1.0309303335588624,0,2.9857766400000201,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},18.990310039702852,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,477,2.3305291073371062E-2,{"$f":"Z494*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF493*Bodencharakterisierung!$E$11/$J$20","v":1.9873117877939032E-5},{"$f":"((150*($J$2^0.87)*(AB494^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z494)*3600*24","v":4.4277198306406973E-2},2.3915996627248484E-4,{"$f":"AE493-AD494*Bodencharakterisierung!$E$8","v":2.8691396921279897E-2},{"$f":"IF(AE494>$J$18,(AE494/(Bodencharakterisierung!$E$11*1000)),0)","v":1.8938215789623696E-5},2.3305291073371062E-2,477,null,{"$f":"(AD494)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH494>0,(AJ494*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK493,NA())","v":1.0330978008142382},null,477,{"$f":"IF(AF494<=$J$9*0.05,AS493*EXP((-$J$6*1)/Heterogenität!$D$4),Z494)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF494>=$J$19, AR493/$J$5<AN494),0, Bodencharakterisierung!$E$8*$J$11*((AR493/$J$5)-AN494))","v":0},0,{"$f":"AQ493-AP494*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ494/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,477,null,{"$f":"(AP494)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF494<=$J$9*1.05,(AV494*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW493,NA())","v":{"$error":"#N/A"}},23072.238162637354,610,7.3851470808142583,1.0330978008142382,0,2.9920492800000202,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},18.938215789623694,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,478,2.3305291073371062E-2,{"$f":"Z495*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF494*Bodencharakterisierung!$E$11/$J$20","v":1.9818601907930042E-5},{"$f":"((150*($J$2^0.87)*(AB495^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z495)*3600*24","v":4.418121622306187E-2},2.3915996627248484E-4,{"$f":"AE494-AD495*Bodencharakterisierung!$E$8","v":2.8612474132409978E-2},{"$f":"IF(AE495>$J$18,(AE495/(Bodencharakterisierung!$E$11*1000)),0)","v":1.888612153954454E-5},2.3305291073371062E-2,478,null,{"$f":"(AD495)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH495>0,(AJ495*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK494,NA())","v":1.0352652680696139},null,478,{"$f":"IF(AF495<=$J$9*0.05,AS494*EXP((-$J$6*1)/Heterogenität!$D$4),Z495)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF495>=$J$19, AR494/$J$5<AN495),0, Bodencharakterisierung!$E$8*$J$11*((AR494/$J$5)-AN495))","v":0},0,{"$f":"AQ494-AP495*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ495/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,478,null,{"$f":"(AP495)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF495<=$J$9*1.05,(AV495*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW494,NA())","v":{"$error":"#N/A"}},23072.238162637354,611,7.3935871880696347,1.0352652680696139,0,2.9983219200000204,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},18.88612153954454,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,479,2.3305291073371062E-2,{"$f":"Z496*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF495*Bodencharakterisierung!$E$11/$J$20","v":1.9764085937921048E-5},{"$f":"((150*($J$2^0.87)*(AB496^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z496)*3600*24","v":4.4085178678901923E-2},2.3915996627248484E-4,{"$f":"AE495-AD496*Bodencharakterisierung!$E$8","v":2.8533551343540058E-2},{"$f":"IF(AE496>$J$18,(AE496/(Bodencharakterisierung!$E$11*1000)),0)","v":1.8834027289465385E-5},2.3305291073371062E-2,479,null,{"$f":"(AD496)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH496>0,(AJ496*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK495,NA())","v":1.0374327353249897},null,479,{"$f":"IF(AF496<=$J$9*0.05,AS495*EXP((-$J$6*1)/Heterogenität!$D$4),Z496)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF496>=$J$19, AR495/$J$5<AN496),0, Bodencharakterisierung!$E$8*$J$11*((AR495/$J$5)-AN496))","v":0},0,{"$f":"AQ495-AP496*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ496/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,479,null,{"$f":"(AP496)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF496<=$J$9*1.05,(AV496*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW495,NA())","v":{"$error":"#N/A"}},23072.238162637354,612,7.4020272953250092,1.0374327353249897,0,3.0045945600000206,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},18.834027289465386,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,480,2.3305291073371062E-2,{"$f":"Z497*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF496*Bodencharakterisierung!$E$11/$J$20","v":1.9709569967912057E-5},{"$f":"((150*($J$2^0.87)*(AB497^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z497)*3600*24","v":4.3989085488768141E-2},2.3915996627248484E-4,{"$f":"AE496-AD497*Bodencharakterisierung!$E$8","v":2.8454628554670139E-2},{"$f":"IF(AE497>$J$18,(AE497/(Bodencharakterisierung!$E$11*1000)),0)","v":1.878193303938623E-5},2.3305291073371062E-2,480,null,{"$f":"(AD497)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH497>0,(AJ497*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK496,NA())","v":1.0396002025803655},null,480,{"$f":"IF(AF497<=$J$9*0.05,AS496*EXP((-$J$6*1)/Heterogenität!$D$4),Z497)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF497>=$J$19, AR496/$J$5<AN497),0, Bodencharakterisierung!$E$8*$J$11*((AR496/$J$5)-AN497))","v":0},0,{"$f":"AQ496-AP497*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ497/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,480,null,{"$f":"(AP497)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF497<=$J$9*1.05,(AV497*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW496,NA())","v":{"$error":"#N/A"}},23072.238162637354,613,7.4104674025803856,1.0396002025803655,0,3.0108672000000207,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},18.781933039386232,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,481,2.3305291073371062E-2,{"$f":"Z498*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF497*Bodencharakterisierung!$E$11/$J$20","v":1.9655053997903067E-5},{"$f":"((150*($J$2^0.87)*(AB498^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z498)*3600*24","v":4.3892936466368826E-2},2.3915996627248484E-4,{"$f":"AE497-AD498*Bodencharakterisierung!$E$8","v":2.8375705765800219E-2},{"$f":"IF(AE498>$J$18,(AE498/(Bodencharakterisierung!$E$11*1000)),0)","v":1.8729838789307075E-5},2.3305291073371062E-2,481,null,{"$f":"(AD498)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH498>0,(AJ498*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK497,NA())","v":1.0417676698357412},null,481,{"$f":"IF(AF498<=$J$9*0.05,AS497*EXP((-$J$6*1)/Heterogenität!$D$4),Z498)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF498>=$J$19, AR497/$J$5<AN498),0, Bodencharakterisierung!$E$8*$J$11*((AR497/$J$5)-AN498))","v":0},0,{"$f":"AQ497-AP498*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ498/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,481,null,{"$f":"(AP498)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF498<=$J$9*1.05,(AV498*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW497,NA())","v":{"$error":"#N/A"}},23072.238162637354,614,7.418907509835762,1.0417676698357412,0,3.0171398400000209,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},18.729838789307074,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,482,2.3305291073371062E-2,{"$f":"Z499*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF498*Bodencharakterisierung!$E$11/$J$20","v":1.9600538027894073E-5},{"$f":"((150*($J$2^0.87)*(AB499^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z499)*3600*24","v":4.3796731424270346E-2},2.3915996627248484E-4,{"$f":"AE498-AD499*Bodencharakterisierung!$E$8","v":2.82967829769303E-2},{"$f":"IF(AE499>$J$18,(AE499/(Bodencharakterisierung!$E$11*1000)),0)","v":1.8677744539227919E-5},2.3305291073371062E-2,482,null,{"$f":"(AD499)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH499>0,(AJ499*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK498,NA())","v":1.043935137091117},null,482,{"$f":"IF(AF499<=$J$9*0.05,AS498*EXP((-$J$6*1)/Heterogenität!$D$4),Z499)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF499>=$J$19, AR498/$J$5<AN499),0, Bodencharakterisierung!$E$8*$J$11*((AR498/$J$5)-AN499))","v":0},0,{"$f":"AQ498-AP499*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ499/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,482,null,{"$f":"(AP499)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF499<=$J$9*1.05,(AV499*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW498,NA())","v":{"$error":"#N/A"}},23072.238162637354,615,7.4273476170911383,1.043935137091117,0,3.0234124800000211,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},18.67774453922792,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,483,2.3305291073371062E-2,{"$f":"Z500*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF499*Bodencharakterisierung!$E$11/$J$20","v":1.9546022057885082E-5},{"$f":"((150*($J$2^0.87)*(AB500^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z500)*3600*24","v":4.3700470173886501E-2},2.3915996627248484E-4,{"$f":"AE499-AD500*Bodencharakterisierung!$E$8","v":2.8217860188060381E-2},{"$f":"IF(AE500>$J$18,(AE500/(Bodencharakterisierung!$E$11*1000)),0)","v":1.8625650289148768E-5},2.3305291073371062E-2,483,null,{"$f":"(AD500)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH500>0,(AJ500*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK499,NA())","v":1.0461026043464927},null,483,{"$f":"IF(AF500<=$J$9*0.05,AS499*EXP((-$J$6*1)/Heterogenität!$D$4),Z500)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF500>=$J$19, AR499/$J$5<AN500),0, Bodencharakterisierung!$E$8*$J$11*((AR499/$J$5)-AN500))","v":0},0,{"$f":"AQ499-AP500*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ500/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,483,null,{"$f":"(AP500)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF500<=$J$9*1.05,(AV500*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW499,NA())","v":{"$error":"#N/A"}},23072.238162637354,616,7.4357877243465129,1.0461026043464927,0,3.0296851200000212,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},18.625650289148769,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,485,2.3305291073371062E-2,{"$f":"Z502*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF501*Bodencharakterisierung!$E$11/$J$20","v":1.9436990117867104E-5},{"$f":"((150*($J$2^0.87)*(AB502^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z502)*3600*24","v":4.3507778288093844E-2},2.3915996627248484E-4,{"$f":"AE501-AD502*Bodencharakterisierung!$E$8","v":2.8060014610320542E-2},{"$f":"IF(AE502>$J$18,(AE502/(Bodencharakterisierung!$E$11*1000)),0)","v":1.8521461788990457E-5},2.3305291073371062E-2,485,null,{"$f":"(AD502)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH502>0,(AJ502*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK501,NA())","v":1.0504375388572442},null,485,{"$f":"IF(AF502<=$J$9*0.05,AS501*EXP((-$J$6*1)/Heterogenität!$D$4),Z502)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF502>=$J$19, AR501/$J$5<AN502),0, Bodencharakterisierung!$E$8*$J$11*((AR501/$J$5)-AN502))","v":0},0,{"$f":"AQ501-AP502*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ502/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,485,null,{"$f":"(AP502)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF502<=$J$9*1.05,(AV502*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW501,NA())","v":{"$error":"#N/A"}},23072.238162637354,618,7.4526679388572656,1.0504375388572442,0,3.0422304000000215,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},18.521461788990457,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,496,2.3305291073371062E-2,{"$f":"Z513*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF512*Bodencharakterisierung!$E$11/$J$20","v":1.8837314447768204E-5},{"$f":"((150*($J$2^0.87)*(AB513^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z513)*3600*24","v":4.2443870995345953E-2},2.3915996627248484E-4,{"$f":"AE512-AD513*Bodencharakterisierung!$E$8","v":2.7191863932751428E-2},{"$f":"IF(AE513>$J$18,(AE513/(Bodencharakterisierung!$E$11*1000)),0)","v":1.7948425038119753E-5},2.3305291073371062E-2,496,null,{"$f":"(AD513)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH513>0,(AJ513*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK512,NA())","v":1.0742796786663775},null,496,{"$f":"IF(AF513<=$J$9*0.05,AS512*EXP((-$J$6*1)/Heterogenität!$D$4),Z513)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF513>=$J$19, AR512/$J$5<AN513),0, Bodencharakterisierung!$E$8*$J$11*((AR512/$J$5)-AN513))","v":0},0,{"$f":"AQ512-AP513*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ513/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,496,null,{"$f":"(AP513)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF513<=$J$9*1.05,(AV513*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW512,NA())","v":{"$error":"#N/A"}},23072.238162637354,629,7.5455091186664003,1.0742796786663775,0,3.1112294400000233,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},17.948425038119755,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,508,2.3305291073371062E-2,{"$f":"Z525*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF524*Bodencharakterisierung!$E$11/$J$20","v":1.8183122807660317E-5},{"$f":"((150*($J$2^0.87)*(AB525^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z525)*3600*24","v":4.1275094724130656E-2},2.3915996627248484E-4,{"$f":"AE524-AD525*Bodencharakterisierung!$E$8","v":2.6244790466312395E-2},{"$f":"IF(AE525>$J$18,(AE525/(Bodencharakterisierung!$E$11*1000)),0)","v":1.7323294037169897E-5},2.3305291073371062E-2,508,null,{"$f":"(AD525)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH525>0,(AJ525*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK524,NA())","v":1.1002892857308866},null,508,{"$f":"IF(AF525<=$J$9*0.05,AS524*EXP((-$J$6*1)/Heterogenität!$D$4),Z525)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF525>=$J$19, AR524/$J$5<AN525),0, Bodencharakterisierung!$E$8*$J$11*((AR524/$J$5)-AN525))","v":0},0,{"$f":"AQ524-AP525*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ525/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,508,null,{"$f":"(AP525)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF525<=$J$9*1.05,(AV525*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW524,NA())","v":{"$error":"#N/A"}},23072.238162637354,641,7.6467904057309113,1.1002892857308866,0,3.1865011200000253,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},17.323294037169898,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,515,2.3305291073371062E-2,{"$f":"Z532*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF531*Bodencharakterisierung!$E$11/$J$20","v":1.7801511017597383E-5},{"$f":"((150*($J$2^0.87)*(AB532^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z532)*3600*24","v":4.058923920112513E-2},2.3915996627248484E-4,{"$f":"AE531-AD532*Bodencharakterisierung!$E$8","v":2.569233094422296E-2},{"$f":"IF(AE532>$J$18,(AE532/(Bodencharakterisierung!$E$11*1000)),0)","v":1.6958634286615814E-5},2.3305291073371062E-2,515,null,{"$f":"(AD532)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH532>0,(AJ532*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK531,NA())","v":1.1154615565185169},null,515,{"$f":"IF(AF532<=$J$9*0.05,AS531*EXP((-$J$6*1)/Heterogenität!$D$4),Z532)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF532>=$J$19, AR531/$J$5<AN532),0, Bodencharakterisierung!$E$8*$J$11*((AR531/$J$5)-AN532))","v":0},0,{"$f":"AQ531-AP532*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ532/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,515,null,{"$f":"(AP532)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF532<=$J$9*1.05,(AV532*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW531,NA())","v":{"$error":"#N/A"}},23072.238162637354,648,7.7058711565185423,1.1154615565185169,0,{"$f":"$G$34/$G$12/$G$8+BC531","v":3.2304096000000264},null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},16.958634286615816,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,524,2.3305291073371062E-2,{"$f":"Z541*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF540*Bodencharakterisierung!$E$11/$J$20","v":1.7310867287516464E-5},{"$f":"((150*($J$2^0.87)*(AB541^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z541)*3600*24","v":3.9702866097547786E-2},2.3915996627248484E-4,{"$f":"AE540-AD541*Bodencharakterisierung!$E$8","v":2.4982025844393685E-2},{"$f":"IF(AE541>$J$18,(AE541/(Bodencharakterisierung!$E$11*1000)),0)","v":1.6489786035903424E-5},2.3305291073371062E-2,524,null,{"$f":"(AD541)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH541>0,(AJ541*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK540,NA())","v":1.1349687618168987},null,524,{"$f":"IF(AF541<=$J$9*0.05,AS540*EXP((-$J$6*1)/Heterogenität!$D$4),Z541)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF541>=$J$19, AR540/$J$5<AN541),0, Bodencharakterisierung!$E$8*$J$11*((AR540/$J$5)-AN541))","v":0},0,{"$f":"AQ540-AP541*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ541/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,524,null,{"$f":"(AP541)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF541<=$J$9*1.05,(AV541*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW540,NA())","v":{"$error":"#N/A"}},23072.238162637354,657,7.781832121816926,1.1349687618168987,0,3.2868633600000279,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},16.489786035903425,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,529,2.3305291073371062E-2,{"$f":"Z546*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF545*Bodencharakterisierung!$E$11/$J$20","v":1.7038287437471511E-5},{"$f":"((150*($J$2^0.87)*(AB546^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z546)*3600*24","v":3.9208161540105126E-2},2.3915996627248484E-4,{"$f":"AE545-AD546*Bodencharakterisierung!$E$8","v":2.4587411900044088E-2},{"$f":"IF(AE546>$J$18,(AE546/(Bodencharakterisierung!$E$11*1000)),0)","v":1.6229314785507648E-5},2.3305291073371062E-2,529,null,{"$f":"(AD546)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH546>0,(AJ546*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK545,NA())","v":1.1458060980937774},null,529,{"$f":"IF(AF546<=$J$9*0.05,AS545*EXP((-$J$6*1)/Heterogenität!$D$4),Z546)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF546>=$J$19, AR545/$J$5<AN546),0, Bodencharakterisierung!$E$8*$J$11*((AR545/$J$5)-AN546))","v":0},0,{"$f":"AQ545-AP546*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ546/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,529,null,{"$f":"(AP546)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF546<=$J$9*1.05,(AV546*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW545,NA())","v":{"$error":"#N/A"}},23072.238162637354,662,7.824032658093806,1.1458060980937774,0,3.3182265600000287,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},16.229314785507647,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,536,2.3305291073371062E-2,{"$f":"Z553*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF552*Bodencharakterisierung!$E$11/$J$20","v":1.6656675647408577E-5},{"$f":"((150*($J$2^0.87)*(AB553^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z553)*3600*24","v":3.8512770849242095E-2},2.3915996627248484E-4,{"$f":"AE552-AD553*Bodencharakterisierung!$E$8","v":2.4034952377954652E-2},{"$f":"IF(AE553>$J$18,(AE553/(Bodencharakterisierung!$E$11*1000)),0)","v":1.5864655034953564E-5},2.3305291073371062E-2,536,null,{"$f":"(AD553)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH553>0,(AJ553*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK552,NA())","v":1.1609783688814077},null,536,{"$f":"IF(AF553<=$J$9*0.05,AS552*EXP((-$J$6*1)/Heterogenität!$D$4),Z553)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF553>=$J$19, AR552/$J$5<AN553),0, Bodencharakterisierung!$E$8*$J$11*((AR552/$J$5)-AN553))","v":0},0,{"$f":"AQ552-AP553*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ553/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,536,null,{"$f":"(AP553)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF553<=$J$9*1.05,(AV553*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW552,NA())","v":{"$error":"#N/A"}},23072.238162637354,669,7.883113408881437,1.1609783688814077,0,3.3621350400000298,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},15.864655034953564,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,548,2.3305291073371062E-2,{"$f":"Z565*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF564*Bodencharakterisierung!$E$11/$J$20","v":1.6002484007300686E-5},{"$f":"((150*($J$2^0.87)*(AB565^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z565)*3600*24","v":3.7312816578924449E-2},2.3915996627248484E-4,{"$f":"AE564-AD565*Bodencharakterisierung!$E$8","v":2.3087878911515619E-2},{"$f":"IF(AE565>$J$18,(AE565/(Bodencharakterisierung!$E$11*1000)),0)","v":1.5239524034003708E-5},2.3305291073371062E-2,548,null,{"$f":"(AD565)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH565>0,(AJ565*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK564,NA())","v":1.1869879759459168},null,548,{"$f":"IF(AF565<=$J$9*0.05,AS564*EXP((-$J$6*1)/Heterogenität!$D$4),Z565)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF565>=$J$19, AR564/$J$5<AN565),0, Bodencharakterisierung!$E$8*$J$11*((AR564/$J$5)-AN565))","v":0},0,{"$f":"AQ564-AP565*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ565/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,548,null,{"$f":"(AP565)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF565<=$J$9*1.05,(AV565*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW564,NA())","v":{"$error":"#N/A"}},23072.238162637354,681,7.984394695945948,1.1869879759459168,0,3.4374067200000318,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},15.239524034003708,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,555,2.3305291073371062E-2,{"$f":"Z572*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF571*Bodencharakterisierung!$E$11/$J$20","v":1.5620872217237752E-5},{"$f":"((150*($J$2^0.87)*(AB572^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z572)*3600*24","v":3.6608097276730825E-2},2.3915996627248484E-4,{"$f":"AE571-AD572*Bodencharakterisierung!$E$8","v":2.2535419389426183E-2},{"$f":"IF(AE572>$J$18,(AE572/(Bodencharakterisierung!$E$11*1000)),0)","v":1.4874864283449625E-5},2.3305291073371062E-2,555,null,{"$f":"(AD572)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH572>0,(AJ572*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK571,NA())","v":1.202160246733547},null,555,{"$f":"IF(AF572<=$J$9*0.05,AS571*EXP((-$J$6*1)/Heterogenität!$D$4),Z572)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF572>=$J$19, AR571/$J$5<AN572),0, Bodencharakterisierung!$E$8*$J$11*((AR571/$J$5)-AN572))","v":0},0,{"$f":"AQ571-AP572*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ572/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,555,null,{"$f":"(AP572)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF572<=$J$9*1.05,(AV572*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW571,NA())","v":{"$error":"#N/A"}},23072.238162637354,688,8.0434754467335789,1.202160246733547,0,3.4813152000000329,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},14.874864283449625,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,565,2.3305291073371062E-2,{"$f":"Z582*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF581*Bodencharakterisierung!$E$11/$J$20","v":1.5075712517147843E-5},{"$f":"((150*($J$2^0.87)*(AB582^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z582)*3600*24","v":3.5595039979156355E-2},2.3915996627248484E-4,{"$f":"AE581-AD582*Bodencharakterisierung!$E$8","v":2.1746191500726989E-2},{"$f":"IF(AE582>$J$18,(AE582/(Bodencharakterisierung!$E$11*1000)),0)","v":1.4353921782658078E-5},2.3305291073371062E-2,565,null,{"$f":"(AD582)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH582>0,(AJ582*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK581,NA())","v":1.2238349192873046},null,565,{"$f":"IF(AF582<=$J$9*0.05,AS581*EXP((-$J$6*1)/Heterogenität!$D$4),Z582)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF582>=$J$19, AR581/$J$5<AN582),0, Bodencharakterisierung!$E$8*$J$11*((AR581/$J$5)-AN582))","v":0},0,{"$f":"AQ581-AP582*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ582/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,565,null,{"$f":"(AP582)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF582<=$J$9*1.05,(AV582*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW581,NA())","v":{"$error":"#N/A"}},23072.238162637354,698,8.127876519287339,1.2238349192873046,0,3.5440416000000345,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},14.353921782658078,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,578,2.3305291073371062E-2,{"$f":"Z595*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF594*Bodencharakterisierung!$E$11/$J$20","v":1.4367004907030965E-5},{"$f":"((150*($J$2^0.87)*(AB595^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z595)*3600*24","v":3.4266465903203105E-2},2.3915996627248484E-4,{"$f":"AE594-AD595*Bodencharakterisierung!$E$8","v":2.0720195245418037E-2},{"$f":"IF(AE595>$J$18,(AE595/(Bodencharakterisierung!$E$11*1000)),0)","v":1.3676696531629067E-5},2.3305291073371062E-2,578,null,{"$f":"(AD595)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH595>0,(AJ595*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK594,NA())","v":1.2520119936071894},null,578,{"$f":"IF(AF595<=$J$9*0.05,AS594*EXP((-$J$6*1)/Heterogenität!$D$4),Z595)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF595>=$J$19, AR594/$J$5<AN595),0, Bodencharakterisierung!$E$8*$J$11*((AR594/$J$5)-AN595))","v":0},0,{"$f":"AQ594-AP595*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ595/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,578,null,{"$f":"(AP595)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF595<=$J$9*1.05,(AV595*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW594,NA())","v":{"$error":"#N/A"}},23072.238162637354,711,8.2375979136072264,1.2520119936071894,0,3.6255859200000367,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},13.676696531629068,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,585,2.3305291073371062E-2,{"$f":"Z602*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF601*Bodencharakterisierung!$E$11/$J$20","v":1.3985393116968029E-5},{"$f":"((150*($J$2^0.87)*(AB602^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z602)*3600*24","v":3.3545400539264081E-2},2.3915996627248484E-4,{"$f":"AE601-AD602*Bodencharakterisierung!$E$8","v":2.0167735723328601E-2},{"$f":"IF(AE602>$J$18,(AE602/(Bodencharakterisierung!$E$11*1000)),0)","v":1.3312036781074984E-5},2.3305291073371062E-2,585,null,{"$f":"(AD602)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH602>0,(AJ602*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK601,NA())","v":1.2671842643948197},null,585,{"$f":"IF(AF602<=$J$9*0.05,AS601*EXP((-$J$6*1)/Heterogenität!$D$4),Z602)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF602>=$J$19, AR601/$J$5<AN602),0, Bodencharakterisierung!$E$8*$J$11*((AR601/$J$5)-AN602))","v":0},0,{"$f":"AQ601-AP602*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ602/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,585,null,{"$f":"(AP602)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF602<=$J$9*1.05,(AV602*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW601,NA())","v":{"$error":"#N/A"}},23072.238162637354,718,8.2966786643948573,1.2671842643948197,0,3.6694944000000378,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},13.312036781074983,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,597,2.3305291073371062E-2,{"$f":"Z614*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF613*Bodencharakterisierung!$E$11/$J$20","v":1.333120147686014E-5},{"$f":"((150*($J$2^0.87)*(AB614^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z614)*3600*24","v":3.2299568946852826E-2},2.3915996627248484E-4,{"$f":"AE613-AD614*Bodencharakterisierung!$E$8","v":1.9220662256889568E-2},{"$f":"IF(AE614>$J$18,(AE614/(Bodencharakterisierung!$E$11*1000)),0)","v":1.2686905780125128E-5},2.3305291073371062E-2,597,null,{"$f":"(AD614)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH614>0,(AJ614*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK613,NA())","v":1.2931938714593287},null,597,{"$f":"IF(AF614<=$J$9*0.05,AS613*EXP((-$J$6*1)/Heterogenität!$D$4),Z614)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF614>=$J$19, AR613/$J$5<AN614),0, Bodencharakterisierung!$E$8*$J$11*((AR613/$J$5)-AN614))","v":0},0,{"$f":"AQ613-AP614*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ614/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,597,null,{"$f":"(AP614)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF614<=$J$9*1.05,(AV614*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW613,NA())","v":{"$error":"#N/A"}},23072.238162637354,730,8.3979599514593684,1.2931938714593287,0,3.7447660800000397,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},12.686905780125128,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,604,2.3305291073371062E-2,{"$f":"Z621*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF620*Bodencharakterisierung!$E$11/$J$20","v":1.2949589686797206E-5},{"$f":"((150*($J$2^0.87)*(AB621^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z621)*3600*24","v":3.1566921624046528E-2},2.3915996627248484E-4,{"$f":"AE620-AD621*Bodencharakterisierung!$E$8","v":1.8668202734800132E-2},{"$f":"IF(AE621>$J$18,(AE621/(Bodencharakterisierung!$E$11*1000)),0)","v":1.2322246029571045E-5},2.3305291073371062E-2,604,null,{"$f":"(AD621)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH621>0,(AJ621*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK620,NA())","v":1.308366142246959},null,604,{"$f":"IF(AF621<=$J$9*0.05,AS620*EXP((-$J$6*1)/Heterogenität!$D$4),Z621)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF621>=$J$19, AR620/$J$5<AN621),0, Bodencharakterisierung!$E$8*$J$11*((AR620/$J$5)-AN621))","v":0},0,{"$f":"AQ620-AP621*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ621/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,604,null,{"$f":"(AP621)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF621<=$J$9*1.05,(AV621*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW620,NA())","v":{"$error":"#N/A"}},23072.238162637354,737,8.4570407022469993,1.308366142246959,0,3.7886745600000409,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},12.322246029571044,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,606,2.3305291073371062E-2,{"$f":"Z623*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF622*Bodencharakterisierung!$E$11/$J$20","v":1.2840557746779223E-5},{"$f":"((150*($J$2^0.87)*(AB623^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z623)*3600*24","v":3.135676545585972E-2},2.3915996627248484E-4,{"$f":"AE622-AD623*Bodencharakterisierung!$E$8","v":1.8510357157060293E-2},{"$f":"IF(AE623>$J$18,(AE623/(Bodencharakterisierung!$E$11*1000)),0)","v":1.2218057529412734E-5},2.3305291073371062E-2,606,null,{"$f":"(AD623)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH623>0,(AJ623*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK622,NA())","v":1.3127010767577105},null,606,{"$f":"IF(AF623<=$J$9*0.05,AS622*EXP((-$J$6*1)/Heterogenität!$D$4),Z623)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF623>=$J$19, AR622/$J$5<AN623),0, Bodencharakterisierung!$E$8*$J$11*((AR622/$J$5)-AN623))","v":0},0,{"$f":"AQ622-AP623*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ623/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,606,null,{"$f":"(AP623)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF623<=$J$9*1.05,(AV623*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW622,NA())","v":{"$error":"#N/A"}},23072.238162637354,739,8.4739209167577521,1.3127010767577105,0,3.8012198400000412,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},12.218057529412734,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,618,2.3305291073371062E-2,{"$f":"Z635*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF634*Bodencharakterisierung!$E$11/$J$20","v":1.2186366106671336E-5},{"$f":"((150*($J$2^0.87)*(AB635^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z635)*3600*24","v":3.0087812952371472E-2},2.3915996627248484E-4,{"$f":"AE634-AD635*Bodencharakterisierung!$E$8","v":1.7563283690621261E-2},{"$f":"IF(AE635>$J$18,(AE635/(Bodencharakterisierung!$E$11*1000)),0)","v":1.1592926528462878E-5},2.3305291073371062E-2,618,null,{"$f":"(AD635)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH635>0,(AJ635*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK634,NA())","v":1.3387106838222196},null,618,{"$f":"IF(AF635<=$J$9*0.05,AS634*EXP((-$J$6*1)/Heterogenität!$D$4),Z635)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF635>=$J$19, AR634/$J$5<AN635),0, Bodencharakterisierung!$E$8*$J$11*((AR634/$J$5)-AN635))","v":0},0,{"$f":"AQ634-AP635*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ635/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,618,null,{"$f":"(AP635)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF635<=$J$9*1.05,(AV635*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW634,NA())","v":{"$error":"#N/A"}},23072.238162637354,751,8.5752022038222631,1.3387106838222196,0,3.8764915200000432,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},11.592926528462877,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,625,2.3305291073371062E-2,{"$f":"Z642*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF641*Bodencharakterisierung!$E$11/$J$20","v":1.1804754316608398E-5},{"$f":"((150*($J$2^0.87)*(AB642^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z642)*3600*24","v":2.9341004537943579E-2},2.3915996627248484E-4,{"$f":"AE641-AD642*Bodencharakterisierung!$E$8","v":1.7010824168531825E-2},{"$f":"IF(AE642>$J$18,(AE642/(Bodencharakterisierung!$E$11*1000)),0)","v":1.1228266777908795E-5},2.3305291073371062E-2,625,null,{"$f":"(AD642)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH642>0,(AJ642*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK641,NA())","v":1.3538829546098499},null,625,{"$f":"IF(AF642<=$J$9*0.05,AS641*EXP((-$J$6*1)/Heterogenität!$D$4),Z642)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF642>=$J$19, AR641/$J$5<AN642),0, Bodencharakterisierung!$E$8*$J$11*((AR641/$J$5)-AN642))","v":0},0,{"$f":"AQ641-AP642*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ642/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,625,null,{"$f":"(AP642)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF642<=$J$9*1.05,(AV642*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW641,NA())","v":{"$error":"#N/A"}},23072.238162637354,758,8.634282954609894,1.3538829546098499,0,3.9204000000000443,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},11.228266777908795,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,637,2.3305291073371062E-2,{"$f":"Z654*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF653*Bodencharakterisierung!$E$11/$J$20","v":1.1150562676500509E-5},{"$f":"((150*($J$2^0.87)*(AB654^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z654)*3600*24","v":2.8048810252801419E-2},2.3915996627248484E-4,{"$f":"AE653-AD654*Bodencharakterisierung!$E$8","v":1.6063750702092792E-2},{"$f":"IF(AE654>$J$18,(AE654/(Bodencharakterisierung!$E$11*1000)),0)","v":1.0603135776958939E-5},2.3305291073371062E-2,637,null,{"$f":"(AD654)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH654>0,(AJ654*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK653,NA())","v":1.3798925616743589},null,637,{"$f":"IF(AF654<=$J$9*0.05,AS653*EXP((-$J$6*1)/Heterogenität!$D$4),Z654)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF654>=$J$19, AR653/$J$5<AN654),0, Bodencharakterisierung!$E$8*$J$11*((AR653/$J$5)-AN654))","v":0},0,{"$f":"AQ653-AP654*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ654/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,637,null,{"$f":"(AP654)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF654<=$J$9*1.05,(AV654*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW653,NA())","v":{"$error":"#N/A"}},23072.238162637354,770,8.735564241674405,1.3798925616743589,0,3.9956716800000462,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},10.60313577695894,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,645,2.3305291073371062E-2,{"$f":"Z662*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF661*Bodencharakterisierung!$E$11/$J$20","v":1.0714434916428585E-5},{"$f":"((150*($J$2^0.87)*(AB662^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z662)*3600*24","v":2.7178514138433071E-2},2.3915996627248484E-4,{"$f":"AE661-AD662*Bodencharakterisierung!$E$8","v":1.5432368391133437E-2},{"$f":"IF(AE662>$J$18,(AE662/(Bodencharakterisierung!$E$11*1000)),0)","v":1.0186381776325701E-5},2.3305291073371062E-2,645,null,{"$f":"(AD662)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH662>0,(AJ662*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK661,NA())","v":1.397232299717365},null,645,{"$f":"IF(AF662<=$J$9*0.05,AS661*EXP((-$J$6*1)/Heterogenität!$D$4),Z662)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF662>=$J$19, AR661/$J$5<AN662),0, Bodencharakterisierung!$E$8*$J$11*((AR661/$J$5)-AN662))","v":0},0,{"$f":"AQ661-AP662*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ662/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,645,null,{"$f":"(AP662)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF662<=$J$9*1.05,(AV662*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW661,NA())","v":{"$error":"#N/A"}},23072.238162637354,778,8.8030850997174088,1.397232299717365,0,4.045852800000044,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},10.186381776325701,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,655,2.3305291073371062E-2,{"$f":"Z672*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF671*Bodencharakterisierung!$E$11/$J$20","v":1.0169275216338677E-5},{"$f":"((150*($J$2^0.87)*(AB672^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z672)*3600*24","v":2.6080090049730213E-2},2.3915996627248484E-4,{"$f":"AE671-AD672*Bodencharakterisierung!$E$8","v":1.4643140502434242E-2},{"$f":"IF(AE672>$J$18,(AE672/(Bodencharakterisierung!$E$11*1000)),0)","v":9.6654392755341535E-6},2.3305291073371062E-2,655,null,{"$f":"(AD672)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH672>0,(AJ672*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK671,NA())","v":1.4189069722711225},null,655,{"$f":"IF(AF672<=$J$9*0.05,AS671*EXP((-$J$6*1)/Heterogenität!$D$4),Z672)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF672>=$J$19, AR671/$J$5<AN672),0, Bodencharakterisierung!$E$8*$J$11*((AR671/$J$5)-AN672))","v":0},0,{"$f":"AQ671-AP672*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ672/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,655,null,{"$f":"(AP672)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF672<=$J$9*1.05,(AV672*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW671,NA())","v":{"$error":"#N/A"}},23072.238162637354,788,8.8874861722711636,1.4189069722711225,0,4.1085792000000412,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},9.6654392755341529,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,667,2.3305291073371062E-2,{"$f":"Z684*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF683*Bodencharakterisierung!$E$11/$J$20","v":9.5150835762307863E-6},{"$f":"((150*($J$2^0.87)*(AB684^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z684)*3600*24","v":2.474548359520793E-2},2.3915996627248484E-4,{"$f":"AE683-AD684*Bodencharakterisierung!$E$8","v":1.369606703599521E-2},{"$f":"IF(AE684>$J$18,(AE684/(Bodencharakterisierung!$E$11*1000)),0)","v":9.0403082745842975E-6},2.3305291073371062E-2,667,null,{"$f":"(AD684)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH684>0,(AJ684*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK683,NA())","v":1.4449165793356316},null,667,{"$f":"IF(AF684<=$J$9*0.05,AS683*EXP((-$J$6*1)/Heterogenität!$D$4),Z684)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF684>=$J$19, AR683/$J$5<AN684),0, Bodencharakterisierung!$E$8*$J$11*((AR683/$J$5)-AN684))","v":0},0,{"$f":"AQ683-AP684*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ684/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,667,null,{"$f":"(AP684)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF684<=$J$9*1.05,(AV684*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW683,NA())","v":{"$error":"#N/A"}},23072.238162637354,800,8.9887674593356692,1.4449165793356316,0,4.1838508800000378,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},9.040308274584298,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,674,2.3305291073371062E-2,{"$f":"Z691*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF690*Bodencharakterisierung!$E$11/$J$20","v":9.1334717861678504E-6},{"$f":"((150*($J$2^0.87)*(AB691^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z691)*3600*24","v":2.3958098168878745E-2},2.3915996627248484E-4,{"$f":"AE690-AD691*Bodencharakterisierung!$E$8","v":1.3143607513905774E-2},{"$f":"IF(AE691>$J$18,(AE691/(Bodencharakterisierung!$E$11*1000)),0)","v":8.6756485240302143E-6},2.3305291073371062E-2,674,null,{"$f":"(AD691)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH691>0,(AJ691*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK690,NA())","v":1.4600888501232618},null,674,{"$f":"IF(AF691<=$J$9*0.05,AS690*EXP((-$J$6*1)/Heterogenität!$D$4),Z691)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF691>=$J$19, AR690/$J$5<AN691),0, Bodencharakterisierung!$E$8*$J$11*((AR690/$J$5)-AN691))","v":0},0,{"$f":"AQ690-AP691*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ691/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,674,null,{"$f":"(AP691)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF691<=$J$9*1.05,(AV691*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW690,NA())","v":{"$error":"#N/A"}},23072.238162637354,807,9.0478482101232967,1.4600888501232618,0,4.2277593600000358,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},8.6756485240302137,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,677,2.3305291073371062E-2,{"$f":"Z694*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF693*Bodencharakterisierung!$E$11/$J$20","v":8.9699238761408786E-6},{"$f":"((150*($J$2^0.87)*(AB694^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z694)*3600*24","v":2.3618543061794003E-2},2.3915996627248484E-4,{"$f":"AE693-AD694*Bodencharakterisierung!$E$8","v":1.2906839147296015E-2},{"$f":"IF(AE694>$J$18,(AE694/(Bodencharakterisierung!$E$11*1000)),0)","v":8.5193657737927487E-6},2.3305291073371062E-2,677,null,{"$f":"(AD694)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH694>0,(AJ694*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK693,NA())","v":1.4665912518893891},null,677,{"$f":"IF(AF694<=$J$9*0.05,AS693*EXP((-$J$6*1)/Heterogenität!$D$4),Z694)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF694>=$J$19, AR693/$J$5<AN694),0, Bodencharakterisierung!$E$8*$J$11*((AR693/$J$5)-AN694))","v":0},0,{"$f":"AQ693-AP694*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ694/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,677,null,{"$f":"(AP694)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF694<=$J$9*1.05,(AV694*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW693,NA())","v":{"$error":"#N/A"}},23072.238162637354,810,9.073168531889424,1.4665912518893891,0,4.246577280000035,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},8.5193657737927495,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,686,2.3305291073371062E-2,{"$f":"Z703*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF702*Bodencharakterisierung!$E$11/$J$20","v":8.4792801460599632E-6},{"$f":"((150*($J$2^0.87)*(AB703^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z703)*3600*24","v":2.2591942979145699E-2},2.3915996627248484E-4,{"$f":"AE702-AD703*Bodencharakterisierung!$E$8","v":1.2196534047466741E-2},{"$f":"IF(AE703>$J$18,(AE703/(Bodencharakterisierung!$E$11*1000)),0)","v":8.0505175230803567E-6},2.3305291073371062E-2,686,null,{"$f":"(AD703)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH703>0,(AJ703*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK702,NA())","v":1.4860984571877709},null,686,{"$f":"IF(AF703<=$J$9*0.05,AS702*EXP((-$J$6*1)/Heterogenität!$D$4),Z703)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF703>=$J$19, AR702/$J$5<AN703),0, Bodencharakterisierung!$E$8*$J$11*((AR702/$J$5)-AN703))","v":0},0,{"$f":"AQ702-AP703*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ703/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,686,null,{"$f":"(AP703)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF703<=$J$9*1.05,(AV703*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW702,NA())","v":{"$error":"#N/A"}},23072.238162637354,819,9.1491294971878023,1.4860984571877709,0,4.3030310400000324,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},8.050517523080357,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,695,2.3305291073371062E-2,{"$f":"Z712*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF711*Bodencharakterisierung!$E$11/$J$20","v":7.9886364159790461E-6},{"$f":"((150*($J$2^0.87)*(AB712^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z712)*3600*24","v":2.1552784363420608E-2},2.3915996627248484E-4,{"$f":"AE711-AD712*Bodencharakterisierung!$E$8","v":1.1486228947637466E-2},{"$f":"IF(AE712>$J$18,(AE712/(Bodencharakterisierung!$E$11*1000)),0)","v":7.5816692723679648E-6},2.3305291073371062E-2,695,null,{"$f":"(AD712)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH712>0,(AJ712*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK711,NA())","v":1.5056056624861527},null,695,{"$f":"IF(AF712<=$J$9*0.05,AS711*EXP((-$J$6*1)/Heterogenität!$D$4),Z712)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF712>=$J$19, AR711/$J$5<AN712),0, Bodencharakterisierung!$E$8*$J$11*((AR711/$J$5)-AN712))","v":0},0,{"$f":"AQ711-AP712*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ712/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,695,null,{"$f":"(AP712)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF712<=$J$9*1.05,(AV712*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW711,NA())","v":{"$error":"#N/A"}},23072.238162637354,828,9.2250904624861825,1.5056056624861527,0,4.3594848000000299,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},7.5816692723679644,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,707,2.3305291073371062E-2,{"$f":"Z724*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF723*Bodencharakterisierung!$E$11/$J$20","v":7.3344447758711572E-6},{"$f":"((150*($J$2^0.87)*(AB724^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z724)*3600*24","v":2.0146059288143923E-2},2.3915996627248484E-4,{"$f":"AE723-AD724*Bodencharakterisierung!$E$8","v":1.0539155481198433E-2},{"$f":"IF(AE724>$J$18,(AE724/(Bodencharakterisierung!$E$11*1000)),0)","v":6.956538271418108E-6},2.3305291073371062E-2,707,null,{"$f":"(AD724)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH724>0,(AJ724*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK723,NA())","v":1.5316152695506617},null,707,{"$f":"IF(AF724<=$J$9*0.05,AS723*EXP((-$J$6*1)/Heterogenität!$D$4),Z724)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF724>=$J$19, AR723/$J$5<AN724),0, Bodencharakterisierung!$E$8*$J$11*((AR723/$J$5)-AN724))","v":0},0,{"$f":"AQ723-AP724*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ724/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,707,null,{"$f":"(AP724)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF724<=$J$9*1.05,(AV724*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW723,NA())","v":{"$error":"#N/A"}},23072.238162637354,840,9.3263717495506882,1.5316152695506617,0,{"$f":"$G$34/$G$12/$G$8+BC723","v":4.4347564800000265},null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},6.9565382714181077,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,719,2.3305291073371062E-2,{"$f":"Z736*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF735*Bodencharakterisierung!$E$11/$J$20","v":6.6802531357632683E-6},{"$f":"((150*($J$2^0.87)*(AB736^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z736)*3600*24","v":1.8712697292517455E-2},2.3915996627248484E-4,{"$f":"AE735-AD736*Bodencharakterisierung!$E$8","v":9.5920820147594003E-3},{"$f":"IF(AE736>$J$18,(AE736/(Bodencharakterisierung!$E$11*1000)),0)","v":6.3314072704682512E-6},2.3305291073371062E-2,719,null,{"$f":"(AD736)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH736>0,(AJ736*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK735,NA())","v":1.5576248766151708},null,719,{"$f":"IF(AF736<=$J$9*0.05,AS735*EXP((-$J$6*1)/Heterogenität!$D$4),Z736)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF736>=$J$19, AR735/$J$5<AN736),0, Bodencharakterisierung!$E$8*$J$11*((AR735/$J$5)-AN736))","v":0},0,{"$f":"AQ735-AP736*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ736/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,719,null,{"$f":"(AP736)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF736<=$J$9*1.05,(AV736*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW735,NA())","v":{"$error":"#N/A"}},23072.238162637354,852,9.4276530366151938,1.5576248766151708,0,4.5100281600000232,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},6.3314072704682509,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,725,2.3305291073371062E-2,{"$f":"Z742*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF741*Bodencharakterisierung!$E$11/$J$20","v":6.353157315709323E-6},{"$f":"((150*($J$2^0.87)*(AB742^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z742)*3600*24","v":1.7985055287185966E-2},2.3915996627248484E-4,{"$f":"AE741-AD742*Bodencharakterisierung!$E$8","v":9.1185452815398839E-3},{"$f":"IF(AE742>$J$18,(AE742/(Bodencharakterisierung!$E$11*1000)),0)","v":6.0188417699933224E-6},2.3305291073371062E-2,725,null,{"$f":"(AD742)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH742>0,(AJ742*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK741,NA())","v":1.5706296801474253},null,725,{"$f":"IF(AF742<=$J$9*0.05,AS741*EXP((-$J$6*1)/Heterogenität!$D$4),Z742)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF742>=$J$19, AR741/$J$5<AN742),0, Bodencharakterisierung!$E$8*$J$11*((AR741/$J$5)-AN742))","v":0},0,{"$f":"AQ741-AP742*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ742/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,725,null,{"$f":"(AP742)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF742<=$J$9*1.05,(AV742*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW741,NA())","v":{"$error":"#N/A"}},23072.238162637354,858,9.4782936801474467,1.5706296801474253,0,4.5476640000000215,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},6.0188417699933225,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,737,2.3305291073371062E-2,{"$f":"Z754*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF753*Bodencharakterisierung!$E$11/$J$20","v":5.698965675601435E-6},{"$f":"((150*($J$2^0.87)*(AB754^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z754)*3600*24","v":1.65055065926384E-2},2.3915996627248484E-4,{"$f":"AE753-AD754*Bodencharakterisierung!$E$8","v":8.171471815100851E-3},{"$f":"IF(AE754>$J$18,(AE754/(Bodencharakterisierung!$E$11*1000)),0)","v":5.3937107690434656E-6},2.3305291073371062E-2,737,null,{"$f":"(AD754)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH754>0,(AJ754*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK753,NA())","v":1.5966392872119344},null,737,{"$f":"IF(AF754<=$J$9*0.05,AS753*EXP((-$J$6*1)/Heterogenität!$D$4),Z754)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF754>=$J$19, AR753/$J$5<AN754),0, Bodencharakterisierung!$E$8*$J$11*((AR753/$J$5)-AN754))","v":0},0,{"$f":"AQ753-AP754*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ754/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,737,null,{"$f":"(AP754)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF754<=$J$9*1.05,(AV754*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW753,NA())","v":{"$error":"#N/A"}},23072.238162637354,870,9.5795749672119523,1.5966392872119344,0,4.6229356800000181,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},5.3937107690434658,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,744,2.3305291073371062E-2,{"$f":"Z761*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF760*Bodencharakterisierung!$E$11/$J$20","v":5.3173538855384982E-6},{"$f":"((150*($J$2^0.87)*(AB761^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z761)*3600*24","v":1.562605980088971E-2},2.3915996627248484E-4,{"$f":"AE760-AD761*Bodencharakterisierung!$E$8","v":7.6190122930114125E-3},{"$f":"IF(AE761>$J$18,(AE761/(Bodencharakterisierung!$E$11*1000)),0)","v":5.0290510184893816E-6},2.3305291073371062E-2,744,null,{"$f":"(AD761)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH761>0,(AJ761*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK760,NA())","v":1.6118115579995647},null,744,{"$f":"IF(AF761<=$J$9*0.05,AS760*EXP((-$J$6*1)/Heterogenität!$D$4),Z761)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF761>=$J$19, AR760/$J$5<AN761),0, Bodencharakterisierung!$E$8*$J$11*((AR760/$J$5)-AN761))","v":0},0,{"$f":"AQ760-AP761*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ761/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,744,null,{"$f":"(AP761)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF761<=$J$9*1.05,(AV761*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW760,NA())","v":{"$error":"#N/A"}},23072.238162637354,877,9.6386557179995798,1.6118115579995647,0,4.6668441600000161,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},5.0290510184893815,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,747,2.3305291073371062E-2,{"$f":"Z764*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3066131107098577E-2},{"$f":"AF763*Bodencharakterisierung!$E$11/$J$20","v":5.1538059755115239E-6},{"$f":"((150*($J$2^0.87)*(AB764^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z764)*3600*24","v":1.5245130871489446E-2},2.3915996627248484E-4,{"$f":"AE763-AD764*Bodencharakterisierung!$E$8","v":7.3822439264016517E-3},{"$f":"IF(AE764>$J$18,(AE764/(Bodencharakterisierung!$E$11*1000)),0)","v":4.8727682682519151E-6},2.3305291073371062E-2,747,null,{"$f":"(AD764)*$G$11*Bodencharakterisierung!$E$8","v":3.4584681384394477E-6},{"$f":"IF(AH764>0,(AJ764*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK763,NA())","v":1.6183139597656919},null,747,{"$f":"IF(AF764<=$J$9*0.05,AS763*EXP((-$J$6*1)/Heterogenität!$D$4),Z764)","v":2.3305291073371062E-2},{"$f":"IF(OR(AF764>=$J$19, AR763/$J$5<AN764),0, Bodencharakterisierung!$E$8*$J$11*((AR763/$J$5)-AN764))","v":0},0,{"$f":"AQ763-AP764*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ764/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.3305291073371062E-2,747,null,{"$f":"(AP764)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF764<=$J$9*1.05,(AV764*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW763,NA())","v":{"$error":"#N/A"}},23072.238162637354,880,9.6639760397657071,1.6183139597656919,0,4.6856620800000153,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},4.8727682682519147,23305.291073371063]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,759,2.3066131107098577E-2,{"$f":"Z776*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.2829425411372957E-2},{"$f":"AF775*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB776^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z776)*3600*24","v":0},0,{"$f":"AE775-AD776*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE776>$J$18,(AE776/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.2829425411372957E-2,{"$error":"#N/A"},null,{"$f":"(AD776)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH776>0,(AJ776*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK775,NA())","v":{"$error":"#N/A"}},null,759,{"$f":"IF(AF776<=$J$9*0.05,AS775*EXP((-$J$6*1)/Heterogenität!$D$4),Z776)","v":2.2595148800357241E-2},{"$f":"IF(OR(AF776>=$J$19, AR775/$J$5<AN776),0, Bodencharakterisierung!$E$8*$J$11*((AR775/$J$5)-AN776))","v":0},0,{"$f":"AQ775-AP776*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ776/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.2595148800357241E-2,759,null,{"$f":"(AP776)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF776<=$J$9*1.05,(AV776*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW775,NA())","v":{"$error":"#N/A"}},22369.19731235367,892,9.7609223923194612,1.6399886323194495,0,4.7609337600000119,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,22595.148800357241]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,766,2.1459338455939291E-2,{"$f":"Z783*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.1239121740121637E-2},{"$f":"AF782*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB783^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z783)*3600*24","v":0},0,{"$f":"AE782-AD783*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE783>$J$18,(AE783/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.1239121740121637E-2,{"$error":"#N/A"},null,{"$f":"(AD783)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH783>0,(AJ783*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK782,NA())","v":{"$error":"#N/A"}},null,766,{"$f":"IF(AF783<=$J$9*0.05,AS782*EXP((-$J$6*1)/Heterogenität!$D$4),Z783)","v":2.1021164898345539E-2},{"$f":"IF(OR(AF783>=$J$19, AR782/$J$5<AN783),0, Bodencharakterisierung!$E$8*$J$11*((AR782/$J$5)-AN783))","v":0},0,{"$f":"AQ782-AP783*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ783/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.1021164898345539E-2,766,null,{"$f":"(AP783)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF783<=$J$9*1.05,(AV783*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW782,NA())","v":{"$error":"#N/A"}},20810.953249362083,899,9.8048308723194584,1.6399886323194495,0,4.8048422400000099,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,21021.164898345538]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,777,1.9157498569295984E-2,{"$f":"Z794*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.8960903440006519E-2},{"$f":"AF793*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB794^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z794)*3600*24","v":0},0,{"$f":"AE793-AD794*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE794>$J$18,(AE794/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.8960903440006519E-2,{"$error":"#N/A"},null,{"$f":"(AD794)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH794>0,(AJ794*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK793,NA())","v":{"$error":"#N/A"}},null,777,{"$f":"IF(AF794<=$J$9*0.05,AS793*EXP((-$J$6*1)/Heterogenität!$D$4),Z794)","v":1.8766325778953867E-2},{"$f":"IF(OR(AF794>=$J$19, AR793/$J$5<AN794),0, Bodencharakterisierung!$E$8*$J$11*((AR793/$J$5)-AN794))","v":0},0,{"$f":"AQ793-AP794*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ794/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},1.8766325778953867E-2,777,null,{"$f":"(AP794)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF794<=$J$9*1.05,(AV794*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW793,NA())","v":{"$error":"#N/A"}},18578.662521164326,910,9.8738299123194562,1.6399886323194495,0,4.8738412800000068,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,18766.325778953866]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,789,1.6927058644901957E-2,{"$f":"Z806*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.6753352392452153E-2},{"$f":"AF805*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB806^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z806)*3600*24","v":0},0,{"$f":"AE805-AD806*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE806>$J$18,(AE806/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.6753352392452153E-2,{"$error":"#N/A"},null,{"$f":"(AD806)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH806>0,(AJ806*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK805,NA())","v":{"$error":"#N/A"}},null,789,{"$f":"IF(AF806<=$J$9*0.05,AS805*EXP((-$J$6*1)/Heterogenität!$D$4),Z806)","v":1.6581428721534862E-2},{"$f":"IF(OR(AF806>=$J$19, AR805/$J$5<AN806),0, Bodencharakterisierung!$E$8*$J$11*((AR805/$J$5)-AN806))","v":0},0,{"$f":"AQ805-AP806*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ806/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},1.6581428721534862E-2,789,null,{"$f":"(AP806)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF806<=$J$9*1.05,(AV806*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW805,NA())","v":{"$error":"#N/A"}},16415.614434319516,922,9.9491015923194528,1.6399886323194495,0,4.9491129600000034,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,16581.428721534863]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,796,1.5747915367250141E-2,{"$f":"Z813*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.5586309537216254E-2},{"$f":"AF812*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB813^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z813)*3600*24","v":0},0,{"$f":"AE812-AD813*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE813>$J$18,(AE813/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.5586309537216254E-2,{"$error":"#N/A"},null,{"$f":"(AD813)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH813>0,(AJ813*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK812,NA())","v":{"$error":"#N/A"}},null,796,{"$f":"IF(AF813<=$J$9*0.05,AS812*EXP((-$J$6*1)/Heterogenität!$D$4),Z813)","v":1.5426362113624864E-2},{"$f":"IF(OR(AF813>=$J$19, AR812/$J$5<AN813),0, Bodencharakterisierung!$E$8*$J$11*((AR812/$J$5)-AN813))","v":0},0,{"$f":"AQ812-AP813*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ813/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},1.5426362113624864E-2,796,null,{"$f":"(AP813)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF813<=$J$9*1.05,(AV813*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW812,NA())","v":{"$error":"#N/A"}},15272.098492488614,929,9.9930100723194499,1.6399886323194495,0,4.9930214400000015,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,15426.362113624864]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,808,1.3914441177807272E-2,{"$f":"Z825*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.3771650544027667E-2},{"$f":"AF824*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB825^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z825)*3600*24","v":0},0,{"$f":"AE824-AD825*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE825>$J$18,(AE825/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.3771650544027667E-2,{"$error":"#N/A"},null,{"$f":"(AD825)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH825>0,(AJ825*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK824,NA())","v":{"$error":"#N/A"}},null,808,{"$f":"IF(AF825<=$J$9*0.05,AS824*EXP((-$J$6*1)/Heterogenität!$D$4),Z825)","v":1.3630325234283329E-2},{"$f":"IF(OR(AF825>=$J$19, AR824/$J$5<AN825),0, Bodencharakterisierung!$E$8*$J$11*((AR824/$J$5)-AN825))","v":0},0,{"$f":"AQ824-AP825*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ825/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},1.3630325234283329E-2,808,null,{"$f":"(AP825)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF825<=$J$9*1.05,(AV825*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW824,NA())","v":{"$error":"#N/A"}},13494.021981940496,941,10.068281752319447,1.6399886323194495,0,5.0682931199999981,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,13630.325234283329]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,815,1.2945157611105948E-2,{"$f":"Z832*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.2812313809759841E-2},{"$f":"AF831*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB832^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z832)*3600*24","v":0},0,{"$f":"AE831-AD832*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE832>$J$18,(AE832/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.2812313809759841E-2,{"$error":"#N/A"},null,{"$f":"(AD832)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH832>0,(AJ832*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK831,NA())","v":{"$error":"#N/A"}},null,815,{"$f":"IF(AF832<=$J$9*0.05,AS831*EXP((-$J$6*1)/Heterogenität!$D$4),Z832)","v":1.2680833257598199E-2},{"$f":"IF(OR(AF832>=$J$19, AR831/$J$5<AN832),0, Bodencharakterisierung!$E$8*$J$11*((AR831/$J$5)-AN832))","v":0},0,{"$f":"AQ831-AP832*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ832/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},1.2680833257598199E-2,815,null,{"$f":"(AP832)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF832<=$J$9*1.05,(AV832*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW831,NA())","v":{"$error":"#N/A"}},12554.024925022217,948,10.112190232319445,1.6399886323194495,0,5.1122015999999961,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,12680.833257598199]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,817,1.2680833257598199E-2,{"$f":"Z834*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.255070196489534E-2},{"$f":"AF833*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB834^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z834)*3600*24","v":0},0,{"$f":"AE833-AD834*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE834>$J$18,(AE834/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.255070196489534E-2,{"$error":"#N/A"},null,{"$f":"(AD834)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH834>0,(AJ834*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK833,NA())","v":{"$error":"#N/A"}},null,817,{"$f":"IF(AF834<=$J$9*0.05,AS833*EXP((-$J$6*1)/Heterogenität!$D$4),Z834)","v":1.2421906085488793E-2},{"$f":"IF(OR(AF834>=$J$19, AR833/$J$5<AN834),0, Bodencharakterisierung!$E$8*$J$11*((AR833/$J$5)-AN834))","v":0},0,{"$f":"AQ833-AP834*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ834/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},1.2421906085488793E-2,817,null,{"$f":"(AP834)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF834<=$J$9*1.05,(AV834*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW833,NA())","v":{"$error":"#N/A"}},12297.687024633906,950,10.124735512319445,1.6399886323194495,0,5.1247468799999956,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,12421.906085488794]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,829,1.1204448610091997E-2,{"$f":"Z846*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.1089468044380324E-2},{"$f":"AF845*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB846^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z846)*3600*24","v":0},0,{"$f":"AE845-AD846*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE846>$J$18,(AE846/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.1089468044380324E-2,{"$error":"#N/A"},null,{"$f":"(AD846)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH846>0,(AJ846*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK845,NA())","v":{"$error":"#N/A"}},null,829,{"$f":"IF(AF846<=$J$9*0.05,AS845*EXP((-$J$6*1)/Heterogenität!$D$4),Z846)","v":1.0975667414509446E-2},{"$f":"IF(OR(AF846>=$J$19, AR845/$J$5<AN846),0, Bodencharakterisierung!$E$8*$J$11*((AR845/$J$5)-AN846))","v":0},0,{"$f":"AQ845-AP846*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ846/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},1.0975667414509446E-2,829,null,{"$f":"(AP846)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF846<=$J$9*1.05,(AV846*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW845,NA())","v":{"$error":"#N/A"}},10865.910740364352,962,10.200007192319442,1.6399886323194495,0,5.2000185599999922,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,10975.667414509446]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,836,1.0423943825679008E-2,{"$f":"Z853*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.0316972835875573E-2},{"$f":"AF852*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB853^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z853)*3600*24","v":0},0,{"$f":"AE852-AD853*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE853>$J$18,(AE853/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.0316972835875573E-2,{"$error":"#N/A"},null,{"$f":"(AD853)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH853>0,(AJ853*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK852,NA())","v":{"$error":"#N/A"}},null,836,{"$f":"IF(AF853<=$J$9*0.05,AS852*EXP((-$J$6*1)/Heterogenität!$D$4),Z853)","v":1.0211099587277471E-2},{"$f":"IF(OR(AF853>=$J$19, AR852/$J$5<AN853),0, Bodencharakterisierung!$E$8*$J$11*((AR852/$J$5)-AN853))","v":0},0,{"$f":"AQ852-AP853*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ853/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},1.0211099587277471E-2,836,null,{"$f":"(AP853)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF853<=$J$9*1.05,(AV853*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW852,NA())","v":{"$error":"#N/A"}},10108.988591404695,969,10.243915672319439,1.6399886323194495,0,5.2439270399999902,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,10211.099587277471]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,846,9.4023044535608766E-3,{"$f":"Z863*EXP((-$J$6/Heterogenität!$D$4)*1)","v":9.305817573868282E-3},{"$f":"AF862*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB863^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z863)*3600*24","v":0},0,{"$f":"AE862-AD863*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE863>$J$18,(AE863/(Bodencharakterisierung!$E$11*1000)),0)","v":0},9.305817573868282E-3,{"$error":"#N/A"},null,{"$f":"(AD863)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH863>0,(AJ863*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK862,NA())","v":{"$error":"#N/A"}},null,846,{"$f":"IF(AF863<=$J$9*0.05,AS862*EXP((-$J$6*1)/Heterogenität!$D$4),Z863)","v":9.210320846962038E-3},{"$f":"IF(OR(AF863>=$J$19, AR862/$J$5<AN863),0, Bodencharakterisierung!$E$8*$J$11*((AR862/$J$5)-AN863))","v":0},0,{"$f":"AQ862-AP863*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ863/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},9.210320846962038E-3,846,null,{"$f":"(AP863)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF863<=$J$9*1.05,(AV863*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW862,NA())","v":{"$error":"#N/A"}},9118.2176384924187,979,10.306642072319436,1.6399886323194495,0,5.3066534399999874,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,9210.3208469620386]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,854,8.6575719178761997E-3,{"$f":"Z871*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.5687275176341143E-3},{"$f":"AF870*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB871^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z871)*3600*24","v":0},0,{"$f":"AE870-AD871*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE871>$J$18,(AE871/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.5687275176341143E-3,{"$error":"#N/A"},null,{"$f":"(AD871)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH871>0,(AJ871*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK870,NA())","v":{"$error":"#N/A"}},null,854,{"$f":"IF(AF871<=$J$9*0.05,AS870*EXP((-$J$6*1)/Heterogenität!$D$4),Z871)","v":8.4807948427036116E-3},{"$f":"IF(OR(AF871>=$J$19, AR870/$J$5<AN871),0, Bodencharakterisierung!$E$8*$J$11*((AR870/$J$5)-AN871))","v":0},0,{"$f":"AQ870-AP871*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ871/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},8.4807948427036116E-3,854,null,{"$f":"(AP871)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF871<=$J$9*1.05,(AV871*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW870,NA())","v":{"$error":"#N/A"}},8395.9868942765752,987,10.356823192319434,1.6399886323194495,0,5.3568345599999851,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,8480.7948427036117]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,866,7.6496013843488017E-3,{"$f":"Z883*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.571100823968795E-3},{"$f":"AF882*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB883^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z883)*3600*24","v":0},0,{"$f":"AE882-AD883*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE883>$J$18,(AE883/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.571100823968795E-3,{"$error":"#N/A"},null,{"$f":"(AD883)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH883>0,(AJ883*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK882,NA())","v":{"$error":"#N/A"}},null,866,{"$f":"IF(AF883<=$J$9*0.05,AS882*EXP((-$J$6*1)/Heterogenität!$D$4),Z883)","v":7.4934058399411165E-3},{"$f":"IF(OR(AF883>=$J$19, AR882/$J$5<AN883),0, Bodencharakterisierung!$E$8*$J$11*((AR882/$J$5)-AN883))","v":0},0,{"$f":"AQ882-AP883*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ883/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},7.4934058399411165E-3,866,null,{"$f":"(AP883)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF883<=$J$9*1.05,(AV883*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW882,NA())","v":{"$error":"#N/A"}},7418.4717815417062,999,10.43209487231943,1.6399886323194495,0,5.4321062399999818,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,7493.4058399411169]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,878,6.7589853014799845E-3,{"$f":"Z895*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.6896242842050197E-3},{"$f":"AF894*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB895^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z895)*3600*24","v":0},0,{"$f":"AE894-AD895*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE895>$J$18,(AE895/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.6896242842050197E-3,{"$error":"#N/A"},null,{"$f":"(AD895)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH895>0,(AJ895*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK894,NA())","v":{"$error":"#N/A"}},null,878,{"$f":"IF(AF895<=$J$9*0.05,AS894*EXP((-$J$6*1)/Heterogenität!$D$4),Z895)","v":6.6209750528717056E-3},{"$f":"IF(OR(AF895>=$J$19, AR894/$J$5<AN895),0, Bodencharakterisierung!$E$8*$J$11*((AR894/$J$5)-AN895))","v":0},0,{"$f":"AQ894-AP895*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ895/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},6.6209750528717056E-3,878,null,{"$f":"(AP895)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF895<=$J$9*1.05,(AV895*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW894,NA())","v":{"$error":"#N/A"}},6554.7653023429884,1011,10.507366552319427,1.6399886323194495,0,5.5073779199999784,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,6620.9750528717059]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,885,6.2881526394576379E-3,{"$f":"Z902*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.2236233285627709E-3},{"$f":"AF901*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB902^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z902)*3600*24","v":0},0,{"$f":"AE901-AD902*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE902>$J$18,(AE902/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.2236233285627709E-3,{"$error":"#N/A"},null,{"$f":"(AD902)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH902>0,(AJ902*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK901,NA())","v":{"$error":"#N/A"}},null,885,{"$f":"IF(AF902<=$J$9*0.05,AS901*EXP((-$J$6*1)/Heterogenität!$D$4),Z902)","v":6.1597562204169978E-3},{"$f":"IF(OR(AF902>=$J$19, AR901/$J$5<AN902),0, Bodencharakterisierung!$E$8*$J$11*((AR901/$J$5)-AN902))","v":0},0,{"$f":"AQ901-AP902*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ902/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},6.1597562204169978E-3,885,null,{"$f":"(AP902)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF902<=$J$9*1.05,(AV902*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW901,NA())","v":{"$error":"#N/A"}},6098.1586582128284,1018,10.551275032319426,1.6399886323194495,0,5.5512863999999764,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,6159.7562204169981]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,895,5.6718576534339578E-3,{"$f":"Z912*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.6136527899620942E-3},{"$f":"AF911*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB912^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z912)*3600*24","v":0},0,{"$f":"AE911-AD912*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE912>$J$18,(AE912/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.6136527899620942E-3,{"$error":"#N/A"},null,{"$f":"(AD912)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH912>0,(AJ912*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK911,NA())","v":{"$error":"#N/A"}},null,895,{"$f":"IF(AF912<=$J$9*0.05,AS911*EXP((-$J$6*1)/Heterogenität!$D$4),Z912)","v":5.5560452274696949E-3},{"$f":"IF(OR(AF912>=$J$19, AR911/$J$5<AN912),0, Bodencharakterisierung!$E$8*$J$11*((AR911/$J$5)-AN912))","v":0},0,{"$f":"AQ911-AP912*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ912/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},5.5560452274696949E-3,895,null,{"$f":"(AP912)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF912<=$J$9*1.05,(AV912*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW911,NA())","v":{"$error":"#N/A"}},5500.4847751949974,1028,10.614001432319423,1.6399886323194495,0,5.6140127999999736,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,5556.0452274696945]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,899,5.4425975502045837E-3,{"$f":"Z916*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.3867453644308172E-3},{"$f":"AF915*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB916^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z916)*3600*24","v":0},0,{"$f":"AE915-AD916*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE916>$J$18,(AE916/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.3867453644308172E-3,{"$error":"#N/A"},null,{"$f":"(AD916)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH916>0,(AJ916*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK915,NA())","v":{"$error":"#N/A"}},null,899,{"$f":"IF(AF916<=$J$9*0.05,AS915*EXP((-$J$6*1)/Heterogenität!$D$4),Z916)","v":5.3314663363500329E-3},{"$f":"IF(OR(AF916>=$J$19, AR915/$J$5<AN916),0, Bodencharakterisierung!$E$8*$J$11*((AR915/$J$5)-AN916))","v":0},0,{"$f":"AQ915-AP916*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ916/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},5.3314663363500329E-3,899,null,{"$f":"(AP916)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF916<=$J$9*1.05,(AV916*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW915,NA())","v":{"$error":"#N/A"}},5278.1516729865325,1032,10.639091992319422,1.6399886323194495,0,{"$f":"$G$34/$G$12/$G$8+BC915","v":5.6391033599999725},null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,5331.4663363500331]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,906,5.0634647989737129E-3,{"$f":"Z923*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.011503290888189E-3},{"$f":"AF922*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB923^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z923)*3600*24","v":0},0,{"$f":"AE922-AD923*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE923>$J$18,(AE923/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.011503290888189E-3,{"$error":"#N/A"},null,{"$f":"(AD923)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH923>0,(AJ923*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK922,NA())","v":{"$error":"#N/A"}},null,906,{"$f":"IF(AF923<=$J$9*0.05,AS922*EXP((-$J$6*1)/Heterogenität!$D$4),Z923)","v":4.9600750141827014E-3},{"$f":"IF(OR(AF923>=$J$19, AR922/$J$5<AN923),0, Bodencharakterisierung!$E$8*$J$11*((AR922/$J$5)-AN923))","v":0},0,{"$f":"AQ922-AP923*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ923/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},4.9600750141827014E-3,906,null,{"$f":"(AP923)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF923<=$J$9*1.05,(AV923*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW922,NA())","v":{"$error":"#N/A"}},4910.474264040874,1039,10.683000472319419,1.6399886323194495,0,5.6830118399999705,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,4960.0750141827011]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,918,4.4739434685900368E-3,{"$f":"Z935*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.4280316554449273E-3},{"$f":"AF934*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB935^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z935)*3600*24","v":0},0,{"$f":"AE934-AD935*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE935>$J$18,(AE935/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.4280316554449273E-3,{"$error":"#N/A"},null,{"$f":"(AD935)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH935>0,(AJ935*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK934,NA())","v":{"$error":"#N/A"}},null,918,{"$f":"IF(AF935<=$J$9*0.05,AS934*EXP((-$J$6*1)/Heterogenität!$D$4),Z935)","v":4.3825909914328078E-3},{"$f":"IF(OR(AF935>=$J$19, AR934/$J$5<AN935),0, Bodencharakterisierung!$E$8*$J$11*((AR934/$J$5)-AN935))","v":0},0,{"$f":"AQ934-AP935*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ935/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},4.3825909914328078E-3,918,null,{"$f":"(AP935)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF935<=$J$9*1.05,(AV935*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW934,NA())","v":{"$error":"#N/A"}},4338.7650815184797,1051,10.758272152319416,1.6399886323194495,0,5.7582835199999671,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,4382.5909914328076]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,926,4.1195738265166941E-3,{"$f":"Z943*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.077298570897489E-3},{"$f":"AF942*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB943^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z943)*3600*24","v":0},0,{"$f":"AE942-AD943*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE943>$J$18,(AE943/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.077298570897489E-3,{"$error":"#N/A"},null,{"$f":"(AD943)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH943>0,(AJ943*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK942,NA())","v":{"$error":"#N/A"}},null,926,{"$f":"IF(AF943<=$J$9*0.05,AS942*EXP((-$J$6*1)/Heterogenität!$D$4),Z943)","v":4.0354571458910927E-3},{"$f":"IF(OR(AF943>=$J$19, AR942/$J$5<AN943),0, Bodencharakterisierung!$E$8*$J$11*((AR942/$J$5)-AN943))","v":0},0,{"$f":"AQ942-AP943*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ943/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},4.0354571458910927E-3,926,null,{"$f":"(AP943)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF943<=$J$9*1.05,(AV943*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW942,NA())","v":{"$error":"#N/A"}},3995.1025744321819,1059,10.808453272319413,1.6399886323194495,0,5.8084646399999649,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,4035.4571458910928]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,936,3.7158188861697618E-3,{"$f":"Z953*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.6776869822732071E-3},{"$f":"AF952*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB953^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z953)*3600*24","v":0},0,{"$f":"AE952-AD953*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE953>$J$18,(AE953/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.6776869822732071E-3,{"$error":"#N/A"},null,{"$f":"(AD953)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH953>0,(AJ953*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK952,NA())","v":{"$error":"#N/A"}},null,936,{"$f":"IF(AF953<=$J$9*0.05,AS952*EXP((-$J$6*1)/Heterogenität!$D$4),Z953)","v":3.6399463897239812E-3},{"$f":"IF(OR(AF953>=$J$19, AR952/$J$5<AN953),0, Bodencharakterisierung!$E$8*$J$11*((AR952/$J$5)-AN953))","v":0},0,{"$f":"AQ952-AP953*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ953/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},3.6399463897239812E-3,936,null,{"$f":"(AP953)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF953<=$J$9*1.05,(AV953*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW952,NA())","v":{"$error":"#N/A"}},3603.5469258267412,1069,10.871179672319411,1.6399886323194495,0,5.8711910399999621,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,3639.9463897239812]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,948,3.2831992116568523E-3,{"$f":"Z965*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.2495068707093116E-3},{"$f":"AF964*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB965^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z965)*3600*24","v":0},0,{"$f":"AE964-AD965*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE965>$J$18,(AE965/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.2495068707093116E-3,{"$error":"#N/A"},null,{"$f":"(AD965)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH965>0,(AJ965*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK964,NA())","v":{"$error":"#N/A"}},null,948,{"$f":"IF(AF965<=$J$9*0.05,AS964*EXP((-$J$6*1)/Heterogenität!$D$4),Z965)","v":3.2161602821104236E-3},{"$f":"IF(OR(AF965>=$J$19, AR964/$J$5<AN965),0, Bodencharakterisierung!$E$8*$J$11*((AR964/$J$5)-AN965))","v":0},0,{"$f":"AQ964-AP965*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ965/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},3.2161602821104236E-3,948,null,{"$f":"(AP965)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF965<=$J$9*1.05,(AV965*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW964,NA())","v":{"$error":"#N/A"}},3183.9986792893192,1081,10.946451352319407,1.6399886323194495,0,5.9464627199999587,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,3216.1602821104234]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,955,3.0544907064858798E-3,{"$f":"Z972*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.0231453827118519E-3},{"$f":"AF971*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB972^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z972)*3600*24","v":0},0,{"$f":"AE971-AD972*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE972>$J$18,(AE972/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.0231453827118519E-3,{"$error":"#N/A"},null,{"$f":"(AD972)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH972>0,(AJ972*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK971,NA())","v":{"$error":"#N/A"}},null,955,{"$f":"IF(AF972<=$J$9*0.05,AS971*EXP((-$J$6*1)/Heterogenität!$D$4),Z972)","v":2.9921217260885577E-3},{"$f":"IF(OR(AF972>=$J$19, AR971/$J$5<AN972),0, Bodencharakterisierung!$E$8*$J$11*((AR971/$J$5)-AN972))","v":0},0,{"$f":"AQ971-AP972*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ972/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.9921217260885577E-3,955,null,{"$f":"(AP972)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF972<=$J$9*1.05,(AV972*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW971,NA())","v":{"$error":"#N/A"}},2962.2005088276724,1088,10.990359832319406,1.6399886323194495,0,5.9903711999999567,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,2992.1217260885578]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,958,2.9614164356529383E-3,{"$f":"Z975*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.9310262443165685E-3},{"$f":"AF974*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB975^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z975)*3600*24","v":0},0,{"$f":"AE974-AD975*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE975>$J$18,(AE975/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.9310262443165685E-3,{"$error":"#N/A"},null,{"$f":"(AD975)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH975>0,(AJ975*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK974,NA())","v":{"$error":"#N/A"}},null,958,{"$f":"IF(AF975<=$J$9*0.05,AS974*EXP((-$J$6*1)/Heterogenität!$D$4),Z975)","v":2.9009479185180347E-3},{"$f":"IF(OR(AF975>=$J$19, AR974/$J$5<AN975),0, Bodencharakterisierung!$E$8*$J$11*((AR974/$J$5)-AN975))","v":0},0,{"$f":"AQ974-AP975*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ975/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.9009479185180347E-3,958,null,{"$f":"(AP975)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF975<=$J$9*1.05,(AV975*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW974,NA())","v":{"$error":"#N/A"}},2871.9384393328546,1091,11.009177752319404,1.6399886323194495,0,6.0091891199999559,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,2900.9479185180348]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,967,2.6988671371668822E-3,{"$f":"Z984*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.6711712387776851E-3},{"$f":"AF983*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB984^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z984)*3600*24","v":0},0,{"$f":"AE983-AD984*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE984>$J$18,(AE984/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.6711712387776851E-3,{"$error":"#N/A"},null,{"$f":"(AD984)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH984>0,(AJ984*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK983,NA())","v":{"$error":"#N/A"}},null,967,{"$f":"IF(AF984<=$J$9*0.05,AS983*EXP((-$J$6*1)/Heterogenität!$D$4),Z984)","v":2.6437595569684825E-3},{"$f":"IF(OR(AF984>=$J$19, AR983/$J$5<AN984),0, Bodencharakterisierung!$E$8*$J$11*((AR983/$J$5)-AN984))","v":0},0,{"$f":"AQ983-AP984*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ984/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.6437595569684825E-3,967,null,{"$f":"(AP984)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF984<=$J$9*1.05,(AV984*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW983,NA())","v":{"$error":"#N/A"}},2617.3219613987976,1100,11.065631512319403,1.6399886323194495,0,6.0656428799999533,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,2643.7595569684827]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,976,2.4595945833174927E-3,{"$f":"Z993*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.4343541108540392E-3},{"$f":"AF992*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB993^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z993)*3600*24","v":0},0,{"$f":"AE992-AD993*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE993>$J$18,(AE993/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.4343541108540392E-3,{"$error":"#N/A"},null,{"$f":"(AD993)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH993>0,(AJ993*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK992,NA())","v":{"$error":"#N/A"}},null,976,{"$f":"IF(AF993<=$J$9*0.05,AS992*EXP((-$J$6*1)/Heterogenität!$D$4),Z993)","v":2.4093726572770716E-3},{"$f":"IF(OR(AF993>=$J$19, AR992/$J$5<AN993),0, Bodencharakterisierung!$E$8*$J$11*((AR992/$J$5)-AN993))","v":0},0,{"$f":"AQ992-AP993*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ993/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.4093726572770716E-3,976,null,{"$f":"(AP993)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF993<=$J$9*1.05,(AV993*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW992,NA())","v":{"$error":"#N/A"}},2385.2789307043008,1109,11.122085272319399,1.6399886323194495,0,6.1220966399999508,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,2409.3726572770715]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,988,2.1732326693854162E-3,{"$f":"Z1005*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.1509308560213967E-3},{"$f":"AF1004*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1005^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1005)*3600*24","v":0},0,{"$f":"AE1004-AD1005*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1005>$J$18,(AE1005/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.1509308560213967E-3,{"$error":"#N/A"},null,{"$f":"(AD1005)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1005>0,(AJ1005*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1004,NA())","v":{"$error":"#N/A"}},null,988,{"$f":"IF(AF1005<=$J$9*0.05,AS1004*EXP((-$J$6*1)/Heterogenität!$D$4),Z1005)","v":2.1288579048893553E-3},{"$f":"IF(OR(AF1005>=$J$19, AR1004/$J$5<AN1005),0, Bodencharakterisierung!$E$8*$J$11*((AR1004/$J$5)-AN1005))","v":0},0,{"$f":"AQ1004-AP1005*Bodencharakterisierung!$E$8","v":6.6397905000974864E-3},{"$f":"AQ1005/(Bodencharakterisierung!$E$11*1000)","v":4.3827000000643478E-6},2.1288579048893553E-3,988,null,{"$f":"(AP1005)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF1005<=$J$9*1.05,(AV1005*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1004,NA())","v":{"$error":"#N/A"}},2107.5693258404617,1121,11.197356952319396,1.6399886323194495,0,6.1973683199999474,null,4.3827000000643475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,2128.8579048893553]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,995,2.0218447202658032E-3,{"$f":"Z1012*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.0010964569815281E-3},{"$f":"AF1011*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1012^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1012)*3600*24","v":0},0,{"$f":"AE1011-AD1012*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1012>$J$18,(AE1012/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.0010964569815281E-3,{"$error":"#N/A"},null,{"$f":"(AD1012)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1012>0,(AJ1012*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1011,NA())","v":{"$error":"#N/A"}},null,995,{"$f":"IF(AF1012<=$J$9*0.05,AS1011*EXP((-$J$6*1)/Heterogenität!$D$4),Z1012)","v":2.1070114673945668E-3},{"$f":"IF(OR(AF1012>=$J$19, AR1011/$J$5<AN1012),0, Bodencharakterisierung!$E$8*$J$11*((AR1011/$J$5)-AN1012))","v":6.3138977779970533E-5},2.1846437494788505E-5,{"$f":"AQ1011-AP1012*Bodencharakterisierung!$E$8","v":6.5893252294845252E-3},{"$f":"AQ1012/(Bodencharakterisierung!$E$11*1000)","v":4.3493895904188281E-6},2.1288579048893553E-3,995,null,{"$f":"(AP1012)*$G$11*Bodencharakterisierung!$E$8","v":3.1591912807033841E-7},{"$f":"IF(AF1012<=$J$9*1.05,(AV1012*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1011,NA())","v":{"$error":"#N/A"}},2085.9413527206211,1128,11.241265432319395,1.6399886323194495,0,6.2412767999999454,null,4.349389590418828,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,2107.0114673945668]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1007,1.7864484774476658E-3,{"$f":"Z1024*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.768115861207481E-3},{"$f":"AF1023*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1024^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1024)*3600*24","v":0},0,{"$f":"AE1023-AD1024*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1024>$J$18,(AE1024/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.768115861207481E-3,{"$error":"#N/A"},null,{"$f":"(AD1024)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1024>0,(AJ1024*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1023,NA())","v":{"$error":"#N/A"}},null,1007,{"$f":"IF(AF1024<=$J$9*0.05,AS1023*EXP((-$J$6*1)/Heterogenität!$D$4),Z1024)","v":2.0801708759093447E-3},{"$f":"IF(OR(AF1024>=$J$19, AR1023/$J$5<AN1024),0, Bodencharakterisierung!$E$8*$J$11*((AR1023/$J$5)-AN1024))","v":8.4021707682855825E-5},2.1568142234758281E-5,{"$f":"AQ1023-AP1024*Bodencharakterisierung!$E$8","v":6.5123118042467306E-3},{"$f":"AQ1024/(Bodencharakterisierung!$E$11*1000)","v":4.2985556463674794E-6},2.101739018144103E-3,1007,null,{"$f":"(AP1024)*$G$11*Bodencharakterisierung!$E$8","v":3.1189472839804267E-7},{"$f":"IF(AF1024<=$J$9*1.05,(AV1024*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1023,NA())","v":{"$error":"#N/A"}},2059.3691671502515,1140,11.316537112319391,1.6399886323194495,0,6.3165484799999421,null,4.298555646367479,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,2080.1708759093449]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1016,1.6280679170885635E-3,{"$f":"Z1033*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.6113606094254932E-3},{"$f":"AF1032*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1033^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1033)*3600*24","v":0},0,{"$f":"AE1032-AD1033*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1033>$J$18,(AE1033/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.6113606094254932E-3,{"$error":"#N/A"},null,{"$f":"(AD1033)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1033>0,(AJ1033*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1032,NA())","v":{"$error":"#N/A"}},null,1016,{"$f":"IF(AF1033<=$J$9*0.05,AS1032*EXP((-$J$6*1)/Heterogenität!$D$4),Z1033)","v":2.0685932138786696E-3},{"$f":"IF(OR(AF1033>=$J$19, AR1032/$J$5<AN1033),0, Bodencharakterisierung!$E$8*$J$11*((AR1032/$J$5)-AN1033))","v":9.0870147202588571E-6},9.0870147202588571E-6,{"$f":"AQ1032-AP1033*Bodencharakterisierung!$E$8","v":6.4563632351447367E-3},{"$f":"AQ1033/(Bodencharakterisierung!$E$11*1000)","v":4.2616258977853048E-6},2.0776802285989286E-3,1016,null,{"$f":"(AP1033)*$G$11*Bodencharakterisierung!$E$8","v":1.3140640289160796E-7},{"$f":"IF(AF1033<=$J$9*1.05,(AV1033*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1032,NA())","v":{"$error":"#N/A"}},2047.907281739883,1149,11.372990872319388,1.6399886323194495,0,6.3730022399999395,null,4.2616258977853052,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,2068.5932138786698]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1025,1.4837288486707803E-3,{"$f":"Z1042*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.4685027551502806E-3},{"$f":"AF1041*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1042^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1042)*3600*24","v":0},0,{"$f":"AE1041-AD1042*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1042>$J$18,(AE1042/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.4685027551502806E-3,{"$error":"#N/A"},null,{"$f":"(AD1042)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1042>0,(AJ1042*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1041,NA())","v":{"$error":"#N/A"}},null,1025,{"$f":"IF(AF1042<=$J$9*0.05,AS1041*EXP((-$J$6*1)/Heterogenität!$D$4),Z1042)","v":2.0442705010691258E-3},{"$f":"IF(OR(AF1042>=$J$19, AR1041/$J$5<AN1042),0, Bodencharakterisierung!$E$8*$J$11*((AR1041/$J$5)-AN1042))","v":7.4035563860120804E-5},2.1195911087883417E-5,{"$f":"AQ1041-AP1042*Bodencharakterisierung!$E$8","v":6.3971937679250237E-3},{"$f":"AQ1042/(Bodencharakterisierung!$E$11*1000)","v":4.2225701438448999E-6},2.0654664121570092E-3,1025,null,{"$f":"(AP1042)*$G$11*Bodencharakterisierung!$E$8","v":3.065119313452334E-7},{"$f":"IF(AF1042<=$J$9*1.05,(AV1042*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1041,NA())","v":{"$error":"#N/A"}},2023.8277960584346,1158,11.429444632319386,1.6399886323194495,0,6.429455999999937,null,4.2225701438448997,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,2044.2705010691259]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1028,1.438517717266583E-3,{"$f":"Z1045*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.4237555824508996E-3},{"$f":"AF1044*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1045^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1045)*3600*24","v":0},0,{"$f":"AE1044-AD1045*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1045>$J$18,(AE1045/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.4237555824508996E-3,{"$error":"#N/A"},null,{"$f":"(AD1045)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1045>0,(AJ1045*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1044,NA())","v":{"$error":"#N/A"}},null,1028,{"$f":"IF(AF1045<=$J$9*0.05,AS1044*EXP((-$J$6*1)/Heterogenität!$D$4),Z1045)","v":2.0442705010691258E-3},{"$f":"IF(OR(AF1045>=$J$19, AR1044/$J$5<AN1045),0, Bodencharakterisierung!$E$8*$J$11*((AR1044/$J$5)-AN1045))","v":8.3298092108106669E-6},8.3298092108106669E-6,{"$f":"AQ1044-AP1045*Bodencharakterisierung!$E$8","v":6.3804556295674539E-3},{"$f":"AQ1045/(Bodencharakterisierung!$E$11*1000)","v":4.21152186770129E-6},2.0526003102799366E-3,1028,null,{"$f":"(AP1045)*$G$11*Bodencharakterisierung!$E$8","v":1.2045653042970227E-7},{"$f":"IF(AF1045<=$J$9*1.05,(AV1045*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1044,NA())","v":{"$error":"#N/A"}},2023.8277960584346,1161,11.448262552319385,1.6399886323194495,0,6.4482739199999362,null,4.2115218677012898,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,2044.2705010691259]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1044,1.2196600851774775E-3,{"$f":"Z1061*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.2071438774237699E-3},{"$f":"AF1060*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1061^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1061)*3600*24","v":0},0,{"$f":"AE1060-AD1061*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1061>$J$18,(AE1061/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.2071438774237699E-3,{"$error":"#N/A"},null,{"$f":"(AD1061)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1061>0,(AJ1061*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1060,NA())","v":{"$error":"#N/A"}},null,1044,{"$f":"IF(AF1061<=$J$9*0.05,AS1060*EXP((-$J$6*1)/Heterogenität!$D$4),Z1061)","v":2.0019568882274712E-3},{"$f":"IF(OR(AF1061>=$J$19, AR1060/$J$5<AN1061),0, Bodencharakterisierung!$E$8*$J$11*((AR1060/$J$5)-AN1061))","v":1.1897256361167058E-4},2.0757184620359085E-5,{"$f":"AQ1060-AP1061*Bodencharakterisierung!$E$8","v":6.2796211703554459E-3},{"$f":"AQ1061/(Bodencharakterisierung!$E$11*1000)","v":4.1449644688814822E-6},2.0227140728478303E-3,1044,null,{"$f":"(AP1061)*$G$11*Bodencharakterisierung!$E$8","v":3.001675521706092E-7},{"$f":"IF(AF1061<=$J$9*1.05,(AV1061*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1060,NA())","v":{"$error":"#N/A"}},1981.9373193451963,1177,11.54862479231938,1.6399886323194495,0,6.5486361599999316,null,4.144964468881482,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,2001.9568882274712]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1047,1.1824954695343881E-3,{"$f":"Z1064*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.1703606467715715E-3},{"$f":"AF1063*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1064^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1064)*3600*24","v":0},0,{"$f":"AE1063-AD1064*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1064>$J$18,(AE1064/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.1703606467715715E-3,{"$error":"#N/A"},null,{"$f":"(AD1064)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1064>0,(AJ1064*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1063,NA())","v":{"$error":"#N/A"}},null,1047,{"$f":"IF(AF1064<=$J$9*0.05,AS1063*EXP((-$J$6*1)/Heterogenität!$D$4),Z1064)","v":2.0019568882274712E-3},{"$f":"IF(OR(AF1064>=$J$19, AR1063/$J$5<AN1064),0, Bodencharakterisierung!$E$8*$J$11*((AR1063/$J$5)-AN1064))","v":5.4626828520554947E-5},2.0757184620359085E-5,{"$f":"AQ1063-AP1064*Bodencharakterisierung!$E$8","v":6.2590715575812908E-3},{"$f":"AQ1064/(Bodencharakterisierung!$E$11*1000)","v":4.1314003680404556E-6},2.0227140728478303E-3,1047,null,{"$f":"(AP1064)*$G$11*Bodencharakterisierung!$E$8","v":3.001675521706092E-7},{"$f":"IF(AF1064<=$J$9*1.05,(AV1064*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1063,NA())","v":{"$error":"#N/A"}},1981.9373193451963,1180,11.56744271231938,1.6399886323194495,0,6.5674540799999308,null,4.1314003680404552,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,2001.9568882274712]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1058,1.0556548754900778E-3,{"$f":"Z1075*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.044821696722958E-3},{"$f":"AF1074*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1075^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1075)*3600*24","v":0},0,{"$f":"AE1074-AD1075*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1075>$J$18,(AE1075/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.044821696722958E-3,{"$error":"#N/A"},null,{"$f":"(AD1075)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1075>0,(AJ1075*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1074,NA())","v":{"$error":"#N/A"}},null,1058,{"$f":"IF(AF1075<=$J$9*0.05,AS1074*EXP((-$J$6*1)/Heterogenität!$D$4),Z1075)","v":1.9740738586406211E-3},{"$f":"IF(OR(AF1075>=$J$19, AR1074/$J$5<AN1075),0, Bodencharakterisierung!$E$8*$J$11*((AR1074/$J$5)-AN1075))","v":1.2168341710330772E-4},2.0468080895741977E-5,{"$f":"AQ1074-AP1075*Bodencharakterisierung!$E$8","v":6.1935542555575304E-3},{"$f":"AQ1075/(Bodencharakterisierung!$E$11*1000)","v":4.0881546241303828E-6},1.9945419395363631E-3,1058,null,{"$f":"(AP1075)*$G$11*Bodencharakterisierung!$E$8","v":2.9598685238261347E-7},{"$f":"IF(AF1075<=$J$9*1.05,(AV1075*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1074,NA())","v":{"$error":"#N/A"}},1954.3331200542148,1191,11.636441752319376,1.6399886323194495,0,6.6364531199999277,null,4.0881546241303823,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1974.073858640621]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1065,9.8211768417601664E-4,{"$f":"Z1082*EXP((-$J$6/Heterogenität!$D$4)*1)","v":9.7203914744014523E-4},{"$f":"AF1081*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1082^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1082)*3600*24","v":0},0,{"$f":"AE1081-AD1082*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1082>$J$18,(AE1082/(Bodencharakterisierung!$E$11*1000)),0)","v":0},9.7203914744014523E-4,{"$error":"#N/A"},null,{"$f":"(AD1082)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1082>0,(AJ1082*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1081,NA())","v":{"$error":"#N/A"}},null,1065,{"$f":"IF(AF1082<=$J$9*0.05,AS1081*EXP((-$J$6*1)/Heterogenität!$D$4),Z1082)","v":1.9695864968969066E-3},{"$f":"IF(OR(AF1082>=$J$19, AR1081/$J$5<AN1082),0, Bodencharakterisierung!$E$8*$J$11*((AR1081/$J$5)-AN1082))","v":2.2223237866185421E-5},2.0421553921699375E-5,{"$f":"AQ1081-AP1082*Bodencharakterisierung!$E$8","v":6.147799879768095E-3},{"$f":"AQ1082/(Bodencharakterisierung!$E$11*1000)","v":4.0579537160185443E-6},1.990008050818606E-3,1065,null,{"$f":"(AP1082)*$G$11*Bodencharakterisierung!$E$8","v":2.9531403050605827E-7},{"$f":"IF(AF1082<=$J$9*1.05,(AV1082*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1081,NA())","v":{"$error":"#N/A"}},1949.8906319279374,1198,11.680350232319375,1.6399886323194495,0,6.6803615999999257,null,4.0579537160185444,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1969.5864968969065]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1077,8.6777318949598429E-4,{"$f":"Z1094*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.5886806121079592E-4},{"$f":"AF1093*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1094^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1094)*3600*24","v":0},0,{"$f":"AE1093-AD1094*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1094>$J$18,(AE1094/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.5886806121079592E-4,{"$error":"#N/A"},null,{"$f":"(AD1094)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1094>0,(AJ1094*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1093,NA())","v":{"$error":"#N/A"}},null,1077,{"$f":"IF(AF1094<=$J$9*0.05,AS1093*EXP((-$J$6*1)/Heterogenität!$D$4),Z1094)","v":1.9362754345507789E-3},{"$f":"IF(OR(AF1094>=$J$19, AR1093/$J$5<AN1094),0, Bodencharakterisierung!$E$8*$J$11*((AR1093/$J$5)-AN1094))","v":1.3138872690359458E-4},2.0076169925128604E-5,{"$f":"AQ1093-AP1094*Bodencharakterisierung!$E$8","v":6.0788072639905094E-3},{"$f":"AQ1094/(Bodencharakterisierung!$E$11*1000)","v":4.0124140356373001E-6},1.9563516044759075E-3,1077,null,{"$f":"(AP1094)*$G$11*Bodencharakterisierung!$E$8","v":2.9031946738462866E-7},{"$f":"IF(AF1094<=$J$9*1.05,(AV1094*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1093,NA())","v":{"$error":"#N/A"}},1916.9126802052713,1210,11.755621912319372,1.6399886323194495,0,6.7556332799999224,null,4.0124140356372999,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1936.275434550779]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1089,7.667414206473797E-4,{"$f":"Z1106*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.5887308500958669E-4},{"$f":"AF1105*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1106^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1106)*3600*24","v":0},0,{"$f":"AE1105-AD1106*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1106>$J$18,(AE1106/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.5887308500958669E-4,{"$error":"#N/A"},null,{"$f":"(AD1106)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1106>0,(AJ1106*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1105,NA())","v":{"$error":"#N/A"}},null,1089,{"$f":"IF(AF1106<=$J$9*0.05,AS1105*EXP((-$J$6*1)/Heterogenität!$D$4),Z1106)","v":1.9232537264832002E-3},{"$f":"IF(OR(AF1106>=$J$19, AR1105/$J$5<AN1106),0, Bodencharakterisierung!$E$8*$J$11*((AR1105/$J$5)-AN1106))","v":2.4006059255777382E-5},1.9941155030441925E-5,{"$f":"AQ1105-AP1106*Bodencharakterisierung!$E$8","v":6.0039146791560256E-3},{"$f":"AQ1106/(Bodencharakterisierung!$E$11*1000)","v":3.9629799862416009E-6},1.9431948815136421E-3,1089,null,{"$f":"(AP1106)*$G$11*Bodencharakterisierung!$E$8","v":2.8836703061702762E-7},{"$f":"IF(AF1106<=$J$9*1.05,(AV1106*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1105,NA())","v":{"$error":"#N/A"}},1904.0211892183681,1222,11.830893592319368,1.6399886323194495,0,6.830904959999919,null,3.9629799862416011,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1923.2537264832001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1096,7.133300152272269E-4,{"$f":"Z1113*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.0600978988244142E-4},{"$f":"AF1112*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1113^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1113)*3600*24","v":0},0,{"$f":"AE1112-AD1113*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1113>$J$18,(AE1113/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.0600978988244142E-4,{"$error":"#N/A"},null,{"$f":"(AD1113)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1113>0,(AJ1113*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1112,NA())","v":{"$error":"#N/A"}},null,1096,{"$f":"IF(AF1113<=$J$9*0.05,AS1112*EXP((-$J$6*1)/Heterogenität!$D$4),Z1113)","v":1.9068830017740729E-3},{"$f":"IF(OR(AF1113>=$J$19, AR1112/$J$5<AN1113),0, Bodencharakterisierung!$E$8*$J$11*((AR1112/$J$5)-AN1113))","v":5.7730739581262414E-5},1.9771416032986515E-5,{"$f":"AQ1112-AP1113*Bodencharakterisierung!$E$8","v":5.9636450472738411E-3},{"$f":"AQ1113/(Bodencharakterisierung!$E$11*1000)","v":3.9363993711378492E-6},1.9266544178070594E-3,1096,null,{"$f":"(AP1113)*$G$11*Bodencharakterisierung!$E$8","v":2.8591245210332537E-7},{"$f":"IF(AF1113<=$J$9*1.05,(AV1113*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1112,NA())","v":{"$error":"#N/A"}},1887.8141717563321,1229,11.874802072319365,1.6399886323194495,0,6.874813439999917,null,3.9363993711378491,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1906.8830017740729]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1098,6.9876468502600569E-4,{"$f":"Z1115*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.9159392976802169E-4},{"$f":"AF1114*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1115^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1115)*3600*24","v":0},0,{"$f":"AE1114-AD1115*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1115>$J$18,(AE1115/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.9159392976802169E-4,{"$error":"#N/A"},null,{"$f":"(AD1115)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1115>0,(AJ1115*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1114,NA())","v":{"$error":"#N/A"}},null,1098,{"$f":"IF(AF1115<=$J$9*0.05,AS1114*EXP((-$J$6*1)/Heterogenität!$D$4),Z1115)","v":1.9068830017740729E-3},{"$f":"IF(OR(AF1115>=$J$19, AR1114/$J$5<AN1115),0, Bodencharakterisierung!$E$8*$J$11*((AR1114/$J$5)-AN1115))","v":1.6870789265173901E-5},1.6870789265173901E-5,{"$f":"AQ1114-AP1115*Bodencharakterisierung!$E$8","v":5.9515531195254486E-3},{"$f":"AQ1115/(Bodencharakterisierung!$E$11*1000)","v":3.9284179006768637E-6},1.9237537910392467E-3,1098,null,{"$f":"(AP1115)*$G$11*Bodencharakterisierung!$E$8","v":2.4396678111859642E-7},{"$f":"IF(AF1115<=$J$9*1.05,(AV1115*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1114,NA())","v":{"$error":"#N/A"}},1887.8141717563321,1231,11.887347352319365,1.6399886323194495,0,6.8873587199999164,null,3.9284179006768638,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1906.8830017740729]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1114,5.9245387458783255E-4,{"$f":"Z1131*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.8637408574424555E-4},{"$f":"AF1130*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1131^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1131)*3600*24","v":0},0,{"$f":"AE1130-AD1131*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1131>$J$18,(AE1131/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.8637408574424555E-4,{"$error":"#N/A"},null,{"$f":"(AD1131)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1131>0,(AJ1131*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1130,NA())","v":{"$error":"#N/A"}},null,1114,{"$f":"IF(AF1131<=$J$9*0.05,AS1130*EXP((-$J$6*1)/Heterogenität!$D$4),Z1131)","v":1.8725711463653148E-3},{"$f":"IF(OR(AF1131>=$J$19, AR1130/$J$5<AN1131),0, Bodencharakterisierung!$E$8*$J$11*((AR1130/$J$5)-AN1131))","v":6.4570270234213425E-5},1.9415655366223587E-5,{"$f":"AQ1130-AP1131*Bodencharakterisierung!$E$8","v":5.8588531259459453E-3},{"$f":"AQ1131/(Bodencharakterisierung!$E$11*1000)","v":3.8672297861029343E-6},1.8919868017315384E-3,1114,null,{"$f":"(AP1131)*$G$11*Bodencharakterisierung!$E$8","v":2.8076783300136522E-7},{"$f":"IF(AF1131<=$J$9*1.05,(AV1131*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1130,NA())","v":{"$error":"#N/A"}},1853.8454349016615,1247,11.98770959231936,1.6399886323194495,0,6.9877209599999119,null,3.8672297861029343,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1872.5711463653147]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1117,5.7440104101321246E-4,{"$f":"Z1134*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.6850651117605611E-4},{"$f":"AF1133*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1134^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1134)*3600*24","v":0},0,{"$f":"AE1133-AD1134*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1134>$J$18,(AE1134/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.6850651117605611E-4,{"$error":"#N/A"},null,{"$f":"(AD1134)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1134>0,(AJ1134*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1133,NA())","v":{"$error":"#N/A"}},null,1117,{"$f":"IF(AF1134<=$J$9*0.05,AS1133*EXP((-$J$6*1)/Heterogenität!$D$4),Z1134)","v":1.8725711463653148E-3},{"$f":"IF(OR(AF1134>=$J$19, AR1133/$J$5<AN1134),0, Bodencharakterisierung!$E$8*$J$11*((AR1133/$J$5)-AN1134))","v":4.383176480179649E-6},4.383176480179649E-6,{"$f":"AQ1133-AP1134*Bodencharakterisierung!$E$8","v":5.8445923451657788E-3},{"$f":"AQ1134/(Bodencharakterisierung!$E$11*1000)","v":3.8578167294823621E-6},1.8769543228454944E-3,1117,null,{"$f":"(AP1134)*$G$11*Bodencharakterisierung!$E$8","v":6.3384672769969873E-8},{"$f":"IF(AF1134<=$J$9*1.05,(AV1134*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1133,NA())","v":{"$error":"#N/A"}},1853.8454349016615,1250,12.00652751231936,1.6399886323194495,0,7.0065388799999111,null,3.8578167294823622,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1872.5711463653147]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1129,5.0752555568535742E-4,{"$f":"Z1146*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.0231730514697112E-4},{"$f":"AF1145*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1146^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1146)*3600*24","v":0},0,{"$f":"AE1145-AD1146*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1146>$J$18,(AE1146/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.0231730514697112E-4,{"$error":"#N/A"},null,{"$f":"(AD1146)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1146>0,(AJ1146*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1145,NA())","v":{"$error":"#N/A"}},null,1129,{"$f":"IF(AF1146<=$J$9*0.05,AS1145*EXP((-$J$6*1)/Heterogenität!$D$4),Z1146)","v":1.8445088396455765E-3},{"$f":"IF(OR(AF1146>=$J$19, AR1145/$J$5<AN1146),0, Bodencharakterisierung!$E$8*$J$11*((AR1145/$J$5)-AN1146))","v":6.9367375709444081E-5},1.9124692816090659E-5,{"$f":"AQ1145-AP1146*Bodencharakterisierung!$E$8","v":5.7728935382367966E-3},{"$f":"AQ1146/(Bodencharakterisierung!$E$11*1000)","v":3.810490784314717E-6},1.8636335324616672E-3,1129,null,{"$f":"(AP1146)*$G$11*Bodencharakterisierung!$E$8","v":2.7656025292516083E-7},{"$f":"IF(AF1146<=$J$9*1.05,(AV1146*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1145,NA())","v":{"$error":"#N/A"}},1826.0637512491207,1262,12.081799192319357,1.6399886323194495,0,7.0818105599999077,null,3.8104907843147169,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1844.5088396455765]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1137,4.6732575191627354E-4,{"$f":"Z1154*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.625300336085857E-4},{"$f":"AF1153*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1154^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1154)*3600*24","v":0},0,{"$f":"AE1153-AD1154*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1154>$J$18,(AE1154/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.625300336085857E-4,{"$error":"#N/A"},null,{"$f":"(AD1154)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1154>0,(AJ1154*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1153,NA())","v":{"$error":"#N/A"}},null,1137,{"$f":"IF(AF1154<=$J$9*0.05,AS1153*EXP((-$J$6*1)/Heterogenität!$D$4),Z1154)","v":1.8355591851636759E-3},{"$f":"IF(OR(AF1154>=$J$19, AR1153/$J$5<AN1154),0, Bodencharakterisierung!$E$8*$J$11*((AR1153/$J$5)-AN1154))","v":8.4673730353530791E-6},8.4673730353530791E-6,{"$f":"AQ1153-AP1154*Bodencharakterisierung!$E$8","v":5.7290277608443331E-3},{"$f":"AQ1154/(Bodencharakterisierung!$E$11*1000)","v":3.7815364758048405E-6},1.844026558199029E-3,1137,null,{"$f":"(AP1154)*$G$11*Bodencharakterisierung!$E$8","v":1.2244582701473251E-7},{"$f":"IF(AF1154<=$J$9*1.05,(AV1154*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1153,NA())","v":{"$error":"#N/A"}},1817.2035933120392,1270,12.131980312319355,1.6399886323194495,0,7.1319916799999055,null,3.7815364758048404,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1835.5591851636759]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1147,4.2152366436221149E-4,{"$f":"Z1164*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.1719796917846373E-4},{"$f":"AF1163*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1164^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1164)*3600*24","v":0},0,{"$f":"AE1163-AD1164*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1164>$J$18,(AE1164/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.1719796917846373E-4,{"$error":"#N/A"},null,{"$f":"(AD1164)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1164>0,(AJ1164*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1163,NA())","v":{"$error":"#N/A"}},null,1147,{"$f":"IF(AF1164<=$J$9*0.05,AS1163*EXP((-$J$6*1)/Heterogenität!$D$4),Z1164)","v":1.8104696419106729E-3},{"$f":"IF(OR(AF1164>=$J$19, AR1163/$J$5<AN1164),0, Bodencharakterisierung!$E$8*$J$11*((AR1163/$J$5)-AN1164))","v":8.4686115740928948E-5},1.8771759186067419E-5,{"$f":"AQ1163-AP1164*Bodencharakterisierung!$E$8","v":5.6716596399721837E-3},{"$f":"AQ1164/(Bodencharakterisierung!$E$11*1000)","v":3.7436697293545765E-6},1.8292414010967404E-3,1147,null,{"$f":"(AP1164)*$G$11*Bodencharakterisierung!$E$8","v":2.714565153162148E-7},{"$f":"IF(AF1164<=$J$9*1.05,(AV1164*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1163,NA())","v":{"$error":"#N/A"}},1792.364945491566,1280,12.194706712319352,1.6399886323194495,0,7.1947180799999026,null,3.7436697293545764,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1810.4696419106729]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1154,3.9216021701847834E-4,{"$f":"Z1171*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.8813585087860576E-4},{"$f":"AF1170*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1171^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1171)*3600*24","v":0},0,{"$f":"AE1170-AD1171*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1171>$J$18,(AE1171/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.8813585087860576E-4,{"$error":"#N/A"},null,{"$f":"(AD1171)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1171>0,(AJ1171*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1170,NA())","v":{"$error":"#N/A"}},null,1154,{"$f":"IF(AF1171<=$J$9*0.05,AS1170*EXP((-$J$6*1)/Heterogenität!$D$4),Z1171)","v":1.7989157104212233E-3},{"$f":"IF(OR(AF1171>=$J$19, AR1170/$J$5<AN1171),0, Bodencharakterisierung!$E$8*$J$11*((AR1170/$J$5)-AN1171))","v":7.413565037810953E-5},1.8651962855573004E-5,{"$f":"AQ1170-AP1171*Bodencharakterisierung!$E$8","v":5.6322678048001387E-3},{"$f":"AQ1171/(Bodencharakterisierung!$E$11*1000)","v":3.7176685180198934E-6},1.8175676732767963E-3,1154,null,{"$f":"(AP1171)*$G$11*Bodencharakterisierung!$E$8","v":2.6972415266968032E-7},{"$f":"IF(AF1171<=$J$9*1.05,(AV1171*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1170,NA())","v":{"$error":"#N/A"}},1780.9265533170112,1287,12.238615192319349,1.6399886323194495,0,7.2386265599999007,null,3.7176685180198934,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1798.9157104212234]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1166,3.4650238744155659E-4,{"$f":"Z1183*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.4294656404364394E-4},{"$f":"AF1182*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1183^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1183)*3600*24","v":0},0,{"$f":"AE1182-AD1183*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1183>$J$18,(AE1183/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.4294656404364394E-4,{"$error":"#N/A"},null,{"$f":"(AD1183)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1183>0,(AJ1183*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1182,NA())","v":{"$error":"#N/A"}},null,1166,{"$f":"IF(AF1183<=$J$9*0.05,AS1182*EXP((-$J$6*1)/Heterogenität!$D$4),Z1183)","v":1.7809421339767353E-3},{"$f":"IF(OR(AF1183>=$J$19, AR1182/$J$5<AN1183),0, Bodencharakterisierung!$E$8*$J$11*((AR1182/$J$5)-AN1183))","v":3.8485419212448658E-5},1.8465604774267619E-5,{"$f":"AQ1182-AP1183*Bodencharakterisierung!$E$8","v":5.5648451191736619E-3},{"$f":"AQ1183/(Bodencharakterisierung!$E$11*1000)","v":3.6731650951641333E-6},1.7994077387510029E-3,1166,null,{"$f":"(AP1183)*$G$11*Bodencharakterisierung!$E$8","v":2.670292472614689E-7},{"$f":"IF(AF1183<=$J$9*1.05,(AV1183*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1182,NA())","v":{"$error":"#N/A"}},1763.1327126369679,1299,12.313886872319346,1.6399886323194495,0,7.3138982399998973,null,3.6731650951641335,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1780.9421339767352]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1176,3.1254206614059578E-4,{"$f":"Z1193*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.0933474511801799E-4},{"$f":"AF1192*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1193^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1193)*3600*24","v":0},0,{"$f":"AE1192-AD1193*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1193>$J$18,(AE1193/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.0933474511801799E-4,{"$error":"#N/A"},null,{"$f":"(AD1193)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1193>0,(AJ1193*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1192,NA())","v":{"$error":"#N/A"}},null,1176,{"$f":"IF(AF1193<=$J$9*0.05,AS1192*EXP((-$J$6*1)/Heterogenität!$D$4),Z1193)","v":1.7629867793788599E-3},{"$f":"IF(OR(AF1193>=$J$19, AR1192/$J$5<AN1193),0, Bodencharakterisierung!$E$8*$J$11*((AR1192/$J$5)-AN1193))","v":4.3251859262447852E-5},1.8279435625219659E-5,{"$f":"AQ1192-AP1193*Bodencharakterisierung!$E$8","v":5.510386812808553E-3},{"$f":"AQ1193/(Bodencharakterisierung!$E$11*1000)","v":3.6372190183554805E-6},1.7812662150040795E-3,1176,null,{"$f":"(AP1193)*$G$11*Bodencharakterisierung!$E$8","v":2.6433707398356679E-7},{"$f":"IF(AF1193<=$J$9*1.05,(AV1193*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1192,NA())","v":{"$error":"#N/A"}},1745.3569115850712,1309,12.376613272319343,1.6399886323194495,0,7.3766246399998945,null,3.6372190183554807,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1762.9867793788599]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1184,2.8778640686848384E-4,{"$f":"Z1201*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.848331295571788E-4},{"$f":"AF1200*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1201^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1201)*3600*24","v":0},0,{"$f":"AE1200-AD1201*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1201>$J$18,(AE1201/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.848331295571788E-4,{"$error":"#N/A"},null,{"$f":"(AD1201)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1201>0,(AJ1201*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1200,NA())","v":{"$error":"#N/A"}},null,1184,{"$f":"IF(AF1201<=$J$9*0.05,AS1200*EXP((-$J$6*1)/Heterogenität!$D$4),Z1201)","v":1.7503140022369177E-3},{"$f":"IF(OR(AF1201>=$J$19, AR1200/$J$5<AN1201),0, Bodencharakterisierung!$E$8*$J$11*((AR1200/$J$5)-AN1201))","v":2.990821516104711E-5},1.8148038602469043E-5,{"$f":"AQ1200-AP1201*Bodencharakterisierung!$E$8","v":5.4666146463373689E-3},{"$f":"AQ1201/(Bodencharakterisierung!$E$11*1000)","v":3.6083264992325867E-6},1.7684620408393867E-3,1184,null,{"$f":"(AP1201)*$G$11*Bodencharakterisierung!$E$8","v":2.6243695489695069E-7},{"$f":"IF(AF1201<=$J$9*1.05,(AV1201*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1200,NA())","v":{"$error":"#N/A"}},1732.8108622145485,1317,12.426794392319341,1.6399886323194495,0,7.4268057599998922,null,3.6083264992325867,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1750.3140022369178]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1187,2.7901718392796536E-4,{"$f":"Z1204*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.7615389678481948E-4},{"$f":"AF1203*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1204^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1204)*3600*24","v":0},0,{"$f":"AE1203-AD1204*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1204>$J$18,(AE1204/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.7615389678481948E-4,{"$error":"#N/A"},null,{"$f":"(AD1204)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1204>0,(AJ1204*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1203,NA())","v":{"$error":"#N/A"}},null,1187,{"$f":"IF(AF1204<=$J$9*0.05,AS1203*EXP((-$J$6*1)/Heterogenität!$D$4),Z1204)","v":1.7433934093771756E-3},{"$f":"IF(OR(AF1204>=$J$19, AR1203/$J$5<AN1204),0, Bodencharakterisierung!$E$8*$J$11*((AR1203/$J$5)-AN1204))","v":4.8586175401841799E-5},1.8076282799675937E-5,{"$f":"AQ1203-AP1204*Bodencharakterisierung!$E$8","v":5.4510029220094054E-3},{"$f":"AQ1204/(Bodencharakterisierung!$E$11*1000)","v":3.5980217306992773E-6},1.7614696921768515E-3,1187,null,{"$f":"(AP1204)*$G$11*Bodencharakterisierung!$E$8","v":2.6139930147369609E-7},{"$f":"IF(AF1204<=$J$9*1.05,(AV1204*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1203,NA())","v":{"$error":"#N/A"}},1725.9594752834039,1320,12.445612312319341,1.6399886323194495,0,7.4456236799998914,null,3.5980217306992772,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1743.3934093771757]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1199,2.4653219825126837E-4,{"$f":"Z1216*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.4400227352159082E-4},{"$f":"AF1215*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1216^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1216)*3600*24","v":0},0,{"$f":"AE1215-AD1216*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1216>$J$18,(AE1216/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.4400227352159082E-4,{"$error":"#N/A"},null,{"$f":"(AD1216)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1216>0,(AJ1216*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1215,NA())","v":{"$error":"#N/A"}},null,1199,{"$f":"IF(AF1216<=$J$9*0.05,AS1215*EXP((-$J$6*1)/Heterogenität!$D$4),Z1216)","v":1.7136212298811935E-3},{"$f":"IF(OR(AF1216>=$J$19, AR1215/$J$5<AN1216),0, Bodencharakterisierung!$E$8*$J$11*((AR1215/$J$5)-AN1216))","v":1.475729534419212E-4},1.7767591523663731E-5,{"$f":"AQ1215-AP1216*Bodencharakterisierung!$E$8","v":5.3897930036521735E-3},{"$f":"AQ1216/(Bodencharakterisierung!$E$11*1000)","v":3.5576191443248672E-6},1.7313888214048573E-3,1199,null,{"$f":"(AP1216)*$G$11*Bodencharakterisierung!$E$8","v":2.5693534808157164E-7},{"$f":"IF(AF1216<=$J$9*1.05,(AV1216*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1215,NA())","v":{"$error":"#N/A"}},1696.4850175823817,1332,12.520883992319337,1.6399886323194495,0,7.520895359999888,null,3.557619144324867,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1713.6212298811936]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1206,2.2935870163906996E-4,{"$f":"Z1223*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.2700501211956952E-4},{"$f":"AF1222*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1223^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1223)*3600*24","v":0},0,{"$f":"AE1222-AD1223*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1223>$J$18,(AE1223/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.2700501211956952E-4,{"$error":"#N/A"},null,{"$f":"(AD1223)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1223>0,(AJ1223*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1222,NA())","v":{"$error":"#N/A"}},null,1206,{"$f":"IF(AF1223<=$J$9*0.05,AS1222*EXP((-$J$6*1)/Heterogenität!$D$4),Z1223)","v":1.7136212298811935E-3},{"$f":"IF(OR(AF1223>=$J$19, AR1222/$J$5<AN1223),0, Bodencharakterisierung!$E$8*$J$11*((AR1222/$J$5)-AN1223))","v":1.9057111688952497E-5},1.7767591523663731E-5,{"$f":"AQ1222-AP1223*Bodencharakterisierung!$E$8","v":5.3487498672325088E-3},{"$f":"AQ1223/(Bodencharakterisierung!$E$11*1000)","v":3.5305279651699729E-6},1.7313888214048573E-3,1206,null,{"$f":"(AP1223)*$G$11*Bodencharakterisierung!$E$8","v":2.5693534808157164E-7},{"$f":"IF(AF1223<=$J$9*1.05,(AV1223*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1222,NA())","v":{"$error":"#N/A"}},1696.4850175823817,1339,12.564792472319334,1.6399886323194495,0,7.564803839999886,null,3.530527965169973,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1713.6212298811936]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1217,2.0475649832019677E-4,{"$f":"Z1234*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.0265527773993621E-4},{"$f":"AF1233*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1234^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1234)*3600*24","v":0},0,{"$f":"AE1233-AD1234*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1234>$J$18,(AE1234/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.0265527773993621E-4,{"$error":"#N/A"},null,{"$f":"(AD1234)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1234>0,(AJ1234*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1233,NA())","v":{"$error":"#N/A"}},null,1217,{"$f":"IF(AF1234<=$J$9*0.05,AS1233*EXP((-$J$6*1)/Heterogenität!$D$4),Z1234)","v":1.6967265160330359E-3},{"$f":"IF(OR(AF1234>=$J$19, AR1233/$J$5<AN1234),0, Bodencharakterisierung!$E$8*$J$11*((AR1233/$J$5)-AN1234))","v":1.4860900357250522E-6},1.4860900357250522E-6,{"$f":"AQ1233-AP1234*Bodencharakterisierung!$E$8","v":5.2957797285016874E-3},{"$f":"AQ1234/(Bodencharakterisierung!$E$11*1000)","v":3.4955641772288365E-6},1.6982126060687609E-3,1217,null,{"$f":"(AP1234)*$G$11*Bodencharakterisierung!$E$8","v":2.1490198044064281E-8},{"$f":"IF(AF1234<=$J$9*1.05,(AV1234*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1233,NA())","v":{"$error":"#N/A"}},1679.7592508727057,1350,12.633791512319332,1.6399886323194495,0,7.6338028799998829,null,3.4955641772288364,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1696.726516033036]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1224,1.904931077563258E-4,{"$f":"Z1241*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.8853825874445487E-4},{"$f":"AF1240*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1241^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1241)*3600*24","v":0},0,{"$f":"AE1240-AD1241*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1241>$J$18,(AE1241/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.8853825874445487E-4,{"$error":"#N/A"},null,{"$f":"(AD1241)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1241>0,(AJ1241*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1240,NA())","v":{"$error":"#N/A"}},null,1224,{"$f":"IF(AF1241<=$J$9*0.05,AS1240*EXP((-$J$6*1)/Heterogenität!$D$4),Z1241)","v":1.680785470389045E-3},{"$f":"IF(OR(AF1241>=$J$19, AR1240/$J$5<AN1241),0, Bodencharakterisierung!$E$8*$J$11*((AR1240/$J$5)-AN1241))","v":4.7699401298991716E-5},1.7427135679715924E-5,{"$f":"AQ1240-AP1241*Bodencharakterisierung!$E$8","v":5.2555230450815442E-3},{"$f":"AQ1241/(Bodencharakterisierung!$E$11*1000)","v":3.4689921089647158E-6},1.6982126060687609E-3,1224,null,{"$f":"(AP1241)*$G$11*Bodencharakterisierung!$E$8","v":2.5201205047791882E-7},{"$f":"IF(AF1241<=$J$9*1.05,(AV1241*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1240,NA())","v":{"$error":"#N/A"}},1663.9776156851547,1357,12.677699992319329,1.6399886323194495,0,7.677711359999881,null,3.468992108964716,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1680.785470389045]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1236,1.6831466774106359E-4,{"$f":"Z1253*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.6658741489820541E-4},{"$f":"AF1252*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1253^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1253)*3600*24","v":0},0,{"$f":"AE1252-AD1253*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1253>$J$18,(AE1253/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.6658741489820541E-4,{"$error":"#N/A"},null,{"$f":"(AD1253)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1253>0,(AJ1253*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1252,NA())","v":{"$error":"#N/A"}},null,1236,{"$f":"IF(AF1253<=$J$9*0.05,AS1252*EXP((-$J$6*1)/Heterogenität!$D$4),Z1253)","v":1.6592194958003476E-3},{"$f":"IF(OR(AF1253>=$J$19, AR1252/$J$5<AN1253),0, Bodencharakterisierung!$E$8*$J$11*((AR1252/$J$5)-AN1253))","v":6.6290253303813814E-5},1.7203530007342191E-5,{"$f":"AQ1252-AP1253*Bodencharakterisierung!$E$8","v":5.1942226819962226E-3},{"$f":"AQ1253/(Bodencharakterisierung!$E$11*1000)","v":3.4285298230998171E-6},1.6764230258076898E-3,1236,null,{"$f":"(AP1253)*$G$11*Bodencharakterisierung!$E$8","v":2.4877851141395276E-7},{"$f":"IF(AF1253<=$J$9*1.05,(AV1253*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1252,NA())","v":{"$error":"#N/A"}},1642.6273008423441,1369,12.752971672319326,1.6399886323194495,0,7.7529830399998776,null,3.4285298230998169,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1659.2194958003477]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1239,1.6318590275997402E-4,{"$f":"Z1256*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.6151128153866633E-4},{"$f":"AF1255*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1256^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1256)*3600*24","v":0},0,{"$f":"AE1255-AD1256*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1256>$J$18,(AE1256/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.6151128153866633E-4,{"$error":"#N/A"},null,{"$f":"(AD1256)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1256>0,(AJ1256*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1255,NA())","v":{"$error":"#N/A"}},null,1239,{"$f":"IF(AF1256<=$J$9*0.05,AS1255*EXP((-$J$6*1)/Heterogenität!$D$4),Z1256)","v":1.6592194958003476E-3},{"$f":"IF(OR(AF1256>=$J$19, AR1255/$J$5<AN1256),0, Bodencharakterisierung!$E$8*$J$11*((AR1255/$J$5)-AN1256))","v":1.2960584337108568E-5},1.2960584337108568E-5,{"$f":"AQ1255-AP1256*Bodencharakterisierung!$E$8","v":5.1785913593601299E-3},{"$f":"AQ1256/(Bodencharakterisierung!$E$11*1000)","v":3.4182121183895249E-6},1.6721800801374562E-3,1239,null,{"$f":"(AP1256)*$G$11*Bodencharakterisierung!$E$8","v":1.8742170223580717E-7},{"$f":"IF(AF1256<=$J$9*1.05,(AV1256*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1255,NA())","v":{"$error":"#N/A"}},1642.6273008423441,1372,12.771789592319326,1.6399886323194495,0,7.7718009599998767,null,3.4182121183895249,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1659.2194958003477]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1248,1.4871838519755514E-4,{"$f":"Z1265*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.471922303052618E-4},{"$f":"AF1264*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1265^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1265)*3600*24","v":0},0,{"$f":"AE1264-AD1265*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1265>$J$18,(AE1265/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.471922303052618E-4,{"$error":"#N/A"},null,{"$f":"(AD1265)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1265>0,(AJ1265*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1264,NA())","v":{"$error":"#N/A"}},null,1248,{"$f":"IF(AF1265<=$J$9*0.05,AS1264*EXP((-$J$6*1)/Heterogenität!$D$4),Z1265)","v":1.6431300509265625E-3},{"$f":"IF(OR(AF1265>=$J$19, AR1264/$J$5<AN1265),0, Bodencharakterisierung!$E$8*$J$11*((AR1264/$J$5)-AN1265))","v":2.8011081890896916E-5},1.7036707445054148E-5,{"$f":"AQ1264-AP1265*Bodencharakterisierung!$E$8","v":5.1318346859844871E-3},{"$f":"AQ1265/(Bodencharakterisierung!$E$11*1000)","v":3.3873496277125329E-6},1.6601667583716166E-3,1248,null,{"$f":"(AP1265)*$G$11*Bodencharakterisierung!$E$8","v":2.4636610717490597E-7},{"$f":"IF(AF1265<=$J$9*1.05,(AV1265*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1264,NA())","v":{"$error":"#N/A"}},1626.6987504172969,1381,12.828243352319323,1.6399886323194495,0,7.8282547199998742,null,3.387349627712533,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1643.1300509265625]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1257,1.3553350946190457E-4,{"$f":"Z1274*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.3414265836934999E-4},{"$f":"AF1273*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1274^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1274)*3600*24","v":0},0,{"$f":"AE1273-AD1274*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1274>$J$18,(AE1274/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.3414265836934999E-4,{"$error":"#N/A"},null,{"$f":"(AD1274)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1274>0,(AJ1274*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1273,NA())","v":{"$error":"#N/A"}},null,1257,{"$f":"IF(AF1274<=$J$9*0.05,AS1273*EXP((-$J$6*1)/Heterogenität!$D$4),Z1274)","v":1.6308400106015784E-3},{"$f":"IF(OR(AF1274>=$J$19, AR1273/$J$5<AN1274),0, Bodencharakterisierung!$E$8*$J$11*((AR1273/$J$5)-AN1274))","v":3.19345372314355E-6},3.19345372314355E-6,{"$f":"AQ1273-AP1274*Bodencharakterisierung!$E$8","v":5.090117664355809E-3},{"$f":"AQ1274/(Bodencharakterisierung!$E$11*1000)","v":3.3598136398388176E-6},1.6340334643247219E-3,1257,null,{"$f":"(AP1274)*$G$11*Bodencharakterisierung!$E$8","v":4.61802120363631E-8},{"$f":"IF(AF1274<=$J$9*1.05,(AV1274*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1273,NA())","v":{"$error":"#N/A"}},1614.5316104955625,1390,12.884697112319321,1.6399886323194495,0,7.8847084799998717,null,3.3598136398388174,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1630.8400106015783]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1269,1.1975382144555951E-4,{"$f":"Z1286*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.1852490223542161E-4},{"$f":"AF1285*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1286^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1286)*3600*24","v":0},0,{"$f":"AE1285-AD1286*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1286>$J$18,(AE1286/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.1852490223542161E-4,{"$error":"#N/A"},null,{"$f":"(AD1286)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1286>0,(AJ1286*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1285,NA())","v":{"$error":"#N/A"}},null,1269,{"$f":"IF(AF1286<=$J$9*0.05,AS1285*EXP((-$J$6*1)/Heterogenität!$D$4),Z1286)","v":1.6118284694419268E-3},{"$f":"IF(OR(AF1286>=$J$19, AR1285/$J$5<AN1286),0, Bodencharakterisierung!$E$8*$J$11*((AR1285/$J$5)-AN1286))","v":9.495027818572416E-7},9.495027818572416E-7,{"$f":"AQ1285-AP1286*Bodencharakterisierung!$E$8","v":5.0308030176878463E-3},{"$f":"AQ1286/(Bodencharakterisierung!$E$11*1000)","v":3.3206620578797667E-6},1.612777972223784E-3,1269,null,{"$f":"(AP1286)*$G$11*Bodencharakterisierung!$E$8","v":1.3730663913338631E-8},{"$f":"IF(AF1286<=$J$9*1.05,(AV1286*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1285,NA())","v":{"$error":"#N/A"}},1595.7101847475074,1402,12.959968792319318,1.6399886323194495,0,7.9599801599998683,null,3.3206620578797668,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1611.8284694419267]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1276,1.1141173930991478E-4,{"$f":"Z1293*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.1026842692939862E-4},{"$f":"AF1292*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1293^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1293)*3600*24","v":0},0,{"$f":"AE1292-AD1293*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1293>$J$18,(AE1293/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.1026842692939862E-4,{"$error":"#N/A"},null,{"$f":"(AD1293)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1293>0,(AJ1293*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1292,NA())","v":{"$error":"#N/A"}},null,1276,{"$f":"IF(AF1293<=$J$9*0.05,AS1292*EXP((-$J$6*1)/Heterogenität!$D$4),Z1293)","v":1.596227570676439E-3},{"$f":"IF(OR(AF1293>=$J$19, AR1292/$J$5<AN1293),0, Bodencharakterisierung!$E$8*$J$11*((AR1292/$J$5)-AN1293))","v":4.9828582535325456E-5},1.6550401547345012E-5,{"$f":"AQ1292-AP1293*Bodencharakterisierung!$E$8","v":4.9925715901134801E-3},{"$f":"AQ1293/(Bodencharakterisierung!$E$11*1000)","v":3.2954267921541122E-6},1.612777972223784E-3,1276,null,{"$f":"(AP1293)*$G$11*Bodencharakterisierung!$E$8","v":2.3933368666165835E-7},{"$f":"IF(AF1293<=$J$9*1.05,(AV1293*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1292,NA())","v":{"$error":"#N/A"}},1580.2652949696746,1409,13.003877272319315,1.6399886323194495,0,8.0038886399998663,null,3.2954267921541121,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1596.227570676439]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1288,9.8440463832369769E-5,{"$f":"Z1305*EXP((-$J$6/Heterogenität!$D$4)*1)","v":9.7430263275943426E-5},{"$f":"AF1304*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1305^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1305)*3600*24","v":0},0,{"$f":"AE1304-AD1305*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1305>$J$18,(AE1305/(Bodencharakterisierung!$E$11*1000)),0)","v":0},9.7430263275943426E-5,{"$error":"#N/A"},null,{"$f":"(AD1305)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1305>0,(AJ1305*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1304,NA())","v":{"$error":"#N/A"}},null,1288,{"$f":"IF(AF1305<=$J$9*0.05,AS1304*EXP((-$J$6*1)/Heterogenität!$D$4),Z1305)","v":1.5810554098594676E-3},{"$f":"IF(OR(AF1305>=$J$19, AR1304/$J$5<AN1305),0, Bodencharakterisierung!$E$8*$J$11*((AR1304/$J$5)-AN1305))","v":9.705328957810984E-6},9.705328957810984E-6,{"$f":"AQ1304-AP1305*Bodencharakterisierung!$E$8","v":4.9346614982372838E-3},{"$f":"AQ1305/(Bodencharakterisierung!$E$11*1000)","v":3.2572023090675142E-6},1.5907607388172785E-3,1288,null,{"$f":"(AP1305)*$G$11*Bodencharakterisierung!$E$8","v":1.4034778268625602E-7},{"$f":"IF(AF1305<=$J$9*1.05,(AV1305*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1304,NA())","v":{"$error":"#N/A"}},1565.244855760873,1421,13.079148952319322,1.6399886323194495,0,8.0791603199998736,null,3.2572023090675142,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1581.0554098594675]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1297,8.9713060819854158E-5,{"$f":"Z1314*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.8792421273567042E-5},{"$f":"AF1313*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1314^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1314)*3600*24","v":0},0,{"$f":"AE1313-AD1314*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1314>$J$18,(AE1314/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.8792421273567042E-5,{"$error":"#N/A"},null,{"$f":"(AD1314)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1314>0,(AJ1314*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1313,NA())","v":{"$error":"#N/A"}},null,1297,{"$f":"IF(AF1314<=$J$9*0.05,AS1313*EXP((-$J$6*1)/Heterogenität!$D$4),Z1314)","v":1.5631792426709611E-3},{"$f":"IF(OR(AF1314>=$J$19, AR1313/$J$5<AN1314),0, Bodencharakterisierung!$E$8*$J$11*((AR1313/$J$5)-AN1314))","v":5.1486073957934735E-5},1.6207741697955727E-5,{"$f":"AQ1313-AP1314*Bodencharakterisierung!$E$8","v":4.8900640981044199E-3},{"$f":"AQ1314/(Bodencharakterisierung!$E$11*1000)","v":3.2277650812570428E-6},1.5793869843689168E-3,1297,null,{"$f":"(AP1314)*$G$11*Bodencharakterisierung!$E$8","v":2.3437851715772434E-7},{"$f":"IF(AF1314<=$J$9*1.05,(AV1314*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1313,NA())","v":{"$error":"#N/A"}},1547.5474502442514,1430,13.135602712319328,1.6399886323194495,0,8.1356140799998791,null,3.2277650812570426,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1563.179242670961]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1306,8.1759400233751442E-5,{"$f":"Z1323*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.0920381517323367E-5},{"$f":"AF1322*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1323^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1323)*3600*24","v":0},0,{"$f":"AE1322-AD1323*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1323>$J$18,(AE1323/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.0920381517323367E-5,{"$error":"#N/A"},null,{"$f":"(AD1323)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1323>0,(AJ1323*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1322,NA())","v":{"$error":"#N/A"}},null,1306,{"$f":"IF(AF1323<=$J$9*0.05,AS1322*EXP((-$J$6*1)/Heterogenität!$D$4),Z1323)","v":1.5483683420212211E-3},{"$f":"IF(OR(AF1323>=$J$19, AR1322/$J$5<AN1323),0, Bodencharakterisierung!$E$8*$J$11*((AR1322/$J$5)-AN1323))","v":6.1763456475734488E-5},1.6054175654157173E-5,{"$f":"AQ1322-AP1323*Bodencharakterisierung!$E$8","v":4.8471694400370833E-3},{"$f":"AQ1323/(Bodencharakterisierung!$E$11*1000)","v":3.1994517756020351E-6},1.5644225176753783E-3,1306,null,{"$f":"(AP1323)*$G$11*Bodencharakterisierung!$E$8","v":2.3215781409482801E-7},{"$f":"IF(AF1323<=$J$9*1.05,(AV1323*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1322,NA())","v":{"$error":"#N/A"}},1532.8846586010088,1439,13.192056472319333,1.6399886323194495,0,8.1920678399998845,null,3.1994517756020353,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1548.368342021221]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1309,7.9268085873443624E-5,{"$f":"Z1326*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.8454633139285823E-5},{"$f":"AF1325*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1326^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1326)*3600*24","v":0},0,{"$f":"AE1325-AD1326*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1326>$J$18,(AE1326/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.8454633139285823E-5,{"$error":"#N/A"},null,{"$f":"(AD1326)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1326>0,(AJ1326*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1325,NA())","v":{"$error":"#N/A"}},null,1309,{"$f":"IF(AF1326<=$J$9*0.05,AS1325*EXP((-$J$6*1)/Heterogenität!$D$4),Z1326)","v":1.5483683420212211E-3},{"$f":"IF(OR(AF1326>=$J$19, AR1325/$J$5<AN1326),0, Bodencharakterisierung!$E$8*$J$11*((AR1325/$J$5)-AN1326))","v":1.199670088522394E-5},1.199670088522394E-5,{"$f":"AQ1325-AP1326*Bodencharakterisierung!$E$8","v":4.832614772813216E-3},{"$f":"AQ1326/(Bodencharakterisierung!$E$11*1000)","v":3.1898447345301755E-6},1.5603650429064451E-3,1309,null,{"$f":"(AP1326)*$G$11*Bodencharakterisierung!$E$8","v":1.7348308090436759E-7},{"$f":"IF(AF1326<=$J$9*1.05,(AV1326*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1325,NA())","v":{"$error":"#N/A"}},1532.8846586010088,1442,13.210874392319335,1.6399886323194495,0,8.2108857599998863,null,3.1898447345301757,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1548.368342021221]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1325,6.7208154065677951E-5,{"$f":"Z1342*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.6518460905057043E-5},{"$f":"AF1341*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1342^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1342)*3600*24","v":0},0,{"$f":"AE1341-AD1342*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1342>$J$18,(AE1342/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.6518460905057043E-5,{"$error":"#N/A"},null,{"$f":"(AD1342)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1342>0,(AJ1342*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1341,NA())","v":{"$error":"#N/A"}},null,1325,{"$f":"IF(AF1342<=$J$9*0.05,AS1341*EXP((-$J$6*1)/Heterogenität!$D$4),Z1342)","v":1.5188481490605219E-3},{"$f":"IF(OR(AF1342>=$J$19, AR1341/$J$5<AN1342),0, Bodencharakterisierung!$E$8*$J$11*((AR1341/$J$5)-AN1342))","v":6.8672558580099258E-5},1.5748097087272357E-5,{"$f":"AQ1341-AP1342*Bodencharakterisierung!$E$8","v":4.7573390019614399E-3},{"$f":"AQ1342/(Bodencharakterisierung!$E$11*1000)","v":3.1401577570702571E-6},1.5345962461477943E-3,1325,null,{"$f":"(AP1342)*$G$11*Bodencharakterisierung!$E$8","v":2.2773164282574409E-7},{"$f":"IF(AF1342<=$J$9*1.05,(AV1342*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1341,NA())","v":{"$error":"#N/A"}},1503.6596675699166,1458,13.311236632319345,1.6399886323194495,0,8.3112479999998961,null,3.140157757070257,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1518.8481490605218]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1328,6.5160234941089213E-5,{"$f":"Z1345*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.4491557620486071E-5},{"$f":"AF1344*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1345^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1345)*3600*24","v":0},0,{"$f":"AE1344-AD1345*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1345>$J$18,(AE1345/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.4491557620486071E-5,{"$error":"#N/A"},null,{"$f":"(AD1345)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1345>0,(AJ1345*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1344,NA())","v":{"$error":"#N/A"}},null,1328,{"$f":"IF(AF1345<=$J$9*0.05,AS1344*EXP((-$J$6*1)/Heterogenität!$D$4),Z1345)","v":1.5188481490605219E-3},{"$f":"IF(OR(AF1345>=$J$19, AR1344/$J$5<AN1345),0, Bodencharakterisierung!$E$8*$J$11*((AR1344/$J$5)-AN1345))","v":1.9854623879416759E-5},1.5748097087272357E-5,{"$f":"AQ1344-AP1345*Bodencharakterisierung!$E$8","v":4.7417483858450413E-3},{"$f":"AQ1345/(Bodencharakterisierung!$E$11*1000)","v":3.1298669213498624E-6},1.5345962461477943E-3,1328,null,{"$f":"(AP1345)*$G$11*Bodencharakterisierung!$E$8","v":2.2773164282574409E-7},{"$f":"IF(AF1345<=$J$9*1.05,(AV1345*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1344,NA())","v":{"$error":"#N/A"}},1503.6596675699166,1461,13.330054552319346,1.6399886323194495,0,8.3300659199998979,null,3.1298669213498624,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1518.8481490605218]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1338,5.8773951340031147E-5,{"$f":"Z1355*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.8170810354753197E-5},{"$f":"AF1354*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1355^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1355)*3600*24","v":0},0,{"$f":"AE1354-AD1355*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1355>$J$18,(AE1355/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.8170810354753197E-5,{"$error":"#N/A"},null,{"$f":"(AD1355)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1355>0,(AJ1355*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1354,NA())","v":{"$error":"#N/A"}},null,1338,{"$f":"IF(AF1355<=$J$9*0.05,AS1354*EXP((-$J$6*1)/Heterogenität!$D$4),Z1355)","v":1.4958538047709137E-3},{"$f":"IF(OR(AF1355>=$J$19, AR1354/$J$5<AN1355),0, Bodencharakterisierung!$E$8*$J$11*((AR1354/$J$5)-AN1355))","v":1.0689450211089241E-4},1.5509681438838439E-5,{"$f":"AQ1354-AP1355*Bodencharakterisierung!$E$8","v":4.6978547554528457E-3},{"$f":"AQ1355/(Bodencharakterisierung!$E$11*1000)","v":3.1008942280216803E-6},1.5113634862097521E-3,1338,null,{"$f":"(AP1355)*$G$11*Bodencharakterisierung!$E$8","v":2.2428393819245844E-7},{"$f":"IF(AF1355<=$J$9*1.05,(AV1355*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1354,NA())","v":{"$error":"#N/A"}},1480.8952667232045,1471,13.392780952319352,1.6399886323194495,0,8.3927923199999039,null,3.1008942280216805,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1495.8538047709137]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1346,5.4118616679272317E-5,{"$f":"Z1363*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.3563248951875975E-5},{"$f":"AF1362*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1363^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1363)*3600*24","v":0},0,{"$f":"AE1362-AD1363*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1363>$J$18,(AE1363/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.3563248951875975E-5,{"$error":"#N/A"},null,{"$f":"(AD1363)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1363>0,(AJ1363*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1362,NA())","v":{"$error":"#N/A"}},null,1346,{"$f":"IF(AF1363<=$J$9*0.05,AS1362*EXP((-$J$6*1)/Heterogenität!$D$4),Z1363)","v":1.4911298775396407E-3},{"$f":"IF(OR(AF1363>=$J$19, AR1362/$J$5<AN1363),0, Bodencharakterisierung!$E$8*$J$11*((AR1362/$J$5)-AN1363))","v":2.9834443276846025E-5},1.5460701647990053E-5,{"$f":"AQ1362-AP1363*Bodencharakterisierung!$E$8","v":4.6585165824335707E-3},{"$f":"AQ1363/(Bodencharakterisierung!$E$11*1000)","v":3.0749284372498816E-6},1.5065905791876307E-3,1346,null,{"$f":"(AP1363)*$G$11*Bodencharakterisierung!$E$8","v":2.2357564637959051E-7},{"$f":"IF(AF1363<=$J$9*1.05,(AV1363*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1362,NA())","v":{"$error":"#N/A"}},1476.2185787642441,1479,13.442962072319357,1.6399886323194495,0,8.4429734399999088,null,3.0749284372498815,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1491.1298775396406]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1358,4.7817777200788088E-5,{"$f":"Z1375*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.7327068977210793E-5},{"$f":"AF1374*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1375^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1375)*3600*24","v":0},0,{"$f":"AE1374-AD1375*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1375>$J$18,(AE1375/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.7327068977210793E-5,{"$error":"#N/A"},null,{"$f":"(AD1375)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1375>0,(AJ1375*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1374,NA())","v":{"$error":"#N/A"}},null,1358,{"$f":"IF(AF1375<=$J$9*0.05,AS1374*EXP((-$J$6*1)/Heterogenität!$D$4),Z1375)","v":1.4669536827976531E-3},{"$f":"IF(OR(AF1375>=$J$19, AR1374/$J$5<AN1375),0, Bodencharakterisierung!$E$8*$J$11*((AR1374/$J$5)-AN1375))","v":1.0086932689337721E-4},1.5210032045348673E-5,{"$f":"AQ1374-AP1375*Bodencharakterisierung!$E$8","v":4.6058268286225824E-3},{"$f":"AQ1375/(Bodencharakterisierung!$E$11*1000)","v":3.0401497218630907E-6},1.4821637148430017E-3,1358,null,{"$f":"(AP1375)*$G$11*Bodencharakterisierung!$E$8","v":2.1995073855106726E-7},{"$f":"IF(AF1375<=$J$9*1.05,(AV1375*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1374,NA())","v":{"$error":"#N/A"}},1452.2841459696765,1491,13.518233752319365,1.6399886323194495,0,8.5182451199999161,null,3.0401497218630906,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1466.9536827976531]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1365,4.4486778489116284E-5,{"$f":"Z1382*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.4030253127148789E-5},{"$f":"AF1381*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1382^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1382)*3600*24","v":0},0,{"$f":"AE1381-AD1382*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1382>$J$18,(AE1382/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.4030253127148789E-5,{"$error":"#N/A"},null,{"$f":"(AD1382)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1382>0,(AJ1382*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1381,NA())","v":{"$error":"#N/A"}},null,1365,{"$f":"IF(AF1382<=$J$9*0.05,AS1381*EXP((-$J$6*1)/Heterogenität!$D$4),Z1382)","v":1.458401702565274E-3},{"$f":"IF(OR(AF1382>=$J$19, AR1381/$J$5<AN1382),0, Bodencharakterisierung!$E$8*$J$11*((AR1381/$J$5)-AN1382))","v":8.3361145820684253E-5},1.5121361288452165E-5,{"$f":"AQ1381-AP1382*Bodencharakterisierung!$E$8","v":4.5735723307740632E-3},{"$f":"AQ1382/(Bodencharakterisierung!$E$11*1000)","v":3.0188596242733092E-6},1.4735230638537261E-3,1365,null,{"$f":"(AP1382)*$G$11*Bodencharakterisierung!$E$8","v":2.1866847968342515E-7},{"$f":"IF(AF1382<=$J$9*1.05,(AV1382*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1381,NA())","v":{"$error":"#N/A"}},1443.8176855396214,1498,13.562142232319369,1.6399886323194495,0,8.5621535999999203,null,3.0188596242733094,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1458.401702565274]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1377,3.9307339926671191E-5,{"$f":"Z1394*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.8903966200870996E-5},{"$f":"AF1393*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1394^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1394)*3600*24","v":0},0,{"$f":"AE1393-AD1394*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1394>$J$18,(AE1394/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.8903966200870996E-5,{"$error":"#N/A"},null,{"$f":"(AD1394)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1394>0,(AJ1394*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1393,NA())","v":{"$error":"#N/A"}},null,1377,{"$f":"IF(AF1394<=$J$9*0.05,AS1393*EXP((-$J$6*1)/Heterogenität!$D$4),Z1394)","v":1.4486177644465153E-3},{"$f":"IF(OR(AF1394>=$J$19, AR1393/$J$5<AN1394),0, Bodencharakterisierung!$E$8*$J$11*((AR1393/$J$5)-AN1394))","v":2.3244334465697136E-6},2.3244334465697136E-6,{"$f":"AQ1393-AP1394*Bodencharakterisierung!$E$8","v":4.5213777620502884E-3},{"$f":"AQ1394/(Bodencharakterisierung!$E$11*1000)","v":2.9844077637295631E-6},1.4509421978930852E-3,1377,null,{"$f":"(AP1394)*$G$11*Bodencharakterisierung!$E$8","v":3.3613397510372644E-8},{"$f":"IF(AF1394<=$J$9*1.05,(AV1394*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1393,NA())","v":{"$error":"#N/A"}},1434.1315868020502,1510,13.637413912319376,1.6399886323194495,0,8.6374252799999276,null,2.9844077637295632,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1448.6177644465154]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1379,3.8504731914752278E-5,{"$f":"Z1396*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.8109594589195111E-5},{"$f":"AF1395*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1396^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1396)*3600*24","v":0},0,{"$f":"AE1395-AD1396*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1396>$J$18,(AE1396/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.8109594589195111E-5,{"$error":"#N/A"},null,{"$f":"(AD1396)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1396>0,(AJ1396*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1395,NA())","v":{"$error":"#N/A"}},null,1379,{"$f":"IF(AF1396<=$J$9*0.05,AS1395*EXP((-$J$6*1)/Heterogenität!$D$4),Z1396)","v":1.436052562487161E-3},{"$f":"IF(OR(AF1396>=$J$19, AR1395/$J$5<AN1396),0, Bodencharakterisierung!$E$8*$J$11*((AR1395/$J$5)-AN1396))","v":1.0733885143714057E-4},1.4889635405924192E-5,{"$f":"AQ1395-AP1396*Bodencharakterisierung!$E$8","v":4.5115506026823784E-3},{"$f":"AQ1396/(Bodencharakterisierung!$E$11*1000)","v":2.9779211898893588E-6},1.4509421978930852E-3,1379,null,{"$f":"(AP1396)*$G$11*Bodencharakterisierung!$E$8","v":2.1531751507983564E-7},{"$f":"IF(AF1396<=$J$9*1.05,(AV1396*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1395,NA())","v":{"$error":"#N/A"}},1421.6920368622893,1512,13.649959192319377,1.6399886323194495,0,8.6499705599999288,null,2.9779211898893587,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1436.0525624871609]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1395,3.264658060390067E-5,{"$f":"Z1412*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.2311559895875183E-5},{"$f":"AF1411*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1412^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1412)*3600*24","v":0},0,{"$f":"AE1411-AD1412*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1412>$J$18,(AE1412/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.2311559895875183E-5,{"$error":"#N/A"},null,{"$f":"(AD1412)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1412>0,(AJ1412*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1411,NA())","v":{"$error":"#N/A"}},null,1395,{"$f":"IF(AF1412<=$J$9*0.05,AS1411*EXP((-$J$6*1)/Heterogenität!$D$4),Z1412)","v":1.4213157252029286E-3},{"$f":"IF(OR(AF1412>=$J$19, AR1411/$J$5<AN1412),0, Bodencharakterisierung!$E$8*$J$11*((AR1411/$J$5)-AN1412))","v":2.1843744097429561E-5},1.4736837284232401E-5,{"$f":"AQ1411-AP1412*Bodencharakterisierung!$E$8","v":4.4383007178444749E-3},{"$f":"AQ1412/(Bodencharakterisierung!$E$11*1000)","v":2.9295714309204455E-6},1.436052562487161E-3,1395,null,{"$f":"(AP1412)*$G$11*Bodencharakterisierung!$E$8","v":2.1310791686103352E-7},{"$f":"IF(AF1412<=$J$9*1.05,(AV1412*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1411,NA())","v":{"$error":"#N/A"}},1407.1025679508994,1528,13.750321432319387,1.6399886323194495,0,8.7503327999999385,null,2.9295714309204457,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1421.3157252029287]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1398,3.1651797192563114E-5,{"$f":"Z1415*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.1326984997546754E-5},{"$f":"AF1414*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1415^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1415)*3600*24","v":0},0,{"$f":"AE1414-AD1415*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1415>$J$18,(AE1415/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.1326984997546754E-5,{"$error":"#N/A"},null,{"$f":"(AD1415)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1415>0,(AJ1415*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1414,NA())","v":{"$error":"#N/A"}},null,1398,{"$f":"IF(AF1415<=$J$9*0.05,AS1414*EXP((-$J$6*1)/Heterogenität!$D$4),Z1415)","v":1.4132782665817905E-3},{"$f":"IF(OR(AF1415>=$J$19, AR1414/$J$5<AN1415),0, Bodencharakterisierung!$E$8*$J$11*((AR1414/$J$5)-AN1415))","v":6.3189494399961056E-5},1.4653501317579785E-5,{"$f":"AQ1414-AP1415*Bodencharakterisierung!$E$8","v":4.4264461128850473E-3},{"$f":"AQ1415/(Bodencharakterisierung!$E$11*1000)","v":2.9217466091650477E-6},1.4279317678993703E-3,1398,null,{"$f":"(AP1415)*$G$11*Bodencharakterisierung!$E$8","v":2.1190280385677032E-7},{"$f":"IF(AF1415<=$J$9*1.05,(AV1415*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1414,NA())","v":{"$error":"#N/A"}},1399.1454839159726,1531,13.769139352319389,1.6399886323194495,0,8.7691507199999403,null,2.9217466091650475,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1413.2782665817906]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1414,{"$f":"AG1430","v":2.6836258738096366E-5},{"$f":"Z1431*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.6560863819643009E-5},{"$f":"AF1430*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1431^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1431)*3600*24","v":0},{"$f":"MIN(AC1431,Z1431-AA1431)","v":0},{"$f":"AE1430-AD1431*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1431>$J$18,(AE1431/(Bodencharakterisierung!$E$11*1000)),0)","v":0},{"$f":"AA1431+AD1431","v":2.6560863819643009E-5},{"$f":"IF(AD1431>0,Y1431,NA())","v":{"$error":"#N/A"}},null,{"$f":"(AD1431)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1431>0,(AJ1431*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1430,NA())","v":{"$error":"#N/A"}},null,1414,{"$f":"IF(AF1431<=$J$9*0.05,AS1430*EXP((-$J$6*1)/Heterogenität!$D$4),Z1431)","v":1.3857390226778535E-3},{"$f":"IF(OR(AF1431>=$J$19, AR1430/$J$5<AN1431),0, Bodencharakterisierung!$E$8*$J$11*((AR1430/$J$5)-AN1431))","v":1.2033111698517286E-4},{"$f":"MIN(AO1431,AS1430-AN1431)","v":1.4367962116720433E-5},{"$f":"AQ1430-AP1431*Bodencharakterisierung!$E$8","v":4.3588341849049202E-3},{"$f":"AQ1431/(Bodencharakterisierung!$E$11*1000)","v":2.8771182738646339E-6},{"$f":"AN1431+AP1431","v":1.4001069847945739E-3},{"$f":"IF(AN1431>$G$5,AM1431,NA())","v":1414},null,{"$f":"(AP1431)*$G$11*Bodencharakterisierung!$E$8","v":2.0777365028713651E-7},{"$f":"IF(AF1431<=$J$9*1.05,(AV1431*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1430,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH1431>($G$5*10^6),BH1431*0.99,9999)","v":1371.8816324510749},{"$f":"AT1431+$G$3","v":1547},{"$f":"IF(ISNUMBER(AT1431),BA1431+BB1431+BC1431+$AZ$17,\"\")","v":13.869501592319398},{"$f":"IF(ISNUMBER(AK1431),AK1431,BA1430)","v":1.6399886323194495},{"$f":"IF(ISNUMBER(AW1431),AW1431,0)","v":0},8.86951295999995,null,{"$f":"AR1431*10^6","v":2.8771182738646339},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF1431*10^6","v":0},{"$f":"AN1431*10^6","v":1385.7390226778534}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1418,2.5751520046732841E-5,{"$f":"Z1435*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.54872567664995E-5},{"$f":"AF1434*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1435^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1435)*3600*24","v":0},0,{"$f":"AE1434-AD1435*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1435>$J$18,(AE1435/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.54872567664995E-5,{"$error":"#N/A"},null,{"$f":"(AD1435)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1435>0,(AJ1435*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1434,NA())","v":{"$error":"#N/A"}},null,1418,{"$f":"IF(AF1435<=$J$9*0.05,AS1434*EXP((-$J$6*1)/Heterogenität!$D$4),Z1435)","v":1.3857390226778535E-3},{"$f":"IF(OR(AF1435>=$J$19, AR1434/$J$5<AN1435),0, Bodencharakterisierung!$E$8*$J$11*((AR1434/$J$5)-AN1435))","v":6.0944958982813676E-5},1.4367962116720433E-5,{"$f":"AQ1434-AP1435*Bodencharakterisierung!$E$8","v":4.3398684749108504E-3},{"$f":"AQ1435/(Bodencharakterisierung!$E$11*1000)","v":2.8645996534065021E-6},1.4001069847945739E-3,1418,null,{"$f":"(AP1435)*$G$11*Bodencharakterisierung!$E$8","v":2.0777365028713651E-7},{"$f":"IF(AF1435<=$J$9*1.05,(AV1435*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1434,NA())","v":{"$error":"#N/A"}},1371.8816324510749,1551,13.894592152319401,1.6399886323194495,0,8.8946035199999525,null,2.8645996534065019,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1385.7390226778534]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1428,2.3227641636450074E-5,{"$f":"Z1445*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.2989278512261932E-5},{"$f":"AF1444*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1445^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1445)*3600*24","v":0},0,{"$f":"AE1444-AD1445*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1445>$J$18,(AE1445/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.2989278512261932E-5,{"$error":"#N/A"},null,{"$f":"(AD1445)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1445>0,(AJ1445*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1444,NA())","v":{"$error":"#N/A"}},null,1428,{"$f":"IF(AF1445<=$J$9*0.05,AS1444*EXP((-$J$6*1)/Heterogenität!$D$4),Z1445)","v":1.3730613097408691E-3},{"$f":"IF(OR(AF1445>=$J$19, AR1444/$J$5<AN1445),0, Bodencharakterisierung!$E$8*$J$11*((AR1444/$J$5)-AN1445))","v":5.0295966937531534E-5},1.4236513917438923E-5,{"$f":"AQ1444-AP1445*Bodencharakterisierung!$E$8","v":4.2969414905352204E-3},{"$f":"AQ1445/(Bodencharakterisierung!$E$11*1000)","v":2.836265010254271E-6},1.387297823658308E-3,1428,null,{"$f":"(AP1445)*$G$11*Bodencharakterisierung!$E$8","v":2.0587279114187142E-7},{"$f":"IF(AF1445<=$J$9*1.05,(AV1445*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1444,NA())","v":{"$error":"#N/A"}},1359.3306966434604,1561,13.957318552319407,1.6399886323194495,0,8.9573299199999585,null,2.8362650102542708,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1373.0613097408691]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1435,2.1609598120096192E-5,{"$f":"Z1452*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.1387839432710849E-5},{"$f":"AF1451*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1452^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1452)*3600*24","v":0},0,{"$f":"AE1451-AD1452*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1452>$J$18,(AE1452/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.1387839432710849E-5,{"$error":"#N/A"},null,{"$f":"(AD1452)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1452>0,(AJ1452*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1451,NA())","v":{"$error":"#N/A"}},null,1435,{"$f":"IF(AF1452<=$J$9*0.05,AS1451*EXP((-$J$6*1)/Heterogenität!$D$4),Z1452)","v":1.3650714662142493E-3},{"$f":"IF(OR(AF1452>=$J$19, AR1451/$J$5<AN1452),0, Bodencharakterisierung!$E$8*$J$11*((AR1451/$J$5)-AN1452))","v":3.4005462322591774E-5},1.4153671645387349E-5,{"$f":"AQ1451-AP1452*Bodencharakterisierung!$E$8","v":4.266828481498606E-3},{"$f":"AQ1452/(Bodencharakterisierung!$E$11*1000)","v":2.8163884366327432E-6},1.3792251378596367E-3,1435,null,{"$f":"(AP1452)*$G$11*Bodencharakterisierung!$E$8","v":2.0467481740541474E-7},{"$f":"IF(AF1452<=$J$9*1.05,(AV1452*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1451,NA())","v":{"$error":"#N/A"}},1351.4207515521068,1568,14.001227032319411,1.6399886323194495,0,9.0012383999999628,null,2.8163884366327432,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1365.0714662142493]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1447,1.9093668901945462E-5,{"$f":"Z1464*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.8897728795630939E-5},{"$f":"AF1463*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1464^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1464)*3600*24","v":0},0,{"$f":"AE1463-AD1464*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1464>$J$18,(AE1464/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.8897728795630939E-5,{"$error":"#N/A"},null,{"$f":"(AD1464)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1464>0,(AJ1464*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1463,NA())","v":{"$error":"#N/A"}},null,1447,{"$f":"IF(AF1464<=$J$9*0.05,AS1463*EXP((-$J$6*1)/Heterogenität!$D$4),Z1464)","v":1.3454183670795804E-3},{"$f":"IF(OR(AF1464>=$J$19, AR1463/$J$5<AN1464),0, Bodencharakterisierung!$E$8*$J$11*((AR1463/$J$5)-AN1464))","v":7.2214233610800663E-5},1.3949899521472362E-5,{"$f":"AQ1463-AP1464*Bodencharakterisierung!$E$8","v":4.2177572365935329E-3},{"$f":"AQ1464/(Bodencharakterisierung!$E$11*1000)","v":2.7839981759693286E-6},1.3593682666010528E-3,1447,null,{"$f":"(AP1464)*$G$11*Bodencharakterisierung!$E$8","v":2.0172808928429107E-7},{"$f":"IF(AF1464<=$J$9*1.05,(AV1464*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1463,NA())","v":{"$error":"#N/A"}},1331.9641834087845,1580,14.076498712319419,1.6399886323194495,0,9.0765100799999701,null,2.7839981759693284,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1345.4183670795803]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1454,1.7763598994128413E-5,{"$f":"Z1471*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.7581308126233272E-5},{"$f":"AF1470*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1471^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1471)*3600*24","v":0},0,{"$f":"AE1470-AD1471*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1471>$J$18,(AE1471/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.7581308126233272E-5,{"$error":"#N/A"},null,{"$f":"(AD1471)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1471>0,(AJ1471*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1470,NA())","v":{"$error":"#N/A"}},null,1454,{"$f":"IF(AF1471<=$J$9*0.05,AS1470*EXP((-$J$6*1)/Heterogenität!$D$4),Z1471)","v":1.3317516448303412E-3},{"$f":"IF(OR(AF1471>=$J$19, AR1470/$J$5<AN1471),0, Bodencharakterisierung!$E$8*$J$11*((AR1470/$J$5)-AN1471))","v":1.1929436854711153E-4},1.3808196831194275E-5,{"$f":"AQ1470-AP1471*Bodencharakterisierung!$E$8","v":4.1901832727045578E-3},{"$f":"AQ1471/(Bodencharakterisierung!$E$11*1000)","v":2.765797539738982E-6},1.3455598416615355E-3,1454,null,{"$f":"(AP1471)*$G$11*Bodencharakterisierung!$E$8","v":1.9967894097951355E-7},{"$f":"IF(AF1471<=$J$9*1.05,(AV1471*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1470,NA())","v":{"$error":"#N/A"}},1318.4341283820377,1587,14.120407192319423,1.6399886323194495,0,9.1204185599999743,null,2.765797539738982,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1331.7516448303411]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1459,1.687066044037548E-5,{"$f":"Z1476*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.6697532948888152E-5},{"$f":"AF1475*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1476^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1476)*3600*24","v":0},0,{"$f":"AE1475-AD1476*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1476>$J$18,(AE1476/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.6697532948888152E-5,{"$error":"#N/A"},null,{"$f":"(AD1476)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1476>0,(AJ1476*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1475,NA())","v":{"$error":"#N/A"}},null,1459,{"$f":"IF(AF1476<=$J$9*0.05,AS1475*EXP((-$J$6*1)/Heterogenität!$D$4),Z1476)","v":1.3317516448303412E-3},{"$f":"IF(OR(AF1476>=$J$19, AR1475/$J$5<AN1476),0, Bodencharakterisierung!$E$8*$J$11*((AR1475/$J$5)-AN1476))","v":4.7953722594378992E-5},1.3808196831194275E-5,{"$f":"AQ1475-AP1476*Bodencharakterisierung!$E$8","v":4.1673997479330883E-3},{"$f":"AQ1476/(Bodencharakterisierung!$E$11*1000)","v":2.7507589095267909E-6},1.3455598416615355E-3,1459,null,{"$f":"(AP1476)*$G$11*Bodencharakterisierung!$E$8","v":1.9967894097951355E-7},{"$f":"IF(AF1476<=$J$9*1.05,(AV1476*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1475,NA())","v":{"$error":"#N/A"}},1318.4341283820377,1592,14.151770392319426,1.6399886323194495,0,9.1517817599999773,null,2.750758909526791,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1331.7516448303411]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1468,1.5374963985702283E-5,{"$f":"Z1485*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.5217185399857342E-5},{"$f":"AF1484*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1485^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1485)*3600*24","v":0},0,{"$f":"AE1484-AD1485*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1485>$J$18,(AE1485/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.5217185399857342E-5,{"$error":"#N/A"},null,{"$f":"(AD1485)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1485>0,(AJ1485*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1484,NA())","v":{"$error":"#N/A"}},null,1468,{"$f":"IF(AF1485<=$J$9*0.05,AS1484*EXP((-$J$6*1)/Heterogenität!$D$4),Z1485)","v":1.3231816406590444E-3},{"$f":"IF(OR(AF1485>=$J$19, AR1484/$J$5<AN1485),0, Bodencharakterisierung!$E$8*$J$11*((AR1484/$J$5)-AN1485))","v":1.2703037537395128E-5},1.2703037537395128E-5,{"$f":"AQ1484-AP1485*Bodencharakterisierung!$E$8","v":4.1297581454094959E-3},{"$f":"AQ1485/(Bodencharakterisierung!$E$11*1000)","v":2.7259129672669938E-6},1.3358846781964394E-3,1468,null,{"$f":"(AP1485)*$G$11*Bodencharakterisierung!$E$8","v":1.8369734395440841E-7},{"$f":"IF(AF1485<=$J$9*1.05,(AV1485*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1484,NA())","v":{"$error":"#N/A"}},1309.9498242524539,1601,14.208224152319431,1.6399886323194495,0,9.2082355199999828,null,2.7259129672669937,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1323.1816406590444]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1484,1.3035800434932822E-5,{"$f":"Z1501*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.2902026452769792E-5},{"$f":"AF1500*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1501^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1501)*3600*24","v":0},0,{"$f":"AE1500-AD1501*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1501>$J$18,(AE1501/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.2902026452769792E-5,{"$error":"#N/A"},null,{"$f":"(AD1501)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1501>0,(AJ1501*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1500,NA())","v":{"$error":"#N/A"}},null,1484,{"$f":"IF(AF1501<=$J$9*0.05,AS1500*EXP((-$J$6*1)/Heterogenität!$D$4),Z1501)","v":1.2941699473643688E-3},{"$f":"IF(OR(AF1501>=$J$19, AR1500/$J$5<AN1501),0, Bodencharakterisierung!$E$8*$J$11*((AR1500/$J$5)-AN1501))","v":1.016452853870022E-4},1.3418532979172799E-5,{"$f":"AQ1500-AP1501*Bodencharakterisierung!$E$8","v":4.0673760167933993E-3},{"$f":"AQ1501/(Bodencharakterisierung!$E$11*1000)","v":2.6847366447481184E-6},1.3075884803435416E-3,1484,null,{"$f":"(AP1501)*$G$11*Bodencharakterisierung!$E$8","v":1.9404405133672759E-7},{"$f":"IF(AF1501<=$J$9*1.05,(AV1501*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1500,NA())","v":{"$error":"#N/A"}},1281.228247890725,1617,14.308586392319441,1.6399886323194495,0,9.3085977599999925,null,2.6847366447481185,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1294.1699473643687]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1487,1.263858278498915E-5,{"$f":"Z1504*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.2508885068574712E-5},{"$f":"AF1503*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1504^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1504)*3600*24","v":0},0,{"$f":"AE1503-AD1504*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1504>$J$18,(AE1504/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.2508885068574712E-5,{"$error":"#N/A"},null,{"$f":"(AD1504)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1504>0,(AJ1504*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1503,NA())","v":{"$error":"#N/A"}},null,1487,{"$f":"IF(AF1504<=$J$9*0.05,AS1503*EXP((-$J$6*1)/Heterogenität!$D$4),Z1504)","v":1.2941699473643688E-3},{"$f":"IF(OR(AF1504>=$J$19, AR1503/$J$5<AN1504),0, Bodencharakterisierung!$E$8*$J$11*((AR1503/$J$5)-AN1504))","v":6.0048826898970905E-5},1.3418532979172799E-5,{"$f":"AQ1503-AP1504*Bodencharakterisierung!$E$8","v":4.054091669144019E-3},{"$f":"AQ1504/(Bodencharakterisierung!$E$11*1000)","v":2.6759680984448968E-6},1.3075884803435416E-3,1487,null,{"$f":"(AP1504)*$G$11*Bodencharakterisierung!$E$8","v":1.9404405133672759E-7},{"$f":"IF(AF1504<=$J$9*1.05,(AV1504*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1503,NA())","v":{"$error":"#N/A"}},1281.228247890725,1620,14.327404312319443,1.6399886323194495,0,9.3274156799999943,null,2.6759680984448968,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1294.1699473643687]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1498,1.1282902877853907E-5,{"$f":"Z1515*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.1167117210846877E-5},{"$f":"AF1514*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1515^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1515)*3600*24","v":0},0,{"$f":"AE1514-AD1515*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1515>$J$18,(AE1515/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.1167117210846877E-5,{"$error":"#N/A"},null,{"$f":"(AD1515)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1515>0,(AJ1515*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1514,NA())","v":{"$error":"#N/A"}},null,1498,{"$f":"IF(AF1515<=$J$9*0.05,AS1514*EXP((-$J$6*1)/Heterogenität!$D$4),Z1515)","v":1.2854289274384669E-3},{"$f":"IF(OR(AF1515>=$J$19, AR1514/$J$5<AN1515),0, Bodencharakterisierung!$E$8*$J$11*((AR1514/$J$5)-AN1515))","v":2.6436779679214185E-6},2.6436779679214185E-6,{"$f":"AQ1514-AP1515*Bodencharakterisierung!$E$8","v":4.0120319903184515E-3},{"$f":"AQ1515/(Bodencharakterisierung!$E$11*1000)","v":2.6482059342035984E-6},1.2880726054063883E-3,1498,null,{"$f":"(AP1515)*$G$11*Bodencharakterisierung!$E$8","v":3.8229960318415023E-8},{"$f":"IF(AF1515<=$J$9*1.05,(AV1515*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1514,NA())","v":{"$error":"#N/A"}},1272.5746381640822,1631,14.396403352319449,1.6399886323194495,0,9.396414720000001,null,2.6482059342035984,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1285.4289274384669]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1505,1.0496932948883011E-5,{"$f":"Z1522*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.0389212941348419E-5},{"$f":"AF1521*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1522^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1522)*3600*24","v":0},0,{"$f":"AE1521-AD1522*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1522>$J$18,(AE1522/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.0389212941348419E-5,{"$error":"#N/A"},null,{"$f":"(AD1522)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1522>0,(AJ1522*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1521,NA())","v":{"$error":"#N/A"}},null,1505,{"$f":"IF(AF1522<=$J$9*0.05,AS1521*EXP((-$J$6*1)/Heterogenität!$D$4),Z1522)","v":1.2748543452312348E-3},{"$f":"IF(OR(AF1522>=$J$19, AR1521/$J$5<AN1522),0, Bodencharakterisierung!$E$8*$J$11*((AR1521/$J$5)-AN1522))","v":2.1307884875076117E-5},1.3218260175153511E-5,{"$f":"AQ1521-AP1522*Bodencharakterisierung!$E$8","v":3.9814978093138439E-3},{"$f":"AQ1522/(Bodencharakterisierung!$E$11*1000)","v":2.6280513592830654E-6},1.2880726054063883E-3,1505,null,{"$f":"(AP1522)*$G$11*Bodencharakterisierung!$E$8","v":1.9114792652749642E-7},{"$f":"IF(AF1522<=$J$9*1.05,(AV1522*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1521,NA())","v":{"$error":"#N/A"}},1262.1058017789226,1638,14.440311832319454,1.6399886323194495,0,9.4403232000000052,null,2.6280513592830652,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1274.8543452312349]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1517,9.2748121042337103E-6,{"$f":"Z1534*EXP((-$J$6/Heterogenität!$D$4)*1)","v":9.1796335568794289E-6},{"$f":"AF1533*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1534^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1534)*3600*24","v":0},0,{"$f":"AE1533-AD1534*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1534>$J$18,(AE1534/(Bodencharakterisierung!$E$11*1000)),0)","v":0},9.1796335568794289E-6,{"$error":"#N/A"},null,{"$f":"(AD1534)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1534>0,(AJ1534*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1533,NA())","v":{"$error":"#N/A"}},null,1517,{"$f":"IF(AF1534<=$J$9*0.05,AS1533*EXP((-$J$6*1)/Heterogenität!$D$4),Z1534)","v":1.2588754321372576E-3},{"$f":"IF(OR(AF1534>=$J$19, AR1533/$J$5<AN1534),0, Bodencharakterisierung!$E$8*$J$11*((AR1533/$J$5)-AN1534))","v":3.1407278033776123E-5},1.305258365580657E-5,{"$f":"AQ1533-AP1534*Bodencharakterisierung!$E$8","v":3.9349047229104645E-3},{"$f":"AQ1534/(Bodencharakterisierung!$E$11*1000)","v":2.5972968468055871E-6},1.2719280157930642E-3,1517,null,{"$f":"(AP1534)*$G$11*Bodencharakterisierung!$E$8","v":1.887520950997728E-7},{"$f":"IF(AF1534<=$J$9*1.05,(AV1534*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1533,NA())","v":{"$error":"#N/A"}},1246.286677815885,1650,14.515583512319461,1.6399886323194495,0,9.5155948800000125,null,2.597296846805587,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1258.8754321372576]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1524,8.6287262972654289E-6,{"$f":"Z1541*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.5401779121055271E-6},{"$f":"AF1540*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1541^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1541)*3600*24","v":0},0,{"$f":"AE1540-AD1541*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1541>$J$18,(AE1541/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.5401779121055271E-6,{"$error":"#N/A"},null,{"$f":"(AD1541)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1541>0,(AJ1541*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1540,NA())","v":{"$error":"#N/A"}},null,1524,{"$f":"IF(AF1541<=$J$9*0.05,AS1540*EXP((-$J$6*1)/Heterogenität!$D$4),Z1541)","v":1.2503438902337093E-3},{"$f":"IF(OR(AF1541>=$J$19, AR1540/$J$5<AN1541),0, Bodencharakterisierung!$E$8*$J$11*((AR1540/$J$5)-AN1541))","v":2.9648803300251304E-5},1.2964124812646837E-5,{"$f":"AQ1540-AP1541*Bodencharakterisierung!$E$8","v":3.9077438120031765E-3},{"$f":"AQ1541/(Bodencharakterisierung!$E$11*1000)","v":2.5793688528073773E-6},1.2633080150463562E-3,1524,null,{"$f":"(AP1541)*$G$11*Bodencharakterisierung!$E$8","v":1.8747290069529381E-7},{"$f":"IF(AF1541<=$J$9*1.05,(AV1541*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1540,NA())","v":{"$error":"#N/A"}},1237.8404513313722,1657,14.559491992319465,1.6399886323194495,0,9.5595033600000168,null,2.5793688528073773,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1250.3438902337093]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1536,7.624114157508567E-6,{"$f":"Z1553*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.5458751482197823E-6},{"$f":"AF1552*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1553^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1553)*3600*24","v":0},0,{"$f":"AE1552-AD1553*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1553>$J$18,(AE1553/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.5458751482197823E-6,{"$error":"#N/A"},null,{"$f":"(AD1553)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1553>0,(AJ1553*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1552,NA())","v":{"$error":"#N/A"}},null,1536,{"$f":"IF(AF1553<=$J$9*0.05,AS1552*EXP((-$J$6*1)/Heterogenität!$D$4),Z1553)","v":1.232213507054681E-3},{"$f":"IF(OR(AF1553>=$J$19, AR1552/$J$5<AN1553),0, Bodencharakterisierung!$E$8*$J$11*((AR1552/$J$5)-AN1553))","v":6.6069002274153651E-5},1.277614088896796E-5,{"$f":"AQ1552-AP1553*Bodencharakterisierung!$E$8","v":3.8628488306951918E-3},{"$f":"AQ1553/(Bodencharakterisierung!$E$11*1000)","v":2.5497352017790044E-6},1.244989647943649E-3,1536,null,{"$f":"(AP1553)*$G$11*Bodencharakterisierung!$E$8","v":1.8475448414458439E-7},{"$f":"IF(AF1553<=$J$9*1.05,(AV1553*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1552,NA())","v":{"$error":"#N/A"}},1219.8913719841341,1669,14.634763672319473,1.6399886323194495,0,9.634775040000024,null,2.5497352017790043,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1232.213507054681]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1539,7.3917975672336526E-6,{"$f":"Z1556*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.3159426014532613E-6},{"$f":"AF1555*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1556^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1556)*3600*24","v":0},0,{"$f":"AE1555-AD1556*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1556>$J$18,(AE1556/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.3159426014532613E-6,{"$error":"#N/A"},null,{"$f":"(AD1556)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1556>0,(AJ1556*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1555,NA())","v":{"$error":"#N/A"}},null,1539,{"$f":"IF(AF1556<=$J$9*0.05,AS1555*EXP((-$J$6*1)/Heterogenität!$D$4),Z1556)","v":1.232213507054681E-3},{"$f":"IF(OR(AF1556>=$J$19, AR1555/$J$5<AN1556),0, Bodencharakterisierung!$E$8*$J$11*((AR1555/$J$5)-AN1556))","v":2.6463911691596346E-5},1.277614088896796E-5,{"$f":"AQ1555-AP1556*Bodencharakterisierung!$E$8","v":3.8502004512151141E-3},{"$f":"AQ1556/(Bodencharakterisierung!$E$11*1000)","v":2.5413864364456201E-6},1.244989647943649E-3,1539,null,{"$f":"(AP1556)*$G$11*Bodencharakterisierung!$E$8","v":1.8475448414458439E-7},{"$f":"IF(AF1556<=$J$9*1.05,(AV1556*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1555,NA())","v":{"$error":"#N/A"}},1219.8913719841341,1672,14.653581592319474,1.6399886323194495,0,{"$f":"$G$34/$G$12/$G$8+BC1555","v":9.6535929600000259},null,2.5413864364456202,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1232.213507054681]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1554,6.332182687527957E-6,{"$f":"Z1571*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.2672015382596361E-6},{"$f":"AF1570*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1571^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1571)*3600*24","v":0},0,{"$f":"AE1570-AD1571*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1571>$J$18,(AE1571/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.2672015382596361E-6,{"$error":"#N/A"},null,{"$f":"(AD1571)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1571>0,(AJ1571*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1570,NA())","v":{"$error":"#N/A"}},null,1554,{"$f":"IF(AF1571<=$J$9*0.05,AS1570*EXP((-$J$6*1)/Heterogenität!$D$4),Z1571)","v":1.2124500421543218E-3},{"$f":"IF(OR(AF1571>=$J$19, AR1570/$J$5<AN1571),0, Bodencharakterisierung!$E$8*$J$11*((AR1570/$J$5)-AN1571))","v":4.3995507697580857E-5},1.2571224443420513E-5,{"$f":"AQ1570-AP1571*Bodencharakterisierung!$E$8","v":3.7941815983491218E-3},{"$f":"AQ1571/(Bodencharakterisierung!$E$11*1000)","v":2.5044102959400142E-6},1.2250212665977423E-3,1554,null,{"$f":"(AP1571)*$G$11*Bodencharakterisierung!$E$8","v":1.8179120810380813E-7},{"$f":"IF(AF1571<=$J$9*1.05,(AV1571*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1570,NA())","v":{"$error":"#N/A"}},1200.3255417327787,1687,14.747671192319483,1.6399886323194495,0,9.747682560000035,null,2.5044102959400143,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1212.4500421543219]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1557,6.1392329151907261E-6,{"$f":"Z1574*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.07623182533892E-6},{"$f":"AF1573*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1574^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1574)*3600*24","v":0},0,{"$f":"AE1573-AD1574*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1574>$J$18,(AE1574/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.07623182533892E-6,{"$error":"#N/A"},null,{"$f":"(AD1574)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1574>0,(AJ1574*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1573,NA())","v":{"$error":"#N/A"}},null,1557,{"$f":"IF(AF1574<=$J$9*0.05,AS1573*EXP((-$J$6*1)/Heterogenität!$D$4),Z1574)","v":1.2124500421543218E-3},{"$f":"IF(OR(AF1574>=$J$19, AR1573/$J$5<AN1574),0, Bodencharakterisierung!$E$8*$J$11*((AR1573/$J$5)-AN1574))","v":5.025642920548489E-6},5.025642920548489E-6,{"$f":"AQ1573-AP1574*Bodencharakterisierung!$E$8","v":3.7842261280526829E-3},{"$f":"AQ1574/(Bodencharakterisierung!$E$11*1000)","v":2.4978390284176124E-6},1.2174756850748703E-3,1557,null,{"$f":"(AP1574)*$G$11*Bodencharakterisierung!$E$8","v":7.2675315132331982E-8},{"$f":"IF(AF1574<=$J$9*1.05,(AV1574*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1573,NA())","v":{"$error":"#N/A"}},1200.3255417327787,1690,14.766489112319485,1.6399886323194495,0,9.7665004800000368,null,2.4978390284176122,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1212.4500421543219]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1569,5.4244637009499063E-6,{"$f":"Z1586*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.3687976055691958E-6},{"$f":"AF1585*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1586^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1586)*3600*24","v":0},0,{"$f":"AE1585-AD1586*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1586>$J$18,(AE1586/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.3687976055691958E-6,{"$error":"#N/A"},null,{"$f":"(AD1586)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1586>0,(AJ1586*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1585,NA())","v":{"$error":"#N/A"}},null,1569,{"$f":"IF(AF1586<=$J$9*0.05,AS1585*EXP((-$J$6*1)/Heterogenität!$D$4),Z1586)","v":1.1904404052105002E-3},{"$f":"IF(OR(AF1586>=$J$19, AR1585/$J$5<AN1586),0, Bodencharakterisierung!$E$8*$J$11*((AR1585/$J$5)-AN1586))","v":8.8443746709176039E-5},1.2343018681270235E-5,{"$f":"AQ1585-AP1586*Bodencharakterisierung!$E$8","v":3.7397558804145121E-3},{"$f":"AQ1586/(Bodencharakterisierung!$E$11*1000)","v":2.4684857296465428E-6},1.2027834238917704E-3,1569,null,{"$f":"(AP1586)*$G$11*Bodencharakterisierung!$E$8","v":1.7849114760578228E-7},{"$f":"IF(AF1586<=$J$9*1.05,(AV1586*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1585,NA())","v":{"$error":"#N/A"}},1178.536001158395,1702,14.841760792319493,1.6399886323194495,0,9.8417721600000441,null,2.4684857296465426,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1190.4404052105001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1576,5.0465941583422922E-6,{"$f":"Z1593*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.9948057775449752E-6},{"$f":"AF1592*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1593^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1593)*3600*24","v":0},0,{"$f":"AE1592-AD1593*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1593>$J$18,(AE1593/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.9948057775449752E-6,{"$error":"#N/A"},null,{"$f":"(AD1593)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1593>0,(AJ1593*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1592,NA())","v":{"$error":"#N/A"}},null,1576,{"$f":"IF(AF1593<=$J$9*0.05,AS1592*EXP((-$J$6*1)/Heterogenität!$D$4),Z1593)","v":1.1900205983541258E-3},{"$f":"IF(OR(AF1593>=$J$19, AR1592/$J$5<AN1593),0, Bodencharakterisierung!$E$8*$J$11*((AR1592/$J$5)-AN1593))","v":3.7058430128331746E-6},3.7058430128331746E-6,{"$f":"AQ1592-AP1593*Bodencharakterisierung!$E$8","v":3.714233747899913E-3},{"$f":"AQ1593/(Bodencharakterisierung!$E$11*1000)","v":2.4516394375576981E-6},1.193726441366959E-3,1576,null,{"$f":"(AP1593)*$G$11*Bodencharakterisierung!$E$8","v":5.3589821848944282E-8},{"$f":"IF(AF1593<=$J$9*1.05,(AV1593*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1592,NA())","v":{"$error":"#N/A"}},1178.1203923705843,1709,14.885669272319497,1.6399886323194495,0,9.8856806400000483,null,2.4516394375576982,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1190.0205983541257]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1588,4.4590370170868733E-6,{"$f":"Z1605*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.4132781746310171E-6},{"$f":"AF1604*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1605^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1605)*3600*24","v":0},0,{"$f":"AE1604-AD1605*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1605>$J$18,(AE1605/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.4132781746310171E-6,{"$error":"#N/A"},null,{"$f":"(AD1605)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1605>0,(AJ1605*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1604,NA())","v":{"$error":"#N/A"}},null,1588,{"$f":"IF(AF1605<=$J$9*0.05,AS1604*EXP((-$J$6*1)/Heterogenität!$D$4),Z1605)","v":1.1730794357187814E-3},{"$f":"IF(OR(AF1605>=$J$19, AR1604/$J$5<AN1605),0, Bodencharakterisierung!$E$8*$J$11*((AR1604/$J$5)-AN1605))","v":3.5177177843840537E-5},1.2163012382909299E-5,{"$f":"AQ1604-AP1605*Bodencharakterisierung!$E$8","v":3.6686171605888758E-3},{"$f":"AQ1605/(Bodencharakterisierung!$E$11*1000)","v":2.4215294789365516E-6},1.1852424481016907E-3,1588,null,{"$f":"(AP1605)*$G$11*Bodencharakterisierung!$E$8","v":1.7588809468976692E-7},{"$f":"IF(AF1605<=$J$9*1.05,(AV1605*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1604,NA())","v":{"$error":"#N/A"}},1161.3486413615938,1721,14.960940952319504,1.6399886323194495,0,9.9609523200000556,null,2.4215294789365518,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1173.0794357187815]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1594,4.1914320142967848E-6,{"$f":"Z1611*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.1484193466576318E-6},{"$f":"AF1610*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1611^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1611)*3600*24","v":0},0,{"$f":"AE1610-AD1611*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1611>$J$18,(AE1611/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.1484193466576318E-6,{"$error":"#N/A"},null,{"$f":"(AD1611)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1611>0,(AJ1611*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1610,NA())","v":{"$error":"#N/A"}},null,1594,{"$f":"IF(AF1611<=$J$9*0.05,AS1610*EXP((-$J$6*1)/Heterogenität!$D$4),Z1611)","v":1.1665309492736654E-3},{"$f":"IF(OR(AF1611>=$J$19, AR1610/$J$5<AN1611),0, Bodencharakterisierung!$E$8*$J$11*((AR1610/$J$5)-AN1611))","v":3.0719710316243638E-5},1.2095114745890034E-5,{"$f":"AQ1610-AP1611*Bodencharakterisierung!$E$8","v":3.6467769883140803E-3},{"$f":"AQ1611/(Bodencharakterisierung!$E$11*1000)","v":2.4071135236396571E-6},1.1786260640195554E-3,1594,null,{"$f":"(AP1611)*$G$11*Bodencharakterisierung!$E$8","v":1.7490623381243717E-7},{"$f":"IF(AF1611<=$J$9*1.05,(AV1611*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1610,NA())","v":{"$error":"#N/A"}},1154.8656397809286,1727,14.998576792319508,1.6399886323194495,0,9.9985881600000592,null,2.4071135236396572,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1166.5309492736653]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1606,{"$f":"AG1622","v":3.703438382390467E-6},{"$f":"Z1623*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.6654335277917292E-6},{"$f":"AF1622*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1623^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1623)*3600*24","v":0},{"$f":"MIN(AC1623,Z1623-AA1623)","v":0},{"$f":"AE1622-AD1623*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1623>$J$18,(AE1623/(Bodencharakterisierung!$E$11*1000)),0)","v":0},{"$f":"AA1623+AD1623","v":3.6654335277917292E-6},{"$f":"IF(AD1623>0,Y1623,NA())","v":{"$error":"#N/A"}},null,{"$f":"(AD1623)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1623>0,(AJ1623*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1622,NA())","v":{"$error":"#N/A"}},null,1606,{"$f":"IF(AF1623<=$J$9*0.05,AS1622*EXP((-$J$6*1)/Heterogenität!$D$4),Z1623)","v":1.1506182303713476E-3},{"$f":"IF(OR(AF1623>=$J$19, AR1622/$J$5<AN1623),0, Bodencharakterisierung!$E$8*$J$11*((AR1622/$J$5)-AN1623))","v":5.379496363409758E-5},{"$f":"MIN(AO1623,AS1622-AN1623)","v":1.1930124557534916E-5},{"$f":"AQ1622-AP1623*Bodencharakterisierung!$E$8","v":3.6045342823956984E-3},{"$f":"AQ1623/(Bodencharakterisierung!$E$11*1000)","v":2.3792305494361044E-6},{"$f":"AN1623+AP1623","v":1.1625483549288825E-3},{"$f":"IF(AN1623>$G$5,AM1623,NA())","v":1606},null,{"$f":"(AP1623)*$G$11*Bodencharakterisierung!$E$8","v":1.7252032734792808E-7},{"$f":"IF(AF1623<=$J$9*1.05,(AV1623*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1622,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH1623>($G$5*10^6),BH1623*0.99,9999)","v":1139.1120480676341},{"$f":"AT1623+$G$3","v":1739},{"$f":"IF(ISNUMBER(AT1623),BA1623+BB1623+BC1623+$AZ$17,\"\")","v":15.073848472319515},{"$f":"IF(ISNUMBER(AK1623),AK1623,BA1622)","v":1.6399886323194495},{"$f":"IF(ISNUMBER(AW1623),AW1623,0)","v":0},10.073859840000067,null,{"$f":"AR1623*10^6","v":2.3792305494361043},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF1623*10^6","v":0},{"$f":"AN1623*10^6","v":1150.6182303713476}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1609,3.5905898390035779E-6,{"$f":"Z1626*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.5537430413347166E-6},{"$f":"AF1625*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1626^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1626)*3600*24","v":0},0,{"$f":"AE1625-AD1626*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1626>$J$18,(AE1626/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.5537430413347166E-6,{"$error":"#N/A"},null,{"$f":"(AD1626)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1626>0,(AJ1626*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1625,NA())","v":{"$error":"#N/A"}},null,1609,{"$f":"IF(AF1626<=$J$9*0.05,AS1625*EXP((-$J$6*1)/Heterogenität!$D$4),Z1626)","v":1.1506182303713476E-3},{"$f":"IF(OR(AF1626>=$J$19, AR1625/$J$5<AN1626),0, Bodencharakterisierung!$E$8*$J$11*((AR1625/$J$5)-AN1626))","v":1.6812461024847534E-5},1.1930124557534916E-5,{"$f":"AQ1625-AP1626*Bodencharakterisierung!$E$8","v":3.5927234590837393E-3},{"$f":"AQ1626/(Bodencharakterisierung!$E$11*1000)","v":2.3714346264579135E-6},1.1625483549288825E-3,1609,null,{"$f":"(AP1626)*$G$11*Bodencharakterisierung!$E$8","v":1.7252032734792808E-7},{"$f":"IF(AF1626<=$J$9*1.05,(AV1626*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1625,NA())","v":{"$error":"#N/A"}},1139.1120480676341,1742,15.092666392319517,1.6399886323194495,0,10.092677760000068,null,2.3714346264579134,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1150.6182303713476]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1619,3.2386800426732614E-6,{"$f":"Z1636*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.2054445594804284E-6},{"$f":"AF1635*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1636^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1636)*3600*24","v":0},0,{"$f":"AE1635-AD1636*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1636>$J$18,(AE1636/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.2054445594804284E-6,{"$error":"#N/A"},null,{"$f":"(AD1636)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1636>0,(AJ1636*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1635,NA())","v":{"$error":"#N/A"}},null,1619,{"$f":"IF(AF1636<=$J$9*0.05,AS1635*EXP((-$J$6*1)/Heterogenität!$D$4),Z1636)","v":1.132511750591512E-3},{"$f":"IF(OR(AF1636>=$J$19, AR1635/$J$5<AN1636),0, Bodencharakterisierung!$E$8*$J$11*((AR1635/$J$5)-AN1636))","v":9.0059584149573452E-5},1.1742388474992324E-5,{"$f":"AQ1635-AP1636*Bodencharakterisierung!$E$8","v":3.5596641402851148E-3},{"$f":"AQ1636/(Bodencharakterisierung!$E$11*1000)","v":2.3496132939175677E-6},1.1442541390665043E-3,1619,null,{"$f":"(AP1636)*$G$11*Bodencharakterisierung!$E$8","v":1.6980549480288064E-7},{"$f":"IF(AF1636<=$J$9*1.05,(AV1636*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1635,NA())","v":{"$error":"#N/A"}},1121.1866330855969,1752,15.155392792319523,1.6399886323194495,0,10.155404160000074,null,2.3496132939175678,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1132.5117505915121]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1627,2.9821524634649593E-6,{"$f":"Z1644*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.9515494780597863E-6},{"$f":"AF1643*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1644^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1644)*3600*24","v":0},0,{"$f":"AE1643-AD1644*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1644>$J$18,(AE1644/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.9515494780597863E-6,{"$error":"#N/A"},null,{"$f":"(AD1644)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1644>0,(AJ1644*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1643,NA())","v":{"$error":"#N/A"}},null,1627,{"$f":"IF(AF1644<=$J$9*0.05,AS1643*EXP((-$J$6*1)/Heterogenität!$D$4),Z1644)","v":1.1259622733109157E-3},{"$f":"IF(OR(AF1644>=$J$19, AR1643/$J$5<AN1644),0, Bodencharakterisierung!$E$8*$J$11*((AR1643/$J$5)-AN1644))","v":6.3838452825696991E-5},1.1674480564547503E-5,{"$f":"AQ1643-AP1644*Bodencharakterisierung!$E$8","v":3.5308703814346245E-3},{"$f":"AQ1644/(Bodencharakterisierung!$E$11*1000)","v":2.3306075124981019E-6},1.1376367538754632E-3,1627,null,{"$f":"(AP1644)*$G$11*Bodencharakterisierung!$E$8","v":1.6882348536258062E-7},{"$f":"IF(AF1644<=$J$9*1.05,(AV1644*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1643,NA())","v":{"$error":"#N/A"}},1114.7026505778065,1760,15.205573912319528,1.6399886323194495,0,10.205585280000079,null,2.3306075124981018,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1125.9622733109156]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1634,2.7744149525367649E-6,{"$f":"Z1651*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.7459437790000084E-6},{"$f":"AF1650*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1651^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1651)*3600*24","v":0},0,{"$f":"AE1650-AD1651*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1651>$J$18,(AE1651/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.7459437790000084E-6,{"$error":"#N/A"},null,{"$f":"(AD1651)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1651>0,(AJ1651*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1650,NA())","v":{"$error":"#N/A"}},null,1634,{"$f":"IF(AF1651<=$J$9*0.05,AS1650*EXP((-$J$6*1)/Heterogenität!$D$4),Z1651)","v":1.1178932007207777E-3},{"$f":"IF(OR(AF1651>=$J$19, AR1650/$J$5<AN1651),0, Bodencharakterisierung!$E$8*$J$11*((AR1650/$J$5)-AN1651))","v":6.6766228399578348E-5},1.1590816810121401E-5,{"$f":"AQ1650-AP1651*Bodencharakterisierung!$E$8","v":3.5066479524021471E-3},{"$f":"AQ1651/(Bodencharakterisierung!$E$11*1000)","v":2.3146191104964667E-6},1.1294840175308991E-3,1634,null,{"$f":"(AP1651)*$G$11*Bodencharakterisierung!$E$8","v":1.6761363225240237E-7},{"$f":"IF(AF1651<=$J$9*1.05,(AV1651*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1650,NA())","v":{"$error":"#N/A"}},1106.7142687135699,1767,15.249482392319532,1.6399886323194495,0,10.249493760000083,null,2.3146191104964666,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1117.8932007207777]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1646,2.4513996144648293E-6,{"$f":"Z1663*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.4262432391477378E-6},{"$f":"AF1662*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1663^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1663)*3600*24","v":0},0,{"$f":"AE1662-AD1663*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1663>$J$18,(AE1663/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.4262432391477378E-6,{"$error":"#N/A"},null,{"$f":"(AD1663)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1663>0,(AJ1663*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1662,NA())","v":{"$error":"#N/A"}},null,1646,{"$f":"IF(AF1663<=$J$9*0.05,AS1662*EXP((-$J$6*1)/Heterogenität!$D$4),Z1663)","v":1.1069205651208071E-3},{"$f":"IF(OR(AF1663>=$J$19, AR1662/$J$5<AN1663),0, Bodencharakterisierung!$E$8*$J$11*((AR1662/$J$5)-AN1663))","v":4.2078727016173933E-5},1.1477047615459941E-5,{"$f":"AQ1662-AP1663*Bodencharakterisierung!$E$8","v":3.464553620948592E-3},{"$f":"AQ1663/(Bodencharakterisierung!$E$11*1000)","v":2.2868340732333941E-6},1.118397612736267E-3,1646,null,{"$f":"(AP1663)*$G$11*Bodencharakterisierung!$E$8","v":1.6596842740894505E-7},{"$f":"IF(AF1663<=$J$9*1.05,(AV1663*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1662,NA())","v":{"$error":"#N/A"}},1095.8513594695992,1779,15.324754072319539,1.6399886323194495,0,10.324765440000091,null,2.2868340732333943,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1106.9205651208072]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1658,2.1659918118245804E-6,{"$f":"Z1675*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.1437643044730703E-6},{"$f":"AF1674*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1675^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1675)*3600*24","v":0},0,{"$f":"AE1674-AD1675*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1675>$J$18,(AE1675/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.1437643044730703E-6,{"$error":"#N/A"},null,{"$f":"(AD1675)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1675>0,(AJ1675*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1674,NA())","v":{"$error":"#N/A"}},null,1658,{"$f":"IF(AF1675<=$J$9*0.05,AS1674*EXP((-$J$6*1)/Heterogenität!$D$4),Z1675)","v":1.0913720122069279E-3},{"$f":"IF(OR(AF1675>=$J$19, AR1674/$J$5<AN1675),0, Bodencharakterisierung!$E$8*$J$11*((AR1674/$J$5)-AN1675))","v":6.8722030755123705E-5},1.1315833262987712E-5,{"$f":"AQ1674-AP1675*Bodencharakterisierung!$E$8","v":3.4245857994246267E-3},{"$f":"AQ1675/(Bodencharakterisierung!$E$11*1000)","v":2.2604526728875424E-6},1.1026878454699156E-3,1658,null,{"$f":"(AP1675)*$G$11*Bodencharakterisierung!$E$8","v":1.6363712292611575E-7},{"$f":"IF(AF1675<=$J$9*1.05,(AV1675*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1674,NA())","v":{"$error":"#N/A"}},1080.4582920848586,1791,15.400025752319547,1.6399886323194495,0,10.400037120000098,null,2.2604526728875425,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1091.3720122069278]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1668,1.9537053153073823E-6,{"$f":"Z1685*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.9336563017231163E-6},{"$f":"AF1684*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1685^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1685)*3600*24","v":0},0,{"$f":"AE1684-AD1685*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1685>$J$18,(AE1685/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.9336563017231163E-6,{"$error":"#N/A"},null,{"$f":"(AD1685)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1685>0,(AJ1685*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1684,NA())","v":{"$error":"#N/A"}},null,1668,{"$f":"IF(AF1685<=$J$9*0.05,AS1684*EXP((-$J$6*1)/Heterogenität!$D$4),Z1685)","v":1.0794428312460628E-3},{"$f":"IF(OR(AF1685>=$J$19, AR1684/$J$5<AN1685),0, Bodencharakterisierung!$E$8*$J$11*((AR1684/$J$5)-AN1685))","v":8.1026306385800187E-5},1.1192146178100803E-5,{"$f":"AQ1684-AP1685*Bodencharakterisierung!$E$8","v":3.3913229720741031E-3},{"$f":"AQ1685/(Bodencharakterisierung!$E$11*1000)","v":2.2384970112700351E-6},1.0906349774241636E-3,1668,null,{"$f":"(AP1685)*$G$11*Bodencharakterisierung!$E$8","v":1.6184849647293061E-7},{"$f":"IF(AF1685<=$J$9*1.05,(AV1685*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1684,NA())","v":{"$error":"#N/A"}},1068.648402933602,1801,15.462752152319553,1.6399886323194495,0,10.462763520000104,null,2.2384970112700349,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1079.4428312460627]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1676,1.7989573042601054E-6,{"$f":"Z1693*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.7804963218652499E-6},{"$f":"AF1692*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1693^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1693)*3600*24","v":0},0,{"$f":"AE1692-AD1693*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1693>$J$18,(AE1693/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.7804963218652499E-6,{"$error":"#N/A"},null,{"$f":"(AD1693)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1693>0,(AJ1693*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1692,NA())","v":{"$error":"#N/A"}},null,1676,{"$f":"IF(AF1693<=$J$9*0.05,AS1692*EXP((-$J$6*1)/Heterogenität!$D$4),Z1693)","v":1.0684365198136614E-3},{"$f":"IF(OR(AF1693>=$J$19, AR1692/$J$5<AN1693),0, Bodencharakterisierung!$E$8*$J$11*((AR1692/$J$5)-AN1693))","v":1.0756417212437201E-4},1.107802781734335E-5,{"$f":"AQ1692-AP1693*Bodencharakterisierung!$E$8","v":3.3654831070547083E-3},{"$f":"AQ1693/(Bodencharakterisierung!$E$11*1000)","v":2.2214409947555829E-6},1.0795145476310047E-3,1676,null,{"$f":"(AP1693)*$G$11*Bodencharakterisierung!$E$8","v":1.6019824237379378E-7},{"$f":"IF(AF1693<=$J$9*1.05,(AV1693*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1692,NA())","v":{"$error":"#N/A"}},1057.7521546155247,1809,15.512933272319557,1.6399886323194495,0,10.512944640000109,null,2.2214409947555831,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1068.4365198136613]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1679,1.7441407553021827E-6,{"$f":"Z1696*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.7262423028477892E-6},{"$f":"AF1695*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1696^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1696)*3600*24","v":0},0,{"$f":"AE1695-AD1696*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1696>$J$18,(AE1696/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.7262423028477892E-6,{"$error":"#N/A"},null,{"$f":"(AD1696)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1696>0,(AJ1696*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1695,NA())","v":{"$error":"#N/A"}},null,1679,{"$f":"IF(AF1696<=$J$9*0.05,AS1695*EXP((-$J$6*1)/Heterogenität!$D$4),Z1696)","v":1.0684365198136614E-3},{"$f":"IF(OR(AF1696>=$J$19, AR1695/$J$5<AN1696),0, Bodencharakterisierung!$E$8*$J$11*((AR1695/$J$5)-AN1696))","v":7.322310630528131E-5},1.107802781734335E-5,{"$f":"AQ1695-AP1696*Bodencharakterisierung!$E$8","v":3.3545158595155379E-3},{"$f":"AQ1696/(Bodencharakterisierung!$E$11*1000)","v":2.2142018874690018E-6},1.0795145476310047E-3,1679,null,{"$f":"(AP1696)*$G$11*Bodencharakterisierung!$E$8","v":1.6019824237379378E-7},{"$f":"IF(AF1696<=$J$9*1.05,(AV1696*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1695,NA())","v":{"$error":"#N/A"}},1057.7521546155247,1812,15.531751192319559,1.6399886323194495,0,10.531762560000111,null,2.2142018874690019,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1068.4365198136613]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1695,1.4787853056238382E-6,{"$f":"Z1712*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.4636099429689025E-6},{"$f":"AF1711*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1712^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1712)*3600*24","v":0},0,{"$f":"AE1711-AD1712*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1712>$J$18,(AE1712/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.4636099429689025E-6,{"$error":"#N/A"},null,{"$f":"(AD1712)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1712>0,(AJ1712*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1711,NA())","v":{"$error":"#N/A"}},null,1695,{"$f":"IF(AF1712<=$J$9*0.05,AS1711*EXP((-$J$6*1)/Heterogenität!$D$4),Z1712)","v":1.0571973989242666E-3},{"$f":"IF(OR(AF1712>=$J$19, AR1711/$J$5<AN1712),0, Bodencharakterisierung!$E$8*$J$11*((AR1711/$J$5)-AN1712))","v":1.2423646614190002E-5},1.0961495583985178E-5,{"$f":"AQ1711-AP1712*Bodencharakterisierung!$E$8","v":3.3000578861264334E-3},{"$f":"AQ1712/(Bodencharakterisierung!$E$11*1000)","v":2.1782560304464909E-6},1.0681588945082518E-3,1695,null,{"$f":"(AP1712)*$G$11*Bodencharakterisierung!$E$8","v":1.5851308150656383E-7},{"$f":"IF(AF1712<=$J$9*1.05,(AV1712*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1711,NA())","v":{"$error":"#N/A"}},1046.6254249350238,1828,15.632113432319569,1.6399886323194495,0,10.632124800000121,null,2.1782560304464909,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1057.1973989242665]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1699,1.4190118605663549E-6,{"$f":"Z1716*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.4044498957470838E-6},{"$f":"AF1715*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1716^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1716)*3600*24","v":0},0,{"$f":"AE1715-AD1716*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1716>$J$18,(AE1716/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.4044498957470838E-6,{"$error":"#N/A"},null,{"$f":"(AD1716)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1716>0,(AJ1716*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1715,NA())","v":{"$error":"#N/A"}},null,1699,{"$f":"IF(AF1716<=$J$9*0.05,AS1715*EXP((-$J$6*1)/Heterogenität!$D$4),Z1716)","v":1.0474341712910209E-3},{"$f":"IF(OR(AF1716>=$J$19, AR1715/$J$5<AN1716),0, Bodencharakterisierung!$E$8*$J$11*((AR1715/$J$5)-AN1716))","v":7.2937136123604315E-5},1.0860266072168327E-5,{"$f":"AQ1715-AP1716*Bodencharakterisierung!$E$8","v":3.2889442000301429E-3},{"$f":"AQ1716/(Bodencharakterisierung!$E$11*1000)","v":2.1709202640462989E-6},1.0582944373631893E-3,1699,null,{"$f":"(AP1716)*$G$11*Bodencharakterisierung!$E$8","v":1.5704921175133283E-7},{"$f":"IF(AF1716<=$J$9*1.05,(AV1716*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1715,NA())","v":{"$error":"#N/A"}},1036.9598295781107,1832,15.657203992319571,1.6399886323194495,0,10.657215360000123,null,2.1709202640462988,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1047.4341712910209]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1704,1.3476811353596439E-6,{"$f":"Z1721*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.3338511697151919E-6},{"$f":"AF1720*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1721^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1721)*3600*24","v":0},0,{"$f":"AE1720-AD1721*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1721>$J$18,(AE1721/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.3338511697151919E-6,{"$error":"#N/A"},null,{"$f":"(AD1721)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1721>0,(AJ1721*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1720,NA())","v":{"$error":"#N/A"}},null,1704,{"$f":"IF(AF1721<=$J$9*0.05,AS1720*EXP((-$J$6*1)/Heterogenität!$D$4),Z1721)","v":1.0474341712910209E-3},{"$f":"IF(OR(AF1721>=$J$19, AR1720/$J$5<AN1721),0, Bodencharakterisierung!$E$8*$J$11*((AR1720/$J$5)-AN1721))","v":1.6827101896922391E-5},1.0860266072168327E-5,{"$f":"AQ1720-AP1721*Bodencharakterisierung!$E$8","v":3.2710247610110658E-3},{"$f":"AQ1721/(Bodencharakterisierung!$E$11*1000)","v":2.1590922514924528E-6},1.0582944373631893E-3,1704,null,{"$f":"(AP1721)*$G$11*Bodencharakterisierung!$E$8","v":1.5704921175133283E-7},{"$f":"IF(AF1721<=$J$9*1.05,(AV1721*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1720,NA())","v":{"$error":"#N/A"}},1036.9598295781107,1837,15.688567192319574,1.6399886323194495,0,10.688578560000126,null,2.1590922514924529,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1047.4341712910209]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1716,1.1907753786510695E-6,{"$f":"Z1733*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.1785555870810043E-6},{"$f":"AF1732*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1733^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1733)*3600*24","v":0},0,{"$f":"AE1732-AD1733*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1733>$J$18,(AE1733/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.1785555870810043E-6,{"$error":"#N/A"},null,{"$f":"(AD1733)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1733>0,(AJ1733*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1732,NA())","v":{"$error":"#N/A"}},null,1716,{"$f":"IF(AF1733<=$J$9*0.05,AS1732*EXP((-$J$6*1)/Heterogenität!$D$4),Z1733)","v":1.0288069250735663E-3},{"$f":"IF(OR(AF1733>=$J$19, AR1732/$J$5<AN1733),0, Bodencharakterisierung!$E$8*$J$11*((AR1732/$J$5)-AN1733))","v":8.4470638321588968E-5},1.0667130450228322E-5,{"$f":"AQ1732-AP1733*Bodencharakterisierung!$E$8","v":3.2345522409445676E-3},{"$f":"AQ1733/(Bodencharakterisierung!$E$11*1000)","v":2.1350179808214969E-6},1.0394740555237946E-3,1716,null,{"$f":"(AP1733)*$G$11*Bodencharakterisierung!$E$8","v":1.542562970119313E-7},{"$f":"IF(AF1733<=$J$9*1.05,(AV1733*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1732,NA())","v":{"$error":"#N/A"}},1018.5188558228307,1849,15.763838872319582,1.6399886323194495,0,10.763850240000133,null,2.1350179808214969,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1028.8069250735664]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1728,1.0521376052527462E-6,{"$f":"Z1745*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.0413405208741788E-6},{"$f":"AF1744*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1745^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1745)*3600*24","v":0},0,{"$f":"AE1744-AD1745*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1745>$J$18,(AE1745/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.0413405208741788E-6,{"$error":"#N/A"},null,{"$f":"(AD1745)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1745>0,(AJ1745*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1744,NA())","v":{"$error":"#N/A"}},null,1728,{"$f":"IF(AF1745<=$J$9*0.05,AS1744*EXP((-$J$6*1)/Heterogenität!$D$4),Z1745)","v":1.0181637318840123E-3},{"$f":"IF(OR(AF1745>=$J$19, AR1744/$J$5<AN1745),0, Bodencharakterisierung!$E$8*$J$11*((AR1744/$J$5)-AN1745))","v":6.747746392790696E-5},1.0556777061858759E-5,{"$f":"AQ1744-AP1745*Bodencharakterisierung!$E$8","v":3.1959423118907131E-3},{"$f":"AQ1745/(Bodencharakterisierung!$E$11*1000)","v":2.1095328791357843E-6},1.028720508945871E-3,1728,null,{"$f":"(AP1745)*$G$11*Bodencharakterisierung!$E$8","v":1.5266048779856933E-7},{"$f":"IF(AF1745<=$J$9*1.05,(AV1745*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1744,NA())","v":{"$error":"#N/A"}},1007.9820945651721,1861,15.839110552319589,1.6399886323194495,0,10.839121920000141,null,2.1095328791357844,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1018.1637318840122]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1735,9.7884542789196761E-7,{"$f":"Z1752*EXP((-$J$6/Heterogenität!$D$4)*1)","v":9.6880047120021853E-7},{"$f":"AF1751*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1752^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1752)*3600*24","v":0},0,{"$f":"AE1751-AD1752*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1752>$J$18,(AE1752/(Bodencharakterisierung!$E$11*1000)),0)","v":0},9.6880047120021853E-7,{"$error":"#N/A"},null,{"$f":"(AD1752)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1752>0,(AJ1752*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1751,NA())","v":{"$error":"#N/A"}},null,1735,{"$f":"IF(AF1752<=$J$9*0.05,AS1751*EXP((-$J$6*1)/Heterogenität!$D$4),Z1752)","v":1.0097214974538113E-3},{"$f":"IF(OR(AF1752>=$J$19, AR1751/$J$5<AN1752),0, Bodencharakterisierung!$E$8*$J$11*((AR1751/$J$5)-AN1752))","v":8.243988160100135E-5},1.0469244198535671E-5,{"$f":"AQ1751-AP1752*Bodencharakterisierung!$E$8","v":3.1743998659295785E-3},{"$f":"AQ1752/(Bodencharakterisierung!$E$11*1000)","v":2.0953134428578076E-6},1.020190741652347E-3,1735,null,{"$f":"(AP1752)*$G$11*Bodencharakterisierung!$E$8","v":1.5139468389506668E-7},{"$f":"IF(AF1752<=$J$9*1.05,(AV1752*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1751,NA())","v":{"$error":"#N/A"}},999.62428247927323,1868,15.883019032319593,1.6399886323194495,0,10.883030400000145,null,2.0953134428578077,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1009.7214974538114]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1740,9.2964093836152745E-7,{"$f":"Z1757*EXP((-$J$6/Heterogenität!$D$4)*1)","v":9.2010092039890682E-7},{"$f":"AF1756*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1757^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1757)*3600*24","v":0},0,{"$f":"AE1756-AD1757*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1757>$J$18,(AE1757/(Bodencharakterisierung!$E$11*1000)),0)","v":0},9.2010092039890682E-7,{"$error":"#N/A"},null,{"$f":"(AD1757)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1757>0,(AJ1757*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1756,NA())","v":{"$error":"#N/A"}},null,1740,{"$f":"IF(AF1757<=$J$9*0.05,AS1756*EXP((-$J$6*1)/Heterogenität!$D$4),Z1757)","v":1.0097214974538113E-3},{"$f":"IF(OR(AF1757>=$J$19, AR1756/$J$5<AN1757),0, Bodencharakterisierung!$E$8*$J$11*((AR1756/$J$5)-AN1757))","v":2.8350078791034225E-5},1.0469244198535671E-5,{"$f":"AQ1756-AP1757*Bodencharakterisierung!$E$8","v":3.157125613001994E-3},{"$f":"AQ1757/(Bodencharakterisierung!$E$11*1000)","v":2.0839112957108873E-6},1.020190741652347E-3,1740,null,{"$f":"(AP1757)*$G$11*Bodencharakterisierung!$E$8","v":1.5139468389506668E-7},{"$f":"IF(AF1757<=$J$9*1.05,(AV1757*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1756,NA())","v":{"$error":"#N/A"}},999.62428247927323,1873,15.914382232319596,1.6399886323194495,0,10.914393600000148,null,2.0839112957108874,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,1009.7214974538114]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1753,8.1297681858017814E-7,{"$f":"Z1770*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.046340131674577E-7},{"$f":"AF1769*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1770^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1770)*3600*24","v":0},0,{"$f":"AE1769-AD1770*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1770>$J$18,(AE1770/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.046340131674577E-7,{"$error":"#N/A"},null,{"$f":"(AD1770)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1770>0,(AJ1770*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1769,NA())","v":{"$error":"#N/A"}},null,1753,{"$f":"IF(AF1770<=$J$9*0.05,AS1769*EXP((-$J$6*1)/Heterogenität!$D$4),Z1770)","v":9.9940707416403397E-4},{"$f":"IF(OR(AF1770>=$J$19, AR1769/$J$5<AN1770),0, Bodencharakterisierung!$E$8*$J$11*((AR1769/$J$5)-AN1770))","v":1.1201500203671247E-7},1.1201500203671247E-7,{"$f":"AQ1769-AP1770*Bodencharakterisierung!$E$8","v":3.1193321086614863E-3},{"$f":"AQ1770/(Bodencharakterisierung!$E$11*1000)","v":2.0589650882254036E-6},9.9951908916607072E-4,1753,null,{"$f":"(AP1770)*$G$11*Bodencharakterisierung!$E$8","v":1.6198376409278246E-9},{"$f":"IF(AF1770<=$J$9*1.05,(AV1770*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1769,NA())","v":{"$error":"#N/A"}},989.41300342239356,1886,15.995926552319604,1.6399886323194495,0,10.995937920000156,null,2.0589650882254036,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,999.40707416403393]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1765,7.1832479774306E-7,{"$f":"Z1782*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.1095331571092979E-7},{"$f":"AF1781*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1782^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1782)*3600*24","v":0},0,{"$f":"AE1781-AD1782*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1782>$J$18,(AE1782/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.1095331571092979E-7,{"$error":"#N/A"},null,{"$f":"(AD1782)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1782>0,(AJ1782*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1781,NA())","v":{"$error":"#N/A"}},null,1765,{"$f":"IF(AF1782<=$J$9*0.05,AS1781*EXP((-$J$6*1)/Heterogenität!$D$4),Z1782)","v":9.8282874112755629E-4},{"$f":"IF(OR(AF1782>=$J$19, AR1781/$J$5<AN1782),0, Bodencharakterisierung!$E$8*$J$11*((AR1781/$J$5)-AN1782))","v":5.2218143384591412E-5},1.019040807009701E-5,{"$f":"AQ1781-AP1782*Bodencharakterisierung!$E$8","v":3.0809029540422805E-3},{"$f":"AQ1782/(Bodencharakterisierung!$E$11*1000)","v":2.0335993095988648E-6},9.930191491976533E-4,1765,null,{"$f":"(AP1782)*$G$11*Bodencharakterisierung!$E$8","v":1.4736246277929599E-7},{"$f":"IF(AF1782<=$J$9*1.05,(AV1782*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1781,NA())","v":{"$error":"#N/A"}},973.00045371628073,1898,16.071198232319613,1.6399886323194495,0,11.071209600000163,null,2.0335993095988649,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,982.82874112755633]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1768,6.9643651481943197E-7,{"$f":"Z1785*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.892896513509274E-7},{"$f":"AF1784*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1785^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1785)*3600*24","v":0},0,{"$f":"AE1784-AD1785*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1785>$J$18,(AE1785/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.892896513509274E-7,{"$error":"#N/A"},null,{"$f":"(AD1785)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1785>0,(AJ1785*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1784,NA())","v":{"$error":"#N/A"}},null,1768,{"$f":"IF(AF1785<=$J$9*0.05,AS1784*EXP((-$J$6*1)/Heterogenität!$D$4),Z1785)","v":9.8282874112755629E-4},{"$f":"IF(OR(AF1785>=$J$19, AR1784/$J$5<AN1785),0, Bodencharakterisierung!$E$8*$J$11*((AR1784/$J$5)-AN1785))","v":2.0628633046778117E-5},1.019040807009701E-5,{"$f":"AQ1784-AP1785*Bodencharakterisierung!$E$8","v":3.070814450052885E-3},{"$f":"AQ1785/(Bodencharakterisierung!$E$11*1000)","v":2.0269402310580099E-6},9.930191491976533E-4,1768,null,{"$f":"(AP1785)*$G$11*Bodencharakterisierung!$E$8","v":1.4736246277929599E-7},{"$f":"IF(AF1785<=$J$9*1.05,(AV1785*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1784,NA())","v":{"$error":"#N/A"}},973.00045371628073,1901,16.090016152319613,1.6399886323194495,0,11.090027520000165,null,2.0269402310580098,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,982.82874112755633]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1775,6.4792256729979502E-7,{"$f":"Z1792*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.4127355618662095E-7},{"$f":"AF1791*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1792^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1792)*3600*24","v":0},0,{"$f":"AE1791-AD1792*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1792>$J$18,(AE1792/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.4127355618662095E-7,{"$error":"#N/A"},null,{"$f":"(AD1792)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1792>0,(AJ1792*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1791,NA())","v":{"$error":"#N/A"}},null,1775,{"$f":"IF(AF1792<=$J$9*0.05,AS1791*EXP((-$J$6*1)/Heterogenität!$D$4),Z1792)","v":9.7319729704793071E-4},{"$f":"IF(OR(AF1792>=$J$19, AR1791/$J$5<AN1792),0, Bodencharakterisierung!$E$8*$J$11*((AR1791/$J$5)-AN1792))","v":5.1518696127234229E-5},1.0090544949119284E-5,{"$f":"AQ1791-AP1792*Bodencharakterisierung!$E$8","v":3.0506510231778665E-3},{"$f":"AQ1792/(Bodencharakterisierung!$E$11*1000)","v":2.0136310384012321E-6},9.8328784199705E-4,1775,null,{"$f":"(AP1792)*$G$11*Bodencharakterisierung!$E$8","v":1.4591835226410596E-7},{"$f":"IF(AF1792<=$J$9*1.05,(AV1792*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1791,NA())","v":{"$error":"#N/A"}},963.46532407745144,1908,16.133924632319619,1.6399886323194495,0,11.133936000000169,null,2.0136310384012321,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,973.19729704793076]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1789,5.6079773817517969E-7,{"$f":"Z1806*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.5504280605588473E-7},{"$f":"AF1805*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1806^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1806)*3600*24","v":0},0,{"$f":"AE1805-AD1806*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1806>$J$18,(AE1806/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.5504280605588473E-7,{"$error":"#N/A"},null,{"$f":"(AD1806)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1806>0,(AJ1806*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1805,NA())","v":{"$error":"#N/A"}},null,1789,{"$f":"IF(AF1806<=$J$9*0.05,AS1805*EXP((-$J$6*1)/Heterogenität!$D$4),Z1806)","v":9.5756608248826142E-4},{"$f":"IF(OR(AF1806>=$J$19, AR1805/$J$5<AN1806),0, Bodencharakterisierung!$E$8*$J$11*((AR1805/$J$5)-AN1806))","v":7.5313071330835988E-5},9.9284735237236809E-6,{"$f":"AQ1805-AP1806*Bodencharakterisierung!$E$8","v":3.0095156414387753E-3},{"$f":"AQ1806/(Bodencharakterisierung!$E$11*1000)","v":1.9864789712467166E-6},9.674945560119851E-4,1789,null,{"$f":"(AP1806)*$G$11*Bodencharakterisierung!$E$8","v":1.4357465373621968E-7},{"$f":"IF(AF1806<=$J$9*1.05,(AV1806*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1805,NA())","v":{"$error":"#N/A"}},947.9904216633787,1922,16.221741592319628,1.6399886323194495,0,11.221752960000178,null,1.9864789712467166,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,957.56608248826137]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1798,{"$f":"AG1814","v":5.1107928217626934E-7},{"$f":"Z1815*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.0583456313358367E-7},{"$f":"AF1814*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1815^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1815)*3600*24","v":0},{"$f":"MIN(AC1815,Z1815-AA1815)","v":0},{"$f":"AE1814-AD1815*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1815>$J$18,(AE1815/(Bodencharakterisierung!$E$11*1000)),0)","v":0},{"$f":"AA1815+AD1815","v":5.0583456313358367E-7},{"$f":"IF(AD1815>0,Y1815,NA())","v":{"$error":"#N/A"}},null,{"$f":"(AD1815)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1815>0,(AJ1815*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1814,NA())","v":{"$error":"#N/A"}},null,1798,{"$f":"IF(AF1815<=$J$9*0.05,AS1814*EXP((-$J$6*1)/Heterogenität!$D$4),Z1815)","v":9.5120241877543832E-4},{"$f":"IF(OR(AF1815>=$J$19, AR1814/$J$5<AN1815),0, Bodencharakterisierung!$E$8*$J$11*((AR1814/$J$5)-AN1815))","v":5.1885632296712285E-5},{"$f":"MIN(AO1815,AS1814-AN1815)","v":9.8624922114758096E-6},{"$f":"AQ1814-AP1815*Bodencharakterisierung!$E$8","v":2.9821934055976724E-3},{"$f":"AQ1815/(Bodencharakterisierung!$E$11*1000)","v":1.9684444921436781E-6},{"$f":"AN1815+AP1815","v":9.6106491098691413E-4},{"$f":"IF(AN1815>$G$5,AM1815,NA())","v":1798},null,{"$f":"(AP1815)*$G$11*Bodencharakterisierung!$E$8","v":1.4262050463803116E-7},{"$f":"IF(AF1815<=$J$9*1.05,(AV1815*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1814,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH1815>($G$5*10^6),BH1815*0.99,9999)","v":941.69039458768395},{"$f":"AT1815+$G$3","v":1931},{"$f":"IF(ISNUMBER(AT1815),BA1815+BB1815+BC1815+$AZ$17,\"\")","v":16.278195352319631},{"$f":"IF(ISNUMBER(AK1815),AK1815,BA1814)","v":1.6399886323194495},{"$f":"IF(ISNUMBER(AW1815),AW1815,0)","v":0},11.278206720000183,null,{"$f":"AR1815*10^6","v":1.9684444921436781},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF1815*10^6","v":0},{"$f":"AN1815*10^6","v":951.20241877543833}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1805,4.7547736736239452E-7,{"$f":"Z1822*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.7059799680299171E-7},{"$f":"AF1821*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1822^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1822)*3600*24","v":0},0,{"$f":"AE1821-AD1822*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1822>$J$18,(AE1822/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.7059799680299171E-7,{"$error":"#N/A"},null,{"$f":"(AD1822)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1822>0,(AJ1822*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1821,NA())","v":{"$error":"#N/A"}},null,1805,{"$f":"IF(AF1822<=$J$9*0.05,AS1821*EXP((-$J$6*1)/Heterogenität!$D$4),Z1822)","v":9.4236222550458395E-4},{"$f":"IF(OR(AF1822>=$J$19, AR1821/$J$5<AN1822),0, Bodencharakterisierung!$E$8*$J$11*((AR1821/$J$5)-AN1822))","v":7.6269433530362377E-5},9.7708331328603178E-6,{"$f":"AQ1821-AP1822*Bodencharakterisierung!$E$8","v":2.9624190548563751E-3},{"$f":"AQ1822/(Bodencharakterisierung!$E$11*1000)","v":1.9553921154167494E-6},9.5213305863744426E-4,1805,null,{"$f":"(AP1822)*$G$11*Bodencharakterisierung!$E$8","v":1.4129503195156478E-7},{"$f":"IF(AF1822<=$J$9*1.05,(AV1822*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1821,NA())","v":{"$error":"#N/A"}},932.93860324953812,1938,16.322103832319637,1.6399886323194495,0,11.322115200000187,null,1.9553921154167493,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,942.36222550458399]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1817,4.2011921611552105E-7,{"$f":"Z1834*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.1580793344411879E-7},{"$f":"AF1833*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1834^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1834)*3600*24","v":0},0,{"$f":"AE1833-AD1834*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1834>$J$18,(AE1834/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.1580793344411879E-7,{"$error":"#N/A"},null,{"$f":"(AD1834)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1834>0,(AJ1834*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1833,NA())","v":{"$error":"#N/A"}},null,1817,{"$f":"IF(AF1834<=$J$9*0.05,AS1833*EXP((-$J$6*1)/Heterogenität!$D$4),Z1834)","v":9.3822966951258541E-4},{"$f":"IF(OR(AF1834>=$J$19, AR1833/$J$5<AN1834),0, Bodencharakterisierung!$E$8*$J$11*((AR1833/$J$5)-AN1834))","v":0},0,{"$f":"AQ1833-AP1834*Bodencharakterisierung!$E$8","v":2.9283853735737652E-3},{"$f":"AQ1834/(Bodencharakterisierung!$E$11*1000)","v":1.9329276393226172E-6},9.3822966951258541E-4,1817,null,{"$f":"(AP1834)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF1834<=$J$9*1.05,(AV1834*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1833,NA())","v":{"$error":"#N/A"}},928.84737281745947,1950,16.397375512319645,1.6399886323194495,0,11.397386880000195,null,1.9329276393226171,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,938.22966951258536]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1820,4.0731764182366626E-7,{"$f":"Z1837*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.0313772949500014E-7},{"$f":"AF1836*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1837^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1837)*3600*24","v":0},0,{"$f":"AE1836-AD1837*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1837>$J$18,(AE1837/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.0313772949500014E-7,{"$error":"#N/A"},null,{"$f":"(AD1837)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1837>0,(AJ1837*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1836,NA())","v":{"$error":"#N/A"}},null,1820,{"$f":"IF(AF1837<=$J$9*0.05,AS1836*EXP((-$J$6*1)/Heterogenität!$D$4),Z1837)","v":9.2860151359683025E-4},{"$f":"IF(OR(AF1837>=$J$19, AR1836/$J$5<AN1837),0, Bodencharakterisierung!$E$8*$J$11*((AR1836/$J$5)-AN1837))","v":7.4193653487685527E-5},9.6281559157551568E-6,{"$f":"AQ1836-AP1837*Bodencharakterisierung!$E$8","v":2.9188534992171675E-3},{"$f":"AQ1837/(Bodencharakterisierung!$E$11*1000)","v":1.9266359730806387E-6},9.3822966951258541E-4,1820,null,{"$f":"(AP1837)*$G$11*Bodencharakterisierung!$E$8","v":1.3923179111268124E-7},{"$f":"IF(AF1837<=$J$9*1.05,(AV1837*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1836,NA())","v":{"$error":"#N/A"}},919.31549846086193,1953,16.416193432319645,1.6399886323194495,0,11.416204800000196,null,1.9266359730806386,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,928.60151359683027]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1835,3.4892861938125155E-7,{"$f":"Z1852*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.45347897879855E-7},{"$f":"AF1851*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1852^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1852)*3600*24","v":0},0,{"$f":"AE1851-AD1852*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1852>$J$18,(AE1852/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.45347897879855E-7,{"$error":"#N/A"},null,{"$f":"(AD1852)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1852>0,(AJ1852*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1851,NA())","v":{"$error":"#N/A"}},null,1835,{"$f":"IF(AF1852<=$J$9*0.05,AS1851*EXP((-$J$6*1)/Heterogenität!$D$4),Z1852)","v":9.1553846125782081E-4},{"$f":"IF(OR(AF1852>=$J$19, AR1851/$J$5<AN1852),0, Bodencharakterisierung!$E$8*$J$11*((AR1851/$J$5)-AN1852))","v":6.6731457855765896E-5},9.4927123451664115E-6,{"$f":"AQ1851-AP1852*Bodencharakterisierung!$E$8","v":2.8757428613326473E-3},{"$f":"AQ1852/(Bodencharakterisierung!$E$11*1000)","v":1.8981801064901963E-6},9.2503117360298722E-4,1835,null,{"$f":"(AP1852)*$G$11*Bodencharakterisierung!$E$8","v":1.3727315530611839E-7},{"$f":"IF(AF1852<=$J$9*1.05,(AV1852*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1851,NA())","v":{"$error":"#N/A"}},906.38307664524257,1968,16.510283032319656,1.6399886323194495,0,11.510294400000205,null,1.8981801064901964,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,915.53846125782081]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1838,3.382963143777709E-7,{"$f":"Z1855*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.3482470207814428E-7},{"$f":"AF1854*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1855^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1855)*3600*24","v":0},0,{"$f":"AE1854-AD1855*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1855>$J$18,(AE1855/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.3482470207814428E-7,{"$error":"#N/A"},null,{"$f":"(AD1855)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1855>0,(AJ1855*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1854,NA())","v":{"$error":"#N/A"}},null,1838,{"$f":"IF(AF1855<=$J$9*0.05,AS1854*EXP((-$J$6*1)/Heterogenität!$D$4),Z1855)","v":9.1553846125782081E-4},{"$f":"IF(OR(AF1855>=$J$19, AR1854/$J$5<AN1855),0, Bodencharakterisierung!$E$8*$J$11*((AR1854/$J$5)-AN1855))","v":3.7304752595404149E-5},9.4927123451664115E-6,{"$f":"AQ1854-AP1855*Bodencharakterisierung!$E$8","v":2.8663450761109324E-3},{"$f":"AQ1855/(Bodencharakterisierung!$E$11*1000)","v":1.8919769479280082E-6},9.2503117360298722E-4,1838,null,{"$f":"(AP1855)*$G$11*Bodencharakterisierung!$E$8","v":1.3727315530611839E-7},{"$f":"IF(AF1855<=$J$9*1.05,(AV1855*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1854,NA())","v":{"$error":"#N/A"}},906.38307664524257,1971,16.529100952319656,1.6399886323194495,0,11.529112320000207,null,1.8919769479280082,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,915.53846125782081]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1845,3.147305057325062E-7,{"$f":"Z1862*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.1150072684242772E-7},{"$f":"AF1861*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1862^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1862)*3600*24","v":0},0,{"$f":"AE1861-AD1862*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1862>$J$18,(AE1862/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.1150072684242772E-7,{"$error":"#N/A"},null,{"$f":"(AD1862)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1862>0,(AJ1862*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1861,NA())","v":{"$error":"#N/A"}},null,1845,{"$f":"IF(AF1862<=$J$9*0.05,AS1861*EXP((-$J$6*1)/Heterogenität!$D$4),Z1862)","v":9.1006863775798172E-4},{"$f":"IF(OR(AF1862>=$J$19, AR1861/$J$5<AN1862),0, Bodencharakterisierung!$E$8*$J$11*((AR1861/$J$5)-AN1862))","v":2.7903423876603553E-5},9.4359987681185776E-6,{"$f":"AQ1861-AP1862*Bodencharakterisierung!$E$8","v":2.8462890348356575E-3},{"$f":"AQ1862/(Bodencharakterisierung!$E$11*1000)","v":1.8787386368552194E-6},9.195046365261003E-4,1845,null,{"$f":"(AP1862)*$G$11*Bodencharakterisierung!$E$8","v":1.364530259914429E-7},{"$f":"IF(AF1862<=$J$9*1.05,(AV1862*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1861,NA())","v":{"$error":"#N/A"}},900.96795138040193,1978,16.573009432319662,1.6399886323194495,0,11.573020800000211,null,1.8787386368552195,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,910.06863775798172]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1857,2.7808754408115625E-7,{"$f":"Z1874*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.7523379694477146E-7},{"$f":"AF1873*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1874^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1874)*3600*24","v":0},0,{"$f":"AE1873-AD1874*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1874>$J$18,(AE1874/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.7523379694477146E-7,{"$error":"#N/A"},null,{"$f":"(AD1874)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1874>0,(AJ1874*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1873,NA())","v":{"$error":"#N/A"}},null,1857,{"$f":"IF(AF1874<=$J$9*0.05,AS1873*EXP((-$J$6*1)/Heterogenität!$D$4),Z1874)","v":8.9971739464019278E-4},{"$f":"IF(OR(AF1874>=$J$19, AR1873/$J$5<AN1874),0, Bodencharakterisierung!$E$8*$J$11*((AR1873/$J$5)-AN1874))","v":2.3669450786725263E-5},9.3286724487009597E-6,{"$f":"AQ1873-AP1874*Bodencharakterisierung!$E$8","v":2.8126641467417527E-3},{"$f":"AQ1874/(Bodencharakterisierung!$E$11*1000)","v":1.8565439912486816E-6},9.0904606708889374E-4,1857,null,{"$f":"(AP1874)*$G$11*Bodencharakterisierung!$E$8","v":1.3490099091673104E-7},{"$f":"IF(AF1874<=$J$9*1.05,(AV1874*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1873,NA())","v":{"$error":"#N/A"}},890.72022069379079,1990,16.648281112319669,1.6399886323194495,0,11.648292480000219,null,1.8565439912486816,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,899.71739464019277]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1869,2.4571079308980345E-7,{"$f":"Z1886*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.4318929765758004E-7},{"$f":"AF1885*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1886^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1886)*3600*24","v":0},0,{"$f":"AE1885-AD1886*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1886>$J$18,(AE1886/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.4318929765758004E-7,{"$error":"#N/A"},null,{"$f":"(AD1886)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1886>0,(AJ1886*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1885,NA())","v":{"$error":"#N/A"}},null,1869,{"$f":"IF(AF1886<=$J$9*0.05,AS1885*EXP((-$J$6*1)/Heterogenität!$D$4),Z1886)","v":8.8563987064186245E-4},{"$f":"IF(OR(AF1886>=$J$19, AR1885/$J$5<AN1886),0, Bodencharakterisierung!$E$8*$J$11*((AR1885/$J$5)-AN1886))","v":6.1042696646032205E-5},9.1827103821104979E-6,{"$f":"AQ1885-AP1886*Bodencharakterisierung!$E$8","v":2.7807093845751761E-3},{"$f":"AQ1886/(Bodencharakterisierung!$E$11*1000)","v":1.8354517389935155E-6},8.9482258102397294E-4,1869,null,{"$f":"(AP1886)*$G$11*Bodencharakterisierung!$E$8","v":1.3279024820091737E-7},{"$f":"IF(AF1886<=$J$9*1.05,(AV1886*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1885,NA())","v":{"$error":"#N/A"}},876.7834719354438,2002,16.723552792319676,1.6399886323194495,0,11.723564160000226,null,1.8354517389935154,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,885.63987064186244]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1875,2.3096468597780001E-7,{"$f":"Z1892*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.2859451577333084E-7},{"$f":"AF1891*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1892^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1892)*3600*24","v":0},0,{"$f":"AE1891-AD1892*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1892>$J$18,(AE1892/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.2859451577333084E-7,{"$error":"#N/A"},null,{"$f":"(AD1892)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1892>0,(AJ1892*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1891,NA())","v":{"$error":"#N/A"}},null,1875,{"$f":"IF(AF1892<=$J$9*0.05,AS1891*EXP((-$J$6*1)/Heterogenität!$D$4),Z1892)","v":8.8563987064186245E-4},{"$f":"IF(OR(AF1892>=$J$19, AR1891/$J$5<AN1892),0, Bodencharakterisierung!$E$8*$J$11*((AR1891/$J$5)-AN1892))","v":4.1112523801097615E-6},4.1112523801097615E-6,{"$f":"AQ1891-AP1892*Bodencharakterisierung!$E$8","v":2.7642011991592572E-3},{"$f":"AQ1892/(Bodencharakterisierung!$E$11*1000)","v":1.8245552469698067E-6},8.8975112302197221E-4,1875,null,{"$f":"(AP1892)*$G$11*Bodencharakterisierung!$E$8","v":5.9452405798941608E-8},{"$f":"IF(AF1892<=$J$9*1.05,(AV1892*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1891,NA())","v":{"$error":"#N/A"}},876.7834719354438,2008,16.76118863231968,1.6399886323194495,0,11.76120000000023,null,1.8245552469698068,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,885.63987064186244]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1887,2.0407428299190827E-7,{"$f":"Z1904*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.0198006333664753E-7},{"$f":"AF1903*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1904^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1904)*3600*24","v":0},0,{"$f":"AE1903-AD1904*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1904>$J$18,(AE1904/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.0198006333664753E-7,{"$error":"#N/A"},null,{"$f":"(AD1904)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1904>0,(AJ1904*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1903,NA())","v":{"$error":"#N/A"}},null,1887,{"$f":"IF(AF1904<=$J$9*0.05,AS1903*EXP((-$J$6*1)/Heterogenität!$D$4),Z1904)","v":8.7331025409562407E-4},{"$f":"IF(OR(AF1904>=$J$19, AR1903/$J$5<AN1904),0, Bodencharakterisierung!$E$8*$J$11*((AR1903/$J$5)-AN1904))","v":2.460335591858576E-5},9.0548714019338854E-6,{"$f":"AQ1903-AP1904*Bodencharakterisierung!$E$8","v":2.7306312126086146E-3},{"$f":"AQ1904/(Bodencharakterisierung!$E$11*1000)","v":1.8023968400056862E-6},8.8236512549755796E-4,1887,null,{"$f":"(AP1904)*$G$11*Bodencharakterisierung!$E$8","v":1.3094158160891896E-7},{"$f":"IF(AF1904<=$J$9*1.05,(AV1904*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1903,NA())","v":{"$error":"#N/A"}},864.57715155466781,2020,16.836460312319687,1.6399886323194495,0,11.836471680000237,null,1.8023968400056862,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,873.31025409562403]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1894,1.8985841572402968E-7,{"$f":"Z1911*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.879100799509147E-7},{"$f":"AF1910*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1911^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1911)*3600*24","v":0},0,{"$f":"AE1910-AD1911*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1911>$J$18,(AE1911/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.879100799509147E-7,{"$error":"#N/A"},null,{"$f":"(AD1911)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1911>0,(AJ1911*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1910,NA())","v":{"$error":"#N/A"}},null,1894,{"$f":"IF(AF1911<=$J$9*0.05,AS1910*EXP((-$J$6*1)/Heterogenität!$D$4),Z1911)","v":8.6366792375119656E-4},{"$f":"IF(OR(AF1911>=$J$19, AR1910/$J$5<AN1911),0, Bodencharakterisierung!$E$8*$J$11*((AR1910/$J$5)-AN1911))","v":6.3545190062716232E-5},8.9548954072924021E-6,{"$f":"AQ1910-AP1911*Bodencharakterisierung!$E$8","v":2.7130052784270788E-3},{"$f":"AQ1911/(Bodencharakterisierung!$E$11*1000)","v":1.7907625600178739E-6},8.7262281915848896E-4,1894,null,{"$f":"(AP1911)*$G$11*Bodencharakterisierung!$E$8","v":1.2949583883906751E-7},{"$f":"IF(AF1911<=$J$9*1.05,(AV1911*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1910,NA())","v":{"$error":"#N/A"}},855.03124451368456,2027,16.88036879231969,1.6399886323194495,0,11.880380160000241,null,1.7907625600178738,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,863.66792375119655]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1906,1.6775387066135786E-7,{"$f":"Z1923*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.6603237274386175E-7},{"$f":"AF1922*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1923^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1923)*3600*24","v":0},0,{"$f":"AE1922-AD1923*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1923>$J$18,(AE1923/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.6603237274386175E-7,{"$error":"#N/A"},null,{"$f":"(AD1923)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1923>0,(AJ1923*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1922,NA())","v":{"$error":"#N/A"}},null,1906,{"$f":"IF(AF1923<=$J$9*0.05,AS1922*EXP((-$J$6*1)/Heterogenität!$D$4),Z1923)","v":8.5557763832148307E-4},{"$f":"IF(OR(AF1923>=$J$19, AR1922/$J$5<AN1923),0, Bodencharakterisierung!$E$8*$J$11*((AR1922/$J$5)-AN1923))","v":4.030348026414182E-5},8.8710117086556687E-6,{"$f":"AQ1922-AP1923*Bodencharakterisierung!$E$8","v":2.6803591613632012E-3},{"$f":"AQ1923/(Bodencharakterisierung!$E$11*1000)","v":1.7692139678965025E-6},8.6444865003013874E-4,1906,null,{"$f":"(AP1923)*$G$11*Bodencharakterisierung!$E$8","v":1.2828280513785405E-7},{"$f":"IF(AF1923<=$J$9*1.05,(AV1923*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1922,NA())","v":{"$error":"#N/A"}},847.02186193826822,2039,16.955640472319697,1.6399886323194495,0,11.955651840000248,null,1.7692139678965024,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,855.57763832148305]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1910,1.6097315223453608E-7,{"$f":"Z1927*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.5932123836064433E-7},{"$f":"AF1926*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1927^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1927)*3600*24","v":0},0,{"$f":"AE1926-AD1927*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1927>$J$18,(AE1927/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.5932123836064433E-7,{"$error":"#N/A"},null,{"$f":"(AD1927)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1927>0,(AJ1927*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1926,NA())","v":{"$error":"#N/A"}},null,1910,{"$f":"IF(AF1927<=$J$9*0.05,AS1926*EXP((-$J$6*1)/Heterogenität!$D$4),Z1927)","v":8.5557763832148307E-4},{"$f":"IF(OR(AF1927>=$J$19, AR1926/$J$5<AN1927),0, Bodencharakterisierung!$E$8*$J$11*((AR1926/$J$5)-AN1927))","v":3.6375078255044312E-6},3.6375078255044312E-6,{"$f":"AQ1926-AP1927*Bodencharakterisierung!$E$8","v":2.6703764821892151E-3},{"$f":"AQ1927/(Bodencharakterisierung!$E$11*1000)","v":1.762624740718954E-6},8.592151461469875E-4,1910,null,{"$f":"(AP1927)*$G$11*Bodencharakterisierung!$E$8","v":5.2601633600742721E-8},{"$f":"IF(AF1927<=$J$9*1.05,(AV1927*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1926,NA())","v":{"$error":"#N/A"}},847.02186193826822,2043,16.980731032319699,1.6399886323194495,0,11.980742400000251,null,1.7626247407189539,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,855.57763832148305]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1915,1.5288137230880881E-7,{"$f":"Z1932*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.5131249665177645E-7},{"$f":"AF1931*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1932^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1932)*3600*24","v":0},0,{"$f":"AE1931-AD1932*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1932>$J$18,(AE1932/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.5131249665177645E-7,{"$error":"#N/A"},null,{"$f":"(AD1932)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1932>0,(AJ1932*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1931,NA())","v":{"$error":"#N/A"}},null,1915,{"$f":"IF(AF1932<=$J$9*0.05,AS1931*EXP((-$J$6*1)/Heterogenität!$D$4),Z1932)","v":8.503978408953009E-4},{"$f":"IF(OR(AF1932>=$J$19, AR1931/$J$5<AN1932),0, Bodencharakterisierung!$E$8*$J$11*((AR1931/$J$5)-AN1932))","v":1.4057893151400304E-5},8.8173052516866057E-6,{"$f":"AQ1931-AP1932*Bodencharakterisierung!$E$8","v":2.6558279285239313E-3},{"$f":"AQ1932/(Bodencharakterisierung!$E$11*1000)","v":1.7530217349992946E-6},8.592151461469875E-4,1915,null,{"$f":"(AP1932)*$G$11*Bodencharakterisierung!$E$8","v":1.2750616148318675E-7},{"$f":"IF(AF1932<=$J$9*1.05,(AV1932*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1931,NA())","v":{"$error":"#N/A"}},841.89386248634787,2048,17.012094232319704,1.6399886323194495,0,12.012105600000254,null,1.7530217349992945,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,850.39784089530087]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1927,1.3508193386645243E-7,{"$f":"Z1944*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.3369571686337728E-7},{"$f":"AF1943*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1944^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1944)*3600*24","v":0},0,{"$f":"AE1943-AD1944*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1944>$J$18,(AE1944/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.3369571686337728E-7,{"$error":"#N/A"},null,{"$f":"(AD1944)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1944>0,(AJ1944*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1943,NA())","v":{"$error":"#N/A"}},null,1927,{"$f":"IF(AF1944<=$J$9*0.05,AS1943*EXP((-$J$6*1)/Heterogenität!$D$4),Z1944)","v":8.3886284628072703E-4},{"$f":"IF(OR(AF1944>=$J$19, AR1943/$J$5<AN1944),0, Bodencharakterisierung!$E$8*$J$11*((AR1943/$J$5)-AN1944))","v":3.0325310210155745E-5},8.6977052671827638E-6,{"$f":"AQ1943-AP1944*Bodencharakterisierung!$E$8","v":2.6250597591482047E-3},{"$f":"AQ1944/(Bodencharakterisierung!$E$11*1000)","v":1.732712712309046E-6},8.475605515479098E-4,1927,null,{"$f":"(AP1944)*$G$11*Bodencharakterisierung!$E$8","v":1.2577663817620849E-7},{"$f":"IF(AF1944<=$J$9*1.05,(AV1944*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1943,NA())","v":{"$error":"#N/A"}},830.47421781791968,2060,17.087365912319711,1.6399886323194495,0,12.087377280000261,null,1.732712712309046,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,838.86284628072701]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1934,1.2567209146014602E-7,{"$f":"Z1951*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.2438243869158039E-7},{"$f":"AF1950*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1951^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1951)*3600*24","v":0},0,{"$f":"AE1950-AD1951*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1951>$J$18,(AE1951/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.2438243869158039E-7,{"$error":"#N/A"},null,{"$f":"(AD1951)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1951>0,(AJ1951*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1950,NA())","v":{"$error":"#N/A"}},null,1934,{"$f":"IF(AF1951<=$J$9*0.05,AS1950*EXP((-$J$6*1)/Heterogenität!$D$4),Z1951)","v":8.3358295332083409E-4},{"$f":"IF(OR(AF1951>=$J$19, AR1950/$J$5<AN1951),0, Bodencharakterisierung!$E$8*$J$11*((AR1950/$J$5)-AN1951))","v":2.4696737221638915E-5},8.6429609749411182E-6,{"$f":"AQ1950-AP1951*Bodencharakterisierung!$E$8","v":2.6068007527399756E-3},{"$f":"AQ1951/(Bodencharakterisierung!$E$11*1000)","v":1.7206605628646705E-6},8.4222591429577521E-4,1934,null,{"$f":"(AP1951)*$G$11*Bodencharakterisierung!$E$8","v":1.2498498649039317E-7},{"$f":"IF(AF1951<=$J$9*1.05,(AV1951*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1950,NA())","v":{"$error":"#N/A"}},825.24712378762581,2067,17.131274392319714,1.6399886323194495,0,12.131285760000265,null,1.7206605628646705,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,833.58295332083412]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1949,1.0765698527471754E-7,{"$f":"Z1966*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.0655220435238365E-7},{"$f":"AF1965*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1966^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1966)*3600*24","v":0},0,{"$f":"AE1965-AD1966*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1966>$J$18,(AE1966/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.0655220435238365E-7,{"$error":"#N/A"},null,{"$f":"(AD1966)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1966>0,(AJ1966*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1965,NA())","v":{"$error":"#N/A"}},null,1949,{"$f":"IF(AF1966<=$J$9*0.05,AS1965*EXP((-$J$6*1)/Heterogenität!$D$4),Z1966)","v":8.2021542955931521E-4},{"$f":"IF(OR(AF1966>=$J$19, AR1965/$J$5<AN1966),0, Bodencharakterisierung!$E$8*$J$11*((AR1965/$J$5)-AN1966))","v":3.6217363236141363E-5},8.5043605084343015E-6,{"$f":"AQ1965-AP1966*Bodencharakterisierung!$E$8","v":2.5688032460933889E-3},{"$f":"AQ1966/(Bodencharakterisierung!$E$11*1000)","v":1.6955797003916758E-6},8.2871979006774951E-4,1949,null,{"$f":"(AP1966)*$G$11*Bodencharakterisierung!$E$8","v":1.2298069913052405E-7},{"$f":"IF(AF1966<=$J$9*1.05,(AV1966*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1965,NA())","v":{"$error":"#N/A"}},812.01327526372211,2082,17.225363992319725,1.6399886323194495,0,12.225375360000275,null,1.6955797003916759,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,820.21542955931523]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1957,9.9129750273574405E-8,{"$f":"Z1974*EXP((-$J$6/Heterogenität!$D$4)*1)","v":9.8112476228063057E-8},{"$f":"AF1973*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1974^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1974)*3600*24","v":0},0,{"$f":"AE1973-AD1974*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1974>$J$18,(AE1974/(Bodencharakterisierung!$E$11*1000)),0)","v":0},9.8112476228063057E-8,{"$error":"#N/A"},null,{"$f":"(AD1974)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1974>0,(AJ1974*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1973,NA())","v":{"$error":"#N/A"}},null,1957,{"$f":"IF(AF1974<=$J$9*0.05,AS1973*EXP((-$J$6*1)/Heterogenität!$D$4),Z1974)","v":8.1285423938431121E-4},{"$f":"IF(OR(AF1974>=$J$19, AR1973/$J$5<AN1974),0, Bodencharakterisierung!$E$8*$J$11*((AR1973/$J$5)-AN1974))","v":4.5780344597046284E-5},8.4280363955691702E-6,{"$f":"AQ1973-AP1974*Bodencharakterisierung!$E$8","v":2.5489068618951014E-3},{"$f":"AQ1974/(Bodencharakterisierung!$E$11*1000)","v":1.6824467735281197E-6},8.2128227577988038E-4,1957,null,{"$f":"(AP1974)*$G$11*Bodencharakterisierung!$E$8","v":1.2187698383630977E-7},{"$f":"IF(AF1974<=$J$9*1.05,(AV1974*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1973,NA())","v":{"$error":"#N/A"}},804.72569699046812,2090,17.27554511231973,1.6399886323194495,0,12.275556480000279,null,1.6824467735281197,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,812.8542393843112]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1964,9.2224346263197651E-8,{"$f":"Z1981*EXP((-$J$6/Heterogenität!$D$4)*1)","v":9.1277935790469842E-8},{"$f":"AF1980*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1981^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1981)*3600*24","v":0},0,{"$f":"AE1980-AD1981*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1981>$J$18,(AE1981/(Bodencharakterisierung!$E$11*1000)),0)","v":0},9.1277935790469842E-8,{"$error":"#N/A"},null,{"$f":"(AD1981)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1981>0,(AJ1981*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1980,NA())","v":{"$error":"#N/A"}},null,1964,{"$f":"IF(AF1981<=$J$9*0.05,AS1980*EXP((-$J$6*1)/Heterogenität!$D$4),Z1981)","v":8.0672627066655754E-4},{"$f":"IF(OR(AF1981>=$J$19, AR1980/$J$5<AN1981),0, Bodencharakterisierung!$E$8*$J$11*((AR1980/$J$5)-AN1981))","v":5.1172079785420286E-5},8.3644988744716433E-6,{"$f":"AQ1980-AP1981*Bodencharakterisierung!$E$8","v":2.5315232296440823E-3},{"$f":"AQ1981/(Bodencharakterisierung!$E$11*1000)","v":1.6709724288079751E-6},8.1509076954102918E-4,1964,null,{"$f":"(AP1981)*$G$11*Bodencharakterisierung!$E$8","v":1.2095817415534143E-7},{"$f":"IF(AF1981<=$J$9*1.05,(AV1981*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1980,NA())","v":{"$error":"#N/A"}},798.65900795989194,2097,17.319453592319732,1.6399886323194495,0,12.319464960000284,null,1.670972428807975,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,806.72627066655753]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1976,8.148699121851269E-8,{"$f":"Z1993*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.0650767975897483E-8},{"$f":"AF1992*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1993^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1993)*3600*24","v":0},0,{"$f":"AE1992-AD1993*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1993>$J$18,(AE1993/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.0650767975897483E-8,{"$error":"#N/A"},null,{"$f":"(AD1993)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1993>0,(AJ1993*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1992,NA())","v":{"$error":"#N/A"}},null,1976,{"$f":"IF(AF1993<=$J$9*0.05,AS1992*EXP((-$J$6*1)/Heterogenität!$D$4),Z1993)","v":8.0169136465288763E-4},{"$f":"IF(OR(AF1993>=$J$19, AR1992/$J$5<AN1993),0, Bodencharakterisierung!$E$8*$J$11*((AR1992/$J$5)-AN1993))","v":2.1923636897643997E-6},2.1923636897643997E-6,{"$f":"AQ1992-AP1993*Bodencharakterisierung!$E$8","v":2.5022028834900006E-3},{"$f":"AQ1993/(Bodencharakterisierung!$E$11*1000)","v":1.6516190650099014E-6},8.0388372834265206E-4,1976,null,{"$f":"(AP1993)*$G$11*Bodencharakterisierung!$E$8","v":3.1703550084477712E-8},{"$f":"IF(AF1993<=$J$9*1.05,(AV1993*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1992,NA())","v":{"$error":"#N/A"}},793.67445100635871,2109,17.394725272319739,1.6399886323194495,0,12.394736640000291,null,1.6516190650099014,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,801.69136465288761]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1979,7.9003977512192081E-8,{"$f":"Z1996*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.8193235070155077E-8},{"$f":"AF1995*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB1996^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z1996)*3600*24","v":0},0,{"$f":"AE1995-AD1996*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE1996>$J$18,(AE1996/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.8193235070155077E-8,{"$error":"#N/A"},null,{"$f":"(AD1996)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH1996>0,(AJ1996*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK1995,NA())","v":{"$error":"#N/A"}},null,1979,{"$f":"IF(AF1996<=$J$9*0.05,AS1995*EXP((-$J$6*1)/Heterogenität!$D$4),Z1996)","v":7.956342366391521E-4},{"$f":"IF(OR(AF1996>=$J$19, AR1995/$J$5<AN1996),0, Bodencharakterisierung!$E$8*$J$11*((AR1995/$J$5)-AN1996))","v":4.2075779405109787E-5},8.24949170349996E-6,{"$f":"AQ1995-AP1996*Bodencharakterisierung!$E$8","v":2.4940358867035356E-3},{"$f":"AQ1996/(Bodencharakterisierung!$E$11*1000)","v":1.6462283080551391E-6},8.0388372834265206E-4,1979,null,{"$f":"(AP1996)*$G$11*Bodencharakterisierung!$E$8","v":1.1929506706138719E-7},{"$f":"IF(AF1996<=$J$9*1.05,(AV1996*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW1995,NA())","v":{"$error":"#N/A"}},787.67789427276057,2112,17.413543192319743,1.6399886323194495,0,12.413554560000293,null,1.646228308055139,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,795.63423663915205]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1990,{"$f":"AG2006","v":7.0529601332589835E-8},{"$f":"Z2007*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.9805823327723496E-8},{"$f":"AF2006*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2007^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2007)*3600*24","v":0},{"$f":"MIN(AC2007,Z2007-AA2007)","v":0},{"$f":"AE2006-AD2007*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2007>$J$18,(AE2007/(Bodencharakterisierung!$E$11*1000)),0)","v":0},{"$f":"AA2007+AD2007","v":6.9805823327723496E-8},{"$f":"IF(AD2007>0,Y2007,NA())","v":{"$error":"#N/A"}},null,{"$f":"(AD2007)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2007>0,(AJ2007*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2006,NA())","v":{"$error":"#N/A"}},null,1990,{"$f":"IF(AF2007<=$J$9*0.05,AS2006*EXP((-$J$6*1)/Heterogenität!$D$4),Z2007)","v":7.8953360561116455E-4},{"$f":"IF(OR(AF2007>=$J$19, AR2006/$J$5<AN2007),0, Bodencharakterisierung!$E$8*$J$11*((AR2006/$J$5)-AN2007))","v":1.463017800371667E-5},{"$f":"MIN(AO2007,AS2006-AN2007)","v":8.1862376317998501E-6},{"$f":"AQ2006-AP2007*Bodencharakterisierung!$E$8","v":2.4662504740111672E-3},{"$f":"AQ2007/(Bodencharakterisierung!$E$11*1000)","v":1.6278881016575361E-6},{"$f":"AN2007+AP2007","v":7.977198432429644E-4},{"$f":"IF(AN2007>$G$5,AM2007,NA())","v":1990},null,{"$f":"(AP2007)*$G$11*Bodencharakterisierung!$E$8","v":1.1838035631355178E-7},{"$f":"IF(AF2007<=$J$9*1.05,(AV2007*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2006,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH2007>($G$5*10^6),BH2007*0.99,9999)","v":781.63826955505294},{"$f":"AT2007+$G$3","v":2123},{"$f":"IF(ISNUMBER(AT2007),BA2007+BB2007+BC2007+$AZ$17,\"\")","v":17.482542232319748},{"$f":"IF(ISNUMBER(AK2007),AK2007,BA2006)","v":1.6399886323194495},{"$f":"IF(ISNUMBER(AW2007),AW2007,0)","v":0},12.482553600000299,null,{"$f":"AR2007*10^6","v":1.6278881016575359},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF2007*10^6","v":0},{"$f":"AN2007*10^6","v":789.5336056111646}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1997,6.5616491085179371E-8,{"$f":"Z2014*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.4943131643091938E-8},{"$f":"AF2013*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2014^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2014)*3600*24","v":0},0,{"$f":"AE2013-AD2014*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2014>$J$18,(AE2014/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.4943131643091938E-8,{"$error":"#N/A"},null,{"$f":"(AD2014)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2014>0,(AJ2014*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2013,NA())","v":{"$error":"#N/A"}},null,1997,{"$f":"IF(AF2014<=$J$9*0.05,AS2013*EXP((-$J$6*1)/Heterogenität!$D$4),Z2014)","v":7.8184273114343414E-4},{"$f":"IF(OR(AF2014>=$J$19, AR2013/$J$5<AN2014),0, Bodencharakterisierung!$E$8*$J$11*((AR2013/$J$5)-AN2014))","v":3.8840378500810115E-5},8.106495204698882E-6,{"$f":"AQ2013-AP2014*Bodencharakterisierung!$E$8","v":2.4500039845948658E-3},{"$f":"AQ2014/(Bodencharakterisierung!$E$11*1000)","v":1.617164346267238E-6},7.8994922634813302E-4,1997,null,{"$f":"(AP2014)*$G$11*Bodencharakterisierung!$E$8","v":1.1722720912211794E-7},{"$f":"IF(AF2014<=$J$9*1.05,(AV2014*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2013,NA())","v":{"$error":"#N/A"}},774.02430383199976,2130,17.526450712319754,1.6399886323194495,0,12.526462080000304,null,1.617164346267238,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,781.84273114343409]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2004,6.1045629366714663E-8,{"$f":"Z2021*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.0419176317299293E-8},{"$f":"AF2020*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2021^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2021)*3600*24","v":0},0,{"$f":"AE2020-AD2021*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2021>$J$18,(AE2021/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.0419176317299293E-8,{"$error":"#N/A"},null,{"$f":"(AD2021)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2021>0,(AJ2021*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2020,NA())","v":{"$error":"#N/A"}},null,2004,{"$f":"IF(AF2021<=$J$9*0.05,AS2020*EXP((-$J$6*1)/Heterogenität!$D$4),Z2021)","v":7.7909901612411626E-4},{"$f":"IF(OR(AF2021>=$J$19, AR2020/$J$5<AN2021),0, Bodencharakterisierung!$E$8*$J$11*((AR2020/$J$5)-AN2021))","v":9.9428840439448864E-6},8.0780471399395344E-6,{"$f":"AQ2020-AP2021*Bodencharakterisierung!$E$8","v":2.4322209580738691E-3},{"$f":"AQ2021/(Bodencharakterisierung!$E$11*1000)","v":1.6054263749662502E-6},7.8717706326405579E-4,2004,null,{"$f":"(AP2021)*$G$11*Bodencharakterisierung!$E$8","v":1.168158245283504E-7},{"$f":"IF(AF2021<=$J$9*1.05,(AV2021*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2020,NA())","v":{"$error":"#N/A"}},771.30802596287504,2137,17.570359192319756,1.6399886323194495,0,12.570370560000308,null,1.6054263749662501,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,779.09901612411625]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2016,5.3938302256300331E-8,{"$f":"Z2033*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.3384784923785596E-8},{"$f":"AF2032*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2033^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2033)*3600*24","v":0},0,{"$f":"AE2032-AD2033*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2033>$J$18,(AE2033/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.3384784923785596E-8,{"$error":"#N/A"},null,{"$f":"(AD2033)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2033>0,(AJ2033*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2032,NA())","v":{"$error":"#N/A"}},null,2016,{"$f":"IF(AF2033<=$J$9*0.05,AS2032*EXP((-$J$6*1)/Heterogenität!$D$4),Z2033)","v":7.6940620110609514E-4},{"$f":"IF(OR(AF2033>=$J$19, AR2032/$J$5<AN2033),0, Bodencharakterisierung!$E$8*$J$11*((AR2032/$J$5)-AN2033))","v":1.5384136528809925E-5},7.977547697617343E-6,{"$f":"AQ2032-AP2033*Bodencharakterisierung!$E$8","v":2.4037387962346536E-3},{"$f":"AQ2033/(Bodencharakterisierung!$E$11*1000)","v":1.5866262681416855E-6},7.7738374880371248E-4,2016,null,{"$f":"(AP2033)*$G$11*Bodencharakterisierung!$E$8","v":1.1536251223440975E-7},{"$f":"IF(AF2033<=$J$9*1.05,(AV2033*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2032,NA())","v":{"$error":"#N/A"}},761.71213909503422,2149,17.645630872319764,1.6399886323194495,0,12.645642240000315,null,1.5866262681416856,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,769.40620110609518]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2021,5.1226937874310541E-8,{"$f":"Z2038*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.0701244687484766E-8},{"$f":"AF2037*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2038^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2038)*3600*24","v":0},0,{"$f":"AE2037-AD2038*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2038>$J$18,(AE2038/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.0701244687484766E-8,{"$error":"#N/A"},null,{"$f":"(AD2038)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2038>0,(AJ2038*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2037,NA())","v":{"$error":"#N/A"}},null,2021,{"$f":"IF(AF2038<=$J$9*0.05,AS2037*EXP((-$J$6*1)/Heterogenität!$D$4),Z2038)","v":7.6140917817550701E-4},{"$f":"IF(OR(AF2038>=$J$19, AR2037/$J$5<AN2038),0, Bodencharakterisierung!$E$8*$J$11*((AR2037/$J$5)-AN2038))","v":6.0777761866211575E-5},7.8946309862937486E-6,{"$f":"AQ2037-AP2038*Bodencharakterisierung!$E$8","v":2.3933029995104761E-3},{"$f":"AQ2038/(Bodencharakterisierung!$E$11*1000)","v":1.5797379534722613E-6},7.6930380916180076E-4,2021,null,{"$f":"(AP2038)*$G$11*Bodencharakterisierung!$E$8","v":1.1416346203915212E-7},{"$f":"IF(AF2038<=$J$9*1.05,(AV2038*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2037,NA())","v":{"$error":"#N/A"}},753.79508639375194,2154,17.676994072319768,1.6399886323194495,0,12.677005440000318,null,1.5797379534722613,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,761.40917817550701]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2034,4.4798277765243605E-8,{"$f":"Z2051*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.4338555783412492E-8},{"$f":"AF2050*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2051^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2051)*3600*24","v":0},0,{"$f":"AE2050-AD2051*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2051>$J$18,(AE2051/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.4338555783412492E-8,{"$error":"#N/A"},null,{"$f":"(AD2051)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2051>0,(AJ2051*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2050,NA())","v":{"$error":"#N/A"}},null,2034,{"$f":"IF(AF2051<=$J$9*0.05,AS2050*EXP((-$J$6*1)/Heterogenität!$D$4),Z2051)","v":7.5723248165082073E-4},{"$f":"IF(OR(AF2051>=$J$19, AR2050/$J$5<AN2051),0, Bodencharakterisierung!$E$8*$J$11*((AR2050/$J$5)-AN2051))","v":1.3296063450139095E-7},1.3296063450139095E-7,{"$f":"AQ2050-AP2051*Bodencharakterisierung!$E$8","v":2.3634604392474951E-3},{"$f":"AQ2051/(Bodencharakterisierung!$E$11*1000)","v":1.560039893892736E-6},7.5736544228532216E-4,2034,null,{"$f":"(AP2051)*$G$11*Bodencharakterisierung!$E$8","v":1.9227303183587113E-9},{"$f":"IF(AF2051<=$J$9*1.05,(AV2051*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2050,NA())","v":{"$error":"#N/A"}},749.6601568343126,2167,17.758538392319775,1.6399886323194495,0,12.758549760000326,null,1.560039893892736,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,757.23248165082077]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2046,3.9582572441802486E-8,{"$f":"Z2063*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.9176374267303984E-8},{"$f":"AF2062*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2063^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2063)*3600*24","v":0},0,{"$f":"AE2062-AD2063*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2063>$J$18,(AE2063/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.9176374267303984E-8,{"$error":"#N/A"},null,{"$f":"(AD2063)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2063>0,(AJ2063*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2062,NA())","v":{"$error":"#N/A"}},null,2046,{"$f":"IF(AF2063<=$J$9*0.05,AS2062*EXP((-$J$6*1)/Heterogenität!$D$4),Z2063)","v":7.4425197626039167E-4},{"$f":"IF(OR(AF2063>=$J$19, AR2062/$J$5<AN2063),0, Bodencharakterisierung!$E$8*$J$11*((AR2062/$J$5)-AN2063))","v":4.4149004720197703E-5},7.7167374413252953E-6,{"$f":"AQ2062-AP2063*Bodencharakterisierung!$E$8","v":2.3345003205405362E-3},{"$f":"AQ2063/(Bodencharakterisierung!$E$11*1000)","v":1.5409243039871526E-6},7.5196871370171697E-4,2046,null,{"$f":"(AP2063)*$G$11*Bodencharakterisierung!$E$8","v":1.1159096143674581E-7},{"$f":"IF(AF2063<=$J$9*1.05,(AV2063*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2062,NA())","v":{"$error":"#N/A"}},736.80945649778766,2179,17.833810072319782,1.6399886323194495,0,12.833821440000333,null,1.5409243039871527,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,744.25197626039164]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2049,3.8376440414656357E-8,{"$f":"Z2066*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.7982619622359355E-8},{"$f":"AF2065*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2066^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2066)*3600*24","v":0},0,{"$f":"AE2065-AD2066*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2066>$J$18,(AE2066/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.7982619622359355E-8,{"$error":"#N/A"},null,{"$f":"(AD2066)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2066>0,(AJ2066*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2065,NA())","v":{"$error":"#N/A"}},null,2049,{"$f":"IF(AF2066<=$J$9*0.05,AS2065*EXP((-$J$6*1)/Heterogenität!$D$4),Z2066)","v":7.4425197626039167E-4},{"$f":"IF(OR(AF2066>=$J$19, AR2065/$J$5<AN2066),0, Bodencharakterisierung!$E$8*$J$11*((AR2065/$J$5)-AN2066))","v":2.0227690136898941E-5},7.7167374413252953E-6,{"$f":"AQ2065-AP2066*Bodencharakterisierung!$E$8","v":2.3268607504736238E-3},{"$f":"AQ2066/(Bodencharakterisierung!$E$11*1000)","v":1.5358816834809397E-6},7.5196871370171697E-4,2049,null,{"$f":"(AP2066)*$G$11*Bodencharakterisierung!$E$8","v":1.1159096143674581E-7},{"$f":"IF(AF2066<=$J$9*1.05,(AV2066*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2065,NA())","v":{"$error":"#N/A"}},736.80945649778766,2182,17.852627992319785,1.6399886323194495,0,12.852639360000335,null,1.5358816834809397,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,744.25197626039164]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2056,3.5703127662309027E-8,{"$f":"Z2073*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.5336740528131737E-8},{"$f":"AF2072*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2073^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2073)*3600*24","v":0},0,{"$f":"AE2072-AD2073*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2073>$J$18,(AE2073/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.5336740528131737E-8,{"$error":"#N/A"},null,{"$f":"(AD2073)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2073>0,(AJ2073*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2072,NA())","v":{"$error":"#N/A"}},null,2056,{"$f":"IF(AF2073<=$J$9*0.05,AS2072*EXP((-$J$6*1)/Heterogenität!$D$4),Z2073)","v":7.4085065234838238E-4},{"$f":"IF(OR(AF2073>=$J$19, AR2072/$J$5<AN2073),0, Bodencharakterisierung!$E$8*$J$11*((AR2072/$J$5)-AN2073))","v":1.3498318322367354E-6},1.3498318322367354E-6,{"$f":"AQ2072-AP2073*Bodencharakterisierung!$E$8","v":2.3123167923652407E-3},{"$f":"AQ2073/(Bodencharakterisierung!$E$11*1000)","v":1.526281711132172E-6},7.4220048418061914E-4,2056,null,{"$f":"(AP2073)*$G$11*Bodencharakterisierung!$E$8","v":1.951978191334601E-8},{"$f":"IF(AF2073<=$J$9*1.05,(AV2073*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2072,NA())","v":{"$error":"#N/A"}},733.44214582489849,2189,17.896536472319788,1.6399886323194495,0,12.896547840000339,null,1.526281711132172,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,740.85065234838237]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2070,3.0902200740197812E-8,{"$f":"Z2087*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.0585080938368098E-8},{"$f":"AF2086*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2087^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2087)*3600*24","v":0},0,{"$f":"AE2086-AD2087*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2087>$J$18,(AE2087/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.0585080938368098E-8,{"$error":"#N/A"},null,{"$f":"(AD2087)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2087>0,(AJ2087*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2086,NA())","v":{"$error":"#N/A"}},null,2070,{"$f":"IF(AF2087<=$J$9*0.05,AS2086*EXP((-$J$6*1)/Heterogenität!$D$4),Z2087)","v":7.2683606073077112E-4},{"$f":"IF(OR(AF2087>=$J$19, AR2086/$J$5<AN2087),0, Bodencharakterisierung!$E$8*$J$11*((AR2086/$J$5)-AN2087))","v":4.2868338368451073E-5},7.5361614378624715E-6,{"$f":"AQ2086-AP2087*Bodencharakterisierung!$E$8","v":2.2797926381631973E-3},{"$f":"AQ2087/(Bodencharakterisierung!$E$11*1000)","v":1.5048136225499652E-6},7.343722221686336E-4,2070,null,{"$f":"(AP2087)*$G$11*Bodencharakterisierung!$E$8","v":1.0897967007274148E-7},{"$f":"IF(AF2087<=$J$9*1.05,(AV2087*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2086,NA())","v":{"$error":"#N/A"}},719.5677001234634,2203,17.984353432319796,1.6399886323194495,0,12.984364800000348,null,1.5048136225499651,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,726.83606073077112]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2074,2.9653114080305484E-8,{"$f":"Z2091*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.934881246308933E-8},{"$f":"AF2090*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2091^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2091)*3600*24","v":0},0,{"$f":"AE2090-AD2091*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2091>$J$18,(AE2091/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.934881246308933E-8,{"$error":"#N/A"},null,{"$f":"(AD2091)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2091>0,(AJ2091*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2090,NA())","v":{"$error":"#N/A"}},null,2074,{"$f":"IF(AF2091<=$J$9*0.05,AS2090*EXP((-$J$6*1)/Heterogenität!$D$4),Z2091)","v":7.2683606073077112E-4},{"$f":"IF(OR(AF2091>=$J$19, AR2090/$J$5<AN2091),0, Bodencharakterisierung!$E$8*$J$11*((AR2090/$J$5)-AN2091))","v":1.1719615240946934E-5},7.5361614378624715E-6,{"$f":"AQ2090-AP2091*Bodencharakterisierung!$E$8","v":2.2698449050652194E-3},{"$f":"AQ2091/(Bodencharakterisierung!$E$11*1000)","v":1.4982474620892537E-6},7.343722221686336E-4,2074,null,{"$f":"(AP2091)*$G$11*Bodencharakterisierung!$E$8","v":1.0897967007274148E-7},{"$f":"IF(AF2091<=$J$9*1.05,(AV2091*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2090,NA())","v":{"$error":"#N/A"}},719.5677001234634,2207,18.009443992319799,1.6399886323194495,0,13.00945536000035,null,1.4982474620892536,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,726.83606073077112]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2086,2.6200706695902662E-8,{"$f":"Z2103*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.5931833841666262E-8},{"$f":"AF2102*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2103^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2103)*3600*24","v":0},0,{"$f":"AE2102-AD2103*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2103>$J$18,(AE2103/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.5931833841666262E-8,{"$error":"#N/A"},null,{"$f":"(AD2103)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2103>0,(AJ2103*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2102,NA())","v":{"$error":"#N/A"}},null,2086,{"$f":"IF(AF2103<=$J$9*0.05,AS2102*EXP((-$J$6*1)/Heterogenität!$D$4),Z2103)","v":7.1758351959716417E-4},{"$f":"IF(OR(AF2103>=$J$19, AR2102/$J$5<AN2103),0, Bodencharakterisierung!$E$8*$J$11*((AR2102/$J$5)-AN2103))","v":1.8941861757651035E-5},7.4402269521364967E-6,{"$f":"AQ2102-AP2103*Bodencharakterisierung!$E$8","v":2.2433041952133023E-3},{"$f":"AQ2103/(Bodencharakterisierung!$E$11*1000)","v":1.480728841724952E-6},7.2502374654930066E-4,2086,null,{"$f":"(AP2103)*$G$11*Bodencharakterisierung!$E$8","v":1.0759237115548523E-7},{"$f":"IF(AF2103<=$J$9*1.05,(AV2103*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2102,NA())","v":{"$error":"#N/A"}},710.40768440119245,2219,18.084715672319806,1.6399886323194495,0,13.084727040000358,null,1.480728841724952,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,717.58351959716413]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2098,2.3150250914815434E-8,{"$f":"Z2115*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.2912681977763495E-8},{"$f":"AF2114*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2115^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2115)*3600*24","v":0},0,{"$f":"AE2114-AD2115*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2115>$J$18,(AE2115/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.2912681977763495E-8,{"$error":"#N/A"},null,{"$f":"(AD2115)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2115>0,(AJ2115*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2114,NA())","v":{"$error":"#N/A"}},null,2098,{"$f":"IF(AF2115<=$J$9*0.05,AS2114*EXP((-$J$6*1)/Heterogenität!$D$4),Z2115)","v":7.0775666071118317E-4},{"$f":"IF(OR(AF2115>=$J$19, AR2114/$J$5<AN2115),0, Bodencharakterisierung!$E$8*$J$11*((AR2114/$J$5)-AN2115))","v":3.343386647620777E-5},7.3383376830248427E-6,{"$f":"AQ2114-AP2115*Bodencharakterisierung!$E$8","v":2.2172945870222683E-3},{"$f":"AQ2115/(Bodencharakterisierung!$E$11*1000)","v":1.4635607835130485E-6},7.1509499839420801E-4,2098,null,{"$f":"(AP2115)*$G$11*Bodencharakterisierung!$E$8","v":1.0611896071659072E-7},{"$f":"IF(AF2115<=$J$9*1.05,(AV2115*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2114,NA())","v":{"$error":"#N/A"}},700.67909410407128,2231,18.159987352319813,1.6399886323194495,0,13.159998720000365,null,1.4635607835130484,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,707.75666071118314]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2105,2.1537598456121506E-8,{"$f":"Z2122*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.1316578632591309E-8},{"$f":"AF2121*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2122^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2122)*3600*24","v":0},0,{"$f":"AE2121-AD2122*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2122>$J$18,(AE2122/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.1316578632591309E-8,{"$error":"#N/A"},null,{"$f":"(AD2122)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2122>0,(AJ2122*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2121,NA())","v":{"$error":"#N/A"}},null,2105,{"$f":"IF(AF2122<=$J$9*0.05,AS2121*EXP((-$J$6*1)/Heterogenität!$D$4),Z2122)","v":7.0356458369290429E-4},{"$f":"IF(OR(AF2122>=$J$19, AR2121/$J$5<AN2122),0, Bodencharakterisierung!$E$8*$J$11*((AR2121/$J$5)-AN2122))","v":2.5790825191408022E-5},7.2948723531154457E-6,{"$f":"AQ2121-AP2122*Bodencharakterisierung!$E$8","v":2.2017837866259941E-3},{"$f":"AQ2122/(Bodencharakterisierung!$E$11*1000)","v":1.4533226314362996E-6},7.1085945604601973E-4,2105,null,{"$f":"(AP2122)*$G$11*Bodencharakterisierung!$E$8","v":1.0549041296689277E-7},{"$f":"IF(AF2122<=$J$9*1.05,(AV2122*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2121,NA())","v":{"$error":"#N/A"}},696.5289378559753,2238,18.203895832319819,1.6399886323194495,0,13.203907200000369,null,1.4533226314362997,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,703.56458369290431]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2111,2.0245039306498752E-8,{"$f":"Z2128*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.0037283784266307E-8},{"$f":"AF2127*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2128^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2128)*3600*24","v":0},0,{"$f":"AE2127-AD2128*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2128>$J$18,(AE2128/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.0037283784266307E-8,{"$error":"#N/A"},null,{"$f":"(AD2128)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2128>0,(AJ2128*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2127,NA())","v":{"$error":"#N/A"}},null,2111,{"$f":"IF(AF2128<=$J$9*0.05,AS2127*EXP((-$J$6*1)/Heterogenität!$D$4),Z2128)","v":6.9948922759413763E-4},{"$f":"IF(OR(AF2128>=$J$19, AR2127/$J$5<AN2128),0, Bodencharakterisierung!$E$8*$J$11*((AR2127/$J$5)-AN2128))","v":2.4734936512162816E-5},7.2526172379162868E-6,{"$f":"AQ2127-AP2128*Bodencharakterisierung!$E$8","v":2.1887405836314819E-3},{"$f":"AQ2128/(Bodencharakterisierung!$E$11*1000)","v":1.4447132565224304E-6},7.0674184483205391E-4,2111,null,{"$f":"(AP2128)*$G$11*Bodencharakterisierung!$E$8","v":1.0487936600999581E-7},{"$f":"IF(AF2128<=$J$9*1.05,(AV2128*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2127,NA())","v":{"$error":"#N/A"}},692.49433531819625,2244,18.241531672319823,1.6399886323194495,0,13.241543040000373,null,1.4447132565224303,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,699.48922759413767]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2123,1.7887980853548518E-8,{"$f":"Z2140*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.7704413573305205E-8},{"$f":"AF2139*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2140^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2140)*3600*24","v":0},0,{"$f":"AE2139-AD2140*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2140>$J$18,(AE2140/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.7704413573305205E-8,{"$error":"#N/A"},null,{"$f":"(AD2140)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2140>0,(AJ2140*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2139,NA())","v":{"$error":"#N/A"}},null,2123,{"$f":"IF(AF2140<=$J$9*0.05,AS2139*EXP((-$J$6*1)/Heterogenität!$D$4),Z2140)","v":6.9102030867672869E-4},{"$f":"IF(OR(AF2140>=$J$19, AR2139/$J$5<AN2140),0, Bodencharakterisierung!$E$8*$J$11*((AR2139/$J$5)-AN2140))","v":2.687645189042995E-5},7.1648076978921178E-6,{"$f":"AQ2139-AP2140*Bodencharakterisierung!$E$8","v":2.1630204267800916E-3},{"$f":"AQ2140/(Bodencharakterisierung!$E$11*1000)","v":1.4277362553003905E-6},6.9818511637462081E-4,2123,null,{"$f":"(AP2140)*$G$11*Bodencharakterisierung!$E$8","v":1.0360956111263849E-7},{"$f":"IF(AF2140<=$J$9*1.05,(AV2140*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2139,NA())","v":{"$error":"#N/A"}},684.11010558996145,2256,18.31680335231983,1.6399886323194495,0,13.31681472000038,null,1.4277362553003905,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,691.02030867672875]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2126,1.7342911008980852E-8,{"$f":"Z2143*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.7164937260491015E-8},{"$f":"AF2142*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2143^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2143)*3600*24","v":0},0,{"$f":"AE2142-AD2143*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2143>$J$18,(AE2143/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.7164937260491015E-8,{"$error":"#N/A"},null,{"$f":"(AD2143)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2143>0,(AJ2143*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2142,NA())","v":{"$error":"#N/A"}},null,2126,{"$f":"IF(AF2143<=$J$9*0.05,AS2142*EXP((-$J$6*1)/Heterogenität!$D$4),Z2143)","v":6.9102030867672869E-4},{"$f":"IF(OR(AF2143>=$J$19, AR2142/$J$5<AN2143),0, Bodencharakterisierung!$E$8*$J$11*((AR2142/$J$5)-AN2143))","v":4.6660786370560113E-6},4.6660786370560113E-6,{"$f":"AQ2142-AP2143*Bodencharakterisierung!$E$8","v":2.1567518477492542E-3},{"$f":"AQ2143/(Bodencharakterisierung!$E$11*1000)","v":1.4235985793724451E-6},6.9568638731378472E-4,2126,null,{"$f":"(AP2143)*$G$11*Bodencharakterisierung!$E$8","v":6.7475692312671912E-8},{"$f":"IF(AF2143<=$J$9*1.05,(AV2143*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2142,NA())","v":{"$error":"#N/A"}},684.11010558996145,2259,18.33562127231983,1.6399886323194495,0,13.335632640000382,null,1.423598579372445,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,691.02030867672875]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2138,1.5323737107976866E-8,{"$f":"Z2155*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.5166484214701501E-8},{"$f":"AF2154*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2155^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2155)*3600*24","v":0},0,{"$f":"AE2154-AD2155*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2155>$J$18,(AE2155/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.5166484214701501E-8,{"$error":"#N/A"},null,{"$f":"(AD2155)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2155>0,(AJ2155*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2154,NA())","v":{"$error":"#N/A"}},null,2138,{"$f":"IF(AF2155<=$J$9*0.05,AS2154*EXP((-$J$6*1)/Heterogenität!$D$4),Z2155)","v":6.8310915481950584E-4},{"$f":"IF(OR(AF2155>=$J$19, AR2154/$J$5<AN2155),0, Bodencharakterisierung!$E$8*$J$11*((AR2154/$J$5)-AN2155))","v":2.0826285519914954E-6},2.0826285519914954E-6,{"$f":"AQ2154-AP2155*Bodencharakterisierung!$E$8","v":2.1320871629884183E-3},{"$f":"AQ2155/(Bodencharakterisierung!$E$11*1000)","v":1.407318259398296E-6},6.8519178337149737E-4,2138,null,{"$f":"(AP2155)*$G$11*Bodencharakterisierung!$E$8","v":3.0116681330605858E-8},{"$f":"IF(AF2155<=$J$9*1.05,(AV2155*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2154,NA())","v":{"$error":"#N/A"}},676.27806327131077,2271,18.410892952319838,1.6399886323194495,0,13.410904320000389,null,1.407318259398296,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,683.10915481950587]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2150,1.3539648495733485E-8,{"$f":"Z2167*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.3400704001653303E-8},{"$f":"AF2166*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2167^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2167)*3600*24","v":0},0,{"$f":"AE2166-AD2167*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2167>$J$18,(AE2167/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.3400704001653303E-8,{"$error":"#N/A"},null,{"$f":"(AD2167)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2167>0,(AJ2167*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2166,NA())","v":{"$error":"#N/A"}},null,2150,{"$f":"IF(AF2167<=$J$9*0.05,AS2166*EXP((-$J$6*1)/Heterogenität!$D$4),Z2167)","v":6.6956180953417488E-4},{"$f":"IF(OR(AF2167>=$J$19, AR2166/$J$5<AN2167),0, Bodencharakterisierung!$E$8*$J$11*((AR2166/$J$5)-AN2167))","v":6.1484507119588343E-5},6.9423163790244486E-6,{"$f":"AQ2166-AP2167*Bodencharakterisierung!$E$8","v":2.1071704401482909E-3},{"$f":"AQ2167/(Bodencharakterisierung!$E$11*1000)","v":1.3908715776556376E-6},6.7650412591319933E-4,2150,null,{"$f":"(AP2167)*$G$11*Bodencharakterisierung!$E$8","v":1.0039213660227331E-7},{"$f":"IF(AF2167<=$J$9*1.05,(AV2167*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2166,NA())","v":{"$error":"#N/A"}},662.8661914388332,2283,18.486164632319845,1.6399886323194495,0,13.486176000000397,null,1.3908715776556375,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,669.56180953417493]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2156,1.2727078952221445E-8,{"$f":"Z2173*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.2596473084078548E-8},{"$f":"AF2172*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2173^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2173)*3600*24","v":0},0,{"$f":"AE2172-AD2173*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2173>$J$18,(AE2173/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.2596473084078548E-8,{"$error":"#N/A"},null,{"$f":"(AD2173)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2173>0,(AJ2173*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2172,NA())","v":{"$error":"#N/A"}},null,2156,{"$f":"IF(AF2173<=$J$9*0.05,AS2172*EXP((-$J$6*1)/Heterogenität!$D$4),Z2173)","v":6.6956180953417488E-4},{"$f":"IF(OR(AF2173>=$J$19, AR2172/$J$5<AN2173),0, Bodencharakterisierung!$E$8*$J$11*((AR2172/$J$5)-AN2173))","v":1.84431738353724E-5},6.9423163790244486E-6,{"$f":"AQ2172-AP2173*Bodencharakterisierung!$E$8","v":2.0934246537178216E-3},{"$f":"AQ2173/(Bodencharakterisierung!$E$11*1000)","v":1.3817984512988921E-6},6.7650412591319933E-4,2156,null,{"$f":"(AP2173)*$G$11*Bodencharakterisierung!$E$8","v":1.0039213660227331E-7},{"$f":"IF(AF2173<=$J$9*1.05,(AV2173*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2172,NA())","v":{"$error":"#N/A"}},662.8661914388332,2289,18.523800472319849,1.6399886323194495,0,13.5238118400004,null,1.3817984512988921,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,669.56180953417493]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2168,1.1245310081757015E-8,{"$f":"Z2185*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.1129910193748338E-8},{"$f":"AF2184*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2185^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2185)*3600*24","v":0},0,{"$f":"AE2184-AD2185*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2185>$J$18,(AE2185/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.1129910193748338E-8,{"$error":"#N/A"},null,{"$f":"(AD2185)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2185>0,(AJ2185*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2184,NA())","v":{"$error":"#N/A"}},null,2168,{"$f":"IF(AF2185<=$J$9*0.05,AS2184*EXP((-$J$6*1)/Heterogenität!$D$4),Z2185)","v":6.6079470734957499E-4},{"$f":"IF(OR(AF2185>=$J$19, AR2184/$J$5<AN2185),0, Bodencharakterisierung!$E$8*$J$11*((AR2184/$J$5)-AN2185))","v":2.7678929337141647E-5},6.8514151414896451E-6,{"$f":"AQ2184-AP2185*Bodencharakterisierung!$E$8","v":2.0690404663401643E-3},{"$f":"AQ2185/(Bodencharakterisierung!$E$11*1000)","v":1.3657032781123197E-6},6.6764612249106464E-4,2168,null,{"$f":"(AP2185)*$G$11*Bodencharakterisierung!$E$8","v":9.9077622979200422E-8},{"$f":"IF(AF2185<=$J$9*1.05,(AV2185*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2184,NA())","v":{"$error":"#N/A"}},654.18676027607921,2301,18.599072152319856,1.6399886323194495,0,13.599083520000407,null,1.3657032781123197,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,660.79470734957499]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2175,1.046195887667287E-8,{"$f":"Z2192*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.0354597774671955E-8},{"$f":"AF2191*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2192^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2192)*3600*24","v":0},0,{"$f":"AE2191-AD2192*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2192>$J$18,(AE2192/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.0354597774671955E-8,{"$error":"#N/A"},null,{"$f":"(AD2192)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2192>0,(AJ2192*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2191,NA())","v":{"$error":"#N/A"}},null,2175,{"$f":"IF(AF2192<=$J$9*0.05,AS2191*EXP((-$J$6*1)/Heterogenität!$D$4),Z2192)","v":6.5733658114220685E-4},{"$f":"IF(OR(AF2192>=$J$19, AR2191/$J$5<AN2192),0, Bodencharakterisierung!$E$8*$J$11*((AR2191/$J$5)-AN2192))","v":1.5607224489033223E-5},6.8155597419308333E-6,{"$f":"AQ2191-AP2192*Bodencharakterisierung!$E$8","v":2.0544036012176774E-3},{"$f":"AQ2192/(Bodencharakterisierung!$E$11*1000)","v":1.3560419810017673E-6},6.6415214088413768E-4,2175,null,{"$f":"(AP2192)*$G$11*Bodencharakterisierung!$E$8","v":9.8559121664378013E-8},{"$f":"IF(AF2192<=$J$9*1.05,(AV2192*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2191,NA())","v":{"$error":"#N/A"}},650.76321533078476,2308,18.642980632319862,1.6399886323194495,0,13.642992000000412,null,1.3560419810017672,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,657.3365811422068]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2187,9.2439099397778064E-9,{"$f":"Z2204*EXP((-$J$6/Heterogenität!$D$4)*1)","v":9.1490485118530038E-9},{"$f":"AF2203*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2204^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2204)*3600*24","v":0},0,{"$f":"AE2203-AD2204*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2204>$J$18,(AE2204/(Bodencharakterisierung!$E$11*1000)),0)","v":0},9.1490485118530038E-9,{"$error":"#N/A"},null,{"$f":"(AD2204)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2204>0,(AJ2204*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2203,NA())","v":{"$error":"#N/A"}},null,2187,{"$f":"IF(AF2204<=$J$9*0.05,AS2203*EXP((-$J$6*1)/Heterogenität!$D$4),Z2204)","v":6.4762995359507935E-4},{"$f":"IF(OR(AF2204>=$J$19, AR2203/$J$5<AN2204),0, Bodencharakterisierung!$E$8*$J$11*((AR2203/$J$5)-AN2204))","v":3.6647814435345428E-5},6.714917085127569E-6,{"$f":"AQ2203-AP2204*Bodencharakterisierung!$E$8","v":2.0308602181086724E-3},{"$f":"AQ2204/(Bodencharakterisierung!$E$11*1000)","v":1.3405017941311369E-6},6.5434487068020692E-4,2187,null,{"$f":"(AP2204)*$G$11*Bodencharakterisierung!$E$8","v":9.7103738360278446E-8},{"$f":"IF(AF2204<=$J$9*1.05,(AV2204*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2203,NA())","v":{"$error":"#N/A"}},641.15365405912848,2320,18.718252312319869,1.6399886323194495,0,13.718263680000419,null,1.3405017941311368,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,647.62995359507931]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2191,8.8702652052782721E-9,{"$f":"Z2208*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.7792381367622178E-9},{"$f":"AF2207*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2208^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2208)*3600*24","v":0},0,{"$f":"AE2207-AD2208*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2208>$J$18,(AE2208/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.7792381367622178E-9,{"$error":"#N/A"},null,{"$f":"(AD2208)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2208>0,(AJ2208*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2207,NA())","v":{"$error":"#N/A"}},null,2191,{"$f":"IF(AF2208<=$J$9*0.05,AS2207*EXP((-$J$6*1)/Heterogenität!$D$4),Z2208)","v":6.4762995359507935E-4},{"$f":"IF(OR(AF2208>=$J$19, AR2207/$J$5<AN2208),0, Bodencharakterisierung!$E$8*$J$11*((AR2207/$J$5)-AN2208))","v":8.893486873047625E-6},6.714917085127569E-6,{"$f":"AQ2207-AP2208*Bodencharakterisierung!$E$8","v":2.0219965275563041E-3},{"$f":"AQ2208/(Bodencharakterisierung!$E$11*1000)","v":1.3346511733044911E-6},6.5434487068020692E-4,2191,null,{"$f":"(AP2208)*$G$11*Bodencharakterisierung!$E$8","v":9.7103738360278446E-8},{"$f":"IF(AF2208<=$J$9*1.05,(AV2208*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2207,NA())","v":{"$error":"#N/A"}},641.15365405912848,2324,18.743342872319872,1.6399886323194495,0,13.743354240000421,null,1.334651173304491,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,647.62995359507931]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2196,8.4243757328563688E-9,{"$f":"Z2213*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.3379244025643069E-9},{"$f":"AF2212*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2213^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2213)*3600*24","v":0},0,{"$f":"AE2212-AD2213*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2213>$J$18,(AE2213/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.3379244025643069E-9,{"$error":"#N/A"},null,{"$f":"(AD2213)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2213>0,(AJ2213*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2212,NA())","v":{"$error":"#N/A"}},null,2196,{"$f":"IF(AF2213<=$J$9*0.05,AS2212*EXP((-$J$6*1)/Heterogenität!$D$4),Z2213)","v":6.4291878895501777E-4},{"$f":"IF(OR(AF2213>=$J$19, AR2212/$J$5<AN2213),0, Bodencharakterisierung!$E$8*$J$11*((AR2212/$J$5)-AN2213))","v":2.5313579038584743E-5},6.6660696225345241E-6,{"$f":"AQ2212-AP2213*Bodencharakterisierung!$E$8","v":2.0125521970103433E-3},{"$f":"AQ2213/(Bodencharakterisierung!$E$11*1000)","v":1.3284172917560021E-6},6.495848585775523E-4,2196,null,{"$f":"(AP2213)*$G$11*Bodencharakterisierung!$E$8","v":9.6397360132957658E-8},{"$f":"IF(AF2213<=$J$9*1.05,(AV2213*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2212,NA())","v":{"$error":"#N/A"}},636.48960106546758,2329,18.774706072319873,1.6399886323194495,0,13.774717440000424,null,1.3284172917560022,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,642.91878895501782]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2208,7.4435554078701951E-9,{"$f":"Z2225*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.3671693007544732E-9},{"$f":"AF2224*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2225^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2225)*3600*24","v":0},0,{"$f":"AE2224-AD2225*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2225>$J$18,(AE2225/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.3671693007544732E-9,{"$error":"#N/A"},null,{"$f":"(AD2225)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2225>0,(AJ2225*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2224,NA())","v":{"$error":"#N/A"}},null,2208,{"$f":"IF(AF2225<=$J$9*0.05,AS2224*EXP((-$J$6*1)/Heterogenität!$D$4),Z2225)","v":6.3618612325994496E-4},{"$f":"IF(OR(AF2225>=$J$19, AR2224/$J$5<AN2225),0, Bodencharakterisierung!$E$8*$J$11*((AR2224/$J$5)-AN2225))","v":1.5829907539030376E-5},6.5962623326564548E-6,{"$f":"AQ2224-AP2225*Bodencharakterisierung!$E$8","v":1.9885326166996851E-3},{"$f":"AQ2225/(Bodencharakterisierung!$E$11*1000)","v":1.3125627833001221E-6},6.4278238559260141E-4,2208,null,{"$f":"(AP2225)*$G$11*Bodencharakterisierung!$E$8","v":9.5387883958341381E-8},{"$f":"IF(AF2225<=$J$9*1.05,(AV2225*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2224,NA())","v":{"$error":"#N/A"}},629.82426202734541,2341,18.84997775231988,1.6399886323194495,0,13.849989120000432,null,1.3125627833001221,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,636.18612325994491]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2215,6.9250354154046181E-9,{"$f":"Z2232*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.8539703842419605E-9},{"$f":"AF2231*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2232^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2232)*3600*24","v":0},0,{"$f":"AE2231-AD2232*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2232>$J$18,(AE2232/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.8539703842419605E-9,{"$error":"#N/A"},null,{"$f":"(AD2232)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2232>0,(AJ2232*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2231,NA())","v":{"$error":"#N/A"}},null,2215,{"$f":"IF(AF2232<=$J$9*0.05,AS2231*EXP((-$J$6*1)/Heterogenität!$D$4),Z2232)","v":6.3183295425245389E-4},{"$f":"IF(OR(AF2232>=$J$19, AR2231/$J$5<AN2232),0, Bodencharakterisierung!$E$8*$J$11*((AR2231/$J$5)-AN2232))","v":1.5393709396141208E-5},6.5511267289361953E-6,{"$f":"AQ2231-AP2232*Bodencharakterisierung!$E$8","v":1.9748211649790862E-3},{"$f":"AQ2232/(Bodencharakterisierung!$E$11*1000)","v":1.3035123201182088E-6},6.3838408098139008E-4,2215,null,{"$f":"(AP2232)*$G$11*Bodencharakterisierung!$E$8","v":9.4735182547613225E-8},{"$f":"IF(AF2232<=$J$9*1.05,(AV2232*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2231,NA())","v":{"$error":"#N/A"}},625.51462470992931,2348,18.893886232319886,1.6399886323194495,0,13.893897600000436,null,1.3035123201182088,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,631.83295425245387]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2227,6.1187779902772914E-9,{"$f":"Z2244*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.0559868098034465E-9},{"$f":"AF2243*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2244^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2244)*3600*24","v":0},0,{"$f":"AE2243-AD2244*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2244>$J$18,(AE2244/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.0559868098034465E-9,{"$error":"#N/A"},null,{"$f":"(AD2244)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2244>0,(AJ2244*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2243,NA())","v":{"$error":"#N/A"}},null,2227,{"$f":"IF(AF2244<=$J$9*0.05,AS2243*EXP((-$J$6*1)/Heterogenität!$D$4),Z2244)","v":6.2574274903810811E-4},{"$f":"IF(OR(AF2244>=$J$19, AR2243/$J$5<AN2244),0, Bodencharakterisierung!$E$8*$J$11*((AR2243/$J$5)-AN2244))","v":5.1968031354044739E-7},5.1968031354044739E-7,{"$f":"AQ2243-AP2244*Bodencharakterisierung!$E$8","v":1.9530526850065019E-3},{"$f":"AQ2244/(Bodencharakterisierung!$E$11*1000)","v":1.2891436864729385E-6},6.2626242935164857E-4,2227,null,{"$f":"(AP2244)*$G$11*Bodencharakterisierung!$E$8","v":7.5150445727447718E-9},{"$f":"IF(AF2244<=$J$9*1.05,(AV2244*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2243,NA())","v":{"$error":"#N/A"}},619.48532154772693,2360,18.969157912319893,1.6399886323194495,0,13.969169280000443,null,1.2891436864729384,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,625.74274903810806]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2232,5.8111999611189286E-9,{"$f":"Z2249*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.7515651604923927E-9},{"$f":"AF2248*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2249^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2249)*3600*24","v":0},0,{"$f":"AE2248-AD2249*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2249>$J$18,(AE2249/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.7515651604923927E-9,{"$error":"#N/A"},null,{"$f":"(AD2249)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2249>0,(AJ2249*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2248,NA())","v":{"$error":"#N/A"}},null,2232,{"$f":"IF(AF2249<=$J$9*0.05,AS2248*EXP((-$J$6*1)/Heterogenität!$D$4),Z2249)","v":6.1983569556789419E-4},{"$f":"IF(OR(AF2249>=$J$19, AR2248/$J$5<AN2249),0, Bodencharakterisierung!$E$8*$J$11*((AR2248/$J$5)-AN2249))","v":3.1150133942271301E-5},6.4267337837543761E-6,{"$f":"AQ2248-AP2249*Bodencharakterisierung!$E$8","v":1.9424485742633075E-3},{"$f":"AQ2249/(Bodencharakterisierung!$E$11*1000)","v":1.2821442734411271E-6},6.2626242935164857E-4,2232,null,{"$f":"(AP2249)*$G$11*Bodencharakterisierung!$E$8","v":9.2936348719932342E-8},{"$f":"IF(AF2249<=$J$9*1.05,(AV2249*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2248,NA())","v":{"$error":"#N/A"}},613.63733861221522,2365,19.000521112319895,1.6399886323194495,0,14.000532480000446,null,1.282144273441127,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,619.83569556789416]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2245,5.0819307343008422E-9,{"$f":"Z2262*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.0297797279397493E-9},{"$f":"AF2261*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2262^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2262)*3600*24","v":0},0,{"$f":"AE2261-AD2262*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2262>$J$18,(AE2262/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.0297797279397493E-9,{"$error":"#N/A"},null,{"$f":"(AD2262)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2262>0,(AJ2262*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2261,NA())","v":{"$error":"#N/A"}},null,2245,{"$f":"IF(AF2262<=$J$9*0.05,AS2261*EXP((-$J$6*1)/Heterogenität!$D$4),Z2262)","v":6.1225369848783517E-4},{"$f":"IF(OR(AF2262>=$J$19, AR2261/$J$5<AN2262),0, Bodencharakterisierung!$E$8*$J$11*((AR2261/$J$5)-AN2262))","v":2.714198188019858E-5},6.3481202461166536E-6,{"$f":"AQ2261-AP2262*Bodencharakterisierung!$E$8","v":1.9175296559456564E-3},{"$f":"AQ2262/(Bodencharakterisierung!$E$11*1000)","v":1.2656961425383871E-6},6.1860181873395182E-4,2245,null,{"$f":"(AP2262)*$G$11*Bodencharakterisierung!$E$8","v":9.1799526285109334E-8},{"$f":"IF(AF2262<=$J$9*1.05,(AV2262*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2261,NA())","v":{"$error":"#N/A"}},606.13116150295684,2378,19.082065432319904,1.6399886323194495,0,14.082076800000454,null,1.265696142538387,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,612.25369848783521]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2257,4.4902594802595481E-9,{"$f":"Z2274*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.4441802314540866E-9},{"$f":"AF2273*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2274^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2274)*3600*24","v":0},0,{"$f":"AE2273-AD2274*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2274>$J$18,(AE2274/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.4441802314540866E-9,{"$error":"#N/A"},null,{"$f":"(AD2274)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2274>0,(AJ2274*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2273,NA())","v":{"$error":"#N/A"}},null,2257,{"$f":"IF(AF2274<=$J$9*0.05,AS2273*EXP((-$J$6*1)/Heterogenität!$D$4),Z2274)","v":6.0686516071225573E-4},{"$f":"IF(OR(AF2274>=$J$19, AR2273/$J$5<AN2274),0, Bodencharakterisierung!$E$8*$J$11*((AR2273/$J$5)-AN2274))","v":7.1201477672402261E-6},6.2922494758222433E-6,{"$f":"AQ2273-AP2274*Bodencharakterisierung!$E$8","v":1.8943352534247502E-3},{"$f":"AQ2274/(Bodencharakterisierung!$E$11*1000)","v":1.2503863058909242E-6},6.1315741018807797E-4,2257,null,{"$f":"(AP2274)*$G$11*Bodencharakterisierung!$E$8","v":9.0991584713846795E-8},{"$f":"IF(AF2274<=$J$9*1.05,(AV2274*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2273,NA())","v":{"$error":"#N/A"}},600.79650910513317,2390,19.157337112319912,1.6399886323194495,0,14.157348480000461,null,1.2503863058909241,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,606.86516071225572]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2264,4.1774668449805877E-9,{"$f":"Z2281*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.134597488549698E-9},{"$f":"AF2280*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2281^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2281)*3600*24","v":0},0,{"$f":"AE2280-AD2281*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2281>$J$18,(AE2281/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.134597488549698E-9,{"$error":"#N/A"},null,{"$f":"(AD2281)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2281>0,(AJ2281*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2280,NA())","v":{"$error":"#N/A"}},null,2264,{"$f":"IF(AF2281<=$J$9*0.05,AS2280*EXP((-$J$6*1)/Heterogenität!$D$4),Z2281)","v":6.0124944941575514E-4},{"$f":"IF(OR(AF2281>=$J$19, AR2280/$J$5<AN2281),0, Bodencharakterisierung!$E$8*$J$11*((AR2280/$J$5)-AN2281))","v":2.2654359460564579E-5},6.234023268833727E-6,{"$f":"AQ2280-AP2281*Bodencharakterisierung!$E$8","v":1.8817878444015899E-3},{"$f":"AQ2281/(Bodencharakterisierung!$E$11*1000)","v":1.2421041877238216E-6},6.0748347268458887E-4,2264,null,{"$f":"(AP2281)*$G$11*Bodencharakterisierung!$E$8","v":9.0149581410239826E-8},{"$f":"IF(AF2281<=$J$9*1.05,(AV2281*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2280,NA())","v":{"$error":"#N/A"}},595.23695492159766,2397,19.201245592319914,1.6399886323194495,0,14.201256960000466,null,1.2421041877238217,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,601.24944941575518]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2271,3.8864634254729845E-9,{"$f":"Z2288*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.8465803594847034E-9},{"$f":"AF2287*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2288^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2288)*3600*24","v":0},0,{"$f":"AE2287-AD2288*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2288>$J$18,(AE2288/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.8465803594847034E-9,{"$error":"#N/A"},null,{"$f":"(AD2288)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2288>0,(AJ2288*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2287,NA())","v":{"$error":"#N/A"}},null,2271,{"$f":"IF(AF2288<=$J$9*0.05,AS2287*EXP((-$J$6*1)/Heterogenität!$D$4),Z2288)","v":5.9837458305288542E-4},{"$f":"IF(OR(AF2288>=$J$19, AR2287/$J$5<AN2288),0, Bodencharakterisierung!$E$8*$J$11*((AR2287/$J$5)-AN2288))","v":8.7530555500357567E-6},6.2042153682720412E-6,{"$f":"AQ2287-AP2288*Bodencharakterisierung!$E$8","v":1.8683851395862579E-3},{"$f":"AQ2288/(Bodencharakterisierung!$E$11*1000)","v":1.233257517878718E-6},6.0457879842115746E-4,2271,null,{"$f":"(AP2288)*$G$11*Bodencharakterisierung!$E$8","v":8.9718532368156803E-8},{"$f":"IF(AF2288<=$J$9*1.05,(AV2288*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2287,NA())","v":{"$error":"#N/A"}},592.39083722235659,2404,19.24515407231992,1.6399886323194495,0,14.24516544000047,null,1.233257517878718,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,598.37458305288544]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2278,3.6157313793377086E-9,{"$f":"Z2295*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.5786265780284114E-9},{"$f":"AF2294*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2295^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2295)*3600*24","v":0},0,{"$f":"AE2294-AD2295*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2295>$J$18,(AE2295/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.5786265780284114E-9,{"$error":"#N/A"},null,{"$f":"(AD2295)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2295>0,(AJ2295*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2294,NA())","v":{"$error":"#N/A"}},null,2278,{"$f":"IF(AF2295<=$J$9*0.05,AS2294*EXP((-$J$6*1)/Heterogenität!$D$4),Z2295)","v":5.9455218616527074E-4},{"$f":"IF(OR(AF2295>=$J$19, AR2294/$J$5<AN2295),0, Bodencharakterisierung!$E$8*$J$11*((AR2294/$J$5)-AN2295))","v":5.4293375325564897E-6},5.4293375325564897E-6,{"$f":"AQ2294-AP2295*Bodencharakterisierung!$E$8","v":1.8556489747396955E-3},{"$f":"AQ2295/(Bodencharakterisierung!$E$11*1000)","v":1.22485080840904E-6},5.9998152369782726E-4,2278,null,{"$f":"(AP2295)*$G$11*Bodencharakterisierung!$E$8","v":7.8513102179427634E-8},{"$f":"IF(AF2295<=$J$9*1.05,(AV2295*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2294,NA())","v":{"$error":"#N/A"}},588.606664303618,2411,19.289062552319923,1.6399886323194495,0,14.289073920000474,null,1.2248508084090399,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,594.55218616527077]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2285,3.3638585974693215E-9,{"$f":"Z2302*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.3293385262038141E-9},{"$f":"AF2301*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2302^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2302)*3600*24","v":0},0,{"$f":"AE2301-AD2302*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2302>$J$18,(AE2302/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.3293385262038141E-9,{"$error":"#N/A"},null,{"$f":"(AD2302)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2302>0,(AJ2302*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2301,NA())","v":{"$error":"#N/A"}},null,2285,{"$f":"IF(AF2302<=$J$9*0.05,AS2301*EXP((-$J$6*1)/Heterogenität!$D$4),Z2302)","v":5.8829376855911201E-4},{"$f":"IF(OR(AF2302>=$J$19, AR2301/$J$5<AN2302),0, Bodencharakterisierung!$E$8*$J$11*((AR2301/$J$5)-AN2302))","v":2.882222988175216E-5},6.0996929738082973E-6,{"$f":"AQ2301-AP2302*Bodencharakterisierung!$E$8","v":1.8433648968174037E-3},{"$f":"AQ2302/(Bodencharakterisierung!$E$11*1000)","v":1.2167425061501014E-6},5.9439346153292031E-4,2285,null,{"$f":"(AP2302)*$G$11*Bodencharakterisierung!$E$8","v":8.8207044569256543E-8},{"$f":"IF(AF2302<=$J$9*1.05,(AV2302*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2301,NA())","v":{"$error":"#N/A"}},582.41083087352081,2418,19.332971032319929,1.6399886323194495,0,14.332982400000478,null,1.2167425061501014,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,588.29376855911198]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2297,2.9722164168019221E-9,{"$f":"Z2314*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.941715395563484E-9},{"$f":"AF2313*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2314^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2314)*3600*24","v":0},0,{"$f":"AE2313-AD2314*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2314>$J$18,(AE2314/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.941715395563484E-9,{"$error":"#N/A"},null,{"$f":"(AD2314)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2314>0,(AJ2314*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2313,NA())","v":{"$error":"#N/A"}},null,2297,{"$f":"IF(AF2314<=$J$9*0.05,AS2313*EXP((-$J$6*1)/Heterogenität!$D$4),Z2314)","v":5.8160127501195966E-4},{"$f":"IF(OR(AF2314>=$J$19, AR2313/$J$5<AN2314),0, Bodencharakterisierung!$E$8*$J$11*((AR2313/$J$5)-AN2314))","v":2.5832016278248056E-5},6.0303022067315038E-6,{"$f":"AQ2313-AP2314*Bodencharakterisierung!$E$8","v":1.8215443304573414E-3},{"$f":"AQ2314/(Bodencharakterisierung!$E$11*1000)","v":1.2023394920510505E-6},5.8763157721869116E-4,2297,null,{"$f":"(AP2314)*$G$11*Bodencharakterisierung!$E$8","v":8.7203591688837848E-8},{"$f":"IF(AF2314<=$J$9*1.05,(AV2314*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2313,NA())","v":{"$error":"#N/A"}},575.78526226183999,2430,19.408242712319936,1.6399886323194495,0,14.408254080000486,null,1.2023394920510504,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,581.60127501195961]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2304,2.7651710534508662E-9,{"$f":"Z2321*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.7367947412306516E-9},{"$f":"AF2320*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2321^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2321)*3600*24","v":0},0,{"$f":"AE2320-AD2321*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2321>$J$18,(AE2321/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.7367947412306516E-9,{"$error":"#N/A"},null,{"$f":"(AD2321)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2321>0,(AJ2321*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2320,NA())","v":{"$error":"#N/A"}},null,2304,{"$f":"IF(AF2321<=$J$9*0.05,AS2320*EXP((-$J$6*1)/Heterogenität!$D$4),Z2321)","v":5.7653090725826364E-4},{"$f":"IF(OR(AF2321>=$J$19, AR2320/$J$5<AN2321),0, Bodencharakterisierung!$E$8*$J$11*((AR2320/$J$5)-AN2321))","v":3.7169665817883957E-5},5.9777303655617585E-6,{"$f":"AQ2320-AP2321*Bodencharakterisierung!$E$8","v":1.8093569485488552E-3},{"$f":"AQ2321/(Bodencharakterisierung!$E$11*1000)","v":1.1942950155437987E-6},5.825086376238254E-4,2304,null,{"$f":"(AP2321)*$G$11*Bodencharakterisierung!$E$8","v":8.6443355598749464E-8},{"$f":"IF(AF2321<=$J$9*1.05,(AV2321*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2320,NA())","v":{"$error":"#N/A"}},570.76559818568091,2437,19.452151192319938,1.6399886323194495,0,14.45216256000049,null,1.1942950155437988,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,576.5309072582636]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2312,2.5461489126119343E-9,{"$f":"Z2329*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.5200202156500341E-9},{"$f":"AF2328*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2329^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2329)*3600*24","v":0},0,{"$f":"AE2328-AD2329*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2329>$J$18,(AE2329/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.5200202156500341E-9,{"$error":"#N/A"},null,{"$f":"(AD2329)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2329>0,(AJ2329*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2328,NA())","v":{"$error":"#N/A"}},null,2312,{"$f":"IF(AF2329<=$J$9*0.05,AS2328*EXP((-$J$6*1)/Heterogenität!$D$4),Z2329)","v":5.7072202888916381E-4},{"$f":"IF(OR(AF2329>=$J$19, AR2328/$J$5<AN2329),0, Bodencharakterisierung!$E$8*$J$11*((AR2328/$J$5)-AN2329))","v":5.0652936773283418E-5},5.917501315948529E-6,{"$f":"AQ2328-AP2329*Bodencharakterisierung!$E$8","v":1.7955522970046918E-3},{"$f":"AQ2329/(Bodencharakterisierung!$E$11*1000)","v":1.1851830343265293E-6},5.7663953020511234E-4,2312,null,{"$f":"(AP2329)*$G$11*Bodencharakterisierung!$E$8","v":8.5572389390054995E-8},{"$f":"IF(AF2329<=$J$9*1.05,(AV2329*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2328,NA())","v":{"$error":"#N/A"}},565.01480860027209,2445,19.502332312319943,1.6399886323194495,0,14.502343680000495,null,1.1851830343265293,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,570.72202888916377]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2327,2.1811582254062265E-9,{"$f":"Z2344*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.1587750796226864E-9},{"$f":"AF2343*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2344^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2344)*3600*24","v":0},0,{"$f":"AE2343-AD2344*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2344>$J$18,(AE2344/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.1587750796226864E-9,{"$error":"#N/A"},null,{"$f":"(AD2344)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2344>0,(AJ2344*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2343,NA())","v":{"$error":"#N/A"}},null,2327,{"$f":"IF(AF2344<=$J$9*0.05,AS2343*EXP((-$J$6*1)/Heterogenität!$D$4),Z2344)","v":5.6658353188908264E-4},{"$f":"IF(OR(AF2344>=$J$19, AR2343/$J$5<AN2344),0, Bodencharakterisierung!$E$8*$J$11*((AR2343/$J$5)-AN2344))","v":3.9668134961195542E-6},3.9668134961195542E-6,{"$f":"AQ2343-AP2344*Bodencharakterisierung!$E$8","v":1.7683692180923154E-3},{"$f":"AQ2344/(Bodencharakterisierung!$E$11*1000)","v":1.1672404079817264E-6},5.7055034538520217E-4,2327,null,{"$f":"(AP2344)*$G$11*Bodencharakterisierung!$E$8","v":5.7363689673004622E-8},{"$f":"IF(AF2344<=$J$9*1.05,(AV2344*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2343,NA())","v":{"$error":"#N/A"}},560.91769657019188,2460,19.596421912319954,1.6399886323194495,0,14.596433280000504,null,1.1672404079817265,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,566.58353188908268]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2334,2.0292181800069449E-9,{"$f":"Z2351*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.0083942499405022E-9},{"$f":"AF2350*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2351^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2351)*3600*24","v":0},0,{"$f":"AE2350-AD2351*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2351>$J$18,(AE2351/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.0083942499405022E-9,{"$error":"#N/A"},null,{"$f":"(AD2351)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2351>0,(AJ2351*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2350,NA())","v":{"$error":"#N/A"}},null,2334,{"$f":"IF(AF2351<=$J$9*0.05,AS2350*EXP((-$J$6*1)/Heterogenität!$D$4),Z2351)","v":5.5907010832674975E-4},{"$f":"IF(OR(AF2351>=$J$19, AR2350/$J$5<AN2351),0, Bodencharakterisierung!$E$8*$J$11*((AR2350/$J$5)-AN2351))","v":4.2991018154984374E-5},5.7966889909088918E-6,{"$f":"AQ2350-AP2351*Bodencharakterisierung!$E$8","v":1.7567774486086356E-3},{"$f":"AQ2351/(Bodencharakterisierung!$E$11*1000)","v":1.1595890749891984E-6},5.6486679731765864E-4,2334,null,{"$f":"(AP2351)*$G$11*Bodencharakterisierung!$E$8","v":8.382533454892692E-8},{"$f":"IF(AF2351<=$J$9*1.05,(AV2351*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2350,NA())","v":{"$error":"#N/A"}},553.47940724348223,2467,19.640330392319957,1.6399886323194495,0,14.640341760000508,null,1.1595890749891984,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,559.07010832674973]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2337,1.967385285225483E-9,{"$f":"Z2354*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.9471958871622624E-9},{"$f":"AF2353*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2354^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2354)*3600*24","v":0},0,{"$f":"AE2353-AD2354*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2354>$J$18,(AE2354/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.9471958871622624E-9,{"$error":"#N/A"},null,{"$f":"(AD2354)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2354>0,(AJ2354*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2353,NA())","v":{"$error":"#N/A"}},null,2337,{"$f":"IF(AF2354<=$J$9*0.05,AS2353*EXP((-$J$6*1)/Heterogenität!$D$4),Z2354)","v":5.5907010832674975E-4},{"$f":"IF(OR(AF2354>=$J$19, AR2353/$J$5<AN2354),0, Bodencharakterisierung!$E$8*$J$11*((AR2353/$J$5)-AN2354))","v":2.5021711573361496E-5},5.7966889909088918E-6,{"$f":"AQ2353-AP2354*Bodencharakterisierung!$E$8","v":1.7510387265076361E-3},{"$f":"AQ2354/(Bodencharakterisierung!$E$11*1000)","v":1.1558011396090006E-6},5.6486679731765864E-4,2337,null,{"$f":"(AP2354)*$G$11*Bodencharakterisierung!$E$8","v":8.382533454892692E-8},{"$f":"IF(AF2354<=$J$9*1.05,(AV2354*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2353,NA())","v":{"$error":"#N/A"}},553.47940724348223,2470,19.65914831231996,1.6399886323194495,0,14.65915968000051,null,1.1558011396090007,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,559.07010832674973]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2351,1.7028349894827486E-9,{"$f":"Z2368*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.6853604186923572E-9},{"$f":"AF2367*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2368^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2368)*3600*24","v":0},0,{"$f":"AE2367-AD2368*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2368>$J$18,(AE2368/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.6853604186923572E-9,{"$error":"#N/A"},null,{"$f":"(AD2368)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2368>0,(AJ2368*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2367,NA())","v":{"$error":"#N/A"}},null,2351,{"$f":"IF(AF2368<=$J$9*0.05,AS2367*EXP((-$J$6*1)/Heterogenität!$D$4),Z2368)","v":5.528321589032797E-4},{"$f":"IF(OR(AF2368>=$J$19, AR2367/$J$5<AN2368),0, Bodencharakterisierung!$E$8*$J$11*((AR2367/$J$5)-AN2368))","v":9.1104776828784286E-6},5.7320111406530079E-6,{"$f":"AQ2367-AP2368*Bodencharakterisierung!$E$8","v":1.7265088317697345E-3},{"$f":"AQ2368/(Bodencharakterisierung!$E$11*1000)","v":1.1396097899470196E-6},5.5856417004393271E-4,2351,null,{"$f":"(AP2368)*$G$11*Bodencharakterisierung!$E$8","v":8.2890034683071099E-8},{"$f":"IF(AF2368<=$J$9*1.05,(AV2368*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2367,NA())","v":{"$error":"#N/A"}},547.30383731424695,2484,19.746965272319969,1.6399886323194495,0,14.746976640000518,null,1.1396097899470197,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,552.83215890327972]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2355,1.6340053133298139E-9,{"$f":"Z2372*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.6172370758341004E-9},{"$f":"AF2371*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2372^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2372)*3600*24","v":0},0,{"$f":"AE2371-AD2372*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2372>$J$18,(AE2372/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.6172370758341004E-9,{"$error":"#N/A"},null,{"$f":"(AD2372)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2372>0,(AJ2372*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2371,NA())","v":{"$error":"#N/A"}},null,2355,{"$f":"IF(AF2372<=$J$9*0.05,AS2371*EXP((-$J$6*1)/Heterogenität!$D$4),Z2372)","v":5.5031380023621115E-4},{"$f":"IF(OR(AF2372>=$J$19, AR2371/$J$5<AN2372),0, Bodencharakterisierung!$E$8*$J$11*((AR2371/$J$5)-AN2372))","v":1.2714265627604631E-5},5.7058996713701179E-6,{"$f":"AQ2371-AP2372*Bodencharakterisierung!$E$8","v":1.7198081025636589E-3},{"$f":"AQ2372/(Bodencharakterisierung!$E$11*1000)","v":1.1351868663786527E-6},5.5601969990758126E-4,2355,null,{"$f":"(AP2372)*$G$11*Bodencharakterisierung!$E$8","v":8.2512439360700863E-8},{"$f":"IF(AF2372<=$J$9*1.05,(AV2372*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2371,NA())","v":{"$error":"#N/A"}},544.81066223384903,2488,19.772055832319971,1.6399886323194495,0,14.772067200000521,null,1.1351868663786526,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,550.31380023621114]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2367,1.4437638434249712E-9,{"$f":"Z2384*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.4289478726219513E-9},{"$f":"AF2383*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2384^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2384)*3600*24","v":0},0,{"$f":"AE2383-AD2384*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2384>$J$18,(AE2384/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.4289478726219513E-9,{"$error":"#N/A"},null,{"$f":"(AD2384)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2384>0,(AJ2384*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2383,NA())","v":{"$error":"#N/A"}},null,2367,{"$f":"IF(AF2384<=$J$9*0.05,AS2383*EXP((-$J$6*1)/Heterogenität!$D$4),Z2384)","v":5.4267125253926196E-4},{"$f":"IF(OR(AF2384>=$J$19, AR2383/$J$5<AN2384),0, Bodencharakterisierung!$E$8*$J$11*((AR2383/$J$5)-AN2384))","v":2.5093767790909205E-5},5.6266583178483714E-6,{"$f":"AQ2383-AP2384*Bodencharakterisierung!$E$8","v":1.6999340035135518E-3},{"$f":"AQ2384/(Bodencharakterisierung!$E$11*1000)","v":1.1220686491838626E-6},5.4829791085711033E-4,2367,null,{"$f":"(AP2384)*$G$11*Bodencharakterisierung!$E$8","v":8.1366538143732407E-8},{"$f":"IF(AF2384<=$J$9*1.05,(AV2384*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2383,NA())","v":{"$error":"#N/A"}},537.24454001386937,2500,19.847327512319978,1.6399886323194495,0,14.847338880000528,null,1.1220686491838625,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,542.67125253926201]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2374,{"$f":"AG2390","v":1.3431908811516924E-9},{"$f":"Z2391*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.3294069947019412E-9},{"$f":"AF2390*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2391^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2391)*3600*24","v":0},{"$f":"MIN(AC2391,Z2391-AA2391)","v":0},{"$f":"AE2390-AD2391*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2391>$J$18,(AE2391/(Bodencharakterisierung!$E$11*1000)),0)","v":0},{"$f":"AA2391+AD2391","v":1.3294069947019412E-9},{"$f":"IF(AD2391>0,Y2391,NA())","v":{"$error":"#N/A"}},null,{"$f":"(AD2391)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2391>0,(AJ2391*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2390,NA())","v":{"$error":"#N/A"}},null,2374,{"$f":"IF(AF2391<=$J$9*0.05,AS2390*EXP((-$J$6*1)/Heterogenität!$D$4),Z2391)","v":5.3892094806388925E-4},{"$f":"IF(OR(AF2391>=$J$19, AR2390/$J$5<AN2391),0, Bodencharakterisierung!$E$8*$J$11*((AR2390/$J$5)-AN2391))","v":2.504337305591314E-5},{"$f":"MIN(AO2391,AS2390-AN2391)","v":5.5877734832968746E-6},{"$f":"AQ2390-AP2391*Bodencharakterisierung!$E$8","v":1.6882253512578026E-3},{"$f":"AQ2391/(Bodencharakterisierung!$E$11*1000)","v":1.1143401658467343E-6},{"$f":"AN2391+AP2391","v":5.4450872154718612E-4},{"$f":"IF(AN2391>$G$5,AM2391,NA())","v":2374},null,{"$f":"(AP2391)*$G$11*Bodencharakterisierung!$E$8","v":8.0804228475183518E-8},{"$f":"IF(AF2391<=$J$9*1.05,(AV2391*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2390,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH2391>($G$5*10^6),BH2391*0.99,9999)","v":533.53173858325033},{"$f":"AT2391+$G$3","v":2507},{"$f":"IF(ISNUMBER(AT2391),BA2391+BB2391+BC2391+$AZ$17,\"\")","v":19.891235992319981},{"$f":"IF(ISNUMBER(AK2391),AK2391,BA2390)","v":1.6399886323194495},{"$f":"IF(ISNUMBER(AW2391),AW2391,0)","v":0},14.891247360000532,null,{"$f":"AR2391*10^6","v":1.1143401658467342},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF2391*10^6","v":0},{"$f":"AN2391*10^6","v":538.92094806388923}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2386,1.1868079088880632E-9,{"$f":"Z2403*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.1746288316747389E-9},{"$f":"AF2402*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2403^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2403)*3600*24","v":0},0,{"$f":"AE2402-AD2403*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2403>$J$18,(AE2403/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.1746288316747389E-9,{"$error":"#N/A"},null,{"$f":"(AD2403)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2403>0,(AJ2403*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2402,NA())","v":{"$error":"#N/A"}},null,2386,{"$f":"IF(AF2403<=$J$9*0.05,AS2402*EXP((-$J$6*1)/Heterogenität!$D$4),Z2403)","v":5.3054975950939641E-4},{"$f":"IF(OR(AF2403>=$J$19, AR2402/$J$5<AN2403),0, Bodencharakterisierung!$E$8*$J$11*((AR2402/$J$5)-AN2403))","v":4.657958585036345E-5},5.5009772553964772E-6,{"$f":"AQ2402-AP2403*Bodencharakterisierung!$E$8","v":1.6690038328877129E-3},{"$f":"AQ2403/(Bodencharakterisierung!$E$11*1000)","v":1.101652694975388E-6},5.3605073676479288E-4,2386,null,{"$f":"(AP2403)*$G$11*Bodencharakterisierung!$E$8","v":7.9549076982193933E-8},{"$f":"IF(AF2403<=$J$9*1.05,(AV2403*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2402,NA())","v":{"$error":"#N/A"}},525.24426191430246,2519,19.966507672319988,1.6399886323194495,0,14.96651904000054,null,1.101652694975388,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,530.54975950939638]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2392,1.115582724492358E-9,{"$f":"Z2409*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.104134563389208E-9},{"$f":"AF2408*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2409^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2409)*3600*24","v":0},0,{"$f":"AE2408-AD2409*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2409>$J$18,(AE2409/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.104134563389208E-9,{"$error":"#N/A"},null,{"$f":"(AD2409)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2409>0,(AJ2409*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2408,NA())","v":{"$error":"#N/A"}},null,2392,{"$f":"IF(AF2409<=$J$9*0.05,AS2408*EXP((-$J$6*1)/Heterogenität!$D$4),Z2409)","v":5.3054975950939641E-4},{"$f":"IF(OR(AF2409>=$J$19, AR2408/$J$5<AN2409),0, Bodencharakterisierung!$E$8*$J$11*((AR2408/$J$5)-AN2409))","v":1.2474341647755242E-5},5.5009772553964772E-6,{"$f":"AQ2408-AP2409*Bodencharakterisierung!$E$8","v":1.6581118979220274E-3},{"$f":"AQ2409/(Bodencharakterisierung!$E$11*1000)","v":1.094463298958434E-6},5.3605073676479288E-4,2392,null,{"$f":"(AP2409)*$G$11*Bodencharakterisierung!$E$8","v":7.9549076982193933E-8},{"$f":"IF(AF2409<=$J$9*1.05,(AV2409*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2408,NA())","v":{"$error":"#N/A"}},525.24426191430246,2525,20.004143512319992,1.6399886323194495,0,15.004154880000543,null,1.094463298958434,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,530.54975950939638]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2404,9.8569936635603294E-10,{"$f":"Z2421*EXP((-$J$6/Heterogenität!$D$4)*1)","v":9.7558407423329799E-10},{"$f":"AF2420*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2421^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2421)*3600*24","v":0},0,{"$f":"AE2420-AD2421*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2421>$J$18,(AE2421/(Bodencharakterisierung!$E$11*1000)),0)","v":0},9.7558407423329799E-10,{"$error":"#N/A"},null,{"$f":"(AD2421)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2421>0,(AJ2421*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2420,NA())","v":{"$error":"#N/A"}},null,2404,{"$f":"IF(AF2421<=$J$9*0.05,AS2420*EXP((-$J$6*1)/Heterogenität!$D$4),Z2421)","v":5.2378173686124679E-4},{"$f":"IF(OR(AF2421>=$J$19, AR2420/$J$5<AN2421),0, Bodencharakterisierung!$E$8*$J$11*((AR2420/$J$5)-AN2421))","v":1.7920209098309201E-5},5.4308033688115322E-6,{"$f":"AQ2420-AP2421*Bodencharakterisierung!$E$8","v":1.6387500174420686E-3},{"$f":"AQ2421/(Bodencharakterisierung!$E$11*1000)","v":1.0816831798297482E-6},5.2921254023005832E-4,2404,null,{"$f":"(AP2421)*$G$11*Bodencharakterisierung!$E$8","v":7.853429948959307E-8},{"$f":"IF(AF2421<=$J$9*1.05,(AV2421*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2420,NA())","v":{"$error":"#N/A"}},518.54391949263436,2537,20.079415192319999,1.6399886323194495,0,15.079426560000551,null,1.0816831798297482,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,523.78173686124683]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2407,9.5566383552620496E-10,{"$f":"Z2424*EXP((-$J$6/Heterogenität!$D$4)*1)","v":9.4585676939891552E-10},{"$f":"AF2423*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2424^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2424)*3600*24","v":0},0,{"$f":"AE2423-AD2424*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2424>$J$18,(AE2424/(Bodencharakterisierung!$E$11*1000)),0)","v":0},9.4585676939891552E-10,{"$error":"#N/A"},null,{"$f":"(AD2424)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2424>0,(AJ2424*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2423,NA())","v":{"$error":"#N/A"}},null,2407,{"$f":"IF(AF2424<=$J$9*0.05,AS2423*EXP((-$J$6*1)/Heterogenität!$D$4),Z2424)","v":5.2378173686124679E-4},{"$f":"IF(OR(AF2424>=$J$19, AR2423/$J$5<AN2424),0, Bodencharakterisierung!$E$8*$J$11*((AR2423/$J$5)-AN2424))","v":1.085120848492178E-6},1.085120848492178E-6,{"$f":"AQ2423-AP2424*Bodencharakterisierung!$E$8","v":1.6348075973386508E-3},{"$f":"AQ2424/(Bodencharakterisierung!$E$11*1000)","v":1.0790809223357431E-6},5.2486685770973898E-4,2407,null,{"$f":"(AP2424)*$G$11*Bodencharakterisierung!$E$8","v":1.5691823089616902E-8},{"$f":"IF(AF2424<=$J$9*1.05,(AV2424*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2423,NA())","v":{"$error":"#N/A"}},518.54391949263436,2540,20.098233112320003,1.6399886323194495,0,15.098244480000552,null,1.0790809223357432,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,523.78173686124683]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2423,8.1026811213262423E-10,{"$f":"Z2440*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.0195310358974751E-10},{"$f":"AF2439*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2440^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2440)*3600*24","v":0},0,{"$f":"AE2439-AD2440*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2440>$J$18,(AE2440/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.0195310358974751E-10,{"$error":"#N/A"},null,{"$f":"(AD2440)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2440>0,(AJ2440*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2439,NA())","v":{"$error":"#N/A"}},null,2423,{"$f":"IF(AF2440<=$J$9*0.05,AS2439*EXP((-$J$6*1)/Heterogenität!$D$4),Z2440)","v":5.1227904512249399E-4},{"$f":"IF(OR(AF2440>=$J$19, AR2439/$J$5<AN2440),0, Bodencharakterisierung!$E$8*$J$11*((AR2439/$J$5)-AN2440))","v":3.6694755248741528E-5},5.3115383149752006E-6,{"$f":"AQ2439-AP2440*Bodencharakterisierung!$E$8","v":1.6088832436908626E-3},{"$f":"AQ2440/(Bodencharakterisierung!$E$11*1000)","v":1.0619691377497443E-6},5.1759058343746919E-4,2423,null,{"$f":"(AP2440)*$G$11*Bodencharakterisierung!$E$8","v":7.680961958119959E-8},{"$f":"IF(AF2440<=$J$9*1.05,(AV2440*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2439,NA())","v":{"$error":"#N/A"}},507.1562546712691,2556,20.198595352320012,1.6399886323194495,0,15.198606720000562,null,1.0619691377497444,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,512.27904512249404]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2426,7.8557819785140139E-10,{"$f":"Z2443*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.7751655834168454E-10},{"$f":"AF2442*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2443^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2443)*3600*24","v":0},0,{"$f":"AE2442-AD2443*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2443>$J$18,(AE2443/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.7751655834168454E-10,{"$error":"#N/A"},null,{"$f":"(AD2443)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2443>0,(AJ2443*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2442,NA())","v":{"$error":"#N/A"}},null,2426,{"$f":"IF(AF2443<=$J$9*0.05,AS2442*EXP((-$J$6*1)/Heterogenität!$D$4),Z2443)","v":5.1227904512249399E-4},{"$f":"IF(OR(AF2443>=$J$19, AR2442/$J$5<AN2443),0, Bodencharakterisierung!$E$8*$J$11*((AR2442/$J$5)-AN2443))","v":2.0229379833307303E-5},5.3115383149752006E-6,{"$f":"AQ2442-AP2443*Bodencharakterisierung!$E$8","v":1.6036248207590372E-3},{"$f":"AQ2443/(Bodencharakterisierung!$E$11*1000)","v":1.058498231524117E-6},5.1759058343746919E-4,2426,null,{"$f":"(AP2443)*$G$11*Bodencharakterisierung!$E$8","v":7.680961958119959E-8},{"$f":"IF(AF2443<=$J$9*1.05,(AV2443*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2442,NA())","v":{"$error":"#N/A"}},507.1562546712691,2559,20.217413272320012,1.6399886323194495,0,15.217424640000564,null,1.0584982315241169,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,512.27904512249404]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2441,6.729654889609903E-10,{"$f":"Z2458*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.6605948623672668E-10},{"$f":"AF2457*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2458^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2458)*3600*24","v":0},0,{"$f":"AE2457-AD2458*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2458>$J$18,(AE2458/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.6605948623672668E-10,{"$error":"#N/A"},null,{"$f":"(AD2458)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2458>0,(AJ2458*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2457,NA())","v":{"$error":"#N/A"}},null,2441,{"$f":"IF(AF2458<=$J$9*0.05,AS2457*EXP((-$J$6*1)/Heterogenität!$D$4),Z2458)","v":5.0657249405582582E-4},{"$f":"IF(OR(AF2458>=$J$19, AR2457/$J$5<AN2458),0, Bodencharakterisierung!$E$8*$J$11*((AR2457/$J$5)-AN2458))","v":7.993122893653824E-8},7.993122893653824E-8,{"$f":"AQ2457-AP2458*Bodencharakterisierung!$E$8","v":1.5811050779694447E-3},{"$f":"AQ2458/(Bodencharakterisierung!$E$11*1000)","v":1.0436337148313166E-6},5.0665242528476239E-4,2441,null,{"$f":"(AP2458)*$G$11*Bodencharakterisierung!$E$8","v":1.155877435725876E-9},{"$f":"IF(AF2458<=$J$9*1.05,(AV2458*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2457,NA())","v":{"$error":"#N/A"}},501.50676911526756,2574,20.311502872320023,1.6399886323194495,0,15.311514240000573,null,1.0436337148313166,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,506.57249405582581]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2444,6.5245936267035282E-10,{"$f":"Z2461*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.4576379475493193E-10},{"$f":"AF2460*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2461^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2461)*3600*24","v":0},0,{"$f":"AE2460-AD2461*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2461>$J$18,(AE2461/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.4576379475493193E-10,{"$error":"#N/A"},null,{"$f":"(AD2461)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2461>0,(AJ2461*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2460,NA())","v":{"$error":"#N/A"}},null,2444,{"$f":"IF(AF2461<=$J$9*0.05,AS2460*EXP((-$J$6*1)/Heterogenität!$D$4),Z2461)","v":5.0145313485060736E-4},{"$f":"IF(OR(AF2461>=$J$19, AR2460/$J$5<AN2461),0, Bodencharakterisierung!$E$8*$J$11*((AR2460/$J$5)-AN2461))","v":3.9284765684020499E-5},5.1992904341550267E-6,{"$f":"AQ2460-AP2461*Bodencharakterisierung!$E$8","v":1.5759577804396311E-3},{"$f":"AQ2461/(Bodencharakterisierung!$E$11*1000)","v":1.040236158706027E-6},5.0665242528476239E-4,2444,null,{"$f":"(AP2461)*$G$11*Bodencharakterisierung!$E$8","v":7.5186414303684117E-8},{"$f":"IF(AF2461<=$J$9*1.05,(AV2461*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2460,NA())","v":{"$error":"#N/A"}},496.43860350210127,2577,20.330320792320023,1.6399886323194495,0,15.330332160000575,null,1.0402361587060271,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,501.45313485060734]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2456,5.7649582253066997E-10,{"$f":"Z2473*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.7057979594947009E-10},{"$f":"AF2472*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2473^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2473)*3600*24","v":0},0,{"$f":"AE2472-AD2473*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2473>$J$18,(AE2473/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.7057979594947009E-10,{"$error":"#N/A"},null,{"$f":"(AD2473)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2473>0,(AJ2473*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2472,NA())","v":{"$error":"#N/A"}},null,2456,{"$f":"IF(AF2473<=$J$9*0.05,AS2472*EXP((-$J$6*1)/Heterogenität!$D$4),Z2473)","v":4.9796744889051611E-4},{"$f":"IF(OR(AF2473>=$J$19, AR2472/$J$5<AN2473),0, Bodencharakterisierung!$E$8*$J$11*((AR2472/$J$5)-AN2473))","v":1.2669822810122941E-5},5.1631492827507435E-6,{"$f":"AQ2472-AP2473*Bodencharakterisierung!$E$8","v":1.5565904261669876E-3},{"$f":"AQ2473/(Bodencharakterisierung!$E$11*1000)","v":1.0274524265128631E-6},5.0313059817326685E-4,2456,null,{"$f":"(AP2473)*$G$11*Bodencharakterisierung!$E$8","v":7.4663780760259804E-8},{"$f":"IF(AF2473<=$J$9*1.05,(AV2473*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2472,NA())","v":{"$error":"#N/A"}},492.98777440161092,2589,20.405592472320031,1.6399886323194495,0,15.405603840000582,null,1.0274524265128631,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,497.9674488905161]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2468,5.0937644918619723E-10,{"$f":"Z2485*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.0414920469378388E-10},{"$f":"AF2484*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2485^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2485)*3600*24","v":0},0,{"$f":"AE2484-AD2485*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2485>$J$18,(AE2485/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.0414920469378388E-10,{"$error":"#N/A"},null,{"$f":"(AD2485)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2485>0,(AJ2485*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2484,NA())","v":{"$error":"#N/A"}},null,2468,{"$f":"IF(AF2485<=$J$9*0.05,AS2484*EXP((-$J$6*1)/Heterogenität!$D$4),Z2485)","v":4.8867658179070107E-4},{"$f":"IF(OR(AF2485>=$J$19, AR2484/$J$5<AN2485),0, Bodencharakterisierung!$E$8*$J$11*((AR2484/$J$5)-AN2485))","v":4.9486449517765445E-5},5.0668174162614909E-6,{"$f":"AQ2484-AP2485*Bodencharakterisierung!$E$8","v":1.5393815593622534E-3},{"$f":"AQ2485/(Bodencharakterisierung!$E$11*1000)","v":1.0160934385229395E-6},4.9374339920696256E-4,2468,null,{"$f":"(AP2485)*$G$11*Bodencharakterisierung!$E$8","v":7.327073535988581E-8},{"$f":"IF(AF2485<=$J$9*1.05,(AV2485*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2484,NA())","v":{"$error":"#N/A"}},483.78981597279403,2601,20.480864152320038,1.6399886323194495,0,15.480875520000589,null,1.0160934385229394,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,488.67658179070105]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2472,4.8878712828666148E-10,{"$f":"Z2489*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.8377117234998446E-10},{"$f":"AF2488*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2489^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2489)*3600*24","v":0},0,{"$f":"AE2488-AD2489*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2489>$J$18,(AE2489/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.8377117234998446E-10,{"$error":"#N/A"},null,{"$f":"(AD2489)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2489>0,(AJ2489*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2488,NA())","v":{"$error":"#N/A"}},null,2472,{"$f":"IF(AF2489<=$J$9*0.05,AS2488*EXP((-$J$6*1)/Heterogenität!$D$4),Z2489)","v":4.8867658179070107E-4},{"$f":"IF(OR(AF2489>=$J$19, AR2488/$J$5<AN2489),0, Bodencharakterisierung!$E$8*$J$11*((AR2488/$J$5)-AN2489))","v":2.8544104513872732E-5},5.0668174162614909E-6,{"$f":"AQ2488-AP2489*Bodencharakterisierung!$E$8","v":1.5326933603727884E-3},{"$f":"AQ2489/(Bodencharakterisierung!$E$11*1000)","v":1.0116787857246128E-6},4.9374339920696256E-4,2472,null,{"$f":"(AP2489)*$G$11*Bodencharakterisierung!$E$8","v":7.327073535988581E-8},{"$f":"IF(AF2489<=$J$9*1.05,(AV2489*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2488,NA())","v":{"$error":"#N/A"}},483.78981597279403,2605,20.50595471232004,1.6399886323194495,0,15.505966080000592,null,1.0116787857246128,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,488.67658179070105]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2477,4.6421683306835536E-10,{"$f":"Z2494*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.5945301862852618E-10},{"$f":"AF2493*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2494^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2494)*3600*24","v":0},0,{"$f":"AE2493-AD2494*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2494>$J$18,(AE2494/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.5945301862852618E-10,{"$error":"#N/A"},null,{"$f":"(AD2494)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2494>0,(AJ2494*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2493,NA())","v":{"$error":"#N/A"}},null,2477,{"$f":"IF(AF2494<=$J$9*0.05,AS2493*EXP((-$J$6*1)/Heterogenität!$D$4),Z2494)","v":4.8867658179070107E-4},{"$f":"IF(OR(AF2494>=$J$19, AR2493/$J$5<AN2494),0, Bodencharakterisierung!$E$8*$J$11*((AR2493/$J$5)-AN2494))","v":2.3661732590068389E-6},2.3661732590068389E-6,{"$f":"AQ2493-AP2494*Bodencharakterisierung!$E$8","v":1.525224324207851E-3},{"$f":"AQ2494/(Bodencharakterisierung!$E$11*1000)","v":1.0067487288500668E-6},4.9104275504970789E-4,2477,null,{"$f":"(AP2494)*$G$11*Bodencharakterisierung!$E$8","v":3.4216992726027447E-8},{"$f":"IF(AF2494<=$J$9*1.05,(AV2494*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2493,NA())","v":{"$error":"#N/A"}},483.78981597279403,2610,20.537317912320045,1.6399886323194495,0,15.537329280000595,null,1.0067487288500667,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,488.67658179070105]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2493,3.9359038499492084E-10,{"$f":"Z2510*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.8955134240565602E-10},{"$f":"AF2509*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2510^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2510)*3600*24","v":0},0,{"$f":"AE2509-AD2510*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2510>$J$18,(AE2510/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.8955134240565602E-10,{"$error":"#N/A"},null,{"$f":"(AD2510)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2510>0,(AJ2510*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2509,NA())","v":{"$error":"#N/A"}},null,2493,{"$f":"IF(AF2510<=$J$9*0.05,AS2509*EXP((-$J$6*1)/Heterogenität!$D$4),Z2510)","v":4.8102560558667867E-4},{"$f":"IF(OR(AF2510>=$J$19, AR2509/$J$5<AN2510),0, Bodencharakterisierung!$E$8*$J$11*((AR2509/$J$5)-AN2510))","v":2.2684442225661321E-6},2.2684442225661321E-6,{"$f":"AQ2509-AP2510*Bodencharakterisierung!$E$8","v":1.5013452598205375E-3},{"$f":"AQ2510/(Bodencharakterisierung!$E$11*1000)","v":9.9098697017857263E-7},4.8329404980924478E-4,2493,null,{"$f":"(AP2510)*$G$11*Bodencharakterisierung!$E$8","v":3.2803742991975039E-8},{"$f":"IF(AF2510<=$J$9*1.05,(AV2510*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2509,NA())","v":{"$error":"#N/A"}},476.21534953081192,2626,20.637680152320055,1.6399886323194495,0,15.637691520000605,null,0.99098697017857262,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,481.02560558667869]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2496,3.815971783983277E-10,{"$f":"Z2513*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.7768121064542127E-10},{"$f":"AF2512*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2513^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2513)*3600*24","v":0},0,{"$f":"AE2512-AD2513*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2513>$J$18,(AE2513/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.7768121064542127E-10,{"$error":"#N/A"},null,{"$f":"(AD2513)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2513>0,(AJ2513*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2512,NA())","v":{"$error":"#N/A"}},null,2496,{"$f":"IF(AF2513<=$J$9*0.05,AS2512*EXP((-$J$6*1)/Heterogenität!$D$4),Z2513)","v":4.7833446409593266E-4},{"$f":"IF(OR(AF2513>=$J$19, AR2512/$J$5<AN2513),0, Bodencharakterisierung!$E$8*$J$11*((AR2512/$J$5)-AN2513))","v":1.597586086886585E-5},4.9595857133121249E-6,{"$f":"AQ2512-AP2513*Bodencharakterisierung!$E$8","v":1.4964352699643588E-3},{"$f":"AQ2513/(Bodencharakterisierung!$E$11*1000)","v":9.8774605278175494E-7},4.8329404980924478E-4,2496,null,{"$f":"(AP2513)*$G$11*Bodencharakterisierung!$E$8","v":7.1720068524373499E-8},{"$f":"IF(AF2513<=$J$9*1.05,(AV2513*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2512,NA())","v":{"$error":"#N/A"}},473.55111945497333,2629,20.656498072320055,1.6399886323194495,0,15.656509440000606,null,0.98774605278175498,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,478.33446409593267]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2508,3.3716916611598006E-10,{"$f":"Z2525*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.3370912066353098E-10},{"$f":"AF2524*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2525^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2525)*3600*24","v":0},0,{"$f":"AE2524-AD2525*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2525>$J$18,(AE2525/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.3370912066353098E-10,{"$error":"#N/A"},null,{"$f":"(AD2525)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2525>0,(AJ2525*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2524,NA())","v":{"$error":"#N/A"}},null,2508,{"$f":"IF(AF2525<=$J$9*0.05,AS2524*EXP((-$J$6*1)/Heterogenität!$D$4),Z2525)","v":4.7402111358410727E-4},{"$f":"IF(OR(AF2525>=$J$19, AR2524/$J$5<AN2525),0, Bodencharakterisierung!$E$8*$J$11*((AR2524/$J$5)-AN2525))","v":1.5065122438512066E-6},1.5065122438512066E-6,{"$f":"AQ2524-AP2525*Bodencharakterisierung!$E$8","v":1.4794910570142671E-3},{"$f":"AQ2525/(Bodencharakterisierung!$E$11*1000)","v":9.7656175380479667E-7},4.7552762582795847E-4,2508,null,{"$f":"(AP2525)*$G$11*Bodencharakterisierung!$E$8","v":2.1785521534954951E-8},{"$f":"IF(AF2525<=$J$9*1.05,(AV2525*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2524,NA())","v":{"$error":"#N/A"}},469.2809024482662,2641,20.731769752320062,1.6399886323194495,0,15.731781120000614,null,0.97656175380479671,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,474.0211135841073]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2513,3.2022038520389109E-10,{"$f":"Z2530*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.1693426891879435E-10},{"$f":"AF2529*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2530^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2530)*3600*24","v":0},0,{"$f":"AE2529-AD2530*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2530>$J$18,(AE2530/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.1693426891879435E-10,{"$error":"#N/A"},null,{"$f":"(AD2530)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2530>0,(AJ2530*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2529,NA())","v":{"$error":"#N/A"}},null,2513,{"$f":"IF(AF2530<=$J$9*0.05,AS2529*EXP((-$J$6*1)/Heterogenität!$D$4),Z2530)","v":4.7064773951387612E-4},{"$f":"IF(OR(AF2530>=$J$19, AR2529/$J$5<AN2530),0, Bodencharakterisierung!$E$8*$J$11*((AR2529/$J$5)-AN2530))","v":1.2748665983087138E-5},4.8798863140823534E-6,{"$f":"AQ2529-AP2530*Bodencharakterisierung!$E$8","v":1.4714392445960309E-3},{"$f":"AQ2530/(Bodencharakterisierung!$E$11*1000)","v":9.7124702613599392E-7},4.7552762582795847E-4,2513,null,{"$f":"(AP2530)*$G$11*Bodencharakterisierung!$E$8","v":7.0567543554643047E-8},{"$f":"IF(AF2530<=$J$9*1.05,(AV2530*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2529,NA())","v":{"$error":"#N/A"}},465.94126211873731,2646,20.763132952320067,1.6399886323194495,0,15.763144320000617,null,0.9712470261359939,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,470.6477395138761]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2526,2.8003473089987598E-10,{"$f":"Z2543*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.7716100164301795E-10},{"$f":"AF2542*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2543^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2543)*3600*24","v":0},0,{"$f":"AE2542-AD2543*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2543>$J$18,(AE2543/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.7716100164301795E-10,{"$error":"#N/A"},null,{"$f":"(AD2543)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2543>0,(AJ2543*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2542,NA())","v":{"$error":"#N/A"}},null,2526,{"$f":"IF(AF2543<=$J$9*0.05,AS2542*EXP((-$J$6*1)/Heterogenität!$D$4),Z2543)","v":4.6490545868541283E-4},{"$f":"IF(OR(AF2543>=$J$19, AR2542/$J$5<AN2543),0, Bodencharakterisierung!$E$8*$J$11*((AR2542/$J$5)-AN2543))","v":9.7375569833513409E-6},4.8203477775637439E-6,{"$f":"AQ2542-AP2543*Bodencharakterisierung!$E$8","v":1.4525745424630006E-3},{"$f":"AQ2543/(Bodencharakterisierung!$E$11*1000)","v":9.5879507753333373E-7},4.6972580646297658E-4,2526,null,{"$f":"(AP2543)*$G$11*Bodencharakterisierung!$E$8","v":6.970656278612964E-8},{"$f":"IF(AF2543<=$J$9*1.05,(AV2543*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2542,NA())","v":{"$error":"#N/A"}},460.25640409855873,2659,20.844677272320073,1.6399886323194495,0,15.844688640000625,null,0.95879507753333371,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,464.90545868541284]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2538,2.4743127582160819E-10,{"$f":"Z2555*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.4489212471665298E-10},{"$f":"AF2554*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2555^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2555)*3600*24","v":0},0,{"$f":"AE2554-AD2555*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2555>$J$18,(AE2555/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.4489212471665298E-10,{"$error":"#N/A"},null,{"$f":"(AD2555)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2555>0,(AJ2555*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2554,NA())","v":{"$error":"#N/A"}},null,2538,{"$f":"IF(AF2555<=$J$9*0.05,AS2554*EXP((-$J$6*1)/Heterogenität!$D$4),Z2555)","v":4.5847742131237268E-4},{"$f":"IF(OR(AF2555>=$J$19, AR2554/$J$5<AN2555),0, Bodencharakterisierung!$E$8*$J$11*((AR2554/$J$5)-AN2555))","v":1.9923034499271629E-5},4.7536990104082855E-6,{"$f":"AQ2554-AP2555*Bodencharakterisierung!$E$8","v":1.4357863088395987E-3},{"$f":"AQ2555/(Bodencharakterisierung!$E$11*1000)","v":9.4771373520765595E-7},4.6323112032278096E-4,2538,null,{"$f":"(AP2555)*$G$11*Bodencharakterisierung!$E$8","v":6.8742761689875925E-8},{"$f":"IF(AF2555<=$J$9*1.05,(AV2555*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2554,NA())","v":{"$error":"#N/A"}},453.8926470992489,2671,20.91994895232008,1.6399886323194495,0,15.919960320000632,null,0.94771373520765601,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,458.47742131237266]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2545,2.3019514923361811E-10,{"$f":"Z2562*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.2783287605052511E-10},{"$f":"AF2561*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2562^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2562)*3600*24","v":0},0,{"$f":"AE2561-AD2562*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2562>$J$18,(AE2562/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.2783287605052511E-10,{"$error":"#N/A"},null,{"$f":"(AD2562)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2562>0,(AJ2562*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2561,NA())","v":{"$error":"#N/A"}},null,2545,{"$f":"IF(AF2562<=$J$9*0.05,AS2561*EXP((-$J$6*1)/Heterogenität!$D$4),Z2562)","v":4.5404456545566625E-4},{"$f":"IF(OR(AF2562>=$J$19, AR2561/$J$5<AN2562),0, Bodencharakterisierung!$E$8*$J$11*((AR2561/$J$5)-AN2562))","v":3.358481017912213E-5},4.7077371777863239E-6,{"$f":"AQ2561-AP2562*Bodencharakterisierung!$E$8","v":1.4263287761773298E-3},{"$f":"AQ2562/(Bodencharakterisierung!$E$11*1000)","v":9.4147113939097678E-7},4.5875230263345257E-4,2545,null,{"$f":"(AP2562)*$G$11*Bodencharakterisierung!$E$8","v":6.8078112266375694E-8},{"$f":"IF(AF2562<=$J$9*1.05,(AV2562*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2561,NA())","v":{"$error":"#N/A"}},449.5041198011096,2678,20.963857432320086,1.6399886323194495,0,15.963868800000636,null,0.94147113939097682,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,454.04456545566626]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2548,2.2318080618169628E-10,{"$f":"Z2565*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.2089051450882943E-10},{"$f":"AF2564*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2565^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2565)*3600*24","v":0},0,{"$f":"AE2564-AD2565*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2565>$J$18,(AE2565/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.2089051450882943E-10,{"$error":"#N/A"},null,{"$f":"(AD2565)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2565>0,(AJ2565*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2564,NA())","v":{"$error":"#N/A"}},null,2548,{"$f":"IF(AF2565<=$J$9*0.05,AS2564*EXP((-$J$6*1)/Heterogenität!$D$4),Z2565)","v":4.5404456545566625E-4},{"$f":"IF(OR(AF2565>=$J$19, AR2564/$J$5<AN2565),0, Bodencharakterisierung!$E$8*$J$11*((AR2564/$J$5)-AN2565))","v":1.8991173572773201E-5},4.7077371777863239E-6,{"$f":"AQ2564-AP2565*Bodencharakterisierung!$E$8","v":1.4216681163713215E-3},{"$f":"AQ2565/(Bodencharakterisierung!$E$11*1000)","v":9.3839479628470065E-7},4.5875230263345257E-4,2548,null,{"$f":"(AP2565)*$G$11*Bodencharakterisierung!$E$8","v":6.8078112266375694E-8},{"$f":"IF(AF2565<=$J$9*1.05,(AV2565*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2564,NA())","v":{"$error":"#N/A"}},449.5041198011096,2681,20.982675352320086,1.6399886323194495,0,15.982686720000638,null,0.93839479628470068,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,454.04456545566626]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2562,1.9317013733972469E-10,{"$f":"Z2579*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.9118781652744328E-10},{"$f":"AF2578*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2579^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2579)*3600*24","v":0},0,{"$f":"AE2578-AD2579*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2579>$J$18,(AE2579/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.9118781652744328E-10,{"$error":"#N/A"},null,{"$f":"(AD2579)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2579>0,(AJ2579*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2578,NA())","v":{"$error":"#N/A"}},null,2562,{"$f":"IF(AF2579<=$J$9*0.05,AS2578*EXP((-$J$6*1)/Heterogenität!$D$4),Z2579)","v":4.4817368110459862E-4},{"$f":"IF(OR(AF2579>=$J$19, AR2578/$J$5<AN2579),0, Bodencharakterisierung!$E$8*$J$11*((AR2578/$J$5)-AN2579))","v":1.469577057510921E-5},4.646865222412836E-6,{"$f":"AQ2578-AP2579*Bodencharakterisierung!$E$8","v":1.4019923037172947E-3},{"$f":"AQ2579/(Bodencharakterisierung!$E$11*1000)","v":9.2540746119953441E-7},4.5282054632701145E-4,2562,null,{"$f":"(AP2579)*$G$11*Bodencharakterisierung!$E$8","v":6.7197849062358273E-8},{"$f":"IF(AF2579<=$J$9*1.05,(AV2579*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2578,NA())","v":{"$error":"#N/A"}},443.69194429355264,2695,21.070492312320077,1.6399886323194495,0,16.070503680000627,null,0.92540746119953443,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,448.17368110459864]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2566,{"$f":"AG2582","v":1.8536207720610606E-10},{"$f":"Z2583*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.8345988306515996E-10},{"$f":"AF2582*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2583^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2583)*3600*24","v":0},{"$f":"MIN(AC2583,Z2583-AA2583)","v":0},{"$f":"AE2582-AD2583*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2583>$J$18,(AE2583/(Bodencharakterisierung!$E$11*1000)),0)","v":0},{"$f":"AA2583+AD2583","v":1.8345988306515996E-10},{"$f":"IF(AD2583>0,Y2583,NA())","v":{"$error":"#N/A"}},null,{"$f":"(AD2583)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2583>0,(AJ2583*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2582,NA())","v":{"$error":"#N/A"}},null,2566,{"$f":"IF(AF2583<=$J$9*0.05,AS2582*EXP((-$J$6*1)/Heterogenität!$D$4),Z2583)","v":4.4386235021198653E-4},{"$f":"IF(OR(AF2583>=$J$19, AR2582/$J$5<AN2583),0, Bodencharakterisierung!$E$8*$J$11*((AR2582/$J$5)-AN2583))","v":4.2125685713223935E-5},{"$f":"MIN(AO2583,AS2582-AN2583)","v":4.6021634149844871E-6},{"$f":"AQ2582-AP2583*Bodencharakterisierung!$E$8","v":1.3973106840111744E-3},{"$f":"AQ2583/(Bodencharakterisierung!$E$11*1000)","v":9.2231728317569269E-7},{"$f":"AN2583+AP2583","v":4.4846451362697101E-4},{"$f":"IF(AN2583>$G$5,AM2583,NA())","v":2566},null,{"$f":"(AP2583)*$G$11*Bodencharakterisierung!$E$8","v":6.655142073603272E-8},{"$f":"IF(AF2583<=$J$9*1.05,(AV2583*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2582,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH2583>($G$5*10^6),BH2583*0.99,9999)","v":439.42372670986668},{"$f":"AT2583+$G$3","v":2699},{"$f":"IF(ISNUMBER(AT2583),BA2583+BB2583+BC2583+$AZ$17,\"\")","v":21.095582872320072},{"$f":"IF(ISNUMBER(AK2583),AK2583,BA2582)","v":1.6399886323194495},{"$f":"IF(ISNUMBER(AW2583),AW2583,0)","v":0},16.095594240000622,null,{"$f":"AR2583*10^6","v":0.92231728317569273},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF2583*10^6","v":0},{"$f":"AN2583*10^6","v":443.86235021198655}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2578,1.6378102496310962E-10,{"$f":"Z2595*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.6210029657044834E-10},{"$f":"AF2594*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2595^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2595)*3600*24","v":0},0,{"$f":"AE2594-AD2595*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2595>$J$18,(AE2595/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.6210029657044834E-10,{"$error":"#N/A"},null,{"$f":"(AD2595)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2595>0,(AJ2595*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2594,NA())","v":{"$error":"#N/A"}},null,2578,{"$f":"IF(AF2595<=$J$9*0.05,AS2594*EXP((-$J$6*1)/Heterogenität!$D$4),Z2595)","v":4.389415727464929E-4},{"$f":"IF(OR(AF2595>=$J$19, AR2594/$J$5<AN2595),0, Bodencharakterisierung!$E$8*$J$11*((AR2594/$J$5)-AN2595))","v":3.8352974014893705E-5},4.5511425928440987E-6,{"$f":"AQ2594-AP2595*Bodencharakterisierung!$E$8","v":1.3807640068104325E-3},{"$f":"AQ2595/(Bodencharakterisierung!$E$11*1000)","v":9.1139538403328877E-7},4.43492715339337E-4,2578,null,{"$f":"(AP2595)*$G$11*Bodencharakterisierung!$E$8","v":6.5813613775613269E-8},{"$f":"IF(AF2595<=$J$9*1.05,(AV2595*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2594,NA())","v":{"$error":"#N/A"}},434.55215701902796,2711,21.170854552320058,1.6399886323194495,0,16.170865920000608,null,0.91139538403328879,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,438.94157274649291]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2585,1.5237199645771489E-10,{"$f":"Z2602*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.5080834803903729E-10},{"$f":"AF2601*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2602^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2602)*3600*24","v":0},0,{"$f":"AE2601-AD2602*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2602>$J$18,(AE2602/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.5080834803903729E-10,{"$error":"#N/A"},null,{"$f":"(AD2602)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2602>0,(AJ2602*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2601,NA())","v":{"$error":"#N/A"}},null,2585,{"$f":"IF(AF2602<=$J$9*0.05,AS2601*EXP((-$J$6*1)/Heterogenität!$D$4),Z2602)","v":4.389415727464929E-4},{"$f":"IF(OR(AF2602>=$J$19, AR2601/$J$5<AN2602),0, Bodencharakterisierung!$E$8*$J$11*((AR2601/$J$5)-AN2602))","v":5.4338290380341922E-6},4.5511425928440987E-6,{"$f":"AQ2601-AP2602*Bodencharakterisierung!$E$8","v":1.3702508674209629E-3},{"$f":"AQ2602/(Bodencharakterisierung!$E$11*1000)","v":9.0445601809964548E-7},4.43492715339337E-4,2585,null,{"$f":"(AP2602)*$G$11*Bodencharakterisierung!$E$8","v":6.5813613775613269E-8},{"$f":"IF(AF2602<=$J$9*1.05,(AV2602*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2601,NA())","v":{"$error":"#N/A"}},434.55215701902796,2718,21.21476303232005,1.6399886323194495,0,16.2147744000006,null,0.90445601809964549,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,438.94157274649291]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2593,1.4030299955916053E-10,{"$f":"Z2610*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.3886320374039739E-10},{"$f":"AF2609*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2610^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2610)*3600*24","v":0},0,{"$f":"AE2609-AD2610*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2610>$J$18,(AE2610/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.3886320374039739E-10,{"$error":"#N/A"},null,{"$f":"(AD2610)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2610>0,(AJ2610*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2609,NA())","v":{"$error":"#N/A"}},null,2593,{"$f":"IF(AF2610<=$J$9*0.05,AS2609*EXP((-$J$6*1)/Heterogenität!$D$4),Z2610)","v":4.3516072570849344E-4},{"$f":"IF(OR(AF2610>=$J$19, AR2609/$J$5<AN2610),0, Bodencharakterisierung!$E$8*$J$11*((AR2609/$J$5)-AN2610))","v":8.9531455062041303E-6},4.5119410793396843E-6,{"$f":"AQ2609-AP2610*Bodencharakterisierung!$E$8","v":1.3595870224940468E-3},{"$f":"AQ2610/(Bodencharakterisierung!$E$11*1000)","v":8.9741717656372724E-7},4.3967266678783312E-4,2593,null,{"$f":"(AP2610)*$G$11*Bodencharakterisierung!$E$8","v":6.524672464468258E-8},{"$f":"IF(AF2610<=$J$9*1.05,(AV2610*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2609,NA())","v":{"$error":"#N/A"}},430.80911845140849,2726,21.264944152320041,1.6399886323194495,0,16.264955520000591,null,0.89741717656372721,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,435.16072570849343]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2603,1.2655205550449282E-10,{"$f":"Z2620*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.252533725045302E-10},{"$f":"AF2619*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2620^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2620)*3600*24","v":0},0,{"$f":"AE2619-AD2620*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2620>$J$18,(AE2620/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.252533725045302E-10,{"$error":"#N/A"},null,{"$f":"(AD2620)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2620>0,(AJ2620*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2619,NA())","v":{"$error":"#N/A"}},null,2603,{"$f":"IF(AF2620<=$J$9*0.05,AS2619*EXP((-$J$6*1)/Heterogenität!$D$4),Z2620)","v":4.2909556846704752E-4},{"$f":"IF(OR(AF2620>=$J$19, AR2619/$J$5<AN2620),0, Bodencharakterisierung!$E$8*$J$11*((AR2619/$J$5)-AN2620))","v":2.8180223666758012E-5},4.4490548157280312E-6,{"$f":"AQ2619-AP2620*Bodencharakterisierung!$E$8","v":1.3468177107779915E-3},{"$f":"AQ2620/(Bodencharakterisierung!$E$11*1000)","v":8.8898858797227162E-7},4.3354462328277555E-4,2603,null,{"$f":"(AP2620)*$G$11*Bodencharakterisierung!$E$8","v":6.4337332732498544E-8},{"$f":"IF(AF2620<=$J$9*1.05,(AV2620*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2619,NA())","v":{"$error":"#N/A"}},424.80461278237703,2736,21.327670552320029,1.6399886323194495,0,16.327681920000579,null,0.88898858797227165,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,429.09556846704754]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2615,1.1181804646409845E-10,{"$f":"Z2632*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.1067056454092414E-10},{"$f":"AF2631*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2632^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2632)*3600*24","v":0},0,{"$f":"AE2631-AD2632*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2632>$J$18,(AE2632/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.1067056454092414E-10,{"$error":"#N/A"},null,{"$f":"(AD2632)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2632>0,(AJ2632*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2631,NA())","v":{"$error":"#N/A"}},null,2615,{"$f":"IF(AF2632<=$J$9*0.05,AS2631*EXP((-$J$6*1)/Heterogenität!$D$4),Z2632)","v":4.2528278903805345E-4},{"$f":"IF(OR(AF2632>=$J$19, AR2631/$J$5<AN2632),0, Bodencharakterisierung!$E$8*$J$11*((AR2631/$J$5)-AN2632))","v":1.4461080509840349E-5},4.4095222129084187E-6,{"$f":"AQ2631-AP2632*Bodencharakterisierung!$E$8","v":1.33054899123179E-3},{"$f":"AQ2632/(Bodencharakterisierung!$E$11*1000)","v":8.7825015922890426E-7},4.2969231125096187E-4,2615,null,{"$f":"(AP2632)*$G$11*Bodencharakterisierung!$E$8","v":6.3765655752391265E-8},{"$f":"IF(AF2632<=$J$9*1.05,(AV2632*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2631,NA())","v":{"$error":"#N/A"}},421.02996114767291,2748,21.402942232320015,1.6399886323194495,0,16.402953600000565,null,0.87825015922890426,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,425.28278903805347]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2618,1.0841080639016043E-10,{"$f":"Z2635*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.0729828972095356E-10},{"$f":"AF2634*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2635^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2635)*3600*24","v":0},0,{"$f":"AE2634-AD2635*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2635>$J$18,(AE2635/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.0729828972095356E-10,{"$error":"#N/A"},null,{"$f":"(AD2635)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2635>0,(AJ2635*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2634,NA())","v":{"$error":"#N/A"}},null,2618,{"$f":"IF(AF2635<=$J$9*0.05,AS2634*EXP((-$J$6*1)/Heterogenität!$D$4),Z2635)","v":4.2528278903805345E-4},{"$f":"IF(OR(AF2635>=$J$19, AR2634/$J$5<AN2635),0, Bodencharakterisierung!$E$8*$J$11*((AR2634/$J$5)-AN2635))","v":7.9188820945983766E-7},7.9188820945983766E-7,{"$f":"AQ2634-AP2635*Bodencharakterisierung!$E$8","v":1.3273773834621486E-3},{"$f":"AQ2635/(Bodencharakterisierung!$E$11*1000)","v":8.761566887538934E-7},4.2607467724751331E-4,2618,null,{"$f":"(AP2635)*$G$11*Bodencharakterisierung!$E$8","v":1.1451415486914626E-8},{"$f":"IF(AF2635<=$J$9*1.05,(AV2635*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2634,NA())","v":{"$error":"#N/A"}},421.02996114767291,2751,21.421760152320012,1.6399886323194495,0,16.421771520000561,null,0.87615668875389341,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,425.28278903805347]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2634,9.1917069750958503E-11,{"$f":"Z2651*EXP((-$J$6/Heterogenität!$D$4)*1)","v":9.0973812563897541E-11},{"$f":"AF2650*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2651^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2651)*3600*24","v":0},0,{"$f":"AE2650-AD2651*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2651>$J$18,(AE2651/(Bodencharakterisierung!$E$11*1000)),0)","v":0},9.0973812563897541E-11,{"$error":"#N/A"},null,{"$f":"(AD2651)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2651>0,(AJ2651*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2650,NA())","v":{"$error":"#N/A"}},null,2634,{"$f":"IF(AF2651<=$J$9*0.05,AS2650*EXP((-$J$6*1)/Heterogenität!$D$4),Z2651)","v":4.1721283605574875E-4},{"$f":"IF(OR(AF2651>=$J$19, AR2650/$J$5<AN2651),0, Bodencharakterisierung!$E$8*$J$11*((AR2650/$J$5)-AN2651))","v":1.5984411870250563E-5},4.3258493301823121E-6,{"$f":"AQ2650-AP2651*Bodencharakterisierung!$E$8","v":1.305875290575363E-3},{"$f":"AQ2651/(Bodencharakterisierung!$E$11*1000)","v":8.6196388816855643E-7},4.2153868538593106E-4,2634,null,{"$f":"(AP2651)*$G$11*Bodencharakterisierung!$E$8","v":6.2555670638787768E-8},{"$f":"IF(AF2651<=$J$9*1.05,(AV2651*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2650,NA())","v":{"$error":"#N/A"}},413.04070769519126,2767,21.522122392319993,1.6399886323194495,0,16.522133760000543,null,0.8619638881685564,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,417.21283605574877]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2642,8.4636553281146514E-11,{"$f":"Z2659*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.3768009088138479E-11},{"$f":"AF2658*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2659^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2659)*3600*24","v":0},0,{"$f":"AE2658-AD2659*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2659>$J$18,(AE2659/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.3768009088138479E-11,{"$error":"#N/A"},null,{"$f":"(AD2659)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2659>0,(AJ2659*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2658,NA())","v":{"$error":"#N/A"}},null,2642,{"$f":"IF(AF2659<=$J$9*0.05,AS2658*EXP((-$J$6*1)/Heterogenität!$D$4),Z2659)","v":4.1467974125392423E-4},{"$f":"IF(OR(AF2659>=$J$19, AR2658/$J$5<AN2659),0, Bodencharakterisierung!$E$8*$J$11*((AR2658/$J$5)-AN2659))","v":7.7001676158494338E-6},4.2995850700618772E-6,{"$f":"AQ2658-AP2659*Bodencharakterisierung!$E$8","v":1.295332026298603E-3},{"$f":"AQ2659/(Bodencharakterisierung!$E$11*1000)","v":8.5500463782086011E-7},4.189793263239861E-4,2642,null,{"$f":"(AP2659)*$G$11*Bodencharakterisierung!$E$8","v":6.2175865823534043E-8},{"$f":"IF(AF2659<=$J$9*1.05,(AV2659*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2658,NA())","v":{"$error":"#N/A"}},410.53294384138502,2775,21.572303512319984,1.6399886323194495,0,16.572314880000533,null,0.85500463782086011,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,414.67974125392425]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2648,7.9557168429629508E-11,{"$f":"Z2665*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.8740749117016631E-11},{"$f":"AF2664*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2665^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2665)*3600*24","v":0},0,{"$f":"AE2664-AD2665*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2665>$J$18,(AE2665/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.8740749117016631E-11,{"$error":"#N/A"},null,{"$f":"(AD2665)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2665>0,(AJ2665*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2664,NA())","v":{"$error":"#N/A"}},null,2648,{"$f":"IF(AF2665<=$J$9*0.05,AS2664*EXP((-$J$6*1)/Heterogenität!$D$4),Z2665)","v":4.1050119534032163E-4},{"$f":"IF(OR(AF2665>=$J$19, AR2664/$J$5<AN2665),0, Bodencharakterisierung!$E$8*$J$11*((AR2664/$J$5)-AN2665))","v":2.6321438121980123E-5},4.2562600366991043E-6,{"$f":"AQ2664-AP2665*Bodencharakterisierung!$E$8","v":1.2882512481089798E-3},{"$f":"AQ2665/(Bodencharakterisierung!$E$11*1000)","v":8.5033085683761039E-7},4.1475745537702073E-4,2648,null,{"$f":"(AP2665)*$G$11*Bodencharakterisierung!$E$8","v":6.1549346888039376E-8},{"$f":"IF(AF2665<=$J$9*1.05,(AV2665*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2664,NA())","v":{"$error":"#N/A"}},406.39618338691838,2781,21.609939352319977,1.6399886323194495,0,16.609950720000526,null,0.85033085683761045,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,410.5011953403216]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2655,7.401519552631802E-11,{"$f":"Z2672*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.3255648193911966E-11},{"$f":"AF2671*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2672^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2672)*3600*24","v":0},0,{"$f":"AE2671-AD2672*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2672>$J$18,(AE2672/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.3255648193911966E-11,{"$error":"#N/A"},null,{"$f":"(AD2672)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2672>0,(AJ2672*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2671,NA())","v":{"$error":"#N/A"}},null,2655,{"$f":"IF(AF2672<=$J$9*0.05,AS2671*EXP((-$J$6*1)/Heterogenität!$D$4),Z2672)","v":4.0628861323940195E-4},{"$f":"IF(OR(AF2672>=$J$19, AR2671/$J$5<AN2672),0, Bodencharakterisierung!$E$8*$J$11*((AR2671/$J$5)-AN2672))","v":4.1103540462290613E-5},4.2125821009196779E-6,{"$f":"AQ2671-AP2672*Bodencharakterisierung!$E$8","v":1.2798382669551229E-3},{"$f":"AQ2672/(Bodencharakterisierung!$E$11*1000)","v":8.4477773396377744E-7},4.1050119534032163E-4,2655,null,{"$f":"(AP2672)*$G$11*Bodencharakterisierung!$E$8","v":6.0917724666309159E-8},{"$f":"IF(AF2672<=$J$9*1.05,(AV2672*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2671,NA())","v":{"$error":"#N/A"}},402.22572710700797,2788,21.653847832319968,1.6399886323194495,0,16.653859200000518,null,0.84477773396377742,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,406.28861323940197]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2667,6.5397867615965644E-11,{"$f":"Z2684*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.4726751697950028E-11},{"$f":"AF2683*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2684^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2684)*3600*24","v":0},0,{"$f":"AE2683-AD2684*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2684>$J$18,(AE2684/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.4726751697950028E-11,{"$error":"#N/A"},null,{"$f":"(AD2684)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2684>0,(AJ2684*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2683,NA())","v":{"$error":"#N/A"}},null,2667,{"$f":"IF(AF2684<=$J$9*0.05,AS2683*EXP((-$J$6*1)/Heterogenität!$D$4),Z2684)","v":4.0402694398487804E-4},{"$f":"IF(OR(AF2684>=$J$19, AR2683/$J$5<AN2684),0, Bodencharakterisierung!$E$8*$J$11*((AR2683/$J$5)-AN2684))","v":1.3382145759808523E-5},4.1891321022996227E-6,{"$f":"AQ2683-AP2684*Bodencharakterisierung!$E$8","v":1.2639337466876528E-3},{"$f":"AQ2684/(Bodencharakterisierung!$E$11*1000)","v":8.3427970078392926E-7},4.0821607608717767E-4,2667,null,{"$f":"(AP2684)*$G$11*Bodencharakterisierung!$E$8","v":6.0578616602623006E-8},{"$f":"IF(AF2684<=$J$9*1.05,(AV2684*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2683,NA())","v":{"$error":"#N/A"}},399.98667454502925,2800,21.729119512319954,1.6399886323194495,0,16.729130880000504,null,0.83427970078392921,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,404.02694398487802]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2674,6.0842235264839242E-11,{"$f":"Z2691*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.0217869455029306E-11},{"$f":"AF2690*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2691^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2691)*3600*24","v":0},0,{"$f":"AE2690-AD2691*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2691>$J$18,(AE2691/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.0217869455029306E-11,{"$error":"#N/A"},null,{"$f":"(AD2691)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2691>0,(AJ2691*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2690,NA())","v":{"$error":"#N/A"}},null,2674,{"$f":"IF(AF2691<=$J$9*0.05,AS2690*EXP((-$J$6*1)/Heterogenität!$D$4),Z2691)","v":4.0027288215575683E-4},{"$f":"IF(OR(AF2691>=$J$19, AR2690/$J$5<AN2691),0, Bodencharakterisierung!$E$8*$J$11*((AR2690/$J$5)-AN2691))","v":2.3810553734344043E-5},4.150208309823566E-6,{"$f":"AQ2690-AP2691*Bodencharakterisierung!$E$8","v":1.2555599161925357E-3},{"$f":"AQ2691/(Bodencharakterisierung!$E$11*1000)","v":8.2875241992906649E-7},4.0442309046558039E-4,2674,null,{"$f":"(AP2691)*$G$11*Bodencharakterisierung!$E$8","v":6.0015743567458335E-8},{"$f":"IF(AF2691<=$J$9*1.05,(AV2691*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2690,NA())","v":{"$error":"#N/A"}},396.27015333419922,2807,21.773027992319946,1.6399886323194495,0,16.773039360000496,null,0.82875241992906645,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,400.2728821557568]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2683,5.5448165726089914E-11,{"$f":"Z2700*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.4879154105373664E-11},{"$f":"AF2699*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2700^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2700)*3600*24","v":0},0,{"$f":"AE2699-AD2700*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2700>$J$18,(AE2700/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.4879154105373664E-11,{"$error":"#N/A"},null,{"$f":"(AD2700)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2700>0,(AJ2700*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2699,NA())","v":{"$error":"#N/A"}},null,2683,{"$f":"IF(AF2700<=$J$9*0.05,AS2699*EXP((-$J$6*1)/Heterogenität!$D$4),Z2700)","v":3.985092826934025E-4},{"$f":"IF(OR(AF2700>=$J$19, AR2699/$J$5<AN2700),0, Bodencharakterisierung!$E$8*$J$11*((AR2699/$J$5)-AN2700))","v":4.3484192176362034E-6},4.1319225216271687E-6,{"$f":"AQ2699-AP2700*Bodencharakterisierung!$E$8","v":1.2438459568854608E-3},{"$f":"AQ2700/(Bodencharakterisierung!$E$11*1000)","v":8.210204335877629E-7},4.0264120521502967E-4,2683,null,{"$f":"(AP2700)*$G$11*Bodencharakterisierung!$E$8","v":5.9751314629584017E-8},{"$f":"IF(AF2700<=$J$9*1.05,(AV2700*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2699,NA())","v":{"$error":"#N/A"}},394.52418986646848,2816,21.829481752319936,1.6399886323194495,0,16.829493120000485,null,0.82102043358776289,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,398.5092826934025]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2688,5.2660903700636997E-11,{"$f":"Z2705*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.2120495090709212E-11},{"$f":"AF2704*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2705^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2705)*3600*24","v":0},0,{"$f":"AE2704-AD2705*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2705>$J$18,(AE2705/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.2120495090709212E-11,{"$error":"#N/A"},null,{"$f":"(AD2705)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2705>0,(AJ2705*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2704,NA())","v":{"$error":"#N/A"}},null,2688,{"$f":"IF(AF2705<=$J$9*0.05,AS2704*EXP((-$J$6*1)/Heterogenität!$D$4),Z2705)","v":3.9449782074948324E-4},{"$f":"IF(OR(AF2705>=$J$19, AR2704/$J$5<AN2705),0, Bodencharakterisierung!$E$8*$J$11*((AR2704/$J$5)-AN2705))","v":2.6522355793062694E-5},4.090329889609441E-6,{"$f":"AQ2704-AP2705*Bodencharakterisierung!$E$8","v":1.2384206950090987E-3},{"$f":"AQ2705/(Bodencharakterisierung!$E$11*1000)","v":8.1743940264626983E-7},3.9858815063909268E-4,2688,null,{"$f":"(AP2705)*$G$11*Bodencharakterisierung!$E$8","v":5.9149847775122025E-8},{"$f":"IF(AF2705<=$J$9*1.05,(AV2705*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2704,NA())","v":{"$error":"#N/A"}},390.55284254198841,2821,21.86084495231993,1.6399886323194495,0,16.86085632000048,null,0.8174394026462698,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,394.49782074948325]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2704,4.4649017194648294E-11,{"$f":"Z2721*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.4190826931640906E-11},{"$f":"AF2720*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2721^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2721)*3600*24","v":0},0,{"$f":"AE2720-AD2721*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2721>$J$18,(AE2721/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.4190826931640906E-11,{"$error":"#N/A"},null,{"$f":"(AD2721)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2721>0,(AJ2721*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2720,NA())","v":{"$error":"#N/A"}},null,2704,{"$f":"IF(AF2721<=$J$9*0.05,AS2720*EXP((-$J$6*1)/Heterogenität!$D$4),Z2721)","v":3.9065455825266219E-4},{"$f":"IF(OR(AF2721>=$J$19, AR2720/$J$5<AN2721),0, Bodencharakterisierung!$E$8*$J$11*((AR2720/$J$5)-AN2721))","v":7.7014194527759721E-7},7.7014194527759721E-7,{"$f":"AQ2720-AP2721*Bodencharakterisierung!$E$8","v":1.2192965373087744E-3},{"$f":"AQ2721/(Bodencharakterisierung!$E$11*1000)","v":8.0481619624341545E-7},3.914247001979398E-4,2704,null,{"$f":"(AP2721)*$G$11*Bodencharakterisierung!$E$8","v":1.1136944955008475E-8},{"$f":"IF(AF2721<=$J$9*1.05,(AV2721*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2720,NA())","v":{"$error":"#N/A"}},386.74801267013555,2837,21.961207192319911,1.6399886323194495,0,16.961218560000461,null,0.80481619624341549,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,390.65455825266218]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2707,4.328850406230344E-11,{"$f":"Z2724*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.2844275447482316E-11},{"$f":"AF2723*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2724^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2724)*3600*24","v":0},0,{"$f":"AE2723-AD2724*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2724>$J$18,(AE2724/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.2844275447482316E-11,{"$error":"#N/A"},null,{"$f":"(AD2724)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2724>0,(AJ2724*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2723,NA())","v":{"$error":"#N/A"}},null,2707,{"$f":"IF(AF2724<=$J$9*0.05,AS2723*EXP((-$J$6*1)/Heterogenität!$D$4),Z2724)","v":3.8740788196542608E-4},{"$f":"IF(OR(AF2724>=$J$19, AR2723/$J$5<AN2724),0, Bodencharakterisierung!$E$8*$J$11*((AR2723/$J$5)-AN2724))","v":2.3403443292697928E-5},4.0168182325137232E-6,{"$f":"AQ2723-AP2724*Bodencharakterisierung!$E$8","v":1.2153198872585857E-3},{"$f":"AQ2724/(Bodencharakterisierung!$E$11*1000)","v":8.0219134472513905E-7},3.914247001979398E-4,2707,null,{"$f":"(AP2724)*$G$11*Bodencharakterisierung!$E$8","v":5.8086803119982034E-8},{"$f":"IF(AF2724<=$J$9*1.05,(AV2724*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2723,NA())","v":{"$error":"#N/A"}},383.53380314577186,2840,21.980025112319908,1.6399886323194495,0,16.980036480000457,null,0.80219134472513909,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,387.4078819654261]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2722,3.7083092914689521E-11,{"$f":"Z2739*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.6702544513777674E-11},{"$f":"AF2738*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2739^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2739)*3600*24","v":0},0,{"$f":"AE2738-AD2739*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2739>$J$18,(AE2739/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.6702544513777674E-11,{"$error":"#N/A"},null,{"$f":"(AD2739)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2739>0,(AJ2739*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2738,NA())","v":{"$error":"#N/A"}},null,2722,{"$f":"IF(AF2739<=$J$9*0.05,AS2738*EXP((-$J$6*1)/Heterogenität!$D$4),Z2739)","v":3.8280710572343498E-4},{"$f":"IF(OR(AF2739>=$J$19, AR2738/$J$5<AN2739),0, Bodencharakterisierung!$E$8*$J$11*((AR2738/$J$5)-AN2739))","v":1.1216150832392204E-5},3.969115326215634E-6,{"$f":"AQ2738-AP2739*Bodencharakterisierung!$E$8","v":1.1970835965415916E-3},{"$f":"AQ2739/(Bodencharakterisierung!$E$11*1000)","v":7.9015418913636407E-7},3.8677622104965061E-4,2722,null,{"$f":"(AP2739)*$G$11*Bodencharakterisierung!$E$8","v":5.7396976205744488E-8},{"$f":"IF(AF2739<=$J$9*1.05,(AV2739*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2738,NA())","v":{"$error":"#N/A"}},378.97903466620062,2855,22.07411471231989,1.6399886323194495,0,17.07412608000044,null,0.79015418913636404,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,382.80710572343497]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2725,3.5953123252010211E-11,{"$f":"Z2742*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.5584170651621277E-11},{"$f":"AF2741*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2742^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2742)*3600*24","v":0},0,{"$f":"AE2741-AD2742*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2742>$J$18,(AE2742/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.5584170651621277E-11,{"$error":"#N/A"},null,{"$f":"(AD2742)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2742>0,(AJ2742*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2741,NA())","v":{"$error":"#N/A"}},null,2725,{"$f":"IF(AF2742<=$J$9*0.05,AS2741*EXP((-$J$6*1)/Heterogenität!$D$4),Z2742)","v":3.8186130533303674E-4},{"$f":"IF(OR(AF2742>=$J$19, AR2741/$J$5<AN2742),0, Bodencharakterisierung!$E$8*$J$11*((AR2741/$J$5)-AN2742))","v":9.1430928154206752E-6},3.9593088446510192E-6,{"$f":"AQ2741-AP2742*Bodencharakterisierung!$E$8","v":1.1934727587753022E-3},{"$f":"AQ2742/(Bodencharakterisierung!$E$11*1000)","v":7.8777079787148663E-7},3.8582061417768775E-4,2725,null,{"$f":"(AP2742)*$G$11*Bodencharakterisierung!$E$8","v":5.725516566541863E-8},{"$f":"IF(AF2742<=$J$9*1.05,(AV2742*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2741,NA())","v":{"$error":"#N/A"}},378.04269227970639,2858,22.092932632319886,1.6399886323194495,0,17.092944000000436,null,0.78777079787148663,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,381.86130533303674]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2737,3.1767228041428455E-11,{"$f":"Z2754*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.1441231289744919E-11},{"$f":"AF2753*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2754^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2754)*3600*24","v":0},0,{"$f":"AE2753-AD2754*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2754>$J$18,(AE2754/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.1441231289744919E-11,{"$error":"#N/A"},null,{"$f":"(AD2754)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2754>0,(AJ2754*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2753,NA())","v":{"$error":"#N/A"}},null,2737,{"$f":"IF(AF2754<=$J$9*0.05,AS2753*EXP((-$J$6*1)/Heterogenität!$D$4),Z2754)","v":3.7555681989506534E-4},{"$f":"IF(OR(AF2754>=$J$19, AR2753/$J$5<AN2754),0, Bodencharakterisierung!$E$8*$J$11*((AR2753/$J$5)-AN2754))","v":2.8567591279074452E-5},3.8939411192310332E-6,{"$f":"AQ2753-AP2754*Bodencharakterisierung!$E$8","v":1.1800203272557196E-3},{"$f":"AQ2754/(Bodencharakterisierung!$E$11*1000)","v":7.7889130511928689E-7},3.7945076101429637E-4,2737,null,{"$f":"(AP2754)*$G$11*Bodencharakterisierung!$E$8","v":5.6309889584430612E-8},{"$f":"IF(AF2754<=$J$9*1.05,(AV2754*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2753,NA())","v":{"$error":"#N/A"}},371.80125169611472,2870,22.168204312319872,1.6399886323194495,0,17.168215680000422,null,0.77889130511928684,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,375.55681989506536]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2744,2.9554314730233423E-11,{"$f":"Z2761*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.9251026996480754E-11},{"$f":"AF2760*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2761^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2761)*3600*24","v":0},0,{"$f":"AE2760-AD2761*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2761>$J$18,(AE2761/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.9251026996480754E-11,{"$error":"#N/A"},null,{"$f":"(AD2761)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2761>0,(AJ2761*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2760,NA())","v":{"$error":"#N/A"}},null,2744,{"$f":"IF(AF2761<=$J$9*0.05,AS2760*EXP((-$J$6*1)/Heterogenität!$D$4),Z2761)","v":3.7555681989506534E-4},{"$f":"IF(OR(AF2761>=$J$19, AR2760/$J$5<AN2761),0, Bodencharakterisierung!$E$8*$J$11*((AR2760/$J$5)-AN2761))","v":4.0209006255173512E-7},4.0209006255173512E-7,{"$f":"AQ2760-AP2761*Bodencharakterisierung!$E$8","v":1.1721776341190005E-3},{"$f":"AQ2761/(Bodencharakterisierung!$E$11*1000)","v":7.7371460997953828E-7},3.7595890995761709E-4,2744,null,{"$f":"(AP2761)*$G$11*Bodencharakterisierung!$E$8","v":5.8145838193249897E-9},{"$f":"IF(AF2761<=$J$9*1.05,(AV2761*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2760,NA())","v":{"$error":"#N/A"}},371.80125169611472,2877,22.212112792319864,1.6399886323194495,0,17.212124160000414,null,0.77371460997953834,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,375.55681989506536]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2756,2.6113410205356222E-11,{"$f":"Z2773*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.5845433191711092E-11},{"$f":"AF2772*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2773^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2773)*3600*24","v":0},0,{"$f":"AE2772-AD2773*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2773>$J$18,(AE2773/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.5845433191711092E-11,{"$error":"#N/A"},null,{"$f":"(AD2773)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2773>0,(AJ2773*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2772,NA())","v":{"$error":"#N/A"}},null,2756,{"$f":"IF(AF2773<=$J$9*0.05,AS2772*EXP((-$J$6*1)/Heterogenität!$D$4),Z2773)","v":3.7013302639691452E-4},{"$f":"IF(OR(AF2773>=$J$19, AR2772/$J$5<AN2773),0, Bodencharakterisierung!$E$8*$J$11*((AR2772/$J$5)-AN2773))","v":1.1238058697497483E-5},3.83770480183286E-6,{"$f":"AQ2772-AP2773*Bodencharakterisierung!$E$8","v":1.1575758258326868E-3},{"$f":"AQ2773/(Bodencharakterisierung!$E$11*1000)","v":7.6407645269484277E-7},3.7397073119874738E-4,2756,null,{"$f":"(AP2773)*$G$11*Bodencharakterisierung!$E$8","v":5.5496661873388224E-8},{"$f":"IF(AF2773<=$J$9*1.05,(AV2773*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2772,NA())","v":{"$error":"#N/A"}},366.43169613294538,2889,22.28738447231985,1.6399886323194495,0,17.2873958400004,null,0.76407645269484281,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,370.13302639691454]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2763,2.4294343305066152E-11,{"$f":"Z2780*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.4045033639412991E-11},{"$f":"AF2779*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2780^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2780)*3600*24","v":0},0,{"$f":"AE2779-AD2780*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2780>$J$18,(AE2780/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.4045033639412991E-11,{"$error":"#N/A"},null,{"$f":"(AD2780)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2780>0,(AJ2780*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2779,NA())","v":{"$error":"#N/A"}},null,2763,{"$f":"IF(AF2780<=$J$9*0.05,AS2779*EXP((-$J$6*1)/Heterogenität!$D$4),Z2780)","v":3.6686738112465592E-4},{"$f":"IF(OR(AF2780>=$J$19, AR2779/$J$5<AN2780),0, Bodencharakterisierung!$E$8*$J$11*((AR2779/$J$5)-AN2780))","v":1.888566982059528E-5},3.8038451307183144E-6,{"$f":"AQ2779-AP2780*Bodencharakterisierung!$E$8","v":1.1498366799404228E-3},{"$f":"AQ2780/(Bodencharakterisierung!$E$11*1000)","v":7.5896810557123614E-7},3.7067122625537423E-4,2763,null,{"$f":"(AP2780)*$G$11*Bodencharakterisierung!$E$8","v":5.5007020586207757E-8},{"$f":"IF(AF2780<=$J$9*1.05,(AV2780*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2779,NA())","v":{"$error":"#N/A"}},363.19870731340939,2896,22.331292952319842,1.6399886323194495,0,17.331304320000392,null,0.75896810557123617,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,366.86738112465594]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2774,2.1688406101818885E-11,{"$f":"Z2791*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.1465838683309288E-11},{"$f":"AF2790*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2791^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2791)*3600*24","v":0},0,{"$f":"AE2790-AD2791*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2791>$J$18,(AE2791/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.1465838683309288E-11,{"$error":"#N/A"},null,{"$f":"(AD2791)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2791>0,(AJ2791*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2790,NA())","v":{"$error":"#N/A"}},null,2774,{"$f":"IF(AF2791<=$J$9*0.05,AS2790*EXP((-$J$6*1)/Heterogenität!$D$4),Z2791)","v":3.6461806263144797E-4},{"$f":"IF(OR(AF2791>=$J$19, AR2790/$J$5<AN2791),0, Bodencharakterisierung!$E$8*$J$11*((AR2790/$J$5)-AN2791))","v":9.095140915901906E-8},9.095140915901906E-8,{"$f":"AQ2790-AP2791*Bodencharakterisierung!$E$8","v":1.1380390704720336E-3},{"$f":"AQ2791/(Bodencharakterisierung!$E$11*1000)","v":7.5118090460200239E-7},3.6470901404060701E-4,2774,null,{"$f":"(AP2791)*$G$11*Bodencharakterisierung!$E$8","v":1.3152391498678104E-9},{"$f":"IF(AF2791<=$J$9*1.05,(AV2791*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2790,NA())","v":{"$error":"#N/A"}},360.97188200513347,2907,22.400291992319829,1.6399886323194495,0,17.400303360000379,null,0.75118090460200238,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,364.61806263144797]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2777,2.1027532398988766E-11,{"$f":"Z2794*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.0811746896739371E-11},{"$f":"AF2793*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2794^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2794)*3600*24","v":0},0,{"$f":"AE2793-AD2794*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2794>$J$18,(AE2794/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.0811746896739371E-11,{"$error":"#N/A"},null,{"$f":"(AD2794)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2794>0,(AJ2794*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2793,NA())","v":{"$error":"#N/A"}},null,2777,{"$f":"IF(AF2794<=$J$9*0.05,AS2793*EXP((-$J$6*1)/Heterogenität!$D$4),Z2794)","v":3.609663534051908E-4},{"$f":"IF(OR(AF2794>=$J$19, AR2793/$J$5<AN2794),0, Bodencharakterisierung!$E$8*$J$11*((AR2793/$J$5)-AN2794))","v":2.7951101112787319E-5},3.7426606354162102E-6,{"$f":"AQ2793-AP2794*Bodencharakterisierung!$E$8","v":1.1343338364429717E-3},{"$f":"AQ2794/(Bodencharakterisierung!$E$11*1000)","v":7.4873520557291862E-7},3.6470901404060701E-4,2777,null,{"$f":"(AP2794)*$G$11*Bodencharakterisierung!$E$8","v":5.4122237773821282E-8},{"$f":"IF(AF2794<=$J$9*1.05,(AV2794*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2793,NA())","v":{"$error":"#N/A"}},357.35668987113888,2910,22.419109912319826,1.6399886323194495,0,17.419121280000375,null,0.74873520557291862,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,360.96635340519077]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2793,1.7828381012612905E-11,{"$f":"Z2810*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.7645425348671793E-11},{"$f":"AF2809*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2810^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2810)*3600*24","v":0},0,{"$f":"AE2809-AD2810*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2810>$J$18,(AE2810/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.7645425348671793E-11,{"$error":"#N/A"},null,{"$f":"(AD2810)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2810>0,(AJ2810*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2809,NA())","v":{"$error":"#N/A"}},null,2793,{"$f":"IF(AF2810<=$J$9*0.05,AS2809*EXP((-$J$6*1)/Heterogenität!$D$4),Z2810)","v":3.5525316526075347E-4},{"$f":"IF(OR(AF2810>=$J$19, AR2809/$J$5<AN2810),0, Bodencharakterisierung!$E$8*$J$11*((AR2809/$J$5)-AN2810))","v":2.8117439426825926E-5},3.6834237448606371E-6,{"$f":"AQ2809-AP2810*Bodencharakterisierung!$E$8","v":1.1165745958012291E-3},{"$f":"AQ2810/(Bodencharakterisierung!$E$11*1000)","v":7.3701293452226337E-7},3.5893658900561411E-4,2793,null,{"$f":"(AP2810)*$G$11*Bodencharakterisierung!$E$8","v":5.3265619077140002E-8},{"$f":"IF(AF2810<=$J$9*1.05,(AV2810*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2809,NA())","v":{"$error":"#N/A"}},351.70063360814595,2926,22.519472152319807,1.6399886323194495,0,17.519483520000357,null,0.73701293452226335,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,355.25316526075346]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2794,1.7645425348671793E-11,{"$f":"Z2811*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.7464347184148291E-11},{"$f":"AF2810*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2811^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2811)*3600*24","v":0},0,{"$f":"AE2810-AD2811*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2811>$J$18,(AE2811/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.7464347184148291E-11,{"$error":"#N/A"},null,{"$f":"(AD2811)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2811>0,(AJ2811*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2810,NA())","v":{"$error":"#N/A"}},null,2794,{"$f":"IF(AF2811<=$J$9*0.05,AS2810*EXP((-$J$6*1)/Heterogenität!$D$4),Z2811)","v":3.5525316526075347E-4},{"$f":"IF(OR(AF2811>=$J$19, AR2810/$J$5<AN2811),0, Bodencharakterisierung!$E$8*$J$11*((AR2810/$J$5)-AN2811))","v":2.4311325819256305E-5},3.6834237448606371E-6,{"$f":"AQ2810-AP2811*Bodencharakterisierung!$E$8","v":1.115359065965425E-3},{"$f":"AQ2811/(Bodencharakterisierung!$E$11*1000)","v":7.3621060459764026E-7},3.5893658900561411E-4,2794,null,{"$f":"(AP2811)*$G$11*Bodencharakterisierung!$E$8","v":5.3265619077140002E-8},{"$f":"IF(AF2811<=$J$9*1.05,(AV2811*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2810,NA())","v":{"$error":"#N/A"}},351.70063360814595,2927,22.525744792319806,1.6399886323194495,0,17.525756160000356,null,0.73621060459764032,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,355.25316526075346]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2807,1.5431034897990347E-11,{"$f":"Z2824*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.5272680909870897E-11},{"$f":"AF2823*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2824^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2824)*3600*24","v":0},0,{"$f":"AE2823-AD2824*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2824>$J$18,(AE2824/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.5272680909870897E-11,{"$error":"#N/A"},null,{"$f":"(AD2824)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2824>0,(AJ2824*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2823,NA())","v":{"$error":"#N/A"}},null,2807,{"$f":"IF(AF2824<=$J$9*0.05,AS2823*EXP((-$J$6*1)/Heterogenität!$D$4),Z2824)","v":3.518218824910428E-4},{"$f":"IF(OR(AF2824>=$J$19, AR2823/$J$5<AN2824),0, Bodencharakterisierung!$E$8*$J$11*((AR2823/$J$5)-AN2824))","v":1.2089227105784083E-5},3.6478466700722283E-6,{"$f":"AQ2823-AP2824*Bodencharakterisierung!$E$8","v":1.10075786214599E-3},{"$f":"AQ2824/(Bodencharakterisierung!$E$11*1000)","v":7.2657284630098344E-7},3.5546972916111503E-4,2807,null,{"$f":"(AP2824)*$G$11*Bodencharakterisierung!$E$8","v":5.275114258873641E-8},{"$f":"IF(AF2824<=$J$9*1.05,(AV2824*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2823,NA())","v":{"$error":"#N/A"}},348.30366366613237,2940,22.607289112319791,1.6399886323194495,0,17.60730048000034,null,0.7265728463009834,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,351.8218824910428]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2814,1.4356105020988003E-11,{"$f":"Z2831*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.4208782012585556E-11},{"$f":"AF2830*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2831^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2831)*3600*24","v":0},0,{"$f":"AE2830-AD2831*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2831>$J$18,(AE2831/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.4208782012585556E-11,{"$error":"#N/A"},null,{"$f":"(AD2831)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2831>0,(AJ2831*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2830,NA())","v":{"$error":"#N/A"}},null,2814,{"$f":"IF(AF2831<=$J$9*0.05,AS2830*EXP((-$J$6*1)/Heterogenität!$D$4),Z2831)","v":3.4898462634216758E-4},{"$f":"IF(OR(AF2831>=$J$19, AR2830/$J$5<AN2831),0, Bodencharakterisierung!$E$8*$J$11*((AR2830/$J$5)-AN2831))","v":1.6486107900848573E-5},3.6184287290347956E-6,{"$f":"AQ2830-AP2831*Bodencharakterisierung!$E$8","v":1.0933161704699634E-3},{"$f":"AQ2831/(Bodencharakterisierung!$E$11*1000)","v":7.2166083859403526E-7},3.5260305507120237E-4,2814,null,{"$f":"(AP2831)*$G$11*Bodencharakterisierung!$E$8","v":5.2325732711982479E-8},{"$f":"IF(AF2831<=$J$9*1.05,(AV2831*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2830,NA())","v":{"$error":"#N/A"}},345.49478007874592,2947,22.651197592319782,1.6399886323194495,0,17.651208960000332,null,0.72166083859403529,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,348.98462634216759]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2826,1.2684674396484405E-11,{"$f":"Z2843*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.2554503685838059E-11},{"$f":"AF2842*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2843^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2843)*3600*24","v":0},0,{"$f":"AE2842-AD2843*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2843>$J$18,(AE2843/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.2554503685838059E-11,{"$error":"#N/A"},null,{"$f":"(AD2843)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2843>0,(AJ2843*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2842,NA())","v":{"$error":"#N/A"}},null,2826,{"$f":"IF(AF2843<=$J$9*0.05,AS2842*EXP((-$J$6*1)/Heterogenität!$D$4),Z2843)","v":3.4490504157940632E-4},{"$f":"IF(OR(AF2843>=$J$19, AR2842/$J$5<AN2843),0, Bodencharakterisierung!$E$8*$J$11*((AR2842/$J$5)-AN2843))","v":1.5924881777985625E-5},3.5761297691555799E-6,{"$f":"AQ2842-AP2843*Bodencharakterisierung!$E$8","v":1.080417760160999E-3},{"$f":"AQ2843/(Bodencharakterisierung!$E$11*1000)","v":7.1314703640990036E-7},3.484811713485619E-4,2826,null,{"$f":"(AP2843)*$G$11*Bodencharakterisierung!$E$8","v":5.1714051721591631E-8},{"$f":"IF(AF2843<=$J$9*1.05,(AV2843*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2842,NA())","v":{"$error":"#N/A"}},341.45599116361223,2959,22.726469272319768,1.6399886323194495,0,17.726480640000318,null,0.7131470364099004,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,344.90504157940632]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2829,1.2298156009736934E-11,{"$f":"Z2846*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.2171951768509366E-11},{"$f":"AF2845*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2846^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2846)*3600*24","v":0},0,{"$f":"AE2845-AD2846*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2846>$J$18,(AE2846/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.2171951768509366E-11,{"$error":"#N/A"},null,{"$f":"(AD2846)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2846>0,(AJ2846*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2845,NA())","v":{"$error":"#N/A"}},null,2829,{"$f":"IF(AF2846<=$J$9*0.05,AS2845*EXP((-$J$6*1)/Heterogenität!$D$4),Z2846)","v":3.4490504157940632E-4},{"$f":"IF(OR(AF2846>=$J$19, AR2845/$J$5<AN2846),0, Bodencharakterisierung!$E$8*$J$11*((AR2845/$J$5)-AN2846))","v":4.8391443340049891E-6},3.5761297691555799E-6,{"$f":"AQ2845-AP2846*Bodencharakterisierung!$E$8","v":1.0768773916895349E-3},{"$f":"AQ2846/(Bodencharakterisierung!$E$11*1000)","v":7.1081015953104619E-7},3.484811713485619E-4,2829,null,{"$f":"(AP2846)*$G$11*Bodencharakterisierung!$E$8","v":5.1714051721591631E-8},{"$f":"IF(AF2846<=$J$9*1.05,(AV2846*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2845,NA())","v":{"$error":"#N/A"}},341.45599116361223,2962,22.745287192319765,1.6399886323194495,0,17.745298560000315,null,0.7108101595310462,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,344.90504157940632]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2843,1.064444799743302E-11,{"$f":"Z2860*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.0535214183702023E-11},{"$f":"AF2859*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2860^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2860)*3600*24","v":0},0,{"$f":"AE2859-AD2860*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2860>$J$18,(AE2860/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.0535214183702023E-11,{"$error":"#N/A"},null,{"$f":"(AD2860)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2860>0,(AJ2860*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2859,NA())","v":{"$error":"#N/A"}},null,2843,{"$f":"IF(AF2860<=$J$9*0.05,AS2859*EXP((-$J$6*1)/Heterogenität!$D$4),Z2860)","v":3.4043978385894406E-4},{"$f":"IF(OR(AF2860>=$J$19, AR2859/$J$5<AN2860),0, Bodencharakterisierung!$E$8*$J$11*((AR2859/$J$5)-AN2860))","v":1.8269951948236307E-6},1.8269951948236307E-6,{"$f":"AQ2859-AP2860*Bodencharakterisierung!$E$8","v":1.0625557480714557E-3},{"$f":"AQ2860/(Bodencharakterisierung!$E$11*1000)","v":7.0135692942010272E-7},3.4226677905376771E-4,2843,null,{"$f":"(AP2860)*$G$11*Bodencharakterisierung!$E$8","v":2.6419993148771608E-8},{"$f":"IF(AF2860<=$J$9*1.05,(AV2860*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2859,NA())","v":{"$error":"#N/A"}},337.03538602035462,2976,22.833104152319748,1.6399886323194495,0,17.833115520000298,null,0.70135692942010275,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,340.43978385894405]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2847,1.0214192621536251E-11,{"$f":"Z2864*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.0109374108213391E-11},{"$f":"AF2863*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2864^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2864)*3600*24","v":0},0,{"$f":"AE2863-AD2864*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2864>$J$18,(AE2864/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.0109374108213391E-11,{"$error":"#N/A"},null,{"$f":"(AD2864)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2864>0,(AJ2864*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2863,NA())","v":{"$error":"#N/A"}},null,2847,{"$f":"IF(AF2864<=$J$9*0.05,AS2863*EXP((-$J$6*1)/Heterogenität!$D$4),Z2864)","v":3.3875442166346584E-4},{"$f":"IF(OR(AF2864>=$J$19, AR2863/$J$5<AN2864),0, Bodencharakterisierung!$E$8*$J$11*((AR2863/$J$5)-AN2864))","v":5.522429972261865E-6},3.5123573903018718E-6,{"$f":"AQ2863-AP2864*Bodencharakterisierung!$E$8","v":1.057919436316257E-3},{"$f":"AQ2864/(Bodencharakterisierung!$E$11*1000)","v":6.9829665763449311E-7},3.4226677905376771E-4,2847,null,{"$f":"(AP2864)*$G$11*Bodencharakterisierung!$E$8","v":5.0791845786310845E-8},{"$f":"IF(AF2864<=$J$9*1.05,(AV2864*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2863,NA())","v":{"$error":"#N/A"}},335.36687744683121,2980,22.858194712319744,1.6399886323194495,0,17.858206080000294,null,0.69829665763449311,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,338.75442166346585]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2863,8.6601943745774551E-12,{"$f":"Z2880*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.5713230625643796E-12},{"$f":"AF2879*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2880^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2880)*3600*24","v":0},0,{"$f":"AE2879-AD2880*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2880>$J$18,(AE2880/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.5713230625643796E-12,{"$error":"#N/A"},null,{"$f":"(AD2880)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2880>0,(AJ2880*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2879,NA())","v":{"$error":"#N/A"}},null,2863,{"$f":"IF(AF2880<=$J$9*0.05,AS2879*EXP((-$J$6*1)/Heterogenität!$D$4),Z2880)","v":3.3249914862575091E-4},{"$f":"IF(OR(AF2880>=$J$19, AR2879/$J$5<AN2880),0, Bodencharakterisierung!$E$8*$J$11*((AR2879/$J$5)-AN2880))","v":1.5631442475565343E-5},3.4474999210635398E-6,{"$f":"AQ2879-AP2880*Bodencharakterisierung!$E$8","v":1.0416454207766209E-3},{"$f":"AQ2880/(Bodencharakterisierung!$E$11*1000)","v":6.8755473318588837E-7},3.3594664854681445E-4,2863,null,{"$f":"(AP2880)*$G$11*Bodencharakterisierung!$E$8","v":4.9853948468475362E-8},{"$f":"IF(AF2880<=$J$9*1.05,(AV2880*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2879,NA())","v":{"$error":"#N/A"}},329.17415713949345,2996,22.958556952319725,1.6399886323194495,0,17.958568320000275,null,0.68755473318588833,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,332.49914862575093]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2866,8.396307083981417E-12,{"$f":"Z2883*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.3101437954519354E-12},{"$f":"AF2882*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2883^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2883)*3600*24","v":0},0,{"$f":"AE2882-AD2883*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2883>$J$18,(AE2883/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.3101437954519354E-12,{"$error":"#N/A"},null,{"$f":"(AD2883)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2883>0,(AJ2883*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2882,NA())","v":{"$error":"#N/A"}},null,2866,{"$f":"IF(AF2883<=$J$9*0.05,AS2882*EXP((-$J$6*1)/Heterogenität!$D$4),Z2883)","v":3.3249914862575091E-4},{"$f":"IF(OR(AF2883>=$J$19, AR2882/$J$5<AN2883),0, Bodencharakterisierung!$E$8*$J$11*((AR2882/$J$5)-AN2883))","v":4.9444480346239872E-6},3.4474999210635398E-6,{"$f":"AQ2882-AP2883*Bodencharakterisierung!$E$8","v":1.0382323958547683E-3},{"$f":"AQ2883/(Bodencharakterisierung!$E$11*1000)","v":6.8530191145529257E-7},3.3594664854681445E-4,2866,null,{"$f":"(AP2883)*$G$11*Bodencharakterisierung!$E$8","v":4.9853948468475362E-8},{"$f":"IF(AF2883<=$J$9*1.05,(AV2883*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2882,NA())","v":{"$error":"#N/A"}},329.17415713949345,2999,22.977374872319722,1.6399886323194495,0,17.977386240000271,null,0.68530191145529262,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,332.49914862575093]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2878,7.4187546926896172E-12,{"$f":"Z2895*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.3426230916509682E-12},{"$f":"AF2894*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2895^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2895)*3600*24","v":0},0,{"$f":"AE2894-AD2895*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2895>$J$18,(AE2895/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.3426230916509682E-12,{"$error":"#N/A"},null,{"$f":"(AD2895)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2895>0,(AJ2895*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2894,NA())","v":{"$error":"#N/A"}},null,2878,{"$f":"IF(AF2895<=$J$9*0.05,AS2894*EXP((-$J$6*1)/Heterogenität!$D$4),Z2895)","v":3.2679664463795193E-4},{"$f":"IF(OR(AF2895>=$J$19, AR2894/$J$5<AN2895),0, Bodencharakterisierung!$E$8*$J$11*((AR2894/$J$5)-AN2895))","v":2.4151309259860874E-5},3.3883738086237054E-6,{"$f":"AQ2894-AP2895*Bodencharakterisierung!$E$8","v":1.0265872942662056E-3},{"$f":"AQ2895/(Bodencharakterisierung!$E$11*1000)","v":6.7761537575327101E-7},3.3018501844657563E-4,2878,null,{"$f":"(AP2895)*$G$11*Bodencharakterisierung!$E$8","v":4.8998931722947069E-8},{"$f":"IF(AF2895<=$J$9*1.05,(AV2895*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2894,NA())","v":{"$error":"#N/A"}},323.5286781915724,3011,23.052646552319707,1.6399886323194495,0,18.052657920000257,null,0.67761537575327102,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,326.79664463795194]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2884,6.9735249575184146E-12,{"$f":"Z2901*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.901962324449821E-12},{"$f":"AF2900*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2901^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2901)*3600*24","v":0},0,{"$f":"AE2900-AD2901*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2901>$J$18,(AE2901/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.901962324449821E-12,{"$error":"#N/A"},null,{"$f":"(AD2901)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2901>0,(AJ2901*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2900,NA())","v":{"$error":"#N/A"}},null,2884,{"$f":"IF(AF2901<=$J$9*0.05,AS2900*EXP((-$J$6*1)/Heterogenität!$D$4),Z2901)","v":3.2679664463795193E-4},{"$f":"IF(OR(AF2901>=$J$19, AR2900/$J$5<AN2901),0, Bodencharakterisierung!$E$8*$J$11*((AR2900/$J$5)-AN2901))","v":3.1438935175992586E-6},3.1438935175992586E-6,{"$f":"AQ2900-AP2901*Bodencharakterisierung!$E$8","v":1.0199589926211685E-3},{"$f":"AQ2901/(Bodencharakterisierung!$E$11*1000)","v":6.7324025915588678E-7},3.2994053815555118E-4,2884,null,{"$f":"(AP2901)*$G$11*Bodencharakterisierung!$E$8","v":4.5463526905147802E-8},{"$f":"IF(AF2901<=$J$9*1.05,(AV2901*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2900,NA())","v":{"$error":"#N/A"}},323.5286781915724,3017,23.0902823923197,1.6399886323194495,0,18.09029376000025,null,0.67324025915588681,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,326.79664463795194]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2896,6.1616220661912605E-12,{"$f":"Z2913*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.0983912178446435E-12},{"$f":"AF2912*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2913^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2913)*3600*24","v":0},0,{"$f":"AE2912-AD2913*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2913>$J$18,(AE2913/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.0983912178446435E-12,{"$error":"#N/A"},null,{"$f":"(AD2913)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2913>0,(AJ2913*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2912,NA())","v":{"$error":"#N/A"}},null,2896,{"$f":"IF(AF2913<=$J$9*0.05,AS2912*EXP((-$J$6*1)/Heterogenität!$D$4),Z2913)","v":3.2245105162455068E-4},{"$f":"IF(OR(AF2913>=$J$19, AR2912/$J$5<AN2913),0, Bodencharakterisierung!$E$8*$J$11*((AR2912/$J$5)-AN2913))","v":8.4762398764333239E-6},3.3433167561993933E-6,{"$f":"AQ2912-AP2913*Bodencharakterisierung!$E$8","v":1.008032739163368E-3},{"$f":"AQ2913/(Bodencharakterisierung!$E$11*1000)","v":6.653681446622891E-7},3.2579436838075008E-4,2896,null,{"$f":"(AP2913)*$G$11*Bodencharakterisierung!$E$8","v":4.8347366234582949E-8},{"$f":"IF(AF2913<=$J$9*1.05,(AV2913*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2912,NA())","v":{"$error":"#N/A"}},319.22654110830518,3029,23.165554072319686,1.6399886323194495,0,18.165565440000236,null,0.66536814466228911,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,322.4510516245507]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2903,5.7324018814447099E-12,{"$f":"Z2920*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.6735757103271513E-12},{"$f":"AF2919*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2920^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2920)*3600*24","v":0},0,{"$f":"AE2919-AD2920*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2920>$J$18,(AE2920/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.6735757103271513E-12,{"$error":"#N/A"},null,{"$f":"(AD2920)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2920>0,(AJ2920*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2919,NA())","v":{"$error":"#N/A"}},null,2903,{"$f":"IF(AF2920<=$J$9*0.05,AS2919*EXP((-$J$6*1)/Heterogenität!$D$4),Z2920)","v":3.2069284835256997E-4},{"$f":"IF(OR(AF2920>=$J$19, AR2919/$J$5<AN2920),0, Bodencharakterisierung!$E$8*$J$11*((AR2919/$J$5)-AN2920))","v":3.3876657431241104E-6},3.3250869181188471E-6,{"$f":"AQ2919-AP2920*Bodencharakterisierung!$E$8","v":1.0009259796157001E-3},{"$f":"AQ2920/(Bodencharakterisierung!$E$11*1000)","v":6.6067721426778885E-7},3.2401793527068882E-4,2903,null,{"$f":"(AP2920)*$G$11*Bodencharakterisierung!$E$8","v":4.808374638568797E-8},{"$f":"IF(AF2920<=$J$9*1.05,(AV2920*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2919,NA())","v":{"$error":"#N/A"}},317.48591986904427,3036,23.209462552319678,1.6399886323194495,0,18.209473920000228,null,0.6606772142677888,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,320.69284835256997]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2915,5.0649985681782454E-12,{"$f":"Z2932*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.0130213204827731E-12},{"$f":"AF2931*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2932^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2932)*3600*24","v":0},0,{"$f":"AE2931-AD2932*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2932>$J$18,(AE2932/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.0130213204827731E-12,{"$error":"#N/A"},null,{"$f":"(AD2932)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2932>0,(AJ2932*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2931,NA())","v":{"$error":"#N/A"}},null,2915,{"$f":"IF(AF2932<=$J$9*0.05,AS2931*EXP((-$J$6*1)/Heterogenität!$D$4),Z2932)","v":3.156389419454403E-4},{"$f":"IF(OR(AF2932>=$J$19, AR2931/$J$5<AN2932),0, Bodencharakterisierung!$E$8*$J$11*((AR2931/$J$5)-AN2932))","v":1.7179242553394815E-5},3.2726857555545196E-6,{"$f":"AQ2931-AP2932*Bodencharakterisierung!$E$8","v":9.8957361254348761E-4},{"$f":"AQ2932/(Bodencharakterisierung!$E$11*1000)","v":6.5318390266896872E-7},3.1891162770099482E-4,2915,null,{"$f":"(AP2932)*$G$11*Bodencharakterisierung!$E$8","v":4.732597846168922E-8},{"$f":"IF(AF2932<=$J$9*1.05,(AV2932*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2931,NA())","v":{"$error":"#N/A"}},312.48255252598591,3048,23.284734232319664,1.6399886323194495,0,18.284745600000214,null,0.65318390266896875,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,315.63894194544031]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2923,4.6638129603786527E-12,{"$f":"Z2940*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.6159526977973455E-12},{"$f":"AF2939*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2940^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2940)*3600*24","v":0},0,{"$f":"AE2939-AD2940*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2940>$J$18,(AE2940/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.6159526977973455E-12,{"$error":"#N/A"},null,{"$f":"(AD2940)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2940>0,(AJ2940*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2939,NA())","v":{"$error":"#N/A"}},null,2923,{"$f":"IF(AF2940<=$J$9*0.05,AS2939*EXP((-$J$6*1)/Heterogenität!$D$4),Z2940)","v":3.126678320824717E-4},{"$f":"IF(OR(AF2940>=$J$19, AR2939/$J$5<AN2940),0, Bodencharakterisierung!$E$8*$J$11*((AR2939/$J$5)-AN2940))","v":2.2328419815364184E-5},3.2418799593279704E-6,{"$f":"AQ2939-AP2940*Bodencharakterisierung!$E$8","v":9.8195485205462276E-4},{"$f":"AQ2940/(Bodencharakterisierung!$E$11*1000)","v":6.4815501785783683E-7},3.1590971204179967E-4,2923,null,{"$f":"(AP2940)*$G$11*Bodencharakterisierung!$E$8","v":4.6880498951095074E-8},{"$f":"IF(AF2940<=$J$9*1.05,(AV2940*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2939,NA())","v":{"$error":"#N/A"}},309.54115376164697,3056,23.334915352319655,1.6399886323194495,0,18.334926720000205,null,0.6481550178578368,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,312.6678320824717]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2933,4.2067177357497658E-12,{"$f":"Z2950*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.1635482053357331E-12},{"$f":"AF2949*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2950^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2950)*3600*24","v":0},0,{"$f":"AE2949-AD2950*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2950>$J$18,(AE2950/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.1635482053357331E-12,{"$error":"#N/A"},null,{"$f":"(AD2950)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2950>0,(AJ2950*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2949,NA())","v":{"$error":"#N/A"}},null,2933,{"$f":"IF(AF2950<=$J$9*0.05,AS2949*EXP((-$J$6*1)/Heterogenität!$D$4),Z2950)","v":3.1147863739877874E-4},{"$f":"IF(OR(AF2950>=$J$19, AR2949/$J$5<AN2950),0, Bodencharakterisierung!$E$8*$J$11*((AR2949/$J$5)-AN2950))","v":1.7257560462917032E-6},1.7257560462917032E-6,{"$f":"AQ2949-AP2950*Bodencharakterisierung!$E$8","v":9.7216376005664453E-4},{"$f":"AQ2950/(Bodencharakterisierung!$E$11*1000)","v":6.4169225086247159E-7},3.1320439344507045E-4,2933,null,{"$f":"(AP2950)*$G$11*Bodencharakterisierung!$E$8","v":2.4955984037976325E-8},{"$f":"IF(AF2950<=$J$9*1.05,(AV2950*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2949,NA())","v":{"$error":"#N/A"}},308.36385102479096,3066,23.397641752319643,1.6399886323194495,0,18.397653120000193,null,0.64169225086247161,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,311.47863739877874]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2936,4.078533621447658E-12,{"$f":"Z2953*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.0366795222958503E-12},{"$f":"AF2952*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2953^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2953)*3600*24","v":0},0,{"$f":"AE2952-AD2953*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2953>$J$18,(AE2953/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.0366795222958503E-12,{"$error":"#N/A"},null,{"$f":"(AD2953)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2953>0,(AJ2953*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2952,NA())","v":{"$error":"#N/A"}},null,2936,{"$f":"IF(AF2953<=$J$9*0.05,AS2952*EXP((-$J$6*1)/Heterogenität!$D$4),Z2953)","v":3.0999027558930567E-4},{"$f":"IF(OR(AF2953>=$J$19, AR2952/$J$5<AN2953),0, Bodencharakterisierung!$E$8*$J$11*((AR2952/$J$5)-AN2953))","v":7.8461799463161782E-6},3.2141178557647796E-6,{"$f":"AQ2952-AP2953*Bodencharakterisierung!$E$8","v":9.6898178337943754E-4},{"$f":"AQ2953/(Bodencharakterisierung!$E$11*1000)","v":6.3959193622405118E-7},3.1320439344507045E-4,2936,null,{"$f":"(AP2953)*$G$11*Bodencharakterisierung!$E$8","v":4.647903397296425E-8},{"$f":"IF(AF2953<=$J$9*1.05,(AV2953*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2952,NA())","v":{"$error":"#N/A"}},306.89037283341258,3069,23.41645967231964,1.6399886323194495,0,18.416471040000189,null,0.63959193622405119,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,309.99027558930567]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2948,3.603684350841945E-12,{"$f":"Z2965*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.5667031766918048E-12},{"$f":"AF2964*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2965^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2965)*3600*24","v":0},0,{"$f":"AE2964-AD2965*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2965>$J$18,(AE2965/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.5667031766918048E-12,{"$error":"#N/A"},null,{"$f":"(AD2965)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2965>0,(AJ2965*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2964,NA())","v":{"$error":"#N/A"}},null,2948,{"$f":"IF(AF2965<=$J$9*0.05,AS2964*EXP((-$J$6*1)/Heterogenität!$D$4),Z2965)","v":3.0555580656905362E-4},{"$f":"IF(OR(AF2965>=$J$19, AR2964/$J$5<AN2965),0, Bodencharakterisierung!$E$8*$J$11*((AR2964/$J$5)-AN2965))","v":1.6172298498995605E-5},3.1681392971414832E-6,{"$f":"AQ2964-AP2965*Bodencharakterisierung!$E$8","v":9.5781521262723298E-4},{"$f":"AQ2965/(Bodencharakterisierung!$E$11*1000)","v":6.3222126246021979E-7},3.0872394586619511E-4,2948,null,{"$f":"(AP2965)*$G$11*Bodencharakterisierung!$E$8","v":4.5814142676446555E-8},{"$f":"IF(AF2965<=$J$9*1.05,(AV2965*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2964,NA())","v":{"$error":"#N/A"}},302.50024850336308,3081,23.491731352319626,1.6399886323194495,0,18.491742720000175,null,0.63222126246021981,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,305.55580656905363]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2955,3.352650768090454E-12,{"$f":"Z2972*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.3182457120842624E-12},{"$f":"AF2971*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2972^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2972)*3600*24","v":0},0,{"$f":"AE2971-AD2972*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2972>$J$18,(AE2972/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.3182457120842624E-12,{"$error":"#N/A"},null,{"$f":"(AD2972)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2972>0,(AJ2972*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2971,NA())","v":{"$error":"#N/A"}},null,2955,{"$f":"IF(AF2972<=$J$9*0.05,AS2971*EXP((-$J$6*1)/Heterogenität!$D$4),Z2972)","v":3.0309651099666261E-4},{"$f":"IF(OR(AF2972>=$J$19, AR2971/$J$5<AN2972),0, Bodencharakterisierung!$E$8*$J$11*((AR2971/$J$5)-AN2972))","v":1.9886621820212196E-5},3.1426402204468929E-6,{"$f":"AQ2971-AP2972*Bodencharakterisierung!$E$8","v":9.5133392896427004E-4},{"$f":"AQ2972/(Bodencharakterisierung!$E$11*1000)","v":6.2794318743516171E-7},3.0623915121710951E-4,2955,null,{"$f":"(AP2972)*$G$11*Bodencharakterisierung!$E$8","v":4.5445403101498681E-8},{"$f":"IF(AF2972<=$J$9*1.05,(AV2972*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2971,NA())","v":{"$error":"#N/A"}},300.06554588669599,3088,23.535639832319617,1.6399886323194495,0,18.535651200000167,null,0.62794318743516175,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,303.09651099666263]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2964,3.0554159392992075E-12,{"$f":"Z2981*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.0240611207435982E-12},{"$f":"AF2980*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2981^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2981)*3600*24","v":0},0,{"$f":"AE2980-AD2981*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2981>$J$18,(AE2981/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.0240611207435982E-12,{"$error":"#N/A"},null,{"$f":"(AD2981)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2981>0,(AJ2981*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2980,NA())","v":{"$error":"#N/A"}},null,2964,{"$f":"IF(AF2981<=$J$9*0.05,AS2980*EXP((-$J$6*1)/Heterogenität!$D$4),Z2981)","v":3.0038470591215328E-4},{"$f":"IF(OR(AF2981>=$J$19, AR2980/$J$5<AN2981),0, Bodencharakterisierung!$E$8*$J$11*((AR2980/$J$5)-AN2981))","v":2.005299300634573E-5},3.1145230121670201E-6,{"$f":"AQ2980-AP2981*Bodencharakterisierung!$E$8","v":9.4293229790236072E-4},{"$f":"AQ2981/(Bodencharakterisierung!$E$11*1000)","v":6.2239755637119524E-7},3.034992289243203E-4,2964,null,{"$f":"(AP2981)*$G$11*Bodencharakterisierung!$E$8","v":4.5038802989893822E-8},{"$f":"IF(AF2981<=$J$9*1.05,(AV2981*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2980,NA())","v":{"$error":"#N/A"}},297.38085885303173,3097,23.592093592319607,1.6399886323194495,0,18.592104960000157,null,0.6223975563711952,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,300.38470591215327]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2973,2.7845329585105723E-12,{"$f":"Z2990*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.7559579535322853E-12},{"$f":"AF2989*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB2990^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z2990)*3600*24","v":0},0,{"$f":"AE2989-AD2990*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE2990>$J$18,(AE2990/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.7559579535322853E-12,{"$error":"#N/A"},null,{"$f":"(AD2990)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH2990>0,(AJ2990*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK2989,NA())","v":{"$error":"#N/A"}},null,2973,{"$f":"IF(AF2990<=$J$9*0.05,AS2989*EXP((-$J$6*1)/Heterogenität!$D$4),Z2990)","v":2.9803792699419941E-4},{"$f":"IF(OR(AF2990>=$J$19, AR2989/$J$5<AN2990),0, Bodencharakterisierung!$E$8*$J$11*((AR2989/$J$5)-AN2990))","v":1.652446777711193E-5},3.090190558481564E-6,{"$f":"AQ2989-AP2990*Bodencharakterisierung!$E$8","v":9.344887204380145E-4},{"$f":"AQ2990/(Bodencharakterisierung!$E$11*1000)","v":6.1682423791288087E-7},3.0112811755268098E-4,2973,null,{"$f":"(AP2990)*$G$11*Bodencharakterisierung!$E$8","v":4.4686933832556158E-8},{"$f":"IF(AF2990<=$J$9*1.05,(AV2990*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW2989,NA())","v":{"$error":"#N/A"}},295.05754772425746,3106,23.648547352319596,1.6399886323194495,0,18.648558720000146,null,0.61682423791288088,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,298.03792699419944]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2985,2.4603396167239245E-12,{"$f":"Z3002*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.435091498693471E-12},{"$f":"AF3001*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3002^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3002)*3600*24","v":0},0,{"$f":"AE3001-AD3002*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3002>$J$18,(AE3002/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.435091498693471E-12,{"$error":"#N/A"},null,{"$f":"(AD3002)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3002>0,(AJ3002*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3001,NA())","v":{"$error":"#N/A"}},null,2985,{"$f":"IF(AF3002<=$J$9*0.05,AS3001*EXP((-$J$6*1)/Heterogenität!$D$4),Z3002)","v":2.9553257766465899E-4},{"$f":"IF(OR(AF3002>=$J$19, AR3001/$J$5<AN3002),0, Bodencharakterisierung!$E$8*$J$11*((AR3001/$J$5)-AN3002))","v":5.4689189556348001E-6},3.0642139758300523E-6,{"$f":"AQ3001-AP3002*Bodencharakterisierung!$E$8","v":9.2314690928337615E-4},{"$f":"AQ3002/(Bodencharakterisierung!$E$11*1000)","v":6.0933789391641994E-7},2.9859679164048904E-4,2985,null,{"$f":"(AP3002)*$G$11*Bodencharakterisierung!$E$8","v":4.4311289092150754E-8},{"$f":"IF(AF3002<=$J$9*1.05,(AV3002*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3001,NA())","v":{"$error":"#N/A"}},292.57725188801243,3118,23.723819032319582,1.6399886323194495,0,18.723830400000132,null,0.6093378939164199,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,295.53257766465902]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2988,2.3853698958006515E-12,{"$f":"Z3005*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3608911204860224E-12},{"$f":"AF3004*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3005^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3005)*3600*24","v":0},0,{"$f":"AE3004-AD3005*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3005>$J$18,(AE3005/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.3608911204860224E-12,{"$error":"#N/A"},null,{"$f":"(AD3005)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3005>0,(AJ3005*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3004,NA())","v":{"$error":"#N/A"}},null,2988,{"$f":"IF(AF3005<=$J$9*0.05,AS3004*EXP((-$J$6*1)/Heterogenität!$D$4),Z3005)","v":2.947788191512542E-4},{"$f":"IF(OR(AF3005>=$J$19, AR3004/$J$5<AN3005),0, Bodencharakterisierung!$E$8*$J$11*((AR3004/$J$5)-AN3005))","v":4.1317096468982041E-6},3.0563986703587486E-6,{"$f":"AQ3004-AP3005*Bodencharakterisierung!$E$8","v":9.203698149091446E-4},{"$f":"AQ3005/(Bodencharakterisierung!$E$11*1000)","v":6.0750482832286773E-7},2.9783521782161294E-4,2988,null,{"$f":"(AP3005)*$G$11*Bodencharakterisierung!$E$8","v":4.4198272748379077E-8},{"$f":"IF(AF3005<=$J$9*1.05,(AV3005*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3004,NA())","v":{"$error":"#N/A"}},291.83103095974167,3121,23.742636952319579,1.6399886323194495,0,18.742648320000129,null,0.60750482832286767,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,294.7788191512542]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3004,2.0224571552863681E-12,{"$f":"Z3021*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.0017026071658125E-12},{"$f":"AF3020*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3021^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3021)*3600*24","v":0},0,{"$f":"AE3020-AD3021*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3021>$J$18,(AE3021/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.0017026071658125E-12,{"$error":"#N/A"},null,{"$f":"(AD3021)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3021>0,(AJ3021*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3020,NA())","v":{"$error":"#N/A"}},null,3004,{"$f":"IF(AF3021<=$J$9*0.05,AS3020*EXP((-$J$6*1)/Heterogenität!$D$4),Z3021)","v":2.8916636304263002E-4},{"$f":"IF(OR(AF3021>=$J$19, AR3020/$J$5<AN3021),0, Bodencharakterisierung!$E$8*$J$11*((AR3020/$J$5)-AN3021))","v":1.4769225878183889E-5},2.9982062146143278E-6,{"$f":"AQ3020-AP3021*Bodencharakterisierung!$E$8","v":9.0626873403958932E-4},{"$f":"AQ3021/(Bodencharakterisierung!$E$11*1000)","v":5.9819718418454741E-7},2.9216456925724435E-4,3004,null,{"$f":"(AP3021)*$G$11*Bodencharakterisierung!$E$8","v":4.3356757518107106E-8},{"$f":"IF(AF3021<=$J$9*1.05,(AV3021*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3020,NA())","v":{"$error":"#N/A"}},286.27469941220369,3137,23.84299919231956,1.6399886323194495,0,18.84301056000011,null,0.59819718418454737,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,289.16636304263]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3005,2.0017026071658125E-12,{"$f":"Z3022*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.981161043170316E-12},{"$f":"AF3021*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3022^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3022)*3600*24","v":0},0,{"$f":"AE3021-AD3022*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3022>$J$18,(AE3022/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.981161043170316E-12,{"$error":"#N/A"},null,{"$f":"(AD3022)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3022>0,(AJ3022*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3021,NA())","v":{"$error":"#N/A"}},null,3005,{"$f":"IF(AF3022<=$J$9*0.05,AS3021*EXP((-$J$6*1)/Heterogenität!$D$4),Z3022)","v":2.8916636304263002E-4},{"$f":"IF(OR(AF3022>=$J$19, AR3021/$J$5<AN3022),0, Bodencharakterisierung!$E$8*$J$11*((AR3021/$J$5)-AN3022))","v":1.1671153469962466E-5},2.9982062146143278E-6,{"$f":"AQ3021-AP3022*Bodencharakterisierung!$E$8","v":9.0527932598876662E-4},{"$f":"AQ3022/(Bodencharakterisierung!$E$11*1000)","v":5.9754410956354237E-7},2.9216456925724435E-4,3005,null,{"$f":"(AP3022)*$G$11*Bodencharakterisierung!$E$8","v":4.3356757518107106E-8},{"$f":"IF(AF3022<=$J$9*1.05,(AV3022*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3021,NA())","v":{"$error":"#N/A"}},286.27469941220369,3138,23.849271832319559,1.6399886323194495,0,18.849283200000109,null,0.59754410956354231,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,289.16636304263]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3013,1.8431528531470889E-12,{"$f":"Z3030*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.8242383340018049E-12},{"$f":"AF3029*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3030^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3030)*3600*24","v":0},0,{"$f":"AE3029-AD3030*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3030>$J$18,(AE3030/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.8242383340018049E-12,{"$error":"#N/A"},null,{"$f":"(AD3030)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3030>0,(AJ3030*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3029,NA())","v":{"$error":"#N/A"}},null,3013,{"$f":"IF(AF3030<=$J$9*0.05,AS3029*EXP((-$J$6*1)/Heterogenität!$D$4),Z3030)","v":2.8681180532190241E-4},{"$f":"IF(OR(AF3030>=$J$19, AR3029/$J$5<AN3030),0, Bodencharakterisierung!$E$8*$J$11*((AR3029/$J$5)-AN3030))","v":1.2402892416545695E-5},2.9737931068217266E-6,{"$f":"AQ3029-AP3030*Bodencharakterisierung!$E$8","v":8.9817206454825273E-4},{"$f":"AQ3030/(Bodencharakterisierung!$E$11*1000)","v":5.9285284788663547E-7},2.8978559842872414E-4,3013,null,{"$f":"(AP3030)*$G$11*Bodencharakterisierung!$E$8","v":4.3003722029864889E-8},{"$f":"IF(AF3030<=$J$9*1.05,(AV3030*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3029,NA())","v":{"$error":"#N/A"}},283.94368726868339,3146,23.89945295231955,1.6399886323194495,0,18.899464320000099,null,0.5928528478866355,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,286.8118053219024]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3025,1.6285610735601206E-12,{"$f":"Z3042*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.6118487051027125E-12},{"$f":"AF3041*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3042^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3042)*3600*24","v":0},0,{"$f":"AE3041-AD3042*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3042>$J$18,(AE3042/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.6118487051027125E-12,{"$error":"#N/A"},null,{"$f":"(AD3042)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3042>0,(AJ3042*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3041,NA())","v":{"$error":"#N/A"}},null,3025,{"$f":"IF(AF3042<=$J$9*0.05,AS3041*EXP((-$J$6*1)/Heterogenität!$D$4),Z3042)","v":2.839788930025752E-4},{"$f":"IF(OR(AF3042>=$J$19, AR3041/$J$5<AN3042),0, Bodencharakterisierung!$E$8*$J$11*((AR3041/$J$5)-AN3042))","v":6.3853576128074162E-6},2.9444202045523105E-6,{"$f":"AQ3041-AP3042*Bodencharakterisierung!$E$8","v":8.8741794243035678E-4},{"$f":"AQ3042/(Bodencharakterisierung!$E$11*1000)","v":5.857544174457801E-7},2.8692331320712751E-4,3025,null,{"$f":"(AP3042)*$G$11*Bodencharakterisierung!$E$8","v":4.2578963454190347E-8},{"$f":"IF(AF3042<=$J$9*1.05,(AV3042*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3041,NA())","v":{"$error":"#N/A"}},281.13910407254946,3158,23.974724632319536,1.6399886323194495,0,18.974736000000085,null,0.58575441744578005,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,283.97889300257521]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3037,1.4389534572712068E-12,{"$f":"Z3054*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.4241868508716036E-12},{"$f":"AF3053*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3054^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3054)*3600*24","v":0},0,{"$f":"AE3053-AD3054*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3054>$J$18,(AE3054/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.4241868508716036E-12,{"$error":"#N/A"},null,{"$f":"(AD3054)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3054>0,(AJ3054*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3053,NA())","v":{"$error":"#N/A"}},null,3037,{"$f":"IF(AF3054<=$J$9*0.05,AS3053*EXP((-$J$6*1)/Heterogenität!$D$4),Z3054)","v":2.7990967439838149E-4},{"$f":"IF(OR(AF3054>=$J$19, AR3053/$J$5<AN3054),0, Bodencharakterisierung!$E$8*$J$11*((AR3053/$J$5)-AN3054))","v":1.4145277577207538E-5},2.9022287256425319E-6,{"$f":"AQ3053-AP3054*Bodencharakterisierung!$E$8","v":8.7720931309255123E-4},{"$f":"AQ3054/(Bodencharakterisierung!$E$11*1000)","v":5.7901604824590845E-7},2.8281190312402402E-4,3037,null,{"$f":"(AP3054)*$G$11*Bodencharakterisierung!$E$8","v":4.1968836735252535E-8},{"$f":"IF(AF3054<=$J$9*1.05,(AV3054*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3053,NA())","v":{"$error":"#N/A"}},277.11057765439767,3170,24.049996312319522,1.6399886323194495,0,19.050007680000071,null,0.57901604824590847,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,279.90967439838147]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3044,1.3387155877399757E-12,{"$f":"Z3061*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.324977626956548E-12},{"$f":"AF3060*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3061^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3061)*3600*24","v":0},0,{"$f":"AE3060-AD3061*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3061>$J$18,(AE3061/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.324977626956548E-12,{"$error":"#N/A"},null,{"$f":"(AD3061)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3061>0,(AJ3061*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3060,NA())","v":{"$error":"#N/A"}},null,3044,{"$f":"IF(AF3061<=$J$9*0.05,AS3060*EXP((-$J$6*1)/Heterogenität!$D$4),Z3061)","v":2.7916485372821056E-4},{"$f":"IF(OR(AF3061>=$J$19, AR3060/$J$5<AN3061),0, Bodencharakterisierung!$E$8*$J$11*((AR3060/$J$5)-AN3061))","v":1.225820121170447E-6},1.225820121170447E-6,{"$f":"AQ3060-AP3061*Bodencharakterisierung!$E$8","v":8.7131181580452424E-4},{"$f":"AQ3061/(Bodencharakterisierung!$E$11*1000)","v":5.7512331076206217E-7},2.8039067384938102E-4,3044,null,{"$f":"(AP3061)*$G$11*Bodencharakterisierung!$E$8","v":1.7726461073739165E-8},{"$f":"IF(AF3061<=$J$9*1.05,(AV3061*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3060,NA())","v":{"$error":"#N/A"}},276.37320519092845,3177,24.093904792319513,1.6399886323194495,0,19.093916160000063,null,0.57512331076206213,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,279.16485372821057]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3055,1.1951180139816785E-12,{"$f":"Z3072*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.1828536580886048E-12},{"$f":"AF3071*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3072^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3072)*3600*24","v":0},0,{"$f":"AE3071-AD3072*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3072>$J$18,(AE3072/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.1828536580886048E-12,{"$error":"#N/A"},null,{"$f":"(AD3072)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3072>0,(AJ3072*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3071,NA())","v":{"$error":"#N/A"}},null,3055,{"$f":"IF(AF3072<=$J$9*0.05,AS3071*EXP((-$J$6*1)/Heterogenität!$D$4),Z3072)","v":2.7588682103697271E-4},{"$f":"IF(OR(AF3072>=$J$19, AR3071/$J$5<AN3072),0, Bodencharakterisierung!$E$8*$J$11*((AR3071/$J$5)-AN3072))","v":4.0314810454566838E-6},2.8605179823121361E-6,{"$f":"AQ3071-AP3072*Bodencharakterisierung!$E$8","v":8.6143704534736166E-4},{"$f":"AQ3072/(Bodencharakterisierung!$E$11*1000)","v":5.6860531046030474E-7},2.7874733901928485E-4,3055,null,{"$f":"(AP3072)*$G$11*Bodencharakterisierung!$E$8","v":4.1365661885016753E-8},{"$f":"IF(AF3072<=$J$9*1.05,(AV3072*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3071,NA())","v":{"$error":"#N/A"}},273.12795282660301,3188,24.1629038323195,1.6399886323194495,0,19.16291520000005,null,0.56860531046030471,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,275.88682103697272]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3058,1.1587012268968586E-12,{"$f":"Z3075*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.1468105817436998E-12},{"$f":"AF3074*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3075^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3075)*3600*24","v":0},0,{"$f":"AE3074-AD3075*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3075>$J$18,(AE3075/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.1468105817436998E-12,{"$error":"#N/A"},null,{"$f":"(AD3075)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3075>0,(AJ3075*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3074,NA())","v":{"$error":"#N/A"}},null,3058,{"$f":"IF(AF3075<=$J$9*0.05,AS3074*EXP((-$J$6*1)/Heterogenität!$D$4),Z3075)","v":2.7412030219065259E-4},{"$f":"IF(OR(AF3075>=$J$19, AR3074/$J$5<AN3075),0, Bodencharakterisierung!$E$8*$J$11*((AR3074/$J$5)-AN3075))","v":1.4291788934411826E-5},2.8422019246367581E-6,{"$f":"AQ3074-AP3075*Bodencharakterisierung!$E$8","v":8.5920621666125681E-4},{"$f":"AQ3075/(Bodencharakterisierung!$E$11*1000)","v":5.6713281627805727E-7},2.7696250411528934E-4,3058,null,{"$f":"(AP3075)*$G$11*Bodencharakterisierung!$E$8","v":4.110079522326141E-8},{"$f":"IF(AF3075<=$J$9*1.05,(AV3075*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3074,NA())","v":{"$error":"#N/A"}},271.37909916874605,3191,24.181721752319497,1.6399886323194495,0,19.181733120000047,null,0.56713281627805723,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,274.12030219065258]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3074,9.8241517648988053E-13,{"$f":"Z3091*EXP((-$J$6/Heterogenität!$D$4)*1)","v":9.7233358687423485E-13},{"$f":"AF3090*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3091^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3091)*3600*24","v":0},0,{"$f":"AE3090-AD3091*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3091>$J$18,(AE3091/(Bodencharakterisierung!$E$11*1000)),0)","v":0},9.7233358687423485E-13,{"$error":"#N/A"},null,{"$f":"(AD3091)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3091>0,(AJ3091*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3090,NA())","v":{"$error":"#N/A"}},null,3074,{"$f":"IF(AF3091<=$J$9*0.05,AS3090*EXP((-$J$6*1)/Heterogenität!$D$4),Z3091)","v":2.6962700164088652E-4},{"$f":"IF(OR(AF3091>=$J$19, AR3090/$J$5<AN3091),0, Bodencharakterisierung!$E$8*$J$11*((AR3090/$J$5)-AN3091))","v":1.618669510377301E-5},2.7956133743964025E-6,{"$f":"AQ3090-AP3091*Bodencharakterisierung!$E$8","v":8.4580233532175516E-4},{"$f":"AQ3091/(Bodencharakterisierung!$E$11*1000)","v":5.5828536984934332E-7},2.7242261501528292E-4,3074,null,{"$f":"(AP3091)*$G$11*Bodencharakterisierung!$E$8","v":4.0427082899524176E-8},{"$f":"IF(AF3091<=$J$9*1.05,(AV3091*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3090,NA())","v":{"$error":"#N/A"}},266.93073162447769,3207,24.282083992319478,1.6399886323194495,0,19.282095360000028,null,0.55828536984934329,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,269.62700164088653]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3077,9.5247971916049548E-13,{"$f":"Z3094*EXP((-$J$6/Heterogenität!$D$4)*1)","v":9.427053285814423E-13},{"$f":"AF3093*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3094^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3094)*3600*24","v":0},0,{"$f":"AE3093-AD3094*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3094>$J$18,(AE3094/(Bodencharakterisierung!$E$11*1000)),0)","v":0},9.427053285814423E-13,{"$error":"#N/A"},null,{"$f":"(AD3094)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3094>0,(AJ3094*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3093,NA())","v":{"$error":"#N/A"}},null,3077,{"$f":"IF(AF3094<=$J$9*0.05,AS3093*EXP((-$J$6*1)/Heterogenität!$D$4),Z3094)","v":2.6962700164088652E-4},{"$f":"IF(OR(AF3094>=$J$19, AR3093/$J$5<AN3094),0, Bodencharakterisierung!$E$8*$J$11*((AR3093/$J$5)-AN3094))","v":7.5205006801980068E-6},2.7956133743964025E-6,{"$f":"AQ3093-AP3094*Bodencharakterisierung!$E$8","v":8.4303467808110287E-4},{"$f":"AQ3094/(Bodencharakterisierung!$E$11*1000)","v":5.5645853338686654E-7},2.7242261501528292E-4,3077,null,{"$f":"(AP3094)*$G$11*Bodencharakterisierung!$E$8","v":4.0427082899524176E-8},{"$f":"IF(AF3094<=$J$9*1.05,(AV3094*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3093,NA())","v":{"$error":"#N/A"}},266.93073162447769,3210,24.300901912319475,1.6399886323194495,0,19.300913280000024,null,0.55645853338686657,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,269.62700164088653]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3085,8.7703623188116376E-13,{"$f":"Z3102*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.6803604583001799E-13},{"$f":"AF3101*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3102^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3102)*3600*24","v":0},0,{"$f":"AE3101-AD3102*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3102>$J$18,(AE3102/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.6803604583001799E-13,{"$error":"#N/A"},null,{"$f":"(AD3102)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3102>0,(AJ3102*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3101,NA())","v":{"$error":"#N/A"}},null,3085,{"$f":"IF(AF3102<=$J$9*0.05,AS3101*EXP((-$J$6*1)/Heterogenität!$D$4),Z3102)","v":2.6730436359912347E-4},{"$f":"IF(OR(AF3102>=$J$19, AR3101/$J$5<AN3102),0, Bodencharakterisierung!$E$8*$J$11*((AR3101/$J$5)-AN3102))","v":9.6046030684693164E-6},2.7715312241149807E-6,{"$f":"AQ3101-AP3102*Bodencharakterisierung!$E$8","v":8.3645882874025567E-4},{"$f":"AQ3102/(Bodencharakterisierung!$E$11*1000)","v":5.5211803877244595E-7},2.7007589482323845E-4,3085,null,{"$f":"(AP3102)*$G$11*Bodencharakterisierung!$E$8","v":4.0078833354453928E-8},{"$f":"IF(AF3102<=$J$9*1.05,(AV3102*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3101,NA())","v":{"$error":"#N/A"}},264.63131996313223,3218,24.351083032319465,1.6399886323194495,0,19.351094400000015,null,0.55211803877244592,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,267.30436359912346]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3095,7.9107886677558597E-13,{"$f":"Z3112*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.8296077914899121E-13},{"$f":"AF3111*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3112^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3112)*3600*24","v":0},0,{"$f":"AE3111-AD3112*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3112>$J$18,(AE3112/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.8296077914899121E-13,{"$error":"#N/A"},null,{"$f":"(AD3112)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3112>0,(AJ3112*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3111,NA())","v":{"$error":"#N/A"}},null,3095,{"$f":"IF(AF3112<=$J$9*0.05,AS3111*EXP((-$J$6*1)/Heterogenität!$D$4),Z3112)","v":2.6556020845968753E-4},{"$f":"IF(OR(AF3112>=$J$19, AR3111/$J$5<AN3112),0, Bodencharakterisierung!$E$8*$J$11*((AR3111/$J$5)-AN3112))","v":0},0,{"$f":"AQ3111-AP3112*Bodencharakterisierung!$E$8","v":8.2884465006378288E-4},{"$f":"AQ3112/(Bodencharakterisierung!$E$11*1000)","v":5.4709217825992267E-7},2.6556020845968753E-4,3095,null,{"$f":"(AP3112)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF3112<=$J$9*1.05,(AV3112*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3111,NA())","v":{"$error":"#N/A"}},262.90460637509068,3228,24.413809432319454,1.6399886323194495,0,19.413820800000003,null,0.54709217825992262,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,265.56020845968754]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3107,6.9897634715809431E-13,{"$f":"Z3124*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.9180341981359947E-13},{"$f":"AF3123*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3124^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3124)*3600*24","v":0},0,{"$f":"AE3123-AD3124*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3124>$J$18,(AE3124/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.9180341981359947E-13,{"$error":"#N/A"},null,{"$f":"(AD3124)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3124>0,(AJ3124*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3123,NA())","v":{"$error":"#N/A"}},null,3107,{"$f":"IF(AF3124<=$J$9*0.05,AS3123*EXP((-$J$6*1)/Heterogenität!$D$4),Z3124)","v":2.6136007911695201E-4},{"$f":"IF(OR(AF3124>=$J$19, AR3123/$J$5<AN3124),0, Bodencharakterisierung!$E$8*$J$11*((AR3123/$J$5)-AN3124))","v":1.1573527724528325E-5},2.7098982233456277E-6,{"$f":"AQ3123-AP3124*Bodencharakterisierung!$E$8","v":8.1855476306233368E-4},{"$f":"AQ3124/(Bodencharakterisierung!$E$11*1000)","v":5.4030017363850406E-7},2.6406997734029764E-4,3107,null,{"$f":"(AP3124)*$G$11*Bodencharakterisierung!$E$8","v":3.9187564749764613E-8},{"$f":"IF(AF3124<=$J$9*1.05,(AV3124*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3123,NA())","v":{"$error":"#N/A"}},258.7464783257825,3240,24.48908111231944,1.6399886323194495,0,19.489092479999989,null,0.54030017363850402,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,261.36007911695202]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3114,6.5028547426167917E-13,{"$f":"Z3131*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.4361221488884893E-13},{"$f":"AF3130*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3131^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3131)*3600*24","v":0},0,{"$f":"AE3130-AD3131*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3131>$J$18,(AE3131/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.4361221488884893E-13,{"$error":"#N/A"},null,{"$f":"(AD3131)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3131>0,(AJ3131*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3130,NA())","v":{"$error":"#N/A"}},null,3114,{"$f":"IF(AF3131<=$J$9*0.05,AS3130*EXP((-$J$6*1)/Heterogenität!$D$4),Z3131)","v":2.5904704610820942E-4},{"$f":"IF(OR(AF3131>=$J$19, AR3130/$J$5<AN3131),0, Bodencharakterisierung!$E$8*$J$11*((AR3130/$J$5)-AN3131))","v":1.7042486556027019E-5},2.6859156623435746E-6,{"$f":"AQ3130-AP3131*Bodencharakterisierung!$E$8","v":8.1308985603981327E-4},{"$f":"AQ3131/(Bodencharakterisierung!$E$11*1000)","v":5.3669297428370512E-7},2.6173296177055299E-4,3114,null,{"$f":"(AP3131)*$G$11*Bodencharakterisierung!$E$8","v":3.8840755355213684E-8},{"$f":"IF(AF3131<=$J$9*1.05,(AV3131*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3130,NA())","v":{"$error":"#N/A"}},256.45657564712735,3247,24.532989592319431,1.6399886323194495,0,19.533000959999981,null,0.5366929742837051,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,259.04704610820943]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3124,5.8655170374906166E-13,{"$f":"Z3141*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.8053248325342152E-13},{"$f":"AF3140*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3141^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3141)*3600*24","v":0},0,{"$f":"AE3140-AD3141*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3141>$J$18,(AE3141/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.8053248325342152E-13,{"$error":"#N/A"},null,{"$f":"(AD3141)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3141>0,(AJ3141*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3140,NA())","v":{"$error":"#N/A"}},null,3124,{"$f":"IF(AF3141<=$J$9*0.05,AS3140*EXP((-$J$6*1)/Heterogenität!$D$4),Z3141)","v":2.5677489638631574E-4},{"$f":"IF(OR(AF3141>=$J$19, AR3140/$J$5<AN3141),0, Bodencharakterisierung!$E$8*$J$11*((AR3140/$J$5)-AN3141))","v":1.3940000389409996E-5},2.6623569975492076E-6,{"$f":"AQ3140-AP3141*Bodencharakterisierung!$E$8","v":8.0501501555921512E-4},{"$f":"AQ3141/(Bodencharakterisierung!$E$11*1000)","v":5.3136304657373935E-7},2.5943725338386495E-4,3124,null,{"$f":"(AP3141)*$G$11*Bodencharakterisierung!$E$8","v":3.8500075880946394E-8},{"$f":"IF(AF3141<=$J$9*1.05,(AV3141*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3140,NA())","v":{"$error":"#N/A"}},254.20714742245258,3257,24.59571599231942,1.6399886323194495,0,19.59572735999997,null,0.53136304657373934,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,256.77489638631573]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3128,5.6284290984633393E-13,{"$f":"Z3145*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.5706699008151442E-13},{"$f":"AF3144*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3145^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3145)*3600*24","v":0},0,{"$f":"AE3144-AD3145*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3145>$J$18,(AE3145/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.5706699008151442E-13,{"$error":"#N/A"},null,{"$f":"(AD3145)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3145>0,(AJ3145*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3144,NA())","v":{"$error":"#N/A"}},null,3128,{"$f":"IF(AF3145<=$J$9*0.05,AS3144*EXP((-$J$6*1)/Heterogenität!$D$4),Z3145)","v":2.5677489638631574E-4},{"$f":"IF(OR(AF3145>=$J$19, AR3144/$J$5<AN3145),0, Bodencharakterisierung!$E$8*$J$11*((AR3144/$J$5)-AN3145))","v":2.9358543573737707E-6},2.6623569975492076E-6,{"$f":"AQ3144-AP3145*Bodencharakterisierung!$E$8","v":8.0150070432244999E-4},{"$f":"AQ3145/(Bodencharakterisierung!$E$11*1000)","v":5.2904336918973593E-7},2.5943725338386495E-4,3128,null,{"$f":"(AP3145)*$G$11*Bodencharakterisierung!$E$8","v":3.8500075880946394E-8},{"$f":"IF(AF3145<=$J$9*1.05,(AV3145*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3144,NA())","v":{"$error":"#N/A"}},254.20714742245258,3261,24.620806552319415,1.6399886323194495,0,19.620817919999965,null,0.52904336918973593,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,256.77489638631573]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3144,4.7721138441668733E-13,{"$f":"Z3161*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.7231421929471433E-13},{"$f":"AF3160*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3161^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3161)*3600*24","v":0},0,{"$f":"AE3160-AD3161*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3161>$J$18,(AE3161/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.7231421929471433E-13,{"$error":"#N/A"},null,{"$f":"(AD3161)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3161>0,(AJ3161*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3160,NA())","v":{"$error":"#N/A"}},null,3144,{"$f":"IF(AF3161<=$J$9*0.05,AS3160*EXP((-$J$6*1)/Heterogenität!$D$4),Z3161)","v":2.5283949718262833E-4},{"$f":"IF(OR(AF3161>=$J$19, AR3160/$J$5<AN3161),0, Bodencharakterisierung!$E$8*$J$11*((AR3160/$J$5)-AN3161))","v":1.9082793086429106E-6},1.9082793086429106E-6,{"$f":"AQ3160-AP3161*Bodencharakterisierung!$E$8","v":7.8913827630011342E-4},{"$f":"AQ3161/(Bodencharakterisierung!$E$11*1000)","v":5.2088335069314413E-7},2.5474777649127123E-4,3144,null,{"$f":"(AP3161)*$G$11*Bodencharakterisierung!$E$8","v":2.7595434516266098E-8},{"$f":"IF(AF3161<=$J$9*1.05,(AV3161*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3160,NA())","v":{"$error":"#N/A"}},250.31110221080203,3277,24.721168792319396,1.6399886323194495,0,19.721180159999946,null,0.52088335069314418,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,252.83949718262832]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3147,4.6267013813184872E-13,{"$f":"Z3164*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.579221959464224E-13},{"$f":"AF3163*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3164^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3164)*3600*24","v":0},0,{"$f":"AE3163-AD3164*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3164>$J$18,(AE3164/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.579221959464224E-13,{"$error":"#N/A"},null,{"$f":"(AD3164)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3164>0,(AJ3164*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3163,NA())","v":{"$error":"#N/A"}},null,3147,{"$f":"IF(AF3164<=$J$9*0.05,AS3163*EXP((-$J$6*1)/Heterogenität!$D$4),Z3164)","v":2.5213354312075321E-4},{"$f":"IF(OR(AF3164>=$J$19, AR3163/$J$5<AN3164),0, Bodencharakterisierung!$E$8*$J$11*((AR3163/$J$5)-AN3164))","v":1.4332274860232206E-6},1.4332274860232206E-6,{"$f":"AQ3163-AP3164*Bodencharakterisierung!$E$8","v":7.8693991720518383E-4},{"$f":"AQ3164/(Bodencharakterisierung!$E$11*1000)","v":5.194322885842797E-7},2.5356677060677641E-4,3147,null,{"$f":"(AP3164)*$G$11*Bodencharakterisierung!$E$8","v":2.0725758047229037E-8},{"$f":"IF(AF3164<=$J$9*1.05,(AV3164*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3163,NA())","v":{"$error":"#N/A"}},249.61220768954567,3280,24.739986712319393,1.6399886323194495,0,19.739998079999943,null,0.5194322885842797,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,252.13354312075322]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3154,4.3044041679672978E-13,{"$f":"Z3171*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.2602321749038662E-13},{"$f":"AF3170*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3171^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3171)*3600*24","v":0},0,{"$f":"AE3170-AD3171*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3171>$J$18,(AE3171/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.2602321749038662E-13,{"$error":"#N/A"},null,{"$f":"(AD3171)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3171>0,(AJ3171*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3170,NA())","v":{"$error":"#N/A"}},null,3154,{"$f":"IF(AF3171<=$J$9*0.05,AS3170*EXP((-$J$6*1)/Heterogenität!$D$4),Z3171)","v":2.490037149471795E-4},{"$f":"IF(OR(AF3171>=$J$19, AR3170/$J$5<AN3171),0, Bodencharakterisierung!$E$8*$J$11*((AR3170/$J$5)-AN3171))","v":1.6476162364163577E-5},2.5817819118423291E-6,{"$f":"AQ3170-AP3171*Bodencharakterisierung!$E$8","v":7.8159627365411702E-4},{"$f":"AQ3171/(Bodencharakterisierung!$E$11*1000)","v":5.1590513112482967E-7},2.5158549685902183E-4,3154,null,{"$f":"(AP3171)*$G$11*Bodencharakterisierung!$E$8","v":3.7334887697436735E-8},{"$f":"IF(AF3171<=$J$9*1.05,(AV3171*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3170,NA())","v":{"$error":"#N/A"}},246.51367779770771,3287,24.783895192319385,1.6399886323194495,0,19.783906559999934,null,0.51590513112482972,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,249.0037149471795]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3165,3.8426914631509672E-13,{"$f":"Z3182*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.80325758704835E-13},{"$f":"AF3181*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3182^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3182)*3600*24","v":0},0,{"$f":"AE3181-AD3182*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3182>$J$18,(AE3182/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.80325758704835E-13,{"$error":"#N/A"},null,{"$f":"(AD3182)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3182>0,(AJ3182*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3181,NA())","v":{"$error":"#N/A"}},null,3165,{"$f":"IF(AF3182<=$J$9*0.05,AS3181*EXP((-$J$6*1)/Heterogenität!$D$4),Z3182)","v":2.4691310631396851E-4},{"$f":"IF(OR(AF3182>=$J$19, AR3181/$J$5<AN3182),0, Bodencharakterisierung!$E$8*$J$11*((AR3181/$J$5)-AN3182))","v":9.8347200291796419E-6},2.5601055462703753E-6,{"$f":"AQ3181-AP3182*Bodencharakterisierung!$E$8","v":7.7295722536692131E-4},{"$f":"AQ3182/(Bodencharakterisierung!$E$11*1000)","v":5.1020278902107022E-7},2.4947321186023888E-4,3165,null,{"$f":"(AP3182)*$G$11*Bodencharakterisierung!$E$8","v":3.7021427962280414E-8},{"$f":"IF(AF3182<=$J$9*1.05,(AV3182*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3181,NA())","v":{"$error":"#N/A"}},244.44397525082883,3298,24.852894232319372,1.6399886323194495,0,19.852905599999922,null,0.51020278902107019,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,246.91310631396851]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3177,3.3953004624137046E-13,{"$f":"Z3194*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.3604577332875433E-13},{"$f":"AF3193*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3194^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3194)*3600*24","v":0},0,{"$f":"AE3193-AD3194*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3194>$J$18,(AE3194/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.3604577332875433E-13,{"$error":"#N/A"},null,{"$f":"(AD3194)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3194>0,(AJ3194*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3193,NA())","v":{"$error":"#N/A"}},null,3177,{"$f":"IF(AF3194<=$J$9*0.05,AS3193*EXP((-$J$6*1)/Heterogenität!$D$4),Z3194)","v":2.4477925513852146E-4},{"$f":"IF(OR(AF3194>=$J$19, AR3193/$J$5<AN3194),0, Bodencharakterisierung!$E$8*$J$11*((AR3193/$J$5)-AN3194))","v":1.3078024987237324E-6},1.3078024987237324E-6,{"$f":"AQ3193-AP3194*Bodencharakterisierung!$E$8","v":7.6398716594474508E-4},{"$f":"AQ3194/(Bodencharakterisierung!$E$11*1000)","v":5.0428195771930373E-7},2.4608705763724521E-4,3177,null,{"$f":"(AP3194)*$G$11*Bodencharakterisierung!$E$8","v":1.8911999962628745E-8},{"$f":"IF(AF3194<=$J$9*1.05,(AV3194*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3193,NA())","v":{"$error":"#N/A"}},242.33146258713623,3310,24.928165912319358,1.6399886323194495,0,19.928177279999908,null,0.50428195771930373,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,244.77925513852145]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3184,3.1587829551580068E-13,{"$f":"Z3201*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.1263673795430391E-13},{"$f":"AF3200*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3201^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3201)*3600*24","v":0},0,{"$f":"AE3200-AD3201*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3201>$J$18,(AE3201/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.1263673795430391E-13,{"$error":"#N/A"},null,{"$f":"(AD3201)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3201>0,(AJ3201*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3200,NA())","v":{"$error":"#N/A"}},null,3184,{"$f":"IF(AF3201<=$J$9*0.05,AS3200*EXP((-$J$6*1)/Heterogenität!$D$4),Z3201)","v":2.4246562110171073E-4},{"$f":"IF(OR(AF3201>=$J$19, AR3200/$J$5<AN3201),0, Bodencharakterisierung!$E$8*$J$11*((AR3200/$J$5)-AN3201))","v":8.0672171740463982E-6},2.5139920299454351E-6,{"$f":"AQ3200-AP3201*Bodencharakterisierung!$E$8","v":7.5852654937597541E-4},{"$f":"AQ3201/(Bodencharakterisierung!$E$11*1000)","v":5.0067759034717853E-7},2.4497961313165616E-4,3184,null,{"$f":"(AP3201)*$G$11*Bodencharakterisierung!$E$8","v":3.6354585056057938E-8},{"$f":"IF(AF3201<=$J$9*1.05,(AV3201*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3200,NA())","v":{"$error":"#N/A"}},240.0409648906936,3317,24.97207439231935,1.6399886323194495,0,19.972085759999899,null,0.50067759034717851,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,242.46562110171072]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3196,2.7910170075216255E-13,{"$f":"Z3213*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.7623754629348904E-13},{"$f":"AF3212*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3213^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3213)*3600*24","v":0},0,{"$f":"AE3212-AD3213*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3213>$J$18,(AE3213/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.7623754629348904E-13,{"$error":"#N/A"},null,{"$f":"(AD3213)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3213>0,(AJ3213*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3212,NA())","v":{"$error":"#N/A"}},null,3196,{"$f":"IF(AF3213<=$J$9*0.05,AS3212*EXP((-$J$6*1)/Heterogenität!$D$4),Z3213)","v":2.4024864374678042E-4},{"$f":"IF(OR(AF3213>=$J$19, AR3212/$J$5<AN3213),0, Bodencharakterisierung!$E$8*$J$11*((AR3212/$J$5)-AN3213))","v":1.0659512190452936E-6},1.0659512190452936E-6,{"$f":"AQ3212-AP3213*Bodencharakterisierung!$E$8","v":7.4984886717275939E-4},{"$f":"AQ3213/(Bodencharakterisierung!$E$11*1000)","v":4.9494974730875204E-7},2.413145949658257E-4,3196,null,{"$f":"(AP3213)*$G$11*Bodencharakterisierung!$E$8","v":1.5414613012608425E-8},{"$f":"IF(AF3213<=$J$9*1.05,(AV3213*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3212,NA())","v":{"$error":"#N/A"}},237.84615730931262,3329,25.047346072319336,1.6399886323194495,0,20.047357439999885,null,0.49494974730875202,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,240.24864374678043]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3203,2.5965940418268626E-13,{"$f":"Z3220*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.5699476746344695E-13},{"$f":"AF3219*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3220^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3220)*3600*24","v":0},0,{"$f":"AE3219-AD3220*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3220>$J$18,(AE3220/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.5699476746344695E-13,{"$error":"#N/A"},null,{"$f":"(AD3220)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3220>0,(AJ3220*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3219,NA())","v":{"$error":"#N/A"}},null,3203,{"$f":"IF(AF3220<=$J$9*0.05,AS3219*EXP((-$J$6*1)/Heterogenität!$D$4),Z3220)","v":2.3733198752367749E-4},{"$f":"IF(OR(AF3220>=$J$19, AR3219/$J$5<AN3220),0, Bodencharakterisierung!$E$8*$J$11*((AR3219/$J$5)-AN3220))","v":1.4688809469756663E-5},2.4607642204060875E-6,{"$f":"AQ3219-AP3220*Bodencharakterisierung!$E$8","v":7.446357879813643E-4},{"$f":"AQ3220/(Bodencharakterisierung!$E$11*1000)","v":4.9150877094479487E-7},2.3979275174408358E-4,3203,null,{"$f":"(AP3220)*$G$11*Bodencharakterisierung!$E$8","v":3.5584863073571042E-8},{"$f":"IF(AF3220<=$J$9*1.05,(AV3220*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3219,NA())","v":{"$error":"#N/A"}},234.95866764844072,3336,25.091254552319327,1.6399886323194495,0,{"$f":"$G$34/$G$12/$G$8+BC3219","v":20.091265919999877},null,0.49150877094479489,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,237.3319875236775]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3214,2.3180699043205081E-13,{"$f":"Z3231*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.2942817646062609E-13},{"$f":"AF3230*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3231^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3231)*3600*24","v":0},0,{"$f":"AE3230-AD3231*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3231>$J$18,(AE3231/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.2942817646062609E-13,{"$error":"#N/A"},null,{"$f":"(AD3231)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3231>0,(AJ3231*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3230,NA())","v":{"$error":"#N/A"}},null,3214,{"$f":"IF(AF3231<=$J$9*0.05,AS3230*EXP((-$J$6*1)/Heterogenität!$D$4),Z3231)","v":2.3495511942423468E-4},{"$f":"IF(OR(AF3231>=$J$19, AR3230/$J$5<AN3231),0, Bodencharakterisierung!$E$8*$J$11*((AR3230/$J$5)-AN3231))","v":1.2483572026383047E-5},2.436119788626123E-6,{"$f":"AQ3230-AP3231*Bodencharakterisierung!$E$8","v":7.3652100805341077E-4},{"$f":"AQ3231/(Bodencharakterisierung!$E$11*1000)","v":4.861524805633074E-7},2.373912392128608E-4,3214,null,{"$f":"(AP3231)*$G$11*Bodencharakterisierung!$E$8","v":3.5228482432490653E-8},{"$f":"IF(AF3231<=$J$9*1.05,(AV3231*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3230,NA())","v":{"$error":"#N/A"}},232.60556822999234,3347,25.160253592319314,1.6399886323194495,0,20.160264959999864,null,0.4861524805633074,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,234.95511942423468]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3217,2.2474353250021658E-13,{"$f":"Z3234*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.224372040581691E-13},{"$f":"AF3233*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3234^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3234)*3600*24","v":0},0,{"$f":"AE3233-AD3234*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3234>$J$18,(AE3234/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.224372040581691E-13,{"$error":"#N/A"},null,{"$f":"(AD3234)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3234>0,(AJ3234*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3233,NA())","v":{"$error":"#N/A"}},null,3217,{"$f":"IF(AF3234<=$J$9*0.05,AS3233*EXP((-$J$6*1)/Heterogenität!$D$4),Z3234)","v":2.3495511942423468E-4},{"$f":"IF(OR(AF3234>=$J$19, AR3233/$J$5<AN3234),0, Bodencharakterisierung!$E$8*$J$11*((AR3233/$J$5)-AN3234))","v":4.9317810953814101E-6},2.436119788626123E-6,{"$f":"AQ3233-AP3234*Bodencharakterisierung!$E$8","v":7.3410924946267094E-4},{"$f":"AQ3234/(Bodencharakterisierung!$E$11*1000)","v":4.8456056070143292E-7},2.373912392128608E-4,3217,null,{"$f":"(AP3234)*$G$11*Bodencharakterisierung!$E$8","v":3.5228482432490653E-8},{"$f":"IF(AF3234<=$J$9*1.05,(AV3234*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3233,NA())","v":{"$error":"#N/A"}},232.60556822999234,3350,25.179071512319311,1.6399886323194495,0,20.179082879999861,null,0.48456056070143294,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,234.95511942423468]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3224,2.0908783997249171E-13,{"$f":"Z3241*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.069421709654676E-13},{"$f":"AF3240*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3241^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3241)*3600*24","v":0},0,{"$f":"AE3240-AD3241*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3241>$J$18,(AE3241/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.069421709654676E-13,{"$error":"#N/A"},null,{"$f":"(AD3241)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3241>0,(AJ3241*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3240,NA())","v":{"$error":"#N/A"}},null,3224,{"$f":"IF(AF3241<=$J$9*0.05,AS3240*EXP((-$J$6*1)/Heterogenität!$D$4),Z3241)","v":2.3265005141859661E-4},{"$f":"IF(OR(AF3241>=$J$19, AR3240/$J$5<AN3241),0, Bodencharakterisierung!$E$8*$J$11*((AR3240/$J$5)-AN3241))","v":1.234431481943432E-5},2.4122198123394762E-6,{"$f":"AQ3240-AP3241*Bodencharakterisierung!$E$8","v":7.292898803016297E-4},{"$f":"AQ3241/(Bodencharakterisierung!$E$11*1000)","v":4.8137945894497005E-7},2.3506227123093609E-4,3224,null,{"$f":"(AP3241)*$G$11*Bodencharakterisierung!$E$8","v":3.4882867287175525E-8},{"$f":"IF(AF3241<=$J$9*1.05,(AV3241*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3240,NA())","v":{"$error":"#N/A"}},230.32355090441064,3357,25.222979992319303,1.6399886323194495,0,20.222991359999853,null,0.48137945894497003,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,232.6500514185966]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3236,1.8474448093252846E-13,{"$f":"Z3253*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.8284862459287794E-13},{"$f":"AF3252*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3253^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3253)*3600*24","v":0},0,{"$f":"AE3252-AD3253*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3253>$J$18,(AE3253/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.8284862459287794E-13,{"$error":"#N/A"},null,{"$f":"(AD3253)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3253>0,(AJ3253*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3252,NA())","v":{"$error":"#N/A"}},null,3236,{"$f":"IF(AF3253<=$J$9*0.05,AS3252*EXP((-$J$6*1)/Heterogenität!$D$4),Z3253)","v":2.3051240149567421E-4},{"$f":"IF(OR(AF3253>=$J$19, AR3252/$J$5<AN3253),0, Bodencharakterisierung!$E$8*$J$11*((AR3252/$J$5)-AN3253))","v":5.6946949383898773E-6},2.3900557016312508E-6,{"$f":"AQ3252-AP3253*Bodencharakterisierung!$E$8","v":7.205015568515033E-4},{"$f":"AQ3253/(Bodencharakterisierung!$E$11*1000)","v":4.7557858538053022E-7},2.3290245719730546E-4,3236,null,{"$f":"(AP3253)*$G$11*Bodencharakterisierung!$E$8","v":3.4562354318822337E-8},{"$f":"IF(AF3253<=$J$9*1.05,(AV3253*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3252,NA())","v":{"$error":"#N/A"}},228.20727748071747,3369,25.298251672319289,1.6399886323194495,0,20.298263039999838,null,0.47557858538053022,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,230.5124014956742]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3245,1.6836565177359881E-13,{"$f":"Z3262*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.6663787573025957E-13},{"$f":"AF3261*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3262^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3262)*3600*24","v":0},0,{"$f":"AE3261-AD3262*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3262>$J$18,(AE3262/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.6663787573025957E-13,{"$error":"#N/A"},null,{"$f":"(AD3262)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3262>0,(AJ3262*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3261,NA())","v":{"$error":"#N/A"}},null,3245,{"$f":"IF(AF3262<=$J$9*0.05,AS3261*EXP((-$J$6*1)/Heterogenität!$D$4),Z3262)","v":2.2889448556016683E-4},{"$f":"IF(OR(AF3262>=$J$19, AR3261/$J$5<AN3262),0, Bodencharakterisierung!$E$8*$J$11*((AR3261/$J$5)-AN3262))","v":1.073021401538977E-6},1.073021401538977E-6,{"$f":"AQ3261-AP3262*Bodencharakterisierung!$E$8","v":7.1441037588346656E-4},{"$f":"AQ3262/(Bodencharakterisierung!$E$11*1000)","v":4.7155800388347631E-7},2.299675069617058E-4,3245,null,{"$f":"(AP3262)*$G$11*Bodencharakterisierung!$E$8","v":1.5516854208191708E-8},{"$f":"IF(AF3262<=$J$9*1.05,(AV3262*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3261,NA())","v":{"$error":"#N/A"}},226.60554070456516,3378,25.354705432319278,1.6399886323194495,0,20.354716799999828,null,0.4715580038834763,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,228.89448556016683]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3254,1.5343891494924552E-13,{"$f":"Z3271*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.5186431776405619E-13},{"$f":"AF3270*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3271^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3271)*3600*24","v":0},0,{"$f":"AE3270-AD3271*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3271>$J$18,(AE3271/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.5186431776405619E-13,{"$error":"#N/A"},null,{"$f":"(AD3271)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3271>0,(AJ3271*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3270,NA())","v":{"$error":"#N/A"}},null,3254,{"$f":"IF(AF3271<=$J$9*0.05,AS3270*EXP((-$J$6*1)/Heterogenität!$D$4),Z3271)","v":2.256170601766488E-4},{"$f":"IF(OR(AF3271>=$J$19, AR3270/$J$5<AN3271),0, Bodencharakterisierung!$E$8*$J$11*((AR3270/$J$5)-AN3271))","v":1.4607538287977174E-5},2.3392986128366528E-6,{"$f":"AQ3270-AP3271*Bodencharakterisierung!$E$8","v":7.0808547368043581E-4},{"$f":"AQ3271/(Bodencharakterisierung!$E$11*1000)","v":4.6738315094418205E-7},2.2795635878948545E-4,3254,null,{"$f":"(AP3271)*$G$11*Bodencharakterisierung!$E$8","v":3.382836117970282E-8},{"$f":"IF(AF3271<=$J$9*1.05,(AV3271*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3270,NA())","v":{"$error":"#N/A"}},223.36088957488232,3387,25.411159192319268,1.6399886323194495,0,20.411170559999817,null,0.46738315094418204,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,225.61706017664881]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3266,1.3557456378562313E-13,{"$f":"Z3283*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.3418329139171494E-13},{"$f":"AF3282*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3283^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3283)*3600*24","v":0},0,{"$f":"AE3282-AD3283*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3283>$J$18,(AE3283/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.3418329139171494E-13,{"$error":"#N/A"},null,{"$f":"(AD3283)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3283>0,(AJ3283*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3282,NA())","v":{"$error":"#N/A"}},null,3266,{"$f":"IF(AF3283<=$J$9*0.05,AS3282*EXP((-$J$6*1)/Heterogenität!$D$4),Z3283)","v":2.2340493128096558E-4},{"$f":"IF(OR(AF3283>=$J$19, AR3282/$J$5<AN3283),0, Bodencharakterisierung!$E$8*$J$11*((AR3282/$J$5)-AN3283))","v":9.6484557098110038E-6},2.3163622708196349E-6,{"$f":"AQ3282-AP3283*Bodencharakterisierung!$E$8","v":6.9960483665923749E-4},{"$f":"AQ3283/(Bodencharakterisierung!$E$11*1000)","v":4.6178537073216998E-7},2.2572129355178522E-4,3266,null,{"$f":"(AP3283)*$G$11*Bodencharakterisierung!$E$8","v":3.3496681052319676E-8},{"$f":"IF(AF3283<=$J$9*1.05,(AV3283*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3282,NA())","v":{"$error":"#N/A"}},221.17088196815592,3399,25.486430872319254,1.6399886323194495,0,20.486442239999803,null,0.46178537073216996,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,223.40493128096557]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3273,1.2613040465189546E-13,{"$f":"Z3290*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.2483604865232807E-13},{"$f":"AF3289*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3290^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3290)*3600*24","v":0},0,{"$f":"AE3289-AD3290*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3290>$J$18,(AE3290/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.2483604865232807E-13,{"$error":"#N/A"},null,{"$f":"(AD3290)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3290>0,(AJ3290*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3289,NA())","v":{"$error":"#N/A"}},null,3273,{"$f":"IF(AF3290<=$J$9*0.05,AS3289*EXP((-$J$6*1)/Heterogenität!$D$4),Z3290)","v":2.2118596331282598E-4},{"$f":"IF(OR(AF3290>=$J$19, AR3289/$J$5<AN3290),0, Bodencharakterisierung!$E$8*$J$11*((AR3289/$J$5)-AN3290))","v":1.6944387954250213E-5},2.2933550182398222E-6,{"$f":"AQ3289-AP3290*Bodencharakterisierung!$E$8","v":6.9501666881653548E-4},{"$f":"AQ3290/(Bodencharakterisierung!$E$11*1000)","v":4.587568771066241E-7},2.234793183310658E-4,3273,null,{"$f":"(AP3290)*$G$11*Bodencharakterisierung!$E$8","v":3.3163975494443592E-8},{"$f":"IF(AF3290<=$J$9*1.05,(AV3290*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3289,NA())","v":{"$error":"#N/A"}},218.97410367969772,3406,25.530339352319245,1.6399886323194495,0,20.530350719999795,null,0.45875687710662411,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,221.18596331282598]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3285,1.1144548693166412E-13,{"$f":"Z3302*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.1030182823150517E-13},{"$f":"AF3301*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3302^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3302)*3600*24","v":0},0,{"$f":"AE3301-AD3302*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3302>$J$18,(AE3302/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.1030182823150517E-13,{"$error":"#N/A"},null,{"$f":"(AD3302)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3302>0,(AJ3302*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3301,NA())","v":{"$error":"#N/A"}},null,3285,{"$f":"IF(AF3302<=$J$9*0.05,AS3301*EXP((-$J$6*1)/Heterogenität!$D$4),Z3302)","v":2.1926867059427865E-4},{"$f":"IF(OR(AF3302>=$J$19, AR3301/$J$5<AN3302),0, Bodencharakterisierung!$E$8*$J$11*((AR3301/$J$5)-AN3302))","v":9.3293568578010845E-6},2.2734756696064155E-6,{"$f":"AQ3301-AP3302*Bodencharakterisierung!$E$8","v":6.8660705065172012E-4},{"$f":"AQ3302/(Bodencharakterisierung!$E$11*1000)","v":4.5320597402753802E-7},2.2154214626388506E-4,3285,null,{"$f":"(AP3302)*$G$11*Bodencharakterisierung!$E$8","v":3.2876502239897158E-8},{"$f":"IF(AF3302<=$J$9*1.05,(AV3302*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3301,NA())","v":{"$error":"#N/A"}},217.07598388833588,3418,25.605611032319231,1.6399886323194495,0,20.605622399999781,null,0.45320597402753804,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,219.26867059427866]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3286,1.1030182823150517E-13,{"$f":"Z3303*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.0916990580939984E-13},{"$f":"AF3302*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3303^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3303)*3600*24","v":0},0,{"$f":"AE3302-AD3303*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3303>$J$18,(AE3303/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.0916990580939984E-13,{"$error":"#N/A"},null,{"$f":"(AD3303)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3303>0,(AJ3303*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3302,NA())","v":{"$error":"#N/A"}},null,3286,{"$f":"IF(AF3303<=$J$9*0.05,AS3302*EXP((-$J$6*1)/Heterogenität!$D$4),Z3303)","v":2.1926867059427865E-4},{"$f":"IF(OR(AF3303>=$J$19, AR3302/$J$5<AN3303),0, Bodencharakterisierung!$E$8*$J$11*((AR3302/$J$5)-AN3303))","v":6.9801547887640817E-6},2.2734756696064155E-6,{"$f":"AQ3302-AP3303*Bodencharakterisierung!$E$8","v":6.8585680368074998E-4},{"$f":"AQ3303/(Bodencharakterisierung!$E$11*1000)","v":4.5271076150544551E-7},2.2154214626388506E-4,3286,null,{"$f":"(AP3303)*$G$11*Bodencharakterisierung!$E$8","v":3.2876502239897158E-8},{"$f":"IF(AF3303<=$J$9*1.05,(AV3303*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3302,NA())","v":{"$error":"#N/A"}},217.07598388833588,3419,25.61188367231923,1.6399886323194495,0,20.61189503999978,null,0.45271076150544554,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,219.26867059427866]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3294,1.0156510197091339E-13,{"$f":"Z3311*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.0052283623454679E-13},{"$f":"AF3310*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3311^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3311)*3600*24","v":0},0,{"$f":"AE3310-AD3311*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3311>$J$18,(AE3311/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.0052283623454679E-13,{"$error":"#N/A"},null,{"$f":"(AD3311)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3311>0,(AJ3311*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3310,NA())","v":{"$error":"#N/A"}},null,3294,{"$f":"IF(AF3311<=$J$9*0.05,AS3310*EXP((-$J$6*1)/Heterogenität!$D$4),Z3311)","v":2.1701852543630382E-4},{"$f":"IF(OR(AF3311>=$J$19, AR3310/$J$5<AN3311),0, Bodencharakterisierung!$E$8*$J$11*((AR3310/$J$5)-AN3311))","v":1.2623223612819014E-5},2.2501451579748334E-6,{"$f":"AQ3310-AP3311*Bodencharakterisierung!$E$8","v":6.8064357022815103E-4},{"$f":"AQ3311/(Bodencharakterisierung!$E$11*1000)","v":4.4926968331891157E-7},2.1926867059427865E-4,3294,null,{"$f":"(AP3311)*$G$11*Bodencharakterisierung!$E$8","v":3.2539122065493782E-8},{"$f":"IF(AF3311<=$J$9*1.05,(AV3311*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3310,NA())","v":{"$error":"#N/A"}},214.84834018194076,3427,25.662064792319221,1.6399886323194495,0,20.662076159999771,null,0.44926968331891159,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,217.0185254363038]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3306,8.9740235715976222E-14,{"$f":"Z3323*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.8819317299658278E-14},{"$f":"AF3322*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3323^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3323)*3600*24","v":0},0,{"$f":"AE3322-AD3323*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3323>$J$18,(AE3323/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.8819317299658278E-14,{"$error":"#N/A"},null,{"$f":"(AD3323)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3323>0,(AJ3323*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3322,NA())","v":{"$error":"#N/A"}},null,3306,{"$f":"IF(AF3323<=$J$9*0.05,AS3322*EXP((-$J$6*1)/Heterogenität!$D$4),Z3323)","v":2.1408124112884185E-4},{"$f":"IF(OR(AF3323>=$J$19, AR3322/$J$5<AN3323),0, Bodencharakterisierung!$E$8*$J$11*((AR3322/$J$5)-AN3323))","v":1.6574943306699545E-5},2.2196900802401573E-6,{"$f":"AQ3322-AP3323*Bodencharakterisierung!$E$8","v":6.727478467780225E-4},{"$f":"AQ3323/(Bodencharakterisierung!$E$11*1000)","v":4.4405798467196205E-7},2.1630093120908201E-4,3306,null,{"$f":"(AP3323)*$G$11*Bodencharakterisierung!$E$8","v":3.2098714259619321E-8},{"$f":"IF(AF3323<=$J$9*1.05,(AV3323*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3322,NA())","v":{"$error":"#N/A"}},211.94042871755346,3439,25.737336472319207,1.6399886323194495,0,20.737347839999757,null,0.44405798467196206,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,214.08124112884187]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3318,7.9292096892349015E-14,{"$f":"Z3335*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.8478397756013547E-14},{"$f":"AF3334*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3335^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3335)*3600*24","v":0},0,{"$f":"AE3334-AD3335*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3335>$J$18,(AE3335/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.8478397756013547E-14,{"$error":"#N/A"},null,{"$f":"(AD3335)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3335>0,(AJ3335*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3334,NA())","v":{"$error":"#N/A"}},null,3318,{"$f":"IF(AF3335<=$J$9*0.05,AS3334*EXP((-$J$6*1)/Heterogenität!$D$4),Z3335)","v":2.1239856639859549E-4},{"$f":"IF(OR(AF3335>=$J$19, AR3334/$J$5<AN3335),0, Bodencharakterisierung!$E$8*$J$11*((AR3334/$J$5)-AN3335))","v":7.3253729055271836E-6},2.2022433558690428E-6,{"$f":"AQ3334-AP3335*Bodencharakterisierung!$E$8","v":6.6454770123550774E-4},{"$f":"AQ3335/(Bodencharakterisierung!$E$11*1000)","v":4.3864534735017013E-7},2.1460080975446453E-4,3318,null,{"$f":"(AP3335)*$G$11*Bodencharakterisierung!$E$8","v":3.1846418939051801E-8},{"$f":"IF(AF3335<=$J$9*1.05,(AV3335*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3334,NA())","v":{"$error":"#N/A"}},210.27458073460951,3451,25.812608152319193,1.6399886323194495,0,20.812619519999743,null,0.43864534735017013,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,212.39856639859548]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3325,7.3768588940795439E-14,{"$f":"Z3342*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.3011572296484653E-14},{"$f":"AF3341*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3342^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3342)*3600*24","v":0},0,{"$f":"AE3341-AD3342*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3342>$J$18,(AE3342/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.3011572296484653E-14,{"$error":"#N/A"},null,{"$f":"(AD3342)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3342>0,(AJ3342*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3341,NA())","v":{"$error":"#N/A"}},null,3325,{"$f":"IF(AF3342<=$J$9*0.05,AS3341*EXP((-$J$6*1)/Heterogenität!$D$4),Z3342)","v":2.1071238769356732E-4},{"$f":"IF(OR(AF3342>=$J$19, AR3341/$J$5<AN3342),0, Bodencharakterisierung!$E$8*$J$11*((AR3341/$J$5)-AN3342))","v":9.6901101784190383E-6},2.1847603007198613E-6,{"$f":"AQ3341-AP3342*Bodencharakterisierung!$E$8","v":6.6004580509710547E-4},{"$f":"AQ3342/(Bodencharakterisierung!$E$11*1000)","v":4.3567379874396402E-7},2.1289714799428719E-4,3325,null,{"$f":"(AP3342)*$G$11*Bodencharakterisierung!$E$8","v":3.1593598242768824E-8},{"$f":"IF(AF3342<=$J$9*1.05,(AV3342*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3341,NA())","v":{"$error":"#N/A"}},208.60526381663166,3458,25.856516632319185,1.6399886323194495,0,20.856527999999734,null,0.435673798743964,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,210.71238769356734]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3335,6.6538609947445907E-14,{"$f":"Z3352*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.585578767928587E-14},{"$f":"AF3351*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3352^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3352)*3600*24","v":0},0,{"$f":"AE3351-AD3352*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3352>$J$18,(AE3352/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.585578767928587E-14,{"$error":"#N/A"},null,{"$f":"(AD3352)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3352>0,(AJ3352*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3351,NA())","v":{"$error":"#N/A"}},null,3335,{"$f":"IF(AF3352<=$J$9*0.05,AS3351*EXP((-$J$6*1)/Heterogenität!$D$4),Z3352)","v":2.0920325805762188E-4},{"$f":"IF(OR(AF3352>=$J$19, AR3351/$J$5<AN3352),0, Bodencharakterisierung!$E$8*$J$11*((AR3351/$J$5)-AN3352))","v":3.5201825132228351E-6},2.1691129695242508E-6,{"$f":"AQ3351-AP3352*Bodencharakterisierung!$E$8","v":6.5337025421965391E-4},{"$f":"AQ3352/(Bodencharakterisierung!$E$11*1000)","v":4.3126749453442505E-7},2.1137237102714614E-4,3335,null,{"$f":"(AP3352)*$G$11*Bodencharakterisierung!$E$8","v":3.1367323765334025E-8},{"$f":"IF(AF3352<=$J$9*1.05,(AV3352*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3351,NA())","v":{"$error":"#N/A"}},207.11122547704568,3468,25.919243032319173,1.6399886323194495,0,20.919254399999723,null,0.43126749453442503,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,209.20325805762189]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3343,6.1268256498262722E-14,{"$f":"Z3360*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.0639518839008988E-14},{"$f":"AF3359*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3360^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3360)*3600*24","v":0},0,{"$f":"AE3359-AD3360*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3360>$J$18,(AE3360/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.0639518839008988E-14,{"$error":"#N/A"},null,{"$f":"(AD3360)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3360>0,(AJ3360*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3359,NA())","v":{"$error":"#N/A"}},null,3343,{"$f":"IF(AF3360<=$J$9*0.05,AS3359*EXP((-$J$6*1)/Heterogenität!$D$4),Z3360)","v":2.0637990278154738E-4},{"$f":"IF(OR(AF3360>=$J$19, AR3359/$J$5<AN3360),0, Bodencharakterisierung!$E$8*$J$11*((AR3359/$J$5)-AN3360))","v":1.6192778744057981E-5},2.139839158954741E-6,{"$f":"AQ3359-AP3360*Bodencharakterisierung!$E$8","v":6.4861485506872605E-4},{"$f":"AQ3360/(Bodencharakterisierung!$E$11*1000)","v":4.2812861720707988E-7},2.0851974194050212E-4,3343,null,{"$f":"(AP3360)*$G$11*Bodencharakterisierung!$E$8","v":3.0943998144732409E-8},{"$f":"IF(AF3360<=$J$9*1.05,(AV3360*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3359,NA())","v":{"$error":"#N/A"}},204.31610375373191,3476,25.969424152319164,1.6399886323194495,0,20.969435519999713,null,0.4281286172070799,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,206.37990278154737]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3355,5.4135009696889707E-14,{"$f":"Z3372*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.3579473743594448E-14},{"$f":"AF3371*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3372^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3372)*3600*24","v":0},0,{"$f":"AE3371-AD3372*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3372>$J$18,(AE3372/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.3579473743594448E-14,{"$error":"#N/A"},null,{"$f":"(AD3372)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3372>0,(AJ3372*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3371,NA())","v":{"$error":"#N/A"}},null,3355,{"$f":"IF(AF3372<=$J$9*0.05,AS3371*EXP((-$J$6*1)/Heterogenität!$D$4),Z3372)","v":2.0496966420231641E-4},{"$f":"IF(OR(AF3372>=$J$19, AR3371/$J$5<AN3372),0, Bodencharakterisierung!$E$8*$J$11*((AR3371/$J$5)-AN3372))","v":4.9746663200404422E-6},2.1252171744754627E-6,{"$f":"AQ3371-AP3372*Bodencharakterisierung!$E$8","v":6.4063542225968064E-4},{"$f":"AQ3372/(Bodencharakterisierung!$E$11*1000)","v":4.2286166485787499E-7},2.0709488137679187E-4,3355,null,{"$f":"(AP3372)*$G$11*Bodencharakterisierung!$E$8","v":3.0732551102693931E-8},{"$f":"IF(AF3372<=$J$9*1.05,(AV3372*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3371,NA())","v":{"$error":"#N/A"}},202.91996756029323,3488,26.04469583231915,1.6399886323194495,0,21.044707199999699,null,0.42286166485787496,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,204.96966420231641]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3358,5.2485446140067181E-14,{"$f":"Z3375*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.194683808367619E-14},{"$f":"AF3374*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3375^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3375)*3600*24","v":0},0,{"$f":"AE3374-AD3375*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3375>$J$18,(AE3375/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.194683808367619E-14,{"$error":"#N/A"},null,{"$f":"(AD3375)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3375>0,(AJ3375*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3374,NA())","v":{"$error":"#N/A"}},null,3358,{"$f":"IF(AF3375<=$J$9*0.05,AS3374*EXP((-$J$6*1)/Heterogenität!$D$4),Z3375)","v":2.0344293261603466E-4},{"$f":"IF(OR(AF3375>=$J$19, AR3374/$J$5<AN3375),0, Bodencharakterisierung!$E$8*$J$11*((AR3374/$J$5)-AN3375))","v":1.4901600999331609E-5},2.1093873383842973E-6,{"$f":"AQ3374-AP3375*Bodencharakterisierung!$E$8","v":6.3904572637224315E-4},{"$f":"AQ3375/(Bodencharakterisierung!$E$11*1000)","v":4.2181236064174464E-7},2.0555231995441896E-4,3358,null,{"$f":"(AP3375)*$G$11*Bodencharakterisierung!$E$8","v":3.0503637440381237E-8},{"$f":"IF(AF3375<=$J$9*1.05,(AV3375*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3374,NA())","v":{"$error":"#N/A"}},201.40850328987432,3491,26.063513752319146,1.6399886323194495,0,21.063525119999696,null,0.42181236064174465,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,203.44293261603465]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3366,4.8328207924319949E-14,{"$f":"Z3383*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.7832261637238538E-14},{"$f":"AF3382*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3383^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3383)*3600*24","v":0},0,{"$f":"AE3382-AD3383*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3383>$J$18,(AE3383/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.7832261637238538E-14,{"$error":"#N/A"},null,{"$f":"(AD3383)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3383>0,(AJ3383*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3382,NA())","v":{"$error":"#N/A"}},null,3366,{"$f":"IF(AF3383<=$J$9*0.05,AS3382*EXP((-$J$6*1)/Heterogenität!$D$4),Z3383)","v":2.0316018882638796E-4},{"$f":"IF(OR(AF3383>=$J$19, AR3382/$J$5<AN3383),0, Bodencharakterisierung!$E$8*$J$11*((AR3382/$J$5)-AN3383))","v":5.25939040249205E-7},5.25939040249205E-7,{"$f":"AQ3382-AP3383*Bodencharakterisierung!$E$8","v":6.3409472205318295E-4},{"$f":"AQ3383/(Bodencharakterisierung!$E$11*1000)","v":4.1854437099219995E-7},2.0368612786663716E-4,3366,null,{"$f":"(AP3383)*$G$11*Bodencharakterisierung!$E$8","v":7.605551388106906E-9},{"$f":"IF(AF3383<=$J$9*1.05,(AV3383*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3382,NA())","v":{"$error":"#N/A"}},201.12858693812407,3499,26.113694872319137,1.6399886323194495,0,21.113706239999686,null,0.41854437099219993,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,203.16018882638795]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3376,4.3591612944043332E-14,{"$f":"Z3393*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.3144273811970756E-14},{"$f":"AF3392*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3393^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3393)*3600*24","v":0},0,{"$f":"AE3392-AD3393*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3393>$J$18,(AE3393/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.3144273811970756E-14,{"$error":"#N/A"},null,{"$f":"(AD3393)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3393>0,(AJ3393*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3392,NA())","v":{"$error":"#N/A"}},null,3376,{"$f":"IF(AF3393<=$J$9*0.05,AS3392*EXP((-$J$6*1)/Heterogenität!$D$4),Z3393)","v":1.9967716076349319E-4},{"$f":"IF(OR(AF3393>=$J$19, AR3392/$J$5<AN3393),0, Bodencharakterisierung!$E$8*$J$11*((AR3392/$J$5)-AN3393))","v":1.6607730478914281E-5},2.0703421311468306E-6,{"$f":"AQ3392-AP3393*Bodencharakterisierung!$E$8","v":6.2784981841895683E-4},{"$f":"AQ3393/(Bodencharakterisierung!$E$11*1000)","v":4.1442232238875036E-7},2.0174750289464003E-4,{"$error":"#N/A"},null,{"$f":"(AP3393)*$G$11*Bodencharakterisierung!$E$8","v":2.9939008638603891E-8},{"$f":"IF(AF3393<=$J$9*1.05,(AV3393*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3392,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,21.176432639999675,null,0.41442232238875037,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,199.67716076349319]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3383,4.0555009926161706E-14,{"$f":"Z3400*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.0138832553581987E-14},{"$f":"AF3399*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3400^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3400)*3600*24","v":0},0,{"$f":"AE3399-AD3400*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3400>$J$18,(AE3400/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.0138832553581987E-14,{"$error":"#N/A"},null,{"$f":"(AD3400)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3400>0,(AJ3400*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3399,NA())","v":{"$error":"#N/A"}},null,3383,{"$f":"IF(AF3400<=$J$9*0.05,AS3399*EXP((-$J$6*1)/Heterogenität!$D$4),Z3400)","v":1.9967716076349319E-4},{"$f":"IF(OR(AF3400>=$J$19, AR3399/$J$5<AN3400),0, Bodencharakterisierung!$E$8*$J$11*((AR3399/$J$5)-AN3400))","v":1.6326134887132901E-6},1.6326134887132901E-6,{"$f":"AQ3399-AP3400*Bodencharakterisierung!$E$8","v":6.232117785480106E-4},{"$f":"AQ3400/(Bodencharakterisierung!$E$11*1000)","v":4.1136090993268027E-7},2.0130977425220648E-4,{"$error":"#N/A"},null,{"$f":"(AP3400)*$G$11*Bodencharakterisierung!$E$8","v":2.3609058911926231E-8},{"$f":"IF(AF3400<=$J$9*1.05,(AV3400*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3399,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,21.220341119999667,null,0.41136090993268026,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,199.67716076349319]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3395,3.5833333296704366E-14,{"$f":"Z3412*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.5465609986332904E-14},{"$f":"AF3411*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3412^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3412)*3600*24","v":0},0,{"$f":"AE3411-AD3412*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3412>$J$18,(AE3412/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.5465609986332904E-14,{"$error":"#N/A"},null,{"$f":"(AD3412)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3412>0,(AJ3412*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3411,NA())","v":{"$error":"#N/A"}},null,3395,{"$f":"IF(AF3412<=$J$9*0.05,AS3411*EXP((-$J$6*1)/Heterogenität!$D$4),Z3412)","v":1.9731057066065845E-4},{"$f":"IF(OR(AF3412>=$J$19, AR3411/$J$5<AN3412),0, Bodencharakterisierung!$E$8*$J$11*((AR3411/$J$5)-AN3412))","v":1.7778335824817521E-6},1.7778335824817521E-6,{"$f":"AQ3411-AP3412*Bodencharakterisierung!$E$8","v":6.1582367076484313E-4},{"$f":"AQ3412/(Bodencharakterisierung!$E$11*1000)","v":4.0648427113190966E-7},1.990884042431402E-4,{"$error":"#N/A"},null,{"$f":"(AP3412)*$G$11*Bodencharakterisierung!$E$8","v":2.5709072033634039E-8},{"$f":"IF(AF3412<=$J$9*1.05,(AV3412*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3411,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,{"$f":"$G$34/$G$12/$G$8+BC3411","v":21.295612799999653},null,0.40648427113190966,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,197.31057066065844]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3407,3.1661384807709952E-14,{"$f":"Z3424*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.1336474224147057E-14},{"$f":"AF3423*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3424^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3424)*3600*24","v":0},0,{"$f":"AE3423-AD3424*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3424>$J$18,(AE3424/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.1336474224147057E-14,{"$error":"#N/A"},null,{"$f":"(AD3424)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3424>0,(AJ3424*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3423,NA())","v":{"$error":"#N/A"}},null,3407,{"$f":"IF(AF3424<=$J$9*0.05,AS3423*EXP((-$J$6*1)/Heterogenität!$D$4),Z3424)","v":1.9443613997080665E-4},{"$f":"IF(OR(AF3424>=$J$19, AR3423/$J$5<AN3424),0, Bodencharakterisierung!$E$8*$J$11*((AR3423/$J$5)-AN3424))","v":7.7004889745740192E-6},2.016000882924812E-6,{"$f":"AQ3423-AP3424*Bodencharakterisierung!$E$8","v":6.0866492252035641E-4},{"$f":"AQ3424/(Bodencharakterisierung!$E$11*1000)","v":4.0175902476591183E-7},1.9645214085373147E-4,{"$error":"#N/A"},null,{"$f":"(AP3424)*$G$11*Bodencharakterisierung!$E$8","v":2.915318533168489E-8},{"$f":"IF(AF3424<=$J$9*1.05,(AV3424*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3423,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,21.370884479999638,null,0.40175902476591185,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,194.43613997080666]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3415,2.9153567335132349E-14,{"$f":"Z3432*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.8854392089535028E-14},{"$f":"AF3431*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3432^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3432)*3600*24","v":0},0,{"$f":"AE3431-AD3432*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3432>$J$18,(AE3432/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.8854392089535028E-14,{"$error":"#N/A"},null,{"$f":"(AD3432)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3432>0,(AJ3432*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3431,NA())","v":{"$error":"#N/A"}},null,3415,{"$f":"IF(AF3432<=$J$9*0.05,AS3431*EXP((-$J$6*1)/Heterogenität!$D$4),Z3432)","v":1.9313663347825274E-4},{"$f":"IF(OR(AF3432>=$J$19, AR3431/$J$5<AN3432),0, Bodencharakterisierung!$E$8*$J$11*((AR3431/$J$5)-AN3432))","v":5.1241877059671437E-6},2.0025270182577278E-6,{"$f":"AQ3431-AP3432*Bodencharakterisierung!$E$8","v":6.0379059618128467E-4},{"$f":"AQ3432/(Bodencharakterisierung!$E$11*1000)","v":3.985416476444123E-7},1.9513916049651047E-4,{"$error":"#N/A"},null,{"$f":"(AP3432)*$G$11*Bodencharakterisierung!$E$8","v":2.8958341134392841E-8},{"$f":"IF(AF3432<=$J$9*1.05,(AV3432*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3431,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,21.421065599999629,null,0.3985416476444123,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,193.13663347825275]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3425,2.6296257978390096E-14,{"$f":"Z3442*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.6026404572508795E-14},{"$f":"AF3441*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3442^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3442)*3600*24","v":0},0,{"$f":"AE3441-AD3442*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3442>$J$18,(AE3442/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.6026404572508795E-14,{"$error":"#N/A"},null,{"$f":"(AD3442)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3442>0,(AJ3442*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3441,NA())","v":{"$error":"#N/A"}},null,3425,{"$f":"IF(AF3442<=$J$9*0.05,AS3441*EXP((-$J$6*1)/Heterogenität!$D$4),Z3442)","v":1.9171125056538594E-4},{"$f":"IF(OR(AF3442>=$J$19, AR3441/$J$5<AN3442),0, Bodencharakterisierung!$E$8*$J$11*((AR3441/$J$5)-AN3442))","v":0},0,{"$f":"AQ3441-AP3442*Bodencharakterisierung!$E$8","v":5.9834531529258622E-4},{"$f":"AQ3442/(Bodencharakterisierung!$E$11*1000)","v":3.9494740283339024E-7},1.9171125056538594E-4,{"$error":"#N/A"},null,{"$f":"(AP3442)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF3442<=$J$9*1.05,(AV3442*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3441,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,21.483791999999617,null,0.39494740283339025,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,191.71125056538594]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3428,2.5494977086692977E-14,{"$f":"Z3445*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.5233346462086096E-14},{"$f":"AF3444*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3445^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3445)*3600*24","v":0},0,{"$f":"AE3444-AD3445*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3445>$J$18,(AE3445/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.5233346462086096E-14,{"$error":"#N/A"},null,{"$f":"(AD3445)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3445>0,(AJ3445*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3444,NA())","v":{"$error":"#N/A"}},null,3428,{"$f":"IF(AF3445<=$J$9*0.05,AS3444*EXP((-$J$6*1)/Heterogenität!$D$4),Z3445)","v":1.8974390091611846E-4},{"$f":"IF(OR(AF3445>=$J$19, AR3444/$J$5<AN3445),0, Bodencharakterisierung!$E$8*$J$11*((AR3444/$J$5)-AN3445))","v":1.5096482821345266E-5},1.9673496492674826E-6,{"$f":"AQ3444-AP3445*Bodencharakterisierung!$E$8","v":5.9639763913981142E-4},{"$f":"AQ3445/(Bodencharakterisierung!$E$11*1000)","v":3.9366180801307685E-7},1.9171125056538594E-4,{"$error":"#N/A"},null,{"$f":"(AP3445)*$G$11*Bodencharakterisierung!$E$8","v":2.8449644751201859E-8},{"$f":"IF(AF3445<=$J$9*1.05,(AV3445*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3444,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,21.502609919999614,null,0.39366180801307687,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,189.74390091611846]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3435,2.3718990397197153E-14,{"$f":"Z3452*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3475585029482494E-14},{"$f":"AF3451*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3452^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3452)*3600*24","v":0},0,{"$f":"AE3451-AD3452*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3452>$J$18,(AE3452/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.3475585029482494E-14,{"$error":"#N/A"},null,{"$f":"(AD3452)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3452>0,(AJ3452*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3451,NA())","v":{"$error":"#N/A"}},null,3435,{"$f":"IF(AF3452<=$J$9*0.05,AS3451*EXP((-$J$6*1)/Heterogenität!$D$4),Z3452)","v":1.8974390091611846E-4},{"$f":"IF(OR(AF3452>=$J$19, AR3451/$J$5<AN3452),0, Bodencharakterisierung!$E$8*$J$11*((AR3451/$J$5)-AN3452))","v":8.6632698613987428E-7},8.6632698613987428E-7,{"$f":"AQ3451-AP3452*Bodencharakterisierung!$E$8","v":5.9221639892883561E-4},{"$f":"AQ3452/(Bodencharakterisierung!$E$11*1000)","v":3.9090191348437996E-7},1.9061022790225834E-4,{"$error":"#N/A"},null,{"$f":"(AP3452)*$G$11*Bodencharakterisierung!$E$8","v":1.2527867124807061E-8},{"$f":"IF(AF3452<=$J$9*1.05,(AV3452*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3451,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,21.546518399999606,null,0.39090191348437997,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,189.74390091611846]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3446,2.1174768529441159E-14,{"$f":"Z3463*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.0957472083265673E-14},{"$f":"AF3462*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3463^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3463)*3600*24","v":0},0,{"$f":"AE3462-AD3463*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3463>$J$18,(AE3463/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.0957472083265673E-14,{"$error":"#N/A"},null,{"$f":"(AD3463)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3463>0,(AJ3463*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3462,NA())","v":{"$error":"#N/A"}},null,3446,{"$f":"IF(AF3463<=$J$9*0.05,AS3462*EXP((-$J$6*1)/Heterogenität!$D$4),Z3463)","v":1.8722809254107984E-4},{"$f":"IF(OR(AF3463>=$J$19, AR3462/$J$5<AN3463),0, Bodencharakterisierung!$E$8*$J$11*((AR3462/$J$5)-AN3463))","v":5.8965048549310097E-6},1.9412646225532677E-6,{"$f":"AQ3462-AP3463*Bodencharakterisierung!$E$8","v":5.856158188550885E-4},{"$f":"AQ3463/(Bodencharakterisierung!$E$11*1000)","v":3.8654509495385378E-7},1.8916935716363311E-4,{"$error":"#N/A"},null,{"$f":"(AP3463)*$G$11*Bodencharakterisierung!$E$8","v":2.8072431812148885E-8},{"$f":"IF(AF3463<=$J$9*1.05,(AV3463*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3462,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,21.615517439999593,null,0.38654509495385375,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,187.22809254107983]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3453,1.9699728684001527E-14,{"$f":"Z3470*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.9497569164396721E-14},{"$f":"AF3469*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3470^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3470)*3600*24","v":0},0,{"$f":"AE3469-AD3470*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3470>$J$18,(AE3470/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.9497569164396721E-14,{"$error":"#N/A"},null,{"$f":"(AD3470)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3470>0,(AJ3470*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3469,NA())","v":{"$error":"#N/A"}},null,3453,{"$f":"IF(AF3470<=$J$9*0.05,AS3469*EXP((-$J$6*1)/Heterogenität!$D$4),Z3470)","v":1.8573113338675492E-4},{"$f":"IF(OR(AF3470>=$J$19, AR3469/$J$5<AN3470),0, Bodencharakterisierung!$E$8*$J$11*((AR3469/$J$5)-AN3470))","v":8.0966372726525476E-6},1.9257434803557642E-6,{"$f":"AQ3469-AP3470*Bodencharakterisierung!$E$8","v":5.8165129569364533E-4},{"$f":"AQ3470/(Bodencharakterisierung!$E$11*1000)","v":3.8392824798260419E-7},1.8765687686711068E-4,{"$error":"#N/A"},null,{"$f":"(AP3470)*$G$11*Bodencharakterisierung!$E$8","v":2.7847982141081887E-8},{"$f":"IF(AF3470<=$J$9*1.05,(AV3470*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3469,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,21.659425919999585,null,0.38392824798260416,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,185.73113338675492]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3465,1.7406158821652748E-14,{"$f":"Z3482*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.7227536021207381E-14},{"$f":"AF3481*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3482^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3482)*3600*24","v":0},0,{"$f":"AE3481-AD3482*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3482>$J$18,(AE3482/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.7227536021207381E-14,{"$error":"#N/A"},null,{"$f":"(AD3482)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3482>0,(AJ3482*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3481,NA())","v":{"$error":"#N/A"}},null,3465,{"$f":"IF(AF3482<=$J$9*0.05,AS3481*EXP((-$J$6*1)/Heterogenität!$D$4),Z3482)","v":1.8396083288301033E-4},{"$f":"IF(OR(AF3482>=$J$19, AR3481/$J$5<AN3482),0, Bodencharakterisierung!$E$8*$J$11*((AR3481/$J$5)-AN3482))","v":3.5004377474118729E-6},1.907388212764419E-6,{"$f":"AQ3481-AP3482*Bodencharakterisierung!$E$8","v":5.7466406582241882E-4},{"$f":"AQ3482/(Bodencharakterisierung!$E$11*1000)","v":3.7931621506430284E-7},1.8586822109577475E-4,{"$error":"#N/A"},null,{"$f":"(AP3482)*$G$11*Bodencharakterisierung!$E$8","v":2.7582548468688441E-8},{"$f":"IF(AF3482<=$J$9*1.05,(AV3482*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3481,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,21.734697599999571,null,0.37931621506430285,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,183.96083288301034]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3477,1.5379621201110765E-14,{"$f":"Z3494*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.5221794822707622E-14},{"$f":"AF3493*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3494^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3494)*3600*24","v":0},0,{"$f":"AE3493-AD3494*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3494>$J$18,(AE3494/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.5221794822707622E-14,{"$error":"#N/A"},null,{"$f":"(AD3494)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3494>0,(AJ3494*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3493,NA())","v":{"$error":"#N/A"}},null,3477,{"$f":"IF(AF3494<=$J$9*0.05,AS3493*EXP((-$J$6*1)/Heterogenität!$D$4),Z3494)","v":1.8199327325805022E-4},{"$f":"IF(OR(AF3494>=$J$19, AR3493/$J$5<AN3494),0, Bodencharakterisierung!$E$8*$J$11*((AR3493/$J$5)-AN3494))","v":1.2810163680096453E-6},1.2810163680096453E-6,{"$f":"AQ3493-AP3494*Bodencharakterisierung!$E$8","v":5.6802085315723076E-4},{"$f":"AQ3494/(Bodencharakterisierung!$E$11*1000)","v":3.7493125620939325E-7},1.8327428962605988E-4,{"$error":"#N/A"},null,{"$f":"(AP3494)*$G$11*Bodencharakterisierung!$E$8","v":1.8524648429382596E-8},{"$f":"IF(AF3494<=$J$9*1.05,(AV3494*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3493,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,21.809969279999557,null,0.37493125620939327,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,181.99327325805024]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3484,1.4308272815513785E-14,{"$f":"Z3501*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.4161440663398519E-14},{"$f":"AF3500*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3501^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3501)*3600*24","v":0},0,{"$f":"AE3500-AD3501*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3501>$J$18,(AE3501/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.4161440663398519E-14,{"$error":"#N/A"},null,{"$f":"(AD3501)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3501>0,(AJ3501*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3500,NA())","v":{"$error":"#N/A"}},null,3484,{"$f":"IF(AF3501<=$J$9*0.05,AS3500*EXP((-$J$6*1)/Heterogenität!$D$4),Z3501)","v":1.7953205182754599E-4},{"$f":"IF(OR(AF3501>=$J$19, AR3500/$J$5<AN3501),0, Bodencharakterisierung!$E$8*$J$11*((AR3500/$J$5)-AN3501))","v":1.4334079957087059E-5},1.8614686295046693E-6,{"$f":"AQ3500-AP3501*Bodencharakterisierung!$E$8","v":5.6431603773670215E-4},{"$f":"AQ3501/(Bodencharakterisierung!$E$11*1000)","v":3.7248583348957239E-7},1.8139352045705066E-4,{"$error":"#N/A"},null,{"$f":"(AP3501)*$G$11*Bodencharakterisierung!$E$8","v":2.6918510008951742E-8},{"$f":"IF(AF3501<=$J$9*1.05,(AV3501*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3500,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,21.853877759999548,null,0.37248583348957237,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,179.53205182754598]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3495,1.2773493300136496E-14,{"$f":"Z3512*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.2642411125825744E-14},{"$f":"AF3511*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3512^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3512)*3600*24","v":0},0,{"$f":"AE3511-AD3512*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3512>$J$18,(AE3512/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.2642411125825744E-14,{"$error":"#N/A"},null,{"$f":"(AD3512)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3512>0,(AJ3512*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3511,NA())","v":{"$error":"#N/A"}},null,3495,{"$f":"IF(AF3512<=$J$9*0.05,AS3511*EXP((-$J$6*1)/Heterogenität!$D$4),Z3512)","v":1.7855053850238128E-4},{"$f":"IF(OR(AF3512>=$J$19, AR3511/$J$5<AN3512),0, Bodencharakterisierung!$E$8*$J$11*((AR3511/$J$5)-AN3512))","v":3.824658504533919E-6},1.8512918602557507E-6,{"$f":"AQ3511-AP3512*Bodencharakterisierung!$E$8","v":5.5789959767816558E-4},{"$f":"AQ3512/(Bodencharakterisierung!$E$11*1000)","v":3.6825055952354164E-7},1.8040183036263703E-4,{"$error":"#N/A"},null,{"$f":"(AP3512)*$G$11*Bodencharakterisierung!$E$8","v":2.67713447757892E-8},{"$f":"IF(AF3512<=$J$9*1.05,(AV3512*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3511,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,21.922876799999536,null,0.36825055952354163,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,178.55053850238127]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3502,1.1883688457313275E-14,{"$f":"Z3519*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.1761737501124996E-14},{"$f":"AF3518*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3519^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3519)*3600*24","v":0},0,{"$f":"AE3518-AD3519*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3519>$J$18,(AE3519/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.1761737501124996E-14,{"$error":"#N/A"},null,{"$f":"(AD3519)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3519>0,(AJ3519*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3518,NA())","v":{"$error":"#N/A"}},null,3502,{"$f":"IF(AF3519<=$J$9*0.05,AS3518*EXP((-$J$6*1)/Heterogenität!$D$4),Z3519)","v":1.767182446841352E-4},{"$f":"IF(OR(AF3519>=$J$19, AR3518/$J$5<AN3519),0, Bodencharakterisierung!$E$8*$J$11*((AR3518/$J$5)-AN3519))","v":1.0332766881125133E-5},1.8322938182460788E-6,{"$f":"AQ3518-AP3519*Bodencharakterisierung!$E$8","v":5.5426538656417528E-4},{"$f":"AQ3519/(Bodencharakterisierung!$E$11*1000)","v":3.6585174030638634E-7},1.7855053850238128E-4,{"$error":"#N/A"},null,{"$f":"(AP3519)*$G$11*Bodencharakterisierung!$E$8","v":2.6496616007395225E-8},{"$f":"IF(AF3519<=$J$9*1.05,(AV3519*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3518,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,21.966785279999527,null,0.36585174030638634,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,176.71824468413521]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3505,1.1521577145066796E-14,{"$f":"Z3522*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.1403342191778937E-14},{"$f":"AF3521*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3522^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3522)*3600*24","v":0},0,{"$f":"AE3521-AD3522*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3522>$J$18,(AE3522/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.1403342191778937E-14,{"$error":"#N/A"},null,{"$f":"(AD3522)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3522>0,(AJ3522*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3521,NA())","v":{"$error":"#N/A"}},null,3505,{"$f":"IF(AF3522<=$J$9*0.05,AS3521*EXP((-$J$6*1)/Heterogenität!$D$4),Z3522)","v":1.767182446841352E-4},{"$f":"IF(OR(AF3522>=$J$19, AR3521/$J$5<AN3522),0, Bodencharakterisierung!$E$8*$J$11*((AR3521/$J$5)-AN3522))","v":4.6527917402625216E-6},1.8322938182460788E-6,{"$f":"AQ3521-AP3522*Bodencharakterisierung!$E$8","v":5.5245141568411173E-4},{"$f":"AQ3522/(Bodencharakterisierung!$E$11*1000)","v":3.6465439979149289E-7},1.7855053850238128E-4,{"$error":"#N/A"},null,{"$f":"(AP3522)*$G$11*Bodencharakterisierung!$E$8","v":2.6496616007395225E-8},{"$f":"IF(AF3522<=$J$9*1.05,(AV3522*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3521,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,21.985603199999524,null,0.36465439979149289,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,176.71824468413521]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3517,1.0180160594080878E-14,{"$f":"Z3534*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.0075691318985201E-14},{"$f":"AF3533*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3534^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3534)*3600*24","v":0},0,{"$f":"AE3533-AD3534*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3534>$J$18,(AE3534/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.0075691318985201E-14,{"$error":"#N/A"},null,{"$f":"(AD3534)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3534>0,(AJ3534*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3533,NA())","v":{"$error":"#N/A"}},null,3517,{"$f":"IF(AF3534<=$J$9*0.05,AS3533*EXP((-$J$6*1)/Heterogenität!$D$4),Z3534)","v":1.7422674541104071E-4},{"$f":"IF(OR(AF3534>=$J$19, AR3533/$J$5<AN3534),0, Bodencharakterisierung!$E$8*$J$11*((AR3533/$J$5)-AN3534))","v":9.0258739163956898E-6},1.8064608391758232E-6,{"$f":"AQ3533-AP3534*Bodencharakterisierung!$E$8","v":5.460801113896114E-4},{"$f":"AQ3534/(Bodencharakterisierung!$E$11*1000)","v":3.6044891840898443E-7},1.7603320625021653E-4,{"$error":"#N/A"},null,{"$f":"(AP3534)*$G$11*Bodencharakterisierung!$E$8","v":2.6123047903887215E-8},{"$f":"IF(AF3534<=$J$9*1.05,(AV3534*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3533,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,22.06087487999951,null,0.36044891840898441,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,174.2267454110407]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3524,9.4710079774482397E-15,{"$f":"Z3541*EXP((-$J$6/Heterogenität!$D$4)*1)","v":9.3738160590413049E-15},{"$f":"AF3540*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3541^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3541)*3600*24","v":0},0,{"$f":"AE3540-AD3541*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3541>$J$18,(AE3541/(Bodencharakterisierung!$E$11*1000)),0)","v":0},9.3738160590413049E-15,{"$error":"#N/A"},null,{"$f":"(AD3541)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3541>0,(AJ3541*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3540,NA())","v":{"$error":"#N/A"}},null,3524,{"$f":"IF(AF3541<=$J$9*0.05,AS3540*EXP((-$J$6*1)/Heterogenität!$D$4),Z3541)","v":1.7266623346334919E-4},{"$f":"IF(OR(AF3541>=$J$19, AR3540/$J$5<AN3541),0, Bodencharakterisierung!$E$8*$J$11*((AR3540/$J$5)-AN3541))","v":1.2845052610290415E-5},1.7902807531854786E-6,{"$f":"AQ3540-AP3541*Bodencharakterisierung!$E$8","v":5.4243450833702661E-4},{"$f":"AQ3541/(Bodencharakterisierung!$E$11*1000)","v":3.5804257976041359E-7},1.7445651421653467E-4,{"$error":"#N/A"},null,{"$f":"(AP3541)*$G$11*Bodencharakterisierung!$E$8","v":2.5889069313126498E-8},{"$f":"IF(AF3541<=$J$9*1.05,(AV3541*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3540,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,22.104783359999502,null,0.35804257976041359,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,172.66623346334919]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3536,8.3683319552763534E-15,{"$f":"Z3553*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.2824557488011792E-15},{"$f":"AF3552*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3553^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3553)*3600*24","v":0},0,{"$f":"AE3552-AD3553*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3553>$J$18,(AE3553/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.2824557488011792E-15,{"$error":"#N/A"},null,{"$f":"(AD3553)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3553>0,(AJ3553*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3552,NA())","v":{"$error":"#N/A"}},null,3536,{"$f":"IF(AF3553<=$J$9*0.05,AS3552*EXP((-$J$6*1)/Heterogenität!$D$4),Z3553)","v":1.7122096310989932E-4},{"$f":"IF(OR(AF3553>=$J$19, AR3552/$J$5<AN3553),0, Bodencharakterisierung!$E$8*$J$11*((AR3552/$J$5)-AN3553))","v":6.3422816632736589E-6},1.7752955435991447E-6,{"$f":"AQ3552-AP3553*Bodencharakterisierung!$E$8","v":5.3585175787381064E-4},{"$f":"AQ3553/(Bodencharakterisierung!$E$11*1000)","v":3.5369752994971E-7},1.7299625865349846E-4,{"$error":"#N/A"},null,{"$f":"(AP3553)*$G$11*Bodencharakterisierung!$E$8","v":2.5672369709468224E-8},{"$f":"IF(AF3553<=$J$9*1.05,(AV3553*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3552,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,22.180055039999488,null,0.35369752994970999,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,171.22096310989932]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3547,7.4707012888475092E-15,{"$f":"Z3564*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.3940366094557092E-15},{"$f":"AF3563*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3564^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3564)*3600*24","v":0},0,{"$f":"AE3563-AD3564*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3564>$J$18,(AE3564/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.3940366094557092E-15,{"$error":"#N/A"},null,{"$f":"(AD3564)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3564>0,(AJ3564*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3563,NA())","v":{"$error":"#N/A"}},null,3547,{"$f":"IF(AF3564<=$J$9*0.05,AS3563*EXP((-$J$6*1)/Heterogenität!$D$4),Z3564)","v":1.6878984090159366E-4},{"$f":"IF(OR(AF3564>=$J$19, AR3563/$J$5<AN3564),0, Bodencharakterisierung!$E$8*$J$11*((AR3563/$J$5)-AN3564))","v":1.2547476923404547E-5},1.7500885809471447E-6,{"$f":"AQ3563-AP3564*Bodencharakterisierung!$E$8","v":5.3025380307475151E-4},{"$f":"AQ3564/(Bodencharakterisierung!$E$11*1000)","v":3.5000251028036402E-7},1.7053992948254081E-4,{"$error":"#N/A"},null,{"$f":"(AP3564)*$G$11*Bodencharakterisierung!$E$8","v":2.5307854366212779E-8},{"$f":"IF(AF3564<=$J$9*1.05,(AV3564*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3563,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,22.249054079999475,null,0.350002510280364,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,168.78984090159366]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3554,6.950290307300968E-15,{"$f":"Z3571*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.8789661092789422E-15},{"$f":"AF3570*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3571^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3571)*3600*24","v":0},0,{"$f":"AE3570-AD3571*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3571>$J$18,(AE3571/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.8789661092789422E-15,{"$error":"#N/A"},null,{"$f":"(AD3571)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3571>0,(AJ3571*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3570,NA())","v":{"$error":"#N/A"}},null,3554,{"$f":"IF(AF3571<=$J$9*0.05,AS3570*EXP((-$J$6*1)/Heterogenität!$D$4),Z3571)","v":1.6873748213679218E-4},{"$f":"IF(OR(AF3571>=$J$19, AR3570/$J$5<AN3571),0, Bodencharakterisierung!$E$8*$J$11*((AR3570/$J$5)-AN3571))","v":4.5518014715335381E-7},4.5518014715335381E-7,{"$f":"AQ3570-AP3571*Bodencharakterisierung!$E$8","v":5.2665587577840195E-4},{"$f":"AQ3571/(Bodencharakterisierung!$E$11*1000)","v":3.4762764077782306E-7},1.6919266228394554E-4,{"$error":"#N/A"},null,{"$f":"(AP3571)*$G$11*Bodencharakterisierung!$E$8","v":6.5823141753853267E-9},{"$f":"IF(AF3571<=$J$9*1.05,(AV3571*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3570,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,22.292962559999467,null,0.34762764077782304,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,168.73748213679218]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3566,6.1410925442705428E-15,{"$f":"Z3583*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.0780723708197978E-15},{"$f":"AF3582*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3583^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3583)*3600*24","v":0},0,{"$f":"AE3582-AD3583*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3583>$J$18,(AE3583/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.0780723708197978E-15,{"$error":"#N/A"},null,{"$f":"(AD3583)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3583>0,(AJ3583*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3582,NA())","v":{"$error":"#N/A"}},null,3566,{"$f":"IF(AF3583<=$J$9*0.05,AS3582*EXP((-$J$6*1)/Heterogenität!$D$4),Z3583)","v":1.6573795416682758E-4},{"$f":"IF(OR(AF3583>=$J$19, AR3582/$J$5<AN3583),0, Bodencharakterisierung!$E$8*$J$11*((AR3582/$J$5)-AN3583))","v":1.1414016532082917E-5},1.7184452539771881E-6,{"$f":"AQ3582-AP3583*Bodencharakterisierung!$E$8","v":5.2037676082929694E-4},{"$f":"AQ3583/(Bodencharakterisierung!$E$11*1000)","v":3.4348301044838082E-7},1.6745639942080477E-4,{"$error":"#N/A"},null,{"$f":"(AP3583)*$G$11*Bodencharakterisierung!$E$8","v":2.4850263408054134E-8},{"$f":"IF(AF3583<=$J$9*1.05,(AV3583*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3582,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,22.368234239999452,null,0.34348301044838081,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,165.73795416682759]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3567,6.0780723708197978E-15,{"$f":"Z3584*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.0156989132804533E-15},{"$f":"AF3583*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3584^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3584)*3600*24","v":0},0,{"$f":"AE3583-AD3584*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3584>$J$18,(AE3584/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.0156989132804533E-15,{"$error":"#N/A"},null,{"$f":"(AD3584)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3584>0,(AJ3584*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3583,NA())","v":{"$error":"#N/A"}},null,3567,{"$f":"IF(AF3584<=$J$9*0.05,AS3583*EXP((-$J$6*1)/Heterogenität!$D$4),Z3584)","v":1.6573795416682758E-4},{"$f":"IF(OR(AF3584>=$J$19, AR3583/$J$5<AN3584),0, Bodencharakterisierung!$E$8*$J$11*((AR3583/$J$5)-AN3584))","v":9.638332191080348E-6},1.7184452539771881E-6,{"$f":"AQ3583-AP3584*Bodencharakterisierung!$E$8","v":5.1980967389548443E-4},{"$f":"AQ3584/(Bodencharakterisierung!$E$11*1000)","v":3.4310869564058379E-7},1.6745639942080477E-4,{"$error":"#N/A"},null,{"$f":"(AP3584)*$G$11*Bodencharakterisierung!$E$8","v":2.4850263408054134E-8},{"$f":"IF(AF3584<=$J$9*1.05,(AV3584*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3583,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,22.374506879999451,null,0.34310869564058377,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,165.73795416682759]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3575,5.5966437730592462E-15,{"$f":"Z3592*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.5392107578787004E-15},{"$f":"AF3591*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3592^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3592)*3600*24","v":0},0,{"$f":"AE3591-AD3592*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3592>$J$18,(AE3592/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.5392107578787004E-15,{"$error":"#N/A"},null,{"$f":"(AD3592)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3592>0,(AJ3592*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3591,NA())","v":{"$error":"#N/A"}},null,3575,{"$f":"IF(AF3592<=$J$9*0.05,AS3591*EXP((-$J$6*1)/Heterogenität!$D$4),Z3592)","v":1.6478925592668581E-4},{"$f":"IF(OR(AF3592>=$J$19, AR3591/$J$5<AN3592),0, Bodencharakterisierung!$E$8*$J$11*((AR3591/$J$5)-AN3592))","v":5.7154379522405921E-6},1.7086087262100681E-6,{"$f":"AQ3591-AP3592*Bodencharakterisierung!$E$8","v":5.1559903306088394E-4},{"$f":"AQ3592/(Bodencharakterisierung!$E$11*1000)","v":3.4032939475965938E-7},1.6649786465289587E-4,{"$error":"#N/A"},null,{"$f":"(AP3592)*$G$11*Bodencharakterisierung!$E$8","v":2.4708018372625839E-8},{"$f":"IF(AF3592<=$J$9*1.05,(AV3592*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3591,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,22.424687999999442,null,0.3403293947596594,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,164.7892559266858]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3587,4.9450462970688674E-15,{"$f":"Z3604*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.8943000050830882E-15},{"$f":"AF3603*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3604^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3604)*3600*24","v":0},0,{"$f":"AE3603-AD3604*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3604>$J$18,(AE3604/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.8943000050830882E-15,{"$error":"#N/A"},null,{"$f":"(AD3604)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3604>0,(AJ3604*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3603,NA())","v":{"$error":"#N/A"}},null,3587,{"$f":"IF(AF3604<=$J$9*0.05,AS3603*EXP((-$J$6*1)/Heterogenität!$D$4),Z3604)","v":1.6203129982739325E-4},{"$f":"IF(OR(AF3604>=$J$19, AR3603/$J$5<AN3604),0, Bodencharakterisierung!$E$8*$J$11*((AR3603/$J$5)-AN3604))","v":1.4471948897881315E-5},1.6800130035626339E-6,{"$f":"AQ3603-AP3604*Bodencharakterisierung!$E$8","v":5.0979688233840435E-4},{"$f":"AQ3604/(Bodencharakterisierung!$E$11*1000)","v":3.3649959230257714E-7},1.6371131283095589E-4,{"$error":"#N/A"},null,{"$f":"(AP3604)*$G$11*Bodencharakterisierung!$E$8","v":2.4294498513038951E-8},{"$f":"IF(AF3604<=$J$9*1.05,(AV3604*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3603,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,{"$f":"$G$34/$G$12/$G$8+BC3603","v":22.499959679999428},null,0.33649959230257714,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,162.03129982739324]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3594,4.6005730946544663E-15,{"$f":"Z3611*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.5533618024767495E-15},{"$f":"AF3610*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3611^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3611)*3600*24","v":0},0,{"$f":"AE3610-AD3611*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3611>$J$18,(AE3611/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.5533618024767495E-15,{"$error":"#N/A"},null,{"$f":"(AD3611)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3611>0,(AJ3611*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3610,NA())","v":{"$error":"#N/A"}},null,3594,{"$f":"IF(AF3611<=$J$9*0.05,AS3610*EXP((-$J$6*1)/Heterogenität!$D$4),Z3611)","v":1.6203129982739325E-4},{"$f":"IF(OR(AF3611>=$J$19, AR3610/$J$5<AN3611),0, Bodencharakterisierung!$E$8*$J$11*((AR3610/$J$5)-AN3611))","v":2.3201451477093986E-6},1.6800130035626339E-6,{"$f":"AQ3610-AP3611*Bodencharakterisierung!$E$8","v":5.0591605230017463E-4},{"$f":"AQ3611/(Bodencharakterisierung!$E$11*1000)","v":3.3393798831694696E-7},1.6371131283095589E-4,{"$error":"#N/A"},null,{"$f":"(AP3611)*$G$11*Bodencharakterisierung!$E$8","v":2.4294498513038951E-8},{"$f":"IF(AF3611<=$J$9*1.05,(AV3611*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3610,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,22.54386815999942,null,0.33393798831694699,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,162.03129982739324]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3606,4.0649446112022352E-15,{"$f":"Z3623*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.0232299630970479E-15},{"$f":"AF3622*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3623^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3623)*3600*24","v":0},0,{"$f":"AE3622-AD3623*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3623>$J$18,(AE3623/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.0232299630970479E-15,{"$error":"#N/A"},null,{"$f":"(AD3623)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3623>0,(AJ3623*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3622,NA())","v":{"$error":"#N/A"}},null,3606,{"$f":"IF(AF3623<=$J$9*0.05,AS3622*EXP((-$J$6*1)/Heterogenität!$D$4),Z3623)","v":1.5952701401849193E-4},{"$f":"IF(OR(AF3623>=$J$19, AR3622/$J$5<AN3623),0, Bodencharakterisierung!$E$8*$J$11*((AR3622/$J$5)-AN3623))","v":8.7396572247377727E-6},1.6540474479689155E-6,{"$f":"AQ3622-AP3623*Bodencharakterisierung!$E$8","v":5.0015843552989872E-4},{"$f":"AQ3623/(Bodencharakterisierung!$E$11*1000)","v":3.3013758120785392E-7},1.6118106146646084E-4,{"$error":"#N/A"},null,{"$f":"(AP3623)*$G$11*Bodencharakterisierung!$E$8","v":2.3919013233803548E-8},{"$f":"IF(AF3623<=$J$9*1.05,(AV3623*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3622,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,22.619139839999406,null,0.33013758120785391,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,159.52701401849194]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3616,3.6665438207017051E-15,{"$f":"Z3633*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.6289175797877888E-15},{"$f":"AF3632*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3633^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3633)*3600*24","v":0},0,{"$f":"AE3632-AD3633*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3633>$J$18,(AE3633/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.6289175797877888E-15,{"$error":"#N/A"},null,{"$f":"(AD3633)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3633>0,(AJ3633*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3632,NA())","v":{"$error":"#N/A"}},null,3616,{"$f":"IF(AF3633<=$J$9*0.05,AS3632*EXP((-$J$6*1)/Heterogenität!$D$4),Z3633)","v":1.5808189973078309E-4},{"$f":"IF(OR(AF3633>=$J$19, AR3632/$J$5<AN3633),0, Bodencharakterisierung!$E$8*$J$11*((AR3632/$J$5)-AN3633))","v":7.3422530554777635E-6},1.6390638565419913E-6,{"$f":"AQ3632-AP3633*Bodencharakterisierung!$E$8","v":4.9520663417757058E-4},{"$f":"AQ3633/(Bodencharakterisierung!$E$11*1000)","v":3.2686906546374298E-7},1.5972096358732508E-4,{"$error":"#N/A"},null,{"$f":"(AP3633)*$G$11*Bodencharakterisierung!$E$8","v":2.3702337030185211E-8},{"$f":"IF(AF3633<=$J$9*1.05,(AV3633*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3632,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,22.681866239999394,null,0.326869065463743,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,158.08189973078308]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3624,3.3761262437899061E-15,{"$f":"Z3641*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.3414802813750007E-15},{"$f":"AF3640*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3641^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3641)*3600*24","v":0},0,{"$f":"AE3640-AD3641*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3641>$J$18,(AE3641/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.3414802813750007E-15,{"$error":"#N/A"},null,{"$f":"(AD3641)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3641>0,(AJ3641*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3640,NA())","v":{"$error":"#N/A"}},null,3624,{"$f":"IF(AF3641<=$J$9*0.05,AS3640*EXP((-$J$6*1)/Heterogenität!$D$4),Z3641)","v":1.5702144873370186E-4},{"$f":"IF(OR(AF3641>=$J$19, AR3640/$J$5<AN3641),0, Bodencharakterisierung!$E$8*$J$11*((AR3640/$J$5)-AN3641))","v":5.298169915604251E-6},1.6280686261967853E-6,{"$f":"AQ3640-AP3641*Bodencharakterisierung!$E$8","v":4.9124759655540598E-4},{"$f":"AQ3641/(Bodencharakterisierung!$E$11*1000)","v":3.24255839310499E-7},1.5864951735989865E-4,{"$error":"#N/A"},null,{"$f":"(AP3641)*$G$11*Bodencharakterisierung!$E$8","v":2.3543336113700835E-8},{"$f":"IF(AF3641<=$J$9*1.05,(AV3641*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3640,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,22.732047359999385,null,0.32425583931049901,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,157.02144873370187]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3636,2.9830557843713528E-15,{"$f":"Z3653*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.9524435290455928E-15},{"$f":"AF3652*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3653^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3653)*3600*24","v":0},0,{"$f":"AE3652-AD3653*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3653>$J$18,(AE3653/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.9524435290455928E-15,{"$error":"#N/A"},null,{"$f":"(AD3653)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3653>0,(AJ3653*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3652,NA())","v":{"$error":"#N/A"}},null,3636,{"$f":"IF(AF3653<=$J$9*0.05,AS3652*EXP((-$J$6*1)/Heterogenität!$D$4),Z3653)","v":1.5565878654430994E-4},{"$f":"IF(OR(AF3653>=$J$19, AR3652/$J$5<AN3653),0, Bodencharakterisierung!$E$8*$J$11*((AR3652/$J$5)-AN3653))","v":0},0,{"$f":"AQ3652-AP3653*Bodencharakterisierung!$E$8","v":4.8582934817763176E-4},{"$f":"AQ3653/(Bodencharakterisierung!$E$11*1000)","v":3.2067943774101106E-7},1.5565878654430994E-4,{"$error":"#N/A"},null,{"$f":"(AP3653)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF3653<=$J$9*1.05,(AV3653*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3652,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,22.807319039999371,null,0.32067943774101104,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,155.65878654430995]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3643,2.7752553478754809E-15,{"$f":"Z3660*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.7467755501632E-15},{"$f":"AF3659*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3660^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3660)*3600*24","v":0},0,{"$f":"AE3659-AD3660*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3660>$J$18,(AE3660/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.7467755501632E-15,{"$error":"#N/A"},null,{"$f":"(AD3660)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3660>0,(AJ3660*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3659,NA())","v":{"$error":"#N/A"}},null,3643,{"$f":"IF(AF3660<=$J$9*0.05,AS3659*EXP((-$J$6*1)/Heterogenität!$D$4),Z3660)","v":1.5406140893496143E-4},{"$f":"IF(OR(AF3660>=$J$19, AR3659/$J$5<AN3660),0, Bodencharakterisierung!$E$8*$J$11*((AR3659/$J$5)-AN3660))","v":5.6755153318332601E-6},1.5973776093485123E-6,{"$f":"AQ3659-AP3660*Bodencharakterisierung!$E$8","v":4.8213940590003654E-4},{"$f":"AQ3660/(Bodencharakterisierung!$E$11*1000)","v":3.1824383227725183E-7},1.5565878654430994E-4,{"$error":"#N/A"},null,{"$f":"(AP3660)*$G$11*Bodencharakterisierung!$E$8","v":2.3099516416113458E-8},{"$f":"IF(AF3660<=$J$9*1.05,(AV3660*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3659,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,22.851227519999362,null,0.31824383227725184,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,154.06140893496143]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3646,2.6906897385153839E-15,{"$f":"Z3663*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.6630777569663382E-15},{"$f":"AF3662*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3663^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3663)*3600*24","v":0},0,{"$f":"AE3662-AD3663*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3663>$J$18,(AE3663/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.6630777569663382E-15,{"$error":"#N/A"},null,{"$f":"(AD3663)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3663>0,(AJ3663*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3662,NA())","v":{"$error":"#N/A"}},null,3646,{"$f":"IF(AF3663<=$J$9*0.05,AS3662*EXP((-$J$6*1)/Heterogenität!$D$4),Z3663)","v":1.5406140893496143E-4},{"$f":"IF(OR(AF3663>=$J$19, AR3662/$J$5<AN3663),0, Bodencharakterisierung!$E$8*$J$11*((AR3662/$J$5)-AN3663))","v":7.2376304116816625E-7},7.2376304116816625E-7,{"$f":"AQ3662-AP3663*Bodencharakterisierung!$E$8","v":4.8084629487428097E-4},{"$f":"AQ3663/(Bodencharakterisierung!$E$11*1000)","v":3.1739029364639007E-7},1.547851719761296E-4,{"$error":"#N/A"},null,{"$f":"(AP3663)*$G$11*Bodencharakterisierung!$E$8","v":1.0466264302814976E-8},{"$f":"IF(AF3663<=$J$9*1.05,(AV3663*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3662,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,22.870045439999359,null,0.3173902936463901,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,154.06140893496143]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3657,2.4020724087960523E-15,{"$f":"Z3674*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3774222315267309E-15},{"$f":"AF3673*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3674^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3674)*3600*24","v":0},0,{"$f":"AE3673-AD3674*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3674>$J$18,(AE3674/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.3774222315267309E-15,{"$error":"#N/A"},null,{"$f":"(AD3674)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3674>0,(AJ3674*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3673,NA())","v":{"$error":"#N/A"}},null,3657,{"$f":"IF(AF3674<=$J$9*0.05,AS3673*EXP((-$J$6*1)/Heterogenität!$D$4),Z3674)","v":1.5184205066638319E-4},{"$f":"IF(OR(AF3674>=$J$19, AR3673/$J$5<AN3674),0, Bodencharakterisierung!$E$8*$J$11*((AR3673/$J$5)-AN3674))","v":6.7252583654570186E-6},1.574366309959154E-6,{"$f":"AQ3673-AP3674*Bodencharakterisierung!$E$8","v":4.7555522279037497E-4},{"$f":"AQ3674/(Bodencharakterisierung!$E$11*1000)","v":3.1389783682533001E-7},1.5341641697634234E-4,{"$error":"#N/A"},null,{"$f":"(AP3674)*$G$11*Bodencharakterisierung!$E$8","v":2.2766752337732909E-8},{"$f":"IF(AF3674<=$J$9*1.05,(AV3674*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3673,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,22.939044479999346,null,0.31389783682533001,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,151.84205066638319]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3664,2.2347434243172384E-15,{"$f":"Z3681*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.2118103847639135E-15},{"$f":"AF3680*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3681^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3681)*3600*24","v":0},0,{"$f":"AE3680-AD3681*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3681>$J$18,(AE3681/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.2118103847639135E-15,{"$error":"#N/A"},null,{"$f":"(AD3681)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3681>0,(AJ3681*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3680,NA())","v":{"$error":"#N/A"}},null,3664,{"$f":"IF(AF3681<=$J$9*0.05,AS3680*EXP((-$J$6*1)/Heterogenität!$D$4),Z3681)","v":1.5049963618678675E-4},{"$f":"IF(OR(AF3681>=$J$19, AR3680/$J$5<AN3681),0, Bodencharakterisierung!$E$8*$J$11*((AR3680/$J$5)-AN3681))","v":9.8875356256179543E-6},1.5604475560869501E-6,{"$f":"AQ3680-AP3681*Bodencharakterisierung!$E$8","v":4.7237980614774739E-4},{"$f":"AQ3681/(Bodencharakterisierung!$E$11*1000)","v":3.1180185224273753E-7},1.520600837428737E-4,{"$error":"#N/A"},null,{"$f":"(AP3681)*$G$11*Bodencharakterisierung!$E$8","v":2.2565474642539758E-8},{"$f":"IF(AF3681<=$J$9*1.05,(AV3681*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3680,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,22.982952959999338,null,0.31180185224273754,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,150.49963618678674]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3676,1.9745601370083802E-15,{"$f":"Z3693*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.9542971102869718E-15},{"$f":"AF3692*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3693^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3693)*3600*24","v":0},0,{"$f":"AE3692-AD3693*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3693>$J$18,(AE3693/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.9542971102869718E-15,{"$error":"#N/A"},null,{"$f":"(AD3693)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3693>0,(AJ3693*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3692,NA())","v":{"$error":"#N/A"}},null,3676,{"$f":"IF(AF3693<=$J$9*0.05,AS3692*EXP((-$J$6*1)/Heterogenität!$D$4),Z3693)","v":1.491660081870095E-4},{"$f":"IF(OR(AF3693>=$J$19, AR3692/$J$5<AN3693),0, Bodencharakterisierung!$E$8*$J$11*((AR3692/$J$5)-AN3693))","v":5.0360010726727282E-6},1.5466199043682365E-6,{"$f":"AQ3692-AP3693*Bodencharakterisierung!$E$8","v":4.6667247294103991E-4},{"$f":"AQ3693/(Bodencharakterisierung!$E$11*1000)","v":3.0803463560464681E-7},1.5071262809137774E-4,{"$error":"#N/A"},null,{"$f":"(AP3693)*$G$11*Bodencharakterisierung!$E$8","v":2.2365514366395034E-8},{"$f":"IF(AF3693<=$J$9*1.05,(AV3693*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3692,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,23.058224639999324,null,0.30803463560464683,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,149.16600818700951]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3683,1.837011767813481E-15,{"$f":"Z3700*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.8181602687676516E-15},{"$f":"AF3699*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3700^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3700)*3600*24","v":0},0,{"$f":"AE3699-AD3700*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3700>$J$18,(AE3700/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.8181602687676516E-15,{"$error":"#N/A"},null,{"$f":"(AD3700)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3700>0,(AJ3700*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3699,NA())","v":{"$error":"#N/A"}},null,3683,{"$f":"IF(AF3700<=$J$9*0.05,AS3699*EXP((-$J$6*1)/Heterogenität!$D$4),Z3700)","v":1.4787437442772934E-4},{"$f":"IF(OR(AF3700>=$J$19, AR3699/$J$5<AN3700),0, Bodencharakterisierung!$E$8*$J$11*((AR3699/$J$5)-AN3700))","v":7.8624178805574247E-6},1.5332276677217386E-6,{"$f":"AQ3699-AP3700*Bodencharakterisierung!$E$8","v":4.6354811729297849E-4},{"$f":"AQ3700/(Bodencharakterisierung!$E$11*1000)","v":3.0597235464883067E-7},1.4940760209545108E-4,{"$error":"#N/A"},null,{"$f":"(AP3700)*$G$11*Bodencharakterisierung!$E$8","v":2.2171850583671538E-8},{"$f":"IF(AF3700<=$J$9*1.05,(AV3700*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3699,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,23.102133119999316,null,0.30597235464883066,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,147.87437442772935]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3696,1.6064782875456448E-15,{"$f":"Z3713*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.5899925336515048E-15},{"$f":"AF3712*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3713^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3713)*3600*24","v":0},0,{"$f":"AE3712-AD3713*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3713>$J$18,(AE3713/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.5899925336515048E-15,{"$error":"#N/A"},null,{"$f":"(AD3713)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3713>0,(AJ3713*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3712,NA())","v":{"$error":"#N/A"}},null,3696,{"$f":"IF(AF3713<=$J$9*0.05,AS3712*EXP((-$J$6*1)/Heterogenität!$D$4),Z3713)","v":1.4637534612489613E-4},{"$f":"IF(OR(AF3713>=$J$19, AR3712/$J$5<AN3713),0, Bodencharakterisierung!$E$8*$J$11*((AR3712/$J$5)-AN3713))","v":3.5943372623226436E-6},1.5176850716668272E-6,{"$f":"AQ3712-AP3713*Bodencharakterisierung!$E$8","v":4.5751143853849731E-4},{"$f":"AQ3713/(Bodencharakterisierung!$E$11*1000)","v":3.0198774821022924E-7},1.4789303119656295E-4,{"$error":"#N/A"},null,{"$f":"(AP3713)*$G$11*Bodencharakterisierung!$E$8","v":2.1947090670537486E-8},{"$f":"IF(AF3713<=$J$9*1.05,(AV3713*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3712,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,23.1836774399993,null,0.30198774821022922,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,146.37534612489614]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3706,1.4490291016658819E-15,{"$f":"Z3723*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.4341590985412167E-15},{"$f":"AF3722*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3723^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3723)*3600*24","v":0},0,{"$f":"AE3722-AD3723*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3723>$J$18,(AE3723/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.4341590985412167E-15,{"$error":"#N/A"},null,{"$f":"(AD3723)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3723>0,(AJ3723*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3722,NA())","v":{"$error":"#N/A"}},null,3706,{"$f":"IF(AF3723<=$J$9*0.05,AS3722*EXP((-$J$6*1)/Heterogenität!$D$4),Z3723)","v":1.4472016162660238E-4},{"$f":"IF(OR(AF3723>=$J$19, AR3722/$J$5<AN3723),0, Bodencharakterisierung!$E$8*$J$11*((AR3722/$J$5)-AN3723))","v":5.8950841102965275E-6},1.500523378318748E-6,{"$f":"AQ3722-AP3723*Bodencharakterisierung!$E$8","v":4.5308573883066818E-4},{"$f":"AQ3723/(Bodencharakterisierung!$E$11*1000)","v":2.9906649427766876E-7},1.4622068500492113E-4,{"$error":"#N/A"},null,{"$f":"(AP3723)*$G$11*Bodencharakterisierung!$E$8","v":2.1698917154831367E-8},{"$f":"IF(AF3723<=$J$9*1.05,(AV3723*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3722,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,23.246403839999289,null,0.29906649427766874,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,144.72016162660239]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3713,1.3480893601434665E-15,{"$f":"Z3730*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.334255205277553E-15},{"$f":"AF3729*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3730^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3730)*3600*24","v":0},0,{"$f":"AE3729-AD3730*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3730>$J$18,(AE3730/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.334255205277553E-15,{"$error":"#N/A"},null,{"$f":"(AD3730)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3730>0,(AJ3730*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3729,NA())","v":{"$error":"#N/A"}},null,3713,{"$f":"IF(AF3730<=$J$9*0.05,AS3729*EXP((-$J$6*1)/Heterogenität!$D$4),Z3730)","v":1.4387038643933294E-4},{"$f":"IF(OR(AF3730>=$J$19, AR3729/$J$5<AN3730),0, Bodencharakterisierung!$E$8*$J$11*((AR3729/$J$5)-AN3730))","v":4.2482936732162042E-6},1.4917125290184023E-6,{"$f":"AQ3729-AP3730*Bodencharakterisierung!$E$8","v":4.4991041869310046E-4},{"$f":"AQ3730/(Bodencharakterisierung!$E$11*1000)","v":2.9697057339478576E-7},1.4536209896835134E-4,{"$error":"#N/A"},null,{"$f":"(AP3730)*$G$11*Bodencharakterisierung!$E$8","v":2.1571504352209045E-8},{"$f":"IF(AF3730<=$J$9*1.05,(AV3730*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3729,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,23.290312319999281,null,0.29697057339478578,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,143.87038643933295]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3716,1.3070113388724989E-15,{"$f":"Z3733*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.2935987285455821E-15},{"$f":"AF3732*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3733^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3733)*3600*24","v":0},0,{"$f":"AE3732-AD3733*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3733>$J$18,(AE3733/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.2935987285455821E-15,{"$error":"#N/A"},null,{"$f":"(AD3733)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3733>0,(AJ3733*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3732,NA())","v":{"$error":"#N/A"}},null,3716,{"$f":"IF(AF3733<=$J$9*0.05,AS3732*EXP((-$J$6*1)/Heterogenität!$D$4),Z3733)","v":1.4354751633391247E-4},{"$f":"IF(OR(AF3733>=$J$19, AR3732/$J$5<AN3733),0, Bodencharakterisierung!$E$8*$J$11*((AR3732/$J$5)-AN3733))","v":3.1166436146304817E-6},1.4883648673249758E-6,{"$f":"AQ3732-AP3733*Bodencharakterisierung!$E$8","v":4.4854237988087861E-4},{"$f":"AQ3733/(Bodencharakterisierung!$E$11*1000)","v":2.9606757747912782E-7},1.4503588120123745E-4,{"$error":"#N/A"},null,{"$f":"(AP3733)*$G$11*Bodencharakterisierung!$E$8","v":2.152309415427567E-8},{"$f":"IF(AF3733<=$J$9*1.05,(AV3733*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3732,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,23.309130239999277,null,0.29606757747912782,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,143.54751633391248]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3728,1.1548406229874324E-15,{"$f":"Z3745*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.1429895955287215E-15},{"$f":"AF3744*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3745^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3745)*3600*24","v":0},0,{"$f":"AE3744-AD3745*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3745>$J$18,(AE3745/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.1429895955287215E-15,{"$error":"#N/A"},null,{"$f":"(AD3745)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3745>0,(AJ3745*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3744,NA())","v":{"$error":"#N/A"}},null,3728,{"$f":"IF(AF3745<=$J$9*0.05,AS3744*EXP((-$J$6*1)/Heterogenität!$D$4),Z3745)","v":1.4211476986184012E-4},{"$f":"IF(OR(AF3745>=$J$19, AR3744/$J$5<AN3745),0, Bodencharakterisierung!$E$8*$J$11*((AR3744/$J$5)-AN3745))","v":2.9780706696076701E-7},2.9780706696076701E-7,{"$f":"AQ3744-AP3745*Bodencharakterisierung!$E$8","v":4.4356316809223469E-4},{"$f":"AQ3745/(Bodencharakterisierung!$E$11*1000)","v":2.927809690377787E-7},1.4241257692880089E-4,{"$error":"#N/A"},null,{"$f":"(AP3745)*$G$11*Bodencharakterisierung!$E$8","v":4.3065579433660072E-9},{"$f":"IF(AF3745<=$J$9*1.05,(AV3745*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3744,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,23.384401919999263,null,0.29278096903777873,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,142.11476986184013]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3737,1.0524563072329008E-15,{"$f":"Z3754*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.0416559523199906E-15},{"$f":"AF3753*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3754^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3754)*3600*24","v":0},0,{"$f":"AE3753-AD3754*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3754>$J$18,(AE3754/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.0416559523199906E-15,{"$error":"#N/A"},null,{"$f":"(AD3754)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3754>0,(AJ3754*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3753,NA())","v":{"$error":"#N/A"}},null,3737,{"$f":"IF(AF3754<=$J$9*0.05,AS3753*EXP((-$J$6*1)/Heterogenität!$D$4),Z3754)","v":1.4028820647878816E-4},{"$f":"IF(OR(AF3754>=$J$19, AR3753/$J$5<AN3754),0, Bodencharakterisierung!$E$8*$J$11*((AR3753/$J$5)-AN3754))","v":6.4525208738536392E-6},1.4545708846495204E-6,{"$f":"AQ3753-AP3754*Bodencharakterisierung!$E$8","v":4.3944598034477574E-4},{"$f":"AQ3754/(Bodencharakterisierung!$E$11*1000)","v":2.9006335336288827E-7},1.4174277736343769E-4,{"$error":"#N/A"},null,{"$f":"(AP3754)*$G$11*Bodencharakterisierung!$E$8","v":2.1034402780984224E-8},{"$f":"IF(AF3754<=$J$9*1.05,(AV3754*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3753,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,23.440855679999252,null,0.29006335336288824,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,140.28820647878817]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3746,9.5914904324106736E-16,{"$f":"Z3763*EXP((-$J$6/Heterogenität!$D$4)*1)","v":9.4930621175230198E-16},{"$f":"AF3762*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3763^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3763)*3600*24","v":0},0,{"$f":"AE3762-AD3763*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3763>$J$18,(AE3763/(Bodencharakterisierung!$E$11*1000)),0)","v":0},9.4930621175230198E-16,{"$error":"#N/A"},null,{"$f":"(AD3763)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3763>0,(AJ3763*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3762,NA())","v":{"$error":"#N/A"}},null,3746,{"$f":"IF(AF3763<=$J$9*0.05,AS3762*EXP((-$J$6*1)/Heterogenität!$D$4),Z3763)","v":1.3928448085092726E-4},{"$f":"IF(OR(AF3763>=$J$19, AR3762/$J$5<AN3763),0, Bodencharakterisierung!$E$8*$J$11*((AR3762/$J$5)-AN3763))","v":3.8258437365444017E-6},1.4441638083092514E-6,{"$f":"AQ3762-AP3763*Bodencharakterisierung!$E$8","v":4.3547774028571449E-4},{"$f":"AQ3763/(Bodencharakterisierung!$E$11*1000)","v":2.8744405299387095E-7},1.4072864465923651E-4,{"$error":"#N/A"},null,{"$f":"(AP3763)*$G$11*Bodencharakterisierung!$E$8","v":2.0883907100214139E-8},{"$f":"IF(AF3763<=$J$9*1.05,(AV3763*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3762,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,23.497309439999242,null,0.28744405299387094,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,139.28448085092725]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3753,8.9233447313000427E-16,{"$f":"Z3770*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.8317729582525942E-16},{"$f":"AF3769*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3770^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3770)*3600*24","v":0},0,{"$f":"AE3769-AD3770*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3770>$J$18,(AE3770/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.8317729582525942E-16,{"$error":"#N/A"},null,{"$f":"(AD3770)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3770>0,(AJ3770*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3769,NA())","v":{"$error":"#N/A"}},null,3753,{"$f":"IF(AF3770<=$J$9*0.05,AS3769*EXP((-$J$6*1)/Heterogenität!$D$4),Z3770)","v":1.3859647013651251E-4},{"$f":"IF(OR(AF3770>=$J$19, AR3769/$J$5<AN3770),0, Bodencharakterisierung!$E$8*$J$11*((AR3769/$J$5)-AN3770))","v":8.4789021583578196E-7},8.4789021583578196E-7,{"$f":"AQ3769-AP3770*Bodencharakterisierung!$E$8","v":4.3257605599873603E-4},{"$f":"AQ3770/(Bodencharakterisierung!$E$11*1000)","v":2.8552874983414921E-7},1.3944436035234829E-4,{"$error":"#N/A"},null,{"$f":"(AP3770)*$G$11*Bodencharakterisierung!$E$8","v":1.2261254849909087E-8},{"$f":"IF(AF3770<=$J$9*1.05,(AV3770*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3769,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,23.541217919999234,null,0.28552874983414922,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,138.59647013651252]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3765,7.8844312073955432E-16,{"$f":"Z3782*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.8035208125971282E-16},{"$f":"AF3781*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3782^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3782)*3600*24","v":0},0,{"$f":"AE3781-AD3782*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3782>$J$18,(AE3782/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.8035208125971282E-16,{"$error":"#N/A"},null,{"$f":"(AD3782)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3782>0,(AJ3782*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3781,NA())","v":{"$error":"#N/A"}},null,3765,{"$f":"IF(AF3782<=$J$9*0.05,AS3781*EXP((-$J$6*1)/Heterogenität!$D$4),Z3782)","v":1.3678363388045596E-4},{"$f":"IF(OR(AF3782>=$J$19, AR3781/$J$5<AN3782),0, Bodencharakterisierung!$E$8*$J$11*((AR3781/$J$5)-AN3782))","v":2.777703382632465E-6},1.4182339081307853E-6,{"$f":"AQ3781-AP3782*Bodencharakterisierung!$E$8","v":4.2734595708470677E-4},{"$f":"AQ3782/(Bodencharakterisierung!$E$11*1000)","v":2.8207653932983943E-7},1.3820186778858674E-4,{"$error":"#N/A"},null,{"$f":"(AP3782)*$G$11*Bodencharakterisierung!$E$8","v":2.0508937430340682E-8},{"$f":"IF(AF3782<=$J$9*1.05,(AV3782*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3781,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,23.61648959999922,null,0.28207653932983945,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,136.78363388045597]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3777,6.9664747172774575E-16,{"$f":"Z3794*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.8949844340976907E-16},{"$f":"AF3793*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3794^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3794)*3600*24","v":0},0,{"$f":"AE3793-AD3794*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3794>$J$18,(AE3794/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.8949844340976907E-16,{"$error":"#N/A"},null,{"$f":"(AD3794)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3794>0,(AJ3794*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3793,NA())","v":{"$error":"#N/A"}},null,3777,{"$f":"IF(AF3794<=$J$9*0.05,AS3793*EXP((-$J$6*1)/Heterogenität!$D$4),Z3794)","v":1.3470024991232287E-4},{"$f":"IF(OR(AF3794>=$J$19, AR3793/$J$5<AN3794),0, Bodencharakterisierung!$E$8*$J$11*((AR3793/$J$5)-AN3794))","v":7.8507391644477444E-6},1.3966324511184385E-6,{"$f":"AQ3793-AP3794*Bodencharakterisierung!$E$8","v":4.224705982307999E-4},{"$f":"AQ3794/(Bodencharakterisierung!$E$11*1000)","v":2.7885848068039599E-7},1.3609688236344131E-4,{"$error":"#N/A"},null,{"$f":"(AP3794)*$G$11*Bodencharakterisierung!$E$8","v":2.0196560940305758E-8},{"$f":"IF(AF3794<=$J$9*1.05,(AV3794*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3793,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,23.691761279999206,null,0.27885848068039598,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,134.70024991232287]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3778,6.8949844340976907E-16,{"$f":"Z3795*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.8242277874839836E-16},{"$f":"AF3794*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3795^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3795)*3600*24","v":0},0,{"$f":"AE3794-AD3795*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3795>$J$18,(AE3795/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.8242277874839836E-16,{"$error":"#N/A"},null,{"$f":"(AD3795)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3795>0,(AJ3795*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3794,NA())","v":{"$error":"#N/A"}},null,3778,{"$f":"IF(AF3795<=$J$9*0.05,AS3794*EXP((-$J$6*1)/Heterogenität!$D$4),Z3795)","v":1.3470024991232287E-4},{"$f":"IF(OR(AF3795>=$J$19, AR3794/$J$5<AN3795),0, Bodencharakterisierung!$E$8*$J$11*((AR3794/$J$5)-AN3795))","v":6.4075867754806068E-6},1.3966324511184385E-6,{"$f":"AQ3794-AP3795*Bodencharakterisierung!$E$8","v":4.2200970952193084E-4},{"$f":"AQ3795/(Bodencharakterisierung!$E$11*1000)","v":2.7855426371084542E-7},1.3609688236344131E-4,{"$error":"#N/A"},null,{"$f":"(AP3795)*$G$11*Bodencharakterisierung!$E$8","v":2.0196560940305758E-8},{"$f":"IF(AF3795<=$J$9*1.05,(AV3795*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3794,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,23.698033919999204,null,0.27855426371084541,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,134.70024991232287]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3786,6.348850317033738E-16,{"$f":"Z3803*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.2836981237866957E-16},{"$f":"AF3802*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3803^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3803)*3600*24","v":0},0,{"$f":"AE3802-AD3803*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3803>$J$18,(AE3803/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.2836981237866957E-16,{"$error":"#N/A"},null,{"$f":"(AD3803)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3803>0,(AJ3803*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3802,NA())","v":{"$error":"#N/A"}},null,3786,{"$f":"IF(AF3803<=$J$9*0.05,AS3802*EXP((-$J$6*1)/Heterogenität!$D$4),Z3803)","v":1.3394641082174771E-4},{"$f":"IF(OR(AF3803>=$J$19, AR3802/$J$5<AN3803),0, Bodencharakterisierung!$E$8*$J$11*((AR3802/$J$5)-AN3803))","v":3.0410202051837211E-6},1.3888163101869616E-6,{"$f":"AQ3802-AP3803*Bodencharakterisierung!$E$8","v":4.1858426338340499E-4},{"$f":"AQ3803/(Bodencharakterisierung!$E$11*1000)","v":2.76293243157363E-7},1.3533522713193467E-4,{"$error":"#N/A"},null,{"$f":"(AP3803)*$G$11*Bodencharakterisierung!$E$8","v":2.0083532515028817E-8},{"$f":"IF(AF3803<=$J$9*1.05,(AV3803*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3802,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,23.748215039999195,null,0.27629324315736298,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,133.94641082174772]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3802,5.3829294040022087E-16,{"$f":"Z3819*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.3276895354824238E-16},{"$f":"AF3818*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3819^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3819)*3600*24","v":0},0,{"$f":"AE3818-AD3819*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3819>$J$18,(AE3819/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.3276895354824238E-16,{"$error":"#N/A"},null,{"$f":"(AD3819)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3819>0,(AJ3819*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3818,NA())","v":{"$error":"#N/A"}},null,3802,{"$f":"IF(AF3819<=$J$9*0.05,AS3818*EXP((-$J$6*1)/Heterogenität!$D$4),Z3819)","v":1.3177276512532974E-4},{"$f":"IF(OR(AF3819>=$J$19, AR3818/$J$5<AN3819),0, Bodencharakterisierung!$E$8*$J$11*((AR3818/$J$5)-AN3819))","v":3.8019378277928242E-6},1.3662789791959052E-6,{"$f":"AQ3818-AP3819*Bodencharakterisierung!$E$8","v":4.1205036121370642E-4},{"$f":"AQ3819/(Bodencharakterisierung!$E$11*1000)","v":2.7198043644469068E-7},1.3313904410452564E-4,{"$error":"#N/A"},null,{"$f":"(AP3819)*$G$11*Bodencharakterisierung!$E$8","v":1.9757622445827572E-8},{"$f":"IF(AF3819<=$J$9*1.05,(AV3819*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3818,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,23.848577279999176,null,0.27198043644469067,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,131.77276512532973]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3805,5.2189046033508721E-16,{"$f":"Z3822*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.1653479648610455E-16},{"$f":"AF3821*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3822^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3822)*3600*24","v":0},0,{"$f":"AE3821-AD3822*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3822>$J$18,(AE3822/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.1653479648610455E-16,{"$error":"#N/A"},null,{"$f":"(AD3822)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3822>0,(AJ3822*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3821,NA())","v":{"$error":"#N/A"}},null,3805,{"$f":"IF(AF3822<=$J$9*0.05,AS3821*EXP((-$J$6*1)/Heterogenität!$D$4),Z3822)","v":1.3138882902724816E-4},{"$f":"IF(OR(AF3822>=$J$19, AR3821/$J$5<AN3822),0, Bodencharakterisierung!$E$8*$J$11*((AR3821/$J$5)-AN3822))","v":3.7196851247995614E-6},1.3622981579718683E-6,{"$f":"AQ3821-AP3822*Bodencharakterisierung!$E$8","v":4.1082707127867724E-4},{"$f":"AQ3822/(Bodencharakterisierung!$E$11*1000)","v":2.7117298434236123E-7},1.3275112718522003E-4,{"$error":"#N/A"},null,{"$f":"(AP3822)*$G$11*Bodencharakterisierung!$E$8","v":1.9700056191814686E-8},{"$f":"IF(AF3822<=$J$9*1.05,(AV3822*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3821,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,23.867395199999173,null,0.2711729843423612,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,131.38882902724816]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3817,4.611285965311463E-16,{"$f":"Z3834*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.5639647371635432E-16},{"$f":"AF3833*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3834^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3834)*3600*24","v":0},0,{"$f":"AE3833-AD3834*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3834>$J$18,(AE3834/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.5639647371635432E-16,{"$error":"#N/A"},null,{"$f":"(AD3834)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3834>0,(AJ3834*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3833,NA())","v":{"$error":"#N/A"}},null,3817,{"$f":"IF(AF3834<=$J$9*0.05,AS3833*EXP((-$J$6*1)/Heterogenität!$D$4),Z3834)","v":1.2978117057420278E-4},{"$f":"IF(OR(AF3834>=$J$19, AR3833/$J$5<AN3834),0, Bodencharakterisierung!$E$8*$J$11*((AR3833/$J$5)-AN3834))","v":4.323488971444938E-6},1.3456292359223542E-6,{"$f":"AQ3833-AP3834*Bodencharakterisierung!$E$8","v":4.0600760657981595E-4},{"$f":"AQ3834/(Bodencharakterisierung!$E$11*1000)","v":2.6799181952463097E-7},1.3112679981012513E-4,{"$error":"#N/A"},null,{"$f":"(AP3834)*$G$11*Bodencharakterisierung!$E$8","v":1.9459008592131162E-8},{"$f":"IF(AF3834<=$J$9*1.05,(AV3834*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3833,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,23.942666879999159,null,0.26799181952463097,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,129.78117057420278]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3823,4.3345438820131157E-16,{"$f":"Z3840*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.290062593821296E-16},{"$f":"AF3839*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3840^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3840)*3600*24","v":0},0,{"$f":"AE3839-AD3840*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3840>$J$18,(AE3840/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.290062593821296E-16,{"$error":"#N/A"},null,{"$f":"(AD3840)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3840>0,(AJ3840*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3839,NA())","v":{"$error":"#N/A"}},null,3823,{"$f":"IF(AF3840<=$J$9*0.05,AS3839*EXP((-$J$6*1)/Heterogenität!$D$4),Z3840)","v":1.2859992699462301E-4},{"$f":"IF(OR(AF3840>=$J$19, AR3839/$J$5<AN3840),0, Bodencharakterisierung!$E$8*$J$11*((AR3839/$J$5)-AN3840))","v":8.7838382622487166E-6},1.3333815740435571E-6,{"$f":"AQ3839-AP3840*Bodencharakterisierung!$E$8","v":4.0374923798763103E-4},{"$f":"AQ3840/(Bodencharakterisierung!$E$11*1000)","v":2.6650114718655513E-7},1.2993330856866657E-4,{"$error":"#N/A"},null,{"$f":"(AP3840)*$G$11*Bodencharakterisierung!$E$8","v":1.928189638962341E-8},{"$f":"IF(AF3840<=$J$9*1.05,(AV3840*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3839,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,23.980302719999152,null,0.26650114718655515,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,128.59992699462302]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3835,3.8298882405936832E-16,{"$f":"Z3852*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.7905857517483776E-16},{"$f":"AF3851*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3852^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3852)*3600*24","v":0},0,{"$f":"AE3851-AD3852*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3852>$J$18,(AE3852/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.7905857517483776E-16,{"$error":"#N/A"},null,{"$f":"(AD3852)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3852>0,(AJ3852*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3851,NA())","v":{"$error":"#N/A"}},null,3835,{"$f":"IF(AF3852<=$J$9*0.05,AS3851*EXP((-$J$6*1)/Heterogenität!$D$4),Z3852)","v":1.277919924452917E-4},{"$f":"IF(OR(AF3852>=$J$19, AR3851/$J$5<AN3852),0, Bodencharakterisierung!$E$8*$J$11*((AR3851/$J$5)-AN3852))","v":1.0331661168191709E-6},1.0331661168191709E-6,{"$f":"AQ3851-AP3852*Bodencharakterisierung!$E$8","v":3.9885132296974126E-4},{"$f":"AQ3852/(Bodencharakterisierung!$E$11*1000)","v":2.6326819998002721E-7},1.2882515856211087E-4,{"$error":"#N/A"},null,{"$f":"(AP3852)*$G$11*Bodencharakterisierung!$E$8","v":1.4940510957687827E-8},{"$f":"IF(AF3852<=$J$9*1.05,(AV3852*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3851,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,24.055574399999138,null,0.26326819998002721,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,127.7919924452917]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3847,3.3839878738580041E-16,{"$f":"Z3864*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.3492612350346382E-16},{"$f":"AF3863*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3864^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3864)*3600*24","v":0},0,{"$f":"AE3863-AD3864*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3864>$J$18,(AE3864/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.3492612350346382E-16,{"$error":"#N/A"},null,{"$f":"(AD3864)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3864>0,(AJ3864*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3863,NA())","v":{"$error":"#N/A"}},null,3847,{"$f":"IF(AF3864<=$J$9*0.05,AS3863*EXP((-$J$6*1)/Heterogenität!$D$4),Z3864)","v":1.2625054285349098E-4},{"$f":"IF(OR(AF3864>=$J$19, AR3863/$J$5<AN3864),0, Bodencharakterisierung!$E$8*$J$11*((AR3863/$J$5)-AN3864))","v":1.4190624610983939E-6},1.3090221082386717E-6,{"$f":"AQ3863-AP3864*Bodencharakterisierung!$E$8","v":3.9407238360544372E-4},{"$f":"AQ3864/(Bodencharakterisierung!$E$11*1000)","v":2.6011378455804868E-7},1.2755956496172965E-4,{"$error":"#N/A"},null,{"$f":"(AP3864)*$G$11*Bodencharakterisierung!$E$8","v":1.8929636612752493E-8},{"$f":"IF(AF3864<=$J$9*1.05,(AV3864*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3863,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,24.130846079999124,null,0.26011378455804868,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,126.25054285349098]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3854,{"$f":"AG3870","v":3.1482584044432639E-16},{"$f":"Z3871*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.1159508322506116E-16},{"$f":"AF3870*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3871^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3871)*3600*24","v":0},{"$f":"MIN(AC3871,Z3871-AA3871)","v":0},{"$f":"AE3870-AD3871*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3871>$J$18,(AE3871/(Bodencharakterisierung!$E$11*1000)),0)","v":0},{"$f":"AA3871+AD3871","v":3.1159508322506116E-16},{"$f":"IF(AD3871>0,Y3871,NA())","v":{"$error":"#N/A"}},null,{"$f":"(AD3871)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3871>0,(AJ3871*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3870,NA())","v":{"$error":"#N/A"}},null,3854,{"$f":"IF(AF3871<=$J$9*0.05,AS3870*EXP((-$J$6*1)/Heterogenität!$D$4),Z3871)","v":1.250207107912855E-4},{"$f":"IF(OR(AF3871>=$J$19, AR3870/$J$5<AN3871),0, Bodencharakterisierung!$E$8*$J$11*((AR3870/$J$5)-AN3871))","v":5.3199073439223271E-6},{"$f":"MIN(AO3871,AS3870-AN3871)","v":1.2962706592352814E-6},{"$f":"AQ3870-AP3871*Bodencharakterisierung!$E$8","v":3.9148384296313796E-4},{"$f":"AQ3871/(Bodencharakterisierung!$E$11*1000)","v":2.5840517687335838E-7},{"$f":"AN3871+AP3871","v":1.2631698145052078E-4},{"$f":"IF(AN3871>$G$5,AM3871,NA())","v":{"$error":"#N/A"}},null,{"$f":"(AP3871)*$G$11*Bodencharakterisierung!$E$8","v":1.8745239195473569E-8},{"$f":"IF(AF3871<=$J$9*1.05,(AV3871*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3870,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH3871>($G$5*10^6),BH3871*0.99,9999)","v":9999},{"$f":"AT3871+$G$3","v":{"$error":"#N/A"}},{"$f":"IF(ISNUMBER(AT3871),BA3871+BB3871+BC3871+$AZ$17,\"\")","v":""},{"$f":"IF(ISNUMBER(AK3871),AK3871,BA3870)","v":1.6399886323194495},{"$f":"IF(ISNUMBER(AW3871),AW3871,0)","v":0},24.174754559999116,null,{"$f":"AR3871*10^6","v":0.2584051768733584},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF3871*10^6","v":0},{"$f":"AN3871*10^6","v":125.0207107912855}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3858,3.0210037921279462E-16,{"$f":"Z3875*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.9900021126054834E-16},{"$f":"AF3874*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3875^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3875)*3600*24","v":0},0,{"$f":"AE3874-AD3875*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3875>$J$18,(AE3875/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.9900021126054834E-16,{"$error":"#N/A"},null,{"$f":"(AD3875)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3875>0,(AJ3875*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3874,NA())","v":{"$error":"#N/A"}},null,3858,{"$f":"IF(AF3875<=$J$9*0.05,AS3874*EXP((-$J$6*1)/Heterogenität!$D$4),Z3875)","v":1.250207107912855E-4},{"$f":"IF(OR(AF3875>=$J$19, AR3874/$J$5<AN3875),0, Bodencharakterisierung!$E$8*$J$11*((AR3874/$J$5)-AN3875))","v":0},0,{"$f":"AQ3874-AP3875*Bodencharakterisierung!$E$8","v":3.90200535010495E-4},{"$f":"AQ3875/(Bodencharakterisierung!$E$11*1000)","v":2.5755810891781849E-7},1.250207107912855E-4,{"$error":"#N/A"},null,{"$f":"(AP3875)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AF3875<=$J$9*1.05,(AV3875*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3874,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,24.199845119999111,null,0.2575581089178185,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,125.0207107912855]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3872,2.6147755598395391E-16,{"$f":"Z3889*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.587942613075108E-16},{"$f":"AF3888*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3889^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3889)*3600*24","v":0},0,{"$f":"AE3888-AD3889*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3889>$J$18,(AE3889/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.587942613075108E-16,{"$error":"#N/A"},null,{"$f":"(AD3889)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3889>0,(AJ3889*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3888,NA())","v":{"$error":"#N/A"}},null,3872,{"$f":"IF(AF3889<=$J$9*0.05,AS3888*EXP((-$J$6*1)/Heterogenität!$D$4),Z3889)","v":1.2303156096838682E-4},{"$f":"IF(OR(AF3889>=$J$19, AR3888/$J$5<AN3889),0, Bodencharakterisierung!$E$8*$J$11*((AR3888/$J$5)-AN3889))","v":2.9282558447897323E-6},1.2756462639976565E-6,{"$f":"AQ3888-AP3889*Bodencharakterisierung!$E$8","v":3.845183428246121E-4},{"$f":"AQ3889/(Bodencharakterisierung!$E$11*1000)","v":2.5380748701294527E-7},1.2430720723238448E-4,{"$error":"#N/A"},null,{"$f":"(AP3889)*$G$11*Bodencharakterisierung!$E$8","v":1.8446991897166796E-8},{"$f":"IF(AF3889<=$J$9*1.05,(AV3889*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3888,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,24.287662079999095,null,0.25380748701294525,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,123.03156096838683]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3875,2.5350999765722225E-16,{"$f":"Z3892*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.5090846642989016E-16},{"$f":"AF3891*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3892^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3892)*3600*24","v":0},0,{"$f":"AE3891-AD3892*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3892>$J$18,(AE3892/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.5090846642989016E-16,{"$error":"#N/A"},null,{"$f":"(AD3892)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3892>0,(AJ3892*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3891,NA())","v":{"$error":"#N/A"}},null,3875,{"$f":"IF(AF3892<=$J$9*0.05,AS3891*EXP((-$J$6*1)/Heterogenität!$D$4),Z3892)","v":1.220579923133327E-4},{"$f":"IF(OR(AF3892>=$J$19, AR3891/$J$5<AN3892),0, Bodencharakterisierung!$E$8*$J$11*((AR3891/$J$5)-AN3892))","v":9.505127131798925E-6},1.2655518686426038E-6,{"$f":"AQ3891-AP3892*Bodencharakterisierung!$E$8","v":3.8358339298035665E-4},{"$f":"AQ3892/(Bodencharakterisierung!$E$11*1000)","v":2.5319035840287569E-7},1.233235441819753E-4,{"$error":"#N/A"},null,{"$f":"(AP3892)*$G$11*Bodencharakterisierung!$E$8","v":1.8301017864571031E-8},{"$f":"IF(AF3892<=$J$9*1.05,(AV3892*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3891,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,24.306479999999091,null,0.25319035840287568,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,122.0579923133327]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3887,2.2399472362692986E-16,{"$f":"Z3904*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.2169607949589641E-16},{"$f":"AF3903*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3904^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3904)*3600*24","v":0},0,{"$f":"AE3903-AD3904*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3904>$J$18,(AE3904/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.2169607949589641E-16,{"$error":"#N/A"},null,{"$f":"(AD3904)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3904>0,(AJ3904*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3903,NA())","v":{"$error":"#N/A"}},null,3887,{"$f":"IF(AF3904<=$J$9*0.05,AS3903*EXP((-$J$6*1)/Heterogenität!$D$4),Z3904)","v":1.211530110004671E-4},{"$f":"IF(OR(AF3904>=$J$19, AR3903/$J$5<AN3904),0, Bodencharakterisierung!$E$8*$J$11*((AR3903/$J$5)-AN3904))","v":3.6407997371403747E-6},1.2561686175348546E-6,{"$f":"AQ3903-AP3904*Bodencharakterisierung!$E$8","v":3.7888903025097098E-4},{"$f":"AQ3904/(Bodencharakterisierung!$E$11*1000)","v":2.5009176914255511E-7},1.2240917961800195E-4,{"$error":"#N/A"},null,{"$f":"(AP3904)*$G$11*Bodencharakterisierung!$E$8","v":1.8165327617173384E-8},{"$f":"IF(AF3904<=$J$9*1.05,(AV3904*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3903,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,24.381751679999077,null,0.2500917691425551,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,121.15301100046709]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3897,2.0204124492146648E-16,{"$f":"Z3914*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.9996788839616311E-16},{"$f":"AF3913*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3914^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3914)*3600*24","v":0},0,{"$f":"AE3913-AD3914*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3914>$J$18,(AE3914/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.9996788839616311E-16,{"$error":"#N/A"},null,{"$f":"(AD3914)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3914>0,(AJ3914*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3913,NA())","v":{"$error":"#N/A"}},null,3897,{"$f":"IF(AF3914<=$J$9*0.05,AS3913*EXP((-$J$6*1)/Heterogenität!$D$4),Z3914)","v":1.1921122096531712E-4},{"$f":"IF(OR(AF3914>=$J$19, AR3913/$J$5<AN3914),0, Bodencharakterisierung!$E$8*$J$11*((AR3913/$J$5)-AN3914))","v":1.1709730967761971E-5},1.2360352697636718E-6,{"$f":"AQ3913-AP3914*Bodencharakterisierung!$E$8","v":3.7541190419421736E-4},{"$f":"AQ3914/(Bodencharakterisierung!$E$11*1000)","v":2.4779663643182662E-7},1.204472562350808E-4,{"$error":"#N/A"},null,{"$f":"(AP3914)*$G$11*Bodencharakterisierung!$E$8","v":1.7874181306726826E-8},{"$f":"IF(AF3914<=$J$9*1.05,(AV3914*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3913,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,24.444478079999065,null,0.24779663643182662,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,119.21122096531712]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3905,1.8603807363655166E-16,{"$f":"Z3922*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.8412894238922072E-16},{"$f":"AF3921*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3922^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3922)*3600*24","v":0},0,{"$f":"AE3921-AD3922*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3922>$J$18,(AE3922/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.8412894238922072E-16,{"$error":"#N/A"},null,{"$f":"(AD3922)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3922>0,(AJ3922*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3921,NA())","v":{"$error":"#N/A"}},null,3905,{"$f":"IF(AF3922<=$J$9*0.05,AS3921*EXP((-$J$6*1)/Heterogenität!$D$4),Z3922)","v":1.1921122096531712E-4},{"$f":"IF(OR(AF3922>=$J$19, AR3921/$J$5<AN3922),0, Bodencharakterisierung!$E$8*$J$11*((AR3921/$J$5)-AN3922))","v":1.4920835059476142E-6},1.2360352697636718E-6,{"$f":"AQ3921-AP3922*Bodencharakterisierung!$E$8","v":3.7214877108204125E-4},{"$f":"AQ3922/(Bodencharakterisierung!$E$11*1000)","v":2.4564275318946618E-7},1.204472562350808E-4,{"$error":"#N/A"},null,{"$f":"(AP3922)*$G$11*Bodencharakterisierung!$E$8","v":1.7874181306726826E-8},{"$f":"IF(AF3922<=$J$9*1.05,(AV3922*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3921,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,24.494659199999056,null,0.24564275318946618,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,119.21122096531712]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3917,1.6437831751571017E-16,{"$f":"Z3934*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.6269145967946954E-16},{"$f":"AF3933*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3934^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3934)*3600*24","v":0},0,{"$f":"AE3933-AD3934*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3934>$J$18,(AE3934/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.6269145967946954E-16,{"$error":"#N/A"},null,{"$f":"(AD3934)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3934>0,(AJ3934*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3933,NA())","v":{"$error":"#N/A"}},null,3917,{"$f":"IF(AF3934<=$J$9*0.05,AS3933*EXP((-$J$6*1)/Heterogenität!$D$4),Z3934)","v":1.1759250334876138E-4},{"$f":"IF(OR(AF3934>=$J$19, AR3933/$J$5<AN3934),0, Bodencharakterisierung!$E$8*$J$11*((AR3933/$J$5)-AN3934))","v":3.7885376028770976E-6},1.219251681359418E-6,{"$f":"AQ3933-AP3934*Bodencharakterisierung!$E$8","v":3.6783539550129968E-4},{"$f":"AQ3934/(Bodencharakterisierung!$E$11*1000)","v":2.4279564059491729E-7},1.1881175503012079E-4,{"$error":"#N/A"},null,{"$f":"(AP3934)*$G$11*Bodencharakterisierung!$E$8","v":1.7631475528458486E-8},{"$f":"IF(AF3934<=$J$9*1.05,(AV3934*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3933,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,24.569930879999042,null,0.24279564059491729,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,117.59250334876137]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3924,1.5292768145681396E-16,{"$f":"Z3941*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.5135833057318004E-16},{"$f":"AF3940*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3941^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3941)*3600*24","v":0},0,{"$f":"AE3940-AD3941*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3941>$J$18,(AE3941/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.5135833057318004E-16,{"$error":"#N/A"},null,{"$f":"(AD3941)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3941>0,(AJ3941*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3940,NA())","v":{"$error":"#N/A"}},null,3924,{"$f":"IF(AF3941<=$J$9*0.05,AS3940*EXP((-$J$6*1)/Heterogenität!$D$4),Z3941)","v":1.1639461954832876E-4},{"$f":"IF(OR(AF3941>=$J$19, AR3940/$J$5<AN3941),0, Bodencharakterisierung!$E$8*$J$11*((AR3940/$J$5)-AN3941))","v":7.9657366468550018E-6},1.2068314862265797E-6,{"$f":"AQ3940-AP3941*Bodencharakterisierung!$E$8","v":3.6543471909347149E-4},{"$f":"AQ3941/(Bodencharakterisierung!$E$11*1000)","v":2.4121103570526173E-7},1.1760145103455534E-4,{"$error":"#N/A"},null,{"$f":"(AP3941)*$G$11*Bodencharakterisierung!$E$8","v":1.7451868339974518E-8},{"$f":"IF(AF3941<=$J$9*1.05,(AV3941*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3940,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,24.613839359999034,null,0.24121103570526173,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,116.39461954832876]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3927,1.4826777779053606E-16,{"$f":"Z3944*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.4674624705212802E-16},{"$f":"AF3943*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3944^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3944)*3600*24","v":0},0,{"$f":"AE3943-AD3944*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3944>$J$18,(AE3944/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.4674624705212802E-16,{"$error":"#N/A"},null,{"$f":"(AD3944)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3944>0,(AJ3944*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3943,NA())","v":{"$error":"#N/A"}},null,3927,{"$f":"IF(AF3944<=$J$9*0.05,AS3943*EXP((-$J$6*1)/Heterogenität!$D$4),Z3944)","v":1.1639461954832876E-4},{"$f":"IF(OR(AF3944>=$J$19, AR3943/$J$5<AN3944),0, Bodencharakterisierung!$E$8*$J$11*((AR3943/$J$5)-AN3944))","v":4.2246484148709369E-6},1.2068314862265797E-6,{"$f":"AQ3943-AP3944*Bodencharakterisierung!$E$8","v":3.6423995592210724E-4},{"$f":"AQ3944/(Bodencharakterisierung!$E$11*1000)","v":2.4042241314990577E-7},1.1760145103455534E-4,{"$error":"#N/A"},null,{"$f":"(AP3944)*$G$11*Bodencharakterisierung!$E$8","v":1.7451868339974518E-8},{"$f":"IF(AF3944<=$J$9*1.05,(AV3944*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3943,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,24.63265727999903,null,0.24042241314990578,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,116.39461954832876]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3938,1.3236380733389952E-16,{"$f":"Z3955*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.3100548387001265E-16},{"$f":"AF3954*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3955^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3955)*3600*24","v":0},0,{"$f":"AE3954-AD3955*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3955>$J$18,(AE3955/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.3100548387001265E-16,{"$error":"#N/A"},null,{"$f":"(AD3955)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3955>0,(AJ3955*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3954,NA())","v":{"$error":"#N/A"}},null,3938,{"$f":"IF(AF3955<=$J$9*0.05,AS3954*EXP((-$J$6*1)/Heterogenität!$D$4),Z3955)","v":1.1526684095833494E-4},{"$f":"IF(OR(AF3955>=$J$19, AR3954/$J$5<AN3955),0, Bodencharakterisierung!$E$8*$J$11*((AR3954/$J$5)-AN3955))","v":2.7648234012833908E-6},1.1951381732781081E-6,{"$f":"AQ3954-AP3955*Bodencharakterisierung!$E$8","v":3.6025759698335468E-4},{"$f":"AQ3955/(Bodencharakterisierung!$E$11*1000)","v":2.3779379338835292E-7},1.1646197913161305E-4,{"$error":"#N/A"},null,{"$f":"(AP3955)*$G$11*Bodencharakterisierung!$E$8","v":1.7282772521408402E-8},{"$f":"IF(AF3955<=$J$9*1.05,(AV3955*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3954,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,24.701656319999017,null,0.23779379338835291,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,115.26684095833494]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3945,1.2314331032397311E-16,{"$f":"Z3962*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.2187960802345069E-16},{"$f":"AF3961*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3962^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3962)*3600*24","v":0},0,{"$f":"AE3961-AD3962*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3962>$J$18,(AE3962/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.2187960802345069E-16,{"$error":"#N/A"},null,{"$f":"(AD3962)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3962>0,(AJ3962*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3961,NA())","v":{"$error":"#N/A"}},null,3945,{"$f":"IF(AF3962<=$J$9*0.05,AS3961*EXP((-$J$6*1)/Heterogenität!$D$4),Z3962)","v":1.1437587094349164E-4},{"$f":"IF(OR(AF3962>=$J$19, AR3961/$J$5<AN3962),0, Bodencharakterisierung!$E$8*$J$11*((AR3961/$J$5)-AN3962))","v":3.7961746417747111E-6},1.1859001975764031E-6,{"$f":"AQ3961-AP3962*Bodencharakterisierung!$E$8","v":3.5780913909986981E-4},{"$f":"AQ3962/(Bodencharakterisierung!$E$11*1000)","v":2.3617764957087115E-7},1.1556177114106805E-4,{"$error":"#N/A"},null,{"$f":"(AP3962)*$G$11*Bodencharakterisierung!$E$8","v":1.7149183086997698E-8},{"$f":"IF(AF3962<=$J$9*1.05,(AV3962*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3961,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,24.745564799999009,null,0.23617764957087115,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,114.37587094349165]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3957,1.0880616945064215E-16,{"$f":"Z3974*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.0768959554756882E-16},{"$f":"AF3973*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3974^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3974)*3600*24","v":0},0,{"$f":"AE3973-AD3974*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3974>$J$18,(AE3974/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.0768959554756882E-16,{"$error":"#N/A"},null,{"$f":"(AD3974)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3974>0,(AJ3974*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3973,NA())","v":{"$error":"#N/A"}},null,3957,{"$f":"IF(AF3974<=$J$9*0.05,AS3973*EXP((-$J$6*1)/Heterogenität!$D$4),Z3974)","v":1.1332088120595837E-4},{"$f":"IF(OR(AF3974>=$J$19, AR3973/$J$5<AN3974),0, Bodencharakterisierung!$E$8*$J$11*((AR3973/$J$5)-AN3974))","v":5.9381495177199214E-7},5.9381495177199214E-7,{"$f":"AQ3973-AP3974*Bodencharakterisierung!$E$8","v":3.5368899672049087E-4},{"$f":"AQ3974/(Bodencharakterisierung!$E$11*1000)","v":2.3345808364388836E-7},1.1391469615773036E-4,{"$error":"#N/A"},null,{"$f":"(AP3974)*$G$11*Bodencharakterisierung!$E$8","v":8.5870980952244242E-9},{"$f":"IF(AF3974<=$J$9*1.05,(AV3974*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3973,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,24.820836479998995,null,0.23345808364388834,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,113.32088120595837]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3964,1.0122670358086392E-16,{"$f":"Z3981*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.0018791050430217E-16},{"$f":"AF3980*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3981^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3981)*3600*24","v":0},0,{"$f":"AE3980-AD3981*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3981>$J$18,(AE3981/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.0018791050430217E-16,{"$error":"#N/A"},null,{"$f":"(AD3981)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3981>0,(AJ3981*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3980,NA())","v":{"$error":"#N/A"}},null,3964,{"$f":"IF(AF3981<=$J$9*0.05,AS3980*EXP((-$J$6*1)/Heterogenität!$D$4),Z3981)","v":1.1235063575371303E-4},{"$f":"IF(OR(AF3981>=$J$19, AR3980/$J$5<AN3981),0, Bodencharakterisierung!$E$8*$J$11*((AR3980/$J$5)-AN3981))","v":2.631668657204455E-6},1.1649016531116885E-6,{"$f":"AQ3980-AP3981*Bodencharakterisierung!$E$8","v":3.5112303758366562E-4},{"$f":"AQ3981/(Bodencharakterisierung!$E$11*1000)","v":2.3176438124334363E-7},1.1351553740682472E-4,{"$error":"#N/A"},null,{"$f":"(AP3981)*$G$11*Bodencharakterisierung!$E$8","v":1.684552525447368E-8},{"$f":"IF(AF3981<=$J$9*1.05,(AV3981*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3980,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,24.864744959998987,null,0.23176438124334364,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,112.35063575371302]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3976,8.9441235855791517E-17,{"$f":"Z3993*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.8523385789757299E-17},{"$f":"AF3992*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB3993^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z3993)*3600*24","v":0},0,{"$f":"AE3992-AD3993*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE3993>$J$18,(AE3993/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.8523385789757299E-17,{"$error":"#N/A"},null,{"$f":"(AD3993)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH3993>0,(AJ3993*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK3992,NA())","v":{"$error":"#N/A"}},null,3976,{"$f":"IF(AF3993<=$J$9*0.05,AS3992*EXP((-$J$6*1)/Heterogenität!$D$4),Z3993)","v":1.1100382799299998E-4},{"$f":"IF(OR(AF3993>=$J$19, AR3992/$J$5<AN3993),0, Bodencharakterisierung!$E$8*$J$11*((AR3992/$J$5)-AN3993))","v":2.8501376566515181E-6},1.1509373477354689E-6,{"$f":"AQ3992-AP3993*Bodencharakterisierung!$E$8","v":3.4699378186268335E-4},{"$f":"AQ3993/(Bodencharakterisierung!$E$11*1000)","v":2.2903879990936195E-7},1.1215476534073545E-4,{"$error":"#N/A"},null,{"$f":"(AP3993)*$G$11*Bodencharakterisierung!$E$8","v":1.6643588843577596E-8},{"$f":"IF(AF3993<=$J$9*1.05,(AV3993*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW3992,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,24.940016639998973,null,0.22903879990936196,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,111.00382799299997]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3987,7.9847305240164793E-17,{"$f":"Z4004*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.9027908530290349E-17},{"$f":"AF4003*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4004^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4004)*3600*24","v":0},0,{"$f":"AE4003-AD4004*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4004>$J$18,(AE4004/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.9027908530290349E-17,{"$error":"#N/A"},null,{"$f":"(AD4004)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4004>0,(AJ4004*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4003,NA())","v":{"$error":"#N/A"}},null,3987,{"$f":"IF(AF4004<=$J$9*0.05,AS4003*EXP((-$J$6*1)/Heterogenität!$D$4),Z4004)","v":1.0983778627571194E-4},{"$f":"IF(OR(AF4004>=$J$19, AR4003/$J$5<AN4004),0, Bodencharakterisierung!$E$8*$J$11*((AR4003/$J$5)-AN4004))","v":2.4496352142522441E-6},1.1388473055656638E-6,{"$f":"AQ4003-AP4004*Bodencharakterisierung!$E$8","v":3.4323043545743083E-4},{"$f":"AQ4004/(Bodencharakterisierung!$E$11*1000)","v":2.2655474287619197E-7},1.109766335812776E-4,{"$error":"#N/A"},null,{"$f":"(AP4004)*$G$11*Bodencharakterisierung!$E$8","v":1.6468755963776045E-8},{"$f":"IF(AF4004<=$J$9*1.05,(AV4004*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4003,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,25.00901567999896,null,0.22655474287619198,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,109.83778627571193]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3994,7.4285121331685867E-17,{"$f":"Z4011*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.3522804008280577E-17},{"$f":"AF4010*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4011^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4011)*3600*24","v":0},0,{"$f":"AE4010-AD4011*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4011>$J$18,(AE4011/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.3522804008280577E-17,{"$error":"#N/A"},null,{"$f":"(AD4011)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4011>0,(AJ4011*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4010,NA())","v":{"$error":"#N/A"}},null,3994,{"$f":"IF(AF4011<=$J$9*0.05,AS4010*EXP((-$J$6*1)/Heterogenität!$D$4),Z4011)","v":1.0880571363742704E-4},{"$f":"IF(OR(AF4011>=$J$19, AR4010/$J$5<AN4011),0, Bodencharakterisierung!$E$8*$J$11*((AR4010/$J$5)-AN4011))","v":5.4205286606900543E-6},1.1281463147398989E-6,{"$f":"AQ4010-AP4011*Bodencharakterisierung!$E$8","v":3.4096147011404316E-4},{"$f":"AQ4011/(Bodencharakterisierung!$E$11*1000)","v":2.2505707598286676E-7},1.0993385995216694E-4,{"$error":"#N/A"},null,{"$f":"(AP4011)*$G$11*Bodencharakterisierung!$E$8","v":1.6314010015290357E-8},{"$f":"IF(AF4011<=$J$9*1.05,(AV4011*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4010,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,25.052924159998952,null,0.22505707598286676,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,108.80571363742703]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3997,7.2021557888195259E-17,{"$f":"Z4014*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.1282469356702355E-17},{"$f":"AF4013*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4014^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4014)*3600*24","v":0},0,{"$f":"AE4013-AD4014*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4014>$J$18,(AE4014/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.1282469356702355E-17,{"$error":"#N/A"},null,{"$f":"(AD4014)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4014>0,(AJ4014*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4013,NA())","v":{"$error":"#N/A"}},null,3997,{"$f":"IF(AF4014<=$J$9*0.05,AS4013*EXP((-$J$6*1)/Heterogenität!$D$4),Z4014)","v":1.0880571363742704E-4},{"$f":"IF(OR(AF4014>=$J$19, AR4013/$J$5<AN4014),0, Bodencharakterisierung!$E$8*$J$11*((AR4013/$J$5)-AN4014))","v":1.9233586330615876E-6},1.1281463147398989E-6,{"$f":"AQ4013-AP4014*Bodencharakterisierung!$E$8","v":3.3984460526245063E-4},{"$f":"AQ4014/(Bodencharakterisierung!$E$11*1000)","v":2.2431987146036346E-7},1.0993385995216694E-4,{"$error":"#N/A"},null,{"$f":"(AP4014)*$G$11*Bodencharakterisierung!$E$8","v":1.6314010015290357E-8},{"$f":"IF(AF4014<=$J$9*1.05,(AV4014*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4013,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,25.071742079998948,null,0.22431987146036347,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,108.80571363742703]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4013,6.10641206390176E-17,{"$f":"Z4030*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.0437477831317451E-17},{"$f":"AF4029*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4030^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4030)*3600*24","v":0},0,{"$f":"AE4029-AD4030*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4030>$J$18,(AE4030/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.0437477831317451E-17,{"$error":"#N/A"},null,{"$f":"(AD4030)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4030>0,(AJ4030*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4029,NA())","v":{"$error":"#N/A"}},null,4013,{"$f":"IF(AF4030<=$J$9*0.05,AS4029*EXP((-$J$6*1)/Heterogenität!$D$4),Z4030)","v":1.0724585844670784E-4},{"$f":"IF(OR(AF4030>=$J$19, AR4029/$J$5<AN4030),0, Bodencharakterisierung!$E$8*$J$11*((AR4029/$J$5)-AN4030))","v":3.1313432564956936E-7},3.1313432564956936E-7,{"$f":"AQ4029-AP4030*Bodencharakterisierung!$E$8","v":3.3473071905407419E-4},{"$f":"AQ4030/(Bodencharakterisierung!$E$11*1000)","v":2.2094436901259023E-7},1.0755899277235741E-4,{"$error":"#N/A"},null,{"$f":"(AP4030)*$G$11*Bodencharakterisierung!$E$8","v":4.5282038845786218E-9},{"$f":"IF(AF4030<=$J$9*1.05,(AV4030*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4029,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,25.17210431999893,null,0.22094436901259024,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,107.24585844670784]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4018,5.7994556437099823E-17,{"$f":"Z4035*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.7399413638075417E-17},{"$f":"AF4034*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4035^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4035)*3600*24","v":0},0,{"$f":"AE4034-AD4035*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4035>$J$18,(AE4035/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.7399413638075417E-17,{"$error":"#N/A"},null,{"$f":"(AD4035)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4035>0,(AJ4035*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4034,NA())","v":{"$error":"#N/A"}},null,4018,{"$f":"IF(AF4035<=$J$9*0.05,AS4034*EXP((-$J$6*1)/Heterogenität!$D$4),Z4035)","v":1.0645521745357875E-4},{"$f":"IF(OR(AF4035>=$J$19, AR4034/$J$5<AN4035),0, Bodencharakterisierung!$E$8*$J$11*((AR4034/$J$5)-AN4035))","v":3.1544770162282331E-6},1.1037753187786536E-6,{"$f":"AQ4034-AP4035*Bodencharakterisierung!$E$8","v":3.3290948977808934E-4},{"$f":"AQ4035/(Bodencharakterisierung!$E$11*1000)","v":2.1974223747728668E-7},1.0755899277235741E-4,{"$error":"#N/A"},null,{"$f":"(AP4035)*$G$11*Bodencharakterisierung!$E$8","v":1.5961583501991837E-8},{"$f":"IF(AF4035<=$J$9*1.05,(AV4035*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4034,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,25.203467519998924,null,0.21974223747728669,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,106.45521745357875]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4027,5.2852952600078706E-17,{"$f":"Z4044*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.2310573175533396E-17},{"$f":"AF4043*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4044^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4044)*3600*24","v":0},0,{"$f":"AE4043-AD4044*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4044>$J$18,(AE4044/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.2310573175533396E-17,{"$error":"#N/A"},null,{"$f":"(AD4044)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4044>0,(AJ4044*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4043,NA())","v":{"$error":"#N/A"}},null,4027,{"$f":"IF(AF4044<=$J$9*0.05,AS4043*EXP((-$J$6*1)/Heterogenität!$D$4),Z4044)","v":1.0544731292171001E-4},{"$f":"IF(OR(AF4044>=$J$19, AR4043/$J$5<AN4044),0, Bodencharakterisierung!$E$8*$J$11*((AR4043/$J$5)-AN4044))","v":3.8324599810530274E-6},1.0933249136921405E-6,{"$f":"AQ4043-AP4044*Bodencharakterisierung!$E$8","v":3.2998360529611819E-4},{"$f":"AQ4044/(Bodencharakterisierung!$E$11*1000)","v":2.1781096059149717E-7},1.0654063783540215E-4,{"$error":"#N/A"},null,{"$f":"(AP4044)*$G$11*Bodencharakterisierung!$E$8","v":1.5810461248594659E-8},{"$f":"IF(AF4044<=$J$9*1.05,(AV4044*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4043,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,25.259921279998913,null,0.21781096059149715,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,105.44731292171001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4034,4.9171202269450383E-17,{"$f":"Z4051*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.8666605135721545E-17},{"$f":"AF4050*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4051^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4051)*3600*24","v":0},0,{"$f":"AE4050-AD4051*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4051>$J$18,(AE4051/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.8666605135721545E-17,{"$error":"#N/A"},null,{"$f":"(AD4051)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4051>0,(AJ4051*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4050,NA())","v":{"$error":"#N/A"}},null,4034,{"$f":"IF(AF4051<=$J$9*0.05,AS4050*EXP((-$J$6*1)/Heterogenität!$D$4),Z4051)","v":1.0480389299157143E-4},{"$f":"IF(OR(AF4051>=$J$19, AR4050/$J$5<AN4051),0, Bodencharakterisierung!$E$8*$J$11*((AR4050/$J$5)-AN4051))","v":2.9049434886472845E-6},1.0866536480136276E-6,{"$f":"AQ4050-AP4051*Bodencharakterisierung!$E$8","v":3.2768136091080463E-4},{"$f":"AQ4051/(Bodencharakterisierung!$E$11*1000)","v":2.1629132733386445E-7},1.0589054663958506E-4,{"$error":"#N/A"},null,{"$f":"(AP4051)*$G$11*Bodencharakterisierung!$E$8","v":1.5713988748820536E-8},{"$f":"IF(AF4051<=$J$9*1.05,(AV4051*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4050,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,25.303829759998905,null,0.21629132733386444,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,104.80389299157143]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4046,{"$f":"AG4062","v":4.3446372784247565E-17},{"$f":"Z4063*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.3000524113358621E-17},{"$f":"AF4062*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4063^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4063)*3600*24","v":0},{"$f":"MIN(AC4063,Z4063-AA4063)","v":0},{"$f":"AE4062-AD4063*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4063>$J$18,(AE4063/(Bodencharakterisierung!$E$11*1000)),0)","v":0},{"$f":"AA4063+AD4063","v":4.3000524113358621E-17},{"$f":"IF(AD4063>0,Y4063,NA())","v":{"$error":"#N/A"}},null,{"$f":"(AD4063)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4063>0,(AJ4063*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4062,NA())","v":{"$error":"#N/A"}},null,4046,{"$f":"IF(AF4063<=$J$9*0.05,AS4062*EXP((-$J$6*1)/Heterogenität!$D$4),Z4063)","v":1.0350243814942168E-4},{"$f":"IF(OR(AF4063>=$J$19, AR4062/$J$5<AN4063),0, Bodencharakterisierung!$E$8*$J$11*((AR4062/$J$5)-AN4063))","v":3.5709162395317009E-6},{"$f":"MIN(AO4063,AS4062-AN4063)","v":1.073159581986319E-6},{"$f":"AQ4062-AP4063*Bodencharakterisierung!$E$8","v":3.2383642071404171E-4},{"$f":"AQ4063/(Bodencharakterisierung!$E$11*1000)","v":2.1375341301256879E-7},{"$f":"AN4063+AP4063","v":1.04575597731408E-4},{"$f":"IF(AN4063>$G$5,AM4063,NA())","v":{"$error":"#N/A"}},null,{"$f":"(AP4063)*$G$11*Bodencharakterisierung!$E$8","v":1.5518852421696819E-8},{"$f":"IF(AF4063<=$J$9*1.05,(AV4063*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4062,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH4063>($G$5*10^6),BH4063*0.99,9999)","v":9999},{"$f":"AT4063+$G$3","v":{"$error":"#N/A"}},{"$f":"IF(ISNUMBER(AT4063),BA4063+BB4063+BC4063+$AZ$17,\"\")","v":""},{"$f":"IF(ISNUMBER(AK4063),AK4063,BA4062)","v":1.6399886323194495},{"$f":"IF(ISNUMBER(AW4063),AW4063,0)","v":0},25.379101439998891,null,{"$f":"AR4063*10^6","v":0.21375341301256878},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF4063*10^6","v":0},{"$f":"AN4063*10^6","v":103.50243814942168}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4053,4.0419887233414467E-17,{"$f":"Z4070*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.0005096496107331E-17},{"$f":"AF4069*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4070^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4070)*3600*24","v":0},0,{"$f":"AE4069-AD4070*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4070>$J$18,(AE4070/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.0005096496107331E-17,{"$error":"#N/A"},null,{"$f":"(AD4070)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4070>0,(AJ4070*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4069,NA())","v":{"$error":"#N/A"}},null,4053,{"$f":"IF(AF4070<=$J$9*0.05,AS4069*EXP((-$J$6*1)/Heterogenität!$D$4),Z4070)","v":1.0268198638956335E-4},{"$f":"IF(OR(AF4070>=$J$19, AR4069/$J$5<AN4070),0, Bodencharakterisierung!$E$8*$J$11*((AR4069/$J$5)-AN4070))","v":4.7099363871170273E-6},1.0646527710996137E-6,{"$f":"AQ4069-AP4070*Bodencharakterisierung!$E$8","v":3.2164220739836966E-4},{"$f":"AQ4070/(Bodencharakterisierung!$E$11*1000)","v":2.1230508739166313E-7},1.0374663916066296E-4,{"$error":"#N/A"},null,{"$f":"(AP4070)*$G$11*Bodencharakterisierung!$E$8","v":1.5395836287893385E-8},{"$f":"IF(AF4070<=$J$9*1.05,(AV4070*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4069,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,25.423009919998883,null,0.21230508739166312,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,102.68198638956335]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4059,3.7994124900779817E-17,{"$f":"Z4076*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.7604227447827359E-17},{"$f":"AF4075*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4076^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4076)*3600*24","v":0},0,{"$f":"AE4075-AD4076*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4076>$J$18,(AE4076/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.7604227447827359E-17,{"$error":"#N/A"},null,{"$f":"(AD4076)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4076>0,(AJ4076*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4075,NA())","v":{"$error":"#N/A"}},null,4059,{"$f":"IF(AF4076<=$J$9*0.05,AS4075*EXP((-$J$6*1)/Heterogenität!$D$4),Z4076)","v":1.0193455999740327E-4},{"$f":"IF(OR(AF4076>=$J$19, AR4075/$J$5<AN4076),0, Bodencharakterisierung!$E$8*$J$11*((AR4075/$J$5)-AN4076))","v":6.2023103653671482E-6},1.0569031198941203E-6,{"$f":"AQ4075-AP4076*Bodencharakterisierung!$E$8","v":3.1978851777569878E-4},{"$f":"AQ4076/(Bodencharakterisierung!$E$11*1000)","v":2.1108152988494968E-7},1.0299146311729739E-4,{"$error":"#N/A"},null,{"$f":"(AP4076)*$G$11*Bodencharakterisierung!$E$8","v":1.5283769363834362E-8},{"$f":"IF(AF4076<=$J$9*1.05,(AV4076*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4075,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,25.460645759998876,null,0.21108152988494969,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,101.93455999740327]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4067,3.4984707250220556E-17,{"$f":"Z4084*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.4625692579274192E-17},{"$f":"AF4083*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4084^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4084)*3600*24","v":0},0,{"$f":"AE4083-AD4084*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4084>$J$18,(AE4084/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.4625692579274192E-17,{"$error":"#N/A"},null,{"$f":"(AD4084)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4084>0,(AJ4084*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4083,NA())","v":{"$error":"#N/A"}},null,4067,{"$f":"IF(AF4084<=$J$9*0.05,AS4083*EXP((-$J$6*1)/Heterogenität!$D$4),Z4084)","v":1.0162266543898417E-4},{"$f":"IF(OR(AF4084>=$J$19, AR4083/$J$5<AN4084),0, Bodencharakterisierung!$E$8*$J$11*((AR4083/$J$5)-AN4084))","v":8.4596015123137743E-7},8.4596015123137743E-7,{"$f":"AQ4083-AP4084*Bodencharakterisierung!$E$8","v":3.1717403144680434E-4},{"$f":"AQ4084/(Bodencharakterisierung!$E$11*1000)","v":2.0935579633452432E-7},1.0246862559021554E-4,{"$error":"#N/A"},null,{"$f":"(AP4084)*$G$11*Bodencharakterisierung!$E$8","v":1.2233344380429186E-8},{"$f":"IF(AF4084<=$J$9*1.05,(AV4084*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4083,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,25.510826879998866,null,0.20935579633452431,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,101.62266543898417]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4083,2.9662096276291954E-17,{"$f":"Z4100*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.9357702483368475E-17},{"$f":"AF4099*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4100^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4100)*3600*24","v":0},0,{"$f":"AE4099-AD4100*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4100>$J$18,(AE4100/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.9357702483368475E-17,{"$error":"#N/A"},null,{"$f":"(AD4100)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4100>0,(AJ4100*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4099,NA())","v":{"$error":"#N/A"}},null,4083,{"$f":"IF(AF4100<=$J$9*0.05,AS4099*EXP((-$J$6*1)/Heterogenität!$D$4),Z4100)","v":1.0001539401919902E-4},{"$f":"IF(OR(AF4100>=$J$19, AR4099/$J$5<AN4100),0, Bodencharakterisierung!$E$8*$J$11*((AR4099/$J$5)-AN4100))","v":9.6034146316220437E-7},9.6034146316220437E-7,{"$f":"AQ4099-AP4100*Bodencharakterisierung!$E$8","v":3.1215622498406335E-4},{"$f":"AQ4100/(Bodencharakterisierung!$E$11*1000)","v":2.0604371286076788E-7},1.0097573548236123E-4,{"$error":"#N/A"},null,{"$f":"(AP4100)*$G$11*Bodencharakterisierung!$E$8","v":1.388740098994954E-8},{"$f":"IF(AF4100<=$J$9*1.05,(AV4100*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4099,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,25.611189119998848,null,0.20604371286076789,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,100.01539401919902]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4086,2.8758253951144208E-17,{"$f":"Z4103*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.8463135429630875E-17},{"$f":"AF4102*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4103^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4103)*3600*24","v":0},0,{"$f":"AE4102-AD4103*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4103>$J$18,(AE4103/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.8463135429630875E-17,{"$error":"#N/A"},null,{"$f":"(AD4103)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4103>0,(AJ4103*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4102,NA())","v":{"$error":"#N/A"}},null,4086,{"$f":"IF(AF4103<=$J$9*0.05,AS4102*EXP((-$J$6*1)/Heterogenität!$D$4),Z4103)","v":9.9616215428587719E-5},{"$f":"IF(OR(AF4103>=$J$19, AR4102/$J$5<AN4103),0, Bodencharakterisierung!$E$8*$J$11*((AR4102/$J$5)-AN4103))","v":2.0687863612558725E-6},1.0328654862610143E-6,{"$f":"AQ4102-AP4103*Bodencharakterisierung!$E$8","v":3.1124037795237156E-4},{"$f":"AQ4103/(Bodencharakterisierung!$E$11*1000)","v":2.0543919336790201E-7},1.0064908091484873E-4,{"$error":"#N/A"},null,{"$f":"(AP4103)*$G$11*Bodencharakterisierung!$E$8","v":1.49361635695232E-8},{"$f":"IF(AF4103<=$J$9*1.05,(AV4103*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4102,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,25.630007039998844,null,0.20543919336790201,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,99.616215428587722]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4098,2.541003197234693E-17,{"$f":"Z4115*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.5149273058400863E-17},{"$f":"AF4114*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4115^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4115)*3600*24","v":0},0,{"$f":"AE4114-AD4115*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4115>$J$18,(AE4115/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.5149273058400863E-17,{"$error":"#N/A"},null,{"$f":"(AD4115)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4115>0,(AJ4115*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4114,NA())","v":{"$error":"#N/A"}},null,4098,{"$f":"IF(AF4115<=$J$9*0.05,AS4114*EXP((-$J$6*1)/Heterogenität!$D$4),Z4115)","v":9.7864395322757287E-5},{"$f":"IF(OR(AF4115>=$J$19, AR4114/$J$5<AN4115),0, Bodencharakterisierung!$E$8*$J$11*((AR4114/$J$5)-AN4115))","v":8.2978966659667677E-6},1.0147018317026996E-6,{"$f":"AQ4114-AP4115*Bodencharakterisierung!$E$8","v":3.0776796323571994E-4},{"$f":"AQ4115/(Bodencharakterisierung!$E$11*1000)","v":2.0314717045262041E-7},9.8879097154459987E-5,{"$error":"#N/A"},null,{"$f":"(AP4115)*$G$11*Bodencharakterisierung!$E$8","v":1.4673500793864584E-8},{"$f":"IF(AF4115<=$J$9*1.05,(AV4115*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4114,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,25.70527871999883,null,0.2031471704526204,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,97.864395322757289]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4108,2.2919622436008209E-17,{"$f":"Z4125*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.268442021898733E-17},{"$f":"AF4124*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4125^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4125)*3600*24","v":0},0,{"$f":"AE4124-AD4125*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4125>$J$18,(AE4125/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.268442021898733E-17,{"$error":"#N/A"},null,{"$f":"(AD4125)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4125>0,(AJ4125*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4124,NA())","v":{"$error":"#N/A"}},null,4108,{"$f":"IF(AF4125<=$J$9*0.05,AS4124*EXP((-$J$6*1)/Heterogenität!$D$4),Z4125)","v":9.731241027598405E-5},{"$f":"IF(OR(AF4125>=$J$19, AR4124/$J$5<AN4125),0, Bodencharakterisierung!$E$8*$J$11*((AR4124/$J$5)-AN4125))","v":3.7903347136025208E-6},1.008978603799586E-6,{"$f":"AQ4124-AP4125*Bodencharakterisierung!$E$8","v":3.0460745893240535E-4},{"$f":"AQ4125/(Bodencharakterisierung!$E$11*1000)","v":2.0106102899828735E-7},9.8321388879783636E-5,{"$error":"#N/A"},null,{"$f":"(AP4125)*$G$11*Bodencharakterisierung!$E$8","v":1.4590737772693247E-8},{"$f":"IF(AF4125<=$J$9*1.05,(AV4125*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4124,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,25.768005119998818,null,0.20106102899828734,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,97.31241027598405]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4116,2.1104217646894053E-17,{"$f":"Z4133*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.0887645197112235E-17},{"$f":"AF4132*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4133^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4133)*3600*24","v":0},0,{"$f":"AE4132-AD4133*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4133>$J$18,(AE4133/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.0887645197112235E-17,{"$error":"#N/A"},null,{"$f":"(AD4133)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4133>0,(AJ4133*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4132,NA())","v":{"$error":"#N/A"}},null,4116,{"$f":"IF(AF4133<=$J$9*0.05,AS4132*EXP((-$J$6*1)/Heterogenität!$D$4),Z4133)","v":9.6184185157330494E-5},{"$f":"IF(OR(AF4133>=$J$19, AR4132/$J$5<AN4133),0, Bodencharakterisierung!$E$8*$J$11*((AR4132/$J$5)-AN4133))","v":7.6685660927519035E-6},9.972806610422083E-7,{"$f":"AQ4132-AP4133*Bodencharakterisierung!$E$8","v":3.0232848268816476E-4},{"$f":"AQ4133/(Bodencharakterisierung!$E$11*1000)","v":1.995567542496137E-7},9.7181465818372702E-5,{"$error":"#N/A"},null,{"$f":"(AP4133)*$G$11*Bodencharakterisierung!$E$8","v":1.4421575002927738E-8},{"$f":"IF(AF4133<=$J$9*1.05,(AV4133*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4132,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,25.818186239998809,null,0.19955675424961369,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,96.184185157330489]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4123,1.963409239415673E-17,{"$f":"Z4140*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.943260643716979E-17},{"$f":"AF4139*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4140^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4140)*3600*24","v":0},0,{"$f":"AE4139-AD4140*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4140>$J$18,(AE4140/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.943260643716979E-17,{"$error":"#N/A"},null,{"$f":"(AD4140)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4140>0,(AJ4140*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4139,NA())","v":{"$error":"#N/A"}},null,4123,{"$f":"IF(AF4140<=$J$9*0.05,AS4139*EXP((-$J$6*1)/Heterogenität!$D$4),Z4140)","v":9.6184185157330494E-5},{"$f":"IF(OR(AF4140>=$J$19, AR4139/$J$5<AN4140),0, Bodencharakterisierung!$E$8*$J$11*((AR4139/$J$5)-AN4140))","v":4.5507497623804401E-7},4.5507497623804401E-7,{"$f":"AQ4139-AP4140*Bodencharakterisierung!$E$8","v":3.0020369223714258E-4},{"$f":"AQ4140/(Bodencharakterisierung!$E$11*1000)","v":1.9815425230174427E-7},9.6639260133568543E-5,{"$error":"#N/A"},null,{"$f":"(AP4140)*$G$11*Bodencharakterisierung!$E$8","v":6.5807933093919143E-9},{"$f":"IF(AF4140<=$J$9*1.05,(AV4140*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4139,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,25.862094719998801,null,0.19815425230174427,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,96.184185157330489]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4135,1.7348164333310857E-17,{"$f":"Z4152*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.7170136674965718E-17},{"$f":"AF4151*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4152^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4152)*3600*24","v":0},0,{"$f":"AE4151-AD4152*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4152>$J$18,(AE4152/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.7170136674965718E-17,{"$error":"#N/A"},null,{"$f":"(AD4152)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4152>0,(AJ4152*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4151,NA())","v":{"$error":"#N/A"}},null,4135,{"$f":"IF(AF4152<=$J$9*0.05,AS4151*EXP((-$J$6*1)/Heterogenität!$D$4),Z4152)","v":9.4770703789515614E-5},{"$f":"IF(OR(AF4152>=$J$19, AR4151/$J$5<AN4152),0, Bodencharakterisierung!$E$8*$J$11*((AR4151/$J$5)-AN4152))","v":3.4892069128716469E-6},9.8262505388018058E-7,{"$f":"AQ4151-AP4152*Bodencharakterisierung!$E$8","v":2.9658685324379013E-4},{"$f":"AQ4152/(Bodencharakterisierung!$E$11*1000)","v":1.9576689983088457E-7},9.5753328843395795E-5,{"$error":"#N/A"},null,{"$f":"(AP4152)*$G$11*Bodencharakterisierung!$E$8","v":1.4209641746666909E-8},{"$f":"IF(AF4152<=$J$9*1.05,(AV4152*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4151,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,25.937366399998787,null,0.19576689983088458,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,94.770703789515608]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4139,1.6646940468236066E-17,{"$f":"Z4156*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.6476108801367402E-17},{"$f":"AF4155*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4156^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4156)*3600*24","v":0},0,{"$f":"AE4155-AD4156*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4156>$J$18,(AE4156/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.6476108801367402E-17,{"$error":"#N/A"},null,{"$f":"(AD4156)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4156>0,(AJ4156*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4155,NA())","v":{"$error":"#N/A"}},null,4139,{"$f":"IF(AF4156<=$J$9*0.05,AS4155*EXP((-$J$6*1)/Heterogenität!$D$4),Z4156)","v":9.4236756952232771E-5},{"$f":"IF(OR(AF4156>=$J$19, AR4155/$J$5<AN4156),0, Bodencharakterisierung!$E$8*$J$11*((AR4155/$J$5)-AN4156))","v":5.2035931482667643E-6},9.7708885420269662E-7,{"$f":"AQ4155-AP4156*Bodencharakterisierung!$E$8","v":2.9546964452075878E-4},{"$f":"AQ4156/(Bodencharakterisierung!$E$11*1000)","v":1.9502946833053385E-7},9.5213845806435467E-5,{"$error":"#N/A"},null,{"$f":"(AP4156)*$G$11*Bodencharakterisierung!$E$8","v":1.4129583321793231E-8},{"$f":"IF(AF4156<=$J$9*1.05,(AV4156*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4155,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,25.962456959998782,null,0.19502946833053386,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,94.236756952232767]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4153,1.4408460259424905E-17,{"$f":"Z4170*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.426059997916349E-17},{"$f":"AF4169*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4170^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4170)*3600*24","v":0},0,{"$f":"AE4169-AD4170*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4170>$J$18,(AE4170/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.426059997916349E-17,{"$error":"#N/A"},null,{"$f":"(AD4170)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4170>0,(AJ4170*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4169,NA())","v":{"$error":"#N/A"}},null,4153,{"$f":"IF(AF4170<=$J$9*0.05,AS4169*EXP((-$J$6*1)/Heterogenität!$D$4),Z4170)","v":9.3391459189046542E-5},{"$f":"IF(OR(AF4170>=$J$19, AR4169/$J$5<AN4170),0, Bodencharakterisierung!$E$8*$J$11*((AR4169/$J$5)-AN4170))","v":2.8216407405471228E-7},2.8216407405471228E-7,{"$f":"AQ4169-AP4170*Bodencharakterisierung!$E$8","v":2.9148892016698987E-4},{"$f":"AQ4170/(Bodencharakterisierung!$E$11*1000)","v":1.9240192750296362E-7},9.3673623263101254E-5,{"$error":"#N/A"},null,{"$f":"(AP4170)*$G$11*Bodencharakterisierung!$E$8","v":4.0803462014987027E-9},{"$f":"IF(AF4170<=$J$9*1.05,(AV4170*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4169,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,26.050273919998766,null,0.19240192750296362,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,93.391459189046543]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4156,1.3969415894476012E-17,{"$f":"Z4173*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.3826061107631639E-17},{"$f":"AF4172*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4173^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4173)*3600*24","v":0},0,{"$f":"AE4172-AD4173*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4173>$J$18,(AE4173/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.3826061107631639E-17,{"$error":"#N/A"},null,{"$f":"(AD4173)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4173>0,(AJ4173*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4172,NA())","v":{"$error":"#N/A"}},null,4156,{"$f":"IF(AF4173<=$J$9*0.05,AS4172*EXP((-$J$6*1)/Heterogenität!$D$4),Z4173)","v":9.2712340243305687E-5},{"$f":"IF(OR(AF4173>=$J$19, AR4172/$J$5<AN4173),0, Bodencharakterisierung!$E$8*$J$11*((AR4172/$J$5)-AN4173))","v":4.6411427952676605E-6},9.6128301979556715E-7,{"$f":"AQ4172-AP4173*Bodencharakterisierung!$E$8","v":2.9053724997739219E-4},{"$f":"AQ4173/(Bodencharakterisierung!$E$11*1000)","v":1.9177376236131497E-7},9.3673623263101254E-5,{"$error":"#N/A"},null,{"$f":"(AP4173)*$G$11*Bodencharakterisierung!$E$8","v":1.3901016745411352E-8},{"$f":"IF(AF4173<=$J$9*1.05,(AV4173*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4172,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,26.069091839998762,null,0.19177376236131496,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,92.71234024330569]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4172,1.1844093941443467E-17,{"$f":"Z4189*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.1722549305993692E-17},{"$f":"AF4188*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4189^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4189)*3600*24","v":0},0,{"$f":"AE4188-AD4189*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4189>$J$18,(AE4189/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.1722549305993692E-17,{"$error":"#N/A"},null,{"$f":"(AD4189)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4189>0,(AJ4189*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4188,NA())","v":{"$error":"#N/A"}},null,4172,{"$f":"IF(AF4189<=$J$9*0.05,AS4188*EXP((-$J$6*1)/Heterogenität!$D$4),Z4189)","v":9.1527633859926657E-5},{"$f":"IF(OR(AF4189>=$J$19, AR4188/$J$5<AN4189),0, Bodencharakterisierung!$E$8*$J$11*((AR4188/$J$5)-AN4189))","v":1.6578337387851839E-6},9.4899945401782969E-7,{"$f":"AQ4188-AP4189*Bodencharakterisierung!$E$8","v":2.8589086008400392E-4},{"$f":"AQ4189/(Bodencharakterisierung!$E$11*1000)","v":1.8870683833927652E-7},9.2476633313944487E-5,{"$error":"#N/A"},null,{"$f":"(AP4189)*$G$11*Bodencharakterisierung!$E$8","v":1.3723385340244119E-8},{"$f":"IF(AF4189<=$J$9*1.05,(AV4189*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4188,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,26.169454079998744,null,0.18870683833927651,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,91.527633859926652]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4175,1.1483189125155787E-17,{"$f":"Z4192*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.1365348111489547E-17},{"$f":"AF4191*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4192^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4192)*3600*24","v":0},0,{"$f":"AE4191-AD4192*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4192>$J$18,(AE4192/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.1365348111489547E-17,{"$error":"#N/A"},null,{"$f":"(AD4192)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4192>0,(AJ4192*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4191,NA())","v":{"$error":"#N/A"}},null,4175,{"$f":"IF(AF4192<=$J$9*0.05,AS4191*EXP((-$J$6*1)/Heterogenität!$D$4),Z4192)","v":9.1258647770597076E-5},{"$f":"IF(OR(AF4192>=$J$19, AR4191/$J$5<AN4192),0, Bodencharakterisierung!$E$8*$J$11*((AR4191/$J$5)-AN4192))","v":1.6285620730429218E-6},9.4621048590900374E-7,{"$f":"AQ4191-AP4192*Bodencharakterisierung!$E$8","v":2.8504287711243276E-4},{"$f":"AQ4192/(Bodencharakterisierung!$E$11*1000)","v":1.8814711360556618E-7},9.220485825650608E-5,{"$error":"#N/A"},null,{"$f":"(AP4192)*$G$11*Bodencharakterisierung!$E$8","v":1.3683054353859429E-8},{"$f":"IF(AF4192<=$J$9*1.05,(AV4192*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4191,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,26.18827199999874,null,0.18814711360556619,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,91.258647770597079]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4188,1.0042120755328816E-17,{"$f":"Z4205*EXP((-$J$6/Heterogenität!$D$4)*1)","v":9.9390680513918613E-18},{"$f":"AF4204*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4205^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4205)*3600*24","v":0},0,{"$f":"AE4204-AD4205*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4205>$J$18,(AE4205/(Bodencharakterisierung!$E$11*1000)),0)","v":0},9.9390680513918613E-18,{"$error":"#N/A"},null,{"$f":"(AD4205)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4205>0,(AJ4205*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4204,NA())","v":{"$error":"#N/A"}},null,4188,{"$f":"IF(AF4205<=$J$9*0.05,AS4204*EXP((-$J$6*1)/Heterogenität!$D$4),Z4205)","v":8.9744817457691016E-5},{"$f":"IF(OR(AF4205>=$J$19, AR4204/$J$5<AN4205),0, Bodencharakterisierung!$E$8*$J$11*((AR4204/$J$5)-AN4205))","v":5.3801005900475357E-6},9.3051441599178422E-7,{"$f":"AQ4204-AP4205*Bodencharakterisierung!$E$8","v":2.8152121456906224E-4},{"$f":"AQ4205/(Bodencharakterisierung!$E$11*1000)","v":1.8582258387396847E-7},9.06753318736828E-5,{"$error":"#N/A"},null,{"$f":"(AP4205)*$G$11*Bodencharakterisierung!$E$8","v":1.3456075070689714E-8},{"$f":"IF(AF4205<=$J$9*1.05,(AV4205*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4204,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,26.269816319998725,null,0.18582258387396847,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,89.744817457691013]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4193,9.5373245827266526E-18,{"$f":"Z4210*EXP((-$J$6/Heterogenität!$D$4)*1)","v":9.4394521202736579E-18},{"$f":"AF4209*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4210^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4210)*3600*24","v":0},0,{"$f":"AE4209-AD4210*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4210>$J$18,(AE4210/(Bodencharakterisierung!$E$11*1000)),0)","v":0},9.4394521202736579E-18,{"$error":"#N/A"},null,{"$f":"(AD4210)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4210>0,(AJ4210*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4209,NA())","v":{"$error":"#N/A"}},null,4193,{"$f":"IF(AF4210<=$J$9*0.05,AS4209*EXP((-$J$6*1)/Heterogenität!$D$4),Z4210)","v":8.9744817457691016E-5},{"$f":"IF(OR(AF4210>=$J$19, AR4209/$J$5<AN4210),0, Bodencharakterisierung!$E$8*$J$11*((AR4209/$J$5)-AN4210))","v":5.7255762721713717E-7},5.7255762721713717E-7,{"$f":"AQ4209-AP4210*Bodencharakterisierung!$E$8","v":2.801039915229715E-4},{"$f":"AQ4210/(Bodencharakterisierung!$E$11*1000)","v":1.8488712311747294E-7},9.0317375084908157E-5,{"$error":"#N/A"},null,{"$f":"(AP4210)*$G$11*Bodencharakterisierung!$E$8","v":8.2796980699305985E-9},{"$f":"IF(AF4210<=$J$9*1.05,(AV4210*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4209,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,26.301179519998719,null,0.18488712311747293,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,89.744817457691013]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4205,8.4269275523277191E-18,{"$f":"Z4222*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.3404500351471609E-18},{"$f":"AF4221*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4222^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4222)*3600*24","v":0},0,{"$f":"AE4221-AD4222*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4222>$J$18,(AE4222/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.3404500351471609E-18,{"$error":"#N/A"},null,{"$f":"(AD4222)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4222>0,(AJ4222*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4221,NA())","v":{"$error":"#N/A"}},null,4205,{"$f":"IF(AF4222<=$J$9*0.05,AS4221*EXP((-$J$6*1)/Heterogenität!$D$4),Z4222)","v":8.8686423919772899E-5},{"$f":"IF(OR(AF4222>=$J$19, AR4221/$J$5<AN4222),0, Bodencharakterisierung!$E$8*$J$11*((AR4221/$J$5)-AN4222))","v":5.6281038951159152E-7},5.6281038951159152E-7,{"$f":"AQ4221-AP4222*Bodencharakterisierung!$E$8","v":2.7680065430649338E-4},{"$f":"AQ4222/(Bodencharakterisierung!$E$11*1000)","v":1.8270670251253688E-7},8.9249234309284484E-5,{"$error":"#N/A"},null,{"$f":"(AP4222)*$G$11*Bodencharakterisierung!$E$8","v":8.1387442490723977E-9},{"$f":"IF(AF4222<=$J$9*1.05,(AV4222*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4221,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,26.376451199998705,null,0.18270670251253687,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,88.686423919772892]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4208,8.170148202621568E-18,{"$f":"Z4225*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.0863057669090699E-18},{"$f":"AF4224*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4225^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4225)*3600*24","v":0},0,{"$f":"AE4224-AD4225*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4225>$J$18,(AE4225/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.0863057669090699E-18,{"$error":"#N/A"},null,{"$f":"(AD4225)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4225>0,(AJ4225*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4224,NA())","v":{"$error":"#N/A"}},null,4208,{"$f":"IF(AF4225<=$J$9*0.05,AS4224*EXP((-$J$6*1)/Heterogenität!$D$4),Z4225)","v":8.8333354571929796E-5},{"$f":"IF(OR(AF4225>=$J$19, AR4224/$J$5<AN4225),0, Bodencharakterisierung!$E$8*$J$11*((AR4224/$J$5)-AN4225))","v":1.5390876632835587E-6},9.1587973735468792E-7,{"$f":"AQ4224-AP4225*Bodencharakterisierung!$E$8","v":2.7589393336651221E-4},{"$f":"AQ4225/(Bodencharakterisierung!$E$11*1000)","v":1.821082068425823E-7},8.9249234309284484E-5,{"$error":"#N/A"},null,{"$f":"(AP4225)*$G$11*Bodencharakterisierung!$E$8","v":1.3244444459716003E-8},{"$f":"IF(AF4225<=$J$9*1.05,(AV4225*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4224,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,26.395269119998702,null,0.1821082068425823,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,88.333354571929803]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4219,7.2937757528745702E-18,{"$f":"Z4236*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.2189266914505015E-18},{"$f":"AF4235*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4236^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4236)*3600*24","v":0},0,{"$f":"AE4235-AD4236*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4236>$J$18,(AE4236/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.2189266914505015E-18,{"$error":"#N/A"},null,{"$f":"(AD4236)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4236>0,(AJ4236*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4235,NA())","v":{"$error":"#N/A"}},null,4219,{"$f":"IF(AF4236<=$J$9*0.05,AS4235*EXP((-$J$6*1)/Heterogenität!$D$4),Z4236)","v":8.7384892710999607E-5},{"$f":"IF(OR(AF4236>=$J$19, AR4235/$J$5<AN4236),0, Bodencharakterisierung!$E$8*$J$11*((AR4235/$J$5)-AN4236))","v":1.4530478198737435E-6},9.0604566047296914E-7,{"$f":"AQ4235-AP4236*Bodencharakterisierung!$E$8","v":2.7290937679580473E-4},{"$f":"AQ4236/(Bodencharakterisierung!$E$11*1000)","v":1.8013820250548167E-7},8.8290938371472576E-5,{"$error":"#N/A"},null,{"$f":"(AP4236)*$G$11*Bodencharakterisierung!$E$8","v":1.3102234866294174E-8},{"$f":"IF(AF4236<=$J$9*1.05,(AV4236*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4235,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,26.464268159998689,null,0.18013820250548168,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,87.384892710999608]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4226,6.7856894498657422E-18,{"$f":"Z4243*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.7160543933948217E-18},{"$f":"AF4242*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4243^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4243)*3600*24","v":0},0,{"$f":"AE4242-AD4243*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4243>$J$18,(AE4243/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.7160543933948217E-18,{"$error":"#N/A"},null,{"$f":"(AD4243)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4243>0,(AJ4243*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4242,NA())","v":{"$error":"#N/A"}},null,4226,{"$f":"IF(AF4243<=$J$9*0.05,AS4242*EXP((-$J$6*1)/Heterogenität!$D$4),Z4243)","v":8.6125970078691346E-5},{"$f":"IF(OR(AF4243>=$J$19, AR4242/$J$5<AN4243),0, Bodencharakterisierung!$E$8*$J$11*((AR4242/$J$5)-AN4243))","v":8.5381197585944498E-6},8.9299258742467867E-7,{"$f":"AQ4242-AP4243*Bodencharakterisierung!$E$8","v":2.7124706128123818E-4},{"$f":"AQ4243/(Bodencharakterisierung!$E$11*1000)","v":1.7904096454207141E-7},8.7018962666116025E-5,{"$error":"#N/A"},null,{"$f":"(AP4243)*$G$11*Bodencharakterisierung!$E$8","v":1.2913475694139079E-8},{"$f":"IF(AF4243<=$J$9*1.05,(AV4243*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4242,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,26.50817663999868,null,0.17904096454207141,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,86.125970078691353]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4242,5.7533073615091443E-18,{"$f":"Z4259*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.694266657395993E-18},{"$f":"AF4258*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4259^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4259)*3600*24","v":0},0,{"$f":"AE4258-AD4259*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4259>$J$18,(AE4259/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.694266657395993E-18,{"$error":"#N/A"},null,{"$f":"(AD4259)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4259>0,(AJ4259*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4258,NA())","v":{"$error":"#N/A"}},null,4242,{"$f":"IF(AF4259<=$J$9*0.05,AS4258*EXP((-$J$6*1)/Heterogenität!$D$4),Z4259)","v":8.5473232461709021E-5},{"$f":"IF(OR(AF4259>=$J$19, AR4258/$J$5<AN4259),0, Bodencharakterisierung!$E$8*$J$11*((AR4258/$J$5)-AN4259))","v":8.770770936512479E-7},8.770770936512479E-7,{"$f":"AQ4258-AP4259*Bodencharakterisierung!$E$8","v":2.6676834973887704E-4},{"$f":"AQ4259/(Bodencharakterisierung!$E$11*1000)","v":1.7608471929958879E-7},8.6350309555360266E-5,{"$error":"#N/A"},null,{"$f":"(AP4259)*$G$11*Bodencharakterisierung!$E$8","v":1.2683323344726932E-8},{"$f":"IF(AF4259<=$J$9*1.05,(AV4259*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4258,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,26.608538879998662,null,0.1760847192995888,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,85.473232461709017]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4245,5.5779966668610274E-18,{"$f":"Z4262*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.5207550091398414E-18},{"$f":"AF4261*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4262^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4262)*3600*24","v":0},0,{"$f":"AE4261-AD4262*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4262>$J$18,(AE4262/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.5207550091398414E-18,{"$error":"#N/A"},null,{"$f":"(AD4262)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4262>0,(AJ4262*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4261,NA())","v":{"$error":"#N/A"}},null,4245,{"$f":"IF(AF4262<=$J$9*0.05,AS4261*EXP((-$J$6*1)/Heterogenität!$D$4),Z4262)","v":8.4645802709736124E-5},{"$f":"IF(OR(AF4262>=$J$19, AR4261/$J$5<AN4262),0, Bodencharakterisierung!$E$8*$J$11*((AR4261/$J$5)-AN4262))","v":7.0892755264737807E-6},8.7764554996992369E-7,{"$f":"AQ4261-AP4262*Bodencharakterisierung!$E$8","v":2.6616954472675011E-4},{"$f":"AQ4262/(Bodencharakterisierung!$E$11*1000)","v":1.7568946846650171E-7},8.5523448259706048E-5,{"$error":"#N/A"},null,{"$f":"(AP4262)*$G$11*Bodencharakterisierung!$E$8","v":1.2691543734187913E-8},{"$f":"IF(AF4262<=$J$9*1.05,(AV4262*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4261,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,26.627356799998658,null,0.17568946846650171,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,84.645802709736131]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4257,4.9285702076131766E-18,{"$f":"Z4274*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.8779929940133362E-18},{"$f":"AF4273*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4274^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4274)*3600*24","v":0},0,{"$f":"AE4273-AD4274*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4274>$J$18,(AE4274/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.8779929940133362E-18,{"$error":"#N/A"},null,{"$f":"(AD4274)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4274>0,(AJ4274*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4273,NA())","v":{"$error":"#N/A"}},null,4257,{"$f":"IF(AF4274<=$J$9*0.05,AS4273*EXP((-$J$6*1)/Heterogenität!$D$4),Z4274)","v":8.4029859099979298E-5},{"$f":"IF(OR(AF4274>=$J$19, AR4273/$J$5<AN4274),0, Bodencharakterisierung!$E$8*$J$11*((AR4273/$J$5)-AN4274))","v":2.8856052232811806E-6},8.7125917107302932E-7,{"$f":"AQ4273-AP4274*Bodencharakterisierung!$E$8","v":2.6290668441137304E-4},{"$f":"AQ4274/(Bodencharakterisierung!$E$11*1000)","v":1.73535765288035E-7},8.4901118271052327E-5,{"$error":"#N/A"},null,{"$f":"(AP4274)*$G$11*Bodencharakterisierung!$E$8","v":1.2599190953414618E-8},{"$f":"IF(AF4274<=$J$9*1.05,(AV4274*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4273,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,26.702628479998644,null,0.17353576528803499,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,84.029859099979305]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4268,4.3999062177469847E-18,{"$f":"Z4285*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.354754178266954E-18},{"$f":"AF4284*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4285^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4285)*3600*24","v":0},0,{"$f":"AE4284-AD4285*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4285>$J$18,(AE4285/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.354754178266954E-18,{"$error":"#N/A"},null,{"$f":"(AD4285)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4285>0,(AJ4285*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4284,NA())","v":{"$error":"#N/A"}},null,4268,{"$f":"IF(AF4285<=$J$9*0.05,AS4284*EXP((-$J$6*1)/Heterogenität!$D$4),Z4285)","v":8.3350411066592976E-5},{"$f":"IF(OR(AF4285>=$J$19, AR4284/$J$5<AN4285),0, Bodencharakterisierung!$E$8*$J$11*((AR4284/$J$5)-AN4285))","v":3.8320619979585472E-7},3.8320619979585472E-7,{"$f":"AQ4284-AP4285*Bodencharakterisierung!$E$8","v":2.6014788727980748E-4},{"$f":"AQ4285/(Bodencharakterisierung!$E$11*1000)","v":1.7171477708238116E-7},8.3733617266388834E-5,{"$error":"#N/A"},null,{"$f":"(AP4285)*$G$11*Bodencharakterisierung!$E$8","v":5.5415061855981716E-9},{"$f":"IF(AF4285<=$J$9*1.05,(AV4285*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4284,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,26.771627519998631,null,0.17171477708238117,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,83.350411066592969]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4275,4.0934076140739056E-18,{"$f":"Z4292*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.0514008773273284E-18},{"$f":"AF4291*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4292^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4292)*3600*24","v":0},0,{"$f":"AE4291-AD4292*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4292>$J$18,(AE4292/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.0514008773273284E-18,{"$error":"#N/A"},null,{"$f":"(AD4292)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4292>0,(AJ4292*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4291,NA())","v":{"$error":"#N/A"}},null,4275,{"$f":"IF(AF4292<=$J$9*0.05,AS4291*EXP((-$J$6*1)/Heterogenität!$D$4),Z4292)","v":8.22222925260405E-5},{"$f":"IF(OR(AF4292>=$J$19, AR4291/$J$5<AN4292),0, Bodencharakterisierung!$E$8*$J$11*((AR4291/$J$5)-AN4292))","v":6.3658845378457908E-6},8.5251751219443206E-7,{"$f":"AQ4291-AP4292*Bodencharakterisierung!$E$8","v":2.5838259200612455E-4},{"$f":"AQ4292/(Bodencharakterisierung!$E$11*1000)","v":1.7054956568061026E-7},8.3074810038234932E-5,{"$error":"#N/A"},null,{"$f":"(AP4292)*$G$11*Bodencharakterisierung!$E$8","v":1.2328169715607284E-8},{"$f":"IF(AF4292<=$J$9*1.05,(AV4292*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4291,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,26.815535999998623,null,0.17054956568061025,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,82.222292526040505]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4282,3.8082597823046984E-18,{"$f":"Z4299*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.7691792456906968E-18},{"$f":"AF4298*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4299^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4299)*3600*24","v":0},0,{"$f":"AE4298-AD4299*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4299>$J$18,(AE4299/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.7691792456906968E-18,{"$error":"#N/A"},null,{"$f":"(AD4299)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4299>0,(AJ4299*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4298,NA())","v":{"$error":"#N/A"}},null,4282,{"$f":"IF(AF4299<=$J$9*0.05,AS4298*EXP((-$J$6*1)/Heterogenität!$D$4),Z4299)","v":8.22222925260405E-5},{"$f":"IF(OR(AF4299>=$J$19, AR4298/$J$5<AN4299),0, Bodencharakterisierung!$E$8*$J$11*((AR4298/$J$5)-AN4299))","v":1.9948851602765013E-7},1.9948851602765013E-7,{"$f":"AQ4298-AP4299*Bodencharakterisierung!$E$8","v":2.5662877612169047E-4},{"$f":"AQ4299/(Bodencharakterisierung!$E$11*1000)","v":1.6939193143345905E-7},8.2421781042068154E-5,{"$error":"#N/A"},null,{"$f":"(AP4299)*$G$11*Bodencharakterisierung!$E$8","v":2.8847832997272437E-9},{"$f":"IF(AF4299<=$J$9*1.05,(AV4299*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4298,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,26.859444479998615,null,0.16939193143345904,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,82.222292526040505]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4294,3.3648775406100489E-18,{"$f":"Z4311*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.3303470129032808E-18},{"$f":"AF4310*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4311^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4311)*3600*24","v":0},0,{"$f":"AE4310-AD4311*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4311>$J$18,(AE4311/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.3303470129032808E-18,{"$error":"#N/A"},null,{"$f":"(AD4311)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4311>0,(AJ4311*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4310,NA())","v":{"$error":"#N/A"}},null,4294,{"$f":"IF(AF4311<=$J$9*0.05,AS4310*EXP((-$J$6*1)/Heterogenität!$D$4),Z4311)","v":8.0928958801498898E-5},{"$f":"IF(OR(AF4311>=$J$19, AR4310/$J$5<AN4311),0, Bodencharakterisierung!$E$8*$J$11*((AR4310/$J$5)-AN4311))","v":3.7157312852376594E-6},8.3910764954757064E-7,{"$f":"AQ4310-AP4311*Bodencharakterisierung!$E$8","v":2.5350392533882572E-4},{"$f":"AQ4311/(Bodencharakterisierung!$E$11*1000)","v":1.6732932365599058E-7},8.1768066451046468E-5,{"$error":"#N/A"},null,{"$f":"(AP4311)*$G$11*Bodencharakterisierung!$E$8","v":1.2134251045071181E-8},{"$f":"IF(AF4311<=$J$9*1.05,(AV4311*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4310,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,26.934716159998601,null,0.16732932365599057,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,80.928958801498894]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4297,3.2623453826730778E-18,{"$f":"Z4314*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.2288670446753695E-18},{"$f":"AF4313*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4314^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4314)*3600*24","v":0},0,{"$f":"AE4313-AD4314*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4314>$J$18,(AE4314/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.2288670446753695E-18,{"$error":"#N/A"},null,{"$f":"(AD4314)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4314>0,(AJ4314*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4313,NA())","v":{"$error":"#N/A"}},null,4297,{"$f":"IF(AF4314<=$J$9*0.05,AS4313*EXP((-$J$6*1)/Heterogenität!$D$4),Z4314)","v":8.0928958801498898E-5},{"$f":"IF(OR(AF4314>=$J$19, AR4313/$J$5<AN4314),0, Bodencharakterisierung!$E$8*$J$11*((AR4313/$J$5)-AN4314))","v":1.1145597141295527E-6},8.3910764954757064E-7,{"$f":"AQ4313-AP4314*Bodencharakterisierung!$E$8","v":2.5267320876577357E-4},{"$f":"AQ4314/(Bodencharakterisierung!$E$11*1000)","v":1.6678099588499905E-7},8.1768066451046468E-5,{"$error":"#N/A"},null,{"$f":"(AP4314)*$G$11*Bodencharakterisierung!$E$8","v":1.2134251045071181E-8},{"$f":"IF(AF4314<=$J$9*1.05,(AV4314*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4313,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,26.953534079998597,null,0.16678099588499906,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,80.928958801498894]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4309,2.8825220272200522E-18,{"$f":"Z4326*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.8529414539228004E-18},{"$f":"AF4325*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4326^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4326)*3600*24","v":0},0,{"$f":"AE4325-AD4326*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4326>$J$18,(AE4326/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.8529414539228004E-18,{"$error":"#N/A"},null,{"$f":"(AD4326)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4326>0,(AJ4326*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4325,NA())","v":{"$error":"#N/A"}},null,4309,{"$f":"IF(AF4326<=$J$9*0.05,AS4325*EXP((-$J$6*1)/Heterogenität!$D$4),Z4326)","v":8.0062873950755942E-5},{"$f":"IF(OR(AF4326>=$J$19, AR4325/$J$5<AN4326),0, Bodencharakterisierung!$E$8*$J$11*((AR4325/$J$5)-AN4326))","v":1.5023087120698746E-7},1.5023087120698746E-7,{"$f":"AQ4325-AP4326*Bodencharakterisierung!$E$8","v":2.4988935754437192E-4},{"$f":"AQ4326/(Bodencharakterisierung!$E$11*1000)","v":1.649434703263181E-7},8.0213104821962931E-5,{"$error":"#N/A"},null,{"$f":"(AP4326)*$G$11*Bodencharakterisierung!$E$8","v":2.1724734686046923E-9},{"$f":"IF(AF4326<=$J$9*1.05,(AV4326*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4325,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,27.028805759998583,null,0.16494347032631809,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,80.062873950755943]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4315,2.7095301206310682E-18,{"$f":"Z4332*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.6817247982163299E-18},{"$f":"AF4331*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4332^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4332)*3600*24","v":0},0,{"$f":"AE4331-AD4332*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4332>$J$18,(AE4332/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.6817247982163299E-18,{"$error":"#N/A"},null,{"$f":"(AD4332)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4332>0,(AJ4332*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4331,NA())","v":{"$error":"#N/A"}},null,4315,{"$f":"IF(AF4332<=$J$9*0.05,AS4331*EXP((-$J$6*1)/Heterogenität!$D$4),Z4332)","v":7.93899542599967E-5},{"$f":"IF(OR(AF4332>=$J$19, AR4331/$J$5<AN4332),0, Bodencharakterisierung!$E$8*$J$11*((AR4331/$J$5)-AN4332))","v":2.3187120793422524E-6},8.2315056196623053E-7,{"$f":"AQ4331-AP4332*Bodencharakterisierung!$E$8","v":2.4825951943167879E-4},{"$f":"AQ4332/(Bodencharakterisierung!$E$11*1000)","v":1.638676695918672E-7},8.0213104821962931E-5,{"$error":"#N/A"},null,{"$f":"(AP4332)*$G$11*Bodencharakterisierung!$E$8","v":1.1903497211800124E-8},{"$f":"IF(AF4332<=$J$9*1.05,(AV4332*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4331,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,27.066441599998576,null,0.16386766959186719,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,79.389954259996699]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4327,2.3940690944671607E-18,{"$f":"Z4344*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3695010475766853E-18},{"$f":"AF4343*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4344^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4344)*3600*24","v":0},0,{"$f":"AE4343-AD4344*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4344>$J$18,(AE4344/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.3695010475766853E-18,{"$error":"#N/A"},null,{"$f":"(AD4344)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4344>0,(AJ4344*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4343,NA())","v":{"$error":"#N/A"}},null,4327,{"$f":"IF(AF4344<=$J$9*0.05,AS4343*EXP((-$J$6*1)/Heterogenität!$D$4),Z4344)","v":7.8642250582010759E-5},{"$f":"IF(OR(AF4344>=$J$19, AR4343/$J$5<AN4344),0, Bodencharakterisierung!$E$8*$J$11*((AR4343/$J$5)-AN4344))","v":2.5454829568927377E-7},2.5454829568927377E-7,{"$f":"AQ4343-AP4344*Bodencharakterisierung!$E$8","v":2.4545422103417814E-4},{"$f":"AQ4344/(Bodencharakterisierung!$E$11*1000)","v":1.6201598748130571E-7},7.8896798877700034E-5,{"$error":"#N/A"},null,{"$f":"(AP4344)*$G$11*Bodencharakterisierung!$E$8","v":3.6809972172867798E-9},{"$f":"IF(AF4344<=$J$9*1.05,(AV4344*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4343,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,27.141713279998562,null,0.16201598748130572,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,78.64225058201076]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4334,2.2272976229318431E-18,{"$f":"Z4351*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.2044409925339585E-18},{"$f":"AF4350*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4351^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4351)*3600*24","v":0},0,{"$f":"AE4350-AD4351*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4351>$J$18,(AE4351/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.2044409925339585E-18,{"$error":"#N/A"},null,{"$f":"(AD4351)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4351>0,(AJ4351*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4350,NA())","v":{"$error":"#N/A"}},null,4334,{"$f":"IF(AF4351<=$J$9*0.05,AS4350*EXP((-$J$6*1)/Heterogenität!$D$4),Z4351)","v":7.8087156307727693E-5},{"$f":"IF(OR(AF4351>=$J$19, AR4350/$J$5<AN4351),0, Bodencharakterisierung!$E$8*$J$11*((AR4350/$J$5)-AN4351))","v":3.9688844955805505E-7},3.9688844955805505E-7,{"$f":"AQ4350-AP4351*Bodencharakterisierung!$E$8","v":2.4372015555727871E-4},{"$f":"AQ4351/(Bodencharakterisierung!$E$11*1000)","v":1.6087138980678463E-7},7.8484044757285744E-5,{"$error":"#N/A"},null,{"$f":"(AP4351)*$G$11*Bodencharakterisierung!$E$8","v":5.7393638187223856E-9},{"$f":"IF(AF4351<=$J$9*1.05,(AV4351*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4350,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,27.185621759998554,null,0.16087138980678464,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,78.087156307727696]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4340,2.093628405942829E-18,{"$f":"Z4357*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.0721434951826058E-18},{"$f":"AF4356*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4357^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4357)*3600*24","v":0},0,{"$f":"AE4356-AD4357*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4357>$J$18,(AE4357/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.0721434951826058E-18,{"$error":"#N/A"},null,{"$f":"(AD4357)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4357>0,(AJ4357*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4356,NA())","v":{"$error":"#N/A"}},null,4340,{"$f":"IF(AF4357<=$J$9*0.05,AS4356*EXP((-$J$6*1)/Heterogenität!$D$4),Z4357)","v":7.7525186982794564E-5},{"$f":"IF(OR(AF4357>=$J$19, AR4356/$J$5<AN4357),0, Bodencharakterisierung!$E$8*$J$11*((AR4356/$J$5)-AN4357))","v":1.4780391320338711E-6},8.0381582060665266E-7,{"$f":"AQ4356-AP4357*Bodencharakterisierung!$E$8","v":2.4217713884864631E-4},{"$f":"AQ4357/(Bodencharakterisierung!$E$11*1000)","v":1.5985289692979954E-7},7.8329002803401217E-5,{"$error":"#N/A"},null,{"$f":"(AP4357)*$G$11*Bodencharakterisierung!$E$8","v":1.1623899468083762E-8},{"$f":"IF(AF4357<=$J$9*1.05,(AV4357*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4356,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,27.223257599998547,null,0.15985289692979954,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,77.525186982794565]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4352,1.8498746420279235E-18,{"$f":"Z4369*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.8308911435767398E-18},{"$f":"AF4368*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4369^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4369)*3600*24","v":0},0,{"$f":"AE4368-AD4369*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4369>$J$18,(AE4369/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.8308911435767398E-18,{"$error":"#N/A"},null,{"$f":"(AD4369)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4369>0,(AJ4369*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4368,NA())","v":{"$error":"#N/A"}},null,4352,{"$f":"IF(AF4369<=$J$9*0.05,AS4368*EXP((-$J$6*1)/Heterogenität!$D$4),Z4369)","v":7.6503064994410593E-5},{"$f":"IF(OR(AF4369>=$J$19, AR4368/$J$5<AN4369),0, Bodencharakterisierung!$E$8*$J$11*((AR4368/$J$5)-AN4369))","v":2.6240160975537262E-6},7.9321800257063017E-7,{"$f":"AQ4368-AP4369*Bodencharakterisierung!$E$8","v":2.393563874352814E-4},{"$f":"AQ4369/(Bodencharakterisierung!$E$11*1000)","v":1.5799101480876659E-7},7.7296282996981223E-5,{"$error":"#N/A"},null,{"$f":"(AP4369)*$G$11*Bodencharakterisierung!$E$8","v":1.1470645490899291E-8},{"$f":"IF(AF4369<=$J$9*1.05,(AV4369*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4368,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,27.298529279998533,null,0.15799101480876659,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,76.503064994410593]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4364,1.6345002682923019E-18,{"$f":"Z4381*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.6177269515460541E-18},{"$f":"AF4380*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4381^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4381)*3600*24","v":0},0,{"$f":"AE4380-AD4381*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4381>$J$18,(AE4381/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.6177269515460541E-18,{"$error":"#N/A"},null,{"$f":"(AD4381)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4381>0,(AJ4381*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4380,NA())","v":{"$error":"#N/A"}},null,4364,{"$f":"IF(AF4381<=$J$9*0.05,AS4380*EXP((-$J$6*1)/Heterogenität!$D$4),Z4381)","v":7.5478169578475649E-5},{"$f":"IF(OR(AF4381>=$J$19, AR4380/$J$5<AN4381),0, Bodencharakterisierung!$E$8*$J$11*((AR4380/$J$5)-AN4381))","v":3.9281234528504046E-6},7.8259142839701341E-7,{"$f":"AQ4380-AP4381*Bodencharakterisierung!$E$8","v":2.3657749004550642E-4},{"$f":"AQ4381/(Bodencharakterisierung!$E$11*1000)","v":1.5615675910594483E-7},7.6260761006872663E-5,{"$error":"#N/A"},null,{"$f":"(AP4381)*$G$11*Bodencharakterisierung!$E$8","v":1.1316975674110873E-8},{"$f":"IF(AF4381<=$J$9*1.05,(AV4381*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4380,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,27.373800959998519,null,0.15615675910594484,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,75.478169578475644]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4367,1.5846949373006175E-18,{"$f":"Z4384*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.5684327251461409E-18},{"$f":"AF4383*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4384^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4384)*3600*24","v":0},0,{"$f":"AE4383-AD4384*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4384>$J$18,(AE4384/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.5684327251461409E-18,{"$error":"#N/A"},null,{"$f":"(AD4384)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4384>0,(AJ4384*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4383,NA())","v":{"$error":"#N/A"}},null,4367,{"$f":"IF(AF4384<=$J$9*0.05,AS4383*EXP((-$J$6*1)/Heterogenität!$D$4),Z4384)","v":7.5478169578475649E-5},{"$f":"IF(OR(AF4384>=$J$19, AR4383/$J$5<AN4384),0, Bodencharakterisierung!$E$8*$J$11*((AR4383/$J$5)-AN4384))","v":1.502147981840773E-6},7.8259142839701341E-7,{"$f":"AQ4383-AP4384*Bodencharakterisierung!$E$8","v":2.3580272453139339E-4},{"$f":"AQ4384/(Bodencharakterisierung!$E$11*1000)","v":1.5564536272699234E-7},7.6260761006872663E-5,{"$error":"#N/A"},null,{"$f":"(AP4384)*$G$11*Bodencharakterisierung!$E$8","v":1.1316975674110873E-8},{"$f":"IF(AF4384<=$J$9*1.05,(AV4384*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4383,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,27.392618879998516,null,0.15564536272699234,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,75.478169578475644]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4383,1.343597745796973E-18,{"$f":"Z4400*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.3298096840835644E-18},{"$f":"AF4399*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4400^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4400)*3600*24","v":0},0,{"$f":"AE4399-AD4400*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4400>$J$18,(AE4400/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.3298096840835644E-18,{"$error":"#N/A"},null,{"$f":"(AD4400)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4400>0,(AJ4400*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4399,NA())","v":{"$error":"#N/A"}},null,4383,{"$f":"IF(AF4400<=$J$9*0.05,AS4399*EXP((-$J$6*1)/Heterogenität!$D$4),Z4400)","v":7.3942212661544127E-5},{"$f":"IF(OR(AF4400>=$J$19, AR4399/$J$5<AN4400),0, Bodencharakterisierung!$E$8*$J$11*((AR4399/$J$5)-AN4400))","v":5.3021990974674769E-6},7.6666593995060306E-7,{"$f":"AQ4399-AP4400*Bodencharakterisierung!$E$8","v":2.3222756959844241E-4},{"$f":"AQ4400/(Bodencharakterisierung!$E$11*1000)","v":1.5328552448742072E-7},7.470887860149473E-5,{"$error":"#N/A"},null,{"$f":"(AP4400)*$G$11*Bodencharakterisierung!$E$8","v":1.1086678792741338E-8},{"$f":"IF(AF4400<=$J$9*1.05,(AV4400*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4399,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,27.492981119998497,null,0.15328552448742072,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,73.942212661544133]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4389,1.2629629636377404E-18,{"$f":"Z4406*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.2500023797584801E-18},{"$f":"AF4405*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4406^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4406)*3600*24","v":0},0,{"$f":"AE4405-AD4406*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4406>$J$18,(AE4406/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.2500023797584801E-18,{"$error":"#N/A"},null,{"$f":"(AD4406)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4406>0,(AJ4406*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4405,NA())","v":{"$error":"#N/A"}},null,4389,{"$f":"IF(AF4406<=$J$9*0.05,AS4405*EXP((-$J$6*1)/Heterogenität!$D$4),Z4406)","v":7.3942212661544127E-5},{"$f":"IF(OR(AF4406>=$J$19, AR4405/$J$5<AN4406),0, Bodencharakterisierung!$E$8*$J$11*((AR4405/$J$5)-AN4406))","v":5.4898382500179819E-7},5.4898382500179819E-7,{"$f":"AQ4405-AP4406*Bodencharakterisierung!$E$8","v":2.3078140613527336E-4},{"$f":"AQ4406/(Bodencharakterisierung!$E$11*1000)","v":1.5233096114539496E-7},7.4491196486545921E-5,{"$error":"#N/A"},null,{"$f":"(AP4406)*$G$11*Bodencharakterisierung!$E$8","v":7.9387996949461612E-9},{"$f":"IF(AF4406<=$J$9*1.05,(AV4406*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4405,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,27.53061695999849,null,0.15233096114539496,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,73.942212661544133]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4397,1.1629268910949551E-18,{"$f":"Z4414*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.1509928819819162E-18},{"$f":"AF4413*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4414^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4414)*3600*24","v":0},0,{"$f":"AE4413-AD4414*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4414>$J$18,(AE4414/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.1509928819819162E-18,{"$error":"#N/A"},null,{"$f":"(AD4414)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4414>0,(AJ4414*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4413,NA())","v":{"$error":"#N/A"}},null,4397,{"$f":"IF(AF4414<=$J$9*0.05,AS4413*EXP((-$J$6*1)/Heterogenität!$D$4),Z4414)","v":7.2823923852726149E-5},{"$f":"IF(OR(AF4414>=$J$19, AR4413/$J$5<AN4414),0, Bodencharakterisierung!$E$8*$J$11*((AR4413/$J$5)-AN4414))","v":6.3351637267162018E-6},7.5507102129876164E-7,{"$f":"AQ4413-AP4414*Bodencharakterisierung!$E$8","v":2.2907090099502054E-4},{"$f":"AQ4414/(Bodencharakterisierung!$E$11*1000)","v":1.5120191484819837E-7},7.3578994874024911E-5,{"$error":"#N/A"},null,{"$f":"(AP4414)*$G$11*Bodencharakterisierung!$E$8","v":1.0919005844169744E-8},{"$f":"IF(AF4414<=$J$9*1.05,(AV4414*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4413,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,27.58079807999848,null,0.15120191484819837,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,72.823923852726153]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4404,1.0819171034643008E-18,{"$f":"Z4421*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.0708144205087638E-18},{"$f":"AF4420*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4421^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4421)*3600*24","v":0},0,{"$f":"AE4420-AD4421*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4421>$J$18,(AE4421/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.0708144205087638E-18,{"$error":"#N/A"},null,{"$f":"(AD4421)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4421>0,(AJ4421*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4420,NA())","v":{"$error":"#N/A"}},null,4404,{"$f":"IF(AF4421<=$J$9*0.05,AS4420*EXP((-$J$6*1)/Heterogenität!$D$4),Z4421)","v":7.2823923852726149E-5},{"$f":"IF(OR(AF4421>=$J$19, AR4420/$J$5<AN4421),0, Bodencharakterisierung!$E$8*$J$11*((AR4420/$J$5)-AN4421))","v":8.736138168008196E-7},7.5507102129876164E-7,{"$f":"AQ4420-AP4421*Bodencharakterisierung!$E$8","v":2.273266869358204E-4},{"$f":"AQ4421/(Bodencharakterisierung!$E$11*1000)","v":1.5005061843948542E-7},7.3578994874024911E-5,{"$error":"#N/A"},null,{"$f":"(AP4421)*$G$11*Bodencharakterisierung!$E$8","v":1.0919005844169744E-8},{"$f":"IF(AF4421<=$J$9*1.05,(AV4421*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4420,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,27.624706559998472,null,0.15005061843948542,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,72.823923852726153]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4416,9.5595331473046697E-19,{"$f":"Z4433*EXP((-$J$6/Heterogenität!$D$4)*1)","v":9.4614327795430171E-19},{"$f":"AF4432*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4433^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4433)*3600*24","v":0},0,{"$f":"AE4432-AD4433*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4433>$J$18,(AE4433/(Bodencharakterisierung!$E$11*1000)),0)","v":0},9.4614327795430171E-19,{"$error":"#N/A"},null,{"$f":"(AD4433)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4433>0,(AJ4433*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4432,NA())","v":{"$error":"#N/A"}},null,4416,{"$f":"IF(AF4433<=$J$9*0.05,AS4432*EXP((-$J$6*1)/Heterogenität!$D$4),Z4433)","v":7.1637847422546921E-5},{"$f":"IF(OR(AF4433>=$J$19, AR4432/$J$5<AN4433),0, Bodencharakterisierung!$E$8*$J$11*((AR4432/$J$5)-AN4433))","v":4.4168292466139907E-6},7.4277325026289283E-7,{"$f":"AQ4432-AP4433*Bodencharakterisierung!$E$8","v":2.2476035253054879E-4},{"$f":"AQ4433/(Bodencharakterisierung!$E$11*1000)","v":1.4835666833699589E-7},7.2380620672809814E-5,{"$error":"#N/A"},null,{"$f":"(AP4433)*$G$11*Bodencharakterisierung!$E$8","v":1.0741169018198135E-8},{"$f":"IF(AF4433<=$J$9*1.05,(AV4433*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4432,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,27.699978239998458,null,0.1483566683369959,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,71.637847422546926]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4423,8.8936135989294508E-19,{"$f":"Z4440*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.802346928126493E-19},{"$f":"AF4439*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4440^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4440)*3600*24","v":0},0,{"$f":"AE4439-AD4440*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4440>$J$18,(AE4440/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.802346928126493E-19,{"$error":"#N/A"},null,{"$f":"(AD4440)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4440>0,(AJ4440*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4439,NA())","v":{"$error":"#N/A"}},null,4423,{"$f":"IF(AF4440<=$J$9*0.05,AS4439*EXP((-$J$6*1)/Heterogenität!$D$4),Z4440)","v":7.1476011295526531E-5},{"$f":"IF(OR(AF4440>=$J$19, AR4439/$J$5<AN4440),0, Bodencharakterisierung!$E$8*$J$11*((AR4439/$J$5)-AN4440))","v":7.9657762219506518E-7},7.4109526089830274E-7,{"$f":"AQ4439-AP4440*Bodencharakterisierung!$E$8","v":2.2309961345382917E-4},{"$f":"AQ4440/(Bodencharakterisierung!$E$11*1000)","v":1.4726047092661992E-7},7.2217106556424833E-5,{"$error":"#N/A"},null,{"$f":"(AP4440)*$G$11*Bodencharakterisierung!$E$8","v":1.0716903783324072E-8},{"$f":"IF(AF4440<=$J$9*1.05,(AV4440*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4439,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,27.74388671999845,null,0.14726047092661992,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,71.476011295526533]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4430,{"$f":"AG4446","v":8.2740821783084907E-19},{"$f":"Z4447*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.1891731673688656E-19},{"$f":"AF4446*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4447^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4447)*3600*24","v":0},{"$f":"MIN(AC4447,Z4447-AA4447)","v":0},{"$f":"AE4446-AD4447*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4447>$J$18,(AE4447/(Bodencharakterisierung!$E$11*1000)),0)","v":0},{"$f":"AA4447+AD4447","v":8.1891731673688656E-19},{"$f":"IF(AD4447>0,Y4447,NA())","v":{"$error":"#N/A"}},null,{"$f":"(AD4447)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4447>0,(AJ4447*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4446,NA())","v":{"$error":"#N/A"}},null,4430,{"$f":"IF(AF4447<=$J$9*0.05,AS4446*EXP((-$J$6*1)/Heterogenität!$D$4),Z4447)","v":7.0773002623607869E-5},{"$f":"IF(OR(AF4447>=$J$19, AR4446/$J$5<AN4447),0, Bodencharakterisierung!$E$8*$J$11*((AR4446/$J$5)-AN4447))","v":3.0783567490017717E-6},{"$f":"MIN(AO4447,AS4446-AN4447)","v":7.3380615248716671E-7},{"$f":"AQ4446-AP4447*Bodencharakterisierung!$E$8","v":2.2163651410331701E-4},{"$f":"AQ4447/(Bodencharakterisierung!$E$11*1000)","v":1.4629472878106734E-7},{"$f":"AN4447+AP4447","v":7.1506808776095035E-5},{"$f":"IF(AN4447>$G$5,AM4447,NA())","v":{"$error":"#N/A"}},null,{"$f":"(AP4447)*$G$11*Bodencharakterisierung!$E$8","v":1.0611496722140499E-8},{"$f":"IF(AF4447<=$J$9*1.05,(AV4447*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4446,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH4447>($G$5*10^6),BH4447*0.99,9999)","v":9999},{"$f":"AT4447+$G$3","v":{"$error":"#N/A"}},{"$f":"IF(ISNUMBER(AT4447),BA4447+BB4447+BC4447+$AZ$17,\"\")","v":""},{"$f":"IF(ISNUMBER(AK4447),AK4447,BA4446)","v":1.6399886323194495},{"$f":"IF(ISNUMBER(AW4447),AW4447,0)","v":0},27.787795199998442,null,{"$f":"AR4447*10^6","v":0.14629472878106733},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF4447*10^6","v":0},{"$f":"AN4447*10^6","v":70.773002623607866}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4437,7.6977074764798585E-19,{"$f":"Z4454*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.6187132491752317E-19},{"$f":"AF4453*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4454^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4454)*3600*24","v":0},0,{"$f":"AE4453-AD4454*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4454>$J$18,(AE4454/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.6187132491752317E-19,{"$error":"#N/A"},null,{"$f":"(AD4454)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4454>0,(AJ4454*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4453,NA())","v":{"$error":"#N/A"}},null,4437,{"$f":"IF(AF4454<=$J$9*0.05,AS4453*EXP((-$J$6*1)/Heterogenität!$D$4),Z4454)","v":7.0091625075866898E-5},{"$f":"IF(OR(AF4454>=$J$19, AR4453/$J$5<AN4454),0, Bodencharakterisierung!$E$8*$J$11*((AR4453/$J$5)-AN4454))","v":5.1558119181378513E-6},7.267413252484814E-7,{"$f":"AQ4453-AP4454*Bodencharakterisierung!$E$8","v":2.2017560205378126E-4},{"$f":"AQ4454/(Bodencharakterisierung!$E$11*1000)","v":1.4533043039853548E-7},7.0818366401115379E-5,{"$error":"#N/A"},null,{"$f":"(AP4454)*$G$11*Bodencharakterisierung!$E$8","v":1.0509332968359341E-8},{"$f":"IF(AF4454<=$J$9*1.05,(AV4454*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4453,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,27.831703679998434,null,0.14533043039853547,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,70.091625075866901]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4453,6.5265699850221969E-19,{"$f":"Z4470*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.4595940243882442E-19},{"$f":"AF4469*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4470^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4470)*3600*24","v":0},0,{"$f":"AE4469-AD4470*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4470>$J$18,(AE4470/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.4595940243882442E-19,{"$error":"#N/A"},null,{"$f":"(AD4470)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4470>0,(AJ4470*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4469,NA())","v":{"$error":"#N/A"}},null,4453,{"$f":"IF(AF4470<=$J$9*0.05,AS4469*EXP((-$J$6*1)/Heterogenität!$D$4),Z4470)","v":6.9329374229142032E-5},{"$f":"IF(OR(AF4470>=$J$19, AR4469/$J$5<AN4470),0, Bodencharakterisierung!$E$8*$J$11*((AR4469/$J$5)-AN4470))","v":1.444917063778115E-6},7.1883796746612983E-7,{"$f":"AQ4469-AP4470*Bodencharakterisierung!$E$8","v":2.1661396452803673E-4},{"$f":"AQ4470/(Bodencharakterisierung!$E$11*1000)","v":1.4297951453995824E-7},7.0048212196608162E-5,{"$error":"#N/A"},null,{"$f":"(AP4470)*$G$11*Bodencharakterisierung!$E$8","v":1.0395043309003026E-8},{"$f":"IF(AF4470<=$J$9*1.05,(AV4470*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4469,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,27.932065919998415,null,0.14297951453995825,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,69.329374229142033]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4456,6.3276969810525879E-19,{"$f":"Z4473*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.2627618643099271E-19},{"$f":"AF4472*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4473^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4473)*3600*24","v":0},0,{"$f":"AE4472-AD4473*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4473>$J$18,(AE4473/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.2627618643099271E-19,{"$error":"#N/A"},null,{"$f":"(AD4473)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4473>0,(AJ4473*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4472,NA())","v":{"$error":"#N/A"}},null,4456,{"$f":"IF(AF4473<=$J$9*0.05,AS4472*EXP((-$J$6*1)/Heterogenität!$D$4),Z4473)","v":6.8738306732761808E-5},{"$f":"IF(OR(AF4473>=$J$19, AR4472/$J$5<AN4473),0, Bodencharakterisierung!$E$8*$J$11*((AR4472/$J$5)-AN4473))","v":5.6104410117965967E-6},7.1270951524140256E-7,{"$f":"AQ4472-AP4473*Bodencharakterisierung!$E$8","v":2.1610146855475281E-4},{"$f":"AQ4473/(Bodencharakterisierung!$E$11*1000)","v":1.426412333694738E-7},6.945101624800321E-5,{"$error":"#N/A"},null,{"$f":"(AP4473)*$G$11*Bodencharakterisierung!$E$8","v":1.0306420379808347E-8},{"$f":"IF(AF4473<=$J$9*1.05,(AV4473*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4472,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,27.950883839998411,null,0.14264123336947379,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,68.738306732761814]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4469,5.5336106106323143E-19,{"$f":"Z4486*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.4768244446566383E-19},{"$f":"AF4485*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4486^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4486)*3600*24","v":0},0,{"$f":"AE4485-AD4486*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4486>$J$18,(AE4486/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.4768244446566383E-19,{"$error":"#N/A"},null,{"$f":"(AD4486)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4486>0,(AJ4486*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4485,NA())","v":{"$error":"#N/A"}},null,4469,{"$f":"IF(AF4486<=$J$9*0.05,AS4485*EXP((-$J$6*1)/Heterogenität!$D$4),Z4486)","v":6.8051528959232253E-5},{"$f":"IF(OR(AF4486>=$J$19, AR4485/$J$5<AN4486),0, Bodencharakterisierung!$E$8*$J$11*((AR4485/$J$5)-AN4486))","v":3.4838893041143613E-6},7.0558869604587799E-7,{"$f":"AQ4485-AP4486*Bodencharakterisierung!$E$8","v":2.1328111787227377E-4},{"$f":"AQ4486/(Bodencharakterisierung!$E$11*1000)","v":1.4077961575727641E-7},6.8757117655278131E-5,{"$error":"#N/A"},null,{"$f":"(AP4486)*$G$11*Bodencharakterisierung!$E$8","v":1.020344693198953E-8},{"$f":"IF(AF4486<=$J$9*1.05,(AV4486*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4485,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,28.032428159998396,null,0.14077961575727641,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,68.051528959232257]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4474,5.2554477080964506E-19,{"$f":"Z4491*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.2015160625890798E-19},{"$f":"AF4490*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4491^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4491)*3600*24","v":0},0,{"$f":"AE4490-AD4491*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4491>$J$18,(AE4491/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.2015160625890798E-19,{"$error":"#N/A"},null,{"$f":"(AD4491)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4491>0,(AJ4491*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4490,NA())","v":{"$error":"#N/A"}},null,4474,{"$f":"IF(AF4491<=$J$9*0.05,AS4490*EXP((-$J$6*1)/Heterogenität!$D$4),Z4491)","v":6.7914882771603118E-5},{"$f":"IF(OR(AF4491>=$J$19, AR4490/$J$5<AN4491),0, Bodencharakterisierung!$E$8*$J$11*((AR4490/$J$5)-AN4491))","v":1.3165630099224566E-6},7.0417188724197376E-7,{"$f":"AQ4490-AP4491*Bodencharakterisierung!$E$8","v":2.1216292485952629E-4},{"$f":"AQ4491/(Bodencharakterisierung!$E$11*1000)","v":1.4004153456074342E-7},6.8619054658845092E-5,{"$error":"#N/A"},null,{"$f":"(AP4491)*$G$11*Bodencharakterisierung!$E$8","v":1.0182958602847603E-8},{"$f":"IF(AF4491<=$J$9*1.05,(AV4491*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4490,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,28.06379135999839,null,0.14004153456074342,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,67.914882771603118]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4486,4.6435744853840468E-19,{"$f":"Z4503*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.5959219109617026E-19},{"$f":"AF4502*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4503^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4503)*3600*24","v":0},0,{"$f":"AE4502-AD4503*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4503>$J$18,(AE4503/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.5959219109617026E-19,{"$error":"#N/A"},null,{"$f":"(AD4503)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4503>0,(AJ4503*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4502,NA())","v":{"$error":"#N/A"}},null,4486,{"$f":"IF(AF4503<=$J$9*0.05,AS4502*EXP((-$J$6*1)/Heterogenität!$D$4),Z4503)","v":6.7104544551812795E-5},{"$f":"IF(OR(AF4503>=$J$19, AR4502/$J$5<AN4503),0, Bodencharakterisierung!$E$8*$J$11*((AR4502/$J$5)-AN4503))","v":1.4029512836107679E-6},6.9576993806312701E-7,{"$f":"AQ4502-AP4503*Bodencharakterisierung!$E$8","v":2.0966407204492472E-4},{"$f":"AQ4503/(Bodencharakterisierung!$E$11*1000)","v":1.3839212676232655E-7},6.7800314489875922E-5,{"$error":"#N/A"},null,{"$f":"(AP4503)*$G$11*Bodencharakterisierung!$E$8","v":1.0061458863619831E-8},{"$f":"IF(AF4503<=$J$9*1.05,(AV4503*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4502,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,28.139063039998376,null,0.13839212676232654,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,67.104544551812793]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4493,4.3201018872451394E-19,{"$f":"Z4510*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.2757688034662464E-19},{"$f":"AF4509*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4510^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4510)*3600*24","v":0},0,{"$f":"AE4509-AD4510*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4510>$J$18,(AE4510/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.2757688034662464E-19,{"$error":"#N/A"},null,{"$f":"(AD4510)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4510>0,(AJ4510*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4509,NA())","v":{"$error":"#N/A"}},null,4493,{"$f":"IF(AF4510<=$J$9*0.05,AS4509*EXP((-$J$6*1)/Heterogenität!$D$4),Z4510)","v":6.6494463161512876E-5},{"$f":"IF(OR(AF4510>=$J$19, AR4509/$J$5<AN4510),0, Bodencharakterisierung!$E$8*$J$11*((AR4509/$J$5)-AN4510))","v":2.9959738107516133E-6},6.8944434128011245E-7,{"$f":"AQ4509-AP4510*Bodencharakterisierung!$E$8","v":2.0827073486606851E-4},{"$f":"AQ4510/(Bodencharakterisierung!$E$11*1000)","v":1.3747243225483069E-7},6.7183907502792989E-5,{"$error":"#N/A"},null,{"$f":"(AP4510)*$G$11*Bodencharakterisierung!$E$8","v":9.9699850468617829E-9},{"$f":"IF(AF4510<=$J$9*1.05,(AV4510*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4509,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,28.182971519998368,null,0.13747243225483069,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,66.494463161512883]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4505,3.8171276762902252E-19,{"$f":"Z4522*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.777956136941273E-19},{"$f":"AF4521*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4522^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4522)*3600*24","v":0},0,{"$f":"AE4521-AD4522*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4522>$J$18,(AE4522/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.777956136941273E-19,{"$error":"#N/A"},null,{"$f":"(AD4522)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4522>0,(AJ4522*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4521,NA())","v":{"$error":"#N/A"}},null,4505,{"$f":"IF(AF4522<=$J$9*0.05,AS4521*EXP((-$J$6*1)/Heterogenität!$D$4),Z4522)","v":6.5956930807941158E-5},{"$f":"IF(OR(AF4522>=$J$19, AR4521/$J$5<AN4522),0, Bodencharakterisierung!$E$8*$J$11*((AR4521/$J$5)-AN4522))","v":3.0197265564860573E-7},3.0197265564860573E-7,{"$f":"AQ4521-AP4522*Bodencharakterisierung!$E$8","v":2.0586050031995028E-4},{"$f":"AQ4522/(Bodencharakterisierung!$E$11*1000)","v":1.3588151836300348E-7},6.6258903463589763E-5,{"$error":"#N/A"},null,{"$f":"(AP4522)*$G$11*Bodencharakterisierung!$E$8","v":4.3667961010278958E-9},{"$f":"IF(AF4522<=$J$9*1.05,(AV4522*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4521,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,28.258243199998354,null,0.1358815183630035,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,65.956930807941163]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4510,3.6252487407274758E-19,{"$f":"Z4527*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.588046271818928E-19},{"$f":"AF4526*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4527^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4527)*3600*24","v":0},0,{"$f":"AE4526-AD4527*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4527>$J$18,(AE4527/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.588046271818928E-19,{"$error":"#N/A"},null,{"$f":"(AD4527)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4527>0,(AJ4527*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4526,NA())","v":{"$error":"#N/A"}},null,4510,{"$f":"IF(AF4527<=$J$9*0.05,AS4526*EXP((-$J$6*1)/Heterogenität!$D$4),Z4527)","v":6.5578951556200359E-5},{"$f":"IF(OR(AF4527>=$J$19, AR4526/$J$5<AN4527),0, Bodencharakterisierung!$E$8*$J$11*((AR4526/$J$5)-AN4527))","v":8.7359672171385624E-7},6.7995190738940432E-7,{"$f":"AQ4526-AP4527*Bodencharakterisierung!$E$8","v":2.0473857967275781E-4},{"$f":"AQ4527/(Bodencharakterisierung!$E$11*1000)","v":1.3514097668168833E-7},6.6258903463589763E-5,{"$error":"#N/A"},null,{"$f":"(AP4527)*$G$11*Bodencharakterisierung!$E$8","v":9.8327159182574857E-9},{"$f":"IF(AF4527<=$J$9*1.05,(AV4527*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4526,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,28.289606399998348,null,0.13514097668168834,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,65.578951556200366]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4523,3.1703027117038051E-19,{"$f":"Z4540*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.1377689198186229E-19},{"$f":"AF4539*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4540^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4540)*3600*24","v":0},0,{"$f":"AE4539-AD4540*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4540>$J$18,(AE4540/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.1377689198186229E-19,{"$error":"#N/A"},null,{"$f":"(AD4540)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4540>0,(AJ4540*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4539,NA())","v":{"$error":"#N/A"}},null,4523,{"$f":"IF(AF4540<=$J$9*0.05,AS4539*EXP((-$J$6*1)/Heterogenität!$D$4),Z4540)","v":6.4443979601846451E-5},{"$f":"IF(OR(AF4540>=$J$19, AR4539/$J$5<AN4540),0, Bodencharakterisierung!$E$8*$J$11*((AR4539/$J$5)-AN4540))","v":4.0966599568229019E-6},6.6818401042119987E-7,{"$f":"AQ4539-AP4540*Bodencharakterisierung!$E$8","v":2.0222933228269561E-4},{"$f":"AQ4540/(Bodencharakterisierung!$E$11*1000)","v":1.3348470777735684E-7},6.5112163612267651E-5,{"$error":"#N/A"},null,{"$f":"(AP4540)*$G$11*Bodencharakterisierung!$E$8","v":9.6625415477083479E-9},{"$f":"IF(AF4540<=$J$9*1.05,(AV4540*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4539,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,28.371150719998333,null,0.13348470777735685,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,64.443979601846451]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4526,3.0736994997231725E-19,{"$f":"Z4543*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.0421570544316185E-19},{"$f":"AF4542*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4543^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4543)*3600*24","v":0},0,{"$f":"AE4542-AD4543*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4543>$J$18,(AE4543/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.0421570544316185E-19,{"$error":"#N/A"},null,{"$f":"(AD4543)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4543>0,(AJ4543*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4542,NA())","v":{"$error":"#N/A"}},null,4526,{"$f":"IF(AF4543<=$J$9*0.05,AS4542*EXP((-$J$6*1)/Heterogenität!$D$4),Z4543)","v":6.4443979601846451E-5},{"$f":"IF(OR(AF4543>=$J$19, AR4542/$J$5<AN4543),0, Bodencharakterisierung!$E$8*$J$11*((AR4542/$J$5)-AN4543))","v":2.0253390087734312E-6},6.6818401042119987E-7,{"$f":"AQ4542-AP4543*Bodencharakterisierung!$E$8","v":2.0156783011237862E-4},{"$f":"AQ4543/(Bodencharakterisierung!$E$11*1000)","v":1.3304807268143804E-7},6.5112163612267651E-5,{"$error":"#N/A"},null,{"$f":"(AP4543)*$G$11*Bodencharakterisierung!$E$8","v":9.6625415477083479E-9},{"$f":"IF(AF4543<=$J$9*1.05,(AV4543*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4542,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,28.38996863999833,null,0.13304807268143803,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,64.443979601846451]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4533,2.8595847986016105E-19,{"$f":"Z4550*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.8302396081968316E-19},{"$f":"AF4549*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4550^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4550)*3600*24","v":0},0,{"$f":"AE4549-AD4550*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4550>$J$18,(AE4550/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.8302396081968316E-19,{"$error":"#N/A"},null,{"$f":"(AD4550)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4550>0,(AJ4550*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4549,NA())","v":{"$error":"#N/A"}},null,4533,{"$f":"IF(AF4550<=$J$9*0.05,AS4549*EXP((-$J$6*1)/Heterogenität!$D$4),Z4550)","v":6.3965305660522868E-5},{"$f":"IF(OR(AF4550>=$J$19, AR4549/$J$5<AN4550),0, Bodencharakterisierung!$E$8*$J$11*((AR4549/$J$5)-AN4550))","v":2.3858021420958321E-6},6.6322090485612445E-7,{"$f":"AQ4549-AP4550*Bodencharakterisierung!$E$8","v":2.0019055691939346E-4},{"$f":"AQ4550/(Bodencharakterisierung!$E$11*1000)","v":1.3213898146494618E-7},6.4628526565378992E-5,{"$error":"#N/A"},null,{"$f":"(AP4550)*$G$11*Bodencharakterisierung!$E$8","v":9.5907705789628161E-9},{"$f":"IF(AF4550<=$J$9*1.05,(AV4550*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4549,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,28.433877119998321,null,0.13213898146494618,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,63.965305660522866]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4549,2.4245244929356146E-19,{"$f":"Z4566*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3996439113487219E-19},{"$f":"AF4565*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4566^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4566)*3600*24","v":0},0,{"$f":"AE4565-AD4566*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4566>$J$18,(AE4566/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.3996439113487219E-19,{"$error":"#N/A"},null,{"$f":"(AD4566)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4566>0,(AJ4566*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4565,NA())","v":{"$error":"#N/A"}},null,4549,{"$f":"IF(AF4566<=$J$9*0.05,AS4565*EXP((-$J$6*1)/Heterogenität!$D$4),Z4566)","v":6.3110580292801845E-5},{"$f":"IF(OR(AF4566>=$J$19, AR4565/$J$5<AN4566),0, Bodencharakterisierung!$E$8*$J$11*((AR4565/$J$5)-AN4566))","v":7.3696552647589623E-7},6.5435872987032353E-7,{"$f":"AQ4565-AP4566*Bodencharakterisierung!$E$8","v":1.9699914982299302E-4},{"$f":"AQ4566/(Bodencharakterisierung!$E$11*1000)","v":1.3003244212738814E-7},6.3764939022672168E-5,{"$error":"#N/A"},null,{"$f":"(AP4566)*$G$11*Bodencharakterisierung!$E$8","v":9.462615560782444E-9},{"$f":"IF(AF4566<=$J$9*1.05,(AV4566*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4565,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,28.534239359998303,null,0.13003244212738815,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,63.110580292801842]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4556,2.2556314904760148E-19,{"$f":"Z4573*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.2324840966293964E-19},{"$f":"AF4572*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4573^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4573)*3600*24","v":0},0,{"$f":"AE4572-AD4573*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4573>$J$18,(AE4573/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.2324840966293964E-19,{"$error":"#N/A"},null,{"$f":"(AD4573)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4573>0,(AJ4573*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4572,NA())","v":{"$error":"#N/A"}},null,4556,{"$f":"IF(AF4573<=$J$9*0.05,AS4572*EXP((-$J$6*1)/Heterogenität!$D$4),Z4573)","v":6.2523123569451435E-5},{"$f":"IF(OR(AF4573>=$J$19, AR4572/$J$5<AN4573),0, Bodencharakterisierung!$E$8*$J$11*((AR4572/$J$5)-AN4573))","v":2.3899861480527021E-6},6.4826771575570341E-7,{"$f":"AQ4572-AP4573*Bodencharakterisierung!$E$8","v":1.9569551211830297E-4},{"$f":"AQ4573/(Bodencharakterisierung!$E$11*1000)","v":1.2917195519359932E-7},6.3171391285207139E-5,{"$error":"#N/A"},null,{"$f":"(AP4573)*$G$11*Bodencharakterisierung!$E$8","v":9.3745340203201168E-9},{"$f":"IF(AF4573<=$J$9*1.05,(AV4573*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4572,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,28.578147839998294,null,0.12917195519359931,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,62.523123569451435]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4563,2.0985036181946966E-19,{"$f":"Z4580*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.0769686777826636E-19},{"$f":"AF4579*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4580^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4580)*3600*24","v":0},0,{"$f":"AE4579-AD4580*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4580>$J$18,(AE4580/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.0769686777826636E-19,{"$error":"#N/A"},null,{"$f":"(AD4580)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4580>0,(AJ4580*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4579,NA())","v":{"$error":"#N/A"}},null,4563,{"$f":"IF(AF4580<=$J$9*0.05,AS4579*EXP((-$J$6*1)/Heterogenität!$D$4),Z4580)","v":6.2258008919497911E-5},{"$f":"IF(OR(AF4580>=$J$19, AR4579/$J$5<AN4580),0, Bodencharakterisierung!$E$8*$J$11*((AR4579/$J$5)-AN4580))","v":5.7727924181103843E-7},5.7727924181103843E-7,{"$f":"AQ4579-AP4580*Bodencharakterisierung!$E$8","v":1.9431255617782101E-4},{"$f":"AQ4580/(Bodencharakterisierung!$E$11*1000)","v":1.2825911298866074E-7},6.2835288161308946E-5,{"$error":"#N/A"},null,{"$f":"(AP4580)*$G$11*Bodencharakterisierung!$E$8","v":8.3479768621110307E-9},{"$f":"IF(AF4580<=$J$9*1.05,(AV4580*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4579,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,28.622056319998286,null,0.12825911298866075,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,62.258008919497911]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4575,1.8541822505288563E-19,{"$f":"Z4592*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.8351545472015975E-19},{"$f":"AF4591*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4592^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4592)*3600*24","v":0},0,{"$f":"AE4591-AD4592*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4592>$J$18,(AE4592/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.8351545472015975E-19,{"$error":"#N/A"},null,{"$f":"(AD4592)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4592>0,(AJ4592*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4591,NA())","v":{"$error":"#N/A"}},null,4575,{"$f":"IF(AF4592<=$J$9*0.05,AS4591*EXP((-$J$6*1)/Heterogenität!$D$4),Z4592)","v":6.1565287465056504E-5},{"$f":"IF(OR(AF4592>=$J$19, AR4591/$J$5<AN4592),0, Bodencharakterisierung!$E$8*$J$11*((AR4591/$J$5)-AN4592))","v":1.3462254368340319E-7},1.3462254368340319E-7,{"$f":"AQ4591-AP4592*Bodencharakterisierung!$E$8","v":1.9215515388040829E-4},{"$f":"AQ4592/(Bodencharakterisierung!$E$11*1000)","v":1.2683508506957643E-7},6.1699910008739905E-5,{"$error":"#N/A"},null,{"$f":"(AP4592)*$G$11*Bodencharakterisierung!$E$8","v":1.9467630193351811E-9},{"$f":"IF(AF4592<=$J$9*1.05,(AV4592*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4591,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,28.697327999998272,null,0.12683508506957641,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,61.565287465056507]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4578,1.7976829262412077E-19,{"$f":"Z4595*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.7792350215720524E-19},{"$f":"AF4594*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4595^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4595)*3600*24","v":0},0,{"$f":"AE4594-AD4595*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4595>$J$18,(AE4595/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.7792350215720524E-19,{"$error":"#N/A"},null,{"$f":"(AD4595)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4595>0,(AJ4595*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4594,NA())","v":{"$error":"#N/A"}},null,4578,{"$f":"IF(AF4595<=$J$9*0.05,AS4594*EXP((-$J$6*1)/Heterogenität!$D$4),Z4595)","v":6.106674270135681E-5},{"$f":"IF(OR(AF4595>=$J$19, AR4594/$J$5<AN4595),0, Bodencharakterisierung!$E$8*$J$11*((AR4594/$J$5)-AN4595))","v":3.5593644968348815E-6},6.3316730738309545E-7,{"$f":"AQ4594-AP4595*Bodencharakterisierung!$E$8","v":1.9152831824609899E-4},{"$f":"AQ4595/(Bodencharakterisierung!$E$11*1000)","v":1.264213321756429E-7},6.1699910008739905E-5,{"$error":"#N/A"},null,{"$f":"(AP4595)*$G$11*Bodencharakterisierung!$E$8","v":9.1561685386383378E-9},{"$f":"IF(AF4595<=$J$9*1.05,(AV4595*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4594,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,28.716145919998269,null,0.12642133217564289,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,61.066742701356809]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4590,1.588385049715921E-19,{"$f":"Z4607*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.5720849694585313E-19},{"$f":"AF4606*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4607^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4607)*3600*24","v":0},0,{"$f":"AE4606-AD4607*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4607>$J$18,(AE4607/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.5720849694585313E-19,{"$error":"#N/A"},null,{"$f":"(AD4607)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4607>0,(AJ4607*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4606,NA())","v":{"$error":"#N/A"}},null,4590,{"$f":"IF(AF4607<=$J$9*0.05,AS4606*EXP((-$J$6*1)/Heterogenität!$D$4),Z4607)","v":6.0176675445787641E-5},{"$f":"IF(OR(AF4607>=$J$19, AR4606/$J$5<AN4607),0, Bodencharakterisierung!$E$8*$J$11*((AR4606/$J$5)-AN4607))","v":5.3582625718204334E-6},6.2393869189340454E-7,{"$f":"AQ4606-AP4607*Bodencharakterisierung!$E$8","v":1.8932780060297515E-4},{"$f":"AQ4607/(Bodencharakterisierung!$E$11*1000)","v":1.2496884528249185E-7},6.0800614137681045E-5,{"$error":"#N/A"},null,{"$f":"(AP4607)*$G$11*Bodencharakterisierung!$E$8","v":9.022714461309023E-9},{"$f":"IF(AF4607<=$J$9*1.05,(AV4607*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4606,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,28.791417599998255,null,0.12496884528249184,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,60.176675445787637]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4596,1.4930595827973583E-19,{"$f":"Z4613*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.4777377368551452E-19},{"$f":"AF4612*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4613^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4613)*3600*24","v":0},0,{"$f":"AE4612-AD4613*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4613>$J$18,(AE4613/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.4777377368551452E-19,{"$error":"#N/A"},null,{"$f":"(AD4613)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4613>0,(AJ4613*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4612,NA())","v":{"$error":"#N/A"}},null,4596,{"$f":"IF(AF4613<=$J$9*0.05,AS4612*EXP((-$J$6*1)/Heterogenität!$D$4),Z4613)","v":6.0176675445787641E-5},{"$f":"IF(OR(AF4613>=$J$19, AR4612/$J$5<AN4613),0, Bodencharakterisierung!$E$8*$J$11*((AR4612/$J$5)-AN4613))","v":1.4899350971696805E-6},6.2393869189340454E-7,{"$f":"AQ4612-AP4613*Bodencharakterisierung!$E$8","v":1.8809240199302624E-4},{"$f":"AQ4613/(Bodencharakterisierung!$E$11*1000)","v":1.2415340065546288E-7},6.0800614137681045E-5,{"$error":"#N/A"},null,{"$f":"(AP4613)*$G$11*Bodencharakterisierung!$E$8","v":9.022714461309023E-9},{"$f":"IF(AF4613<=$J$9*1.05,(AV4613*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4612,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,28.829053439998248,null,0.12415340065546288,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,60.176675445787637]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4603,1.3890526665857599E-19,{"$f":"Z4620*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.3747981443896849E-19},{"$f":"AF4619*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4620^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4620)*3600*24","v":0},0,{"$f":"AE4619-AD4620*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4620>$J$18,(AE4620/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.3747981443896849E-19,{"$error":"#N/A"},null,{"$f":"(AD4620)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4620>0,(AJ4620*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4619,NA())","v":{"$error":"#N/A"}},null,4603,{"$f":"IF(AF4620<=$J$9*0.05,AS4619*EXP((-$J$6*1)/Heterogenität!$D$4),Z4620)","v":5.9757574782679254E-5},{"$f":"IF(OR(AF4620>=$J$19, AR4619/$J$5<AN4620),0, Bodencharakterisierung!$E$8*$J$11*((AR4619/$J$5)-AN4620))","v":1.5283398725781079E-6},6.1959326872779326E-7,{"$f":"AQ4619-AP4620*Bodencharakterisierung!$E$8","v":1.8679801077144614E-4},{"$f":"AQ4620/(Bodencharakterisierung!$E$11*1000)","v":1.2329901701085553E-7},6.0377168051407047E-5,{"$error":"#N/A"},null,{"$f":"(AP4620)*$G$11*Bodencharakterisierung!$E$8","v":8.9598757354113081E-9},{"$f":"IF(AF4620<=$J$9*1.05,(AV4620*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4619,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,28.872961919998239,null,0.12329901701085552,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,59.757574782679256]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4615,1.227330168555438E-19,{"$f":"Z4632*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.2147352500541921E-19},{"$f":"AF4631*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4632^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4632)*3600*24","v":0},0,{"$f":"AE4631-AD4632*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4632>$J$18,(AE4632/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.2147352500541921E-19,{"$error":"#N/A"},null,{"$f":"(AD4632)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4632>0,(AJ4632*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4631,NA())","v":{"$error":"#N/A"}},null,4615,{"$f":"IF(AF4632<=$J$9*0.05,AS4631*EXP((-$J$6*1)/Heterogenität!$D$4),Z4632)","v":5.9181904815057292E-5},{"$f":"IF(OR(AF4632>=$J$19, AR4631/$J$5<AN4632),0, Bodencharakterisierung!$E$8*$J$11*((AR4631/$J$5)-AN4632))","v":1.1485271157018029E-7},1.1485271157018029E-7,{"$f":"AQ4631-AP4632*Bodencharakterisierung!$E$8","v":1.8471638855446361E-4},{"$f":"AQ4632/(Bodencharakterisierung!$E$11*1000)","v":1.2192500894684067E-7},5.9296757526627475E-5,{"$error":"#N/A"},null,{"$f":"(AP4632)*$G$11*Bodencharakterisierung!$E$8","v":1.6608734721357231E-9},{"$f":"IF(AF4632<=$J$9*1.05,(AV4632*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4631,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,28.948233599998225,null,0.12192500894684068,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,59.181904815057294]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4627,1.0844364500223349E-19,{"$f":"Z4644*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.0733079134168284E-19},{"$f":"AF4643*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4644^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4644)*3600*24","v":0},0,{"$f":"AE4643-AD4644*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4644>$J$18,(AE4644/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.0733079134168284E-19,{"$error":"#N/A"},null,{"$f":"(AD4644)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4644>0,(AJ4644*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4643,NA())","v":{"$error":"#N/A"}},null,4627,{"$f":"IF(AF4644<=$J$9*0.05,AS4643*EXP((-$J$6*1)/Heterogenität!$D$4),Z4644)","v":5.8457443776268608E-5},{"$f":"IF(OR(AF4644>=$J$19, AR4643/$J$5<AN4644),0, Bodencharakterisierung!$E$8*$J$11*((AR4643/$J$5)-AN4644))","v":4.0692270995738363E-7},4.0692270995738363E-7,{"$f":"AQ4643-AP4644*Bodencharakterisierung!$E$8","v":1.8245210549778628E-4},{"$f":"AQ4644/(Bodencharakterisierung!$E$11*1000)","v":1.2043043267180614E-7},5.8864366486225994E-5,{"$error":"#N/A"},null,{"$f":"(AP4644)*$G$11*Bodencharakterisierung!$E$8","v":5.8844682457916875E-9},{"$f":"IF(AF4644<=$J$9*1.05,(AV4644*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4643,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,29.023505279998211,null,0.12043043267180614,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,58.457443776268605]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4631,1.040602837179937E-19,{"$f":"Z4648*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.0299241231205632E-19},{"$f":"AF4647*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4648^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4648)*3600*24","v":0},0,{"$f":"AE4647-AD4648*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4648>$J$18,(AE4648/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.0299241231205632E-19,{"$error":"#N/A"},null,{"$f":"(AD4648)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4648>0,(AJ4648*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4647,NA())","v":{"$error":"#N/A"}},null,4631,{"$f":"IF(AF4648<=$J$9*0.05,AS4647*EXP((-$J$6*1)/Heterogenität!$D$4),Z4648)","v":5.8260297656569424E-5},{"$f":"IF(OR(AF4648>=$J$19, AR4647/$J$5<AN4648),0, Bodencharakterisierung!$E$8*$J$11*((AR4647/$J$5)-AN4648))","v":4.0620008538693319E-8},4.0620008538693319E-8,{"$f":"AQ4647-AP4648*Bodencharakterisierung!$E$8","v":1.818406727536085E-4},{"$f":"AQ4648/(Bodencharakterisierung!$E$11*1000)","v":1.2002684670205181E-7},5.8300917665108115E-5,{"$error":"#N/A"},null,{"$f":"(AP4648)*$G$11*Bodencharakterisierung!$E$8","v":5.8740184447990368E-10},{"$f":"IF(AF4648<=$J$9*1.05,(AV4648*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4647,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,29.048595839998207,null,0.12002684670205181,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,58.260297656569421]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4645,9.0067509125541165E-20,{"$f":"Z4662*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.9143232214478527E-20},{"$f":"AF4661*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4662^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4662)*3600*24","v":0},0,{"$f":"AE4661-AD4662*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4662>$J$18,(AE4662/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.9143232214478527E-20,{"$error":"#N/A"},null,{"$f":"(AD4662)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4662>0,(AJ4662*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4661,NA())","v":{"$error":"#N/A"}},null,4645,{"$f":"IF(AF4662<=$J$9*0.05,AS4661*EXP((-$J$6*1)/Heterogenität!$D$4),Z4662)","v":5.7301062345768738E-5},{"$f":"IF(OR(AF4662>=$J$19, AR4661/$J$5<AN4662),0, Bodencharakterisierung!$E$8*$J$11*((AR4661/$J$5)-AN4662))","v":1.7664949262365428E-6},5.9412304882694781E-7,{"$f":"AQ4661-AP4662*Bodencharakterisierung!$E$8","v":1.7921524658581935E-4},{"$f":"AQ4662/(Bodencharakterisierung!$E$11*1000)","v":1.1829389213585435E-7},5.7895185394595685E-5,{"$error":"#N/A"},null,{"$f":"(AP4662)*$G$11*Bodencharakterisierung!$E$8","v":8.5915534556458129E-9},{"$f":"IF(AF4662<=$J$9*1.05,(AV4662*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4661,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,29.13641279999819,null,0.11829389213585435,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,57.301062345768734]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4652,8.3793383174414321E-20,{"$f":"Z4669*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.2933491631727334E-20},{"$f":"AF4668*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4669^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4669)*3600*24","v":0},0,{"$f":"AE4668-AD4669*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4669>$J$18,(AE4669/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.2933491631727334E-20,{"$error":"#N/A"},null,{"$f":"(AD4669)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4669>0,(AJ4669*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4668,NA())","v":{"$error":"#N/A"}},null,4652,{"$f":"IF(AF4669<=$J$9*0.05,AS4668*EXP((-$J$6*1)/Heterogenität!$D$4),Z4669)","v":5.6680839614999799E-5},{"$f":"IF(OR(AF4669>=$J$19, AR4668/$J$5<AN4669),0, Bodencharakterisierung!$E$8*$J$11*((AR4668/$J$5)-AN4669))","v":4.1881784539690257E-6},5.8769230208908217E-7,{"$f":"AQ4668-AP4669*Bodencharakterisierung!$E$8","v":1.7805493433995488E-4},{"$f":"AQ4669/(Bodencharakterisierung!$E$11*1000)","v":1.1752800946531675E-7},5.7268531917088881E-5,{"$error":"#N/A"},null,{"$f":"(AP4669)*$G$11*Bodencharakterisierung!$E$8","v":8.498559076001428E-9},{"$f":"IF(AF4669<=$J$9*1.05,(AV4669*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4668,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,29.180321279998182,null,0.11752800946531676,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,56.680839614999798]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4664,7.4037615397309964E-20,{"$f":"Z4681*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.3277837991159136E-20},{"$f":"AF4680*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4681^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4681)*3600*24","v":0},0,{"$f":"AE4680-AD4681*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4681>$J$18,(AE4681/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.3277837991159136E-20,{"$error":"#N/A"},null,{"$f":"(AD4681)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4681>0,(AJ4681*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4680,NA())","v":{"$error":"#N/A"}},null,4664,{"$f":"IF(AF4681<=$J$9*0.05,AS4680*EXP((-$J$6*1)/Heterogenität!$D$4),Z4681)","v":5.587248126538213E-5},{"$f":"IF(OR(AF4681>=$J$19, AR4680/$J$5<AN4681),0, Bodencharakterisierung!$E$8*$J$11*((AR4680/$J$5)-AN4681))","v":5.6554095519599692E-6},5.7931088108991645E-7,{"$f":"AQ4680-AP4681*Bodencharakterisierung!$E$8","v":1.7600324366252992E-4},{"$f":"AQ4681/(Bodencharakterisierung!$E$11*1000)","v":1.1617375819308906E-7},5.6451792146472046E-5,{"$error":"#N/A"},null,{"$f":"(AP4681)*$G$11*Bodencharakterisierung!$E$8","v":8.3773561927085126E-9},{"$f":"IF(AF4681<=$J$9*1.05,(AV4681*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4680,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,29.255592959998168,null,0.11617375819308906,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,55.872481265382127]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4670,6.9594316048359409E-20,{"$f":"Z4687*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.8880135983991959E-20},{"$f":"AF4686*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4687^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4687)*3600*24","v":0},0,{"$f":"AE4686-AD4687*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4687>$J$18,(AE4687/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.8880135983991959E-20,{"$error":"#N/A"},null,{"$f":"(AD4687)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4687>0,(AJ4687*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4686,NA())","v":{"$error":"#N/A"}},null,4670,{"$f":"IF(AF4687<=$J$9*0.05,AS4686*EXP((-$J$6*1)/Heterogenität!$D$4),Z4687)","v":5.587248126538213E-5},{"$f":"IF(OR(AF4687>=$J$19, AR4686/$J$5<AN4687),0, Bodencharakterisierung!$E$8*$J$11*((AR4686/$J$5)-AN4687))","v":2.0637678942134191E-6},5.7931088108991645E-7,{"$f":"AQ4686-AP4687*Bodencharakterisierung!$E$8","v":1.7485620811797195E-4},{"$f":"AQ4687/(Bodencharakterisierung!$E$11*1000)","v":1.1541663902176366E-7},5.6451792146472046E-5,{"$error":"#N/A"},null,{"$f":"(AP4687)*$G$11*Bodencharakterisierung!$E$8","v":8.3773561927085126E-9},{"$f":"IF(AF4687<=$J$9*1.05,(AV4687*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4686,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,29.293228799998161,null,0.11541663902176366,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,55.872481265382127]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4673,6.747368749101459E-20,{"$f":"Z4690*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.6781269414199855E-20},{"$f":"AF4689*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4690^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4690)*3600*24","v":0},0,{"$f":"AE4689-AD4690*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4690>$J$18,(AE4690/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.6781269414199855E-20,{"$error":"#N/A"},null,{"$f":"(AD4690)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4690>0,(AJ4690*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4689,NA())","v":{"$error":"#N/A"}},null,4673,{"$f":"IF(AF4690<=$J$9*0.05,AS4689*EXP((-$J$6*1)/Heterogenität!$D$4),Z4690)","v":5.587248126538213E-5},{"$f":"IF(OR(AF4690>=$J$19, AR4689/$J$5<AN4690),0, Bodencharakterisierung!$E$8*$J$11*((AR4689/$J$5)-AN4690))","v":2.6794706534011052E-7},2.6794706534011052E-7,{"$f":"AQ4689-AP4690*Bodencharakterisierung!$E$8","v":1.7438544040489039E-4},{"$f":"AQ4690/(Bodencharakterisierung!$E$11*1000)","v":1.151059012573534E-7},5.6140428330722237E-5,{"$error":"#N/A"},null,{"$f":"(AP4690)*$G$11*Bodencharakterisierung!$E$8","v":3.8747554731267736E-9},{"$f":"IF(AF4690<=$J$9*1.05,(AV4690*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4689,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,29.312046719998158,null,0.1151059012573534,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,55.872481265382127]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4685,5.9617964266937367E-20,{"$f":"Z4702*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.9006161982279074E-20},{"$f":"AF4701*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4702^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4702)*3600*24","v":0},0,{"$f":"AE4701-AD4702*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4702>$J$18,(AE4702/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.9006161982279074E-20,{"$error":"#N/A"},null,{"$f":"(AD4702)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4702>0,(AJ4702*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4701,NA())","v":{"$error":"#N/A"}},null,4685,{"$f":"IF(AF4702<=$J$9*0.05,AS4701*EXP((-$J$6*1)/Heterogenität!$D$4),Z4702)","v":5.5020171757249284E-5},{"$f":"IF(OR(AF4702>=$J$19, AR4701/$J$5<AN4702),0, Bodencharakterisierung!$E$8*$J$11*((AR4701/$J$5)-AN4702))","v":2.3697277105599518E-6},5.7047375481709728E-7,{"$f":"AQ4701-AP4702*Bodencharakterisierung!$E$8","v":1.722966217108817E-4},{"$f":"AQ4702/(Bodencharakterisierung!$E$11*1000)","v":1.1372714304348627E-7},5.5590645512066381E-5,{"$error":"#N/A"},null,{"$f":"(AP4702)*$G$11*Bodencharakterisierung!$E$8","v":8.2495634014388815E-9},{"$f":"IF(AF4702<=$J$9*1.05,(AV4702*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4701,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,29.387318399998144,null,0.11372714304348627,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,55.020171757249287]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4697,5.2676855163831752E-20,{"$f":"Z4714*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.2136282859256785E-20},{"$f":"AF4713*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4714^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4714)*3600*24","v":0},0,{"$f":"AE4713-AD4714*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4714>$J$18,(AE4714/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.2136282859256785E-20,{"$error":"#N/A"},null,{"$f":"(AD4714)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4714>0,(AJ4714*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4713,NA())","v":{"$error":"#N/A"}},null,4697,{"$f":"IF(AF4714<=$J$9*0.05,AS4713*EXP((-$J$6*1)/Heterogenität!$D$4),Z4714)","v":5.4467256727526504E-5},{"$f":"IF(OR(AF4714>=$J$19, AR4713/$J$5<AN4714),0, Bodencharakterisierung!$E$8*$J$11*((AR4713/$J$5)-AN4714))","v":1.3184776137142548E-6},5.64740884434718E-7,{"$f":"AQ4713-AP4714*Bodencharakterisierung!$E$8","v":1.7023703422665024E-4},{"$f":"AQ4714/(Bodencharakterisierung!$E$11*1000)","v":1.1236767935752491E-7},5.5031997611961222E-5,{"$error":"#N/A"},null,{"$f":"(AP4714)*$G$11*Bodencharakterisierung!$E$8","v":8.1666609413479157E-9},{"$f":"IF(AF4714<=$J$9*1.05,(AV4714*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4713,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,29.46259007999813,null,0.11236767935752491,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,54.467256727526504]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4704,4.9007371826100319E-20,{"$f":"Z4721*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.8504455927897897E-20},{"$f":"AF4720*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4721^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4721)*3600*24","v":0},0,{"$f":"AE4720-AD4721*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4721>$J$18,(AE4721/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.8504455927897897E-20,{"$error":"#N/A"},null,{"$f":"(AD4721)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4721>0,(AJ4721*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4720,NA())","v":{"$error":"#N/A"}},null,4704,{"$f":"IF(AF4721<=$J$9*0.05,AS4720*EXP((-$J$6*1)/Heterogenität!$D$4),Z4721)","v":5.4058132164460518E-5},{"$f":"IF(OR(AF4721>=$J$19, AR4720/$J$5<AN4721),0, Bodencharakterisierung!$E$8*$J$11*((AR4720/$J$5)-AN4721))","v":1.6767287040563335E-6},5.604988979372933E-7,{"$f":"AQ4720-AP4721*Bodencharakterisierung!$E$8","v":1.6907589302268274E-4},{"$f":"AQ4721/(Bodencharakterisierung!$E$11*1000)","v":1.116012495199226E-7},5.4618631062397811E-5,{"$error":"#N/A"},null,{"$f":"(AP4721)*$G$11*Bodencharakterisierung!$E$8","v":8.1053180026709688E-9},{"$f":"IF(AF4721<=$J$9*1.05,(AV4721*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4720,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,29.506498559998121,null,0.1116012495199226,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,54.058132164460517]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4711,4.559350564554371E-20,{"$f":"Z4728*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.5125622998718854E-20},{"$f":"AF4727*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4728^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4728)*3600*24","v":0},0,{"$f":"AE4727-AD4728*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4728>$J$18,(AE4728/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.5125622998718854E-20,{"$error":"#N/A"},null,{"$f":"(AD4728)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4728>0,(AJ4728*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4727,NA())","v":{"$error":"#N/A"}},null,4711,{"$f":"IF(AF4728<=$J$9*0.05,AS4727*EXP((-$J$6*1)/Heterogenität!$D$4),Z4728)","v":5.3768601618329608E-5},{"$f":"IF(OR(AF4728>=$J$19, AR4727/$J$5<AN4728),0, Bodencharakterisierung!$E$8*$J$11*((AR4727/$J$5)-AN4728))","v":7.6165323596864097E-7},5.5749691570949607E-7,{"$f":"AQ4727-AP4728*Bodencharakterisierung!$E$8","v":1.6788096482871415E-4},{"$f":"AQ4728/(Bodencharakterisierung!$E$11*1000)","v":1.1081251803875521E-7},5.4326098534039104E-5,{"$error":"#N/A"},null,{"$f":"(AP4728)*$G$11*Bodencharakterisierung!$E$8","v":8.0619066406072637E-9},{"$f":"IF(AF4728<=$J$9*1.05,(AV4728*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4727,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,29.550407039998113,null,0.11081251803875521,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,53.768601618329605]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4722,4.0702909876140458E-20,{"$f":"Z4739*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.0285214747488215E-20},{"$f":"AF4738*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4739^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4739)*3600*24","v":0},0,{"$f":"AE4738-AD4739*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4739>$J$18,(AE4739/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.0285214747488215E-20,{"$error":"#N/A"},null,{"$f":"(AD4739)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4739>0,(AJ4739*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4738,NA())","v":{"$error":"#N/A"}},null,4722,{"$f":"IF(AF4739<=$J$9*0.05,AS4738*EXP((-$J$6*1)/Heterogenität!$D$4),Z4739)","v":5.3009405704093787E-5},{"$f":"IF(OR(AF4739>=$J$19, AR4738/$J$5<AN4739),0, Bodencharakterisierung!$E$8*$J$11*((AR4738/$J$5)-AN4739))","v":2.6811654266287924E-6},5.4962523283386735E-7,{"$f":"AQ4738-AP4739*Bodencharakterisierung!$E$8","v":1.6612699254707819E-4},{"$f":"AQ4739/(Bodencharakterisierung!$E$11*1000)","v":1.0965478055912751E-7},5.3559030936927655E-5,{"$error":"#N/A"},null,{"$f":"(AP4739)*$G$11*Bodencharakterisierung!$E$8","v":7.9480750288807251E-9},{"$f":"IF(AF4739<=$J$9*1.05,(AV4739*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4738,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,29.6194060799981,null,0.10965478055912752,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,53.009405704093787]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4734,3.5964013777656149E-20,{"$f":"Z4751*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.5594949418193365E-20},{"$f":"AF4750*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4751^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4751)*3600*24","v":0},0,{"$f":"AE4750-AD4751*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4751>$J$18,(AE4751/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.5594949418193365E-20,{"$error":"#N/A"},null,{"$f":"(AD4751)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4751>0,(AJ4751*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4750,NA())","v":{"$error":"#N/A"}},null,4734,{"$f":"IF(AF4751<=$J$9*0.05,AS4750*EXP((-$J$6*1)/Heterogenität!$D$4),Z4751)","v":5.2535452909607338E-5},{"$f":"IF(OR(AF4751>=$J$19, AR4750/$J$5<AN4751),0, Bodencharakterisierung!$E$8*$J$11*((AR4750/$J$5)-AN4751))","v":1.0175853147472456E-6},5.447110782312635E-7,{"$f":"AQ4750-AP4751*Bodencharakterisierung!$E$8","v":1.6411803532147111E-4},{"$f":"AQ4751/(Bodencharakterisierung!$E$11*1000)","v":1.0832873618578952E-7},5.3080163987838601E-5,{"$error":"#N/A"},null,{"$f":"(AP4751)*$G$11*Bodencharakterisierung!$E$8","v":7.8770119350638144E-9},{"$f":"IF(AF4751<=$J$9*1.05,(AV4751*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4750,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,29.694677759998086,null,0.10832873618578952,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,52.535452909607336]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4737,3.4868143899422925E-20,{"$f":"Z4754*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.4510325406930529E-20},{"$f":"AF4753*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4754^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4754)*3600*24","v":0},0,{"$f":"AE4753-AD4754*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4754>$J$18,(AE4754/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.4510325406930529E-20,{"$error":"#N/A"},null,{"$f":"(AD4754)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4754>0,(AJ4754*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4753,NA())","v":{"$error":"#N/A"}},null,4737,{"$f":"IF(AF4754<=$J$9*0.05,AS4753*EXP((-$J$6*1)/Heterogenität!$D$4),Z4754)","v":5.2446395861968198E-5},{"$f":"IF(OR(AF4754>=$J$19, AR4753/$J$5<AN4754),0, Bodencharakterisierung!$E$8*$J$11*((AR4753/$J$5)-AN4754))","v":2.9332274231784099E-7},2.9332274231784099E-7,{"$f":"AQ4753-AP4754*Bodencharakterisierung!$E$8","v":1.6369172776357964E-4},{"$f":"AQ4754/(Bodencharakterisierung!$E$11*1000)","v":1.080473450584684E-7},5.2739718604286039E-5,{"$error":"#N/A"},null,{"$f":"(AP4754)*$G$11*Bodencharakterisierung!$E$8","v":4.2417105772215052E-9},{"$f":"IF(AF4754<=$J$9*1.05,(AV4754*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4753,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,29.713495679998083,null,0.1080473450584684,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,52.446395861968199]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4744,3.2439219988558858E-20,{"$f":"Z4761*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.2106327224681989E-20},{"$f":"AF4760*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4761^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4761)*3600*24","v":0},0,{"$f":"AE4760-AD4761*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4761>$J$18,(AE4761/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.2106327224681989E-20,{"$error":"#N/A"},null,{"$f":"(AD4761)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4761>0,(AJ4761*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4760,NA())","v":{"$error":"#N/A"}},null,4744,{"$f":"IF(AF4761<=$J$9*0.05,AS4760*EXP((-$J$6*1)/Heterogenität!$D$4),Z4761)","v":5.1837000206538798E-5},{"$f":"IF(OR(AF4761>=$J$19, AR4760/$J$5<AN4761),0, Bodencharakterisierung!$E$8*$J$11*((AR4760/$J$5)-AN4761))","v":2.9717780133613886E-6},5.37469208143332E-7,{"$f":"AQ4760-AP4761*Bodencharakterisierung!$E$8","v":1.6256452158883386E-4},{"$f":"AQ4761/(Bodencharakterisierung!$E$11*1000)","v":1.0730331458008836E-7},5.237446941468213E-5,{"$error":"#N/A"},null,{"$f":"(AP4761)*$G$11*Bodencharakterisierung!$E$8","v":7.7722879825052451E-9},{"$f":"IF(AF4761<=$J$9*1.05,(AV4761*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4760,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,29.757404159998075,null,0.10730331458008836,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,51.837000206538796]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4760,2.7503882183332576E-20,{"$f":"Z4777*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.7221636082452761E-20},{"$f":"AF4776*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4777^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4777)*3600*24","v":0},0,{"$f":"AE4776-AD4777*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4777>$J$18,(AE4777/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.7221636082452761E-20,{"$error":"#N/A"},null,{"$f":"(AD4777)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4777>0,(AJ4777*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4776,NA())","v":{"$error":"#N/A"}},null,4760,{"$f":"IF(AF4777<=$J$9*0.05,AS4776*EXP((-$J$6*1)/Heterogenität!$D$4),Z4777)","v":5.0969491870283591E-5},{"$f":"IF(OR(AF4777>=$J$19, AR4776/$J$5<AN4777),0, Bodencharakterisierung!$E$8*$J$11*((AR4776/$J$5)-AN4777))","v":3.5231473497017155E-6},5.2847449362113753E-7,{"$f":"AQ4776-AP4777*Bodencharakterisierung!$E$8","v":1.6003592343777793E-4},{"$f":"AQ4777/(Bodencharakterisierung!$E$11*1000)","v":1.0563427289622305E-7},5.1497966363904728E-5,{"$error":"#N/A"},null,{"$f":"(AP4777)*$G$11*Bodencharakterisierung!$E$8","v":7.6422163234637583E-9},{"$f":"IF(AF4777<=$J$9*1.05,(AV4777*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4776,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,29.857766399998056,null,0.10563427289622304,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,50.969491870283591]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4762,2.6942286404009997E-20,{"$f":"Z4779*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.6665803424784345E-20},{"$f":"AF4778*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4779^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4779)*3600*24","v":0},0,{"$f":"AE4778-AD4779*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4779>$J$18,(AE4779/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.6665803424784345E-20,{"$error":"#N/A"},null,{"$f":"(AD4779)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4779>0,(AJ4779*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4778,NA())","v":{"$error":"#N/A"}},null,4762,{"$f":"IF(AF4779<=$J$9*0.05,AS4778*EXP((-$J$6*1)/Heterogenität!$D$4),Z4779)","v":5.0969491870283591E-5},{"$f":"IF(OR(AF4779>=$J$19, AR4778/$J$5<AN4779),0, Bodencharakterisierung!$E$8*$J$11*((AR4778/$J$5)-AN4779))","v":2.4309928213333585E-6},5.2847449362113753E-7,{"$f":"AQ4778-AP4779*Bodencharakterisierung!$E$8","v":1.5968713027198798E-4},{"$f":"AQ4779/(Bodencharakterisierung!$E$11*1000)","v":1.0540404638415049E-7},5.1497966363904728E-5,{"$error":"#N/A"},null,{"$f":"(AP4779)*$G$11*Bodencharakterisierung!$E$8","v":7.6422163234637583E-9},{"$f":"IF(AF4779<=$J$9*1.05,(AV4779*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4778,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,29.870311679998053,null,0.10540404638415049,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,50.969491870283591]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4774,2.3805491115596174E-20,{"$f":"Z4791*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3561198073540536E-20},{"$f":"AF4790*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4791^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4791)*3600*24","v":0},0,{"$f":"AE4790-AD4791*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4791>$J$18,(AE4791/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.3561198073540536E-20,{"$error":"#N/A"},null,{"$f":"(AD4791)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4791>0,(AJ4791*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4790,NA())","v":{"$error":"#N/A"}},null,4774,{"$f":"IF(AF4791<=$J$9*0.05,AS4790*EXP((-$J$6*1)/Heterogenität!$D$4),Z4791)","v":5.0172447186221497E-5},{"$f":"IF(OR(AF4791>=$J$19, AR4790/$J$5<AN4791),0, Bodencharakterisierung!$E$8*$J$11*((AR4790/$J$5)-AN4791))","v":4.526319786811077E-6},5.2021037776777307E-7,{"$f":"AQ4790-AP4791*Bodencharakterisierung!$E$8","v":1.5787130316147619E-4},{"$f":"AQ4791/(Bodencharakterisierung!$E$11*1000)","v":1.0420548063463775E-7},5.069265756398927E-5,{"$error":"#N/A"},null,{"$f":"(AP4791)*$G$11*Bodencharakterisierung!$E$8","v":7.5227097780469151E-9},{"$f":"IF(AF4791<=$J$9*1.05,(AV4791*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4790,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,29.945583359998039,null,0.10420548063463775,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,50.172447186221497]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4786,2.1033901828405419E-20,{"$f":"Z4803*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.0818050962779111E-20},{"$f":"AF4802*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4803^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4803)*3600*24","v":0},0,{"$f":"AE4802-AD4803*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4803>$J$18,(AE4803/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.0818050962779111E-20,{"$error":"#N/A"},null,{"$f":"(AD4803)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4803>0,(AJ4803*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4802,NA())","v":{"$error":"#N/A"}},null,4786,{"$f":"IF(AF4803<=$J$9*0.05,AS4802*EXP((-$J$6*1)/Heterogenität!$D$4),Z4803)","v":4.9881272569473433E-5},{"$f":"IF(OR(AF4803>=$J$19, AR4802/$J$5<AN4803),0, Bodencharakterisierung!$E$8*$J$11*((AR4802/$J$5)-AN4803))","v":1.2349160543299806E-6},5.1719134908032049E-7,{"$f":"AQ4802-AP4803*Bodencharakterisierung!$E$8","v":1.55912339086377E-4},{"$f":"AQ4803/(Bodencharakterisierung!$E$11*1000)","v":1.0291243504051288E-7},5.0398463918553754E-5,{"$error":"#N/A"},null,{"$f":"(AP4803)*$G$11*Bodencharakterisierung!$E$8","v":7.4790519088503068E-9},{"$f":"IF(AF4803<=$J$9*1.05,(AV4803*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4802,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.020855039998025,null,0.10291243504051288,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,49.881272569473431]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4791,1.997657206743492E-20,{"$f":"Z4808*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.9771571568327379E-20},{"$f":"AF4807*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4808^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4808)*3600*24","v":0},0,{"$f":"AE4807-AD4808*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4808>$J$18,(AE4808/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.9771571568327379E-20,{"$error":"#N/A"},null,{"$f":"(AD4808)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4808>0,(AJ4808*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4807,NA())","v":{"$error":"#N/A"}},null,4791,{"$f":"IF(AF4808<=$J$9*0.05,AS4807*EXP((-$J$6*1)/Heterogenität!$D$4),Z4808)","v":4.9533763814239425E-5},{"$f":"IF(OR(AF4808>=$J$19, AR4807/$J$5<AN4808),0, Bodencharakterisierung!$E$8*$J$11*((AR4807/$J$5)-AN4808))","v":2.3293402140923972E-6},5.1358822284318264E-7,{"$f":"AQ4807-AP4808*Bodencharakterisierung!$E$8","v":1.5517840737625473E-4},{"$f":"AQ4808/(Bodencharakterisierung!$E$11*1000)","v":1.0242799166749487E-7},5.0047352037082608E-5,{"$error":"#N/A"},null,{"$f":"(AP4808)*$G$11*Bodencharakterisierung!$E$8","v":7.4269474639294592E-9},{"$f":"IF(AF4808<=$J$9*1.05,(AV4808*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4807,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.05221823999802,null,0.10242799166749486,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,49.533763814239428]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4804,1.7469637292592147E-20,{"$f":"Z4821*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.7290363073165524E-20},{"$f":"AF4820*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4821^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4821)*3600*24","v":0},0,{"$f":"AE4820-AD4821*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4821>$J$18,(AE4821/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.7290363073165524E-20,{"$error":"#N/A"},null,{"$f":"(AD4821)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4821>0,(AJ4821*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4820,NA())","v":{"$error":"#N/A"}},null,4804,{"$f":"IF(AF4821<=$J$9*0.05,AS4820*EXP((-$J$6*1)/Heterogenität!$D$4),Z4821)","v":4.9047116311619414E-5},{"$f":"IF(OR(AF4821>=$J$19, AR4820/$J$5<AN4821),0, Bodencharakterisierung!$E$8*$J$11*((AR4820/$J$5)-AN4821))","v":7.2442512167124044E-7},5.0854244382750227E-7,{"$f":"AQ4820-AP4821*Bodencharakterisierung!$E$8","v":1.5314860647308053E-4},{"$f":"AQ4821/(Bodencharakterisierung!$E$11*1000)","v":1.0108818909114226E-7},4.9555658755446916E-5,{"$error":"#N/A"},null,{"$f":"(AP4821)*$G$11*Bodencharakterisierung!$E$8","v":7.3539809627573747E-9},{"$f":"IF(AF4821<=$J$9*1.05,(AV4821*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4820,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.133762559998004,null,0.10108818909114227,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,49.047116311619412]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4807,1.6937314915813789E-20,{"$f":"Z4824*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.6763503413041318E-20},{"$f":"AF4823*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4824^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4824)*3600*24","v":0},0,{"$f":"AE4823-AD4824*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4824>$J$18,(AE4824/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.6763503413041318E-20,{"$error":"#N/A"},null,{"$f":"(AD4824)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4824>0,(AJ4824*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4823,NA())","v":{"$error":"#N/A"}},null,4807,{"$f":"IF(AF4824<=$J$9*0.05,AS4823*EXP((-$J$6*1)/Heterogenität!$D$4),Z4824)","v":4.8740694800005301E-5},{"$f":"IF(OR(AF4824>=$J$19, AR4823/$J$5<AN4824),0, Bodencharakterisierung!$E$8*$J$11*((AR4823/$J$5)-AN4824))","v":2.4658848394162249E-6},5.0536532851317139E-7,{"$f":"AQ4823-AP4824*Bodencharakterisierung!$E$8","v":1.5274941389668514E-4},{"$f":"AQ4824/(Bodencharakterisierung!$E$11*1000)","v":1.0082469564137634E-7},4.9246060128518473E-5,{"$error":"#N/A"},null,{"$f":"(AP4824)*$G$11*Bodencharakterisierung!$E$8","v":7.308037018802129E-9},{"$f":"IF(AF4824<=$J$9*1.05,(AV4824*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4823,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.152580479998001,null,0.10082469564137633,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,48.740694800005301]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4814,{"$f":"AG4830","v":1.5757457183680945E-20},{"$f":"Z4831*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.5595753435089054E-20},{"$f":"AF4830*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4831^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4831)*3600*24","v":0},{"$f":"MIN(AC4831,Z4831-AA4831)","v":0},{"$f":"AE4830-AD4831*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4831>$J$18,(AE4831/(Bodencharakterisierung!$E$11*1000)),0)","v":0},{"$f":"AA4831+AD4831","v":1.5595753435089054E-20},{"$f":"IF(AD4831>0,Y4831,NA())","v":{"$error":"#N/A"}},null,{"$f":"(AD4831)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4831>0,(AJ4831*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4830,NA())","v":{"$error":"#N/A"}},null,4814,{"$f":"IF(AF4831<=$J$9*0.05,AS4830*EXP((-$J$6*1)/Heterogenität!$D$4),Z4831)","v":4.8613737207843413E-5},{"$f":"IF(OR(AF4831>=$J$19, AR4830/$J$5<AN4831),0, Bodencharakterisierung!$E$8*$J$11*((AR4830/$J$5)-AN4831))","v":1.8654149165666032E-7},{"$f":"MIN(AO4831,AS4830-AN4831)","v":1.8654149165666032E-7},{"$f":"AQ4830-AP4831*Bodencharakterisierung!$E$8","v":1.5173043104897642E-4},{"$f":"AQ4831/(Bodencharakterisierung!$E$11*1000)","v":1.0015209970229467E-7},{"$f":"AN4831+AP4831","v":4.8800278699500076E-5},{"$f":"IF(AN4831>$G$5,AM4831,NA())","v":{"$error":"#N/A"}},null,{"$f":"(AP4831)*$G$11*Bodencharakterisierung!$E$8","v":2.6975576867931326E-9},{"$f":"IF(AF4831<=$J$9*1.05,(AV4831*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4830,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH4831>($G$5*10^6),BH4831*0.99,9999)","v":9999},{"$f":"AT4831+$G$3","v":{"$error":"#N/A"}},{"$f":"IF(ISNUMBER(AT4831),BA4831+BB4831+BC4831+$AZ$17,\"\")","v":""},{"$f":"IF(ISNUMBER(AK4831),AK4831,BA4830)","v":1.6399886323194495},{"$f":"IF(ISNUMBER(AW4831),AW4831,0)","v":0},30.196488959997993,null,{"$f":"AR4831*10^6","v":0.10015209970229466},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF4831*10^6","v":0},{"$f":"AN4831*10^6","v":48.613737207843414}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4826,1.3922872074237664E-20,{"$f":"Z4843*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.3779994922212067E-20},{"$f":"AF4842*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4843^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4843)*3600*24","v":0},0,{"$f":"AE4842-AD4843*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4843>$J$18,(AE4843/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.3779994922212067E-20,{"$error":"#N/A"},null,{"$f":"(AD4843)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4843>0,(AJ4843*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4842,NA())","v":{"$error":"#N/A"}},null,4826,{"$f":"IF(AF4843<=$J$9*0.05,AS4842*EXP((-$J$6*1)/Heterogenität!$D$4),Z4843)","v":4.7987040135026568E-5},{"$f":"IF(OR(AF4843>=$J$19, AR4842/$J$5<AN4843),0, Bodencharakterisierung!$E$8*$J$11*((AR4842/$J$5)-AN4843))","v":7.6625718274334931E-7},4.9755109978878828E-7,{"$f":"AQ4842-AP4843*Bodencharakterisierung!$E$8","v":1.4985690047906295E-4},{"$f":"AQ4843/(Bodencharakterisierung!$E$11*1000)","v":9.8915445860767622E-8},4.8484591234815357E-5,{"$error":"#N/A"},null,{"$f":"(AP4843)*$G$11*Bodencharakterisierung!$E$8","v":7.1950362457590087E-9},{"$f":"IF(AF4843<=$J$9*1.05,(AV4843*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4842,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.271760639997979,null,9.8915445860767628E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,47.987040135026568]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4832,1.3087303720354266E-20,{"$f":"Z4849*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.2953001209113202E-20},{"$f":"AF4848*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4849^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4849)*3600*24","v":0},0,{"$f":"AE4848-AD4849*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4849>$J$18,(AE4849/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.2953001209113202E-20,{"$error":"#N/A"},null,{"$f":"(AD4849)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4849>0,(AJ4849*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4848,NA())","v":{"$error":"#N/A"}},null,4832,{"$f":"IF(AF4849<=$J$9*0.05,AS4848*EXP((-$J$6*1)/Heterogenität!$D$4),Z4849)","v":4.7744140852476373E-5},{"$f":"IF(OR(AF4849>=$J$19, AR4848/$J$5<AN4849),0, Bodencharakterisierung!$E$8*$J$11*((AR4848/$J$5)-AN4849))","v":3.194120297793489E-7},3.194120297793489E-7,{"$f":"AQ4848-AP4849*Bodencharakterisierung!$E$8","v":1.4901484746372855E-4},{"$f":"AQ4849/(Bodencharakterisierung!$E$11*1000)","v":9.8359635289589806E-8},4.8063552882255722E-5,{"$error":"#N/A"},null,{"$f":"(AP4849)*$G$11*Bodencharakterisierung!$E$8","v":4.6189851305111277E-9},{"$f":"IF(AF4849<=$J$9*1.05,(AV4849*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4848,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.309396479997972,null,9.8359635289589811E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,47.74414085247637]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4844,1.1563595151881106E-20,{"$f":"Z4861*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.1444929007879476E-20},{"$f":"AF4860*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4861^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4861)*3600*24","v":0},0,{"$f":"AE4860-AD4861*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4861>$J$18,(AE4861/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.1444929007879476E-20,{"$error":"#N/A"},null,{"$f":"(AD4861)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4861>0,(AJ4861*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4860,NA())","v":{"$error":"#N/A"}},null,4844,{"$f":"IF(AF4861<=$J$9*0.05,AS4860*EXP((-$J$6*1)/Heterogenität!$D$4),Z4861)","v":4.6942557862745601E-5},{"$f":"IF(OR(AF4861>=$J$19, AR4860/$J$5<AN4861),0, Bodencharakterisierung!$E$8*$J$11*((AR4860/$J$5)-AN4861))","v":2.8973157397881411E-6},4.8672144032612779E-7,{"$f":"AQ4860-AP4861*Bodencharakterisierung!$E$8","v":1.4728103310298769E-4},{"$f":"AQ4861/(Bodencharakterisierung!$E$11*1000)","v":9.7215203368308702E-8},4.7429279303071728E-5,{"$error":"#N/A"},null,{"$f":"(AP4861)*$G$11*Bodencharakterisierung!$E$8","v":7.0384296330992314E-9},{"$f":"IF(AF4861<=$J$9*1.05,(AV4861*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4860,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.384668159997958,null,9.7215203368308703E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,46.942557862745602]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4856,1.0217286592703037E-20,{"$f":"Z4873*EXP((-$J$6/Heterogenität!$D$4)*1)","v":1.0112436328906108E-20},{"$f":"AF4872*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4873^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4873)*3600*24","v":0},0,{"$f":"AE4872-AD4873*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4873>$J$18,(AE4873/(Bodencharakterisierung!$E$11*1000)),0)","v":0},1.0112436328906108E-20,{"$error":"#N/A"},null,{"$f":"(AD4873)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4873>0,(AJ4873*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4872,NA())","v":{"$error":"#N/A"}},null,4856,{"$f":"IF(AF4873<=$J$9*0.05,AS4872*EXP((-$J$6*1)/Heterogenität!$D$4),Z4873)","v":4.6358883159108079E-5},{"$f":"IF(OR(AF4873>=$J$19, AR4872/$J$5<AN4873),0, Bodencharakterisierung!$E$8*$J$11*((AR4872/$J$5)-AN4873))","v":3.1979069583478264E-6},4.806696398838289E-7,{"$f":"AQ4872-AP4873*Bodencharakterisierung!$E$8","v":1.4555727164478231E-4},{"$f":"AQ4873/(Bodencharakterisierung!$E$11*1000)","v":9.6077407026258949E-8},4.6839552798991908E-5,{"$error":"#N/A"},null,{"$f":"(AP4873)*$G$11*Bodencharakterisierung!$E$8","v":6.9509151575952575E-9},{"$f":"IF(AF4873<=$J$9*1.05,(AV4873*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4872,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.459939839997944,null,9.6077407026258943E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,46.358883159108082]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4863,9.5055477694163165E-21,{"$f":"Z4880*EXP((-$J$6/Heterogenität!$D$4)*1)","v":9.4080014020794742E-21},{"$f":"AF4879*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4880^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4880)*3600*24","v":0},0,{"$f":"AE4879-AD4880*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4880>$J$18,(AE4880/(Bodencharakterisierung!$E$11*1000)),0)","v":0},9.4080014020794742E-21,{"$error":"#N/A"},null,{"$f":"(AD4880)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4880>0,(AJ4880*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4879,NA())","v":{"$error":"#N/A"}},null,4863,{"$f":"IF(AF4880<=$J$9*0.05,AS4879*EXP((-$J$6*1)/Heterogenität!$D$4),Z4880)","v":4.6098737214524214E-5},{"$f":"IF(OR(AF4880>=$J$19, AR4879/$J$5<AN4880),0, Bodencharakterisierung!$E$8*$J$11*((AR4879/$J$5)-AN4880))","v":2.5351952327295274E-6},4.7797233035048754E-7,{"$f":"AQ4879-AP4880*Bodencharakterisierung!$E$8","v":1.4453455316265534E-4},{"$f":"AQ4880/(Bodencharakterisierung!$E$11*1000)","v":9.5402345321884713E-8},4.6576709544874701E-5,{"$error":"#N/A"},null,{"$f":"(AP4880)*$G$11*Bodencharakterisierung!$E$8","v":6.9119096366213101E-9},{"$f":"IF(AF4880<=$J$9*1.05,(AV4880*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4879,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.503848319997935,null,9.5402345321884713E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,46.098737214524213]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4875,8.3988504012055848E-21,{"$f":"Z4892*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.3126610130380578E-21},{"$f":"AF4891*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4892^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4892)*3600*24","v":0},0,{"$f":"AE4891-AD4892*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4892>$J$18,(AE4892/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.3126610130380578E-21,{"$error":"#N/A"},null,{"$f":"(AD4892)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4892>0,(AJ4892*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4891,NA())","v":{"$error":"#N/A"}},null,4875,{"$f":"IF(AF4892<=$J$9*0.05,AS4891*EXP((-$J$6*1)/Heterogenität!$D$4),Z4892)","v":4.5690725850432424E-5},{"$f":"IF(OR(AF4892>=$J$19, AR4891/$J$5<AN4892),0, Bodencharakterisierung!$E$8*$J$11*((AR4891/$J$5)-AN4892))","v":1.0482458077444513E-6},4.7374188599802887E-7,{"$f":"AQ4891-AP4892*Bodencharakterisierung!$E$8","v":1.427875948577083E-4},{"$f":"AQ4892/(Bodencharakterisierung!$E$11*1000)","v":9.4249237529840455E-8},4.6164467736430453E-5,{"$error":"#N/A"},null,{"$f":"(AP4892)*$G$11*Bodencharakterisierung!$E$8","v":6.8507336077379908E-9},{"$f":"IF(AF4892<=$J$9*1.05,(AV4892*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4891,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.579119999997921,null,9.4249237529840449E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,45.690725850432422]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4876,8.3126610130380578E-21,{"$f":"Z4893*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.2273561043263895E-21},{"$f":"AF4892*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4893^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4893)*3600*24","v":0},0,{"$f":"AE4892-AD4893*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4893>$J$18,(AE4893/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.2273561043263895E-21,{"$error":"#N/A"},null,{"$f":"(AD4893)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4893>0,(AJ4893*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4892,NA())","v":{"$error":"#N/A"}},null,4876,{"$f":"IF(AF4893<=$J$9*0.05,AS4892*EXP((-$J$6*1)/Heterogenität!$D$4),Z4893)","v":4.5690725850432424E-5},{"$f":"IF(OR(AF4893>=$J$19, AR4892/$J$5<AN4893),0, Bodencharakterisierung!$E$8*$J$11*((AR4892/$J$5)-AN4893))","v":5.5872422031144504E-7},4.7374188599802887E-7,{"$f":"AQ4892-AP4893*Bodencharakterisierung!$E$8","v":1.4263126003532896E-4},{"$f":"AQ4893/(Bodencharakterisierung!$E$11*1000)","v":9.4146046227939911E-8},4.6164467736430453E-5,{"$error":"#N/A"},null,{"$f":"(AP4893)*$G$11*Bodencharakterisierung!$E$8","v":6.8507336077379908E-9},{"$f":"IF(AF4893<=$J$9*1.05,(AV4893*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4892,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.58539263999792,null,9.4146046227939914E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,45.690725850432422]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4877,8.2273561043263895E-21,{"$f":"Z4894*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.1429265985018226E-21},{"$f":"AF4893*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4894^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4894)*3600*24","v":0},0,{"$f":"AE4893-AD4894*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4894>$J$18,(AE4894/(Bodencharakterisierung!$E$11*1000)),0)","v":0},8.1429265985018226E-21,{"$error":"#N/A"},null,{"$f":"(AD4894)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4894>0,(AJ4894*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4893,NA())","v":{"$error":"#N/A"}},null,4877,{"$f":"IF(AF4894<=$J$9*0.05,AS4893*EXP((-$J$6*1)/Heterogenität!$D$4),Z4894)","v":4.5690725850432424E-5},{"$f":"IF(OR(AF4894>=$J$19, AR4893/$J$5<AN4894),0, Bodencharakterisierung!$E$8*$J$11*((AR4893/$J$5)-AN4894))","v":6.9202632878571229E-8},6.9202632878571229E-8,{"$f":"AQ4893-AP4894*Bodencharakterisierung!$E$8","v":1.4260842316647903E-4},{"$f":"AQ4894/(Bodencharakterisierung!$E$11*1000)","v":9.4130972387114877E-8},4.5759928483310995E-5,{"$error":"#N/A"},null,{"$f":"(AP4894)*$G$11*Bodencharakterisierung!$E$8","v":1.00073229076298E-9},{"$f":"IF(AF4894<=$J$9*1.05,(AV4894*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4893,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.591665279997919,null,9.4130972387114875E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,45.690725850432422]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4878,{"$f":"AG4894","v":8.1429265985018226E-21},{"$f":"Z4895*EXP((-$J$6/Heterogenität!$D$4)*1)","v":8.0593635121397647E-21},{"$f":"AF4894*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4895^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4895)*3600*24","v":0},{"$f":"MIN(AC4895,Z4895-AA4895)","v":0},{"$f":"AE4894-AD4895*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4895>$J$18,(AE4895/(Bodencharakterisierung!$E$11*1000)),0)","v":0},{"$f":"AA4895+AD4895","v":8.0593635121397647E-21},{"$f":"IF(AD4895>0,Y4895,NA())","v":{"$error":"#N/A"}},null,{"$f":"(AD4895)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4895>0,(AJ4895*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4894,NA())","v":{"$error":"#N/A"}},null,4878,{"$f":"IF(AF4895<=$J$9*0.05,AS4894*EXP((-$J$6*1)/Heterogenität!$D$4),Z4895)","v":4.5290337997689273E-5},{"$f":"IF(OR(AF4895>=$J$19, AR4894/$J$5<AN4895),0, Bodencharakterisierung!$E$8*$J$11*((AR4894/$J$5)-AN4895))","v":3.9107538029364074E-6},{"$f":"MIN(AO4895,AS4894-AN4895)","v":4.6959048562172115E-7},{"$f":"AQ4894-AP4895*Bodencharakterisierung!$E$8","v":1.4245345830622388E-4},{"$f":"AQ4895/(Bodencharakterisierung!$E$11*1000)","v":9.4028685350642824E-8},{"$f":"AN4895+AP4895","v":4.5759928483310995E-5},{"$f":"IF(AN4895>$G$5,AM4895,NA())","v":{"$error":"#N/A"}},null,{"$f":"(AP4895)*$G$11*Bodencharakterisierung!$E$8","v":6.7907006258173962E-9},{"$f":"IF(AF4895<=$J$9*1.05,(AV4895*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4894,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH4895>($G$5*10^6),BH4895*0.99,9999)","v":9999},{"$f":"AT4895+$G$3","v":{"$error":"#N/A"}},{"$f":"IF(ISNUMBER(AT4895),BA4895+BB4895+BC4895+$AZ$17,\"\")","v":""},{"$f":"IF(ISNUMBER(AK4895),AK4895,BA4894)","v":1.6399886323194495},{"$f":"IF(ISNUMBER(AW4895),AW4895,0)","v":0},30.597937919997918,null,{"$f":"AR4895*10^6","v":9.4028685350642821E-2},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF4895*10^6","v":0},{"$f":"AN4895*10^6","v":45.290337997689271}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4879,8.0593635121397647E-21,{"$f":"Z4896*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.9766579540039394E-21},{"$f":"AF4895*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4896^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4896)*3600*24","v":0},0,{"$f":"AE4895-AD4896*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4896>$J$18,(AE4896/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.9766579540039394E-21,{"$error":"#N/A"},null,{"$f":"(AD4896)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4896>0,(AJ4896*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4895,NA())","v":{"$error":"#N/A"}},null,4879,{"$f":"IF(AF4896<=$J$9*0.05,AS4895*EXP((-$J$6*1)/Heterogenität!$D$4),Z4896)","v":4.5290337997689273E-5},{"$f":"IF(OR(AF4896>=$J$19, AR4895/$J$5<AN4896),0, Bodencharakterisierung!$E$8*$J$11*((AR4895/$J$5)-AN4896))","v":3.425521893411042E-6},4.6959048562172115E-7,{"$f":"AQ4895-AP4896*Bodencharakterisierung!$E$8","v":1.4229849344596872E-4},{"$f":"AQ4896/(Bodencharakterisierung!$E$11*1000)","v":9.3926398314170772E-8},4.5759928483310995E-5,{"$error":"#N/A"},null,{"$f":"(AP4896)*$G$11*Bodencharakterisierung!$E$8","v":6.7907006258173962E-9},{"$f":"IF(AF4896<=$J$9*1.05,(AV4896*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4895,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.604210559997917,null,9.3926398314170767E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,45.290337997689271]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4880,7.9766579540039394E-21,{"$f":"Z4897*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.8948011241003431E-21},{"$f":"AF4896*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4897^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4897)*3600*24","v":0},0,{"$f":"AE4896-AD4897*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4897>$J$18,(AE4897/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.8948011241003431E-21,{"$error":"#N/A"},null,{"$f":"(AD4897)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4897>0,(AJ4897*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4896,NA())","v":{"$error":"#N/A"}},null,4880,{"$f":"IF(AF4897<=$J$9*0.05,AS4896*EXP((-$J$6*1)/Heterogenität!$D$4),Z4897)","v":4.5290337997689273E-5},{"$f":"IF(OR(AF4897>=$J$19, AR4896/$J$5<AN4897),0, Bodencharakterisierung!$E$8*$J$11*((AR4896/$J$5)-AN4897))","v":2.9402899838856765E-6},4.6959048562172115E-7,{"$f":"AQ4896-AP4897*Bodencharakterisierung!$E$8","v":1.4214352858571357E-4},{"$f":"AQ4897/(Bodencharakterisierung!$E$11*1000)","v":9.3824111277698719E-8},4.5759928483310995E-5,{"$error":"#N/A"},null,{"$f":"(AP4897)*$G$11*Bodencharakterisierung!$E$8","v":6.7907006258173962E-9},{"$f":"IF(AF4897<=$J$9*1.05,(AV4897*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4896,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.610483199997915,null,9.3824111277698713E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,45.290337997689271]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4881,7.8948011241003431E-21,{"$f":"Z4898*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.8137843127409175E-21},{"$f":"AF4897*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4898^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4898)*3600*24","v":0},0,{"$f":"AE4897-AD4898*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4898>$J$18,(AE4898/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.8137843127409175E-21,{"$error":"#N/A"},null,{"$f":"(AD4898)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4898>0,(AJ4898*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4897,NA())","v":{"$error":"#N/A"}},null,4881,{"$f":"IF(AF4898<=$J$9*0.05,AS4897*EXP((-$J$6*1)/Heterogenität!$D$4),Z4898)","v":4.5290337997689273E-5},{"$f":"IF(OR(AF4898>=$J$19, AR4897/$J$5<AN4898),0, Bodencharakterisierung!$E$8*$J$11*((AR4897/$J$5)-AN4898))","v":2.4550580743603771E-6},4.6959048562172115E-7,{"$f":"AQ4897-AP4898*Bodencharakterisierung!$E$8","v":1.4198856372545841E-4},{"$f":"AQ4898/(Bodencharakterisierung!$E$11*1000)","v":9.3721824241226679E-8},4.5759928483310995E-5,{"$error":"#N/A"},null,{"$f":"(AP4898)*$G$11*Bodencharakterisierung!$E$8","v":6.7907006258173962E-9},{"$f":"IF(AF4898<=$J$9*1.05,(AV4898*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4897,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.616755839997914,null,9.3721824241226673E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,45.290337997689271]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4882,7.8137843127409175E-21,{"$f":"Z4899*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.7335988996168212E-21},{"$f":"AF4898*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4899^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4899)*3600*24","v":0},0,{"$f":"AE4898-AD4899*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4899>$J$18,(AE4899/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.7335988996168212E-21,{"$error":"#N/A"},null,{"$f":"(AD4899)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4899>0,(AJ4899*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4898,NA())","v":{"$error":"#N/A"}},null,4882,{"$f":"IF(AF4899<=$J$9*0.05,AS4898*EXP((-$J$6*1)/Heterogenität!$D$4),Z4899)","v":4.5290337997689273E-5},{"$f":"IF(OR(AF4899>=$J$19, AR4898/$J$5<AN4899),0, Bodencharakterisierung!$E$8*$J$11*((AR4898/$J$5)-AN4899))","v":1.9698261648350777E-6},4.6959048562172115E-7,{"$f":"AQ4898-AP4899*Bodencharakterisierung!$E$8","v":1.4183359886520326E-4},{"$f":"AQ4899/(Bodencharakterisierung!$E$11*1000)","v":9.3619537204754626E-8},4.5759928483310995E-5,{"$error":"#N/A"},null,{"$f":"(AP4899)*$G$11*Bodencharakterisierung!$E$8","v":6.7907006258173962E-9},{"$f":"IF(AF4899<=$J$9*1.05,(AV4899*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4898,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.623028479997913,null,9.3619537204754633E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,45.290337997689271]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4883,7.7335988996168212E-21,{"$f":"Z4900*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.6542363528812169E-21},{"$f":"AF4899*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4900^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4900)*3600*24","v":0},0,{"$f":"AE4899-AD4900*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4900>$J$18,(AE4900/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.6542363528812169E-21,{"$error":"#N/A"},null,{"$f":"(AD4900)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4900>0,(AJ4900*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4899,NA())","v":{"$error":"#N/A"}},null,4883,{"$f":"IF(AF4900<=$J$9*0.05,AS4899*EXP((-$J$6*1)/Heterogenität!$D$4),Z4900)","v":4.5290337997689273E-5},{"$f":"IF(OR(AF4900>=$J$19, AR4899/$J$5<AN4900),0, Bodencharakterisierung!$E$8*$J$11*((AR4899/$J$5)-AN4900))","v":1.4845942553097123E-6},4.6959048562172115E-7,{"$f":"AQ4899-AP4900*Bodencharakterisierung!$E$8","v":1.416786340049481E-4},{"$f":"AQ4900/(Bodencharakterisierung!$E$11*1000)","v":9.3517250168282573E-8},4.5759928483310995E-5,{"$error":"#N/A"},null,{"$f":"(AP4900)*$G$11*Bodencharakterisierung!$E$8","v":6.7907006258173962E-9},{"$f":"IF(AF4900<=$J$9*1.05,(AV4900*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4899,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.629301119997912,null,9.3517250168282579E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,45.290337997689271]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4884,7.6542363528812169E-21,{"$f":"Z4901*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.5756882282414719E-21},{"$f":"AF4900*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4901^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4901)*3600*24","v":0},0,{"$f":"AE4900-AD4901*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4901>$J$18,(AE4901/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.5756882282414719E-21,{"$error":"#N/A"},null,{"$f":"(AD4901)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4901>0,(AJ4901*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4900,NA())","v":{"$error":"#N/A"}},null,4884,{"$f":"IF(AF4901<=$J$9*0.05,AS4900*EXP((-$J$6*1)/Heterogenität!$D$4),Z4901)","v":4.5290337997689273E-5},{"$f":"IF(OR(AF4901>=$J$19, AR4900/$J$5<AN4901),0, Bodencharakterisierung!$E$8*$J$11*((AR4900/$J$5)-AN4901))","v":9.9936234578441308E-7},4.6959048562172115E-7,{"$f":"AQ4900-AP4901*Bodencharakterisierung!$E$8","v":1.4152366914469295E-4},{"$f":"AQ4901/(Bodencharakterisierung!$E$11*1000)","v":9.3414963131810534E-8},4.5759928483310995E-5,{"$error":"#N/A"},null,{"$f":"(AP4901)*$G$11*Bodencharakterisierung!$E$8","v":6.7907006258173962E-9},{"$f":"IF(AF4901<=$J$9*1.05,(AV4901*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4900,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.635573759997911,null,9.3414963131810538E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,45.290337997689271]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4885,7.5756882282414719E-21,{"$f":"Z4902*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.4979461680606712E-21},{"$f":"AF4901*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4902^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4902)*3600*24","v":0},0,{"$f":"AE4901-AD4902*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4902>$J$18,(AE4902/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.4979461680606712E-21,{"$error":"#N/A"},null,{"$f":"(AD4902)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4902>0,(AJ4902*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4901,NA())","v":{"$error":"#N/A"}},null,4885,{"$f":"IF(AF4902<=$J$9*0.05,AS4901*EXP((-$J$6*1)/Heterogenität!$D$4),Z4902)","v":4.5290337997689273E-5},{"$f":"IF(OR(AF4902>=$J$19, AR4901/$J$5<AN4902),0, Bodencharakterisierung!$E$8*$J$11*((AR4901/$J$5)-AN4902))","v":5.1413043625911368E-7},4.6959048562172115E-7,{"$f":"AQ4901-AP4902*Bodencharakterisierung!$E$8","v":1.413687042844378E-4},{"$f":"AQ4902/(Bodencharakterisierung!$E$11*1000)","v":9.3312676095338481E-8},4.5759928483310995E-5,{"$error":"#N/A"},null,{"$f":"(AP4902)*$G$11*Bodencharakterisierung!$E$8","v":6.7907006258173962E-9},{"$f":"IF(AF4902<=$J$9*1.05,(AV4902*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4901,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.64184639999791,null,9.3312676095338484E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,45.290337997689271]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4886,7.4979461680606712E-21,{"$f":"Z4903*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.4210019004683541E-21},{"$f":"AF4902*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4903^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4903)*3600*24","v":0},0,{"$f":"AE4902-AD4903*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4903>$J$18,(AE4903/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.4210019004683541E-21,{"$error":"#N/A"},null,{"$f":"(AD4903)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4903>0,(AJ4903*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4902,NA())","v":{"$error":"#N/A"}},null,4886,{"$f":"IF(AF4903<=$J$9*0.05,AS4902*EXP((-$J$6*1)/Heterogenität!$D$4),Z4903)","v":4.5290337997689273E-5},{"$f":"IF(OR(AF4903>=$J$19, AR4902/$J$5<AN4903),0, Bodencharakterisierung!$E$8*$J$11*((AR4902/$J$5)-AN4903))","v":2.8898526733748098E-8},2.8898526733748098E-8,{"$f":"AQ4902-AP4903*Bodencharakterisierung!$E$8","v":1.4135916777061565E-4},{"$f":"AQ4903/(Bodencharakterisierung!$E$11*1000)","v":9.3306381366742999E-8},4.5319236524423024E-5,{"$error":"#N/A"},null,{"$f":"(AP4903)*$G$11*Bodencharakterisierung!$E$8","v":4.1789867892286514E-10},{"$f":"IF(AF4903<=$J$9*1.05,(AV4903*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4902,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.648119039997908,null,9.3306381366743005E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,45.290337997689271]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4887,7.4210019004683541E-21,{"$f":"Z4904*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.3448472384803743E-21},{"$f":"AF4903*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4904^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4904)*3600*24","v":0},0,{"$f":"AE4903-AD4904*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4904>$J$18,(AE4904/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.3448472384803743E-21,{"$error":"#N/A"},null,{"$f":"(AD4904)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4904>0,(AJ4904*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4903,NA())","v":{"$error":"#N/A"}},null,4887,{"$f":"IF(AF4904<=$J$9*0.05,AS4903*EXP((-$J$6*1)/Heterogenität!$D$4),Z4904)","v":4.4854168439902937E-5},{"$f":"IF(OR(AF4904>=$J$19, AR4903/$J$5<AN4904),0, Bodencharakterisierung!$E$8*$J$11*((AR4903/$J$5)-AN4904))","v":4.2617969911262598E-6},4.6506808452008739E-7,{"$f":"AQ4903-AP4904*Bodencharakterisierung!$E$8","v":1.4120569530272402E-4},{"$f":"AQ4904/(Bodencharakterisierung!$E$11*1000)","v":9.3205079407738634E-8},4.5319236524423024E-5,{"$error":"#N/A"},null,{"$f":"(AP4904)*$G$11*Bodencharakterisierung!$E$8","v":6.7253026398458488E-9},{"$f":"IF(AF4904<=$J$9*1.05,(AV4904*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4903,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.654391679997907,null,9.3205079407738631E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.854168439902935]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4888,7.3448472384803743E-21,{"$f":"Z4905*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.2694740791277921E-21},{"$f":"AF4904*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4905^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4905)*3600*24","v":0},0,{"$f":"AE4904-AD4905*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4905>$J$18,(AE4905/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.2694740791277921E-21,{"$error":"#N/A"},null,{"$f":"(AD4905)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4905>0,(AJ4905*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4904,NA())","v":{"$error":"#N/A"}},null,4888,{"$f":"IF(AF4905<=$J$9*0.05,AS4904*EXP((-$J$6*1)/Heterogenität!$D$4),Z4905)","v":4.4854168439902937E-5},{"$f":"IF(OR(AF4905>=$J$19, AR4904/$J$5<AN4905),0, Bodencharakterisierung!$E$8*$J$11*((AR4904/$J$5)-AN4905))","v":3.7812381177661815E-6},4.6506808452008739E-7,{"$f":"AQ4904-AP4905*Bodencharakterisierung!$E$8","v":1.4105222283483239E-4},{"$f":"AQ4905/(Bodencharakterisierung!$E$11*1000)","v":9.3103777448734255E-8},4.5319236524423024E-5,{"$error":"#N/A"},null,{"$f":"(AP4905)*$G$11*Bodencharakterisierung!$E$8","v":6.7253026398458488E-9},{"$f":"IF(AF4905<=$J$9*1.05,(AV4905*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4904,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.660664319997906,null,9.3103777448734257E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.854168439902935]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4889,7.2694740791277921E-21,{"$f":"Z4906*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.1948744025947068E-21},{"$f":"AF4905*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4906^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4906)*3600*24","v":0},0,{"$f":"AE4905-AD4906*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4906>$J$18,(AE4906/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.1948744025947068E-21,{"$error":"#N/A"},null,{"$f":"(AD4906)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4906>0,(AJ4906*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4905,NA())","v":{"$error":"#N/A"}},null,4889,{"$f":"IF(AF4906<=$J$9*0.05,AS4905*EXP((-$J$6*1)/Heterogenität!$D$4),Z4906)","v":4.4854168439902937E-5},{"$f":"IF(OR(AF4906>=$J$19, AR4905/$J$5<AN4906),0, Bodencharakterisierung!$E$8*$J$11*((AR4905/$J$5)-AN4906))","v":3.3006792444061037E-6},4.6506808452008739E-7,{"$f":"AQ4905-AP4906*Bodencharakterisierung!$E$8","v":1.4089875036694076E-4},{"$f":"AQ4906/(Bodencharakterisierung!$E$11*1000)","v":9.3002475489729877E-8},4.5319236524423024E-5,{"$error":"#N/A"},null,{"$f":"(AP4906)*$G$11*Bodencharakterisierung!$E$8","v":6.7253026398458488E-9},{"$f":"IF(AF4906<=$J$9*1.05,(AV4906*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4905,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.666936959997905,null,9.3002475489729883E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.854168439902935]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4890,7.1948744025947068E-21,{"$f":"Z4907*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.121040271364935E-21},{"$f":"AF4906*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4907^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4907)*3600*24","v":0},0,{"$f":"AE4906-AD4907*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4907>$J$18,(AE4907/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.121040271364935E-21,{"$error":"#N/A"},null,{"$f":"(AD4907)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4907>0,(AJ4907*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4906,NA())","v":{"$error":"#N/A"}},null,4890,{"$f":"IF(AF4907<=$J$9*0.05,AS4906*EXP((-$J$6*1)/Heterogenität!$D$4),Z4907)","v":4.4854168439902937E-5},{"$f":"IF(OR(AF4907>=$J$19, AR4906/$J$5<AN4907),0, Bodencharakterisierung!$E$8*$J$11*((AR4906/$J$5)-AN4907))","v":2.8201203710460259E-6},4.6506808452008739E-7,{"$f":"AQ4906-AP4907*Bodencharakterisierung!$E$8","v":1.4074527789904913E-4},{"$f":"AQ4907/(Bodencharakterisierung!$E$11*1000)","v":9.2901173530725498E-8},4.5319236524423024E-5,{"$error":"#N/A"},null,{"$f":"(AP4907)*$G$11*Bodencharakterisierung!$E$8","v":6.7253026398458488E-9},{"$f":"IF(AF4907<=$J$9*1.05,(AV4907*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4906,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.673209599997904,null,9.2901173530725495E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.854168439902935]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4891,7.121040271364935E-21,{"$f":"Z4908*EXP((-$J$6/Heterogenität!$D$4)*1)","v":7.047963829377451E-21},{"$f":"AF4907*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4908^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4908)*3600*24","v":0},0,{"$f":"AE4907-AD4908*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4908>$J$18,(AE4908/(Bodencharakterisierung!$E$11*1000)),0)","v":0},7.047963829377451E-21,{"$error":"#N/A"},null,{"$f":"(AD4908)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4908>0,(AJ4908*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4907,NA())","v":{"$error":"#N/A"}},null,4891,{"$f":"IF(AF4908<=$J$9*0.05,AS4907*EXP((-$J$6*1)/Heterogenität!$D$4),Z4908)","v":4.4854168439902937E-5},{"$f":"IF(OR(AF4908>=$J$19, AR4907/$J$5<AN4908),0, Bodencharakterisierung!$E$8*$J$11*((AR4907/$J$5)-AN4908))","v":2.3395614976858815E-6},4.6506808452008739E-7,{"$f":"AQ4907-AP4908*Bodencharakterisierung!$E$8","v":1.405918054311575E-4},{"$f":"AQ4908/(Bodencharakterisierung!$E$11*1000)","v":9.2799871571721119E-8},4.5319236524423024E-5,{"$error":"#N/A"},null,{"$f":"(AP4908)*$G$11*Bodencharakterisierung!$E$8","v":6.7253026398458488E-9},{"$f":"IF(AF4908<=$J$9*1.05,(AV4908*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4907,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.679482239997903,null,9.2799871571721121E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.854168439902935]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4892,7.047963829377451E-21,{"$f":"Z4909*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.9756373011904866E-21},{"$f":"AF4908*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4909^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4909)*3600*24","v":0},0,{"$f":"AE4908-AD4909*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4909>$J$18,(AE4909/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.9756373011904866E-21,{"$error":"#N/A"},null,{"$f":"(AD4909)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4909>0,(AJ4909*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4908,NA())","v":{"$error":"#N/A"}},null,4892,{"$f":"IF(AF4909<=$J$9*0.05,AS4908*EXP((-$J$6*1)/Heterogenität!$D$4),Z4909)","v":4.4854168439902937E-5},{"$f":"IF(OR(AF4909>=$J$19, AR4908/$J$5<AN4909),0, Bodencharakterisierung!$E$8*$J$11*((AR4908/$J$5)-AN4909))","v":1.8590026243258035E-6},4.6506808452008739E-7,{"$f":"AQ4908-AP4909*Bodencharakterisierung!$E$8","v":1.4043833296326587E-4},{"$f":"AQ4909/(Bodencharakterisierung!$E$11*1000)","v":9.2698569612716741E-8},4.5319236524423024E-5,{"$error":"#N/A"},null,{"$f":"(AP4909)*$G$11*Bodencharakterisierung!$E$8","v":6.7253026398458488E-9},{"$f":"IF(AF4909<=$J$9*1.05,(AV4909*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4908,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.685754879997901,null,9.2698569612716747E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.854168439902935]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4893,6.9756373011904866E-21,{"$f":"Z4910*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.904052991154213E-21},{"$f":"AF4909*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4910^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4910)*3600*24","v":0},0,{"$f":"AE4909-AD4910*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4910>$J$18,(AE4910/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.904052991154213E-21,{"$error":"#N/A"},null,{"$f":"(AD4910)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4910>0,(AJ4910*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4909,NA())","v":{"$error":"#N/A"}},null,4893,{"$f":"IF(AF4910<=$J$9*0.05,AS4909*EXP((-$J$6*1)/Heterogenität!$D$4),Z4910)","v":4.4854168439902937E-5},{"$f":"IF(OR(AF4910>=$J$19, AR4909/$J$5<AN4910),0, Bodencharakterisierung!$E$8*$J$11*((AR4909/$J$5)-AN4910))","v":1.3784437509657254E-6},4.6506808452008739E-7,{"$f":"AQ4909-AP4910*Bodencharakterisierung!$E$8","v":1.4028486049537424E-4},{"$f":"AQ4910/(Bodencharakterisierung!$E$11*1000)","v":9.2597267653712375E-8},4.5319236524423024E-5,{"$error":"#N/A"},null,{"$f":"(AP4910)*$G$11*Bodencharakterisierung!$E$8","v":6.7253026398458488E-9},{"$f":"IF(AF4910<=$J$9*1.05,(AV4910*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4909,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.6920275199979,null,9.2597267653712373E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.854168439902935]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4894,6.904052991154213E-21,{"$f":"Z4911*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.833203282591914E-21},{"$f":"AF4910*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4911^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4911)*3600*24","v":0},0,{"$f":"AE4910-AD4911*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4911>$J$18,(AE4911/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.833203282591914E-21,{"$error":"#N/A"},null,{"$f":"(AD4911)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4911>0,(AJ4911*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4910,NA())","v":{"$error":"#N/A"}},null,4894,{"$f":"IF(AF4911<=$J$9*0.05,AS4910*EXP((-$J$6*1)/Heterogenität!$D$4),Z4911)","v":4.4854168439902937E-5},{"$f":"IF(OR(AF4911>=$J$19, AR4910/$J$5<AN4911),0, Bodencharakterisierung!$E$8*$J$11*((AR4910/$J$5)-AN4911))","v":8.9788487760564751E-7},4.6506808452008739E-7,{"$f":"AQ4910-AP4911*Bodencharakterisierung!$E$8","v":1.4013138802748261E-4},{"$f":"AQ4911/(Bodencharakterisierung!$E$11*1000)","v":9.2495965694707997E-8},4.5319236524423024E-5,{"$error":"#N/A"},null,{"$f":"(AP4911)*$G$11*Bodencharakterisierung!$E$8","v":6.7253026398458488E-9},{"$f":"IF(AF4911<=$J$9*1.05,(AV4911*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4910,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.698300159997899,null,9.2495965694707999E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.854168439902935]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4895,6.833203282591914E-21,{"$f":"Z4912*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.76308063698956E-21},{"$f":"AF4911*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4912^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4912)*3600*24","v":0},0,{"$f":"AE4911-AD4912*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4912>$J$18,(AE4912/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.76308063698956E-21,{"$error":"#N/A"},null,{"$f":"(AD4912)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4912>0,(AJ4912*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4911,NA())","v":{"$error":"#N/A"}},null,4895,{"$f":"IF(AF4912<=$J$9*0.05,AS4911*EXP((-$J$6*1)/Heterogenität!$D$4),Z4912)","v":4.4854168439902937E-5},{"$f":"IF(OR(AF4912>=$J$19, AR4911/$J$5<AN4912),0, Bodencharakterisierung!$E$8*$J$11*((AR4911/$J$5)-AN4912))","v":4.1732600424556957E-7},4.1732600424556957E-7,{"$f":"AQ4911-AP4912*Bodencharakterisierung!$E$8","v":1.3999367044608159E-4},{"$f":"AQ4912/(Bodencharakterisierung!$E$11*1000)","v":9.2405063000713919E-8},4.5271494444148508E-5,{"$error":"#N/A"},null,{"$f":"(AP4912)*$G$11*Bodencharakterisierung!$E$8","v":6.0349092346882466E-9},{"$f":"IF(AF4912<=$J$9*1.05,(AV4912*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4911,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.704572799997898,null,9.2405063000713925E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.854168439902935]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4896,6.76308063698956E-21,{"$f":"Z4913*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.6936775931936968E-21},{"$f":"AF4912*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4913^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4913)*3600*24","v":0},0,{"$f":"AE4912-AD4913*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4913>$J$18,(AE4913/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.6936775931936968E-21,{"$error":"#N/A"},null,{"$f":"(AD4913)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4913>0,(AJ4913*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4912,NA())","v":{"$error":"#N/A"}},null,4896,{"$f":"IF(AF4913<=$J$9*0.05,AS4912*EXP((-$J$6*1)/Heterogenität!$D$4),Z4913)","v":4.480691629104667E-5},{"$f":"IF(OR(AF4913>=$J$19, AR4912/$J$5<AN4913),0, Bodencharakterisierung!$E$8*$J$11*((AR4912/$J$5)-AN4913))","v":4.4790275411226783E-7},4.4790275411226783E-7,{"$f":"AQ4912-AP4913*Bodencharakterisierung!$E$8","v":1.3984586253722455E-4},{"$f":"AQ4913/(Bodencharakterisierung!$E$11*1000)","v":9.230750002457066E-8},4.5254819045158936E-5,{"$error":"#N/A"},null,{"$f":"(AP4913)*$G$11*Bodencharakterisierung!$E$8","v":6.4770765289858399E-9},{"$f":"IF(AF4913<=$J$9*1.05,(AV4913*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4912,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.710845439997897,null,9.2307500024570666E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.806916291046669]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4897,6.6936775931936968E-21,{"$f":"Z4914*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.6249867666175702E-21},{"$f":"AF4913*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4914^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4914)*3600*24","v":0},0,{"$f":"AE4913-AD4914*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4914>$J$18,(AE4914/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.6249867666175702E-21,{"$error":"#N/A"},null,{"$f":"(AD4914)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4914>0,(AJ4914*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4913,NA())","v":{"$error":"#N/A"}},null,4897,{"$f":"IF(AF4914<=$J$9*0.05,AS4913*EXP((-$J$6*1)/Heterogenität!$D$4),Z4914)","v":4.4790412015766621E-5},{"$f":"IF(OR(AF4914>=$J$19, AR4913/$J$5<AN4914),0, Bodencharakterisierung!$E$8*$J$11*((AR4913/$J$5)-AN4914))","v":1.4638006543030165E-7},1.4638006543030165E-7,{"$f":"AQ4913-AP4914*Bodencharakterisierung!$E$8","v":1.3979755711563253E-4},{"$f":"AQ4914/(Bodencharakterisierung!$E$11*1000)","v":9.2275615257843253E-8},4.4936792081196922E-5,{"$error":"#N/A"},null,{"$f":"(AP4914)*$G$11*Bodencharakterisierung!$E$8","v":2.1167873548559858E-9},{"$f":"IF(AF4914<=$J$9*1.05,(AV4914*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4913,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.717118079997896,null,9.2275615257843252E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.79041201576662]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4898,6.6249867666175702E-21,{"$f":"Z4915*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.5570008484553938E-21},{"$f":"AF4914*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4915^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4915)*3600*24","v":0},0,{"$f":"AE4914-AD4915*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4915>$J$18,(AE4915/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.5570008484553938E-21,{"$error":"#N/A"},null,{"$f":"(AD4915)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4915>0,(AJ4915*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4914,NA())","v":{"$error":"#N/A"}},null,4898,{"$f":"IF(AF4915<=$J$9*0.05,AS4914*EXP((-$J$6*1)/Heterogenität!$D$4),Z4915)","v":4.447564865910028E-5},{"$f":"IF(OR(AF4915>=$J$19, AR4914/$J$5<AN4915),0, Bodencharakterisierung!$E$8*$J$11*((AR4914/$J$5)-AN4915))","v":3.0713603069462516E-6},4.611434220966421E-7,{"$f":"AQ4914-AP4915*Bodencharakterisierung!$E$8","v":1.3964537978634065E-4},{"$f":"AQ4915/(Bodencharakterisierung!$E$11*1000)","v":9.2175168175802407E-8},4.4936792081196922E-5,{"$error":"#N/A"},null,{"$f":"(AP4915)*$G$11*Bodencharakterisierung!$E$8","v":6.6685484925812884E-9},{"$f":"IF(AF4915<=$J$9*1.05,(AV4915*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4914,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.723390719997894,null,9.2175168175802402E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.47564865910028]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4899,6.5570008484553938E-21,{"$f":"Z4916*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.4897126049046812E-21},{"$f":"AF4915*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4916^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4916)*3600*24","v":0},0,{"$f":"AE4915-AD4916*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4916>$J$18,(AE4916/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.4897126049046812E-21,{"$error":"#N/A"},null,{"$f":"(AD4916)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4916>0,(AJ4916*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4915,NA())","v":{"$error":"#N/A"}},null,4899,{"$f":"IF(AF4916<=$J$9*0.05,AS4915*EXP((-$J$6*1)/Heterogenität!$D$4),Z4916)","v":4.447564865910028E-5},{"$f":"IF(OR(AF4916>=$J$19, AR4915/$J$5<AN4916),0, Bodencharakterisierung!$E$8*$J$11*((AR4915/$J$5)-AN4916))","v":2.5948568212064227E-6},4.611434220966421E-7,{"$f":"AQ4915-AP4916*Bodencharakterisierung!$E$8","v":1.3949320245704877E-4},{"$f":"AQ4916/(Bodencharakterisierung!$E$11*1000)","v":9.207472109376156E-8},4.4936792081196922E-5,{"$error":"#N/A"},null,{"$f":"(AP4916)*$G$11*Bodencharakterisierung!$E$8","v":6.6685484925812884E-9},{"$f":"IF(AF4916<=$J$9*1.05,(AV4916*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4915,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.729663359997893,null,9.2074721093761566E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.47564865910028]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4900,6.4897126049046812E-21,{"$f":"Z4917*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.4231148763965592E-21},{"$f":"AF4916*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4917^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4917)*3600*24","v":0},0,{"$f":"AE4916-AD4917*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4917>$J$18,(AE4917/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.4231148763965592E-21,{"$error":"#N/A"},null,{"$f":"(AD4917)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4917>0,(AJ4917*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4916,NA())","v":{"$error":"#N/A"}},null,4900,{"$f":"IF(AF4917<=$J$9*0.05,AS4916*EXP((-$J$6*1)/Heterogenität!$D$4),Z4917)","v":4.447564865910028E-5},{"$f":"IF(OR(AF4917>=$J$19, AR4916/$J$5<AN4917),0, Bodencharakterisierung!$E$8*$J$11*((AR4916/$J$5)-AN4917))","v":2.1183533354665938E-6},4.611434220966421E-7,{"$f":"AQ4916-AP4917*Bodencharakterisierung!$E$8","v":1.3934102512775688E-4},{"$f":"AQ4917/(Bodencharakterisierung!$E$11*1000)","v":9.1974274011720714E-8},4.4936792081196922E-5,{"$error":"#N/A"},null,{"$f":"(AP4917)*$G$11*Bodencharakterisierung!$E$8","v":6.6685484925812884E-9},{"$f":"IF(AF4917<=$J$9*1.05,(AV4917*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4916,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.735935999997892,null,9.1974274011720716E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.47564865910028]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4901,6.4231148763965592E-21,{"$f":"Z4918*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.3572005768339798E-21},{"$f":"AF4917*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4918^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4918)*3600*24","v":0},0,{"$f":"AE4917-AD4918*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4918>$J$18,(AE4918/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.3572005768339798E-21,{"$error":"#N/A"},null,{"$f":"(AD4918)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4918>0,(AJ4918*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4917,NA())","v":{"$error":"#N/A"}},null,4901,{"$f":"IF(AF4918<=$J$9*0.05,AS4917*EXP((-$J$6*1)/Heterogenität!$D$4),Z4918)","v":4.447564865910028E-5},{"$f":"IF(OR(AF4918>=$J$19, AR4917/$J$5<AN4918),0, Bodencharakterisierung!$E$8*$J$11*((AR4917/$J$5)-AN4918))","v":1.6418498497267646E-6},4.611434220966421E-7,{"$f":"AQ4917-AP4918*Bodencharakterisierung!$E$8","v":1.39188847798465E-4},{"$f":"AQ4918/(Bodencharakterisierung!$E$11*1000)","v":9.1873826929679868E-8},4.4936792081196922E-5,{"$error":"#N/A"},null,{"$f":"(AP4918)*$G$11*Bodencharakterisierung!$E$8","v":6.6685484925812884E-9},{"$f":"IF(AF4918<=$J$9*1.05,(AV4918*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4917,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.742208639997891,null,9.1873826929679867E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.47564865910028]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4902,6.3572005768339798E-21,{"$f":"Z4919*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.2919626928377465E-21},{"$f":"AF4918*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4919^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4919)*3600*24","v":0},0,{"$f":"AE4918-AD4919*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4919>$J$18,(AE4919/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.2919626928377465E-21,{"$error":"#N/A"},null,{"$f":"(AD4919)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4919>0,(AJ4919*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4918,NA())","v":{"$error":"#N/A"}},null,4902,{"$f":"IF(AF4919<=$J$9*0.05,AS4918*EXP((-$J$6*1)/Heterogenität!$D$4),Z4919)","v":4.447564865910028E-5},{"$f":"IF(OR(AF4919>=$J$19, AR4918/$J$5<AN4919),0, Bodencharakterisierung!$E$8*$J$11*((AR4918/$J$5)-AN4919))","v":1.1653463639869357E-6},4.611434220966421E-7,{"$f":"AQ4918-AP4919*Bodencharakterisierung!$E$8","v":1.3903667046917312E-4},{"$f":"AQ4919/(Bodencharakterisierung!$E$11*1000)","v":9.1773379847639022E-8},4.4936792081196922E-5,{"$error":"#N/A"},null,{"$f":"(AP4919)*$G$11*Bodencharakterisierung!$E$8","v":6.6685484925812884E-9},{"$f":"IF(AF4919<=$J$9*1.05,(AV4919*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4918,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.74848127999789,null,9.1773379847639017E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.47564865910028]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4903,6.2919626928377465E-21,{"$f":"Z4920*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.2273942830002827E-21},{"$f":"AF4919*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4920^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4920)*3600*24","v":0},0,{"$f":"AE4919-AD4920*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4920>$J$18,(AE4920/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.2273942830002827E-21,{"$error":"#N/A"},null,{"$f":"(AD4920)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4920>0,(AJ4920*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4919,NA())","v":{"$error":"#N/A"}},null,4903,{"$f":"IF(AF4920<=$J$9*0.05,AS4919*EXP((-$J$6*1)/Heterogenität!$D$4),Z4920)","v":4.447564865910028E-5},{"$f":"IF(OR(AF4920>=$J$19, AR4919/$J$5<AN4920),0, Bodencharakterisierung!$E$8*$J$11*((AR4919/$J$5)-AN4920))","v":6.8884287824717287E-7},4.611434220966421E-7,{"$f":"AQ4919-AP4920*Bodencharakterisierung!$E$8","v":1.3888449313988123E-4},{"$f":"AQ4920/(Bodencharakterisierung!$E$11*1000)","v":9.1672932765598175E-8},4.4936792081196922E-5,{"$error":"#N/A"},null,{"$f":"(AP4920)*$G$11*Bodencharakterisierung!$E$8","v":6.6685484925812884E-9},{"$f":"IF(AF4920<=$J$9*1.05,(AV4920*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4919,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.754753919997889,null,9.1672932765598181E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.47564865910028]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4904,6.2273942830002827E-21,{"$f":"Z4921*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.1634884771470549E-21},{"$f":"AF4920*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4921^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4921)*3600*24","v":0},0,{"$f":"AE4920-AD4921*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4921>$J$18,(AE4921/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.1634884771470549E-21,{"$error":"#N/A"},null,{"$f":"(AD4921)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4921>0,(AJ4921*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4920,NA())","v":{"$error":"#N/A"}},null,4904,{"$f":"IF(AF4921<=$J$9*0.05,AS4920*EXP((-$J$6*1)/Heterogenität!$D$4),Z4921)","v":4.447564865910028E-5},{"$f":"IF(OR(AF4921>=$J$19, AR4920/$J$5<AN4921),0, Bodencharakterisierung!$E$8*$J$11*((AR4920/$J$5)-AN4921))","v":2.1233939250734394E-7},2.1233939250734394E-7,{"$f":"AQ4920-AP4921*Bodencharakterisierung!$E$8","v":1.3881442114035381E-4},{"$f":"AQ4921/(Bodencharakterisierung!$E$11*1000)","v":9.1626680620695587E-8},4.468798805160762E-5,{"$error":"#N/A"},null,{"$f":"(AP4921)*$G$11*Bodencharakterisierung!$E$8","v":3.0706185277076854E-9},{"$f":"IF(AF4921<=$J$9*1.05,(AV4921*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4920,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.761026559997887,null,9.162668062069558E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.47564865910028]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4905,6.1634884771470549E-21,{"$f":"Z4922*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.1002384756055758E-21},{"$f":"AF4921*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4922^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4922)*3600*24","v":0},0,{"$f":"AE4921-AD4922*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4922>$J$18,(AE4922/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.1002384756055758E-21,{"$error":"#N/A"},null,{"$f":"(AD4922)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4922>0,(AJ4922*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4921,NA())","v":{"$error":"#N/A"}},null,4905,{"$f":"IF(AF4922<=$J$9*0.05,AS4921*EXP((-$J$6*1)/Heterogenität!$D$4),Z4922)","v":4.4229397867878081E-5},{"$f":"IF(OR(AF4922>=$J$19, AR4921/$J$5<AN4922),0, Bodencharakterisierung!$E$8*$J$11*((AR4921/$J$5)-AN4922))","v":2.3995782907233671E-6},4.5859018372953911E-7,{"$f":"AQ4921-AP4922*Bodencharakterisierung!$E$8","v":1.3866308637972306E-4},{"$f":"AQ4922/(Bodencharakterisierung!$E$11*1000)","v":9.1526789689586184E-8},4.468798805160762E-5,{"$error":"#N/A"},null,{"$f":"(AP4922)*$G$11*Bodencharakterisierung!$E$8","v":6.6316263702039744E-9},{"$f":"IF(AF4922<=$J$9*1.05,(AV4922*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4921,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.767299199997886,null,9.1526789689586177E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.229397867878085]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4906,6.1002384756055758E-21,{"$f":"Z4923*EXP((-$J$6/Heterogenität!$D$4)*1)","v":6.0376375484819092E-21},{"$f":"AF4922*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4923^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4923)*3600*24","v":0},0,{"$f":"AE4922-AD4923*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4923>$J$18,(AE4923/(Bodencharakterisierung!$E$11*1000)),0)","v":0},6.0376375484819092E-21,{"$error":"#N/A"},null,{"$f":"(AD4923)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4923>0,(AJ4923*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4922,NA())","v":{"$error":"#N/A"}},null,4906,{"$f":"IF(AF4923<=$J$9*0.05,AS4922*EXP((-$J$6*1)/Heterogenität!$D$4),Z4923)","v":4.4229397867878081E-5},{"$f":"IF(OR(AF4923>=$J$19, AR4922/$J$5<AN4923),0, Bodencharakterisierung!$E$8*$J$11*((AR4922/$J$5)-AN4923))","v":1.9257130882671056E-6},4.5859018372953911E-7,{"$f":"AQ4922-AP4923*Bodencharakterisierung!$E$8","v":1.3851175161909231E-4},{"$f":"AQ4923/(Bodencharakterisierung!$E$11*1000)","v":9.142689875847678E-8},4.468798805160762E-5,{"$error":"#N/A"},null,{"$f":"(AP4923)*$G$11*Bodencharakterisierung!$E$8","v":6.6316263702039744E-9},{"$f":"IF(AF4923<=$J$9*1.05,(AV4923*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4922,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.773571839997885,null,9.1426898758476774E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.229397867878085]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4907,6.0376375484819092E-21,{"$f":"Z4924*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.9756790349445993E-21},{"$f":"AF4923*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4924^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4924)*3600*24","v":0},0,{"$f":"AE4923-AD4924*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4924>$J$18,(AE4924/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.9756790349445993E-21,{"$error":"#N/A"},null,{"$f":"(AD4924)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4924>0,(AJ4924*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4923,NA())","v":{"$error":"#N/A"}},null,4907,{"$f":"IF(AF4924<=$J$9*0.05,AS4923*EXP((-$J$6*1)/Heterogenität!$D$4),Z4924)","v":4.4229397867878081E-5},{"$f":"IF(OR(AF4924>=$J$19, AR4923/$J$5<AN4924),0, Bodencharakterisierung!$E$8*$J$11*((AR4923/$J$5)-AN4924))","v":1.4518478858108439E-6},4.5859018372953911E-7,{"$f":"AQ4923-AP4924*Bodencharakterisierung!$E$8","v":1.3836041685846156E-4},{"$f":"AQ4924/(Bodencharakterisierung!$E$11*1000)","v":9.1327007827367364E-8},4.468798805160762E-5,{"$error":"#N/A"},null,{"$f":"(AP4924)*$G$11*Bodencharakterisierung!$E$8","v":6.6316263702039744E-9},{"$f":"IF(AF4924<=$J$9*1.05,(AV4924*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4923,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.779844479997884,null,9.1327007827367357E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.229397867878085]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4908,5.9756790349445993E-21,{"$f":"Z4925*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.9143563425159473E-21},{"$f":"AF4924*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4925^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4925)*3600*24","v":0},0,{"$f":"AE4924-AD4925*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4925>$J$18,(AE4925/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.9143563425159473E-21,{"$error":"#N/A"},null,{"$f":"(AD4925)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4925>0,(AJ4925*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4924,NA())","v":{"$error":"#N/A"}},null,4908,{"$f":"IF(AF4925<=$J$9*0.05,AS4924*EXP((-$J$6*1)/Heterogenität!$D$4),Z4925)","v":4.4229397867878081E-5},{"$f":"IF(OR(AF4925>=$J$19, AR4924/$J$5<AN4925),0, Bodencharakterisierung!$E$8*$J$11*((AR4924/$J$5)-AN4925))","v":9.7798268335451608E-7},4.5859018372953911E-7,{"$f":"AQ4924-AP4925*Bodencharakterisierung!$E$8","v":1.3820908209783082E-4},{"$f":"AQ4925/(Bodencharakterisierung!$E$11*1000)","v":9.122711689625796E-8},4.468798805160762E-5,{"$error":"#N/A"},null,{"$f":"(AP4925)*$G$11*Bodencharakterisierung!$E$8","v":6.6316263702039744E-9},{"$f":"IF(AF4925<=$J$9*1.05,(AV4925*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4924,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.786117119997883,null,9.1227116896257954E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.229397867878085]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4909,5.9143563425159473E-21,{"$f":"Z4926*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.8536629463705645E-21},{"$f":"AF4925*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4926^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4926)*3600*24","v":0},0,{"$f":"AE4925-AD4926*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4926>$J$18,(AE4926/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.8536629463705645E-21,{"$error":"#N/A"},null,{"$f":"(AD4926)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4926>0,(AJ4926*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4925,NA())","v":{"$error":"#N/A"}},null,4909,{"$f":"IF(AF4926<=$J$9*0.05,AS4925*EXP((-$J$6*1)/Heterogenität!$D$4),Z4926)","v":4.4229397867878081E-5},{"$f":"IF(OR(AF4926>=$J$19, AR4925/$J$5<AN4926),0, Bodencharakterisierung!$E$8*$J$11*((AR4925/$J$5)-AN4926))","v":5.0411748089825457E-7},4.5859018372953911E-7,{"$f":"AQ4925-AP4926*Bodencharakterisierung!$E$8","v":1.3805774733720007E-4},{"$f":"AQ4926/(Bodencharakterisierung!$E$11*1000)","v":9.1127225965148557E-8},4.468798805160762E-5,{"$error":"#N/A"},null,{"$f":"(AP4926)*$G$11*Bodencharakterisierung!$E$8","v":6.6316263702039744E-9},{"$f":"IF(AF4926<=$J$9*1.05,(AV4926*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4925,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.792389759997882,null,9.1127225965148551E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.229397867878085]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4910,5.8536629463705645E-21,{"$f":"Z4927*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.793592388641119E-21},{"$f":"AF4926*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4927^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4927)*3600*24","v":0},0,{"$f":"AE4926-AD4927*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4927>$J$18,(AE4927/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.793592388641119E-21,{"$error":"#N/A"},null,{"$f":"(AD4927)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4927>0,(AJ4927*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4926,NA())","v":{"$error":"#N/A"}},null,4910,{"$f":"IF(AF4927<=$J$9*0.05,AS4926*EXP((-$J$6*1)/Heterogenität!$D$4),Z4927)","v":4.4229397867878081E-5},{"$f":"IF(OR(AF4927>=$J$19, AR4926/$J$5<AN4927),0, Bodencharakterisierung!$E$8*$J$11*((AR4926/$J$5)-AN4927))","v":3.0252278441993036E-8},3.0252278441993036E-8,{"$f":"AQ4926-AP4927*Bodencharakterisierung!$E$8","v":1.380477640853142E-4},{"$f":"AQ4927/(Bodencharakterisierung!$E$11*1000)","v":9.1120636359943371E-8},4.4259650146320072E-5,{"$error":"#N/A"},null,{"$f":"(AP4927)*$G$11*Bodencharakterisierung!$E$8","v":4.374751457676079E-10},{"$f":"IF(AF4927<=$J$9*1.05,(AV4927*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4926,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.79866239999788,null,9.1120636359943372E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,44.229397867878085]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4911,5.793592388641119E-21,{"$f":"Z4928*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.7341382777312096E-21},{"$f":"AF4927*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4928^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4928)*3600*24","v":0},0,{"$f":"AE4927-AD4928*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4928>$J$18,(AE4928/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.7341382777312096E-21,{"$error":"#N/A"},null,{"$f":"(AD4928)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4928>0,(AJ4928*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4927,NA())","v":{"$error":"#N/A"}},null,4911,{"$f":"IF(AF4928<=$J$9*0.05,AS4927*EXP((-$J$6*1)/Heterogenität!$D$4),Z4928)","v":4.3805455585827302E-5},{"$f":"IF(OR(AF4928>=$J$19, AR4927/$J$5<AN4928),0, Bodencharakterisierung!$E$8*$J$11*((AR4927/$J$5)-AN4928))","v":4.1422526459797031E-6},4.541945604927703E-7,{"$f":"AQ4927-AP4928*Bodencharakterisierung!$E$8","v":1.3789787988035157E-4},{"$f":"AQ4928/(Bodencharakterisierung!$E$11*1000)","v":9.1021702891321174E-8},4.4259650146320072E-5,{"$error":"#N/A"},null,{"$f":"(AP4928)*$G$11*Bodencharakterisierung!$E$8","v":6.568061706142981E-9},{"$f":"IF(AF4928<=$J$9*1.05,(AV4928*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4927,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.804935039997879,null,9.102170289132118E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.805455585827303]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4912,5.7341382777312096E-21,{"$f":"Z4929*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.6752942876352905E-21},{"$f":"AF4928*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4929^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4929)*3600*24","v":0},0,{"$f":"AE4928-AD4929*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4929>$J$18,(AE4929/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.6752942876352905E-21,{"$error":"#N/A"},null,{"$f":"(AD4929)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4929>0,(AJ4929*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4928,NA())","v":{"$error":"#N/A"}},null,4912,{"$f":"IF(AF4929<=$J$9*0.05,AS4928*EXP((-$J$6*1)/Heterogenität!$D$4),Z4929)","v":4.3805455585827302E-5},{"$f":"IF(OR(AF4929>=$J$19, AR4928/$J$5<AN4929),0, Bodencharakterisierung!$E$8*$J$11*((AR4928/$J$5)-AN4929))","v":3.6729294790245821E-6},4.541945604927703E-7,{"$f":"AQ4928-AP4929*Bodencharakterisierung!$E$8","v":1.3774799567538895E-4},{"$f":"AQ4929/(Bodencharakterisierung!$E$11*1000)","v":9.0922769422698976E-8},4.4259650146320072E-5,{"$error":"#N/A"},null,{"$f":"(AP4929)*$G$11*Bodencharakterisierung!$E$8","v":6.568061706142981E-9},{"$f":"IF(AF4929<=$J$9*1.05,(AV4929*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4928,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.811207679997878,null,9.0922769422698974E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.805455585827303]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4913,5.6752942876352905E-21,{"$f":"Z4930*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.6170541572655758E-21},{"$f":"AF4929*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4930^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4930)*3600*24","v":0},0,{"$f":"AE4929-AD4930*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4930>$J$18,(AE4930/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.6170541572655758E-21,{"$error":"#N/A"},null,{"$f":"(AD4930)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4930>0,(AJ4930*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4929,NA())","v":{"$error":"#N/A"}},null,4913,{"$f":"IF(AF4930<=$J$9*0.05,AS4929*EXP((-$J$6*1)/Heterogenität!$D$4),Z4930)","v":4.3805455585827302E-5},{"$f":"IF(OR(AF4930>=$J$19, AR4929/$J$5<AN4930),0, Bodencharakterisierung!$E$8*$J$11*((AR4929/$J$5)-AN4930))","v":3.2036063120695272E-6},4.541945604927703E-7,{"$f":"AQ4929-AP4930*Bodencharakterisierung!$E$8","v":1.3759811147042632E-4},{"$f":"AQ4930/(Bodencharakterisierung!$E$11*1000)","v":9.0823835954076779E-8},4.4259650146320072E-5,{"$error":"#N/A"},null,{"$f":"(AP4930)*$G$11*Bodencharakterisierung!$E$8","v":6.568061706142981E-9},{"$f":"IF(AF4930<=$J$9*1.05,(AV4930*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4929,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.817480319997877,null,9.0823835954076781E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.805455585827303]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4914,5.6170541572655758E-21,{"$f":"Z4931*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.5594116897858494E-21},{"$f":"AF4930*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4931^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4931)*3600*24","v":0},0,{"$f":"AE4930-AD4931*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4931>$J$18,(AE4931/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.5594116897858494E-21,{"$error":"#N/A"},null,{"$f":"(AD4931)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4931>0,(AJ4931*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4930,NA())","v":{"$error":"#N/A"}},null,4914,{"$f":"IF(AF4931<=$J$9*0.05,AS4930*EXP((-$J$6*1)/Heterogenität!$D$4),Z4931)","v":4.3805455585827302E-5},{"$f":"IF(OR(AF4931>=$J$19, AR4930/$J$5<AN4931),0, Bodencharakterisierung!$E$8*$J$11*((AR4930/$J$5)-AN4931))","v":2.7342831451144057E-6},4.541945604927703E-7,{"$f":"AQ4930-AP4931*Bodencharakterisierung!$E$8","v":1.3744822726546369E-4},{"$f":"AQ4931/(Bodencharakterisierung!$E$11*1000)","v":9.0724902485454582E-8},4.4259650146320072E-5,{"$error":"#N/A"},null,{"$f":"(AP4931)*$G$11*Bodencharakterisierung!$E$8","v":6.568061706142981E-9},{"$f":"IF(AF4931<=$J$9*1.05,(AV4931*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4930,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.823752959997876,null,9.0724902485454575E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.805455585827303]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4915,5.5594116897858494E-21,{"$f":"Z4932*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.5023607519521124E-21},{"$f":"AF4931*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4932^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4932)*3600*24","v":0},0,{"$f":"AE4931-AD4932*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4932>$J$18,(AE4932/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.5023607519521124E-21,{"$error":"#N/A"},null,{"$f":"(AD4932)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4932>0,(AJ4932*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4931,NA())","v":{"$error":"#N/A"}},null,4915,{"$f":"IF(AF4932<=$J$9*0.05,AS4931*EXP((-$J$6*1)/Heterogenität!$D$4),Z4932)","v":4.3805455585827302E-5},{"$f":"IF(OR(AF4932>=$J$19, AR4931/$J$5<AN4932),0, Bodencharakterisierung!$E$8*$J$11*((AR4931/$J$5)-AN4932))","v":2.2649599781593508E-6},4.541945604927703E-7,{"$f":"AQ4931-AP4932*Bodencharakterisierung!$E$8","v":1.3729834306050107E-4},{"$f":"AQ4932/(Bodencharakterisierung!$E$11*1000)","v":9.0625969016832385E-8},4.4259650146320072E-5,{"$error":"#N/A"},null,{"$f":"(AP4932)*$G$11*Bodencharakterisierung!$E$8","v":6.568061706142981E-9},{"$f":"IF(AF4932<=$J$9*1.05,(AV4932*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4931,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.830025599997875,null,9.0625969016832383E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.805455585827303]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4916,5.5023607519521124E-21,{"$f":"Z4933*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.4458952734599976E-21},{"$f":"AF4932*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4933^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4933)*3600*24","v":0},0,{"$f":"AE4932-AD4933*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4933>$J$18,(AE4933/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.4458952734599976E-21,{"$error":"#N/A"},null,{"$f":"(AD4933)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4933>0,(AJ4933*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4932,NA())","v":{"$error":"#N/A"}},null,4916,{"$f":"IF(AF4933<=$J$9*0.05,AS4932*EXP((-$J$6*1)/Heterogenität!$D$4),Z4933)","v":4.3805455585827302E-5},{"$f":"IF(OR(AF4933>=$J$19, AR4932/$J$5<AN4933),0, Bodencharakterisierung!$E$8*$J$11*((AR4932/$J$5)-AN4933))","v":1.7956368112042298E-6},4.541945604927703E-7,{"$f":"AQ4932-AP4933*Bodencharakterisierung!$E$8","v":1.3714845885553844E-4},{"$f":"AQ4933/(Bodencharakterisierung!$E$11*1000)","v":9.0527035548210187E-8},4.4259650146320072E-5,{"$error":"#N/A"},null,{"$f":"(AP4933)*$G$11*Bodencharakterisierung!$E$8","v":6.568061706142981E-9},{"$f":"IF(AF4933<=$J$9*1.05,(AV4933*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4932,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.836298239997873,null,9.0527035548210191E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.805455585827303]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4917,5.4458952734599976E-21,{"$f":"Z4934*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.3900092462988798E-21},{"$f":"AF4933*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4934^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4934)*3600*24","v":0},0,{"$f":"AE4933-AD4934*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4934>$J$18,(AE4934/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.3900092462988798E-21,{"$error":"#N/A"},null,{"$f":"(AD4934)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4934>0,(AJ4934*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4933,NA())","v":{"$error":"#N/A"}},null,4917,{"$f":"IF(AF4934<=$J$9*0.05,AS4933*EXP((-$J$6*1)/Heterogenität!$D$4),Z4934)","v":4.3805455585827302E-5},{"$f":"IF(OR(AF4934>=$J$19, AR4933/$J$5<AN4934),0, Bodencharakterisierung!$E$8*$J$11*((AR4933/$J$5)-AN4934))","v":1.3263136442491749E-6},4.541945604927703E-7,{"$f":"AQ4933-AP4934*Bodencharakterisierung!$E$8","v":1.3699857465057581E-4},{"$f":"AQ4934/(Bodencharakterisierung!$E$11*1000)","v":9.042810207958799E-8},4.4259650146320072E-5,{"$error":"#N/A"},null,{"$f":"(AP4934)*$G$11*Bodencharakterisierung!$E$8","v":6.568061706142981E-9},{"$f":"IF(AF4934<=$J$9*1.05,(AV4934*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4933,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.842570879997872,null,9.0428102079587985E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.805455585827303]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4918,5.3900092462988798E-21,{"$f":"Z4935*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.3346967241126139E-21},{"$f":"AF4934*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4935^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4935)*3600*24","v":0},0,{"$f":"AE4934-AD4935*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4935>$J$18,(AE4935/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.3346967241126139E-21,{"$error":"#N/A"},null,{"$f":"(AD4935)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4935>0,(AJ4935*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4934,NA())","v":{"$error":"#N/A"}},null,4918,{"$f":"IF(AF4935<=$J$9*0.05,AS4934*EXP((-$J$6*1)/Heterogenität!$D$4),Z4935)","v":4.3805455585827302E-5},{"$f":"IF(OR(AF4935>=$J$19, AR4934/$J$5<AN4935),0, Bodencharakterisierung!$E$8*$J$11*((AR4934/$J$5)-AN4935))","v":8.5699047729405393E-7},4.541945604927703E-7,{"$f":"AQ4934-AP4935*Bodencharakterisierung!$E$8","v":1.3684869044561319E-4},{"$f":"AQ4935/(Bodencharakterisierung!$E$11*1000)","v":9.0329168610965806E-8},4.4259650146320072E-5,{"$error":"#N/A"},null,{"$f":"(AP4935)*$G$11*Bodencharakterisierung!$E$8","v":6.568061706142981E-9},{"$f":"IF(AF4935<=$J$9*1.05,(AV4935*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4934,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.848843519997871,null,9.0329168610965807E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.805455585827303]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4919,5.3346967241126139E-21,{"$f":"Z4936*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.2799518215668351E-21},{"$f":"AF4935*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4936^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4936)*3600*24","v":0},0,{"$f":"AE4935-AD4936*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4936>$J$18,(AE4936/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.2799518215668351E-21,{"$error":"#N/A"},null,{"$f":"(AD4936)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4936>0,(AJ4936*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4935,NA())","v":{"$error":"#N/A"}},null,4919,{"$f":"IF(AF4936<=$J$9*0.05,AS4935*EXP((-$J$6*1)/Heterogenität!$D$4),Z4936)","v":4.3805455585827302E-5},{"$f":"IF(OR(AF4936>=$J$19, AR4935/$J$5<AN4936),0, Bodencharakterisierung!$E$8*$J$11*((AR4935/$J$5)-AN4936))","v":3.8766731033906524E-7},3.8766731033906524E-7,{"$f":"AQ4935-AP4936*Bodencharakterisierung!$E$8","v":1.3672076023320129E-4},{"$f":"AQ4936/(Bodencharakterisierung!$E$11*1000)","v":9.0244726226535505E-8},4.419312289616637E-5,{"$error":"#N/A"},null,{"$f":"(AP4936)*$G$11*Bodencharakterisierung!$E$8","v":5.6060178549892414E-9},{"$f":"IF(AF4936<=$J$9*1.05,(AV4936*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4935,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.85511615999787,null,9.024472622653551E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.805455585827303]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4920,5.2799518215668351E-21,{"$f":"Z4937*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.2257687137227494E-21},{"$f":"AF4936*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4937^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4937)*3600*24","v":0},0,{"$f":"AE4936-AD4937*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4937>$J$18,(AE4937/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.2257687137227494E-21,{"$error":"#N/A"},null,{"$f":"(AD4937)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4937>0,(AJ4937*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4936,NA())","v":{"$error":"#N/A"}},null,4920,{"$f":"IF(AF4937<=$J$9*0.05,AS4936*EXP((-$J$6*1)/Heterogenität!$D$4),Z4937)","v":4.3739611041367036E-5},{"$f":"IF(OR(AF4937>=$J$19, AR4936/$J$5<AN4937),0, Bodencharakterisierung!$E$8*$J$11*((AR4936/$J$5)-AN4937))","v":6.3059730188375066E-7},4.5351185479933313E-7,{"$f":"AQ4936-AP4937*Bodencharakterisierung!$E$8","v":1.365711013211175E-4},{"$f":"AQ4937/(Bodencharakterisierung!$E$11*1000)","v":9.0145941466084157E-8},4.419312289616637E-5,{"$error":"#N/A"},null,{"$f":"(AP4937)*$G$11*Bodencharakterisierung!$E$8","v":6.5581891680025734E-9},{"$f":"IF(AF4937<=$J$9*1.05,(AV4937*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4936,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.861388799997869,null,9.0145941466084151E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.739611041367034]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4921,5.2257687137227494E-21,{"$f":"Z4938*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.1721416354173529E-21},{"$f":"AF4937*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4938^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4938)*3600*24","v":0},0,{"$f":"AE4937-AD4938*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4938>$J$18,(AE4938/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.1721416354173529E-21,{"$error":"#N/A"},null,{"$f":"(AD4938)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4938>0,(AJ4938*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4937,NA())","v":{"$error":"#N/A"}},null,4921,{"$f":"IF(AF4938<=$J$9*0.05,AS4937*EXP((-$J$6*1)/Heterogenität!$D$4),Z4938)","v":4.3739611041367036E-5},{"$f":"IF(OR(AF4938>=$J$19, AR4937/$J$5<AN4938),0, Bodencharakterisierung!$E$8*$J$11*((AR4937/$J$5)-AN4938))","v":1.6197958062529966E-7},1.6197958062529966E-7,{"$f":"AQ4937-AP4938*Bodencharakterisierung!$E$8","v":1.3651764805951115E-4},{"$f":"AQ4938/(Bodencharakterisierung!$E$11*1000)","v":9.0110658785155876E-8},4.3901590621992339E-5,{"$error":"#N/A"},null,{"$f":"(AP4938)*$G$11*Bodencharakterisierung!$E$8","v":2.3423703699310705E-9},{"$f":"IF(AF4938<=$J$9*1.05,(AV4938*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4937,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.867661439997867,null,9.0110658785155881E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.739611041367034]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4922,5.1721416354173529E-21,{"$f":"Z4939*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.1190648806500075E-21},{"$f":"AF4938*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4939^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4939)*3600*24","v":0},0,{"$f":"AE4938-AD4939*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4939>$J$18,(AE4939/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.1190648806500075E-21,{"$error":"#N/A"},null,{"$f":"(AD4939)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4939>0,(AJ4939*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4938,NA())","v":{"$error":"#N/A"}},null,4922,{"$f":"IF(AF4939<=$J$9*0.05,AS4938*EXP((-$J$6*1)/Heterogenität!$D$4),Z4939)","v":4.3451070484766462E-5},{"$f":"IF(OR(AF4939>=$J$19, AR4938/$J$5<AN4939),0, Bodencharakterisierung!$E$8*$J$11*((AR4938/$J$5)-AN4939))","v":2.8145608057437256E-6},4.5052013722587643E-7,{"$f":"AQ4938-AP4939*Bodencharakterisierung!$E$8","v":1.3636897641422662E-4},{"$f":"AQ4939/(Bodencharakterisierung!$E$11*1000)","v":9.0012525685958168E-8},4.3901590621992339E-5,{"$error":"#N/A"},null,{"$f":"(AP4939)*$G$11*Bodencharakterisierung!$E$8","v":6.5149262420694733E-9},{"$f":"IF(AF4939<=$J$9*1.05,(AV4939*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4938,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.873934079997866,null,9.0012525685958175E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.451070484766461]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4923,5.1190648806500075E-21,{"$f":"Z4940*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.0665328019753157E-21},{"$f":"AF4939*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4940^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4940)*3600*24","v":0},0,{"$f":"AE4939-AD4940*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4940>$J$18,(AE4940/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.0665328019753157E-21,{"$error":"#N/A"},null,{"$f":"(AD4940)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4940>0,(AJ4940*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4939,NA())","v":{"$error":"#N/A"}},null,4923,{"$f":"IF(AF4940<=$J$9*0.05,AS4939*EXP((-$J$6*1)/Heterogenität!$D$4),Z4940)","v":4.3451070484766462E-5},{"$f":"IF(OR(AF4940>=$J$19, AR4939/$J$5<AN4940),0, Bodencharakterisierung!$E$8*$J$11*((AR4939/$J$5)-AN4940))","v":2.3490344521245718E-6},4.5052013722587643E-7,{"$f":"AQ4939-AP4940*Bodencharakterisierung!$E$8","v":1.3622030476894209E-4},{"$f":"AQ4940/(Bodencharakterisierung!$E$11*1000)","v":8.9914392586760461E-8},4.3901590621992339E-5,{"$error":"#N/A"},null,{"$f":"(AP4940)*$G$11*Bodencharakterisierung!$E$8","v":6.5149262420694733E-9},{"$f":"IF(AF4940<=$J$9*1.05,(AV4940*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4939,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.880206719997865,null,8.9914392586760455E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.451070484766461]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4924,5.0665328019753157E-21,{"$f":"Z4941*EXP((-$J$6/Heterogenität!$D$4)*1)","v":5.0145398099022253E-21},{"$f":"AF4940*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4941^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4941)*3600*24","v":0},0,{"$f":"AE4940-AD4941*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4941>$J$18,(AE4941/(Bodencharakterisierung!$E$11*1000)),0)","v":0},5.0145398099022253E-21,{"$error":"#N/A"},null,{"$f":"(AD4941)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4941>0,(AJ4941*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4940,NA())","v":{"$error":"#N/A"}},null,4924,{"$f":"IF(AF4941<=$J$9*0.05,AS4940*EXP((-$J$6*1)/Heterogenität!$D$4),Z4941)","v":4.3451070484766462E-5},{"$f":"IF(OR(AF4941>=$J$19, AR4940/$J$5<AN4941),0, Bodencharakterisierung!$E$8*$J$11*((AR4940/$J$5)-AN4941))","v":1.8835080985054178E-6},4.5052013722587643E-7,{"$f":"AQ4940-AP4941*Bodencharakterisierung!$E$8","v":1.3607163312365756E-4},{"$f":"AQ4941/(Bodencharakterisierung!$E$11*1000)","v":8.9816259487562754E-8},4.3901590621992339E-5,{"$error":"#N/A"},null,{"$f":"(AP4941)*$G$11*Bodencharakterisierung!$E$8","v":6.5149262420694733E-9},{"$f":"IF(AF4941<=$J$9*1.05,(AV4941*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4940,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.886479359997864,null,8.981625948756275E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.451070484766461]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4925,5.0145398099022253E-21,{"$f":"Z4942*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.9630803722992958E-21},{"$f":"AF4941*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4942^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4942)*3600*24","v":0},0,{"$f":"AE4941-AD4942*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4942>$J$18,(AE4942/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.9630803722992958E-21,{"$error":"#N/A"},null,{"$f":"(AD4942)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4942>0,(AJ4942*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4941,NA())","v":{"$error":"#N/A"}},null,4925,{"$f":"IF(AF4942<=$J$9*0.05,AS4941*EXP((-$J$6*1)/Heterogenität!$D$4),Z4942)","v":4.3451070484766462E-5},{"$f":"IF(OR(AF4942>=$J$19, AR4941/$J$5<AN4942),0, Bodencharakterisierung!$E$8*$J$11*((AR4941/$J$5)-AN4942))","v":1.4179817448862638E-6},4.5052013722587643E-7,{"$f":"AQ4941-AP4942*Bodencharakterisierung!$E$8","v":1.3592296147837304E-4},{"$f":"AQ4942/(Bodencharakterisierung!$E$11*1000)","v":8.9718126388365047E-8},4.3901590621992339E-5,{"$error":"#N/A"},null,{"$f":"(AP4942)*$G$11*Bodencharakterisierung!$E$8","v":6.5149262420694733E-9},{"$f":"IF(AF4942<=$J$9*1.05,(AV4942*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4941,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.892751999997863,null,8.9718126388365044E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.451070484766461]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4926,4.9630803722992958E-21,{"$f":"Z4943*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.9121490138060749E-21},{"$f":"AF4942*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4943^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4943)*3600*24","v":0},0,{"$f":"AE4942-AD4943*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4943>$J$18,(AE4943/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.9121490138060749E-21,{"$error":"#N/A"},null,{"$f":"(AD4943)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4943>0,(AJ4943*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4942,NA())","v":{"$error":"#N/A"}},null,4926,{"$f":"IF(AF4943<=$J$9*0.05,AS4942*EXP((-$J$6*1)/Heterogenität!$D$4),Z4943)","v":4.3451070484766462E-5},{"$f":"IF(OR(AF4943>=$J$19, AR4942/$J$5<AN4943),0, Bodencharakterisierung!$E$8*$J$11*((AR4942/$J$5)-AN4943))","v":9.5245539126710999E-7},4.5052013722587643E-7,{"$f":"AQ4942-AP4943*Bodencharakterisierung!$E$8","v":1.3577428983308851E-4},{"$f":"AQ4943/(Bodencharakterisierung!$E$11*1000)","v":8.9619993289167339E-8},4.3901590621992339E-5,{"$error":"#N/A"},null,{"$f":"(AP4943)*$G$11*Bodencharakterisierung!$E$8","v":6.5149262420694733E-9},{"$f":"IF(AF4943<=$J$9*1.05,(AV4943*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4942,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.899024639997862,null,8.9619993289167338E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.451070484766461]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4927,4.9121490138060749E-21,{"$f":"Z4944*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.8617403152505096E-21},{"$f":"AF4943*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4944^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4944)*3600*24","v":0},0,{"$f":"AE4943-AD4944*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4944>$J$18,(AE4944/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.8617403152505096E-21,{"$error":"#N/A"},null,{"$f":"(AD4944)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4944>0,(AJ4944*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4943,NA())","v":{"$error":"#N/A"}},null,4927,{"$f":"IF(AF4944<=$J$9*0.05,AS4943*EXP((-$J$6*1)/Heterogenität!$D$4),Z4944)","v":4.3451070484766462E-5},{"$f":"IF(OR(AF4944>=$J$19, AR4943/$J$5<AN4944),0, Bodencharakterisierung!$E$8*$J$11*((AR4943/$J$5)-AN4944))","v":4.869290376479562E-7},4.5052013722587643E-7,{"$f":"AQ4943-AP4944*Bodencharakterisierung!$E$8","v":1.3562561818780398E-4},{"$f":"AQ4944/(Bodencharakterisierung!$E$11*1000)","v":8.9521860189969632E-8},4.3901590621992339E-5,{"$error":"#N/A"},null,{"$f":"(AP4944)*$G$11*Bodencharakterisierung!$E$8","v":6.5149262420694733E-9},{"$f":"IF(AF4944<=$J$9*1.05,(AV4944*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4943,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.90529727999786,null,8.9521860189969632E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.451070484766461]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4928,4.8617403152505096E-21,{"$f":"Z4945*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.811848913072339E-21},{"$f":"AF4944*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4945^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4945)*3600*24","v":0},0,{"$f":"AE4944-AD4945*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4945>$J$18,(AE4945/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.811848913072339E-21,{"$error":"#N/A"},null,{"$f":"(AD4945)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4945>0,(AJ4945*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4944,NA())","v":{"$error":"#N/A"}},null,4928,{"$f":"IF(AF4945<=$J$9*0.05,AS4944*EXP((-$J$6*1)/Heterogenität!$D$4),Z4945)","v":4.3451070484766462E-5},{"$f":"IF(OR(AF4945>=$J$19, AR4944/$J$5<AN4945),0, Bodencharakterisierung!$E$8*$J$11*((AR4944/$J$5)-AN4945))","v":2.1402684028802288E-8},2.1402684028802288E-8,{"$f":"AQ4944-AP4945*Bodencharakterisierung!$E$8","v":1.3561855530207448E-4},{"$f":"AQ4945/(Bodencharakterisierung!$E$11*1000)","v":8.951719821919108E-8},4.3472473168795262E-5,{"$error":"#N/A"},null,{"$f":"(AP4945)*$G$11*Bodencharakterisierung!$E$8","v":3.0950205397823541E-10},{"$f":"IF(AF4945<=$J$9*1.05,(AV4945*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4944,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.911569919997859,null,8.9517198219191074E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.451070484766461]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4929,4.811848913072339E-21,{"$f":"Z4946*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.7624694987524041E-21},{"$f":"AF4945*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4946^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4946)*3600*24","v":0},0,{"$f":"AE4945-AD4946*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4946>$J$18,(AE4946/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.7624694987524041E-21,{"$error":"#N/A"},null,{"$f":"(AD4946)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4946>0,(AJ4946*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4945,NA())","v":{"$error":"#N/A"}},null,4929,{"$f":"IF(AF4946<=$J$9*0.05,AS4945*EXP((-$J$6*1)/Heterogenität!$D$4),Z4946)","v":4.302635665456257E-5},{"$f":"IF(OR(AF4946>=$J$19, AR4945/$J$5<AN4946),0, Bodencharakterisierung!$E$8*$J$11*((AR4945/$J$5)-AN4946))","v":4.1500878858378099E-6},4.4611651423269205E-7,{"$f":"AQ4945-AP4946*Bodencharakterisierung!$E$8","v":1.3547133685237769E-4},{"$f":"AQ4946/(Bodencharakterisierung!$E$11*1000)","v":8.9420024325001774E-8},4.3472473168795262E-5,{"$error":"#N/A"},null,{"$f":"(AP4946)*$G$11*Bodencharakterisierung!$E$8","v":6.4512458943382167E-9},{"$f":"IF(AF4946<=$J$9*1.05,(AV4946*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4945,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.917842559997858,null,8.9420024325001776E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.026356654562569]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4930,4.7624694987524041E-21,{"$f":"Z4947*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.7135968182478131E-21},{"$f":"AF4946*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4947^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4947)*3600*24","v":0},0,{"$f":"AE4946-AD4947*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4947>$J$18,(AE4947/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.7135968182478131E-21,{"$error":"#N/A"},null,{"$f":"(AD4947)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4947>0,(AJ4947*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4946,NA())","v":{"$error":"#N/A"}},null,4930,{"$f":"IF(AF4947<=$J$9*0.05,AS4946*EXP((-$J$6*1)/Heterogenität!$D$4),Z4947)","v":4.302635665456257E-5},{"$f":"IF(OR(AF4947>=$J$19, AR4946/$J$5<AN4947),0, Bodencharakterisierung!$E$8*$J$11*((AR4946/$J$5)-AN4947))","v":3.689111833937275E-6},4.4611651423269205E-7,{"$f":"AQ4946-AP4947*Bodencharakterisierung!$E$8","v":1.353241184026809E-4},{"$f":"AQ4947/(Bodencharakterisierung!$E$11*1000)","v":8.9322850430812468E-8},4.3472473168795262E-5,{"$error":"#N/A"},null,{"$f":"(AP4947)*$G$11*Bodencharakterisierung!$E$8","v":6.4512458943382167E-9},{"$f":"IF(AF4947<=$J$9*1.05,(AV4947*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4946,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.924115199997857,null,8.9322850430812464E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.026356654562569]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4931,4.7135968182478131E-21,{"$f":"Z4948*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.6652256714329037E-21},{"$f":"AF4947*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4948^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4948)*3600*24","v":0},0,{"$f":"AE4947-AD4948*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4948>$J$18,(AE4948/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.6652256714329037E-21,{"$error":"#N/A"},null,{"$f":"(AD4948)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4948>0,(AJ4948*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4947,NA())","v":{"$error":"#N/A"}},null,4931,{"$f":"IF(AF4948<=$J$9*0.05,AS4947*EXP((-$J$6*1)/Heterogenität!$D$4),Z4948)","v":4.302635665456257E-5},{"$f":"IF(OR(AF4948>=$J$19, AR4947/$J$5<AN4948),0, Bodencharakterisierung!$E$8*$J$11*((AR4947/$J$5)-AN4948))","v":3.2281357820367401E-6},4.4611651423269205E-7,{"$f":"AQ4947-AP4948*Bodencharakterisierung!$E$8","v":1.351768999529841E-4},{"$f":"AQ4948/(Bodencharakterisierung!$E$11*1000)","v":8.9225676536623176E-8},4.3472473168795262E-5,{"$error":"#N/A"},null,{"$f":"(AP4948)*$G$11*Bodencharakterisierung!$E$8","v":6.4512458943382167E-9},{"$f":"IF(AF4948<=$J$9*1.05,(AV4948*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4947,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,{"$f":"$G$34/$G$12/$G$8+BC4947","v":30.930387839997856},null,8.922567653662318E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.026356654562569]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4932,4.6652256714329037E-21,{"$f":"Z4949*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.6173509115459406E-21},{"$f":"AF4948*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4949^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4949)*3600*24","v":0},0,{"$f":"AE4948-AD4949*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4949>$J$18,(AE4949/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.6173509115459406E-21,{"$error":"#N/A"},null,{"$f":"(AD4949)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4949>0,(AJ4949*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4948,NA())","v":{"$error":"#N/A"}},null,4932,{"$f":"IF(AF4949<=$J$9*0.05,AS4948*EXP((-$J$6*1)/Heterogenität!$D$4),Z4949)","v":4.302635665456257E-5},{"$f":"IF(OR(AF4949>=$J$19, AR4948/$J$5<AN4949),0, Bodencharakterisierung!$E$8*$J$11*((AR4948/$J$5)-AN4949))","v":2.7671597301363378E-6},4.4611651423269205E-7,{"$f":"AQ4948-AP4949*Bodencharakterisierung!$E$8","v":1.3502968150328731E-4},{"$f":"AQ4949/(Bodencharakterisierung!$E$11*1000)","v":8.912850264243387E-8},4.3472473168795262E-5,{"$error":"#N/A"},null,{"$f":"(AP4949)*$G$11*Bodencharakterisierung!$E$8","v":6.4512458943382167E-9},{"$f":"IF(AF4949<=$J$9*1.05,(AV4949*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4948,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.936660479997855,null,8.9128502642433868E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.026356654562569]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4933,4.6173509115459406E-21,{"$f":"Z4950*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.5699674446414951E-21},{"$f":"AF4949*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4950^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4950)*3600*24","v":0},0,{"$f":"AE4949-AD4950*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4950>$J$18,(AE4950/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.5699674446414951E-21,{"$error":"#N/A"},null,{"$f":"(AD4950)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4950>0,(AJ4950*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4949,NA())","v":{"$error":"#N/A"}},null,4933,{"$f":"IF(AF4950<=$J$9*0.05,AS4949*EXP((-$J$6*1)/Heterogenität!$D$4),Z4950)","v":4.302635665456257E-5},{"$f":"IF(OR(AF4950>=$J$19, AR4949/$J$5<AN4950),0, Bodencharakterisierung!$E$8*$J$11*((AR4949/$J$5)-AN4950))","v":2.3061836782358029E-6},4.4611651423269205E-7,{"$f":"AQ4949-AP4950*Bodencharakterisierung!$E$8","v":1.3488246305359052E-4},{"$f":"AQ4950/(Bodencharakterisierung!$E$11*1000)","v":8.9031328748244564E-8},4.3472473168795262E-5,{"$error":"#N/A"},null,{"$f":"(AP4950)*$G$11*Bodencharakterisierung!$E$8","v":6.4512458943382167E-9},{"$f":"IF(AF4950<=$J$9*1.05,(AV4950*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4949,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.942933119997853,null,8.903132874824457E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.026356654562569]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4934,4.5699674446414951E-21,{"$f":"Z4951*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.523070229048439E-21},{"$f":"AF4950*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4951^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4951)*3600*24","v":0},0,{"$f":"AE4950-AD4951*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4951>$J$18,(AE4951/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.523070229048439E-21,{"$error":"#N/A"},null,{"$f":"(AD4951)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4951>0,(AJ4951*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4950,NA())","v":{"$error":"#N/A"}},null,4934,{"$f":"IF(AF4951<=$J$9*0.05,AS4950*EXP((-$J$6*1)/Heterogenität!$D$4),Z4951)","v":4.302635665456257E-5},{"$f":"IF(OR(AF4951>=$J$19, AR4950/$J$5<AN4951),0, Bodencharakterisierung!$E$8*$J$11*((AR4950/$J$5)-AN4951))","v":1.8452076263352682E-6},4.4611651423269205E-7,{"$f":"AQ4950-AP4951*Bodencharakterisierung!$E$8","v":1.3473524460389373E-4},{"$f":"AQ4951/(Bodencharakterisierung!$E$11*1000)","v":8.8934154854055271E-8},4.3472473168795262E-5,{"$error":"#N/A"},null,{"$f":"(AP4951)*$G$11*Bodencharakterisierung!$E$8","v":6.4512458943382167E-9},{"$f":"IF(AF4951<=$J$9*1.05,(AV4951*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4950,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.949205759997852,null,8.8934154854055272E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.026356654562569]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4935,4.523070229048439E-21,{"$f":"Z4952*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.4766542748335051E-21},{"$f":"AF4951*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4952^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4952)*3600*24","v":0},0,{"$f":"AE4951-AD4952*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4952>$J$18,(AE4952/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.4766542748335051E-21,{"$error":"#N/A"},null,{"$f":"(AD4952)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4952>0,(AJ4952*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4951,NA())","v":{"$error":"#N/A"}},null,4935,{"$f":"IF(AF4952<=$J$9*0.05,AS4951*EXP((-$J$6*1)/Heterogenität!$D$4),Z4952)","v":4.302635665456257E-5},{"$f":"IF(OR(AF4952>=$J$19, AR4951/$J$5<AN4952),0, Bodencharakterisierung!$E$8*$J$11*((AR4951/$J$5)-AN4952))","v":1.3842315744348659E-6},4.4611651423269205E-7,{"$f":"AQ4951-AP4952*Bodencharakterisierung!$E$8","v":1.3458802615419694E-4},{"$f":"AQ4952/(Bodencharakterisierung!$E$11*1000)","v":8.8836980959865965E-8},4.3472473168795262E-5,{"$error":"#N/A"},null,{"$f":"(AP4952)*$G$11*Bodencharakterisierung!$E$8","v":6.4512458943382167E-9},{"$f":"IF(AF4952<=$J$9*1.05,(AV4952*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4951,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.955478399997851,null,8.883698095986596E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.026356654562569]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4936,4.4766542748335051E-21,{"$f":"Z4953*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.4307146432703501E-21},{"$f":"AF4952*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4953^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4953)*3600*24","v":0},0,{"$f":"AE4952-AD4953*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4953>$J$18,(AE4953/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.4307146432703501E-21,{"$error":"#N/A"},null,{"$f":"(AD4953)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4953>0,(AJ4953*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4952,NA())","v":{"$error":"#N/A"}},null,4936,{"$f":"IF(AF4953<=$J$9*0.05,AS4952*EXP((-$J$6*1)/Heterogenität!$D$4),Z4953)","v":4.302635665456257E-5},{"$f":"IF(OR(AF4953>=$J$19, AR4952/$J$5<AN4953),0, Bodencharakterisierung!$E$8*$J$11*((AR4952/$J$5)-AN4953))","v":9.2325552253433118E-7},4.4611651423269205E-7,{"$f":"AQ4952-AP4953*Bodencharakterisierung!$E$8","v":1.3444080770450015E-4},{"$f":"AQ4953/(Bodencharakterisierung!$E$11*1000)","v":8.8739807065676659E-8},4.3472473168795262E-5,{"$error":"#N/A"},null,{"$f":"(AP4953)*$G$11*Bodencharakterisierung!$E$8","v":6.4512458943382167E-9},{"$f":"IF(AF4953<=$J$9*1.05,(AV4953*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4952,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.96175103999785,null,8.8739807065676662E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.026356654562569]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4937,4.4307146432703501E-21,{"$f":"Z4954*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.385246446314067E-21},{"$f":"AF4953*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4954^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4954)*3600*24","v":0},0,{"$f":"AE4953-AD4954*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4954>$J$18,(AE4954/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.385246446314067E-21,{"$error":"#N/A"},null,{"$f":"(AD4954)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4954>0,(AJ4954*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4953,NA())","v":{"$error":"#N/A"}},null,4937,{"$f":"IF(AF4954<=$J$9*0.05,AS4953*EXP((-$J$6*1)/Heterogenität!$D$4),Z4954)","v":4.302635665456257E-5},{"$f":"IF(OR(AF4954>=$J$19, AR4953/$J$5<AN4954),0, Bodencharakterisierung!$E$8*$J$11*((AR4953/$J$5)-AN4954))","v":4.6227947063379644E-7},4.4611651423269205E-7,{"$f":"AQ4953-AP4954*Bodencharakterisierung!$E$8","v":1.3429358925480335E-4},{"$f":"AQ4954/(Bodencharakterisierung!$E$11*1000)","v":8.8642633171487366E-8},4.3472473168795262E-5,{"$error":"#N/A"},null,{"$f":"(AP4954)*$G$11*Bodencharakterisierung!$E$8","v":6.4512458943382167E-9},{"$f":"IF(AF4954<=$J$9*1.05,(AV4954*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4953,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.968023679997849,null,8.8642633171487364E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.026356654562569]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4938,4.385246446314067E-21,{"$f":"Z4955*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.3402448460810908E-21},{"$f":"AF4954*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4955^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4955)*3600*24","v":0},0,{"$f":"AE4954-AD4955*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4955>$J$18,(AE4955/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.3402448460810908E-21,{"$error":"#N/A"},null,{"$f":"(AD4955)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4955>0,(AJ4955*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4954,NA())","v":{"$error":"#N/A"}},null,4938,{"$f":"IF(AF4955<=$J$9*0.05,AS4954*EXP((-$J$6*1)/Heterogenität!$D$4),Z4955)","v":4.302635665456257E-5},{"$f":"IF(OR(AF4955>=$J$19, AR4954/$J$5<AN4955),0, Bodencharakterisierung!$E$8*$J$11*((AR4954/$J$5)-AN4955))","v":1.3034187333941437E-9},1.3034187333941437E-9,{"$f":"AQ4954-AP4955*Bodencharakterisierung!$E$8","v":1.3429315912662134E-4},{"$f":"AQ4955/(Bodencharakterisierung!$E$11*1000)","v":8.8642349258495929E-8},4.3027660073295962E-5,{"$error":"#N/A"},null,{"$f":"(AP4955)*$G$11*Bodencharakterisierung!$E$8","v":1.8848606774566893E-11},{"$f":"IF(AF4955<=$J$9*1.05,(AV4955*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4954,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.974296319997848,null,8.8642349258495928E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,43.026356654562569]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4939,4.3402448460810908E-21,{"$f":"Z4956*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.2957050543344379E-21},{"$f":"AF4955*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4956^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4956)*3600*24","v":0},0,{"$f":"AE4955-AD4956*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4956>$J$18,(AE4956/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.2957050543344379E-21,{"$error":"#N/A"},null,{"$f":"(AD4956)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4956>0,(AJ4956*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4955,NA())","v":{"$error":"#N/A"}},null,4939,{"$f":"IF(AF4956<=$J$9*0.05,AS4955*EXP((-$J$6*1)/Heterogenität!$D$4),Z4956)","v":4.2586108251457896E-5},{"$f":"IF(OR(AF4956>=$J$19, AR4955/$J$5<AN4956),0, Bodencharakterisierung!$E$8*$J$11*((AR4955/$J$5)-AN4956))","v":4.3025793985863756E-6},4.4155182183806601E-7,{"$f":"AQ4955-AP4956*Bodencharakterisierung!$E$8","v":1.3414744702541477E-4},{"$f":"AQ4956/(Bodencharakterisierung!$E$11*1000)","v":8.8546169653739124E-8},4.3027660073295962E-5,{"$error":"#N/A"},null,{"$f":"(AP4956)*$G$11*Bodencharakterisierung!$E$8","v":6.3852363382463556E-9},{"$f":"IF(AF4956<=$J$9*1.05,(AV4956*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4955,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.980568959997846,null,8.8546169653739126E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.586108251457894]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4940,4.2957050543344379E-21,{"$f":"Z4957*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.2516223319742338E-21},{"$f":"AF4956*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4957^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4957)*3600*24","v":0},0,{"$f":"AE4956-AD4957*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4957>$J$18,(AE4957/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.2516223319742338E-21,{"$error":"#N/A"},null,{"$f":"(AD4957)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4957>0,(AJ4957*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4956,NA())","v":{"$error":"#N/A"}},null,4940,{"$f":"IF(AF4957<=$J$9*0.05,AS4956*EXP((-$J$6*1)/Heterogenität!$D$4),Z4957)","v":4.2586108251457896E-5},{"$f":"IF(OR(AF4957>=$J$19, AR4956/$J$5<AN4957),0, Bodencharakterisierung!$E$8*$J$11*((AR4956/$J$5)-AN4957))","v":3.8463200828099368E-6},4.4155182183806601E-7,{"$f":"AQ4956-AP4957*Bodencharakterisierung!$E$8","v":1.3400173492420821E-4},{"$f":"AQ4957/(Bodencharakterisierung!$E$11*1000)","v":8.8449990048982319E-8},4.3027660073295962E-5,{"$error":"#N/A"},null,{"$f":"(AP4957)*$G$11*Bodencharakterisierung!$E$8","v":6.3852363382463556E-9},{"$f":"IF(AF4957<=$J$9*1.05,(AV4957*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4956,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.986841599997845,null,8.8449990048982324E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.586108251457894]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4941,4.2516223319742338E-21,{"$f":"Z4958*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.2079919885334632E-21},{"$f":"AF4957*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4958^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4958)*3600*24","v":0},0,{"$f":"AE4957-AD4958*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4958>$J$18,(AE4958/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.2079919885334632E-21,{"$error":"#N/A"},null,{"$f":"(AD4958)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4958>0,(AJ4958*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4957,NA())","v":{"$error":"#N/A"}},null,4941,{"$f":"IF(AF4958<=$J$9*0.05,AS4957*EXP((-$J$6*1)/Heterogenität!$D$4),Z4958)","v":4.2586108251457896E-5},{"$f":"IF(OR(AF4958>=$J$19, AR4957/$J$5<AN4958),0, Bodencharakterisierung!$E$8*$J$11*((AR4957/$J$5)-AN4958))","v":3.3900607670334981E-6},4.4155182183806601E-7,{"$f":"AQ4957-AP4958*Bodencharakterisierung!$E$8","v":1.3385602282300164E-4},{"$f":"AQ4958/(Bodencharakterisierung!$E$11*1000)","v":8.83538104442255E-8},4.3027660073295962E-5,{"$error":"#N/A"},null,{"$f":"(AP4958)*$G$11*Bodencharakterisierung!$E$8","v":6.3852363382463556E-9},{"$f":"IF(AF4958<=$J$9*1.05,(AV4958*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4957,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,30.993114239997844,null,8.8353810444225495E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.586108251457894]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4942,{"$f":"AG4958","v":4.2079919885334632E-21},{"$f":"Z4959*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.1648093816789E-21},{"$f":"AF4958*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4959^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4959)*3600*24","v":0},{"$f":"MIN(AC4959,Z4959-AA4959)","v":0},{"$f":"AE4958-AD4959*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4959>$J$18,(AE4959/(Bodencharakterisierung!$E$11*1000)),0)","v":0},{"$f":"AA4959+AD4959","v":4.1648093816789E-21},{"$f":"IF(AD4959>0,Y4959,NA())","v":{"$error":"#N/A"}},null,{"$f":"(AD4959)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4959>0,(AJ4959*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4958,NA())","v":{"$error":"#N/A"}},null,4942,{"$f":"IF(AF4959<=$J$9*0.05,AS4958*EXP((-$J$6*1)/Heterogenität!$D$4),Z4959)","v":4.2586108251457896E-5},{"$f":"IF(OR(AF4959>=$J$19, AR4958/$J$5<AN4959),0, Bodencharakterisierung!$E$8*$J$11*((AR4958/$J$5)-AN4959))","v":2.9338014512569928E-6},{"$f":"MIN(AO4959,AS4958-AN4959)","v":4.4155182183806601E-7},{"$f":"AQ4958-AP4959*Bodencharakterisierung!$E$8","v":1.3371031072179507E-4},{"$f":"AQ4959/(Bodencharakterisierung!$E$11*1000)","v":8.8257630839468695E-8},{"$f":"AN4959+AP4959","v":4.3027660073295962E-5},{"$f":"IF(AN4959>$G$5,AM4959,NA())","v":{"$error":"#N/A"}},null,{"$f":"(AP4959)*$G$11*Bodencharakterisierung!$E$8","v":6.3852363382463556E-9},{"$f":"IF(AF4959<=$J$9*1.05,(AV4959*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4958,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH4959>($G$5*10^6),BH4959*0.99,9999)","v":9999},{"$f":"AT4959+$G$3","v":{"$error":"#N/A"}},{"$f":"IF(ISNUMBER(AT4959),BA4959+BB4959+BC4959+$AZ$17,\"\")","v":""},{"$f":"IF(ISNUMBER(AK4959),AK4959,BA4958)","v":1.6399886323194495},{"$f":"IF(ISNUMBER(AW4959),AW4959,0)","v":0},30.999386879997843,null,{"$f":"AR4959*10^6","v":8.8257630839468693E-2},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF4959*10^6","v":0},{"$f":"AN4959*10^6","v":42.586108251457894}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4943,4.1648093816789E-21,{"$f":"Z4960*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.1220699167171535E-21},{"$f":"AF4959*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4960^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4960)*3600*24","v":0},0,{"$f":"AE4959-AD4960*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4960>$J$18,(AE4960/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.1220699167171535E-21,{"$error":"#N/A"},null,{"$f":"(AD4960)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4960>0,(AJ4960*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4959,NA())","v":{"$error":"#N/A"}},null,4943,{"$f":"IF(AF4960<=$J$9*0.05,AS4959*EXP((-$J$6*1)/Heterogenität!$D$4),Z4960)","v":4.2586108251457896E-5},{"$f":"IF(OR(AF4960>=$J$19, AR4959/$J$5<AN4960),0, Bodencharakterisierung!$E$8*$J$11*((AR4959/$J$5)-AN4960))","v":2.477542135480554E-6},4.4155182183806601E-7,{"$f":"AQ4959-AP4960*Bodencharakterisierung!$E$8","v":1.3356459862058851E-4},{"$f":"AQ4960/(Bodencharakterisierung!$E$11*1000)","v":8.8161451234711889E-8},4.3027660073295962E-5,{"$error":"#N/A"},null,{"$f":"(AP4960)*$G$11*Bodencharakterisierung!$E$8","v":6.3852363382463556E-9},{"$f":"IF(AF4960<=$J$9*1.05,(AV4960*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4959,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.005659519997842,null,8.8161451234711891E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.586108251457894]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4944,4.1220699167171535E-21,{"$f":"Z4961*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.0797690461057875E-21},{"$f":"AF4960*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4961^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4961)*3600*24","v":0},0,{"$f":"AE4960-AD4961*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4961>$J$18,(AE4961/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.0797690461057875E-21,{"$error":"#N/A"},null,{"$f":"(AD4961)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4961>0,(AJ4961*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4960,NA())","v":{"$error":"#N/A"}},null,4944,{"$f":"IF(AF4961<=$J$9*0.05,AS4960*EXP((-$J$6*1)/Heterogenität!$D$4),Z4961)","v":4.2586108251457896E-5},{"$f":"IF(OR(AF4961>=$J$19, AR4960/$J$5<AN4961),0, Bodencharakterisierung!$E$8*$J$11*((AR4960/$J$5)-AN4961))","v":2.0212828197041813E-6},4.4155182183806601E-7,{"$f":"AQ4960-AP4961*Bodencharakterisierung!$E$8","v":1.3341888651938194E-4},{"$f":"AQ4961/(Bodencharakterisierung!$E$11*1000)","v":8.8065271629955071E-8},4.3027660073295962E-5,{"$error":"#N/A"},null,{"$f":"(AP4961)*$G$11*Bodencharakterisierung!$E$8","v":6.3852363382463556E-9},{"$f":"IF(AF4961<=$J$9*1.05,(AV4961*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4960,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.011932159997841,null,8.8065271629955075E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.586108251457894]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4945,4.0797690461057875E-21,{"$f":"Z4962*EXP((-$J$6/Heterogenität!$D$4)*1)","v":4.037902268969455E-21},{"$f":"AF4961*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4962^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4962)*3600*24","v":0},0,{"$f":"AE4961-AD4962*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4962>$J$18,(AE4962/(Bodencharakterisierung!$E$11*1000)),0)","v":0},4.037902268969455E-21,{"$error":"#N/A"},null,{"$f":"(AD4962)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4962>0,(AJ4962*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4961,NA())","v":{"$error":"#N/A"}},null,4945,{"$f":"IF(AF4962<=$J$9*0.05,AS4961*EXP((-$J$6*1)/Heterogenität!$D$4),Z4962)","v":4.2586108251457896E-5},{"$f":"IF(OR(AF4962>=$J$19, AR4961/$J$5<AN4962),0, Bodencharakterisierung!$E$8*$J$11*((AR4961/$J$5)-AN4962))","v":1.5650235039276765E-6},4.4155182183806601E-7,{"$f":"AQ4961-AP4962*Bodencharakterisierung!$E$8","v":1.3327317441817537E-4},{"$f":"AQ4962/(Bodencharakterisierung!$E$11*1000)","v":8.7969092025198265E-8},4.3027660073295962E-5,{"$error":"#N/A"},null,{"$f":"(AP4962)*$G$11*Bodencharakterisierung!$E$8","v":6.3852363382463556E-9},{"$f":"IF(AF4962<=$J$9*1.05,(AV4962*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4961,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.018204799997839,null,8.7969092025198259E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.586108251457894]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4946,4.037902268969455E-21,{"$f":"Z4963*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.9964651306209986E-21},{"$f":"AF4962*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4963^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4963)*3600*24","v":0},0,{"$f":"AE4962-AD4963*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4963>$J$18,(AE4963/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.9964651306209986E-21,{"$error":"#N/A"},null,{"$f":"(AD4963)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4963>0,(AJ4963*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4962,NA())","v":{"$error":"#N/A"}},null,4946,{"$f":"IF(AF4963<=$J$9*0.05,AS4962*EXP((-$J$6*1)/Heterogenität!$D$4),Z4963)","v":4.2586108251457896E-5},{"$f":"IF(OR(AF4963>=$J$19, AR4962/$J$5<AN4963),0, Bodencharakterisierung!$E$8*$J$11*((AR4962/$J$5)-AN4963))","v":1.1087641881512377E-6},4.4155182183806601E-7,{"$f":"AQ4962-AP4963*Bodencharakterisierung!$E$8","v":1.3312746231696881E-4},{"$f":"AQ4963/(Bodencharakterisierung!$E$11*1000)","v":8.787291242044146E-8},4.3027660073295962E-5,{"$error":"#N/A"},null,{"$f":"(AP4963)*$G$11*Bodencharakterisierung!$E$8","v":6.3852363382463556E-9},{"$f":"IF(AF4963<=$J$9*1.05,(AV4963*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4962,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.024477439997838,null,8.7872912420441457E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.586108251457894]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4947,3.9964651306209986E-21,{"$f":"Z4964*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.9554532220874651E-21},{"$f":"AF4963*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4964^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4964)*3600*24","v":0},0,{"$f":"AE4963-AD4964*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4964>$J$18,(AE4964/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.9554532220874651E-21,{"$error":"#N/A"},null,{"$f":"(AD4964)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4964>0,(AJ4964*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4963,NA())","v":{"$error":"#N/A"}},null,4947,{"$f":"IF(AF4964<=$J$9*0.05,AS4963*EXP((-$J$6*1)/Heterogenität!$D$4),Z4964)","v":4.2586108251457896E-5},{"$f":"IF(OR(AF4964>=$J$19, AR4963/$J$5<AN4964),0, Bodencharakterisierung!$E$8*$J$11*((AR4963/$J$5)-AN4964))","v":6.5250487237479884E-7},4.4155182183806601E-7,{"$f":"AQ4963-AP4964*Bodencharakterisierung!$E$8","v":1.3298175021576224E-4},{"$f":"AQ4964/(Bodencharakterisierung!$E$11*1000)","v":8.7776732815684641E-8},4.3027660073295962E-5,{"$error":"#N/A"},null,{"$f":"(AP4964)*$G$11*Bodencharakterisierung!$E$8","v":6.3852363382463556E-9},{"$f":"IF(AF4964<=$J$9*1.05,(AV4964*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4963,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.030750079997837,null,8.7776732815684641E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.586108251457894]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4948,3.9554532220874651E-21,{"$f":"Z4965*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.9148621796409829E-21},{"$f":"AF4964*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4965^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4965)*3600*24","v":0},0,{"$f":"AE4964-AD4965*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4965>$J$18,(AE4965/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.9148621796409829E-21,{"$error":"#N/A"},null,{"$f":"(AD4965)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4965>0,(AJ4965*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4964,NA())","v":{"$error":"#N/A"}},null,4948,{"$f":"IF(AF4965<=$J$9*0.05,AS4964*EXP((-$J$6*1)/Heterogenität!$D$4),Z4965)","v":4.2586108251457896E-5},{"$f":"IF(OR(AF4965>=$J$19, AR4964/$J$5<AN4965),0, Bodencharakterisierung!$E$8*$J$11*((AR4964/$J$5)-AN4965))","v":1.9624555659829381E-7},1.9624555659829381E-7,{"$f":"AQ4964-AP4965*Bodencharakterisierung!$E$8","v":1.3291698918208481E-4},{"$f":"AQ4965/(Bodencharakterisierung!$E$11*1000)","v":8.773398625880185E-8},4.2782353808056188E-5,{"$error":"#N/A"},null,{"$f":"(AP4965)*$G$11*Bodencharakterisierung!$E$8","v":2.837887190668999E-9},{"$f":"IF(AF4965<=$J$9*1.05,(AV4965*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4964,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.037022719997836,null,8.7733986258801855E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.586108251457894]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4949,3.9148621796409829E-21,{"$f":"Z4966*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.874687684334457E-21},{"$f":"AF4965*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4966^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4966)*3600*24","v":0},0,{"$f":"AE4965-AD4966*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4966>$J$18,(AE4966/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.874687684334457E-21,{"$error":"#N/A"},null,{"$f":"(AD4966)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4966>0,(AJ4966*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4965,NA())","v":{"$error":"#N/A"}},null,4949,{"$f":"IF(AF4966<=$J$9*0.05,AS4965*EXP((-$J$6*1)/Heterogenität!$D$4),Z4966)","v":4.234331933036699E-5},{"$f":"IF(OR(AF4966>=$J$19, AR4965/$J$5<AN4966),0, Bodencharakterisierung!$E$8*$J$11*((AR4965/$J$5)-AN4966))","v":2.3662809067392079E-6},4.3903447768919764E-7,{"$f":"AQ4965-AP4966*Bodencharakterisierung!$E$8","v":1.3277210780444738E-4},{"$f":"AQ4966/(Bodencharakterisierung!$E$11*1000)","v":8.7638354986433918E-8},4.2782353808056188E-5,{"$error":"#N/A"},null,{"$f":"(AP4966)*$G$11*Bodencharakterisierung!$E$8","v":6.348833278536818E-9},{"$f":"IF(AF4966<=$J$9*1.05,(AV4966*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4965,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.043295359997835,null,8.7638354986433922E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.343319330366988]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4950,3.874687684334457E-21,{"$f":"Z4967*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.8349254615420255E-21},{"$f":"AF4966*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4967^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4967)*3600*24","v":0},0,{"$f":"AE4966-AD4967*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4967>$J$18,(AE4967/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.8349254615420255E-21,{"$error":"#N/A"},null,{"$f":"(AD4967)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4967>0,(AJ4967*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4966,NA())","v":{"$error":"#N/A"}},null,4950,{"$f":"IF(AF4967<=$J$9*0.05,AS4966*EXP((-$J$6*1)/Heterogenität!$D$4),Z4967)","v":4.234331933036699E-5},{"$f":"IF(OR(AF4967>=$J$19, AR4966/$J$5<AN4967),0, Bodencharakterisierung!$E$8*$J$11*((AR4966/$J$5)-AN4967))","v":1.9126227844402481E-6},4.3903447768919764E-7,{"$f":"AQ4966-AP4967*Bodencharakterisierung!$E$8","v":1.3262722642680996E-4},{"$f":"AQ4967/(Bodencharakterisierung!$E$11*1000)","v":8.7542723714065986E-8},4.2782353808056188E-5,{"$error":"#N/A"},null,{"$f":"(AP4967)*$G$11*Bodencharakterisierung!$E$8","v":6.348833278536818E-9},{"$f":"IF(AF4967<=$J$9*1.05,(AV4967*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4966,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.049567999997834,null,8.754272371406599E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.343319330366988]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4951,3.8349254615420255E-21,{"$f":"Z4968*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.7955712805042335E-21},{"$f":"AF4967*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4968^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4968)*3600*24","v":0},0,{"$f":"AE4967-AD4968*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4968>$J$18,(AE4968/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.7955712805042335E-21,{"$error":"#N/A"},null,{"$f":"(AD4968)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4968>0,(AJ4968*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4967,NA())","v":{"$error":"#N/A"}},null,4951,{"$f":"IF(AF4968<=$J$9*0.05,AS4967*EXP((-$J$6*1)/Heterogenität!$D$4),Z4968)","v":4.234331933036699E-5},{"$f":"IF(OR(AF4968>=$J$19, AR4967/$J$5<AN4968),0, Bodencharakterisierung!$E$8*$J$11*((AR4967/$J$5)-AN4968))","v":1.4589646621413548E-6},4.3903447768919764E-7,{"$f":"AQ4967-AP4968*Bodencharakterisierung!$E$8","v":1.3248234504917254E-4},{"$f":"AQ4968/(Bodencharakterisierung!$E$11*1000)","v":8.7447092441698041E-8},4.2782353808056188E-5,{"$error":"#N/A"},null,{"$f":"(AP4968)*$G$11*Bodencharakterisierung!$E$8","v":6.348833278536818E-9},{"$f":"IF(AF4968<=$J$9*1.05,(AV4968*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4967,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.055840639997832,null,8.7447092441698043E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.343319330366988]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4952,3.7955712805042335E-21,{"$f":"Z4969*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.756620953877873E-21},{"$f":"AF4968*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4969^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4969)*3600*24","v":0},0,{"$f":"AE4968-AD4969*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4969>$J$18,(AE4969/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.756620953877873E-21,{"$error":"#N/A"},null,{"$f":"(AD4969)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4969>0,(AJ4969*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4968,NA())","v":{"$error":"#N/A"}},null,4952,{"$f":"IF(AF4969<=$J$9*0.05,AS4968*EXP((-$J$6*1)/Heterogenität!$D$4),Z4969)","v":4.234331933036699E-5},{"$f":"IF(OR(AF4969>=$J$19, AR4968/$J$5<AN4969),0, Bodencharakterisierung!$E$8*$J$11*((AR4968/$J$5)-AN4969))","v":1.0053065398424615E-6},4.3903447768919764E-7,{"$f":"AQ4968-AP4969*Bodencharakterisierung!$E$8","v":1.3233746367153512E-4},{"$f":"AQ4969/(Bodencharakterisierung!$E$11*1000)","v":8.7351461169330109E-8},4.2782353808056188E-5,{"$error":"#N/A"},null,{"$f":"(AP4969)*$G$11*Bodencharakterisierung!$E$8","v":6.348833278536818E-9},{"$f":"IF(AF4969<=$J$9*1.05,(AV4969*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4968,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.062113279997831,null,8.7351461169330111E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.343319330366988]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4953,3.756620953877873E-21,{"$f":"Z4970*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.7180703372904447E-21},{"$f":"AF4969*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4970^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4970)*3600*24","v":0},0,{"$f":"AE4969-AD4970*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4970>$J$18,(AE4970/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.7180703372904447E-21,{"$error":"#N/A"},null,{"$f":"(AD4970)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4970>0,(AJ4970*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4969,NA())","v":{"$error":"#N/A"}},null,4953,{"$f":"IF(AF4970<=$J$9*0.05,AS4969*EXP((-$J$6*1)/Heterogenität!$D$4),Z4970)","v":4.234331933036699E-5},{"$f":"IF(OR(AF4970>=$J$19, AR4969/$J$5<AN4970),0, Bodencharakterisierung!$E$8*$J$11*((AR4969/$J$5)-AN4970))","v":5.5164841754356827E-7},4.3903447768919764E-7,{"$f":"AQ4969-AP4970*Bodencharakterisierung!$E$8","v":1.3219258229389769E-4},{"$f":"AQ4970/(Bodencharakterisierung!$E$11*1000)","v":8.7255829896962177E-8},4.2782353808056188E-5,{"$error":"#N/A"},null,{"$f":"(AP4970)*$G$11*Bodencharakterisierung!$E$8","v":6.348833278536818E-9},{"$f":"IF(AF4970<=$J$9*1.05,(AV4970*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4969,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.06838591999783,null,8.7255829896962178E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.343319330366988]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4954,3.7180703372904447E-21,{"$f":"Z4971*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.6799153288991901E-21},{"$f":"AF4970*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4971^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4971)*3600*24","v":0},0,{"$f":"AE4970-AD4971*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4971>$J$18,(AE4971/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.6799153288991901E-21,{"$error":"#N/A"},null,{"$f":"(AD4971)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4971>0,(AJ4971*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4970,NA())","v":{"$error":"#N/A"}},null,4954,{"$f":"IF(AF4971<=$J$9*0.05,AS4970*EXP((-$J$6*1)/Heterogenität!$D$4),Z4971)","v":4.234331933036699E-5},{"$f":"IF(OR(AF4971>=$J$19, AR4970/$J$5<AN4971),0, Bodencharakterisierung!$E$8*$J$11*((AR4970/$J$5)-AN4971))","v":9.7990295244675026E-8},9.7990295244675026E-8,{"$f":"AQ4970-AP4971*Bodencharakterisierung!$E$8","v":1.3216024549646694E-4},{"$f":"AQ4971/(Bodencharakterisierung!$E$11*1000)","v":8.7234485476215804E-8},4.2441309625611665E-5,{"$error":"#N/A"},null,{"$f":"(AP4971)*$G$11*Bodencharakterisierung!$E$8","v":1.4170277712527545E-9},{"$f":"IF(AF4971<=$J$9*1.05,(AV4971*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4970,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.074658559997829,null,8.7234485476215803E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.343319330366988]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4955,3.6799153288991901E-21,{"$f":"Z4972*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.6421518689546485E-21},{"$f":"AF4971*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4972^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4972)*3600*24","v":0},0,{"$f":"AE4971-AD4972*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4972>$J$18,(AE4972/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.6421518689546485E-21,{"$error":"#N/A"},null,{"$f":"(AD4972)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4972>0,(AJ4972*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4971,NA())","v":{"$error":"#N/A"}},null,4955,{"$f":"IF(AF4972<=$J$9*0.05,AS4971*EXP((-$J$6*1)/Heterogenität!$D$4),Z4972)","v":4.2005774958970268E-5},{"$f":"IF(OR(AF4972>=$J$19, AR4971/$J$5<AN4972),0, Bodencharakterisierung!$E$8*$J$11*((AR4971/$J$5)-AN4972))","v":3.295614851440217E-6},4.3553466664139672E-7,{"$f":"AQ4971-AP4972*Bodencharakterisierung!$E$8","v":1.3201651905647528E-4},{"$f":"AQ4972/(Bodencharakterisierung!$E$11*1000)","v":8.7139616538927579E-8},4.2441309625611665E-5,{"$error":"#N/A"},null,{"$f":"(AP4972)*$G$11*Bodencharakterisierung!$E$8","v":6.2982228641433519E-9},{"$f":"IF(AF4972<=$J$9*1.05,(AV4972*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4971,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.080931199997828,null,8.7139616538927586E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.005774958970271]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4956,3.6421518689546485E-21,{"$f":"Z4973*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.6047759393686951E-21},{"$f":"AF4972*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4973^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4973)*3600*24","v":0},0,{"$f":"AE4972-AD4973*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4973>$J$18,(AE4973/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.6047759393686951E-21,{"$error":"#N/A"},null,{"$f":"(AD4973)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4973>0,(AJ4973*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4972,NA())","v":{"$error":"#N/A"}},null,4956,{"$f":"IF(AF4973<=$J$9*0.05,AS4972*EXP((-$J$6*1)/Heterogenität!$D$4),Z4973)","v":4.2005774958970268E-5},{"$f":"IF(OR(AF4973>=$J$19, AR4972/$J$5<AN4973),0, Bodencharakterisierung!$E$8*$J$11*((AR4972/$J$5)-AN4973))","v":2.8455731141611904E-6},4.3553466664139672E-7,{"$f":"AQ4972-AP4973*Bodencharakterisierung!$E$8","v":1.3187279261648362E-4},{"$f":"AQ4973/(Bodencharakterisierung!$E$11*1000)","v":8.7044747601639355E-8},4.2441309625611665E-5,{"$error":"#N/A"},null,{"$f":"(AP4973)*$G$11*Bodencharakterisierung!$E$8","v":6.2982228641433519E-9},{"$f":"IF(AF4973<=$J$9*1.05,(AV4973*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4972,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.087203839997827,null,8.7044747601639355E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.005774958970271]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4957,3.6047759393686951E-21,{"$f":"Z4974*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.5677835632870101E-21},{"$f":"AF4973*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4974^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4974)*3600*24","v":0},0,{"$f":"AE4973-AD4974*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4974>$J$18,(AE4974/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.5677835632870101E-21,{"$error":"#N/A"},null,{"$f":"(AD4974)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4974>0,(AJ4974*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4973,NA())","v":{"$error":"#N/A"}},null,4957,{"$f":"IF(AF4974<=$J$9*0.05,AS4973*EXP((-$J$6*1)/Heterogenität!$D$4),Z4974)","v":4.2005774958970268E-5},{"$f":"IF(OR(AF4974>=$J$19, AR4973/$J$5<AN4974),0, Bodencharakterisierung!$E$8*$J$11*((AR4973/$J$5)-AN4974))","v":2.3955313768821633E-6},4.3553466664139672E-7,{"$f":"AQ4973-AP4974*Bodencharakterisierung!$E$8","v":1.3172906617649197E-4},{"$f":"AQ4974/(Bodencharakterisierung!$E$11*1000)","v":8.694987866435113E-8},4.2441309625611665E-5,{"$error":"#N/A"},null,{"$f":"(AP4974)*$G$11*Bodencharakterisierung!$E$8","v":6.2982228641433519E-9},{"$f":"IF(AF4974<=$J$9*1.05,(AV4974*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4973,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.093476479997825,null,8.6949878664351124E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.005774958970271]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4958,3.5677835632870101E-21,{"$f":"Z4975*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.5311708046659347E-21},{"$f":"AF4974*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4975^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4975)*3600*24","v":0},0,{"$f":"AE4974-AD4975*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4975>$J$18,(AE4975/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.5311708046659347E-21,{"$error":"#N/A"},null,{"$f":"(AD4975)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4975>0,(AJ4975*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4974,NA())","v":{"$error":"#N/A"}},null,4958,{"$f":"IF(AF4975<=$J$9*0.05,AS4974*EXP((-$J$6*1)/Heterogenität!$D$4),Z4975)","v":4.2005774958970268E-5},{"$f":"IF(OR(AF4975>=$J$19, AR4974/$J$5<AN4975),0, Bodencharakterisierung!$E$8*$J$11*((AR4974/$J$5)-AN4975))","v":1.9454896396031366E-6},4.3553466664139672E-7,{"$f":"AQ4974-AP4975*Bodencharakterisierung!$E$8","v":1.3158533973650031E-4},{"$f":"AQ4975/(Bodencharakterisierung!$E$11*1000)","v":8.6855009727062905E-8},4.2441309625611665E-5,{"$error":"#N/A"},null,{"$f":"(AP4975)*$G$11*Bodencharakterisierung!$E$8","v":6.2982228641433519E-9},{"$f":"IF(AF4975<=$J$9*1.05,(AV4975*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4974,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.099749119997824,null,8.6855009727062907E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.005774958970271]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4959,3.5311708046659347E-21,{"$f":"Z4976*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.4949337678536706E-21},{"$f":"AF4975*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4976^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4976)*3600*24","v":0},0,{"$f":"AE4975-AD4976*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4976>$J$18,(AE4976/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.4949337678536706E-21,{"$error":"#N/A"},null,{"$f":"(AD4976)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4976>0,(AJ4976*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4975,NA())","v":{"$error":"#N/A"}},null,4959,{"$f":"IF(AF4976<=$J$9*0.05,AS4975*EXP((-$J$6*1)/Heterogenität!$D$4),Z4976)","v":4.2005774958970268E-5},{"$f":"IF(OR(AF4976>=$J$19, AR4975/$J$5<AN4976),0, Bodencharakterisierung!$E$8*$J$11*((AR4975/$J$5)-AN4976))","v":1.4954479023241761E-6},4.3553466664139672E-7,{"$f":"AQ4975-AP4976*Bodencharakterisierung!$E$8","v":1.3144161329650865E-4},{"$f":"AQ4976/(Bodencharakterisierung!$E$11*1000)","v":8.676014078977468E-8},4.2441309625611665E-5,{"$error":"#N/A"},null,{"$f":"(AP4976)*$G$11*Bodencharakterisierung!$E$8","v":6.2982228641433519E-9},{"$f":"IF(AF4976<=$J$9*1.05,(AV4976*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4975,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.106021759997823,null,8.6760140789774676E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.005774958970271]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4960,3.4949337678536706E-21,{"$f":"Z4977*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.4590685971757766E-21},{"$f":"AF4976*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4977^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4977)*3600*24","v":0},0,{"$f":"AE4976-AD4977*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4977>$J$18,(AE4977/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.4590685971757766E-21,{"$error":"#N/A"},null,{"$f":"(AD4977)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4977>0,(AJ4977*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4976,NA())","v":{"$error":"#N/A"}},null,4960,{"$f":"IF(AF4977<=$J$9*0.05,AS4976*EXP((-$J$6*1)/Heterogenität!$D$4),Z4977)","v":4.2005774958970268E-5},{"$f":"IF(OR(AF4977>=$J$19, AR4976/$J$5<AN4977),0, Bodencharakterisierung!$E$8*$J$11*((AR4976/$J$5)-AN4977))","v":1.0454061650451492E-6},4.3553466664139672E-7,{"$f":"AQ4976-AP4977*Bodencharakterisierung!$E$8","v":1.3129788685651699E-4},{"$f":"AQ4977/(Bodencharakterisierung!$E$11*1000)","v":8.6665271852486456E-8},4.2441309625611665E-5,{"$error":"#N/A"},null,{"$f":"(AP4977)*$G$11*Bodencharakterisierung!$E$8","v":6.2982228641433519E-9},{"$f":"IF(AF4977<=$J$9*1.05,(AV4977*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4976,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.112294399997822,null,8.6665271852486458E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.005774958970271]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4961,3.4590685971757766E-21,{"$f":"Z4978*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.4235714765249203E-21},{"$f":"AF4977*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4978^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4978)*3600*24","v":0},0,{"$f":"AE4977-AD4978*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4978>$J$18,(AE4978/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.4235714765249203E-21,{"$error":"#N/A"},null,{"$f":"(AD4978)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4978>0,(AJ4978*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4977,NA())","v":{"$error":"#N/A"}},null,4961,{"$f":"IF(AF4978<=$J$9*0.05,AS4977*EXP((-$J$6*1)/Heterogenität!$D$4),Z4978)","v":4.2005774958970268E-5},{"$f":"IF(OR(AF4978>=$J$19, AR4977/$J$5<AN4978),0, Bodencharakterisierung!$E$8*$J$11*((AR4977/$J$5)-AN4978))","v":5.9536442776612232E-7},4.3553466664139672E-7,{"$f":"AQ4977-AP4978*Bodencharakterisierung!$E$8","v":1.3115416041652533E-4},{"$f":"AQ4978/(Bodencharakterisierung!$E$11*1000)","v":8.6570402915198244E-8},4.2441309625611665E-5,{"$error":"#N/A"},null,{"$f":"(AP4978)*$G$11*Bodencharakterisierung!$E$8","v":6.2982228641433519E-9},{"$f":"IF(AF4978<=$J$9*1.05,(AV4978*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4977,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.118567039997821,null,8.6570402915198241E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.005774958970271]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4962,3.4235714765249203E-21,{"$f":"Z4979*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.3884386289548384E-21},{"$f":"AF4978*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4979^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4979)*3600*24","v":0},0,{"$f":"AE4978-AD4979*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4979>$J$18,(AE4979/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.3884386289548384E-21,{"$error":"#N/A"},null,{"$f":"(AD4979)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4979>0,(AJ4979*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4978,NA())","v":{"$error":"#N/A"}},null,4962,{"$f":"IF(AF4979<=$J$9*0.05,AS4978*EXP((-$J$6*1)/Heterogenität!$D$4),Z4979)","v":4.2005774958970268E-5},{"$f":"IF(OR(AF4979>=$J$19, AR4978/$J$5<AN4979),0, Bodencharakterisierung!$E$8*$J$11*((AR4978/$J$5)-AN4979))","v":1.4532269048716171E-7},1.4532269048716171E-7,{"$f":"AQ4978-AP4979*Bodencharakterisierung!$E$8","v":1.3110620392866457E-4},{"$f":"AQ4979/(Bodencharakterisierung!$E$11*1000)","v":8.6538748467765386E-8},4.2151097649457432E-5,{"$error":"#N/A"},null,{"$f":"(AP4979)*$G$11*Bodencharakterisierung!$E$8","v":2.1014967625038057E-9},{"$f":"IF(AF4979<=$J$9*1.05,(AV4979*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4978,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.12483967999782,null,8.6538748467765381E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,42.005774958970271]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4963,3.3884386289548384E-21,{"$f":"Z4980*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.3536663162784621E-21},{"$f":"AF4979*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4980^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4980)*3600*24","v":0},0,{"$f":"AE4979-AD4980*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4980>$J$18,(AE4980/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.3536663162784621E-21,{"$error":"#N/A"},null,{"$f":"(AD4980)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4980>0,(AJ4980*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4979,NA())","v":{"$error":"#N/A"}},null,4963,{"$f":"IF(AF4980<=$J$9*0.05,AS4979*EXP((-$J$6*1)/Heterogenität!$D$4),Z4980)","v":4.1718541151430642E-5},{"$f":"IF(OR(AF4980>=$J$19, AR4979/$J$5<AN4980),0, Bodencharakterisierung!$E$8*$J$11*((AR4979/$J$5)-AN4980))","v":2.8023445425305139E-6},4.3255649802679023E-7,{"$f":"AQ4979-AP4980*Bodencharakterisierung!$E$8","v":1.3096346028431573E-4},{"$f":"AQ4980/(Bodencharakterisierung!$E$11*1000)","v":8.6444528240472428E-8},4.2151097649457432E-5,{"$error":"#N/A"},null,{"$f":"(AP4980)*$G$11*Bodencharakterisierung!$E$8","v":6.2551558683369477E-9},{"$f":"IF(AF4980<=$J$9*1.05,(AV4980*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4979,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.131112319997818,null,8.6444528240472426E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,41.718541151430642]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4964,3.3536663162784621E-21,{"$f":"Z4981*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.3192508386701706E-21},{"$f":"AF4980*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4981^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4981)*3600*24","v":0},0,{"$f":"AE4980-AD4981*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4981>$J$18,(AE4981/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.3192508386701706E-21,{"$error":"#N/A"},null,{"$f":"(AD4981)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4981>0,(AJ4981*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4980,NA())","v":{"$error":"#N/A"}},null,4964,{"$f":"IF(AF4981<=$J$9*0.05,AS4980*EXP((-$J$6*1)/Heterogenität!$D$4),Z4981)","v":4.1718541151430642E-5},{"$f":"IF(OR(AF4981>=$J$19, AR4980/$J$5<AN4981),0, Bodencharakterisierung!$E$8*$J$11*((AR4980/$J$5)-AN4981))","v":2.3553801726343591E-6},4.3255649802679023E-7,{"$f":"AQ4980-AP4981*Bodencharakterisierung!$E$8","v":1.308207166399669E-4},{"$f":"AQ4981/(Bodencharakterisierung!$E$11*1000)","v":8.635030801317947E-8},4.2151097649457432E-5,{"$error":"#N/A"},null,{"$f":"(AP4981)*$G$11*Bodencharakterisierung!$E$8","v":6.2551558683369477E-9},{"$f":"IF(AF4981<=$J$9*1.05,(AV4981*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4980,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.137384959997817,null,8.6350308013179472E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,41.718541151430642]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4965,3.3192508386701706E-21,{"$f":"Z4982*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.2851885342721226E-21},{"$f":"AF4981*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4982^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4982)*3600*24","v":0},0,{"$f":"AE4981-AD4982*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4982>$J$18,(AE4982/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.2851885342721226E-21,{"$error":"#N/A"},null,{"$f":"(AD4982)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4982>0,(AJ4982*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4981,NA())","v":{"$error":"#N/A"}},null,4965,{"$f":"IF(AF4982<=$J$9*0.05,AS4981*EXP((-$J$6*1)/Heterogenität!$D$4),Z4982)","v":4.1718541151430642E-5},{"$f":"IF(OR(AF4982>=$J$19, AR4981/$J$5<AN4982),0, Bodencharakterisierung!$E$8*$J$11*((AR4981/$J$5)-AN4982))","v":1.9084158027382038E-6},4.3255649802679023E-7,{"$f":"AQ4981-AP4982*Bodencharakterisierung!$E$8","v":1.3067797299561807E-4},{"$f":"AQ4982/(Bodencharakterisierung!$E$11*1000)","v":8.6256087785886512E-8},4.2151097649457432E-5,{"$error":"#N/A"},null,{"$f":"(AP4982)*$G$11*Bodencharakterisierung!$E$8","v":6.2551558683369477E-9},{"$f":"IF(AF4982<=$J$9*1.05,(AV4982*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4981,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.143657599997816,null,8.6256087785886518E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,41.718541151430642]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4966,3.2851885342721226E-21,{"$f":"Z4983*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.2514757788046313E-21},{"$f":"AF4982*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4983^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4983)*3600*24","v":0},0,{"$f":"AE4982-AD4983*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4983>$J$18,(AE4983/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.2514757788046313E-21,{"$error":"#N/A"},null,{"$f":"(AD4983)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4983>0,(AJ4983*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4982,NA())","v":{"$error":"#N/A"}},null,4966,{"$f":"IF(AF4983<=$J$9*0.05,AS4982*EXP((-$J$6*1)/Heterogenität!$D$4),Z4983)","v":4.1718541151430642E-5},{"$f":"IF(OR(AF4983>=$J$19, AR4982/$J$5<AN4983),0, Bodencharakterisierung!$E$8*$J$11*((AR4982/$J$5)-AN4983))","v":1.461451432842115E-6},4.3255649802679023E-7,{"$f":"AQ4982-AP4983*Bodencharakterisierung!$E$8","v":1.3053522935126924E-4},{"$f":"AQ4983/(Bodencharakterisierung!$E$11*1000)","v":8.6161867558593554E-8},4.2151097649457432E-5,{"$error":"#N/A"},null,{"$f":"(AP4983)*$G$11*Bodencharakterisierung!$E$8","v":6.2551558683369477E-9},{"$f":"IF(AF4983<=$J$9*1.05,(AV4983*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4982,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.149930239997815,null,8.616186755859355E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,41.718541151430642]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4967,3.2514757788046313E-21,{"$f":"Z4984*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.2181089851805331E-21},{"$f":"AF4983*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4984^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4984)*3600*24","v":0},0,{"$f":"AE4983-AD4984*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4984>$J$18,(AE4984/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.2181089851805331E-21,{"$error":"#N/A"},null,{"$f":"(AD4984)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4984>0,(AJ4984*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4983,NA())","v":{"$error":"#N/A"}},null,4967,{"$f":"IF(AF4984<=$J$9*0.05,AS4983*EXP((-$J$6*1)/Heterogenität!$D$4),Z4984)","v":4.1718541151430642E-5},{"$f":"IF(OR(AF4984>=$J$19, AR4983/$J$5<AN4984),0, Bodencharakterisierung!$E$8*$J$11*((AR4983/$J$5)-AN4984))","v":1.0144870629459599E-6},4.3255649802679023E-7,{"$f":"AQ4983-AP4984*Bodencharakterisierung!$E$8","v":1.3039248570692041E-4},{"$f":"AQ4984/(Bodencharakterisierung!$E$11*1000)","v":8.6067647331300596E-8},4.2151097649457432E-5,{"$error":"#N/A"},null,{"$f":"(AP4984)*$G$11*Bodencharakterisierung!$E$8","v":6.2551558683369477E-9},{"$f":"IF(AF4984<=$J$9*1.05,(AV4984*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4983,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.156202879997814,null,8.6067647331300595E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,41.718541151430642]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4968,3.2181089851805331E-21,{"$f":"Z4985*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.1850846031235176E-21},{"$f":"AF4984*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4985^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4985)*3600*24","v":0},0,{"$f":"AE4984-AD4985*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4985>$J$18,(AE4985/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.1850846031235176E-21,{"$error":"#N/A"},null,{"$f":"(AD4985)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4985>0,(AJ4985*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4984,NA())","v":{"$error":"#N/A"}},null,4968,{"$f":"IF(AF4985<=$J$9*0.05,AS4984*EXP((-$J$6*1)/Heterogenität!$D$4),Z4985)","v":4.1718541151430642E-5},{"$f":"IF(OR(AF4985>=$J$19, AR4984/$J$5<AN4985),0, Bodencharakterisierung!$E$8*$J$11*((AR4984/$J$5)-AN4985))","v":5.6752269304980481E-7},4.3255649802679023E-7,{"$f":"AQ4984-AP4985*Bodencharakterisierung!$E$8","v":1.3024974206257158E-4},{"$f":"AQ4985/(Bodencharakterisierung!$E$11*1000)","v":8.5973427104007638E-8},4.2151097649457432E-5,{"$error":"#N/A"},null,{"$f":"(AP4985)*$G$11*Bodencharakterisierung!$E$8","v":6.2551558683369477E-9},{"$f":"IF(AF4985<=$J$9*1.05,(AV4985*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4984,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.162475519997813,null,8.5973427104007641E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,41.718541151430642]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4969,3.1850846031235176E-21,{"$f":"Z4986*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.1523991187903738E-21},{"$f":"AF4985*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4986^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4986)*3600*24","v":0},0,{"$f":"AE4985-AD4986*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4986>$J$18,(AE4986/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.1523991187903738E-21,{"$error":"#N/A"},null,{"$f":"(AD4986)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4986>0,(AJ4986*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4985,NA())","v":{"$error":"#N/A"}},null,4969,{"$f":"IF(AF4986<=$J$9*0.05,AS4985*EXP((-$J$6*1)/Heterogenität!$D$4),Z4986)","v":4.1718541151430642E-5},{"$f":"IF(OR(AF4986>=$J$19, AR4985/$J$5<AN4986),0, Bodencharakterisierung!$E$8*$J$11*((AR4985/$J$5)-AN4986))","v":1.2055832315371596E-7},1.2055832315371596E-7,{"$f":"AQ4985-AP4986*Bodencharakterisierung!$E$8","v":1.3020995781593084E-4},{"$f":"AQ4986/(Bodencharakterisierung!$E$11*1000)","v":8.5947166875201877E-8},4.1839099474584356E-5,{"$error":"#N/A"},null,{"$f":"(AP4986)*$G$11*Bodencharakterisierung!$E$8","v":1.7433817454873211E-9},{"$f":"IF(AF4986<=$J$9*1.05,(AV4986*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4985,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.168748159997811,null,8.5947166875201875E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,41.718541151430642]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4970,{"$f":"AG4986","v":3.1523991187903738E-21},{"$f":"Z4987*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.12004905439711E-21},{"$f":"AF4986*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4987^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4987)*3600*24","v":0},{"$f":"MIN(AC4987,Z4987-AA4987)","v":0},{"$f":"AE4986-AD4987*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4987>$J$18,(AE4987/(Bodencharakterisierung!$E$11*1000)),0)","v":0},{"$f":"AA4987+AD4987","v":3.12004905439711E-21},{"$f":"IF(AD4987>0,Y4987,NA())","v":{"$error":"#N/A"}},null,{"$f":"(AD4987)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4987>0,(AJ4987*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4986,NA())","v":{"$error":"#N/A"}},null,4970,{"$f":"IF(AF4987<=$J$9*0.05,AS4986*EXP((-$J$6*1)/Heterogenität!$D$4),Z4987)","v":4.1409744716143004E-5},{"$f":"IF(OR(AF4987>=$J$19, AR4986/$J$5<AN4987),0, Bodencharakterisierung!$E$8*$J$11*((AR4986/$J$5)-AN4987))","v":3.0139046527994416E-6},{"$f":"MIN(AO4987,AS4986-AN4987)","v":4.2935475844135167E-7},{"$f":"AQ4986-AP4987*Bodencharakterisierung!$E$8","v":1.300682707456452E-4},{"$f":"AQ4987/(Bodencharakterisierung!$E$11*1000)","v":8.5853644056531483E-8},{"$f":"AN4987+AP4987","v":4.1839099474584356E-5},{"$f":"IF(AN4987>$G$5,AM4987,NA())","v":{"$error":"#N/A"}},null,{"$f":"(AP4987)*$G$11*Bodencharakterisierung!$E$8","v":6.2088558352820688E-9},{"$f":"IF(AF4987<=$J$9*1.05,(AV4987*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4986,NA())","v":{"$error":"#N/A"}},{"$f":"IF(BH4987>($G$5*10^6),BH4987*0.99,9999)","v":9999},{"$f":"AT4987+$G$3","v":{"$error":"#N/A"}},{"$f":"IF(ISNUMBER(AT4987),BA4987+BB4987+BC4987+$AZ$17,\"\")","v":""},{"$f":"IF(ISNUMBER(AK4987),AK4987,BA4986)","v":1.6399886323194495},{"$f":"IF(ISNUMBER(AW4987),AW4987,0)","v":0},31.17502079999781,null,{"$f":"AR4987*10^6","v":8.5853644056531481E-2},{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},{"$f":"AF4987*10^6","v":0},{"$f":"AN4987*10^6","v":41.409744716143003}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4971,3.12004905439711E-21,{"$f":"Z4988*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.0880309678489133E-21},{"$f":"AF4987*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4988^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4988)*3600*24","v":0},0,{"$f":"AE4987-AD4988*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4988>$J$18,(AE4988/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.0880309678489133E-21,{"$error":"#N/A"},null,{"$f":"(AD4988)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4988>0,(AJ4988*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4987,NA())","v":{"$error":"#N/A"}},null,4971,{"$f":"IF(AF4988<=$J$9*0.05,AS4987*EXP((-$J$6*1)/Heterogenität!$D$4),Z4988)","v":4.1409744716143004E-5},{"$f":"IF(OR(AF4988>=$J$19, AR4987/$J$5<AN4988),0, Bodencharakterisierung!$E$8*$J$11*((AR4987/$J$5)-AN4988))","v":2.5702486681036196E-6},4.2935475844135167E-7,{"$f":"AQ4987-AP4988*Bodencharakterisierung!$E$8","v":1.2992658367535955E-4},{"$f":"AQ4988/(Bodencharakterisierung!$E$11*1000)","v":8.576012123786109E-8},4.1839099474584356E-5,{"$error":"#N/A"},null,{"$f":"(AP4988)*$G$11*Bodencharakterisierung!$E$8","v":6.2088558352820688E-9},{"$f":"IF(AF4988<=$J$9*1.05,(AV4988*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4987,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.181293439997809,null,8.5760121237861087E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,41.409744716143003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4972,3.0880309678489133E-21,{"$f":"Z4989*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.0563414523739064E-21},{"$f":"AF4988*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4989^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4989)*3600*24","v":0},0,{"$f":"AE4988-AD4989*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4989>$J$18,(AE4989/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.0563414523739064E-21,{"$error":"#N/A"},null,{"$f":"(AD4989)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4989>0,(AJ4989*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4988,NA())","v":{"$error":"#N/A"}},null,4972,{"$f":"IF(AF4989<=$J$9*0.05,AS4988*EXP((-$J$6*1)/Heterogenität!$D$4),Z4989)","v":4.1409744716143004E-5},{"$f":"IF(OR(AF4989>=$J$19, AR4988/$J$5<AN4989),0, Bodencharakterisierung!$E$8*$J$11*((AR4988/$J$5)-AN4989))","v":2.1265926834077976E-6},4.2935475844135167E-7,{"$f":"AQ4988-AP4989*Bodencharakterisierung!$E$8","v":1.2978489660507391E-4},{"$f":"AQ4989/(Bodencharakterisierung!$E$11*1000)","v":8.5666598419190696E-8},4.1839099474584356E-5,{"$error":"#N/A"},null,{"$f":"(AP4989)*$G$11*Bodencharakterisierung!$E$8","v":6.2088558352820688E-9},{"$f":"IF(AF4989<=$J$9*1.05,(AV4989*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4988,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.187566079997808,null,8.5666598419190693E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,41.409744716143003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4973,3.0563414523739064E-21,{"$f":"Z4990*EXP((-$J$6/Heterogenität!$D$4)*1)","v":3.024977136160661E-21},{"$f":"AF4989*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4990^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4990)*3600*24","v":0},0,{"$f":"AE4989-AD4990*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4990>$J$18,(AE4990/(Bodencharakterisierung!$E$11*1000)),0)","v":0},3.024977136160661E-21,{"$error":"#N/A"},null,{"$f":"(AD4990)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4990>0,(AJ4990*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4989,NA())","v":{"$error":"#N/A"}},null,4973,{"$f":"IF(AF4990<=$J$9*0.05,AS4989*EXP((-$J$6*1)/Heterogenität!$D$4),Z4990)","v":4.1409744716143004E-5},{"$f":"IF(OR(AF4990>=$J$19, AR4989/$J$5<AN4990),0, Bodencharakterisierung!$E$8*$J$11*((AR4989/$J$5)-AN4990))","v":1.6829366987119756E-6},4.2935475844135167E-7,{"$f":"AQ4989-AP4990*Bodencharakterisierung!$E$8","v":1.2964320953478826E-4},{"$f":"AQ4990/(Bodencharakterisierung!$E$11*1000)","v":8.5573075600520302E-8},4.1839099474584356E-5,{"$error":"#N/A"},null,{"$f":"(AP4990)*$G$11*Bodencharakterisierung!$E$8","v":6.2088558352820688E-9},{"$f":"IF(AF4990<=$J$9*1.05,(AV4990*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4989,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.193838719997807,null,8.5573075600520299E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,41.409744716143003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4974,3.024977136160661E-21,{"$f":"Z4991*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.993934681999432E-21},{"$f":"AF4990*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4991^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4991)*3600*24","v":0},0,{"$f":"AE4990-AD4991*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4991>$J$18,(AE4991/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.993934681999432E-21,{"$error":"#N/A"},null,{"$f":"(AD4991)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4991>0,(AJ4991*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4990,NA())","v":{"$error":"#N/A"}},null,4974,{"$f":"IF(AF4991<=$J$9*0.05,AS4990*EXP((-$J$6*1)/Heterogenität!$D$4),Z4991)","v":4.1409744716143004E-5},{"$f":"IF(OR(AF4991>=$J$19, AR4990/$J$5<AN4991),0, Bodencharakterisierung!$E$8*$J$11*((AR4990/$J$5)-AN4991))","v":1.2392807140160873E-6},4.2935475844135167E-7,{"$f":"AQ4990-AP4991*Bodencharakterisierung!$E$8","v":1.2950152246450262E-4},{"$f":"AQ4991/(Bodencharakterisierung!$E$11*1000)","v":8.5479552781849909E-8},4.1839099474584356E-5,{"$error":"#N/A"},null,{"$f":"(AP4991)*$G$11*Bodencharakterisierung!$E$8","v":6.2088558352820688E-9},{"$f":"IF(AF4991<=$J$9*1.05,(AV4991*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4990,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.200111359997805,null,8.5479552781849905E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,41.409744716143003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4975,2.993934681999432E-21,{"$f":"Z4992*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.9632107869270744E-21},{"$f":"AF4991*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4992^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4992)*3600*24","v":0},0,{"$f":"AE4991-AD4992*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4992>$J$18,(AE4992/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.9632107869270744E-21,{"$error":"#N/A"},null,{"$f":"(AD4992)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4992>0,(AJ4992*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4991,NA())","v":{"$error":"#N/A"}},null,4975,{"$f":"IF(AF4992<=$J$9*0.05,AS4991*EXP((-$J$6*1)/Heterogenität!$D$4),Z4992)","v":4.1409744716143004E-5},{"$f":"IF(OR(AF4992>=$J$19, AR4991/$J$5<AN4992),0, Bodencharakterisierung!$E$8*$J$11*((AR4991/$J$5)-AN4992))","v":7.9562472932026536E-7},4.2935475844135167E-7,{"$f":"AQ4991-AP4992*Bodencharakterisierung!$E$8","v":1.2935983539421697E-4},{"$f":"AQ4992/(Bodencharakterisierung!$E$11*1000)","v":8.5386029963179515E-8},4.1839099474584356E-5,{"$error":"#N/A"},null,{"$f":"(AP4992)*$G$11*Bodencharakterisierung!$E$8","v":6.2088558352820688E-9},{"$f":"IF(AF4992<=$J$9*1.05,(AV4992*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4991,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.206383999997804,null,8.5386029963179511E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,41.409744716143003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4976,2.9632107869270744E-21,{"$f":"Z4993*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.9328021818756022E-21},{"$f":"AF4992*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4993^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4993)*3600*24","v":0},0,{"$f":"AE4992-AD4993*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4993>$J$18,(AE4993/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.9328021818756022E-21,{"$error":"#N/A"},null,{"$f":"(AD4993)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4993>0,(AJ4993*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4992,NA())","v":{"$error":"#N/A"}},null,4976,{"$f":"IF(AF4993<=$J$9*0.05,AS4992*EXP((-$J$6*1)/Heterogenität!$D$4),Z4993)","v":4.1409744716143004E-5},{"$f":"IF(OR(AF4993>=$J$19, AR4992/$J$5<AN4993),0, Bodencharakterisierung!$E$8*$J$11*((AR4992/$J$5)-AN4993))","v":3.5196874462444332E-7},3.5196874462444332E-7,{"$f":"AQ4992-AP4993*Bodencharakterisierung!$E$8","v":1.2924368570849091E-4},{"$f":"AQ4993/(Bodencharakterisierung!$E$11*1000)","v":8.5309363503954395E-8},4.176171346076745E-5,{"$error":"#N/A"},null,{"$f":"(AP4993)*$G$11*Bodencharakterisierung!$E$8","v":5.0897844985614307E-9},{"$f":"IF(AF4993<=$J$9*1.05,(AV4993*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4992,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.212656639997803,null,8.5309363503954391E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,41.409744716143003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4977,2.9328021818756022E-21,{"$f":"Z4994*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.9027056313243551E-21},{"$f":"AF4993*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4994^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4994)*3600*24","v":0},0,{"$f":"AE4993-AD4994*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4994>$J$18,(AE4994/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.9027056313243551E-21,{"$error":"#N/A"},null,{"$f":"(AD4994)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4994>0,(AJ4994*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4993,NA())","v":{"$error":"#N/A"}},null,4977,{"$f":"IF(AF4994<=$J$9*0.05,AS4993*EXP((-$J$6*1)/Heterogenität!$D$4),Z4994)","v":4.1333152841150461E-5},{"$f":"IF(OR(AF4994>=$J$19, AR4993/$J$5<AN4994),0, Bodencharakterisierung!$E$8*$J$11*((AR4993/$J$5)-AN4994))","v":7.3682186916514221E-7},4.285606196169898E-7,{"$f":"AQ4993-AP4994*Bodencharakterisierung!$E$8","v":1.2910226070401729E-4},{"$f":"AQ4994/(Bodencharakterisierung!$E$11*1000)","v":8.5216013666018017E-8},4.176171346076745E-5,{"$error":"#N/A"},null,{"$f":"(AP4994)*$G$11*Bodencharakterisierung!$E$8","v":6.1973718738801677E-9},{"$f":"IF(AF4994<=$J$9*1.05,(AV4994*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4993,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.218929279997802,null,8.5216013666018012E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,41.333152841150458]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4978,2.9027056313243551E-21,{"$f":"Z4995*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.8729179329557347E-21},{"$f":"AF4994*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4995^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4995)*3600*24","v":0},0,{"$f":"AE4994-AD4995*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4995>$J$18,(AE4995/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.8729179329557347E-21,{"$error":"#N/A"},null,{"$f":"(AD4995)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4995>0,(AJ4995*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4994,NA())","v":{"$error":"#N/A"}},null,4978,{"$f":"IF(AF4995<=$J$9*0.05,AS4994*EXP((-$J$6*1)/Heterogenität!$D$4),Z4995)","v":4.1333152841150461E-5},{"$f":"IF(OR(AF4995>=$J$19, AR4994/$J$5<AN4995),0, Bodencharakterisierung!$E$8*$J$11*((AR4994/$J$5)-AN4995))","v":2.9398647498372858E-7},2.9398647498372858E-7,{"$f":"AQ4994-AP4995*Bodencharakterisierung!$E$8","v":1.2900524516727265E-4},{"$f":"AQ4995/(Bodencharakterisierung!$E$11*1000)","v":8.5151977008100761E-8},4.162713931613419E-5,{"$error":"#N/A"},null,{"$f":"(AP4995)*$G$11*Bodencharakterisierung!$E$8","v":4.2513087483251018E-9},{"$f":"IF(AF4995<=$J$9*1.05,(AV4995*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4994,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.225201919997801,null,8.515197700810076E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,41.333152841150458]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4979,2.8729179329557347E-21,{"$f":"Z4996*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.8434359173144717E-21},{"$f":"AF4995*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4996^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4996)*3600*24","v":0},0,{"$f":"AE4995-AD4996*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4996>$J$18,(AE4996/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.8434359173144717E-21,{"$error":"#N/A"},null,{"$f":"(AD4996)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4996>0,(AJ4996*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4995,NA())","v":{"$error":"#N/A"}},null,4979,{"$f":"IF(AF4996<=$J$9*0.05,AS4995*EXP((-$J$6*1)/Heterogenität!$D$4),Z4996)","v":4.1199959702563861E-5},{"$f":"IF(OR(AF4996>=$J$19, AR4995/$J$5<AN4996),0, Bodencharakterisierung!$E$8*$J$11*((AR4995/$J$5)-AN4996))","v":1.291926993619982E-6},4.2717961357032885E-7,{"$f":"AQ4995-AP4996*Bodencharakterisierung!$E$8","v":1.2886427589479444E-4},{"$f":"AQ4996/(Bodencharakterisierung!$E$11*1000)","v":8.5058927983362669E-8},4.162713931613419E-5,{"$error":"#N/A"},null,{"$f":"(AP4996)*$G$11*Bodencharakterisierung!$E$8","v":6.1774012847978483E-9},{"$f":"IF(AF4996<=$J$9*1.05,(AV4996*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4995,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.2314745599978,null,8.5058927983362675E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,41.199959702563859]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4980,2.8434359173144717E-21,{"$f":"Z4997*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.8142564474703935E-21},{"$f":"AF4996*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4997^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4997)*3600*24","v":0},0,{"$f":"AE4996-AD4997*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4997>$J$18,(AE4997/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.8142564474703935E-21,{"$error":"#N/A"},null,{"$f":"(AD4997)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4997>0,(AJ4997*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4996,NA())","v":{"$error":"#N/A"}},null,4980,{"$f":"IF(AF4997<=$J$9*0.05,AS4996*EXP((-$J$6*1)/Heterogenität!$D$4),Z4997)","v":4.1199959702563861E-5},{"$f":"IF(OR(AF4997>=$J$19, AR4996/$J$5<AN4997),0, Bodencharakterisierung!$E$8*$J$11*((AR4996/$J$5)-AN4997))","v":8.5051860492867918E-7},4.2717961357032885E-7,{"$f":"AQ4996-AP4997*Bodencharakterisierung!$E$8","v":1.2872330662231624E-4},{"$f":"AQ4997/(Bodencharakterisierung!$E$11*1000)","v":8.4965878958624577E-8},4.162713931613419E-5,{"$error":"#N/A"},null,{"$f":"(AP4997)*$G$11*Bodencharakterisierung!$E$8","v":6.1774012847978483E-9},{"$f":"IF(AF4997<=$J$9*1.05,(AV4997*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4996,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.237747199997798,null,8.4965878958624577E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,41.199959702563859]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4981,2.8142564474703935E-21,{"$f":"Z4998*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.7853764186846477E-21},{"$f":"AF4997*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4998^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4998)*3600*24","v":0},0,{"$f":"AE4997-AD4998*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4998>$J$18,(AE4998/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.7853764186846477E-21,{"$error":"#N/A"},null,{"$f":"(AD4998)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4998>0,(AJ4998*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4997,NA())","v":{"$error":"#N/A"}},null,4981,{"$f":"IF(AF4998<=$J$9*0.05,AS4997*EXP((-$J$6*1)/Heterogenität!$D$4),Z4998)","v":4.1199959702563861E-5},{"$f":"IF(OR(AF4998>=$J$19, AR4997/$J$5<AN4998),0, Bodencharakterisierung!$E$8*$J$11*((AR4997/$J$5)-AN4998))","v":4.0911021623737625E-7},4.0911021623737625E-7,{"$f":"AQ4997-AP4998*Bodencharakterisierung!$E$8","v":1.285883002509579E-4},{"$f":"AQ4998/(Bodencharakterisierung!$E$11*1000)","v":8.4876765842216434E-8},4.1609069918801239E-5,{"$error":"#N/A"},null,{"$f":"(AP4998)*$G$11*Bodencharakterisierung!$E$8","v":5.9161015533636207E-9},{"$f":"IF(AF4998<=$J$9*1.05,(AV4998*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4997,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.244019839997797,null,8.4876765842216428E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,41.199959702563859]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4982,2.7853764186846477E-21,{"$f":"Z4999*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.756792758079355E-21},{"$f":"AF4998*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB4999^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z4999)*3600*24","v":0},0,{"$f":"AE4998-AD4999*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE4999>$J$18,(AE4999/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.756792758079355E-21,{"$error":"#N/A"},null,{"$f":"(AD4999)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH4999>0,(AJ4999*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4998,NA())","v":{"$error":"#N/A"}},null,4982,{"$f":"IF(AF4999<=$J$9*0.05,AS4998*EXP((-$J$6*1)/Heterogenität!$D$4),Z4999)","v":4.1182075734215387E-5},{"$f":"IF(OR(AF4999>=$J$19, AR4998/$J$5<AN4999),0, Bodencharakterisierung!$E$8*$J$11*((AR4998/$J$5)-AN4999))","v":1.6115616832901954E-7},1.6115616832901954E-7,{"$f":"AQ4998-AP4999*Bodencharakterisierung!$E$8","v":1.2853511871540932E-4},{"$f":"AQ4999/(Bodencharakterisierung!$E$11*1000)","v":8.4841662518421993E-8},4.1343231902544409E-5,{"$error":"#N/A"},null,{"$f":"(AP4999)*$G$11*Bodencharakterisierung!$E$8","v":2.3304630878057687E-9},{"$f":"IF(AF4999<=$J$9*1.05,(AV4999*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4998,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.250292479997796,null,8.4841662518421998E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,41.182075734215388]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4983,2.756792758079355E-21,{"$f":"Z5000*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.7285024243106501E-21},{"$f":"AF4999*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB5000^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z5000)*3600*24","v":0},0,{"$f":"AE4999-AD5000*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE5000>$J$18,(AE5000/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.7285024243106501E-21,{"$error":"#N/A"},null,{"$f":"(AD5000)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH5000>0,(AJ5000*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK4999,NA())","v":{"$error":"#N/A"}},null,4983,{"$f":"IF(AF5000<=$J$9*0.05,AS4999*EXP((-$J$6*1)/Heterogenität!$D$4),Z5000)","v":4.091896575987839E-5},{"$f":"IF(OR(AF5000>=$J$19, AR4999/$J$5<AN5000),0, Bodencharakterisierung!$E$8*$J$11*((AR4999/$J$5)-AN5000))","v":2.5660508098899276E-6},4.2426614266601916E-7,{"$f":"AQ4999-AP5000*Bodencharakterisierung!$E$8","v":1.2839511088832953E-4},{"$f":"AQ5000/(Bodencharakterisierung!$E$11*1000)","v":8.4749248111108607E-8},4.1343231902544409E-5,{"$error":"#N/A"},null,{"$f":"(AP5000)*$G$11*Bodencharakterisierung!$E$8","v":6.1352698760513478E-9},{"$f":"IF(AF5000<=$J$9*1.05,(AV5000*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW4999,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.256565119997795,null,8.4749248111108608E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,40.91896575987839]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4984,2.7285024243106501E-21,{"$f":"Z5001*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.7005024072450775E-21},{"$f":"AF5000*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB5001^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z5001)*3600*24","v":0},0,{"$f":"AE5000-AD5001*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE5001>$J$18,(AE5001/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.7005024072450775E-21,{"$error":"#N/A"},null,{"$f":"(AD5001)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH5001>0,(AJ5001*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK5000,NA())","v":{"$error":"#N/A"}},null,4984,{"$f":"IF(AF5001<=$J$9*0.05,AS5000*EXP((-$J$6*1)/Heterogenität!$D$4),Z5001)","v":4.091896575987839E-5},{"$f":"IF(OR(AF5001>=$J$19, AR5000/$J$5<AN5001),0, Bodencharakterisierung!$E$8*$J$11*((AR5000/$J$5)-AN5001))","v":2.1276529358779933E-6},4.2426614266601916E-7,{"$f":"AQ5000-AP5001*Bodencharakterisierung!$E$8","v":1.2825510306124974E-4},{"$f":"AQ5001/(Bodencharakterisierung!$E$11*1000)","v":8.4656833703795207E-8},4.1343231902544409E-5,{"$error":"#N/A"},null,{"$f":"(AP5001)*$G$11*Bodencharakterisierung!$E$8","v":6.1352698760513478E-9},{"$f":"IF(AF5001<=$J$9*1.05,(AV5001*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW5000,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.262837759997794,null,8.4656833703795203E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,40.91896575987839]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4985,2.7005024072450775E-21,{"$f":"Z5002*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.6727897276393095E-21},{"$f":"AF5001*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB5002^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z5002)*3600*24","v":0},0,{"$f":"AE5001-AD5002*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE5002>$J$18,(AE5002/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.6727897276393095E-21,{"$error":"#N/A"},null,{"$f":"(AD5002)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH5002>0,(AJ5002*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK5001,NA())","v":{"$error":"#N/A"}},null,4985,{"$f":"IF(AF5002<=$J$9*0.05,AS5001*EXP((-$J$6*1)/Heterogenität!$D$4),Z5002)","v":4.091896575987839E-5},{"$f":"IF(OR(AF5002>=$J$19, AR5001/$J$5<AN5002),0, Bodencharakterisierung!$E$8*$J$11*((AR5001/$J$5)-AN5002))","v":1.6892550618659925E-6},4.2426614266601916E-7,{"$f":"AQ5001-AP5002*Bodencharakterisierung!$E$8","v":1.2811509523416996E-4},{"$f":"AQ5002/(Bodencharakterisierung!$E$11*1000)","v":8.4564419296481821E-8},4.1343231902544409E-5,{"$error":"#N/A"},null,{"$f":"(AP5002)*$G$11*Bodencharakterisierung!$E$8","v":6.1352698760513478E-9},{"$f":"IF(AF5002<=$J$9*1.05,(AV5002*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW5001,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.269110399997793,null,8.4564419296481827E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,40.91896575987839]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4986,2.6727897276393095E-21,{"$f":"Z5003*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.6453614368231504E-21},{"$f":"AF5002*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB5003^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z5003)*3600*24","v":0},0,{"$f":"AE5002-AD5003*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE5003>$J$18,(AE5003/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.6453614368231504E-21,{"$error":"#N/A"},null,{"$f":"(AD5003)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH5003>0,(AJ5003*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK5002,NA())","v":{"$error":"#N/A"}},null,4986,{"$f":"IF(AF5003<=$J$9*0.05,AS5002*EXP((-$J$6*1)/Heterogenität!$D$4),Z5003)","v":4.091896575987839E-5},{"$f":"IF(OR(AF5003>=$J$19, AR5002/$J$5<AN5003),0, Bodencharakterisierung!$E$8*$J$11*((AR5002/$J$5)-AN5003))","v":1.2508571878541245E-6},4.2426614266601916E-7,{"$f":"AQ5002-AP5003*Bodencharakterisierung!$E$8","v":1.2797508740709017E-4},{"$f":"AQ5003/(Bodencharakterisierung!$E$11*1000)","v":8.4472004889168434E-8},4.1343231902544409E-5,{"$error":"#N/A"},null,{"$f":"(AP5003)*$G$11*Bodencharakterisierung!$E$8","v":6.1352698760513478E-9},{"$f":"IF(AF5003<=$J$9*1.05,(AV5003*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW5002,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.275383039997791,null,8.4472004889168437E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,40.91896575987839]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4987,2.6453614368231504E-21,{"$f":"Z5004*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.618214616385793E-21},{"$f":"AF5003*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB5004^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z5004)*3600*24","v":0},0,{"$f":"AE5003-AD5004*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE5004>$J$18,(AE5004/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.618214616385793E-21,{"$error":"#N/A"},null,{"$f":"(AD5004)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH5004>0,(AJ5004*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK5003,NA())","v":{"$error":"#N/A"}},null,4987,{"$f":"IF(AF5004<=$J$9*0.05,AS5003*EXP((-$J$6*1)/Heterogenität!$D$4),Z5004)","v":4.091896575987839E-5},{"$f":"IF(OR(AF5004>=$J$19, AR5003/$J$5<AN5004),0, Bodencharakterisierung!$E$8*$J$11*((AR5003/$J$5)-AN5004))","v":8.1245931384218999E-7},4.2426614266601916E-7,{"$f":"AQ5003-AP5004*Bodencharakterisierung!$E$8","v":1.2783507958001039E-4},{"$f":"AQ5004/(Bodencharakterisierung!$E$11*1000)","v":8.4379590481855034E-8},4.1343231902544409E-5,{"$error":"#N/A"},null,{"$f":"(AP5004)*$G$11*Bodencharakterisierung!$E$8","v":6.1352698760513478E-9},{"$f":"IF(AF5004<=$J$9*1.05,(AV5004*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW5003,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.28165567999779,null,8.4379590481855032E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,40.91896575987839]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4988,2.618214616385793E-21,{"$f":"Z5005*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.5913463778652959E-21},{"$f":"AF5004*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB5005^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z5005)*3600*24","v":0},0,{"$f":"AE5004-AD5005*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE5005>$J$18,(AE5005/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.5913463778652959E-21,{"$error":"#N/A"},null,{"$f":"(AD5005)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH5005>0,(AJ5005*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK5004,NA())","v":{"$error":"#N/A"}},null,4988,{"$f":"IF(AF5005<=$J$9*0.05,AS5004*EXP((-$J$6*1)/Heterogenität!$D$4),Z5005)","v":4.091896575987839E-5},{"$f":"IF(OR(AF5005>=$J$19, AR5004/$J$5<AN5005),0, Bodencharakterisierung!$E$8*$J$11*((AR5004/$J$5)-AN5005))","v":3.7406143983018936E-7},3.7406143983018936E-7,{"$f":"AQ5004-AP5005*Bodencharakterisierung!$E$8","v":1.2771163930486642E-4},{"$f":"AQ5005/(Bodencharakterisierung!$E$11*1000)","v":8.4298111752387071E-8},4.1293027199708576E-5,{"$error":"#N/A"},null,{"$f":"(AP5005)*$G$11*Bodencharakterisierung!$E$8","v":5.4092647345398594E-9},{"$f":"IF(AF5005<=$J$9*1.05,(AV5005*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW5004,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.287928319997789,null,8.4298111752387064E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,40.91896575987839]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4989,2.5913463778652959E-21,{"$f":"Z5006*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.5647538624412462E-21},{"$f":"AF5005*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB5006^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z5006)*3600*24","v":0},0,{"$f":"AE5005-AD5006*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE5006>$J$18,(AE5006/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.5647538624412462E-21,{"$error":"#N/A"},null,{"$f":"(AD5006)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH5006>0,(AJ5006*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK5005,NA())","v":{"$error":"#N/A"}},null,4989,{"$f":"IF(AF5006<=$J$9*0.05,AS5005*EXP((-$J$6*1)/Heterogenität!$D$4),Z5006)","v":4.0869276260006514E-5},{"$f":"IF(OR(AF5006>=$J$19, AR5005/$J$5<AN5006),0, Bodencharakterisierung!$E$8*$J$11*((AR5005/$J$5)-AN5006))","v":4.7316448587362549E-7},4.237509397020625E-7,{"$f":"AQ5005-AP5006*Bodencharakterisierung!$E$8","v":1.2757180149476475E-4},{"$f":"AQ5006/(Bodencharakterisierung!$E$11*1000)","v":8.4205809567501488E-8},4.1293027199708576E-5,{"$error":"#N/A"},null,{"$f":"(AP5006)*$G$11*Bodencharakterisierung!$E$8","v":6.1278195779791211E-9},{"$f":"IF(AF5006<=$J$9*1.05,(AV5006*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW5005,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.294200959997788,null,8.4205809567501483E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,40.869276260006515]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4990,2.5647538624412462E-21,{"$f":"Z5007*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.538434240630578E-21},{"$f":"AF5006*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB5007^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z5007)*3600*24","v":0},0,{"$f":"AE5006-AD5007*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE5007>$J$18,(AE5007/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.538434240630578E-21,{"$error":"#N/A"},null,{"$f":"(AD5007)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH5007>0,(AJ5007*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK5006,NA())","v":{"$error":"#N/A"}},null,4990,{"$f":"IF(AF5007<=$J$9*0.05,AS5006*EXP((-$J$6*1)/Heterogenität!$D$4),Z5007)","v":4.0869276260006514E-5},{"$f":"IF(OR(AF5007>=$J$19, AR5006/$J$5<AN5007),0, Bodencharakterisierung!$E$8*$J$11*((AR5006/$J$5)-AN5007))","v":3.5298975539531816E-8},3.5298975539531816E-8,{"$f":"AQ5006-AP5007*Bodencharakterisierung!$E$8","v":1.275601528328367E-4},{"$f":"AQ5007/(Bodencharakterisierung!$E$11*1000)","v":8.4198120681740393E-8},4.0904575235546045E-5,{"$error":"#N/A"},null,{"$f":"(AP5007)*$G$11*Bodencharakterisierung!$E$8","v":5.1045492322880236E-10},{"$f":"IF(AF5007<=$J$9*1.05,(AV5007*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW5006,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.300473599997787,null,8.4198120681740388E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,40.869276260006515]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4991,2.538434240630578E-21,{"$f":"Z5008*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.5123847119865098E-21},{"$f":"AF5007*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB5008^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z5008)*3600*24","v":0},0,{"$f":"AE5007-AD5008*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE5008>$J$18,(AE5008/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.5123847119865098E-21,{"$error":"#N/A"},null,{"$f":"(AD5008)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH5008>0,(AJ5008*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK5007,NA())","v":{"$error":"#N/A"}},null,4991,{"$f":"IF(AF5008<=$J$9*0.05,AS5007*EXP((-$J$6*1)/Heterogenität!$D$4),Z5008)","v":4.0484810607722907E-5},{"$f":"IF(OR(AF5008>=$J$19, AR5007/$J$5<AN5008),0, Bodencharakterisierung!$E$8*$J$11*((AR5007/$J$5)-AN5008))","v":3.7562727041786342E-6},4.1976462782313846E-7,{"$f":"AQ5007-AP5008*Bodencharakterisierung!$E$8","v":1.2742163050565505E-4},{"$f":"AQ5008/(Bodencharakterisierung!$E$11*1000)","v":8.4106686802412574E-8},4.0904575235546045E-5,{"$error":"#N/A"},null,{"$f":"(AP5008)*$G$11*Bodencharakterisierung!$E$8","v":6.0701739241599786E-9},{"$f":"IF(AF5008<=$J$9*1.05,(AV5008*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW5007,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.306746239997786,null,8.4106686802412581E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,40.484810607722906]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4992,2.5123847119865098E-21,{"$f":"Z5009*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.4866025048005739E-21},{"$f":"AF5008*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB5009^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z5009)*3600*24","v":0},0,{"$f":"AE5008-AD5009*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE5009>$J$18,(AE5009/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.4866025048005739E-21,{"$error":"#N/A"},null,{"$f":"(AD5009)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH5009>0,(AJ5009*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK5008,NA())","v":{"$error":"#N/A"}},null,4992,{"$f":"IF(AF5009<=$J$9*0.05,AS5008*EXP((-$J$6*1)/Heterogenität!$D$4),Z5009)","v":4.0484810607722907E-5},{"$f":"IF(OR(AF5009>=$J$19, AR5008/$J$5<AN5009),0, Bodencharakterisierung!$E$8*$J$11*((AR5008/$J$5)-AN5009))","v":3.3225262843801916E-6},4.1976462782313846E-7,{"$f":"AQ5008-AP5009*Bodencharakterisierung!$E$8","v":1.272831081784734E-4},{"$f":"AQ5009/(Bodencharakterisierung!$E$11*1000)","v":8.4015252923084756E-8},4.0904575235546045E-5,{"$error":"#N/A"},null,{"$f":"(AP5009)*$G$11*Bodencharakterisierung!$E$8","v":6.0701739241599786E-9},{"$f":"IF(AF5009<=$J$9*1.05,(AV5009*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW5008,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.313018879997784,null,8.401525292308476E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,40.484810607722906]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4993,2.4866025048005739E-21,{"$f":"Z5010*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.4610848758077018E-21},{"$f":"AF5009*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB5010^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z5010)*3600*24","v":0},0,{"$f":"AE5009-AD5010*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE5010>$J$18,(AE5010/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.4610848758077018E-21,{"$error":"#N/A"},null,{"$f":"(AD5010)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH5010>0,(AJ5010*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK5009,NA())","v":{"$error":"#N/A"}},null,4993,{"$f":"IF(AF5010<=$J$9*0.05,AS5009*EXP((-$J$6*1)/Heterogenität!$D$4),Z5010)","v":4.0484810607722907E-5},{"$f":"IF(OR(AF5010>=$J$19, AR5009/$J$5<AN5010),0, Bodencharakterisierung!$E$8*$J$11*((AR5009/$J$5)-AN5010))","v":2.888779864581749E-6},4.1976462782313846E-7,{"$f":"AQ5009-AP5010*Bodencharakterisierung!$E$8","v":1.2714458585129176E-4},{"$f":"AQ5010/(Bodencharakterisierung!$E$11*1000)","v":8.3923819043756937E-8},4.0904575235546045E-5,{"$error":"#N/A"},null,{"$f":"(AP5010)*$G$11*Bodencharakterisierung!$E$8","v":6.0701739241599786E-9},{"$f":"IF(AF5010<=$J$9*1.05,(AV5010*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW5009,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.319291519997783,null,8.3923819043756939E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,40.484810607722906]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4994,2.4610848758077018E-21,{"$f":"Z5011*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.4358291098943369E-21},{"$f":"AF5010*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB5011^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z5011)*3600*24","v":0},0,{"$f":"AE5010-AD5011*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE5011>$J$18,(AE5011/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.4358291098943369E-21,{"$error":"#N/A"},null,{"$f":"(AD5011)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH5011>0,(AJ5011*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK5010,NA())","v":{"$error":"#N/A"}},null,4994,{"$f":"IF(AF5011<=$J$9*0.05,AS5010*EXP((-$J$6*1)/Heterogenität!$D$4),Z5011)","v":4.0484810607722907E-5},{"$f":"IF(OR(AF5011>=$J$19, AR5010/$J$5<AN5011),0, Bodencharakterisierung!$E$8*$J$11*((AR5010/$J$5)-AN5011))","v":2.4550334447833064E-6},4.1976462782313846E-7,{"$f":"AQ5010-AP5011*Bodencharakterisierung!$E$8","v":1.2700606352411011E-4},{"$f":"AQ5011/(Bodencharakterisierung!$E$11*1000)","v":8.3832385164429119E-8},4.0904575235546045E-5,{"$error":"#N/A"},null,{"$f":"(AP5011)*$G$11*Bodencharakterisierung!$E$8","v":6.0701739241599786E-9},{"$f":"IF(AF5011<=$J$9*1.05,(AV5011*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW5010,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.325564159997782,null,8.3832385164429118E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,40.484810607722906]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4995,2.4358291098943369E-21,{"$f":"Z5012*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.4108325198095427E-21},{"$f":"AF5011*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB5012^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z5012)*3600*24","v":0},0,{"$f":"AE5011-AD5012*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE5012>$J$18,(AE5012/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.4108325198095427E-21,{"$error":"#N/A"},null,{"$f":"(AD5012)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH5012>0,(AJ5012*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK5011,NA())","v":{"$error":"#N/A"}},null,4995,{"$f":"IF(AF5012<=$J$9*0.05,AS5011*EXP((-$J$6*1)/Heterogenität!$D$4),Z5012)","v":4.0484810607722907E-5},{"$f":"IF(OR(AF5012>=$J$19, AR5011/$J$5<AN5012),0, Bodencharakterisierung!$E$8*$J$11*((AR5011/$J$5)-AN5012))","v":2.0212870249847973E-6},4.1976462782313846E-7,{"$f":"AQ5011-AP5012*Bodencharakterisierung!$E$8","v":1.2686754119692846E-4},{"$f":"AQ5012/(Bodencharakterisierung!$E$11*1000)","v":8.3740951285101301E-8},4.0904575235546045E-5,{"$error":"#N/A"},null,{"$f":"(AP5012)*$G$11*Bodencharakterisierung!$E$8","v":6.0701739241599786E-9},{"$f":"IF(AF5012<=$J$9*1.05,(AV5012*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW5011,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,{"$f":"$G$34/$G$12/$G$8+BC5011","v":31.331836799997781},null,8.3740951285101298E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,40.484810607722906]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4996,2.4108325198095427E-21,{"$f":"Z5013*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3860924458790756E-21},{"$f":"AF5012*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB5013^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z5013)*3600*24","v":0},0,{"$f":"AE5012-AD5013*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE5013>$J$18,(AE5013/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.3860924458790756E-21,{"$error":"#N/A"},null,{"$f":"(AD5013)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH5013>0,(AJ5013*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK5012,NA())","v":{"$error":"#N/A"}},null,4996,{"$f":"IF(AF5013<=$J$9*0.05,AS5012*EXP((-$J$6*1)/Heterogenität!$D$4),Z5013)","v":4.0484810607722907E-5},{"$f":"IF(OR(AF5013>=$J$19, AR5012/$J$5<AN5013),0, Bodencharakterisierung!$E$8*$J$11*((AR5012/$J$5)-AN5013))","v":1.5875406051863547E-6},4.1976462782313846E-7,{"$f":"AQ5012-AP5013*Bodencharakterisierung!$E$8","v":1.2672901886974682E-4},{"$f":"AQ5013/(Bodencharakterisierung!$E$11*1000)","v":8.3649517405773469E-8},4.0904575235546045E-5,{"$error":"#N/A"},null,{"$f":"(AP5013)*$G$11*Bodencharakterisierung!$E$8","v":6.0701739241599786E-9},{"$f":"IF(AF5013<=$J$9*1.05,(AV5013*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW5012,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.33810943999778,null,8.3649517405773463E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,40.484810607722906]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4997,2.3860924458790756E-21,{"$f":"Z5014*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.36160625572239E-21},{"$f":"AF5013*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB5014^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z5014)*3600*24","v":0},0,{"$f":"AE5013-AD5014*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE5014>$J$18,(AE5014/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.36160625572239E-21,{"$error":"#N/A"},null,{"$f":"(AD5014)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH5014>0,(AJ5014*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK5013,NA())","v":{"$error":"#N/A"}},null,4997,{"$f":"IF(AF5014<=$J$9*0.05,AS5013*EXP((-$J$6*1)/Heterogenität!$D$4),Z5014)","v":4.0484810607722907E-5},{"$f":"IF(OR(AF5014>=$J$19, AR5013/$J$5<AN5014),0, Bodencharakterisierung!$E$8*$J$11*((AR5013/$J$5)-AN5014))","v":1.1537941853878458E-6},4.1976462782313846E-7,{"$f":"AQ5013-AP5014*Bodencharakterisierung!$E$8","v":1.2659049654256517E-4},{"$f":"AQ5014/(Bodencharakterisierung!$E$11*1000)","v":8.355808352644565E-8},4.0904575235546045E-5,{"$error":"#N/A"},null,{"$f":"(AP5014)*$G$11*Bodencharakterisierung!$E$8","v":6.0701739241599786E-9},{"$f":"IF(AF5014<=$J$9*1.05,(AV5014*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW5013,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.344382079997779,null,8.3558083526445656E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,40.484810607722906]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4998,2.36160625572239E-21,{"$f":"Z5015*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3373713439725512E-21},{"$f":"AF5014*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB5015^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z5015)*3600*24","v":0},0,{"$f":"AE5014-AD5015*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE5015>$J$18,(AE5015/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.3373713439725512E-21,{"$error":"#N/A"},null,{"$f":"(AD5015)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH5015>0,(AJ5015*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK5014,NA())","v":{"$error":"#N/A"}},null,4998,{"$f":"IF(AF5015<=$J$9*0.05,AS5014*EXP((-$J$6*1)/Heterogenität!$D$4),Z5015)","v":4.0484810607722907E-5},{"$f":"IF(OR(AF5015>=$J$19, AR5014/$J$5<AN5015),0, Bodencharakterisierung!$E$8*$J$11*((AR5014/$J$5)-AN5015))","v":7.2004776558940315E-7},4.1976462782313846E-7,{"$f":"AQ5014-AP5015*Bodencharakterisierung!$E$8","v":1.2645197421538352E-4},{"$f":"AQ5015/(Bodencharakterisierung!$E$11*1000)","v":8.3466649647117832E-8},4.0904575235546045E-5,{"$error":"#N/A"},null,{"$f":"(AP5015)*$G$11*Bodencharakterisierung!$E$8","v":6.0701739241599786E-9},{"$f":"IF(AF5015<=$J$9*1.05,(AV5015*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW5014,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.350654719997777,null,8.3466649647117835E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,40.484810607722906]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4999,2.3373713439725512E-21,{"$f":"Z5016*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.3133851319990189E-21},{"$f":"AF5015*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB5016^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z5016)*3600*24","v":0},0,{"$f":"AE5015-AD5016*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE5016>$J$18,(AE5016/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.3133851319990189E-21,{"$error":"#N/A"},null,{"$f":"(AD5016)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH5016>0,(AJ5016*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK5015,NA())","v":{"$error":"#N/A"}},null,4999,{"$f":"IF(AF5016<=$J$9*0.05,AS5015*EXP((-$J$6*1)/Heterogenität!$D$4),Z5016)","v":4.0484810607722907E-5},{"$f":"IF(OR(AF5016>=$J$19, AR5015/$J$5<AN5016),0, Bodencharakterisierung!$E$8*$J$11*((AR5015/$J$5)-AN5016))","v":2.863013457909605E-7},2.863013457909605E-7,{"$f":"AQ5015-AP5016*Bodencharakterisierung!$E$8","v":1.2635749477127249E-4},{"$f":"AQ5016/(Bodencharakterisierung!$E$11*1000)","v":8.3404286977737624E-8},4.0771111953513869E-5,{"$error":"#N/A"},null,{"$f":"(AP5016)*$G$11*Bodencharakterisierung!$E$8","v":4.1401748705811276E-9},{"$f":"IF(AF5016<=$J$9*1.05,(AV5016*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW5015,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.356927359997776,null,8.3404286977737621E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,40.484810607722906]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5000,2.3133851319990189E-21,{"$f":"Z5017*EXP((-$J$6/Heterogenität!$D$4)*1)","v":2.2896450676332782E-21},{"$f":"AF5016*Bodencharakterisierung!$E$11/$J$20","v":0},{"$f":"((150*($J$2^0.87)*(AB5017^0.79)*$J$3)/(Bodencharakterisierung!$E$13^2))*($J$12-Z5017)*3600*24","v":0},0,{"$f":"AE5016-AD5017*Bodencharakterisierung!$E$8","v":6.593016037702449E-3},{"$f":"IF(AE5017>$J$18,(AE5017/(Bodencharakterisierung!$E$11*1000)),0)","v":0},2.2896450676332782E-21,{"$error":"#N/A"},null,{"$f":"(AD5017)*$G$11*Bodencharakterisierung!$E$8","v":0},{"$f":"IF(AH5017>0,(AJ5017*Schadstoffbelastung!$K$11+$G$34)/($G$12*$G$7)+AK5016,NA())","v":{"$error":"#N/A"}},null,5000,{"$f":"IF(AF5017<=$J$9*0.05,AS5016*EXP((-$J$6*1)/Heterogenität!$D$4),Z5017)","v":4.0352716932014416E-5},{"$f":"IF(OR(AF5017>=$J$19, AR5016/$J$5<AN5017),0, Bodencharakterisierung!$E$8*$J$11*((AR5016/$J$5)-AN5017))","v":1.2814377364429944E-6},4.1839502149945354E-7,{"$f":"AQ5016-AP5017*Bodencharakterisierung!$E$8","v":1.2621942441417766E-4},{"$f":"AQ5017/(Bodencharakterisierung!$E$11*1000)","v":8.3313151428500103E-8},4.0771111953513869E-5,{"$error":"#N/A"},null,{"$f":"(AP5017)*$G$11*Bodencharakterisierung!$E$8","v":6.0503681853212601E-9},{"$f":"IF(AF5017<=$J$9*1.05,(AV5017*Schadstoffbelastung!$K$11)/($G$12*$G$7)+AW5016,NA())","v":{"$error":"#N/A"}},9999,{"$error":"#N/A"},"",1.6399886323194495,0,31.363199999997775,null,8.3313151428500098E-2,{"$f":"#REF!*10^6","v":{"$error":"#REF!"}},0,40.352716932014417]

{"sheet":"Berechnung","index":11,"n_rows":15,"n_cols":10,"rows_kept":15,"cut":false,"hidden":true,"merged":[[13,6,15,8],[13,0,15,3],[9,0,9,5],[9,6,9,7],[10,0,12,1],[10,3,12,3],[10,4,12,4],[10,6,10,7],[11,6,11,7],[12,6,12,7],[1,6,1,7],[2,0,2,5],[2,6,2,9],[7,6,7,7],[8,6,8,7]],"read":"row_number_cap"}
[]
[null,"Parameter",null,"Einheit","Wert",null,"  Ergebnisparameter",null,"Einheit","Wert"]
["Schadstoffbelastung",null,null,null,null,null,"Dimensionierung Injektionen"]
[null,"Mittlere Konzentration Grundwasser","Cw","µg/L",{"$f":"Schadstoffbelastung!U17","v":2880.0000000809991},null," Infiltriertes Volumen pro Pegel",null,"m3",{"$f":"Calculation!D7","v":30}]
[null,"Mittlere Konzentration Boden","Cges"," mg/kg",{"$f":"Schadstoffbelastung!Y17","v":48.013267327521973},null," Injektionsradius (ROI)",null,"m",{"$f":"Calculation!D8","v":3.5682482323055424}]
[null,"Grenzkonzentration Boden","Cgrenz"," mg/kg",{"$f":"Schadstoffbelastung!X17","v":4.1740000000612856},null," Dauer eines Injektionszyklus",null,"h",{"$f":"Calculation!D9","v":3.4138042220062674}]
[null,"Konzentration Residualphase","Cres"," mg/kg",{"$f":"Schadstoffbelastung!Z17","v":43.839267327460682},null," Durchflussrate pro Pegel",null,"L/s",{"$f":"Calculation!D10","v":2.4410694906329149}]
[null,"Konzentration sorbierte Phase","Cs"," mg/kg",{"$f":"Calculation!D22","v":4382.7000000643475},null," Injektionen unproduktiver Substrat-Verbrauch",null,"Anzahl",{"$f":"Calculation!D11","v":3.36}]
[null,"Sanierungszielwert","-","µg/L",{"$f":"Sanierungsdesign!E4","v":200},null," Injektionen für Schadstoffabbau",null,"Anzahl",{"$f":"Calculation!D12","v":22.803875992319128}]
["Sanierungserfolg",null,null,null,null,null," Gesamtinjektionen für betrachteten Stoff",null,"Anzahl",{"$f":"SUM(J8:J9)","v":26.163875992319127}]
[" Gesamtdauer der mikrobiellen Sanierung",null,null,"Tage",{"$f":"Calculation!C32","v":3374.4779325910808},null," Gesamtzahl der Injektionskampagnen",null,"Anzahl",{"$f":"ROUNDUP(Calculation!G24,0)","v":6}]
[null,null,null,null,null,null," Schadstoffendkonzentration ",null,"µg/L",{"$f":"Calculation!D5","v":199.57993256231023}]
[]
["  Verwendetes Substrat",null,null,null,null,null,"  Betrachteter Schadstoff"]
[null,null,null,null,{"$f":"Sanierungsdesign!E16","v":"Glucose"},null,null,null,null,{"$f":"Calculation!C30","v":"Summe LCKW"}]